Release 6.3i Map G.35
Xilinx Mapping Report File for Design 'ctrl_x'

Design Information
------------------
Command Line   : C:/Xilinx6/bin/nt/map.exe -intstyle ise -p xc2s50-pq208-6 -cm
area -pr b -k 4 -c 100 -tx off -o ctrl_x_map.ncd ctrl_x.ngd ctrl_x.pcf 
Target Device  : x2s50
Target Package : pq208
Target Speed   : -6
Mapper Version : spartan2 -- $Revision: 1.16.8.2 $
Mapped Date    : Wed Aug 15 10:24:15 2012

Design Summary
--------------
Number of errors:      0
Number of warnings:    0
Logic Utilization:
  Number of Slice Flip Flops:       333 out of  1,536   21%
  Number of 4 input LUTs:           320 out of  1,536   20%
Logic Distribution:
    Number of occupied Slices:                         299 out of    768   38%
    Number of Slices containing only related logic:    299 out of    299  100%
    Number of Slices containing unrelated logic:         0 out of    299    0%
        *See NOTES below for an explanation of the effects of unrelated logic
Total Number 4 input LUTs:          382 out of  1,536   24%
      Number used as logic:                       320
      Number used as a route-thru:                 46
      Number used as Shift registers:              16
   Number of bonded IOBs:           113 out of    140   80%
      IOB Flip Flops:                              52
   Number of Tbufs:                 274 out of    832   32%
   Number of GCLKs:                   2 out of      4   50%
   Number of GCLKIOBs:                1 out of      4   25%
   Number of DLLs:                    1 out of      4   25%
   Number of Startups:                1 out of      1  100%

   Number of RPM macros:            1
Total equivalent gate count for design:  15,599
Additional JTAG gate count for IOBs:  5,472
Peak Memory Usage:  63 MB

NOTES:

   Related logic is defined as being logic that shares connectivity -
   e.g. two LUTs are "related" if they share common inputs.
   When assembling slices, Map gives priority to combine logic that
   is related.  Doing so results in the best timing performance.

   Unrelated logic shares no connectivity.  Map will only begin
   packing unrelated logic into a slice once 99% of the slices are
   occupied through related logic packing.

   Note that once logic distribution reaches the 99% level through
   related logic packing, this does not mean the device is completely
   utilized.  Unrelated logic packing will then begin, continuing until
   all usable LUTs and FFs are occupied.  Depending on your timing
   budget, increased levels of unrelated logic packing may adversely
   affect the overall timing performance of your design.


Table of Contents
-----------------
Section 1 - Errors
Section 2 - Warnings
Section 3 - Informational
Section 4 - Removed Logic Summary
Section 5 - Removed Logic
Section 6 - IOB Properties
Section 7 - RPMs
Section 8 - Guide Report
Section 9 - Area Group Summary
Section 10 - Modular Design Summary
Section 11 - Timing Report
Section 12 - Configuration String Information
Section 13 - Additional Device Resource Counts

Section 1 - Errors
------------------

Section 2 - Warnings
--------------------

Section 3 - Informational
-------------------------
INFO:LIT:95 - All of the external outputs in this design are using slew rate
   limited output drivers. The delay on speed critical outputs can be
   dramatically reduced by designating them as fast outputs in the schematic.
INFO:MapLib:562 - No environment variables are currently set.
INFO:MapLib:159 - Net Timing constraints on signal clkin_p are pushed forward
   through input buffer.

Section 4 - Removed Logic Summary
---------------------------------
   4 block(s) optimized away

Section 5 - Removed Logic
-------------------------

Optimized Block(s):
TYPE 		BLOCK
GND 		U6_S1_F0/GND
VCC 		U6_S1_F0/VCC
GND 		XST_GND
VCC 		XST_VCC

To enable printing of redundant blocks removed and signals merged, set the
detailed map report option and rerun map.

Section 6 - IOB Properties
--------------------------

+------------------------------------------------------------------------------------------------------------------------+
| IOB Name                           | Type    | Direction | IO Standard | Drive    | Slew | Reg (s)  | Resistor | IOB   |
|                                    |         |           |             | Strength | Rate |          |          | Delay |
+------------------------------------------------------------------------------------------------------------------------+
| clkin_p                            | GCLKIOB | INPUT     | LVTTL       |          |      |          |          |       |
| add_in<0>                          | IOB     | INPUT     | LVTTL       |          |      | INFF     |          |       |
| add_in<1>                          | IOB     | INPUT     | LVTTL       |          |      | INFF     |          |       |
| add_in<2>                          | IOB     | INPUT     | LVTTL       |          |      | INFF     |          |       |
| add_in<3>                          | IOB     | INPUT     | LVTTL       |          |      |          |          |       |
| add_in<4>                          | IOB     | INPUT     | LVTTL       |          |      |          |          |       |
| add_in<5>                          | IOB     | INPUT     | LVTTL       |          |      |          |          |       |
| add_in<6>                          | IOB     | INPUT     | LVTTL       |          |      |          |          |       |
| am0                                | IOB     | INPUT     | LVTTL       |          |      |          |          |       |
| am1                                | IOB     | INPUT     | LVTTL       |          |      |          |          |       |
| am3                                | IOB     | INPUT     | LVTTL       |          |      |          |          |       |
| am4                                | IOB     | INPUT     | LVTTL       |          |      |          |          |       |
| am5                                | IOB     | INPUT     | LVTTL       |          |      |          |          |       |
| as                                 | IOB     | INPUT     | LVTTL       |          |      |          |          |       |
| bcrsttl                            | IOB     | INPUT     | LVTTL       |          |      |          |          |       |
| brd_sel                            | IOB     | INPUT     | LVTTL       |          |      |          |          |       |
| db<0>                              | IOB     | BIDIR     | LVTTL       | 12       | SLOW | INFF     |          |       |
| db<1>                              | IOB     | BIDIR     | LVTTL       | 12       | SLOW | INFF     |          |       |
| db<2>                              | IOB     | BIDIR     | LVTTL       | 12       | SLOW | INFF     |          |       |
| db<3>                              | IOB     | BIDIR     | LVTTL       | 12       | SLOW | INFF     |          |       |
| db<4>                              | IOB     | BIDIR     | LVTTL       | 12       | SLOW | INFF     |          |       |
| db<5>                              | IOB     | BIDIR     | LVTTL       | 12       | SLOW | INFF     |          |       |
| db<6>                              | IOB     | BIDIR     | LVTTL       | 12       | SLOW | INFF     |          |       |
| db<7>                              | IOB     | BIDIR     | LVTTL       | 12       | SLOW | INFF     |          |       |
| db<8>                              | IOB     | BIDIR     | LVTTL       | 12       | SLOW | INFF     |          |       |
| db<9>                              | IOB     | BIDIR     | LVTTL       | 12       | SLOW | INFF     |          |       |
| db<10>                             | IOB     | BIDIR     | LVTTL       | 12       | SLOW | INFF     |          |       |
| db<11>                             | IOB     | BIDIR     | LVTTL       | 12       | SLOW | INFF     |          |       |
| db<12>                             | IOB     | BIDIR     | LVTTL       | 12       | SLOW | INFF     |          |       |
| db<13>                             | IOB     | BIDIR     | LVTTL       | 12       | SLOW | INFF     |          |       |
| db<14>                             | IOB     | BIDIR     | LVTTL       | 12       | SLOW | INFF     |          |       |
| db<15>                             | IOB     | BIDIR     | LVTTL       | 12       | SLOW | INFF     |          |       |
| delay_0<0>                         | IOB     | OUTPUT    | LVTTL       | 12       | SLOW | OUTFF    |          |       |
| delay_0<1>                         | IOB     | OUTPUT    | LVTTL       | 12       | SLOW | OUTFF    |          |       |
| delay_0<2>                         | IOB     | OUTPUT    | LVTTL       | 12       | SLOW | OUTFF    |          |       |
| delay_0<3>                         | IOB     | OUTPUT    | LVTTL       | 12       | SLOW | OUTFF    |          |       |
| delay_0<4>                         | IOB     | OUTPUT    | LVTTL       | 12       | SLOW | OUTFF    |          |       |
| delay_0<5>                         | IOB     | OUTPUT    | LVTTL       | 12       | SLOW | OUTFF    |          |       |
| delay_0<6>                         | IOB     | OUTPUT    | LVTTL       | 12       | SLOW | OUTFF    |          |       |
| delay_1<0>                         | IOB     | OUTPUT    | LVTTL       | 12       | SLOW | OUTFF    |          |       |
| delay_1<1>                         | IOB     | OUTPUT    | LVTTL       | 12       | SLOW | OUTFF    |          |       |
| delay_1<2>                         | IOB     | OUTPUT    | LVTTL       | 12       | SLOW | OUTFF    |          |       |
| delay_1<3>                         | IOB     | OUTPUT    | LVTTL       | 12       | SLOW | OUTFF    |          |       |
| delay_1<4>                         | IOB     | OUTPUT    | LVTTL       | 12       | SLOW | OUTFF    |          |       |
| delay_1<5>                         | IOB     | OUTPUT    | LVTTL       | 12       | SLOW | OUTFF    |          |       |
| delay_1<6>                         | IOB     | OUTPUT    | LVTTL       | 12       | SLOW | OUTFF    |          |       |
| difbcr                             | IOB     | OUTPUT    | LVTTL       | 12       | SLOW |          |          |       |
| difevr                             | IOB     | OUTPUT    | LVTTL       | 12       | SLOW |          |          |       |
| difrst                             | IOB     | OUTPUT    | LVTTL       | 12       | SLOW |          |          |       |
| diftrg                             | IOB     | OUTPUT    | LVTTL       | 12       | SLOW |          |          |       |
| done_in                            | IOB     | INPUT     | LVTTL       |          |      |          |          |       |
| done_out                           | IOB     | OUTPUT    | LVTTL       | 12       | SLOW |          |          |       |
| ds0                                | IOB     | INPUT     | LVTTL       |          |      | INFF     |          |       |
| ds1                                | IOB     | INPUT     | LVTTL       |          |      |          |          |       |
| dtack                              | IOB     | OUTPUT    | LVTTL       | 12       | SLOW |          |          |       |
| evrsttl                            | IOB     | INPUT     | LVTTL       |          |      |          |          |       |
| fltb                               | IOB     | INPUT     | LVTTL       |          |      |          |          |       |
| g245                               | IOB     | OUTPUT    | LVTTL       | 12       | SLOW |          |          |       |
| iack                               | IOB     | INPUT     | LVTTL       |          |      |          |          |       |
| iackin                             | IOB     | INPUT     | LVTTL       |          |      |          |          |       |
| iackout                            | IOB     | OUTPUT    | LVTTL       | 12       | SLOW |          |          |       |
| int_ext<0>                         | IOB     | INPUT     | LVTTL       |          |      |          |          |       |
| int_ext<1>                         | IOB     | INPUT     | LVTTL       |          |      |          |          |       |
| intled                             | IOB     | OUTPUT    | LVTTL       | 12       | SLOW |          |          |       |
| irq<1>                             | IOB     | OUTPUT    | LVTTL       | 12       | SLOW |          |          |       |
| irq<2>                             | IOB     | OUTPUT    | LVTTL       | 12       | SLOW |          |          |       |
| irq<3>                             | IOB     | OUTPUT    | LVTTL       | 12       | SLOW |          |          |       |
| irq<4>                             | IOB     | OUTPUT    | LVTTL       | 12       | SLOW |          |          |       |
| irq<5>                             | IOB     | OUTPUT    | LVTTL       | 12       | SLOW |          |          |       |
| irq<6>                             | IOB     | OUTPUT    | LVTTL       | 12       | SLOW |          |          |       |
| irq<7>                             | IOB     | OUTPUT    | LVTTL       | 12       | SLOW |          |          |       |
| jroberr                            | IOB     | INPUT     | LVTTL       |          |      |          |          |       |
| jtadd<0>                           | IOB     | OUTPUT    | LVTTL       | 12       | SLOW | OUTFF    |          |       |
| jtadd<1>                           | IOB     | OUTPUT    | LVTTL       | 12       | SLOW | OUTFF    |          |       |
| jtadd<2>                           | IOB     | OUTPUT    | LVTTL       | 12       | SLOW | OUTFF    |          |       |
| jtadd<3>                           | IOB     | OUTPUT    | LVTTL       | 12       | SLOW | OUTFF    |          |       |
| jtck                               | IOB     | OUTPUT    | LVTTL       | 24       | SLOW | OUTFF    |          |       |
| jtdi                               | IOB     | OUTPUT    | LVTTL       | 24       | SLOW | OUTFF    |          |       |
| jtdo                               | IOB     | INPUT     | LVTTL       |          |      |          |          |       |
| jtms                               | IOB     | OUTPUT    | LVTTL       | 24       | SLOW | OUTFF    |          |       |
| jtrkadv                            | IOB     | OUTPUT    | LVTTL       | 24       | SLOW | OUTFF    |          |       |
| jtrkrst                            | IOB     | OUTPUT    | LVTTL       | 24       | SLOW | OUTFF    |          |       |
| jtrktm                             | IOB     | OUTPUT    | LVTTL       | 24       | SLOW |          |          |       |
| locked                             | IOB     | OUTPUT    | LVTTL       | 12       | SLOW |          |          |       |
| lword                              | IOB     | INPUT     | LVTTL       |          |      |          |          |       |
| mcbcrst                            | IOB     | OUTPUT    | LVTTL       | 12       | SLOW |          |          |       |
| mcevrst                            | IOB     | OUTPUT    | LVTTL       | 12       | SLOW |          |          |       |
| mctrg                              | IOB     | OUTPUT    | LVTTL       | 12       | SLOW |          |          |       |
| plsttl<0>                          | IOB     | INPUT     | LVTTL       |          |      |          |          |       |
| plsttl<1>                          | IOB     | INPUT     | LVTTL       |          |      |          |          |       |
| pulse<0>                           | IOB     | OUTPUT    | LVTTL       | 12       | SLOW |          |          |       |
| pulse<1>                           | IOB     | OUTPUT    | LVTTL       | 12       | SLOW |          |          |       |
| robrsttl                           | IOB     | INPUT     | LVTTL       |          |      |          |          |       |
| ron<0>                             | IOB     | OUTPUT    | LVTTL       | 12       | SLOW | OUTFF    |          |       |
| ron<1>                             | IOB     | OUTPUT    | LVTTL       | 12       | SLOW | OUTFF    |          |       |
| ron<2>                             | IOB     | OUTPUT    | LVTTL       | 12       | SLOW | OUTFF    |          |       |
| ron<3>                             | IOB     | OUTPUT    | LVTTL       | 12       | SLOW | OUTFF    |          |       |
| ron<4>                             | IOB     | OUTPUT    | LVTTL       | 12       | SLOW | OUTFF    |          |       |
| ron<5>                             | IOB     | OUTPUT    | LVTTL       | 12       | SLOW | OUTFF    |          |       |
| ron<6>                             | IOB     | OUTPUT    | LVTTL       | 12       | SLOW | OUTFF    |          |       |
| sysreset                           | IOB     | INPUT     | LVTTL       |          |      |          |          |       |
| tdio                               | IOB     | BIDIR     | LVTTL       | 12       | SLOW | INFF     |          |       |
| tp1                                | IOB     | OUTPUT    | LVTTL       | 12       | SLOW |          |          |       |
| tp2                                | IOB     | OUTPUT    | LVTTL       | 12       | SLOW |          |          |       |
| tp3                                | IOB     | OUTPUT    | LVTTL       | 12       | SLOW |          |          |       |
| trg_dly_p                          | IOB     | OUTPUT    | LVTTL       | 12       | SLOW |          |          |       |
| trganal                            | IOB     | OUTPUT    | LVTTL       | 12       | SLOW |          |          |       |
| trgled                             | IOB     | OUTPUT    | LVTTL       | 12       | SLOW |          |          |       |
| trgnim                             | IOB     | INPUT     | LVTTL       |          |      |          |          |       |
| trgros                             | IOB     | OUTPUT    | LVTTL       | 12       | SLOW |          |          |       |
| trgttc                             | IOB     | OUTPUT    | LVTTL       | 12       | SLOW |          |          |       |
| trgttl                             | IOB     | INPUT     | LVTTL       |          |      |          |          |       |
| veto                               | IOB     | INPUT     | LVTTL       |          |      | INFF     |          |       |
| write                              | IOB     | INPUT     | LVTTL       |          |      |          |          |       |
+------------------------------------------------------------------------------------------------------------------------+

Section 7 - RPMs
----------------
U6_S1_F0/hset                           

Section 8 - Guide Report
------------------------
Guide not run on this design.

Section 9 - Area Group Summary
------------------------------
No area groups were found in this design.

Section 10 - Modular Design Summary
-----------------------------------
Modular Design not used for this design.

Section 11 - Timing Report
--------------------------
This design was not run using timing mode.

Section 12 - Configuration String Details
-----------------------------------------
Use the "-detail" map option to print out Configuration Strings

Section 13 - Additional Device Resource Counts
----------------------------------------------
Number of JTAG Gates for IOBs = 114
Number of Equivalent Gates for Design = 15,599
Number of RPM Macros = 1
Number of Hard Macros = 0
PCI IOBs = 0
PCI LOGICs = 0
CAPTUREs = 0
BSCANs = 0
STARTUPs = 1
DLLs = 1
GCLKIOBs = 1
GCLKs = 2
Block RAMs = 0
TBUFs = 274
Total Registers (Flops & Latches in Slices & IOBs) not driven by LUTs = 270
IOB Latches not driven by LUTs = 0
IOB Latches = 0
IOB Flip Flops not driven by LUTs = 50
IOB Flip Flops = 52
Unbonded IOBs = 0
Bonded IOBs = 113
Shift Registers = 16
Static Shift Registers = 16
Dynamic Shift Registers = 0
16x1 ROMs = 0
16x1 RAMs = 0
32x1 RAMs = 0
Dual Port RAMs = 0
MULTANDs = 0
MUXF5s + MUXF6s = 2
4 input LUTs used as Route-Thrus = 46
4 input LUTs = 320
Slice Latches not driven by LUTs = 0
Slice Latches = 0
Slice Flip Flops not driven by LUTs = 220
Slice Flip Flops = 333
Slices = 299
Number of LUT signals with 4 loads = 5
Number of LUT signals with 3 loads = 6
Number of LUT signals with 2 loads = 74
Number of LUT signals with 1 load = 190
NGM Average fanout of LUT = 3.88
NGM Maximum fanout of LUT = 99
NGM Average fanin for LUT = 3.0688
Number of LUT symbols = 320
Number of IPAD symbols = 36
Number of IBUF symbols = 52
Number of BIPAD symbols = 17
