Field=Comment~String~Comment~100|Field=Description~String~Description~100|Field=Designator~String~Designator~100|Field=Footprint~String~Footprint~100|Field=LibRef~String~LibRef~100|Field=Quantity~Integer~Quantity~100|ReportField=Currency~<none>|ReportField=ProductionQuantity~1|ReportField=ProjectFileName~VME-PATCH.PrjPCB|ReportField=ProjectFullPath~C:\Users\Public\Documents\Altium\Cris\VME-PATCH.PrjPCB|ReportField=Title~Bill of Materials For PCB Document [PCB1.PcbDoc]|ReportField=TotalQuantity~216|ReportField=ReportTime~13:58:54|ReportField=ReportDate~30/07/2012|ReportField=ReportDateTime~30/07/2012 13:58:54|ReportField=OutputName~Bill of Materials|ReportField=OutputType~BOM_PartType|ReportField=GeneratorName~BOM|ReportField=GeneratorDescription~Bill of Materials|ReportField=VariantName~None|ReportField=DataSourceFileName~PCB1.PcbDoc|ReportField=DataSourceFullPath~C:\Users\Public\Documents\Altium\Cris\PCB1.PcbDoc
Cap|Capacitor|C1, C2, C3, C4, C5, C6, C7, C8, C38, C39, C40, C42, C43, C44, C45, C46, C47, C48, C49, C50, C51, C52, C53, C54, C55, C56, C57, C58, C59, C60, C61, C62, C63, C64, C65, C66, C67, C68, C69, C70, C71|0603 (1608m)|Cap|41
Cap|Capacitor|C9, C10, C12, C13, C14, C15, C16, C17, C18, C19, C21, C24, C27, C30|0805 (2012m)|Cap|14
Cap|Capacitor|C11, C20, C22, C23, C25, C26, C28, C29, C31, C32|0402 (1005m)|Cap|10
Cap Pol1|Polarized Capacitor (Radial)|C33, C35, C36, C37|Cap Ta D (EIA7343)|Cap Pol1|4
T491B|Solid Tantalum Chip Capacitor, Standard T491 Series - Industrial Grade|C34, C41|B|T491B|2
LED3|Typical BLUE SiC LED|D1, D3, D4, D6, D7|LED 0805 (2012m)|LED3|5
PMLL4148|Default Diode|D2|D1206 (3216m)|Diode|1
Diode 1N4148|High Conductance Fast Diode|D5|1206 (3216m)|Diode 1N4148|1
Fuse 1|Fuse|F1|1206 (3216m)|Fuse 1|1
VME_DIN96||J1, J2|0903196X922|VME_DIN96|2
D Connector 15|Receptacle Assembly, 15 Position, Right Angle|J3|DSUB1.385-2H15|D Connector 15|1
light guide||LG1, LG2|light guide|light guide|2
Header 7X2|Header, 7-Pin, Dual row|P1|con14_conexcon2160|Header 7X2|1
Header 2|Header, 2-Pin|P2, P3, P4, P5, P6|SPADE|Header 2|5
PMBT2222A|NPN Switching Transistor|Q1, Q2|SOT23_N|PMBT2222A|2
Res3|Resistor|R1, R2, R3, R4, R5, R6, R7, R8, R24, R25, R26, R28, R29|0603 (1608m)|Res3|13
Res1|Resistor|R9, R10, R11, R12, R13, R14, R15, R16, R17, R18, R19, R20, R23, R27, R30, R31, R32, R33, R34, R42, R43, R44, R45, R46, R47, R48, R49, R50, R51, R52, R53, R54, R55, R56, R57, R58, R59, R60, R61, R62, R63, R64, R65, R66, R67, R68, R69, R70, R71, R72, R73|0603 (1608m)|Res1|51
Res3|Resistor|R21, R22|2512 (6432m)|Res3|2
RES 0603|Resistor|R35, R36, R37, R38, R39, R40, R41, R74, R75, R76, R77, R78, R79, R80, R81, R82, R83, R84, R85|0603 (1608m)|RES 0603|19
SW DIP-6|DIP Switch, 6 Position, SPST|S1|DIP-12/SW|SW DIP-6|1
IXO71-40MHz||U1|XTAL7X5|IXO71-40MHz|1
SN74LVC2G07||U2, U4, U5, U6|SOT26A-6N|SN74LVC2G07|4
MAX4618||U3|NSO16_N|MAX4618|1
XC6SLX9-2TQG144C|Spartan-6 LX 1.2V FPGA, 102 User I/Os, 144-Pin TQFP (0.5mm Pitch), Speed Grade 2, Commercial Grade, Pb-Free|U7|TQG144_N|XC6SLX9-2TQG144C|1
XCF04SVOG20C|XCF00S Series, Platform Flash In-System Programmable Configuration 3.3V PROM, 20-Pin TSOP, 4-Megabit, Commercial Grade, Pb-Free|U8|VOG20_N|XCF04SVOG20C|1
PULSADOR||U9|PULSADOR|PULSADOR|1
PH1||U10, U11, U25|PIN1|TESTPOINT|3
mic29301-3.3V||U12|TO263-5____DDPAK-ET5_M + vias|mic29301|1
MCP1824-1202E/OT||U13|SOT23-5AN|MCP1824-1202E/OT|1
SN74LVC1G126DBVR|Tri-state buffer|U14, U28, U29, U30, U38|SOT23-5AN|SN74LVC1G126DBVR|5
MIC1555||U15|SOT23-5AN|MIC1555|1
TESTPOINT||U16, U19, U20|PIN1|TESTPOINT|3
MAX4375TEUA||U17, U18|UMAX10|MAX4375TEUA|2
SN74LVTH16245ADGGR|3.3-V ABT 16-Bit Bus Transceiver with 3-State Outputs|U21, U31|DGG048|SN74LVC16245ADGG, SN74LVTH16245ADGGR|2
SN74LVCH244APW|Octal Buffer/Driver with 3-State Outputs|U22|PW020_N|SN74LVCH244APW|1
SN74LVTH16244ADGGR||U23, U24|DGG048|SN74LVCH16244ADGG|2
SN74ALS642A-1DW|Octal Bus Transceiver with Open-Collector Outputs|U26|DW020_N|SN74ALS642A-1DW|1
SN74ALS688DW|8-Bit Identity Comparator|U27, U35|DW020_N|SN74ALS688DW|2
SN74LVTH16244ADGGR|3.3-V ABT 16-Bit Buffer/Driver with 3-State Outputs|U32, U33, U34, U36, U37|DGG048_N|SN74LVTH16244ADGGR|5
