Par Statistics
Total Non-vccgnd Signals=414
Total Non-vccgnd Design Pins=1416
Total Non-vccgnd Conns=1416
Total Non-vccgnd Timing Constrained Conns=574
Phase 1 CPU=4.4 sec
Phase 2 CPU=4.5 sec
Phase 3 CPU=5.7 sec
Phase 4 CPU=6.4 sec
Phase 5 CPU=6.9 sec
Phase 6 CPU=7.0 sec
Phase 7 CPU=7.0 sec
Phase 8 CPU=7.0 sec
Phase 9 CPU=7.0 sec
Phase 10 CPU=7.1 sec
AvgWirelenPerPin Fanout 1=5.0
AvgWirelenPerPin Fanout 2=10.0
AvgWirelenPerPin Fanout 3=11.7
AvgWirelenPerPin Fanout 4=9.0
AvgWirelenPerPin Fanout 10=12.9
AvgWirelenPerPin Fanout 50=4.5
AvgWirelenPerPin Fanout 100=19.1
AvgWirelenPerPin Fanout 500=0.0
AvgWirelenPerPin Fanout 5000=0.0
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
AvgWirelenPerPin Fanout 100000=0.0
IRR Gamma=1.1815