Release 13.3 - par O.76xd (nt)
Copyright (c) 1995-2011 Xilinx, Inc.  All rights reserved.

Fri Nov 01 08:59:01 2013


INFO: The IO information is provided in three file formats as part of the Place and Route (PAR) process.  These formats are:
1. The <design name>_pad.txt file (this file) designed to provide information on IO usage in a human readable ASCII text format viewable through common text editors.
2. The <design namd>_pad.csv file for use with spreadsheet programs such as MS Excel. This file can also be read by PACE to communicate post PAR IO information.
3. The <design name>.pad file designed for parsing by customers.  It uses the "|" as a data field separator.

INPUT FILE:       vme_patch_map.ncd
OUTPUT FILE:      vme_patch_pad.txt
PART TYPE:        xc6slx4
SPEED GRADE:      -2
PACKAGE:          tqg144

Pinout by Pin Number:

+--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
|Pin Number|Signal Name       |Pin Usage|Pin Name                  |Direction|IO Standard|IO Bank Number|Drive (mA)|Slew Rate|Termination|IOB Delay|Voltage|Constraint|IO Register|Signal Integrity|
+--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
|P1        |SignalDetect_3<1> |IOB      |IO_L83N_VREF_3            |INPUT    |LVCMOS25*  |3             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P2        |SignalDetect_3<0> |IOB      |IO_L83P_3                 |INPUT    |LVCMOS25*  |3             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P3        |                  |         |GND                       |         |           |              |          |         |           |         |       |          |           |                |
|P4        |                  |         |VCCO_3                    |         |           |3             |          |         |           |         |2.50   |          |           |                |
|P5        |SignalDetect_5<2> |IOB      |IO_L52N_3                 |INPUT    |LVCMOS25*  |3             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P6        |SignalDetect_5<1> |IOB      |IO_L52P_3                 |INPUT    |LVCMOS25*  |3             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P7        |SignalDetect_5<0> |IOB      |IO_L51N_3                 |INPUT    |LVCMOS25*  |3             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P8        |SignalDetect_4<2> |IOB      |IO_L51P_3                 |INPUT    |LVCMOS25*  |3             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P9        |SignalDetect_4<1> |IOB      |IO_L50N_3                 |INPUT    |LVCMOS25*  |3             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P10       |SignalDetect_4<0> |IOB      |IO_L50P_3                 |INPUT    |LVCMOS25*  |3             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P11       |SignalDetect_7<2> |IOB      |IO_L49N_3                 |INPUT    |LVCMOS25*  |3             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P12       |SignalDetect_7<1> |IOB      |IO_L49P_3                 |INPUT    |LVCMOS25*  |3             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P13       |                  |         |GND                       |         |           |              |          |         |           |         |       |          |           |                |
|P14       |SignalDetect_7<0> |IOB      |IO_L44N_GCLK20_3          |INPUT    |LVCMOS25*  |3             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P15       |SignalDetect_6<2> |IOB      |IO_L44P_GCLK21_3          |INPUT    |LVCMOS25*  |3             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P16       |SignalDetect_6<1> |IOB      |IO_L43N_GCLK22_IRDY2_3    |INPUT    |LVCMOS25*  |3             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P17       |SignalDetect_6<0> |IOB      |IO_L43P_GCLK23_3          |INPUT    |LVCMOS25*  |3             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P18       |                  |         |VCCO_3                    |         |           |3             |          |         |           |         |2.50   |          |           |                |
|P19       |                  |         |VCCINT                    |         |           |              |          |         |           |         |1.2    |          |           |                |
|P20       |                  |         |VCCAUX                    |         |           |              |          |         |           |         |2.5    |          |           |                |
|P21       |clk               |IOB      |IO_L42N_GCLK24_3          |INPUT    |LVCMOS25*  |3             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P22       |SignalDetect_12<2>|IOB      |IO_L42P_GCLK25_TRDY2_3    |INPUT    |LVCMOS25*  |3             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P23       |SignalDetect_12<1>|IOB      |IO_L41N_GCLK26_3          |INPUT    |LVCMOS25*  |3             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P24       |SignalDetect_12<0>|IOB      |IO_L41P_GCLK27_3          |INPUT    |LVCMOS25*  |3             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P25       |                  |         |GND                       |         |           |              |          |         |           |         |       |          |           |                |
|P26       |SignalDetect_2<2> |IOB      |IO_L37N_3                 |INPUT    |LVCMOS25*  |3             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P27       |SignalDetect_2<1> |IOB      |IO_L37P_3                 |INPUT    |LVCMOS25*  |3             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P28       |                  |         |VCCINT                    |         |           |              |          |         |           |         |1.2    |          |           |                |
|P29       |SignalDetect_2<0> |IOB      |IO_L36N_3                 |INPUT    |LVCMOS25*  |3             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P30       |SCL               |IOB      |IO_L36P_3                 |BIDIR    |LVCMOS25*  |3             |12        |SLOW     |PULLUP     |NONE     |       |LOCATED   |YES        |NONE            |
|P31       |                  |         |VCCO_3                    |         |           |3             |          |         |           |         |2.50   |          |           |                |
|P32       |SignalDetect_8<2> |IOB      |IO_L2N_3                  |INPUT    |LVCMOS25*  |3             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P33       |SignalDetect_8<1> |IOB      |IO_L2P_3                  |INPUT    |LVCMOS25*  |3             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P34       |SignalDetect_8<0> |IOB      |IO_L1N_VREF_3             |INPUT    |LVCMOS25*  |3             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P35       |iack              |IOB      |IO_L1P_3                  |INPUT    |LVCMOS25*  |3             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P36       |                  |         |VCCAUX                    |         |           |              |          |         |           |         |2.5    |          |           |                |
|P37       |                  |         |PROGRAM_B_2               |         |           |              |          |         |           |         |       |          |           |                |
|P38       |SDA               |IOB      |IO_L65N_CSO_B_2           |BIDIR    |LVCMOS25*  |2             |12        |SLOW     |PULLUP     |NONE     |       |LOCATED   |YES        |NONE            |
|P39       |                  |IOBM     |IO_L65P_INIT_B_2          |UNUSED   |           |2             |          |         |           |         |       |          |           |                |
|P40       |Vwrite            |IOB      |IO_L64N_D9_2              |INPUT    |LVCMOS25*  |2             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P41       |LEDS<1>           |IOB      |IO_L64P_D8_2              |OUTPUT   |LVCMOS25*  |2             |12        |SLOW     |           |         |       |LOCATED   |NO         |NONE            |
|P42       |                  |         |VCCO_2                    |         |           |2             |          |         |           |         |2.50   |          |           |                |
|P43       |Read_J2           |IOB      |IO_L62N_D6_2              |OUTPUT   |LVCMOS25*  |2             |12        |SLOW     |           |         |       |LOCATED   |NO         |NONE            |
|P44       |lword             |IOB      |IO_L62P_D5_2              |INPUT    |LVCMOS25*  |2             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P45       |Write_J2          |IOB      |IO_L49N_D4_2              |OUTPUT   |LVCMOS25*  |2             |12        |SLOW     |           |         |       |LOCATED   |NO         |NONE            |
|P46       |add_hold          |IOB      |IO_L49P_D3_2              |OUTPUT   |LVCMOS25*  |2             |12        |SLOW     |           |         |       |LOCATED   |NO         |NONE            |
|P47       |Reset_J2          |IOB      |IO_L48N_RDWR_B_VREF_2     |OUTPUT   |LVCMOS25*  |2             |12        |SLOW     |           |         |       |LOCATED   |NO         |NONE            |
|P48       |DoutOE            |IOB      |IO_L48P_D7_2              |OUTPUT   |LVCMOS25*  |2             |12        |SLOW     |           |         |       |LOCATED   |NO         |NONE            |
|P49       |                  |         |GND                       |         |           |              |          |         |           |         |       |          |           |                |
|P50       |DoutDir           |IOB      |IO_L31N_GCLK30_D15_2      |OUTPUT   |LVCMOS25*  |2             |12        |SLOW     |           |         |       |LOCATED   |NO         |NONE            |
|P51       |iackout           |IOB      |IO_L31P_GCLK31_D14_2      |OUTPUT   |LVCMOS25*  |2             |12        |SLOW     |           |         |       |LOCATED   |NO         |NONE            |
|P52       |                  |         |VCCINT                    |         |           |              |          |         |           |         |1.2    |          |           |                |
|P53       |                  |         |VCCAUX                    |         |           |              |          |         |           |         |2.5    |          |           |                |
|P54       |                  |         |GND                       |         |           |              |          |         |           |         |       |          |           |                |
|P55       |I2C_Add_p<1>      |IOB      |IO_L30N_GCLK0_USERCCLK_2  |OUTPUT   |LVCMOS25*  |2             |12        |SLOW     |           |         |       |LOCATED   |NO         |NONE            |
|P56       |I2C_Add_p<0>      |IOB      |IO_L30P_GCLK1_D13_2       |OUTPUT   |LVCMOS25*  |2             |12        |SLOW     |           |         |       |LOCATED   |NO         |NONE            |
|P57       |as                |IOB      |IO_L14N_D12_2             |INPUT    |LVCMOS25*  |2             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P58       |ds1               |IOB      |IO_L14P_D11_2             |INPUT    |LVCMOS25*  |2             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P59       |irq<7>            |IOB      |IO_L13N_D10_2             |OUTPUT   |LVCMOS25*  |2             |12        |SLOW     |           |         |       |LOCATED   |NO         |NONE            |
|P60       |Spare_J2          |IOB      |IO_L13P_M1_2              |OUTPUT   |LVCMOS25*  |2             |12        |SLOW     |           |         |       |LOCATED   |NO         |NONE            |
|P61       |iackin            |IOB      |IO_L12N_D2_MISO3_2        |INPUT    |LVCMOS25*  |2             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P62       |dtack_p           |IOB      |IO_L12P_D1_MISO2_2        |OUTPUT   |LVCMOS25*  |2             |12        |SLOW     |           |         |       |LOCATED   |NO         |NONE            |
|P63       |                  |         |VCCO_2                    |         |           |2             |          |         |           |         |2.50   |          |           |                |
|P64       |ds0               |IOB      |IO_L3N_MOSI_CSI_B_MISO0_2 |INPUT    |LVCMOS25*  |2             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P65       |TP<0>             |IOB      |IO_L3P_D0_DIN_MISO_MISO1_2|OUTPUT   |LVCMOS25*  |2             |12        |SLOW     |           |         |       |LOCATED   |NO         |NONE            |
|P66       |brd_sel_16_p      |IOB      |IO_L2N_CMPMOSI_2          |INPUT    |LVCMOS25*  |2             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P67       |add_mod_ok        |IOB      |IO_L2P_CMPCLK_2           |INPUT    |LVCMOS25*  |2             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P68       |                  |         |GND                       |         |           |              |          |         |           |         |       |          |           |                |
|P69       |LEDS<0>           |IOB      |IO_L1N_M0_CMPMISO_2       |OUTPUT   |LVCMOS25*  |2             |12        |SLOW     |           |         |       |LOCATED   |NO         |NONE            |
|P70       |TP<1>             |IOB      |IO_L1P_CCLK_2             |OUTPUT   |LVCMOS25*  |2             |12        |SLOW     |           |         |       |LOCATED   |NO         |NONE            |
|P71       |                  |         |DONE_2                    |         |           |              |          |         |           |         |       |          |           |                |
|P72       |                  |         |CMPCS_B_2                 |         |           |              |          |         |           |         |       |          |           |                |
|P73       |                  |         |SUSPEND                   |         |           |              |          |         |           |         |       |          |           |                |
|P74       |DOUT_J2<6>        |IOB      |IO_L74N_DOUT_BUSY_1       |BIDIR    |LVCMOS25*  |1             |12        |SLOW     |           |NONE     |       |LOCATED   |NO         |NONE            |
|P75       |SignalDetect_1<0> |IOB      |IO_L74P_AWAKE_1           |INPUT    |LVCMOS25*  |1             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P76       |                  |         |VCCO_1                    |         |           |1             |          |         |           |         |2.50   |          |           |                |
|P77       |                  |         |GND                       |         |           |              |          |         |           |         |       |          |           |                |
|P78       |SignalDetect_1<2> |IOB      |IO_L47N_1                 |INPUT    |LVCMOS25*  |1             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P79       |SignalDetect_1<1> |IOB      |IO_L47P_1                 |INPUT    |LVCMOS25*  |1             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P80       |SignalDetect_11<1>|IOB      |IO_L46N_1                 |INPUT    |LVCMOS25*  |1             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P81       |DOUT_J2<3>        |IOB      |IO_L46P_1                 |BIDIR    |LVCMOS25*  |1             |12        |SLOW     |           |NONE     |       |LOCATED   |NO         |NONE            |
|P82       |SignalDetect_11<2>|IOB      |IO_L45N_1                 |INPUT    |LVCMOS25*  |1             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P83       |DOUT_J2<5>        |IOB      |IO_L45P_1                 |BIDIR    |LVCMOS25*  |1             |12        |SLOW     |           |NONE     |       |LOCATED   |NO         |NONE            |
|P84       |DOUT_J2<1>        |IOB      |IO_L43N_GCLK4_1           |BIDIR    |LVCMOS25*  |1             |12        |SLOW     |           |NONE     |       |LOCATED   |NO         |NONE            |
|P85       |DOUT_J2<2>        |IOB      |IO_L43P_GCLK5_1           |BIDIR    |LVCMOS25*  |1             |12        |SLOW     |           |NONE     |       |LOCATED   |NO         |NONE            |
|P86       |                  |         |VCCO_1                    |         |           |1             |          |         |           |         |2.50   |          |           |                |
|P87       |DOUT_J2<0>        |IOB      |IO_L42N_GCLK6_TRDY1_1     |BIDIR    |LVCMOS25*  |1             |12        |SLOW     |           |NONE     |       |LOCATED   |NO         |NONE            |
|P88       |DOUT_J2<4>        |IOB      |IO_L42P_GCLK7_1           |BIDIR    |LVCMOS25*  |1             |12        |SLOW     |           |NONE     |       |LOCATED   |NO         |NONE            |
|P89       |                  |         |VCCINT                    |         |           |              |          |         |           |         |1.2    |          |           |                |
|P90       |                  |         |VCCAUX                    |         |           |              |          |         |           |         |2.5    |          |           |                |
|P91       |                  |         |GND                       |         |           |              |          |         |           |         |       |          |           |                |
|P92       |SignalDetect_11<0>|IOB      |IO_L41N_GCLK8_1           |INPUT    |LVCMOS25*  |1             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P93       |SignalDetect_9<2> |IOB      |IO_L41P_GCLK9_IRDY1_1     |INPUT    |LVCMOS25*  |1             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P94       |SignalDetect_9<1> |IOB      |IO_L40N_GCLK10_1          |INPUT    |LVCMOS25*  |1             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P95       |SignalDetect_9<0> |IOB      |IO_L40P_GCLK11_1          |INPUT    |LVCMOS25*  |1             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P96       |                  |         |GND                       |         |           |              |          |         |           |         |       |          |           |                |
|P97       |SignalDetect_10<2>|IOB      |IO_L34N_1                 |INPUT    |LVCMOS25*  |1             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P98       |SignalDetect_10<1>|IOB      |IO_L34P_1                 |INPUT    |LVCMOS25*  |1             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P99       |SignalDetect_10<0>|IOB      |IO_L33N_1                 |INPUT    |LVCMOS25*  |1             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P100      |SignalDetect_3<2> |IOB      |IO_L33P_1                 |INPUT    |LVCMOS25*  |1             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P101      |add_p_1<1>        |IOB      |IO_L32N_1                 |INPUT    |LVCMOS25*  |1             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P102      |add_p_1<2>        |IOB      |IO_L32P_1                 |INPUT    |LVCMOS25*  |1             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P103      |                  |         |VCCO_1                    |         |           |1             |          |         |           |         |2.50   |          |           |                |
|P104      |add_p_1<3>        |IOB      |IO_L1N_VREF_1             |INPUT    |LVCMOS25*  |1             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P105      |add_p_1<0>        |IOB      |IO_L1P_1                  |INPUT    |LVCMOS25*  |1             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P106      |                  |         |TDO                       |         |           |              |          |         |           |         |       |          |           |                |
|P107      |                  |         |TMS                       |         |           |              |          |         |           |         |       |          |           |                |
|P108      |                  |         |GND                       |         |           |              |          |         |           |         |       |          |           |                |
|P109      |                  |         |TCK                       |         |           |              |          |         |           |         |       |          |           |                |
|P110      |                  |         |TDI                       |         |           |              |          |         |           |         |       |          |           |                |
|P111      |db<3>             |IOB      |IO_L66N_SCP0_0            |BIDIR    |LVCMOS25*  |0             |12        |SLOW     |           |NONE     |       |LOCATED   |NO         |NONE            |
|P112      |db<6>             |IOB      |IO_L66P_SCP1_0            |BIDIR    |LVCMOS25*  |0             |12        |SLOW     |           |NONE     |       |LOCATED   |NO         |NONE            |
|P113      |                  |         |GND                       |         |           |              |          |         |           |         |       |          |           |                |
|P114      |db<5>             |IOB      |IO_L65N_SCP2_0            |BIDIR    |LVCMOS25*  |0             |12        |SLOW     |           |NONE     |       |LOCATED   |NO         |NONE            |
|P115      |db<4>             |IOB      |IO_L65P_SCP3_0            |BIDIR    |LVCMOS25*  |0             |12        |SLOW     |           |NONE     |       |LOCATED   |NO         |NONE            |
|P116      |db<1>             |IOB      |IO_L64N_SCP4_0            |BIDIR    |LVCMOS25*  |0             |12        |SLOW     |           |NONE     |       |LOCATED   |NO         |NONE            |
|P117      |db<2>             |IOB      |IO_L64P_SCP5_0            |BIDIR    |LVCMOS25*  |0             |12        |SLOW     |           |NONE     |       |LOCATED   |NO         |NONE            |
|P118      |db<7>             |IOB      |IO_L63N_SCP6_0            |BIDIR    |LVCMOS25*  |0             |12        |SLOW     |           |NONE     |       |LOCATED   |NO         |NONE            |
|P119      |db<0>             |IOB      |IO_L63P_SCP7_0            |BIDIR    |LVCMOS25*  |0             |12        |SLOW     |           |NONE     |       |LOCATED   |NO         |NONE            |
|P120      |add_p_2<8>        |IOB      |IO_L62N_VREF_0            |INPUT    |LVCMOS25*  |0             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P121      |add_p_2<7>        |IOB      |IO_L62P_0                 |INPUT    |LVCMOS25*  |0             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P122      |                  |         |VCCO_0                    |         |           |0             |          |         |           |         |2.50   |          |           |                |
|P123      |g245_p            |IOB      |IO_L37N_GCLK12_0          |OUTPUT   |LVCMOS25*  |0             |12        |SLOW     |           |         |       |LOCATED   |NO         |NONE            |
|P124      |BRDSEL_J2<11>     |IOB      |IO_L37P_GCLK13_0          |OUTPUT   |LVCMOS25*  |0             |12        |SLOW     |           |         |       |LOCATED   |NO         |NONE            |
|P125      |                  |         |VCCO_0                    |         |           |0             |          |         |           |         |2.50   |          |           |                |
|P126      |add_p_2<6>        |IOB      |IO_L36N_GCLK14_0          |INPUT    |LVCMOS25*  |0             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P127      |add_p_2<5>        |IOB      |IO_L36P_GCLK15_0          |INPUT    |LVCMOS25*  |0             |          |         |           |NONE     |       |LOCATED   |NO         |NONE            |
|P128      |                  |         |VCCINT                    |         |           |              |          |         |           |         |1.2    |          |           |                |
|P129      |                  |         |VCCAUX                    |         |           |              |          |         |           |         |2.5    |          |           |                |
|P130      |                  |         |GND                       |         |           |              |          |         |           |         |       |          |           |                |
|P131      |BRDSEL_J2<10>     |IOB      |IO_L35N_GCLK16_0          |OUTPUT   |LVCMOS25*  |0             |12        |SLOW     |           |         |       |LOCATED   |NO         |NONE            |
|P132      |BRDSEL_J2<9>      |IOB      |IO_L35P_GCLK17_0          |OUTPUT   |LVCMOS25*  |0             |12        |SLOW     |           |         |       |LOCATED   |NO         |NONE            |
|P133      |BRDSEL_J2<8>      |IOB      |IO_L34N_GCLK18_0          |OUTPUT   |LVCMOS25*  |0             |12        |SLOW     |           |         |       |LOCATED   |NO         |NONE            |
|P134      |BRDSEL_J2<7>      |IOB      |IO_L34P_GCLK19_0          |OUTPUT   |LVCMOS25*  |0             |12        |SLOW     |           |         |       |LOCATED   |NO         |NONE            |
|P135      |                  |         |VCCO_0                    |         |           |0             |          |         |           |         |2.50   |          |           |                |
|P136      |                  |         |GND                       |         |           |              |          |         |           |         |       |          |           |                |
|P137      |BRDSEL_J2<6>      |IOB      |IO_L4N_0                  |OUTPUT   |LVCMOS25*  |0             |12        |SLOW     |           |         |       |LOCATED   |NO         |NONE            |
|P138      |DOUT_J2<7>        |IOB      |IO_L4P_0                  |BIDIR    |LVCMOS25*  |0             |12        |SLOW     |           |NONE     |       |LOCATED   |NO         |NONE            |
|P139      |BRDSEL_J2<4>      |IOB      |IO_L3N_0                  |OUTPUT   |LVCMOS25*  |0             |12        |SLOW     |           |         |       |LOCATED   |NO         |NONE            |
|P140      |BRDSEL_J2<5>      |IOB      |IO_L3P_0                  |OUTPUT   |LVCMOS25*  |0             |12        |SLOW     |           |         |       |LOCATED   |NO         |NONE            |
|P141      |BRDSEL_J2<2>      |IOB      |IO_L2N_0                  |OUTPUT   |LVCMOS25*  |0             |12        |SLOW     |           |         |       |LOCATED   |NO         |NONE            |
|P142      |BRDSEL_J2<1>      |IOB      |IO_L2P_0                  |OUTPUT   |LVCMOS25*  |0             |12        |SLOW     |           |         |       |LOCATED   |NO         |NONE            |
|P143      |BRDSEL_J2<0>      |IOB      |IO_L1N_VREF_0             |OUTPUT   |LVCMOS25*  |0             |12        |SLOW     |           |         |       |LOCATED   |NO         |NONE            |
|P144      |BRDSEL_J2<3>      |IOB      |IO_L1P_HSWAPEN_0          |OUTPUT   |LVCMOS25*  |0             |12        |SLOW     |           |         |       |LOCATED   |NO         |NONE            |
+--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+

* Default value.
** This default Pullup/Pulldown value can be overridden in Bitgen. 
****** Special VCCO requirements may apply. Please consult the device 
       family datasheet for specific guideline on VCCO requirements. 


