14/3/05
18:13
MC serial number  351033903000022

2
Position 0	ROB serial number  F0276

Position 1	ROB serial number  F0801

Position 2	ROB serial number  F0574

Position 3	ROB serial number  F0711

Position 4	ROB serial number  F0554

Position 5	ROB serial number  F0581

Position 6	ROB serial number  F0337



ON ROB 0


ON ROB 1


ON ROB 2


ON ROB 3


ON ROB 4


ON ROB 5


ON ROB 6
Retardo 99



































FLTB no parpadea al hacer el corto
FLTB no parpadea al hacer el corto
FLTB no parpadea al hacer el corto
FLTB no parpadea al hacer el corto
FLTB no parpadea al hacer el corto
FLTB no parpadea al hacer el corto
FLTB no parpadea al hacer el corto
*****************************
*****************************
MC CONFIGURATION
*****************************
*****************************

ROB 0

TDC nº: 0
ROB 0 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 0 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 0 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 0 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 1

TDC nº: 0
ROB 1 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 1 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 1 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 1 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 2

TDC nº: 0
ROB 2 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 2 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 2 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 2 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 3

TDC nº: 0
ROB 3 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 3 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 3 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 3 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 4

TDC nº: 0
ROB 4 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 4 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 4 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 4 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 5

TDC nº: 0
ROB 5 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 5 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 5 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 5 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 6

TDC nº: 0
ROB 6 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 6 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 6 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 6 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



*****************************
*****************************
SEQUENCE PATGEN
*****************************
*****************************



RUN 0
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 3
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE



RUN 1
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 3
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE



RUN 2
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 3
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE



*****************************
*****************************
SEQUENCE TDC
*****************************
*****************************



RUN 0
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 3
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE


*****************************
*****************************
MC CONFIGURATION
*****************************
*****************************

ROB 0

TDC nº: 0
ROB 0 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 0 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 0 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 0 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 1

TDC nº: 0
ROB 1 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 1 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 1 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 1 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 2

TDC nº: 0
ROB 2 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 2 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 2 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 2 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 3

TDC nº: 0
ROB 3 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 3 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 3 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 3 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 4

TDC nº: 0
ROB 4 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 4 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 4 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 4 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 5

TDC nº: 0
ROB 5 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 5 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 5 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 5 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 6

TDC nº: 0
ROB 6 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 6 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 6 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 6 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



*****************************
*****************************
BUNCH RESET TEST
*****************************
*****************************



RUN 0
***********
ROS channel 0
Faltan canales?:  FALSE



ROS channel 1
Faltan canales?:  FALSE



ROS channel 2
Faltan canales?:  FALSE



ROS channel 3
Faltan canales?:  FALSE



ROS channel 4
Faltan canales?:  FALSE



ROS channel 5
Faltan canales?:  FALSE



ROS channel 6
Faltan canales?:  FALSE




*****************************
*****************************
EVENT RESET TEST
*****************************
*****************************



RUN 0
***********
ROS channel 0
Faltan canales?:  FALSE



ROS channel 1
Faltan canales?:  FALSE



ROS channel 2
Faltan canales?:  FALSE



ROS channel 3
Faltan canales?:  FALSE



ROS channel 4
Faltan canales?:  FALSE



ROS channel 5
Faltan canales?:  FALSE



ROS channel 6
Faltan canales?:  FALSE




RUN 1
***********
ROS channel 0
Faltan canales?:  FALSE



ROS channel 1
Faltan canales?:  FALSE



ROS channel 2
Faltan canales?:  FALSE



ROS channel 3
Faltan canales?:  FALSE



ROS channel 4
Faltan canales?:  FALSE



ROS channel 5
Faltan canales?:  FALSE



ROS channel 6
Faltan canales?:  FALSE




RUN 2
***********
ROS channel 0
Faltan canales?:  FALSE



ROS channel 1
Faltan canales?:  FALSE



ROS channel 2
Faltan canales?:  FALSE



ROS channel 3
Faltan canales?:  FALSE



ROS channel 4
Faltan canales?:  FALSE



ROS channel 5
Faltan canales?:  FALSE



ROS channel 6
Faltan canales?:  FALSE




*****************************
*****************************
ADQ ALL CHANNELS
*****************************
*****************************



RUN 0
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 3
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE



RUN 1
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 3
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE



RUN 2
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 3
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE



RUN 3
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 3
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE



*****************************
*****************************
TEST PULSE
*****************************
*****************************



RUN 0
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 3
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE



*****************************
*****************************
TEST ROLINK
*****************************
*****************************



RUN 0
***********
ROS channel 0


ROS channel 1
No hay ningún dato de tiempo


ROS channel 2
No hay ningún dato de tiempo


ROS channel 3
No hay ningún dato de tiempo


ROS channel 4
No hay ningún dato de tiempo


ROS channel 5
No hay ningún dato de tiempo


ROS channel 6
No hay ningún dato de tiempo



RUN 1
***********
ROS channel 0
No hay ningún dato de tiempo


ROS channel 1


ROS channel 2
No hay ningún dato de tiempo


ROS channel 3
No hay ningún dato de tiempo


ROS channel 4
No hay ningún dato de tiempo


ROS channel 5
No hay ningún dato de tiempo


ROS channel 6
No hay ningún dato de tiempo



RUN 2
***********
ROS channel 0
No hay ningún dato de tiempo


ROS channel 1
No hay ningún dato de tiempo


ROS channel 2


ROS channel 3
No hay ningún dato de tiempo


ROS channel 4
No hay ningún dato de tiempo


ROS channel 5
No hay ningún dato de tiempo


ROS channel 6
No hay ningún dato de tiempo



RUN 3
***********
ROS channel 0
No hay ningún dato de tiempo


ROS channel 1
No hay ningún dato de tiempo


ROS channel 2
No hay ningún dato de tiempo


ROS channel 3


ROS channel 4
No hay ningún dato de tiempo


ROS channel 5
No hay ningún dato de tiempo


ROS channel 6
No hay ningún dato de tiempo



RUN 4
***********
ROS channel 0
No hay ningún dato de tiempo


ROS channel 1
No hay ningún dato de tiempo


ROS channel 2
No hay ningún dato de tiempo


ROS channel 3
No hay ningún dato de tiempo


ROS channel 4


ROS channel 5
No hay ningún dato de tiempo


ROS channel 6
No hay ningún dato de tiempo



RUN 5
***********
ROS channel 0
No hay ningún dato de tiempo


ROS channel 1
No hay ningún dato de tiempo


ROS channel 2
No hay ningún dato de tiempo


ROS channel 3
No hay ningún dato de tiempo


ROS channel 4
No hay ningún dato de tiempo


ROS channel 5


ROS channel 6
No hay ningún dato de tiempo



RUN 6
***********
ROS channel 0
No hay ningún dato de tiempo


ROS channel 1
No hay ningún dato de tiempo


ROS channel 2
No hay ningún dato de tiempo


ROS channel 3
No hay ningún dato de tiempo


ROS channel 4
No hay ningún dato de tiempo


ROS channel 5
No hay ningún dato de tiempo


ROS channel 6



RUN 7
***********
ROS channel 0
No hay ningún dato de tiempo


ROS channel 1
No hay ningún dato de tiempo


ROS channel 2
No hay ningún dato de tiempo


ROS channel 3
No hay ningún dato de tiempo


ROS channel 4
No hay ningún dato de tiempo


ROS channel 5
No hay ningún dato de tiempo


ROS channel 6
No hay ningún dato de tiempo



