12/11/04
11:35
MC serial number  351033901000024

MB1
Position 0	ROB serial number  361
Position 1	ROB serial number  F0640

Position 2	ROB serial number  F0678

Position 3	ROB serial number  G0069

Position 4	ROB serial number  F0638

Position 5	ROB serial number  386


ON ROB 0


ON ROB 1


ON ROB 2


ON ROB 3


ON ROB 4


ON ROB 5
Retardo 90






























FLTB no parpadea al hacer el corto
FLTB no parpadea al hacer el corto
FLTB no parpadea al hacer el corto
FLTB no parpadea al hacer el corto
FLTB no parpadea al hacer el corto
FLTB no parpadea al hacer el corto
*****************************
*****************************
MC CONFIGURATION
*****************************
*****************************

ROB 0

TDC nº: 0
ROB 0 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 0 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 0 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 0 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 1

TDC nº: 0
ROB 1 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 1 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 1 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 1 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 2

TDC nº: 0
ROB 2 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 2 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 2 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 2 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 3

TDC nº: 0
ROB 3 TDC 0
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 4

TDC nº: 0
ROB 4 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 4 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 4 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 4 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 5

TDC nº: 0
ROB 5 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 5 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 5 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 5 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ERROR I FUERA RANGO (0,6;1,2)   I = 0,396790  ROB 3
*****************************
*****************************
SEQUENCE PATGEN
*****************************
*****************************



RUN 0
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE



RUN 1
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE



RUN 2
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE




RUN 0
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE


*****************************
*****************************
MC CONFIGURATION
*****************************
*****************************

ROB 0

TDC nº: 0
ROB 0 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 0 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 0 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 0 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 1

TDC nº: 0
ROB 1 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 1 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 1 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 1 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 2

TDC nº: 0
ROB 2 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 2 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 2 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 2 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 3

TDC nº: 0
ROB 3 TDC 0
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

ROBERROR a 1  con ROB 3


ROB 4

TDC nº: 0
ROB 4 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 4 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 4 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 4 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 5

TDC nº: 0
ROB 5 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 5 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 5 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 5 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



*****************************
*****************************
BUNCH RESET TEST
*****************************
*****************************



RUN 0
***********
ROS channel 0
Faltan canales?:  FALSE



ROS channel 1
Faltan canales?:  FALSE



ROS channel 2
Faltan canales?:  FALSE



ROS channel 4
Faltan canales?:  FALSE



ROS channel 5
Faltan canales?:  FALSE



ROS channel 6
Faltan canales?:  FALSE




*****************************
*****************************
EVENT RESET TEST
*****************************
*****************************



RUN 0
***********
ROS channel 0
Faltan canales?:  FALSE



ROS channel 1
Faltan canales?:  FALSE



ROS channel 2
Faltan canales?:  FALSE



ROS channel 4
Faltan canales?:  FALSE



ROS channel 5
Faltan canales?:  FALSE



ROS channel 6
Faltan canales?:  FALSE




RUN 1
***********
ROS channel 0
Faltan canales?:  FALSE



ROS channel 1
Faltan canales?:  FALSE



ROS channel 2
Faltan canales?:  FALSE



ROS channel 4
Faltan canales?:  FALSE



ROS channel 5
Faltan canales?:  FALSE



ROS channel 6
Faltan canales?:  FALSE




RUN 2
***********
ROS channel 0
Faltan canales?:  FALSE



ROS channel 1
Faltan canales?:  FALSE



ROS channel 2
Faltan canales?:  FALSE



ROS channel 4
Faltan canales?:  FALSE



ROS channel 5
Faltan canales?:  FALSE



ROS channel 6
Faltan canales?:  FALSE




*****************************
*****************************
ADQ ALL CHANNELS
*****************************
*****************************



RUN 0
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE



RUN 1
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE



RUN 2
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE



RUN 3
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE



*****************************
*****************************
TEST PULSE
*****************************
*****************************



RUN 0
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE



*****************************
*****************************
TEST ROLINK
*****************************
*****************************



RUN 0
***********
ROS channel 0


ROS channel 1
No hay ningún dato de tiempo


ROS channel 2
No hay ningún dato de tiempo


ROS channel 4
No hay ningún dato de tiempo


ROS channel 5
No hay ningún dato de tiempo


ROS channel 6
No hay ningún dato de tiempo



RUN 1
***********
ROS channel 0
No hay ningún dato de tiempo


ROS channel 1


ROS channel 2
No hay ningún dato de tiempo


ROS channel 4
No hay ningún dato de tiempo


ROS channel 5
No hay ningún dato de tiempo


ROS channel 6
No hay ningún dato de tiempo



RUN 2
***********
ROS channel 0
No hay ningún dato de tiempo


ROS channel 1
No hay ningún dato de tiempo


ROS channel 2


ROS channel 4
No hay ningún dato de tiempo


ROS channel 5
No hay ningún dato de tiempo


ROS channel 6
No hay ningún dato de tiempo



RUN 3
***********
ROS channel 0
No hay ningún dato de tiempo


ROS channel 1
No hay ningún dato de tiempo


ROS channel 2
No hay ningún dato de tiempo


ROS channel 4


ROS channel 5
No hay ningún dato de tiempo


ROS channel 6
No hay ningún dato de tiempo



RUN 4
***********
ROS channel 0
No hay ningún dato de tiempo


ROS channel 1
No hay ningún dato de tiempo


ROS channel 2
No hay ningún dato de tiempo


ROS channel 4
No hay ningún dato de tiempo


ROS channel 5


ROS channel 6
No hay ningún dato de tiempo



RUN 5
***********
ROS channel 0
No hay ningún dato de tiempo


ROS channel 1
No hay ningún dato de tiempo


ROS channel 2
No hay ningún dato de tiempo


ROS channel 4
No hay ningún dato de tiempo


ROS channel 5
No hay ningún dato de tiempo


ROS channel 6



RUN 6
***********
ROS channel 0
No hay ningún dato de tiempo


ROS channel 1
No hay ningún dato de tiempo


ROS channel 2
No hay ningún dato de tiempo


ROS channel 4
No hay ningún dato de tiempo


ROS channel 5
No hay ningún dato de tiempo


ROS channel 6
No hay ningún dato de tiempo



RUN 7
***********
ROS channel 0
No hay ningún dato de tiempo


ROS channel 1
No hay ningún dato de tiempo


ROS channel 2
No hay ningún dato de tiempo


ROS channel 4
No hay ningún dato de tiempo


ROS channel 5
No hay ningún dato de tiempo


ROS channel 6
No hay ningún dato de tiempo



