22/11/04
11:02
MC serial number  351033901100001

MB1
Position 0	ROB serial number  F0365

Position 1	ROB serial number  F0656

Position 2	ROB serial number  F0669

Position 3	ROB serial number  G0020

Position 4	ROB serial number  F0701

Position 5	ROB serial number  F0407



ON ROB 0


ON ROB 1


ON ROB 2


ON ROB 3


ON ROB 4


ON ROB 5
Retardo 90






























FLTB no parpadea al hacer el corto
FLTB no parpadea al hacer el corto
FLTB no parpadea al hacer el corto
FLTB no parpadea al hacer el corto
FLTB no parpadea al hacer el corto
FLTB no parpadea al hacer el corto
*****************************
*****************************
MC CONFIGURATION
*****************************
*****************************

ROB 0

TDC nº: 0
ROB 0 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 0 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 0 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 0 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 1

TDC nº: 0
ROB 1 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 1 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 1 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 1 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 2

TDC nº: 0
ROB 2 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 2 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 2 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 2 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 3

TDC nº: 0
ROB 3 TDC 0
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 4

TDC nº: 0
ROB 4 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 4 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 4 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 4 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 5

TDC nº: 0
ROB 5 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 5 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 5 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 5 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



*****************************
*****************************
SEQUENCE PATGEN
*****************************
*****************************



RUN 0
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE



RUN 1
***********
ROS channel 0
Faltan canales?:  FALSE
ERROR Event ID
Ev init  127
Ev0 matriz 128
Ev1 matriz 129


ROS channel 1
Faltan canales?:  FALSE
ERROR Event ID
Ev init  127
Ev0 matriz 128
Ev1 matriz 129


ROS channel 2
Faltan canales?:  FALSE
ERROR Event ID
Ev init  127
Ev0 matriz 128
Ev1 matriz 129


ROS channel 4
Faltan canales?:  FALSE
ERROR Event ID
Ev init  127
Ev0 matriz 128
Ev1 matriz 129


ROS channel 5
Faltan canales?:  FALSE
ERROR Event ID
Ev init  127
Ev0 matriz 128
Ev1 matriz 129


ROS channel 6
Faltan canales?:  FALSE
ERROR Event ID
Ev init  127
Ev0 matriz 128
Ev1 matriz 129



RUN 2
***********
ROS channel 0
Faltan canales?:  FALSE
ERROR Event ID
Ev init  255
Ev0 matriz 256
Ev1 matriz 257


ROS channel 1
Faltan canales?:  FALSE
ERROR Event ID
Ev init  255
Ev0 matriz 256
Ev1 matriz 257


ROS channel 2
Faltan canales?:  FALSE
ERROR Event ID
Ev init  255
Ev0 matriz 256
Ev1 matriz 257


ROS channel 4
Faltan canales?:  FALSE
ERROR Event ID
Ev init  255
Ev0 matriz 256
Ev1 matriz 257


ROS channel 5
Faltan canales?:  FALSE
ERROR Event ID
Ev init  255
Ev0 matriz 256
Ev1 matriz 257


ROS channel 6
Faltan canales?:  FALSE
ERROR Event ID
Ev init  255
Ev0 matriz 256
Ev1 matriz 257




RUN 0
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE


*****************************
*****************************
MC CONFIGURATION
*****************************
*****************************

ROB 0

TDC nº: 0
ROB 0 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 0 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 0 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 0 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 1

TDC nº: 0
ROB 1 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 1 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 1 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 1 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 2

TDC nº: 0
ROB 2 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 2 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 2 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 2 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 3

TDC nº: 0
ROB 3 TDC 0
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

ROBERROR a 1  con ROB 3


ROB 4

TDC nº: 0
ROB 4 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 4 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 4 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 4 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 5

TDC nº: 0
ROB 5 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 5 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 5 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 5 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



*****************************
*****************************
BUNCH RESET TEST
*****************************
*****************************



RUN 0
***********
ROS channel 0
Faltan canales?:  FALSE



ROS channel 1
Faltan canales?:  FALSE



ROS channel 2
Faltan canales?:  FALSE



ROS channel 4
Faltan canales?:  FALSE



ROS channel 5
Faltan canales?:  FALSE



ROS channel 6
Faltan canales?:  FALSE




*****************************
*****************************
EVENT RESET TEST
*****************************
*****************************



RUN 0
***********
ROS channel 0
Faltan canales?:  FALSE



ROS channel 1
Faltan canales?:  FALSE



ROS channel 2
Faltan canales?:  FALSE



ROS channel 4
Faltan canales?:  FALSE



ROS channel 5
Faltan canales?:  FALSE



ROS channel 6
Faltan canales?:  FALSE




RUN 1
***********
ROS channel 0
Faltan canales?:  FALSE



ROS channel 1
Faltan canales?:  FALSE



ROS channel 2
Faltan canales?:  FALSE



ROS channel 4
Faltan canales?:  FALSE



ROS channel 5
Faltan canales?:  FALSE



ROS channel 6
Faltan canales?:  FALSE




RUN 2
***********
ROS channel 0
Faltan canales?:  FALSE



ROS channel 1
Faltan canales?:  FALSE



ROS channel 2
Faltan canales?:  FALSE



ROS channel 4
Faltan canales?:  FALSE



ROS channel 5
Faltan canales?:  FALSE



ROS channel 6
Faltan canales?:  FALSE




*****************************
*****************************
ADQ ALL CHANNELS
*****************************
*****************************



RUN 0
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE



RUN 1
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE



RUN 2
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE



RUN 3
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE



*****************************
*****************************
TEST PULSE
*****************************
*****************************



RUN 0
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE



*****************************
*****************************
TEST ROLINK
*****************************
*****************************



RUN 0
***********
ROS channel 0


ROS channel 1
No hay ningún dato de tiempo


ROS channel 2
No hay ningún dato de tiempo


ROS channel 4
No hay ningún dato de tiempo


ROS channel 5
No hay ningún dato de tiempo


ROS channel 6
No hay ningún dato de tiempo



RUN 1
***********
ROS channel 0
No hay ningún dato de tiempo


ROS channel 1


ROS channel 2
No hay ningún dato de tiempo


ROS channel 4
No hay ningún dato de tiempo


ROS channel 5
No hay ningún dato de tiempo


ROS channel 6
No hay ningún dato de tiempo



RUN 2
***********
ROS channel 0
No hay ningún dato de tiempo


ROS channel 1
No hay ningún dato de tiempo


ROS channel 2


ROS channel 4
No hay ningún dato de tiempo


ROS channel 5
No hay ningún dato de tiempo


ROS channel 6
No hay ningún dato de tiempo



RUN 3
***********
ROS channel 0
No hay ningún dato de tiempo


ROS channel 1
No hay ningún dato de tiempo


ROS channel 2
No hay ningún dato de tiempo


ROS channel 4


ROS channel 5
No hay ningún dato de tiempo


ROS channel 6
No hay ningún dato de tiempo



RUN 4
***********
ROS channel 0
No hay ningún dato de tiempo


ROS channel 1
No hay ningún dato de tiempo


ROS channel 2
No hay ningún dato de tiempo


ROS channel 4
No hay ningún dato de tiempo


ROS channel 5


ROS channel 6
No hay ningún dato de tiempo



RUN 5
***********
ROS channel 0
No hay ningún dato de tiempo


ROS channel 1
No hay ningún dato de tiempo


ROS channel 2
No hay ningún dato de tiempo


ROS channel 4
No hay ningún dato de tiempo


ROS channel 5
No hay ningún dato de tiempo


ROS channel 6



RUN 6
***********
ROS channel 0
No hay ningún dato de tiempo


ROS channel 1
No hay ningún dato de tiempo


ROS channel 2
No hay ningún dato de tiempo


ROS channel 4
No hay ningún dato de tiempo


ROS channel 5
No hay ningún dato de tiempo


ROS channel 6
No hay ningún dato de tiempo



RUN 7
***********
ROS channel 0
No hay ningún dato de tiempo


ROS channel 1
No hay ningún dato de tiempo


ROS channel 2
No hay ningún dato de tiempo


ROS channel 4
No hay ningún dato de tiempo


ROS channel 5
No hay ningún dato de tiempo


ROS channel 6
No hay ningún dato de tiempo



