12/7/05
19:34
MC serial number  351033902100005

1
Position 0	ROB serial number  F0467

Position 1	ROB serial number  F1149

Position 2	ROB serial number  F1046

Position 3	ROB serial number  F1146

Position 4	ROB serial number  F1184

Position 5	ROB serial number  F0405



ON ROB 0


ON ROB 1


ON ROB 2


ON ROB 3


ON ROB 4


ON ROB 5
Retardo 99
OK reloj TRB, se apaga correctamente

OK RPC - Alingment connectors































FLTB no parpadea al hacer el corto
FLTB no parpadea al hacer el corto
FLTB no parpadea al hacer el corto
FLTB no parpadea al hacer el corto
FLTB no parpadea al hacer el corto
FLTB no parpadea al hacer el corto
*****************************
*****************************
MC CONFIGURATION
*****************************
*****************************

ROB 0

TDC nº: 0
ROB 0 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 0 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 0 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 0 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 1

TDC nº: 0
ROB 1 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 1 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 1 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 1 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 2

TDC nº: 0
ROB 2 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 2 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 2 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 2 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 3

TDC nº: 0
ROB 3 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 3 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 3 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 3 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 4

TDC nº: 0
ROB 4 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 4 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 4 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 4 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 5

TDC nº: 0
ROB 5 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 5 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 5 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 5 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



*****************************
*****************************
SEQUENCE PATGEN
*****************************
*****************************



RUN 0
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE



RUN 1
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE



RUN 2
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE



*****************************
*****************************
SEQUENCE TDC
*****************************
*****************************



RUN 0
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE


*****************************
*****************************
MC CONFIGURATION
*****************************
*****************************

ROB 0

TDC nº: 0
ROB 0 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 0 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 0 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 0 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 1

TDC nº: 0
ROB 1 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 1 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 1 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 1 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 2

TDC nº: 0
ROB 2 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 2 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 2 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 2 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 3

TDC nº: 0
ROB 3 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 3 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 3 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 3 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 4

TDC nº: 0
ROB 4 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 4 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 4 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 4 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 5

TDC nº: 0
ROB 5 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 5 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 5 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 5 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



*****************************
*****************************
BUNCH RESET TEST
*****************************
*****************************



RUN 0
***********
ROS channel 0
Faltan canales?:  FALSE



ROS channel 1
Faltan canales?:  FALSE



ROS channel 2
Faltan canales?:  FALSE



ROS channel 4
Faltan canales?:  FALSE



ROS channel 5
Faltan canales?:  FALSE



ROS channel 6
Faltan canales?:  FALSE




*****************************
*****************************
EVENT RESET TEST
*****************************
*****************************



RUN 0
***********
ROS channel 0
Faltan canales?:  FALSE



ROS channel 1
Faltan canales?:  FALSE



ROS channel 2
Faltan canales?:  FALSE



ROS channel 4
Faltan canales?:  FALSE



ROS channel 5
Faltan canales?:  FALSE



ROS channel 6
Faltan canales?:  FALSE




RUN 1
***********
ROS channel 0
Faltan canales?:  FALSE



ROS channel 1
Faltan canales?:  FALSE



ROS channel 2
Faltan canales?:  FALSE



ROS channel 4
Faltan canales?:  FALSE



ROS channel 5
Faltan canales?:  FALSE



ROS channel 6
Faltan canales?:  FALSE




RUN 2
***********
ROS channel 0
Faltan canales?:  FALSE



ROS channel 1
Faltan canales?:  FALSE



ROS channel 2
Faltan canales?:  FALSE



ROS channel 4
Faltan canales?:  FALSE



ROS channel 5
Faltan canales?:  FALSE



ROS channel 6
Faltan canales?:  FALSE




*****************************
*****************************
ADQ ALL CHANNELS
*****************************
*****************************



RUN 0
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE



RUN 1
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE



RUN 2
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE



RUN 3
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE



*****************************
*****************************
TEST PULSE
*****************************
*****************************



RUN 0
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE



*****************************
*****************************
TEST ROLINK
*****************************
*****************************



RUN 0
***********
ROS channel 0


ROS channel 1
No hay ningún dato de tiempo


ROS channel 2
No hay ningún dato de tiempo


ROS channel 4
No hay ningún dato de tiempo


ROS channel 5
No hay ningún dato de tiempo


ROS channel 6
No hay ningún dato de tiempo



RUN 1
***********
ROS channel 0
No hay ningún dato de tiempo


ROS channel 1


ROS channel 2
No hay ningún dato de tiempo


ROS channel 4
No hay ningún dato de tiempo


ROS channel 5
No hay ningún dato de tiempo


ROS channel 6
No hay ningún dato de tiempo



RUN 2
***********
ROS channel 0
No hay ningún dato de tiempo


ROS channel 1
No hay ningún dato de tiempo


ROS channel 2


ROS channel 4
No hay ningún dato de tiempo


ROS channel 5
No hay ningún dato de tiempo


ROS channel 6
No hay ningún dato de tiempo



RUN 3
***********
ROS channel 0
No hay ningún dato de tiempo


ROS channel 1
No hay ningún dato de tiempo


ROS channel 2
No hay ningún dato de tiempo


ROS channel 4


ROS channel 5
No hay ningún dato de tiempo


ROS channel 6
No hay ningún dato de tiempo



RUN 4
***********
ROS channel 0
No hay ningún dato de tiempo


ROS channel 1
No hay ningún dato de tiempo


ROS channel 2
No hay ningún dato de tiempo


ROS channel 4
No hay ningún dato de tiempo


ROS channel 5


ROS channel 6
No hay ningún dato de tiempo



RUN 5
***********
ROS channel 0
No hay ningún dato de tiempo


ROS channel 1
No hay ningún dato de tiempo


ROS channel 2
No hay ningún dato de tiempo


ROS channel 4
No hay ningún dato de tiempo


ROS channel 5
No hay ningún dato de tiempo


ROS channel 6



RUN 6
***********
ROS channel 0
No hay ningún dato de tiempo


ROS channel 1
No hay ningún dato de tiempo


ROS channel 2
No hay ningún dato de tiempo


ROS channel 4
No hay ningún dato de tiempo


ROS channel 5
No hay ningún dato de tiempo


ROS channel 6
No hay ningún dato de tiempo



RUN 7
***********
ROS channel 0
No hay ningún dato de tiempo


ROS channel 1
No hay ningún dato de tiempo


ROS channel 2
No hay ningún dato de tiempo


ROS channel 4
No hay ningún dato de tiempo


ROS channel 5
No hay ningún dato de tiempo


ROS channel 6
No hay ningún dato de tiempo



