12/7/05
10:19
MC serial number  351033902100008

1
Position 0	ROB serial number  F0466

Position 1	ROB serial number  F1185

Position 2	ROB serial number  F1064

Position 3	ROB serial number  F1070

Position 4	ROB serial number  F1066

Position 5	ROB serial number  F1173



ON ROB 0


ON ROB 1


ON ROB 2


ON ROB 3


ON ROB 4


ON ROB 5
Retardo 99
OK reloj TRB, se apaga correctamente

OK RPC - Alingment connectors

*****************************
*****************************
MC CONFIGURATION
*****************************
*****************************

ROB 0

TDC nº: 0
ROB 0 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 0 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 0 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 0 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 1

TDC nº: 0
ROB 1 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 1 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 1 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 1 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 2

TDC nº: 0
ROB 2 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 2 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 2 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 2 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 3

TDC nº: 0
ROB 3 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 3 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 3 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 3 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 4

TDC nº: 0
ROB 4 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 4 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 4 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 4 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 5

TDC nº: 0
ROB 5 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 5 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 5 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 5 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



*****************************
*****************************
SEQUENCE PATGEN
*****************************
*****************************



RUN 0
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE



RUN 1
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE



RUN 2
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE



*****************************
*****************************
SEQUENCE TDC
*****************************
*****************************



RUN 0
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE


*****************************
*****************************
MC CONFIGURATION
*****************************
*****************************

ROB 0

TDC nº: 0
ROB 0 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 0 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 0 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 0 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 1

TDC nº: 0
ROB 1 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 1 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 1 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 1 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 2

TDC nº: 0
ROB 2 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 2 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 2 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 2 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 3

TDC nº: 0
ROB 3 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 3 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 3 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 3 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 4

TDC nº: 0
ROB 4 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 4 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 4 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 4 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



ROB 5

TDC nº: 0
ROB 5 TDC 0
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 1
ROB 5 TDC 1
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 2
ROB 5 TDC 2
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nº: 3
ROB 5 TDC 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock

LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   



*****************************
*****************************
BUNCH RESET TEST
*****************************
*****************************



RUN 0
***********
ROS channel 0
Faltan canales?:  FALSE



ROS channel 1
Faltan canales?:  FALSE



ROS channel 2
Faltan canales?:  FALSE



ROS channel 4
Faltan canales?:  FALSE



ROS channel 5
Faltan canales?:  FALSE



ROS channel 6
Faltan canales?:  FALSE




*****************************
*****************************
EVENT RESET TEST
*****************************
*****************************



RUN 0
***********
ROS channel 0
Faltan canales?:  FALSE



ROS channel 1
Faltan canales?:  FALSE



ROS channel 2
Faltan canales?:  FALSE



ROS channel 4
Faltan canales?:  FALSE



ROS channel 5
Faltan canales?:  FALSE



ROS channel 6
Faltan canales?:  FALSE




RUN 1
***********
ROS channel 0
Faltan canales?:  FALSE



ROS channel 1
Faltan canales?:  FALSE



ROS channel 2
Faltan canales?:  FALSE



ROS channel 4
Faltan canales?:  FALSE



ROS channel 5
Faltan canales?:  FALSE



ROS channel 6
Faltan canales?:  FALSE




RUN 2
***********
ROS channel 0
Faltan canales?:  FALSE



ROS channel 1
Faltan canales?:  FALSE



ROS channel 2
Faltan canales?:  FALSE



ROS channel 4
Faltan canales?:  FALSE



ROS channel 5
Faltan canales?:  FALSE



ROS channel 6
Faltan canales?:  FALSE




*****************************
*****************************
ADQ ALL CHANNELS
*****************************
*****************************



RUN 0
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE



RUN 1
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE



RUN 2
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE



RUN 3
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE



*****************************
*****************************
TEST PULSE
*****************************
*****************************



RUN 0
***********
ROS channel 0
Faltan canales?:  FALSE


ROS channel 1
Faltan canales?:  FALSE


ROS channel 2
Faltan canales?:  FALSE


ROS channel 4
Faltan canales?:  FALSE


ROS channel 5
Faltan canales?:  FALSE


ROS channel 6
Faltan canales?:  FALSE



*****************************
*****************************
TEST ROLINK
*****************************
*****************************



RUN 0
***********
ROS channel 0


ROS channel 1
No hay ningún dato de tiempo


ROS channel 2
No hay ningún dato de tiempo


ROS channel 4
No hay ningún dato de tiempo


ROS channel 5
No hay ningún dato de tiempo


ROS channel 6
No hay ningún dato de tiempo



RUN 1
***********
ROS channel 0
No hay ningún dato de tiempo


ROS channel 1


ROS channel 2
No hay ningún dato de tiempo


ROS channel 4
No hay ningún dato de tiempo


ROS channel 5
No hay ningún dato de tiempo


ROS channel 6
No hay ningún dato de tiempo



RUN 2
***********
ROS channel 0
No hay ningún dato de tiempo


ROS channel 1
No hay ningún dato de tiempo


ROS channel 2


ROS channel 4
No hay ningún dato de tiempo


ROS channel 5
No hay ningún dato de tiempo


ROS channel 6
No hay ningún dato de tiempo



RUN 3
***********
ROS channel 0
No hay ningún dato de tiempo


ROS channel 1
No hay ningún dato de tiempo


ROS channel 2
No hay ningún dato de tiempo


ROS channel 4


ROS channel 5
No hay ningún dato de tiempo


ROS channel 6
No hay ningún dato de tiempo



RUN 4
***********
ROS channel 0
No hay ningún dato de tiempo


ROS channel 1
No hay ningún dato de tiempo


ROS channel 2
No hay ningún dato de tiempo


ROS channel 4
No hay ningún dato de tiempo


ROS channel 5


ROS channel 6
No hay ningún dato de tiempo



RUN 5
***********
ROS channel 0
No hay ningún dato de tiempo


ROS channel 1
No hay ningún dato de tiempo


ROS channel 2
No hay ningún dato de tiempo


ROS channel 4
No hay ningún dato de tiempo


ROS channel 5
No hay ningún dato de tiempo


ROS channel 6



RUN 6
***********
ROS channel 0
No hay ningún dato de tiempo


ROS channel 1
No hay ningún dato de tiempo


ROS channel 2
No hay ningún dato de tiempo


ROS channel 4
No hay ningún dato de tiempo


ROS channel 5
No hay ningún dato de tiempo


ROS channel 6
No hay ningún dato de tiempo



RUN 7
***********
ROS channel 0
No hay ningún dato de tiempo


ROS channel 1
No hay ningún dato de tiempo


ROS channel 2
No hay ningún dato de tiempo


ROS channel 4
No hay ningún dato de tiempo


ROS channel 5
No hay ningún dato de tiempo


ROS channel 6
No hay ningún dato de tiempo



