Release 6.3i - Par G.35
Copyright (c) 1995-2004 Xilinx, Inc.  All rights reserved.

Fri Dec 04 18:06:26 2009


INPUT FILE:       ceros_map.ncd
OUTPUT FILE:      ceros_pad.txt
PART TYPE:        xc2s50e
SPEED GRADE:      -7
PACKAGE:          ft256

Pinout by Pin Number:

-----     |-----       |-----    |-----               |-----    |-----      |-----         |-----     |-----    |-----      |-----    |-----  |-----     |
Pin Number|Signal Name |Pin Usage|Pin Name            |Direction|IO Standard|IO Bank Number|Drive (mA)|Slew Rate|Termination|IOB Delay|Voltage|Constraint|
A1        |            |         |GND                 |         |           |              |          |         |           |         |       |          |
A2        |            |         |TCK                 |         |           |              |          |         |           |         |       |          |
A3        |vspare_0    |IOB      |IO_L0N_YY           |INPUT    |LVTTL      |0             |          |         |NONE**     |NONE     |       |LOCATED   |
A4        |tp<3>       |IOB      |IO_L0P_YY           |OUTPUT   |LVTTL      |0             |12        |SLOW     |NONE**     |         |       |LOCATED   |
A5        |dout<1>     |IOB      |IO_L4P_Y            |TRISTATE |LVTTL      |0             |12        |SLOW     |NONE**     |         |       |LOCATED   |
A6        |add<5>      |IOB      |IO                  |INPUT    |LVTTL      |0             |          |         |NONE**     |NONE     |       |LOCATED   |
A7        |add<4>      |IOB      |IO                  |INPUT    |LVTTL      |0             |          |         |NONE**     |NONE     |       |LOCATED   |
A8        |            |DLLIOB   |IO_LVDS_DLL_L8P     |UNUSED   |           |1             |          |         |           |         |       |          |
A9        |fout<7>     |IOB      |IO_L9N_Y            |INPUT    |LVTTL      |1             |          |         |NONE**     |NONE     |       |LOCATED   |
A10       |db<1>       |IOB      |IO_L11N_Y           |BIDIR    |LVTTL      |1             |12        |SLOW     |NONE**     |NONE     |       |LOCATED   |
A11       |fout<12>    |IOB      |IO_L13N_Y           |INPUT    |LVTTL      |1             |          |         |NONE**     |NONE     |       |LOCATED   |
A12       |lock<0>     |IOB      |IO_L16N_YY          |INPUT    |LVTTL      |1             |          |         |NONE**     |NONE     |       |LOCATED   |
A13       |            |IOB      |IO_WRITE_L18N_YY    |UNUSED   |           |1             |          |         |           |         |       |          |
A14       |            |IOB      |IO_CS_L18P_YY       |UNUSED   |           |1             |          |         |           |         |       |          |
A15       |            |         |CCLK                |         |           |              |          |         |           |         |       |          |
A16       |            |         |GND                 |         |           |              |          |         |           |         |       |          |
B1        |            |         |TMS                 |         |           |              |          |         |           |         |       |          |
B2        |            |         |GND                 |         |           |              |          |         |           |         |       |          |
B3        |cspare_0    |IOB      |IO                  |INPUT    |LVTTL      |0             |          |         |NONE**     |NONE     |       |LOCATED   |
B4        |valen       |IOB      |IO_L1P_YY           |INPUT    |LVTTL      |0             |          |         |NONE**     |NONE     |       |LOCATED   |
B5        |ef<2>       |IOB      |IO_L4N_Y            |INPUT    |LVTTL      |0             |          |         |NONE**     |NONE     |       |LOCATED   |
B6        |ef<1>       |IOB      |IO_L5P_Y            |INPUT    |LVTTL      |0             |          |         |NONE**     |NONE     |       |LOCATED   |
B7        |wclkena_p   |IOB      |IO_L6N_Y            |OUTPUT   |LVTTL      |0             |12        |SLOW     |NONE**     |         |       |LOCATED   |
B8        |            |GCLKIOB  |GCK2                |UNUSED   |           |1             |          |         |           |         |       |          |
B9        |fout<6>     |IOB      |IO_L9P_Y            |INPUT    |LVTTL      |1             |          |         |NONE**     |NONE     |       |LOCATED   |
B10       |db<0>       |IOB      |IO_L11P_Y           |BIDIR    |LVTTL      |1             |12        |SLOW     |NONE**     |NONE     |       |LOCATED   |
B11       |ren<0>      |IOB      |IO_L13P_Y           |OUTPUT   |LVTTL      |1             |12        |FAST     |NONE**     |         |       |LOCATED   |
B12       |par<0>      |IOB      |IO_L16P_YY          |INPUT    |LVTTL      |1             |          |         |NONE**     |NONE     |       |LOCATED   |
B13       |hasul<3>    |IOB      |IO_L17P_Y           |OUTPUT   |LVTTL      |1             |12        |SLOW     |NONE**     |         |       |LOCATED   |
B14       |            |         |TDO                 |         |           |              |          |         |           |         |       |          |
B15       |            |         |GND                 |         |           |              |          |         |           |         |       |          |
B16       |            |IOB      |IO_DIN_D0_L19N_YY   |UNUSED   |           |2             |          |         |           |         |       |          |
C1        |            |IOB      |IO_L83N             |UNUSED   |           |7             |          |         |           |         |       |          |
C2        |tp<0>       |IOB      |IO_L83P             |OUTPUT   |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |
C3        |            |         |VCCINT              |         |           |              |          |         |           |         |1.8    |          |
C4        |            |IOB      |IO_L1N_YY           |UNUSED   |           |0             |          |         |           |         |       |          |
C5        |ceros_id<0> |IOB      |IO_VREF_0_L2N_YY    |INPUT    |LVTTL      |0             |          |         |NONE**     |NONE     |       |LOCATED   |
C6        |ceros_id<1> |IOB      |IO_L5N_Y            |INPUT    |LVTTL      |0             |          |         |NONE**     |NONE     |       |LOCATED   |
C7        |recoff_p    |IOB      |IO_L6P_Y            |OUTPUT   |LVTTL      |0             |12        |SLOW     |NONE**     |         |       |LOCATED   |
C8        |            |GCLKIOB  |GCK3                |UNUSED   |           |0             |          |         |           |         |       |          |
C9        |fout<14>    |IOB      |IO_L10N_Y           |INPUT    |LVTTL      |1             |          |         |NONE**     |NONE     |       |LOCATED   |
C10       |fout<4>     |IOB      |IO                  |INPUT    |LVTTL      |1             |          |         |NONE**     |NONE     |       |LOCATED   |
C11       |lock<5>     |IOB      |IO_L14N_Y           |INPUT    |LVTTL      |1             |          |         |NONE**     |NONE     |       |LOCATED   |
C12       |add<3>      |IOB      |IO_L17N_Y           |INPUT    |LVTTL      |1             |          |         |NONE**     |NONE     |       |LOCATED   |
C13       |            |         |TDI                 |         |           |              |          |         |           |         |       |          |
C14       |            |         |VCCINT              |         |           |              |          |         |           |         |1.8    |          |
C15       |            |IOB      |IO_DOUT_BUSY_L19P_YY|UNUSED   |           |2             |          |         |           |         |       |          |
C16       |oe<2>       |IOB      |IO_VREF_2_L22P_Y    |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |
D1        |            |IOB      |IO_L82N_YY          |UNUSED   |           |7             |          |         |           |         |       |          |
D2        |cspare_1    |IOB      |IO_L82P_YY          |INPUT    |LVTTL      |7             |          |         |NONE**     |NONE     |       |LOCATED   |
D3        |            |IOB      |IO                  |UNUSED   |           |7             |          |         |           |         |       |          |
D4        |            |         |VCCINT              |         |           |              |          |         |           |         |1.8    |          |
D5        |txena_p     |IOB      |IO_L2P_YY           |TRISTATE |LVTTL      |0             |24        |FAST     |NONE**     |         |       |LOCATED   |
D6        |dout<12>    |IOB      |IO_L3P_Y            |TRISTATE |LVTTL      |0             |12        |SLOW     |NONE**     |         |       |LOCATED   |
D7        |ef<5>       |IOB      |IO_VREF_0_L7N_Y     |INPUT    |LVTTL      |0             |          |         |NONE**     |NONE     |       |LOCATED   |
D8        |            |DLLIOB   |IO_LVDS_DLL_L8N     |UNUSED   |           |0             |          |         |           |         |       |          |
D9        |locked_p    |IOB      |IO_VREF_1_L10P_Y    |OUTPUT   |LVTTL      |1             |12        |SLOW     |NONE**     |         |       |LOCATED   |
D10       |fout<15>    |IOB      |IO_L12N_Y           |INPUT    |LVTTL      |1             |          |         |NONE**     |NONE     |       |LOCATED   |
D11       |fout<13>    |IOB      |IO_L14P_Y           |INPUT    |LVTTL      |1             |          |         |NONE**     |NONE     |       |LOCATED   |
D12       |oe<0>       |IOB      |IO_VREF_1_L15P_YY   |OUTPUT   |LVTTL      |1             |12        |SLOW     |NONE**     |         |       |LOCATED   |
D13       |            |         |VCCINT              |         |           |              |          |         |           |         |1.8    |          |
D14       |db<15>      |IOB      |IO_L20P             |BIDIR    |LVTTL      |2             |12        |SLOW     |NONE**     |NONE     |       |LOCATED   |
D15       |hasul<5>    |IOB      |IO_L22N_Y           |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |
D16       |ren<3>      |IOB      |IO_L24P_Y           |OUTPUT   |LVTTL      |2             |12        |FAST     |NONE**     |         |       |LOCATED   |
E1        |dout<15>    |IOB      |IO_L80N             |TRISTATE |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |
E2        |            |IOB      |IO_L80P             |UNUSED   |           |7             |          |         |           |         |       |          |
E3        |            |IOB      |IO_VREF_7_L81P_Y    |UNUSED   |           |7             |          |         |           |         |       |          |
E4        |            |IOB      |IO_L81N_Y           |UNUSED   |           |7             |          |         |           |         |       |          |
E5        |            |         |VCCINT              |         |           |              |          |         |           |         |1.8    |          |
E6        |evid<1>     |IOB      |IO_L3N_Y            |INPUT    |LVTTL      |0             |          |         |NONE**     |NONE     |       |LOCATED   |
E7        |ef<0>       |IOB      |IO_L7P_Y            |INPUT    |LVTTL      |0             |          |         |NONE**     |NONE     |       |LOCATED   |
E8        |            |         |VCCO_0              |         |           |0             |          |         |           |         |3.30   |          |
E9        |            |         |VCCO_1              |         |           |1             |          |         |           |         |3.30   |          |
E10       |db<11>      |IOB      |IO_L12P_Y           |BIDIR    |LVTTL      |1             |12        |SLOW     |NONE**     |NONE     |       |LOCATED   |
E11       |par<1>      |IOB      |IO_L15N_YY          |INPUT    |LVTTL      |1             |          |         |NONE**     |NONE     |       |LOCATED   |
E12       |            |         |VCCINT              |         |           |              |          |         |           |         |1.8    |          |
E13       |hasul<0>    |IOB      |IO_L20N             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |
E14       |hasul<1>    |IOB      |IO_L23P             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |
E15       |            |IOB      |IO_D1_L24N_Y        |UNUSED   |           |2             |          |         |           |         |       |          |
E16       |oe<5>       |IOB      |IO_L26P             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |
F1        |dout<14>    |IOB      |IO_L78N_YY          |TRISTATE |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |
F2        |dout<11>    |IOB      |IO_L78P_YY          |TRISTATE |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |
F3        |            |IOB      |IO_L79N_Y           |UNUSED   |           |7             |          |         |           |         |       |          |
F4        |            |IOB      |IO_L79P_Y           |UNUSED   |           |7             |          |         |           |         |       |          |
F5        |evid<3>     |IOB      |IO_L77P             |INPUT    |LVTTL      |7             |          |         |NONE**     |NONE     |       |LOCATED   |
F6        |            |         |GND                 |         |           |              |          |         |           |         |       |          |
F7        |            |         |VCCO_0              |         |           |0             |          |         |           |         |3.30   |          |
F8        |            |         |VCCO_0              |         |           |0             |          |         |           |         |3.30   |          |
F9        |            |         |VCCO_1              |         |           |1             |          |         |           |         |3.30   |          |
F10       |            |         |VCCO_1              |         |           |1             |          |         |           |         |3.30   |          |
F11       |            |         |GND                 |         |           |              |          |         |           |         |       |          |
F12       |lock<1>     |IOB      |IO_L21P_Y           |INPUT    |LVTTL      |2             |          |         |NONE**     |NONE     |       |LOCATED   |
F13       |lock<3>     |IOB      |IO_L23N             |INPUT    |LVTTL      |2             |          |         |NONE**     |NONE     |       |LOCATED   |
F14       |            |IOB      |IO_D2_L25P_YY       |UNUSED   |           |2             |          |         |           |         |       |          |
F15       |db<12>      |IOB      |IO_L26N             |BIDIR    |LVTTL      |2             |12        |SLOW     |NONE**     |NONE     |       |LOCATED   |
F16       |hasul<4>    |IOB      |IO_VREF_2_L28P_Y    |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |
G1        |evid<9>     |IOB      |IO_L75N_Y           |INPUT    |LVTTL      |7             |          |         |NONE**     |NONE     |       |LOCATED   |
G2        |evid<2>     |IOB      |IO_VREF_7_L75P_Y    |INPUT    |LVTTL      |7             |          |         |NONE**     |NONE     |       |LOCATED   |
G3        |evid<10>    |IOB      |IO_L76P_YY          |INPUT    |LVTTL      |7             |          |         |NONE**     |NONE     |       |LOCATED   |
G4        |token       |IOB      |IO_L76N_YY          |INPUT    |LVTTL      |7             |          |         |NONE**     |NONE     |       |LOCATED   |
G5        |evid<0>     |IOB      |IO_L77N             |INPUT    |LVTTL      |7             |          |         |NONE**     |NONE     |       |LOCATED   |
G6        |            |         |VCCO_7              |         |           |7             |          |         |           |         |3.30   |          |
G7        |            |         |GND                 |         |           |              |          |         |           |         |       |          |
G8        |            |         |GND                 |         |           |              |          |         |           |         |       |          |
G9        |            |         |GND                 |         |           |              |          |         |           |         |       |          |
G10       |            |         |GND                 |         |           |              |          |         |           |         |       |          |
G11       |            |         |VCCO_2              |         |           |2             |          |         |           |         |3.30   |          |
G12       |hasul<2>    |IOB      |IO_L21N_Y           |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |
G13       |oe<3>       |IOB      |IO_L25N_YY          |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |
G14       |oe<4>       |IOB      |IO_L27P_YY          |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |
G15       |            |IOB      |IO_D3_L28N_Y        |UNUSED   |           |2             |          |         |           |         |       |          |
G16       |fout<10>    |IOB      |IO_L30P_YY          |INPUT    |LVTTL      |2             |          |         |NONE**     |NONE     |       |LOCATED   |
H1        |evid<4>     |IOB      |IO_IRDY_L73N_YY     |INPUT    |LVTTL      |7             |          |         |NONE**     |NONE     |       |LOCATED   |
H2        |ef<3>       |IOB      |IO_L73P_YY          |INPUT    |LVTTL      |7             |          |         |NONE**     |NONE     |       |LOCATED   |
H3        |evid<11>    |IOB      |IO_L74N             |INPUT    |LVTTL      |7             |          |         |NONE**     |NONE     |       |LOCATED   |
H4        |dout<0>     |IOB      |IO_L74P             |TRISTATE |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |
H5        |            |         |VCCO_7              |         |           |7             |          |         |           |         |3.30   |          |
H6        |            |         |VCCO_7              |         |           |7             |          |         |           |         |3.30   |          |
H7        |            |         |GND                 |         |           |              |          |         |           |         |       |          |
H8        |            |         |GND                 |         |           |              |          |         |           |         |       |          |
H9        |            |         |GND                 |         |           |              |          |         |           |         |       |          |
H10       |            |         |GND                 |         |           |              |          |         |           |         |       |          |
H11       |            |         |VCCO_2              |         |           |2             |          |         |           |         |3.30   |          |
H12       |            |         |VCCO_2              |         |           |2             |          |         |           |         |3.30   |          |
H13       |lock<2>     |IOB      |IO_L27N_YY          |INPUT    |LVTTL      |2             |          |         |NONE**     |NONE     |       |LOCATED   |
H14       |db<14>      |IOB      |IO_L29N             |BIDIR    |LVTTL      |2             |12        |SLOW     |NONE**     |NONE     |       |LOCATED   |
H15       |lock<4>     |IOB      |IO_L29P             |INPUT    |LVTTL      |2             |          |         |NONE**     |NONE     |       |LOCATED   |
H16       |db<13>      |IOB      |IO_IRDY_L30N_YY     |BIDIR    |LVTTL      |2             |12        |SLOW     |NONE**     |NONE     |       |LOCATED   |
J1        |evid<7>     |IOB      |IO_L71P_Y           |INPUT    |LVTTL      |6             |          |         |NONE**     |NONE     |       |LOCATED   |
J2        |evid<6>     |IOB      |IO_L72P             |INPUT    |LVTTL      |6             |          |         |NONE**     |NONE     |       |LOCATED   |
J3        |dout<5>     |IOB      |IO_L72N             |TRISTATE |LVTTL      |6             |12        |SLOW     |NONE**     |         |       |LOCATED   |
J4        |ef<4>       |IOB      |IO_TRDY             |INPUT    |LVTTL      |6             |          |         |NONE**     |NONE     |       |LOCATED   |
J5        |            |         |VCCO_6              |         |           |6             |          |         |           |         |3.30   |          |
J6        |            |         |VCCO_6              |         |           |6             |          |         |           |         |3.30   |          |
J7        |            |         |GND                 |         |           |              |          |         |           |         |       |          |
J8        |            |         |GND                 |         |           |              |          |         |           |         |       |          |
J9        |            |         |GND                 |         |           |              |          |         |           |         |       |          |
J10       |            |         |GND                 |         |           |              |          |         |           |         |       |          |
J11       |            |         |VCCO_3              |         |           |3             |          |         |           |         |3.30   |          |
J12       |            |         |VCCO_3              |         |           |3             |          |         |           |         |3.30   |          |
J13       |fout<11>    |IOB      |IO_TRDY             |INPUT    |LVTTL      |3             |          |         |NONE**     |NONE     |       |LOCATED   |
J14       |            |IOB      |IO_D4_L32P_Y        |UNUSED   |           |3             |          |         |           |         |       |          |
J15       |fout<8>     |IOB      |IO_L31N             |INPUT    |LVTTL      |3             |          |         |NONE**     |NONE     |       |LOCATED   |
J16       |fout<9>     |IOB      |IO_L31P             |INPUT    |LVTTL      |3             |          |         |NONE**     |NONE     |       |LOCATED   |
K1        |dout<8>     |IOB      |IO_VREF_6_L71N_Y    |TRISTATE |LVTTL      |6             |12        |SLOW     |NONE**     |         |       |LOCATED   |
K2        |dout<9>     |IOB      |IO_L70P_YY          |TRISTATE |LVTTL      |6             |12        |SLOW     |NONE**     |         |       |LOCATED   |
K3        |fout<5>     |IOB      |IO_L70N_YY          |INPUT    |LVTTL      |6             |          |         |NONE**     |NONE     |       |LOCATED   |
K4        |            |IOB      |IO_L68P_YY          |UNUSED   |           |6             |          |         |           |         |       |          |
K5        |dout<7>     |IOB      |IO_L68N_YY          |TRISTATE |LVTTL      |6             |12        |SLOW     |NONE**     |         |       |LOCATED   |
K6        |            |         |VCCO_6              |         |           |6             |          |         |           |         |3.30   |          |
K7        |            |         |GND                 |         |           |              |          |         |           |         |       |          |
K8        |            |         |GND                 |         |           |              |          |         |           |         |       |          |
K9        |            |         |GND                 |         |           |              |          |         |           |         |       |          |
K10       |            |         |GND                 |         |           |              |          |         |           |         |       |          |
K11       |            |         |VCCO_3              |         |           |3             |          |         |           |         |3.30   |          |
K12       |db<10>      |IOB      |IO_L33P_YY          |BIDIR    |LVTTL      |3             |12        |SLOW     |NONE**     |NONE     |       |LOCATED   |
K13       |ren<5>      |IOB      |IO_VREF_3_L32N_Y    |OUTPUT   |LVTTL      |3             |12        |FAST     |NONE**     |         |       |LOCATED   |
K14       |db<7>       |IOB      |IO_L35P_YY          |BIDIR    |LVTTL      |3             |12        |SLOW     |NONE**     |NONE     |       |LOCATED   |
K15       |db<8>       |IOB      |IO_L34N             |BIDIR    |LVTTL      |3             |12        |SLOW     |NONE**     |NONE     |       |LOCATED   |
K16       |db<9>       |IOB      |IO_L34P             |BIDIR    |LVTTL      |3             |12        |SLOW     |NONE**     |NONE     |       |LOCATED   |
L1        |db<4>       |IOB      |IO_L69P             |BIDIR    |LVTTL      |6             |12        |SLOW     |NONE**     |NONE     |       |LOCATED   |
L2        |evid<5>     |IOB      |IO_L69N             |INPUT    |LVTTL      |6             |          |         |NONE**     |NONE     |       |LOCATED   |
L3        |dout<3>     |IOB      |IO_L67P_Y           |TRISTATE |LVTTL      |6             |12        |SLOW     |NONE**     |         |       |LOCATED   |
L4        |            |IOB      |IO_L65P_Y           |UNUSED   |           |6             |          |         |           |         |       |          |
L5        |            |IOB      |IO_VREF_6_L65N_Y    |UNUSED   |           |6             |          |         |           |         |       |          |
L6        |            |         |GND                 |         |           |              |          |         |           |         |       |          |
L7        |            |         |VCCO_5              |         |           |5             |          |         |           |         |3.30   |          |
L8        |            |         |VCCO_5              |         |           |5             |          |         |           |         |3.30   |          |
L9        |            |         |VCCO_4              |         |           |4             |          |         |           |         |3.30   |          |
L10       |            |         |VCCO_4              |         |           |4             |          |         |           |         |3.30   |          |
L11       |            |         |GND                 |         |           |              |          |         |           |         |       |          |
L12       |add<2>      |IOB      |IO_L33N_YY          |INPUT    |LVTTL      |3             |          |         |NONE**     |NONE     |       |LOCATED   |
L13       |            |IOB      |IO_D5_L35N_YY       |UNUSED   |           |3             |          |         |           |         |       |          |
L14       |ff<2>       |IOB      |IO                  |INPUT    |LVTTL      |3             |          |         |NONE**     |NONE     |       |LOCATED   |
L15       |ff<5>       |IOB      |IO_L36N_Y           |INPUT    |LVTTL      |3             |          |         |NONE**     |NONE     |       |LOCATED   |
L16       |            |IOB      |IO_D6_L36P_Y        |UNUSED   |           |3             |          |         |           |         |       |          |
M1        |dout<2>     |IOB      |IO_L66P             |TRISTATE |LVTTL      |6             |12        |SLOW     |NONE**     |         |       |LOCATED   |
M2        |dout<4>     |IOB      |IO_L67N_Y           |TRISTATE |LVTTL      |6             |12        |SLOW     |NONE**     |         |       |LOCATED   |
M3        |            |IOB      |IO_L64P_YY          |UNUSED   |           |6             |          |         |           |         |       |          |
M4        |            |IOB      |IO_L64N_YY          |UNUSED   |           |6             |          |         |           |         |       |          |
M5        |            |         |VCCINT              |         |           |              |          |         |           |         |1.8    |          |
M6        |fsen        |IOB      |IO_L55N_Y           |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |
M7        |paf<5>      |IOB      |IO_VREF_5_L53N_Y    |INPUT    |LVTTL      |5             |          |         |NONE**     |NONE     |       |LOCATED   |
M8        |            |         |VCCO_5              |         |           |5             |          |         |           |         |3.30   |          |
M9        |            |         |VCCO_4              |         |           |4             |          |         |           |         |3.30   |          |
M10       |paf<1>      |IOB      |IO_L48P_Y           |INPUT    |LVTTL      |4             |          |         |NONE**     |NONE     |       |LOCATED   |
M11       |add<0>      |IOB      |IO_VREF_4_L45P_YY   |INPUT    |LVTTL      |4             |          |         |NONE**     |NONE     |       |LOCATED   |
M12       |            |         |VCCINT              |         |           |              |          |         |           |         |1.8    |          |
M13       |ff<3>       |IOB      |IO                  |INPUT    |LVTTL      |3             |          |         |NONE**     |NONE     |       |LOCATED   |
M14       |db<2>       |IOB      |IO_L39P_YY          |BIDIR    |LVTTL      |3             |12        |SLOW     |NONE**     |NONE     |       |LOCATED   |
M15       |ff<0>       |IOB      |IO_VREF_3_L38N_Y    |INPUT    |LVTTL      |3             |          |         |NONE**     |NONE     |       |LOCATED   |
M16       |ff<4>       |IOB      |IO_L38P_Y           |INPUT    |LVTTL      |3             |          |         |NONE**     |NONE     |       |LOCATED   |
N1        |vspare_1    |IOB      |IO_L66N             |INPUT    |LVTTL      |6             |          |         |NONE**     |NONE     |       |LOCATED   |
N2        |            |IOB      |IO_L63P             |UNUSED   |           |6             |          |         |           |         |       |          |
N3        |            |IOB      |IO_L63N             |UNUSED   |           |6             |          |         |           |         |       |          |
N4        |            |         |VCCINT              |         |           |              |          |         |           |         |1.8    |          |
N5        |lives_p     |IOB      |IO_L59N_YY          |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |
N6        |dout<6>     |IOB      |IO_L57N_Y           |TRISTATE |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |
N7        |load_paepaf |IOB      |IO_L55P_Y           |INPUT    |LVTTL      |5             |          |         |NONE**     |NONE     |       |LOCATED   |
N8        |add<1>      |IOB      |IO_L53P_Y           |INPUT    |LVTTL      |5             |          |         |NONE**     |NONE     |       |LOCATED   |
N9        |led<1>      |IOB      |IO_L51P_Y           |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |
N10       |paf<4>      |IOB      |IO_L48N_Y           |INPUT    |LVTTL      |4             |          |         |NONE**     |NONE     |       |LOCATED   |
N11       |enw         |IOB      |IO_L45N_YY          |INPUT    |LVTTL      |4             |          |         |NONE**     |NONE     |       |LOCATED   |
N12       |ren<2>      |IOB      |IO_L44P_YY          |OUTPUT   |LVTTL      |4             |12        |FAST     |NONE**     |         |       |LOCATED   |
N13       |            |         |VCCINT              |         |           |              |          |         |           |         |1.8    |          |
N14       |fsi         |IOB      |IO_L39N_YY          |OUTPUT   |LVTTL      |3             |12        |SLOW     |NONE**     |         |       |LOCATED   |
N15       |ff<1>       |IOB      |IO_L40N             |INPUT    |LVTTL      |3             |          |         |NONE**     |NONE     |       |LOCATED   |
N16       |sff         |IOB      |IO_L40P             |OUTPUT   |LVTTL      |3             |12        |SLOW     |NONE**     |         |       |LOCATED   |
P1        |tp<2>       |IOB      |IO_L62P_YY          |OUTPUT   |LVTTL      |6             |12        |SLOW     |NONE**     |         |       |LOCATED   |
P2        |            |IOB      |IO_L62N_YY          |UNUSED   |           |6             |          |         |           |         |       |          |
P3        |            |         |VCCINT              |         |           |              |          |         |           |         |1.8    |          |
P4        |tp<1>       |IOB      |IO_L61N_YY          |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |
P5        |ceros_done_p|IOB      |IO_L59P_YY          |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |
P6        |dout<10>    |IOB      |IO_L57P_Y           |TRISTATE |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |
P7        |fout<0>     |IOB      |IO                  |INPUT    |LVTTL      |5             |          |         |NONE**     |NONE     |       |LOCATED   |
P8        |clk20_p     |IOB      |IO                  |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |
P9        |spaf_p      |IOB      |IO_L51N_Y           |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |
P10       |fout<3>     |IOB      |IO_L49N_Y           |INPUT    |LVTTL      |4             |          |         |NONE**     |NONE     |       |LOCATED   |
P11       |paf<2>      |IOB      |IO_L47N_Y           |INPUT    |LVTTL      |4             |          |         |NONE**     |NONE     |       |LOCATED   |
P12       |mrs         |IOB      |IO_L44N_YY          |INPUT    |LVTTL      |4             |          |         |NONE**     |NONE     |       |LOCATED   |
P13       |ren<1>      |IOB      |IO_L43P_Y           |OUTPUT   |LVTTL      |4             |12        |FAST     |NONE**     |         |       |LOCATED   |
P14       |            |         |VCCINT              |         |           |              |          |         |           |         |1.8    |          |
P15       |            |IOB      |IO_INIT_L41N_YY     |UNUSED   |           |3             |          |         |           |         |       |          |
P16       |            |IOB      |IO_D7_L41P_YY       |UNUSED   |           |3             |          |         |           |         |       |          |
R1        |            |         |M1                  |         |           |              |          |         |           |         |       |          |
R2        |            |         |GND                 |         |           |              |          |         |           |         |       |          |
R3        |            |         |M2                  |         |           |              |          |         |           |         |       |          |
R4        |doneout     |IOB      |IO_L61P_YY          |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |
R5        |led<0>      |IOB      |IO_VREF_5_L58N_YY   |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |
R6        |ren<4>      |IOB      |IO_L56N_Y           |OUTPUT   |LVTTL      |5             |12        |FAST     |NONE**     |         |       |LOCATED   |
R7        |cs          |IOB      |IO_L54N_Y           |INPUT    |LVTTL      |5             |          |         |NONE**     |NONE     |       |LOCATED   |
R8        |            |DLLIOB   |IO_LVDS_DLL_L52N    |UNUSED   |           |5             |          |         |           |         |       |          |
R9        |            |DLLIOB   |IO_LVDS_DLL_L52P    |UNUSED   |           |4             |          |         |           |         |       |          |
R10       |fout<2>     |IOB      |IO_VREF_4_L50P_Y    |INPUT    |LVTTL      |4             |          |         |NONE**     |NONE     |       |LOCATED   |
R11       |paf<0>      |IOB      |IO_L49P_Y           |INPUT    |LVTTL      |4             |          |         |NONE**     |NONE     |       |LOCATED   |
R12       |db<3>       |IOB      |IO_L47P_Y           |BIDIR    |LVTTL      |4             |12        |SLOW     |NONE**     |NONE     |       |LOCATED   |
R13       |oe<1>       |IOB      |IO_L43N_Y           |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |
R14       |reset       |IOB      |IO_L42P_YY          |INPUT    |LVTTL      |4             |          |         |NONE**     |NONE     |       |LOCATED   |
R15       |            |         |GND                 |         |           |              |          |         |           |         |       |          |
R16       |            |         |PROGRAM             |         |           |              |          |         |           |         |       |          |
T1        |            |         |GND                 |         |           |              |          |         |           |         |       |          |
T2        |            |         |M0                  |         |           |              |          |         |           |         |       |          |
T3        |evid<8>     |IOB      |IO_L60N_Y           |INPUT    |LVTTL      |5             |          |         |NONE**     |NONE     |       |LOCATED   |
T4        |donein      |IOB      |IO_L60P_Y           |INPUT    |LVTTL      |5             |          |         |NONE**     |NONE     |       |LOCATED   |
T5        |dout<13>    |IOB      |IO_L58P_YY          |TRISTATE |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |
T6        |etr_x       |IOB      |IO_L56P_Y           |INPUT    |LVTTL      |5             |          |         |NONE**     |NONE     |       |LOCATED   |
T7        |fld         |IOB      |IO_L54P_Y           |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |
T8        |clkin_p     |GCLKIOB  |GCK1                |INPUT    |LVTTL      |5             |          |         |           |         |       |LOCATED   |
T9        |clk_slow    |GCLKIOB  |GCK0                |INPUT    |LVTTL      |4             |          |         |           |         |       |LOCATED   |
T10       |paf<3>      |IOB      |IO_L50N_Y           |INPUT    |LVTTL      |4             |          |         |NONE**     |NONE     |       |LOCATED   |
T11       |fout<1>     |IOB      |IO                  |INPUT    |LVTTL      |4             |          |         |NONE**     |NONE     |       |LOCATED   |
T12       |db<6>       |IOB      |IO_L46N_Y           |BIDIR    |LVTTL      |4             |12        |SLOW     |NONE**     |NONE     |       |LOCATED   |
T13       |db<5>       |IOB      |IO_L46P_Y           |BIDIR    |LVTTL      |4             |12        |SLOW     |NONE**     |NONE     |       |LOCATED   |
T14       |fmrs        |IOB      |IO_L42N_YY          |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |
T15       |            |         |DONE                |         |           |              |          |         |           |         |       |          |
T16       |            |         |GND                 |         |           |              |          |         |           |         |       |          |

-----     |-----       |-----    |-----               |-----    |-----      |-----         |-----     |-----    |-----      |-----    |-----  |-----     |

* Default value.
** This default Pullup/Pulldown value can be overridden in Bitgen.

