iMPACT Version: G.35
iMPACT log file Started on 2012/11/29 17:08:34
// *** BATCH CMD : setPreference -pref UserLevel:NOVICE
// *** BATCH CMD : setPreference -pref MessageLevel:DETAILED
// *** BATCH CMD : setPreference -pref ConcurrentMode:FALSE
// *** BATCH CMD : setPreference -pref UseHighz:FALSE
// *** BATCH CMD : setPreference -pref ConfigOnFailure:STOP
// *** BATCH CMD : setPreference -pref StartupCLock:AUTO_CORRECTION
// *** BATCH CMD : setPreference -pref AutoSignature:FALSE
// *** BATCH CMD : setPreference -pref KeepSVF:FALSE
// *** BATCH CMD : setPreference -pref svfUseTime:FALSE
// *** BATCH CMD : setPreference -pref UserLevel:NOVICE
// *** BATCH CMD : setPreference -pref MessageLevel:DETAILED
// *** BATCH CMD : setPreference -pref ConcurrentMode:FALSE
// *** BATCH CMD : setPreference -pref UseHighz:FALSE
// *** BATCH CMD : setPreference -pref ConfigOnFailure:STOP
// *** BATCH CMD : setPreference -pref StartupCLock:AUTO_CORRECTION
// *** BATCH CMD : setPreference -pref AutoSignature:FALSE
// *** BATCH CMD : setPreference -pref KeepSVF:FALSE
// *** BATCH CMD : setPreference -pref svfUseTime:FALSE
// *** BATCH CMD : setMode -pff
// *** BATCH CMD : setMode -pff
// *** BATCH CMD : setMode -pff
// *** BATCH CMD : addConfigDevice -size 128 -name "xc18v01" -path "f:\cris\cms\vhdl_ise6_2010\2012_firmware\ceros_dec2011_cuofdeser/"
// *** BATCH CMD : setSubmode -pffserial
// *** BATCH CMD : addPromDevice -position 1 -size -1 -name "xc18v01"
'1': Added Device xc18v01 successfully.
----------------------------------------------------------------------
// *** BATCH CMD : setMode -pff
// *** BATCH CMD : setSubmode -pffserial
// *** BATCH CMD : setAttribute -configdevice -attr size -value "0"
// *** BATCH CMD : addCollection -name "ceros_CUOFdeserser"
// *** BATCH CMD : setAttribute -collection -attr dir -value "UP"
// *** BATCH CMD : addDesign -version 0 -name "0000"
// *** BATCH CMD : addDeviceChain -index 0
// *** BATCH CMD : addDevice -position 1 -file "F:\CRIS\CMS\VHDL_ISE6_2010\2012_firmware\ceros_DEC2011_CUOFdeser\ceros.bit"
'1': Loading file 'F:\CRIS\CMS\VHDL_ISE6_2010\2012_firmware\ceros_DEC2011_CUOFdeser\ceros.bit' ...
INFO:iMPACT - Elapsed time =      0 sec.
done.
INFO:iMPACT:501 - '1': Added Device xc2s50e successfully.
----------------------------------------------------------------------
----------------------------------------------------------------------
GUI --- Add one device.
// *** BATCH CMD : setMode -pff
Collection : ceros_CUOFdeserser
Design : 0
Device Chain : 0
----------------------------------------------------------------------
Position	PartName       	FileName            
1       	xc2s50e        	F:\CRIS\CMS\VHDL_ISE6_2010\2012_firmware\ceros_DEC2011_CUOFdeser\ceros.bit
----------------------------------------------------------------------
// *** BATCH CMD : setAttribute -configdevice -attr fillValue -value "FF"
// *** BATCH CMD : setAttribute -configdevice -attr fileFormat -value "mcs"
// *** BATCH CMD : setAttribute -collection -attr dir -value "UP"
// *** BATCH CMD : setAttribute -configdevice -attr path -value "f:\cris\cms\vhdl_ise6_2010\2012_firmware\ceros_dec2011_cuofdeser/"
// *** BATCH CMD : setAttribute -collection -attr name -value "ceros_CUOFdeserser"
// *** BATCH CMD : generate
0x133a4 (78756) bytes loaded up from 0x0
Using user-specified prom size of 128K
Writing file "f:\cris\cms\vhdl_ise6_2010\2012_firmware\ceros_dec2011_cuofdeser//ceros_CUOFdeserser.mcs".
Writing file "f:\cris\cms\vhdl_ise6_2010\2012_firmware\ceros_dec2011_cuofdeser//ceros_CUOFdeserser.prm".
Writing file "f:\cris\cms\vhdl_ise6_2010\2012_firmware\ceros_dec2011_cuofdeser//ceros_CUOFdeserser.sig".
GUI --- Total configuration bit size = 630048 bits.
GUI --- Total configuration byte size = 78756 bytes.
GUI --- Boundary-Scan File selected
// *** BATCH CMD : setMode -bsfile
// *** BATCH CMD : setCable -port svf -file "F:\CRIS\CMS\VHDL_ISE6_2010\2012_firmware\ceros_DEC2011_CUOFdeser\ceros_CUOFdeserser_DEC2012.svf"
xc18v01_pc20
xc18v01_so20
xc18v01_vq44
xc18v02_pc44
xc18v02_vq44
xc18v04_pc44
xc18v04_vq44
xcf01s_vo20
xcf02s_vo20
xcf04s_vo20
xcf08p_fs48
xcf08p_vo48
xcf16p_fs48
xcf16p_vo48
xcf32p_fs48
xcf32p_vo48
// *** BATCH CMD : addDevice -position 1 -part "xc18v01"
INFO:iMPACT:1777 - 
Reading C:/Xilinx6/xc18v00/data/xc18v01.bsd...
Reading C:/Xilinx6/xc18v00/data/xc18v01.bsd...
INFO:iMPACT:501 - '1': Added Device xc18v01 successfully.
----------------------------------------------------------------------
----------------------------------------------------------------------
// *** BATCH CMD : setAttribute -position 1 -attr configFileName -value "F:\CRIS\CMS\VHDL_ISE6_2010\2012_firmware\ceros_DEC2011_CUOFdeser\ceros_CUOFdeserser.mcs"
'1': Loading file 'F:\CRIS\CMS\VHDL_ISE6_2010\2012_firmware\ceros_DEC2011_CUOFdeser\ceros_CUOFdeserser.mcs' ...
done.
GUI --- Add one device.
// *** BATCH CMD : Program -p 1 -e -v -parallel -u 12340007 
PROGRESS_START - Starting Operation.
Validating chain...
Boundary-scan chain validated successfully.
'1': Putting device in ISP mode...done.
'1': Erasing device...done.
'1': Erasure completed successfully.
'1': Putting device in ISP mode...done.
'1': Programming device...done.
'1': Putting device in ISP mode...done.
'1': Putting device in ISP mode...done.
'1': Verifying device...done.
'1': Verification completed successfully.
'1': Calculated checksum matches expected checksum, 00107005a
'1': Putting device in ISP mode...done.
'1': Setting usercode...done.
'1': Putting device in ISP mode...done.
'1': Setting user-programmable bits...
'1': Setting parallel mode bit...done.
'1': Putting device in ISP mode...done.
'1': Programming completed successfully.
PROGRESS_END - End Operation.
Elapsed time =      1 sec.
*****   Closing iMPACT program.   *****
