Release 6.3i - netgen G.35
Copyright (c) 1995-2004 Xilinx, Inc.  All rights reserved.

Loading device database for application netgen from file "ceros_map.ncd".
   "ceros" is an NCD, version 2.38, device xc2s50e, package ft256, speed -7
Loading device for application netgen from file '2s50e.nph' in environment
C:/Xilinx.
Loading constraints from file "ceros.pcf"...
WARNING:Anno:28 - This .ncd is not completely routed; therefore, some delay
   calculations may be inaccurate.
  Flattening design ...
  Flattening design completed.
  Specializing design ...
  Specializing design completed.
  Preping physical only global signals ...
  Preping design's networks ...
  Preping design's macros ...
Writing VHDL netlist ceros_map.vhd ...
Writing VHDL SDF file ceros_map.sdf ...
Total memory usage is 89020 kilobytes
