// Created using Xilinx iMPACT Software [ISE Foundation - 6.3i]
TRST OFF;
ENDIR IDLE;
ENDDR IDLE;
STATE RESET IDLE;
TIR 0 ;
HIR 0 ;
TDR 0 ;
HDR 0 ;
// Validating chain...
TIR 0 ;
HIR 0 ;
TDR 0 ;
HDR 0 ;
SIR 8 TDI (ff) SMASK (ff) TDO (01) MASK (03) ;
TIR 0 ;
HIR 0 ;
HDR 0 ;
TDR 0 ;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) SMASK (ffffffff) TDO (f5034093) MASK (0ffeffff) ;
//Loading device with 'conld' instruction.
SIR 8 TDI (f0) ;
RUNTEST 110000 TCK;
//Check for Read/Write Protect.
SIR 8 TDI (ff) TDO (01) MASK (ff) ;
//Loading device with 'bypass' instruction.
SIR 8 TDI (ff) ;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) TDO (f5034093) ;
//Loading device with 'ispen' instruction.
SIR 8 TDI (e8) ;
SDR 6 TDI (34) SMASK (3f) ;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) SMASK (ffffffff) TDO (f5034093) MASK (0ffeffff) ;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) TDO (f5034093) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0001) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'ferase' instruction. 
SIR 8 TDI (ec) ;
RUNTEST 1 TCK;
RUNTEST 15000000 TCK;
//Loading device with 'conld' instruction.
SIR 8 TDI (f0) ;
RUNTEST 110000 TCK;
STATE RESET;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) SMASK (ffffffff) TDO (f5034093) MASK (0ffeffff) ;
//Loading device with 'ispen' instruction.
SIR 8 TDI (e8) ;
SDR 6 TDI (34) SMASK (3f) ;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000000000000000000c4000000000000000054fba80000000000000000000000000000000000000000000000000000000000000000000000000000000000000000d53ff0000000000000160400000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000c480000000000000001200400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000c480070da000a0002000c800000008001000c000000008004000c900000008001000c638000008003000c6dfc01008004800cb0000000800680
0ce00000008001000c66aa9955ffffffff) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0000) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (b804000500014000500014000500014000500014000500014000500014000500014000500014000500014000500048ff0000000000000420000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000004800000000000000054ffc000000
0000000000000000000000000000000000000000000000000000000000000000000000000000000000015bff0000000000000d2ff80000000000000000000000000000000000000000000000000000000000000000000000000000000000000000015bff0000000000000140028000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0020) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (139b00c6e035f2064c005e0047431934025501d304c3a80200000000000006200f000d508844001400774019d1454400dd0c64441d110074c8d100165019d00554809504464419102a2401c90045a8030000000000000c8043400c100044408108254008100056008c08305008d0006420892002
4004d00104005d0003604014821481c18003a0100000000000000c2007401d540045001500574211f91144419c0134c01110045401914006c000d00354201100c7200910026c20930807080100000000000006800f401d32046c0027006fc00930241e218f0a74c813c004cc009b800ec011f0075c215a050bca3b
b486cc00b3000780030000000000000163) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0040) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000a001f400cd04c04230d00f34808180114058d0030600050041400050cc24431d23706804401834038100314000d0002a00700000000000002004f420dd0040c031d20f744ad30010401cd0035607810001403d304b4e02980046c06c5000340e958024400d10004a01300000000
000004200fc00df0026c12df0127c02d3a085c80d720b5c009b0005c00931820c005f0014c905b0807c029300a5e00d70005080300000000000006001fc00ff20cfc403f103fc0077001fc40bf303dc80bf208dc40ef00edc10bf302fc207b080fc40bf002fdc0d7400d80070000000000000e200bc00d300d4c08
460463c45d140454499f2074c819f0006d) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0060) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (e1003ac00a11008400e1002e500ff4038400710838400f30838c8061001988130000000000000e2057c00db0800d80532070c40976010c00d780749009b0004c20c32004c01db0034c41530025c61930030c00534007a81500000000000006600bc00df000fc00ff0237e88f70315c00ff083f80
ca70303c00c7003dd00d9003fc08b7402fc00bf2837c8836023db80200000000000000404bc4dcf8240c178f0433e05813051c118701704858725c1c11c541e6e05cf2070d05570063c81812025405cf0164101200000000000002001b001ed0648589ad805b621a90158425ed027944f210b4940f39006a419290
07a64521014a40da582784092801588006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0080) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (024d009b002700100000000000000c084bc00170087c001f0405c221a0007c02171007c001f0405e001f20848021f6087c001f0085c82174604c401f0007001200000000000006005fc005b01dcc0073409cc807f009cc0057119cc067b005ae2363419d4807b005cd017104df40371009f80071
041da01700000000000008004b400cd8100440d19032428cd0136440c101b640381427249ac100774aec50074460c16132486c90093009512077281200000000000004000f401e9d04c403c1207a6218d005c423f5001c481b9a04a400e1107b401e9147862361087b603a1487f401e10071000300000000000006
204f400e50008400a12018400ab481ac00) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (00a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0006e24530005c00110004400134007c84130107c801f0003c001b0105c00138004c841b0106b01c0000000000000080434408920234148d1021414818020400819021400911025454910d33400810023420c1052260081002441481052020100000000000000200634009180205009d00a54009
1502544095802449091252540491102768add02b7424990825400912024400990024a0180000000000000820074409b01a7c029d00655029120244068190255408100254109100a74039180a742291416243390402040091202620010000000000000c0043c009708a48049f0266400831025c05930024c3493206
7c00930667c01931027c009300e7c09930) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (00c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (7420d90825490912420400910025a0180000000000000e8043480810d274108d80236028520276008121216409000264429d0c224048dc023410892020500810c22490810423a0100000000000000c0071c001b0045c071b00078021f01564001b0954400151015400110146c551548474255848
16c001101404070103c7081c0000000000000e4063c00b3202fe91bf002fc01b740a3c20b100a1c00b3102ec21bb8d6ec00af122fc20b30028c20b30026015bb016788180000000000000e4867c009f053ec14bf002e400bf052fc00af052bc00af002bc00bf452fe54ff452fc14bf202a414bf052fc14af053fb8
190000000000000ac073cc0134004c045f) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (00e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (534805120184237c001dc0475001b40471481c4807f00d940a6000dc4027d045cc0671401e48071101441071201ca814000000000000042053c00130084c82170087c00130087c80132004c801b0086400131084c401f0006d12132407c42170086cc01208850014000000000000060055c009f0
065c05970427c009f0026c129f30e7c029f0026d019b0122c049f0c27c209701628109f4067c8997502580150000000000000e2017c009100274009d00a74039500a7c00910025c22810066c009f4426f009fc0674029300244009302e6c10930223a0050000000000000220614009141250a29980a54039c00264
0099002440295222540695102644085262) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0100) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (09e24054c29f3207cc8113007c409d7427dc0df700778000000000000000062043c00db6806c009b0017c405f0037c005f0035800cd2021c00cf2017c40592015c009d00264001f2bb7c44db4035b010000000000000000057c01e3405d901ef006be016700fbc2163017ac01eb0069501e3205c
c40ef1078c01b1006ac2127047ac31e3017c1015000000000000020017400e100b90038d04194c065013f40061833a500ed008d402f100b8440fd003a401e1103a400610038400e1433880050000000000000a0053600c10071611cc08d3451cc003340341103641ac94141400c144b0418cd00b402041003260ad
58032401d90032a0140000000000000200) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0120) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000062054500d120f4403dd0066c021d20bec215f017cc00c78166c0089a1e5e40d00476802930026c4c9d113d405d4817da8150000000000000c2010400c54440400890012421041434400498135420c104224010c0847407090002402892062601091176402c10037080400000000
0000040000644e1040c446ad332a4002d013a408ed003a414e4112e704790009404e1002a404b1042a4043d8039644e502390800000000000000062054405ef017ac2a89035a4152f09784102a0039405410062811a50064485ab20394056b0112c4d01417ec08cb017980150000000000000e0000c41e31264d0d
bf085f4299f007ec017f007cc01c7026ec) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0140) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (411030490c501a54041183224200940066c8c102224060581304088801302010000000000000020007440d50824481dd00976119100374005d1034491d104654239104455804900164019d14674911d4034524910034a001000000000000080207420d504805019d006640315003640855003454
39500e1403510067c07130143c019108e3403110036c01d3203620810000000000000c2203c00f1083cc00bf112fc4033203fc007b103cc80f7203dc00f3042dc08b3027d410bb0027c2037503cc11e3003708800000000000000c0007c00df0017d03cb04e6c101f1237c00530037c82df0827c2017802480ad37
0a5c01df0027c02170035e00df00370001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0160) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (022040010007a010000000000000040004401d70114404910124504110107400170034c10c10536d01912874400dd0046d00011045c08180004c2033000718010000000000000ec80cca1df00ccc00b30084c09332257c033700fec017f0874d801b006ac499d204cc4133804ac003f2024cc03f
004f88030000000000000e4017c04df410bc842f1216c063f00b6c046f093fc90ff20238981f412fc0c17010dc0caf092f8022b40b7c04b7f13f88050000000000000ac003c06d70224d489f9127c4813b0b7c02df02b4c00d705a5c04539505c480b0200c009f8027c021f103c600a10736a00000000000000000
8043412c504144c0cd01126040501b2442) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0180) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0c34c401381c4c1a970236c025f0026c075b0124c20d708b6c025b20a6c0a9300a5c385f0205000300000000000006001fc00ff041dd00ef0153c093f000fc8537903dc083f003fc019f200cc00ff012fc88b7000c400bb0017d003f000d80070000000000000e2008d00df00c6c015300544031
31a07c001f0034d135f00f4d001e0062c07cf00845060940c28011722e6c03420043a00200000000000006200c400d500d642391c024442410023410150036480513042404d10067401dd0004400d908674110d0004401111845a0030000000000000c8040420cd01024148100004040141034240d913042055012
04205d00224049d20016001980064c0050) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (01a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (fc20f70024c009f023dc049d020db00200000000000000004bc0dc30150c00930140c0d114047c04470232c01450162c03470160425c728a2c09834081409914063d068f0140101200000000000002001b401e1224c401a90168405a120486013d027a41d61427840d6d0969405fd806a41b610c
ed549a9027a48d8d0b4880060000000000000a001f400c100c040681000070001800300105213240141007240245a0a0400c520024400130414050100234018d0042a00700000000000002004f400c11054425db01f443a1100c48011d0074401412464c414a04a5400dd0036c40d100a44219f00144805d02a480
1300000000000004200fc00d342a4c02d3) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (01c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (4b400c50450439cd04374400d04c040201003048a4022704024904a04125d04b0409d1c07000dd18274402010077281200000000000004000f401e548ca401bd006b40121044c40331807948165007c7017900e8611fd00eb401e1147d401ed006e50369044d000300000000000006204f400e10
01c400ad100b4002f200840021403c400710038400610008540ed1028400e30028400e1003840081000988130000000000000e0057c20d32046c008f0007c00132044c00130075c81570070c205b1024c00cf0007d80d20027c00178022c305b0007a01500000000000006200bc20ff001bd40df003fca03f000fd
002f023dc20576023c007b2227c08ef002) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (01e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0095802540095002744891412462295a034402910024a0180000000000000800044008d00644029120e45409d20a44109d20274029d042440a8300e5400952022c02910c205009b80244839104a620010000000000000c2040c009f0024c009340e4c229a0a24c009f1227c009f00e4c019510e5
c00920027401930024c00974024c059b016708100000000000000c004bc001b0007c001f0007c041f0007c041f3007c101f1007c04171087c401f0005c50170105c20178007c100f2187001200000000000006205fc0057009ec016f011fc1273001cd00730015c0175025cc027b0058c007d009fc2073005dc007
f181ed007b001d88170000000000000c20) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0200) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000e0063c00b300a4c37930264c08830224c00930024c029b00aec05a7002cc009f0827c00b9082ec00b31165c91bf00aba0180000000000000e4067c009f052fc14bf052fc14bf252ac14af0526894bf852fc00e3002bc54bf802ec14bf202bc14af052fc14bf052b981900000000
00000ac070d001f0004c04130104c205b0004d001f0017c001f9004c04170015c40174007c80430004d04152104d04130006b01c0000000000000080404008d00205149105204008d00314008d00234008d002059591802142081202740081002441481052041481402020100000000000000200604009d0064406
9100a44008d00344c08d08274029d20344) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0220) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (971027c01972064c04971425c009f0027400970827c099f0825d038f00e580150000000000000e2017c009304244629302e6d109b0064c049b40244079b2466c029f0426c029d0427c429a0266c05930027c219f00e7a80500000000000006206340091002c414e5942a444bd08a8484e900280c
4a98225480990137410950224714990424400d100260009d0425a8180000000000000e8043400810128480a181aa604b90128614a90428424a901264088d00264149d10224108900265108545a36558d0123a0100000000000000c207340011004c503054044401150044c01110144501110044ca2110005401170
004405110004c011128c04031d0046001c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0240) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (17bc01714048001500000000000002001740061003c400ed00ba40035101a600e90009080e120b9600fd003848ce5003941031043864245013b40061045c88050000000000000a0053400410034400cd003241acd11b2593c908315b0c90073623cd00f1480cd2031581d500f5404dd103758ac1
00f2a0140000000000000200534007100144125d02d44434704944025110144d25100915006d84d848047201440171029c40273001440071001c8014000000000000042053c0013000cc001f0884c001f0804c88130004c021b0047e1a1f0005c00173086c10130087422172005c44130104081400000000000006
0057c009f4127c519f8025c019700a5d00) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0260) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (801f400a9271b40869003a41c71209e580f50a3c410f1013e60c6d012a7106942396404508090000000000000000062057405650672c01eb002bc034f037f405a1004ac0187017ac07e12772c01e311784019d01e842d41103840d67024188150000000000000e0003c41532070c0df3027bc25d
71077c89d30074c8df3026ec49c6007ac01c10275c8dde026cc017b00fcc0d760057a000000000000000066043c005f0023d001f1005d001f0005440d74026880574833c001f1037c00dd0034c00094021c005b03b4d005f0805a810000000000000004057c01634068c012f004ac01ee006ac01fb007cc217b207
bc01ec0879c01ff8079c51673079d116f4) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0280) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (44231d00c6c485110344011591c600810000000000000c2203c007f100c00853006cc22fb14ecc12bf804ec82b3085fc10b6007fc80f3283cc003f000dc0173083cd1023000f08800000000000000c0007c005f0097e0c9f1017c009f0017c42170097c02d70017c029f0c37c10d700348061f00
05c825f1136c081704170001000000000000062057c405322d6501db03b7407dd00f7c011b5036403930816d00970074c01f30673c065e22a6540db04fdc03d70195a8150000000000000c20134004500a042219000540415000340b9900225110508124020100d2443c940335400d10224114000f142345800628
0400000000000004000340461006e48ca9) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (02a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (15c0677010ed021b010f8c03f070fc083f080e80c0f0313c1c331236c24ff0a3bc143f1007c0c5b203fc081f010fb8050000000000000ac003c045f0505c04130004d12da01a44a45d0102e0c130397c065100b7e16d10134c467f1907c282512b8c04110706b0000000000000000080414884d0
311644c5123040c0d40144200504116041141314245131a6408c9213451009040240445483040045010020100000000000000200074005d00954005109b44a05900244405d21b7402110433401510137480d120344114d2047400850030484518844a001000000000000080205c205f08044801540c44031f11c05
021f9044002c12255641034072400dba03) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (02c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (010f32f54219f0024402152446c011702654030d0035000000000000000002200d401d91034400990034401d110374415d0076420d100344111910064015d8226411154044604dd0034401952035a0030000000000000c8040440992232400890030404d508334804d2020424c108344c01d0001
4015500204100100024048d00314001d0033a8100000000000000c20055005b20bcc011100748009120b7000dd0074600db0074501110046c015d0026e0e518244484d90064481970076000100000000000006800cc20b18036c0031407cc03d7053bc00af006ec49d3007ac81370044e007f226cc0017090ec890
7006dc013f007788030000000000000e60) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (02e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000a001c6008918334000d0072602c184f144d8d0032400c506f340b0d0071400c900a14841100004005d00314000d1032284700000000000002004c403c782bec93cd0074422da88fc4005d0037e20d108f6c031500b1480c100f6c01510062c0ad100f04109d0034a05300000000
000004200cc43932031c04d70034d10532234d205f8036e00d31035c12172234c00db1235c8a5302a6e08970635c221f0035000300000000000006001fc00df0037c0177003dc00fb003bc00fd203dd00ff483f80033083fc80df0c7fc405b2005c01f3002fe80b7003d00870000000000000e2000c0399803680c
590030f05470037c83df20f4c40c01832c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0300) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (ad083ac80ef0839400218038400e1403b400ed080b400ed20384006d003990130000000000000e0054c00d34034e001f0036400c30030d00d70034c00df0036c20830830400cb1067c809f1007c005f0036c201f0037a81500000000000006600bc28960034c00ef023dc08cf0237c009f0037c2
4fb203fc0047013bc24d71036ca01b003fd00f7003a8002f0035a802000000000000004048d078b0071c008f0572c05c10171c008d00b2489c74371c4d0c09f1c01cb20354ad03402040dcf0371c000f0072001200000000000002001840bad237b4212d017a405f14278409ad0079481e4007a6092d00b9449e10
279481650848405f900794012d89788246) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0320) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0258019f002700100000000000000c004bc00170085c0c1f0007d021f0087c0a1f2107c60172087e401f1044d001700078021f0c07c821e0087c001f0006001200000000000006205cc087300144007d0016c8771001c4407701181005d0012e8172801e491602017c267f001f4007d001ac007f
0015a0170000000000000c204840bc100334034d0030402d108344018d0090400cd2031418010033010c108334078d00f3400dd00304010d0033201200000000000004080c401c1097a4018d007a501f1807c481850878401ed007a4a121083a421f1147b401a90c7b401ed007a4033d0079000300000000000006
204c400e303b34802d0038500e120b8420) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0340) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0804c001b2904e04538804c00138006c001b0005e441f8005c041a0904e001b0004c001f0006181c0000000000000080405948105206148d0020400c10d205148180254008060205209d08654148d80204148105204808100305208d002028100000000000000200604008102204249d28244019
900a4408d1c0244008100244009900254009d0465002990064408990024400dd002420180000000000000800044009140244009d00244019102e44029110254209103244418500e04009d00e44828520245879108244088d002620010000000000000c2040c00930024d018f1124d109b0024c01830024c0093082
6d22930165c409f0025c009b0022c019b0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0360) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (74809920654009121264849d2025a8180000000000000e80405108d04224008d00235009102214088108254008100225208900204028d08234008420234008100265409d0023a0100000000000000c60704071fa040c805d0004c011ba0c4407130004405150006c20510006c021d10074071d08
07c00514006c001d0007081c0000000000000e2060c15bf946cc11bf082fc02b309edc0db38025c0893082ec00a7003ce05bf002fc13bf082fe00b30028800af0027a0180000000000000e6067c14bf0527c00bf0027d14bb8527c14bf082fc148f002fc00b7202ed00bd052bc34bd102fc14bf002ec00af0025a8
190000000000000ac070c04130114c041f) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0380) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (5041073445c4287d081c48169041c4037d08154807b211950961081a40271005d400792414c02710098c007d20142004000000000000040050c40130004d001f0004c081b4004c101fa084c80130007c20151007818112304c001f8884c00172106c801f00050814000000000000040057c109f0
8278018f0025c019f0023c41872027c009f0425e45938425c029f0067c099f0027c509f0027c009f00250055000000000000040014c049c8026d019c0027c21914025488910ca14a0932826e019380244208f00274019701274009300664018f002509050000000000000600604209500244089d00244049988244
a2914024400955026400991826500dd092) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (03a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (09a50050c09f3107cc09bf0077c091b0078f01df0a7faa02000000000000064043c00d30017c401f0037c00df0017c009f0037c06df0023c001f0002c00df0007d005b2025c40070804860df0835b010000000000000004050c01f78078c01afa078c817f204cc017d0078c0ffb006bc0127101b
c41e3404cc012d106ad0167005ac01ef00781014000000000000020010480ed00584824d10b8500a11018410ed2038404e9002840221044e400e100684814d202a403f9200e002fd103880040000000000000a0050523d500304018d1060626850070403cd0030400d900234400500b3403c118f04208d0032403c
50012400cd803280140000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (03c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000062050410930027420012032c01830034501150274500f96824442870000405d928165008f28774029b8004529df003580140000000000000c2018512810007453011031404080014401810070400c50001402080001480c502004014d002241309000000a8d0033280600000000
000004000040471112b60421203840421010c41025013c400e90228444a5011842ce9030e4042d022b600290018404ed1839000000000000000006205440581225fc2d6140314012b4b50403fb057ac01ef0163c810b114bc09c7014ec017d0a6a0152b0100405ac017988150000000000000e0008c0163007cc41
53026ec29b34068c09374278c29d30260c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (03e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (c909304b0c501234000510004000d800061019242240c0508015109921b028100000000000000a00074601100244015100655009940274001d0034500d58064440d500d54001d08044089d2227401150046400dd00342001000000000000080207412512114405514035480d50245c039d003442
0c50062c44150044402cd14855001900674111714454008d003620830000000000000c2203c02b3021cc0053103cd0073104fc053f003dc00f7002cc13b7101dc83df008cc013f006fc0037200ec02bf003f00800000000000000c0007c025f20a7c085f0837c089f0007c02df0037c00df0027c0a1f1087c22df0
007c081f0227c22170007c00df10370001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0400) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (8014801d3003a0100000000000000c2007401d10187480510037418d10700404010117440d10035484dd0077401dd80776231148174941f00444801d804708010000000000000e800fc01f3020fc035300ffc0033000dc0333085bc83d708b5c03fb0077c01ff087ec34330017c211b004cc011f
004fa8030000000000000ee017c081f0307c087f003bc8c060305c009f0037c04fb0a0ec881f020f4161f2007cb41b002fe4c3f090fc80ad033728050000000000000a4003e0a120184e045300b5c8c194307c041f0534c0ce71334c2c970a154261f8504c241f21274a4170206c049f0136100000000000000000
80434040041a07205100b14001d0103410) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0420) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0034d02174314c80130016cc0d70036c00df0637c00d70036c081b4014c809f1084c405700c5000300000000000006001fc00ff0437c0077403fc031e107ec003f001fc00ff2833c90fd003fc00ff803fc203b0017c21fe000ec093f000d80070000000000000e200bc00d341b7c005b0033c001
34035481132077c00d71034c40db0837c00dd003649311004740d192045d031d2047a00200000000000006200f400d10007480580037410d10225401915057400d12035420cc0037000dd00374011506174005520456805d20c580030000000000000c0043400c19303424499137400011101484110513444c5013
2400c90033400cd3032400011813400090) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0440) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (cc08cf101dc08cf021dc047f0015b80200000000000000404b809cb4642c014f0030c19052151c2101435262dce0870e01dd2373c05c70371c0d830350c01cf0092d07170140101200000000000002001b401e520685057c0278421e10a4941f21065f485e90b7860dec107b405ed0079405a902
58481bd205a6096d024880060000000000000a001f400c900c60044d2130651012085000010116600cd20f0402cd00f3400c50031024010014412090302420052402a80700000000000002004f400d700e48445d11344031b00f452201805760ed1063c113dd0077400dd00345031e2015431dc00844104d0804a0
1300000000000004200fc00d31024c005f) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0460) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (4b400cd0064440410033412d184f240a418413400c10831420dd1033440cd0032400c90137418d10132401d141b3281200000000000004200f401ed006860161807f611e1205a60125004f441e50170601ed207b401ed007b431e900d3081e1807a40161006d000300000000000006004f400ed0
03840061003b400e1402c40031081b440e10039400ed083b400ed003a400a1081b400e1003840071003988130000000000000e0057c80df0014c00534837c00db1064c80170037e00d70834c20df0037c00df0036c00120017c00530044800530067a01500000000000006400bc00fb0007c006b303fe00df003ec
80bf201fc08d7243dc00ff8037c08fe003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0480) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (409d80a74009d002640091c0264049c10266009d01a48018000000000000080007400910124e028b01644029d10e44009100e450091c0245839300674009d00244029b00244029d02644219d206620010000000000000c2043c00930026c819300e6c029f00a4c01930024e009300a0c08960167
c009f0026c00830026c819f0066c059f006708100000000000000c004bc001f0487d001f1007c40172205d101f1007c001f0007c021f1007c001f0006c02170007c001f0005d0c1f0007001200000000000006205fc005f049cc00730017c0273201ec0067619fcc0570014c005f0013c005f0816ca07b405fc037
3601ed0373015da8170000000000000c20) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (04a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000e8063c009f01e6c289300a5c07931865c02930024c4093ab6cc48bf002fc009f0025c20b101e7440a3102d820b4102b80180000000000000e2067c009f153dc14bf152bc14bf152ec14bf052bc149f0527c149b0026c009f0827c20bf052fc14be202bd14bf002bb01900000000
00000a8073c00131104c00030005c841f1105c00130004400114104c404f2007c001f0006c04130106c001d0806c001f0006b01c0000000000000080434008045204009800205148d8531400d140604008105204008500234008d8020414c905204818900204408d0020201000000000000002006340091802450a
9120214029da0255089100604808140a44) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (04c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (9f00a7c109f0827c809e0027c009f0027c009b1223c789f2027c889f002582150000000000000e2017c009f0064c00912025c009103a5c009340a4500911025c009d0027c009f00250209241274029b2164483973227a8050000000000000620634009c002c400e0002c600a11038522b1002840
0f108214208c00274809d002540a900025402d5006442291002588180000000000000c00434008d91a8484a14029608a11429604b12028410a140a16848d90234008d002048091a1a3400890020524850023a0100000000000000c20734001d00cc5011100445031b03c44051105546051b01454210d00074001d0
005480110147c20170004491110007081c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (04e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (068c81b300481015000000000000020017400e500fc400e5243b610ed802a400a9009b4402500324002d00bb680ed8039400ad013c443ed0418600e0000880050000000000000a0053400cd007068cc501b7601cd0032412c90071601d50832419cd0033400cd8033403d54030403cd8430411d1
003280140000000000000200534005300144415320d74025d039440241801748655c0145827d20df4605d0815c857b20144827d109cc00714018a014000000000000042053c0013008cc001b4007c001f8004c2013a085c40171004c40172407c001f1007c061300854021f0086c0a133044081400000000000006
0057c009f2127c809f1027c109f4067c05) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0500) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (802848439000e4906d2039400e5082b40029001b400ed203a408a1003b4142d2319484a106090000000000000000062057405c10063400ad097ac858b02604048d0902c457b037a4094f026b401cd0030405030439c01270358408f1014188150000000000000e0003c41d3206fc01fe0364c01a
30130c01ff006dc09fb0073c09db107fc81de0a7cc09aa007ec0dbf0845c0df3005b8000000000000000064043c00db0013d00db0807c805f1035d00170027c401f0005c401f0037c80dd1837c009b0830c201f10165009f1005b010000000000000004057c01ef4058c4177087fc816d007ac0179407dc01e5006
ac016f007bc01ee007bc01e720f8d016f0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0520) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (44471110345431716d04078f004620810000000000000c2203c00f30410c0833001fc11ba407ac18b3241cc02fb00fcc03bf003fc40fd203cc00274034e193b105ed00bf000f08800000000000000c0007c00d70037c005f8037c005f2485c42df0097c029b0086c829f0007c00df0835c929f01
34c02172c17c129fe0070001000000000000062057c00db4037c009f0014c03db0016d00dd0075400d50017c00990027000df0036c1191407ec831d0cd5c0490000588150000000000000c2013400c900834005d20224090800a24010d1220400490002400150003440cd003202201007506314009040081000328
04000000000000040003404e9084b4006d) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0540) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (17c30ff0107c443f000fc4213050fc043f490ee061f870fc003f0006e0cfb013fc141b203fc0417201fc84362107b8050000000000000ac003c02d34584c00130105c20170196d0a030094c041b1134c101f0217402df1034c2413803441a130814c421f8806b000000000000000008043414c10
220502814503402850402400d14205406010102406490502008c980b05140100b04400515144281d04802010000000000000020007440d18024400910401404d501165005104244800904104205d0067440dd00344019110340801108144815d0c44a001000000000000080207420d14014040110a17426512086c
10010080501910086c879d0956400d9003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0560) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (40db80c3c40d90046c40d10443c031f0057c00df1035208000000000000006000d4b0110037490912034400dd0035402d50036500dd0037400d98047400d50004480d100470435d08c5400dd003528030000000000000e805040451c5324141104314c0cd0032020cd1230412c50033400c10007
400c90002400c100034140d8803400cd003100100000000000000c00054849103b7c0011013c44ef703b4401df00fc806fd2074c81d10047041d70044483d100c64805d0044c80dd007700010000000000000e200cc03a3013cc010b043cd0cff01be401ff013cc20d71077c81fb4043c41f3204fc30f31406c011
f004ec01db007fb0830000000000000e40) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0580) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00000000000000200c4000d0034400410030400c10033409cd1031420dd0033400cd8003480c9a080512c1800160215800140dd50030202300000000000000004d40003303d48091003d420f5203c401cd803dc00fd0037400d91007400dd0170001e100a74005d0297081dc0034a01700000000
000004000cc021f0834d0013003cd00d30037c429f2035c00dd0037c40d70087400df1436c00d30185c1a170295c00d710350007000000000000040217c003f083fc043f403fd80d70036c04ff203dc00ff103cc80f7b80fc00ff00fe400df2004c007f001ec00ff003d0181000000000000040000c00120036c01
031031c40cf0036c035d0034400d700374) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (05a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (ed0338464c10039400ed000b420e14039400e1201b4006d2038420ed003900130000000000000e2043c00130a34c01034134c84d30834c00cf0037c00f30072c01cf0007c00d20044c89f30043c005f0014e00df0035201000000000000004600bc003f0235c003f003fc08df123fc40ef003dc5
adf0a3fc08f70207c20fd283dc40df003f8405f081fc00ff02352002000000000000006048c014f0870c81030034c01c30173c05cd0371c05cf2173ca5c70173c29cf80f0451c34041c09470211c41c70170003200000000000000021948531007b401710079489e50b78405ed007b4c5ed027b401e9214f401ed0
378481e1014b6416d004b401ed01780002) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (05c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (026c019f0025001000000000000004004bc081f0007e001f0006d00070807c441f2005c801f2007c001f0407ce0170187c22170e87c001f8007c021f0805001200000000000004205fc00730014c00730014c005b0014d037d0015c00510014c005d009f6205900dcc0059405fc037d04d8d005d
0015800300000000000008004b410090032400010035400c90030400cd0030400c10830420cd0003400c980b1440c980b340fcd0120400dd0031281200000000000004000340121097041031027848de95270403fd0279401e10078401ed044b601e90c7c405e9084b4216d3058401fd0079080000000000000006
405f4002b203ac8021043840ce12038400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (05e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0106d04050104c001f1106c641f0007c001d0007c601f0005c04170106c00130004c001f0006001e0000000000000080414009105204008105234148505204009d05206148d00234008d00236008d00234148d15224009920214808d002000100000000000000000604809120205208100264009
520244009d00264009d00274009d00374409d80254189502a64449104644049d0024201c0000000000000000054008140244009100254009720245088d00244a09d00274209d00274009d01276029d00244128b10e54109d00242005000000000000042040c20970024c80930024c00930020c009f0026c008f002
7c409f0827c809f0027c019f0026c01930) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0600) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (74009d00276219d30244809d002528180000000000000480484148104a04009900a0414814720600dd00a00048d20234208148274808900274028d20234608d00204008d002100160000000000000c00605011b01c5405150006e4b1300c45001d8006c0b1d9007400110007400112006c801d00
074001d00044051d0007001c000000000000068070c00930164c02938164d05830164c00bf1164c898f002fc00bb8027c809b002ec05bf002fc00bf802e802af0027a0180000000000000cc077c14bf0527c14bf4521c14970527c00ff2027c149f0027c009f282fc009d802bc008f282dc14b6402fc14af0027a8
19000000000000086070c0013010480013) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0620) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (014005d00154a05d001c4207b0014400410014c007700174405f2015c005d105b6037d089c44471809c5207d00142100000000000000042050c201f0004c02170000c00130006c421b0004c001f0007c001f0007c001f0287c081f0404c06130004c001f0005001000000000000004215fc089f0
027c01970027c00970027c049f3027c009f0027c00972067c00970ca6c008f0127c209f1225c009f00250013000000000000040114c03939824c1a8900244008100244009d0024c009d0027e00990323c209b0027c009f11a74309d00245009f002520050000000000000620604108900254009d20244009910244
609d18264009d00274209120274009988a) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0640) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0cdb007fc01df007ec01fe227dc41bf0157c013b0a7d2002000000000000062043c02cf1137416cf0277c04df0035480cf0036c00d70037c00df0037c00df2037c001f0035c801fc003c001f00353814000000000000006050c01ef0078c45ef0078c71e10078c01eb007ac01ef007bc41ed007b
c41ef007b401ed007ad017100784812f1078181000000000000006201140cfd0339428fd013840ce14230400f10071400ed003b400e50039400eda03b440ed00384416100e8410bd003800000000000000000a0040620cd0034400cd0830480c10034500c90032400dd0033420cda033620cd20d3405cd8032423c
101704c11d803020100000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0660) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000060052c11f3003ec08f3003cc00f3003d400830035400ff0037c00db00b7400dd01b6c00db1175c119d00174005c00352010000000000000040008400d50032680d50032400d90031403c80033400cd0033400c520b0400cd84f20200d00934020d0403400150031200200000000
0000040002400f10b3a400f10138448e18339400b90039400ed013b428e9013f400ed003a40c6980394202c080b4002d01390104000000000000040054481c51372c08e5017ac01cb0275410cf0832c01ed017b40dc50179c41cd0232c454d101b4012d0d4b002a72071001500000000000004201ac03d302fcc01
fa1074c0dfc1375c01e3007cc19ff0277c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0680) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (950a33484c58133430c10236412cd10306040580134040104044004d22302810000000000000020004400dd2035400d50034440d90834404910034400dd1037400d14037400dd8064410110437401196047401550034280100000000000008220d500dd0036d80d10837c00d10035c00950035c2
0d70037400d10032400dd24e46031522874111104c04015d003620830000000000000c0200c20ff003c000f31034c40f34038c11b30034c00df003fc00f3003f800ff103dd0343800988033001cc003f003d00800000000000000c0017c80df2037c20df0033c00df2037c009f0032c00cf0037c20d70335c00df0
0a7c005f0937c061f0887c805720350001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (06a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00340011400420130000000000000c4514401dd1075c81d70074400111034441b500354015d0064401d54407401d500454019f0106c941120444011b0004080300000000000006000cc01ef0075c01ff007cc0107087bc00b3107cc011f006bc41b30007c01f3484cc001f004cc0112004ad6133
0047a0830000000000000ec017c14ef0236c04ef003fc88d7223d904bf013dc00d7053f880ff0333c00ff003fca21f010fc8417900fc047f0237a8010000000000000a6000c06ff01b9c00f70434c08e90234c0293003441cdf04b740ed34137606df82a448a110285cbe130005c085711b4180000000000000000
8041410cd08b3488c10132500c90033402) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (06c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0036c1a1f0126f08bf0035c00130867c4cd72005e10d70036c04970026c8a9501c7c081b0825000b000000000000000217c00ff003fc00f7003fd003f002cc009f003fc00ff003ec00ff011fc00ff00af4809f002fc203f010ec003b000d0181000000000000042210d00cf0035c20d72034c011
70022c01930031c000f81f6e11c73097c20d324c0c819d10c7801034003881030041208800000000000004000c400dd0035400d50034604910025401d500354049d08644c1d58007400d100144239500460439104054031d00452803000000000000048042400cd0031400c51030454458022480c100334009d802
2480d50203680c100044009d0403400118) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (06e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (38289f023cc00b3412fc003f00053802000000000000080048c01cf0172c00cf0370d0b0f2060c228f2231c018b8163409c340c5c25c30222c09860023c0d191143c240f00441036000000000000080019401ed017b401ed817840d39047c5092d20786016d034f405e1026b425e0007c401a910
6a401a9004d441210048000f00000000000008000c412cd8032400cd86b04001d00f04008d84314080900a30004120e540ac100826088502436000908834010d0000002300000000000000004d400dd0037400dd0034c001100e44008d00b4000950267402d203a6400d102b44438d02e442b91884580a112024a0
5700000000000004200cc00df0036c00df) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0700) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (4b400c50033400cd00316040d0066403898033480c508a3480cd01f3400cd80f3403c10635400d10030600cd01b52812000000000000040003401e5807b421ed20786113d806b4c38d807b4a161846f423e100c3401e590fb403a1406b401e1004a4012d8069000000000000000004004f400e14
03b400ef00396802d002ac08a9003b400e5002b400ef003bc00ed003b480e50039c00e110084002d00090017000000000000062043c00d30073c00df0036e001f0024c04bf0837c80130025c00531037c00df0017c00d30007c00920002c010f0005301000000000000006600bc00df0037800ff023fc00170225c
001f0037c08a7002fc00df121ec00df003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0720) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (409940274119d00a448091023640891002444491002420180000000000000800074029d00274009100224039320a44009d00274099101234029324234029d0024401914065d069120a74419108240001000000000000042043c009f0027c00930226c01938026c028f00a7c019f0166c05930227
c009f00e4d189b0824c30932025c20932025001000000000000006004bc00191007800170007c021f2007c121a0007c001f0007c001f1005c021f0407c80171005c2a1f2087c981f000500120000000000000e201fc00570017c405f0016c006f015d4007f0017c0a71821fc0073a05fc805f20dfc026300dfc437
3415ac037f011da0030000000000000420) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0740) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000c0063c00bf002fc00930028c08a3422cc15b3022cd00f3002be00b3136fc20bf002fc61b3002fc00b3002bc00b38227b0190000000000000ca067c009f0027c009f002fc54a7152dc00bd0526c00fd902b800bf052f4009f202f000bf0529c14ff002f420bf452fa01900000000
000008607bc005f0007c00130006d00114014e041b2007c001f0007e00590107c001f1004c04132806c00114015c00131006001b00000000000000a0534008d00234008140244009100206148d00334008100234008105224008d0020434c1002040081002740081802000100000000000000000734009d0027400
91042440a9100247029900276009508274) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0760) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (9f1425d019f0065c019f0167c009f0065c499f0427c049b2867c419f00e500530000000000000e2017c00970027440910026c189b0266400830024c098182634889b0127c809d00678009340a3c02930927c0991006320050000000000000600634009d002740095802740091102640095002440
095042540095e0274009da1a5000910467420950227600910024a01c00000000000004804b4008500234008100224009901264008100204208180374008900236808d002240289002740081002760081002300160000000000000c60734001d0007400158007c05110046c02150144c00158005c405503c74001d0
005c005500074401140074005141571018) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0780) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (05a481af01780030000000000000002801400ed003b400e1000a50075102840261001b002e5001c401e500ba401fd003b01061143b480e5008e4413d03380000000000000000040451402cd0033420c1ac03500cd00204044940f7421c10c1142fc504324c0cd0b33601c90073001c110f2501cd
20322030000000000000020011c007d00174005140d84026700984007300df40175001e44373801ec0d7d005f40071001f4417480586117d001c2100000000000000042043c081f0007c001b0207c201b0104c00130207c021b0087c821b4080c801f0007c02190007c18170104c221f0085005000000000000006
004fc109f0027c009f2027c109f6027c05) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (07a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000e41065000c408cd000a618fd001a58431002b404ad002b40c3d010b40425300c400b1033d0008000000000000044155cc18d017b409e14122c0d610342c05e3017ac0deb10d3c05c1087e40dcd02784536d0549c8d231102805210179001500000000000004010bc01bf027fc09d3084cc01f
7004cc09ff027cc01c70051c09eb5267cc1ff007ec09ef0247c09df084d40981007d3142000000000000040141c00df0037c00d70005c40b7000ed00db0017c00970017800cb1016c205f20174805f0027c001f0004c000f18352050000000000000004041c01ef007bc01e3004bc01ef0048401cb207fc01e3005
bc01e52062c21fd007bc216b006fc01210) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (07c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (5401091a06481134044421110036218f000000000000042210c20bf003fc00f3004cc01f3007e820f7008fc28f3005dc00b30029c00bb802f8017d042fc0033200ec403b003d00a5000000000000040005c029f1037c00d70087c101f0027d245f0006c10db00978065708a7c00df0326e061f00
87c00128007c241f00350001000000000000042053c208f0037400db0002c008780344024d0006c01dd0292c139300b7c008f00a3c015f00f7c101501a0c1003013d003800000000000004001b6000d0033400c90002400010002400c100026018500135020103526400d00014030d00c14130d044242101807728
02000000000000040003440ad013b404e9) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (07e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (14c109f1537c08ff000bc0c0f0201c409f0007c88bfc13f42c1b010dc241d0006c8c1b000ec0c37010bc083f6133a30100000000000000e003d029f05b7c00d31284c0e590295c10d78507c2a930315c0410110749e1b0806d041f1507c04130086c04130e3680030000000000000080434148d0
0334c0c50011400150105404c9003340481051240c41460244445040140c09090360d09008442411013020100000000000000200074419d0037400d10604604990115401dd08374809102154019182874811100444045d8407401191106411110834200100000000000000021c4059d1037400d500854819fa4c1c
01d904874019100c744551000440555044) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0800) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0400010000400010000400010000400010000400010000000000000000000000000800020000800020000800020000800020000800020000800020000800020000800020000800020000800020000000000000000000000000084002100084002100084002100084002100084002100084002100
084002100084002100084002100084002100000000000000000000000008000200008000200008000200008000200008000200008000200008000200008000200008000200008000200000000000000000000000000850021400850021400850021400850021400850021400850021400850021400850021400850
0214008500214000000000000000000ee0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0820) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000850021400850021400850021400850021400850021400850021400850021400850021400850021400850021400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000400010000400010000400010000400010000400010000400010000400010000400010000400010000400010000000000000000000000000010000400010000400010000400010000400010000400010000400010000400010000400010000400010000400000000000000000000000004000100004
0001000040001000040001000040001000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0840) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000040001000040001000040001000040001000040001000040001000040000000000000000000000008400210008400210008400210008400210008400210008400210008400210008400210008400210008400210000000000000000000020033800ce0033800ce0033800ce0033800ce00338
00ce0033800ce0033800ce0033800ce0033800ce0033800ce00008000000000000000000000840021000840021000840021000840021000840021000840021000840021000840021000840021000840021000000000000000000000000080002000080002000080002000080002000080002000080002000080002
0000800020000800020000800020000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0860) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000000000000000000000f0f00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000003c3c00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000420800000000000000000000000000000000000000000000000000000000000000000000000000000000000000000010820000000000000000000004000100004000100004000100004000100004000100004000100004000100004000100004000100004000100000000000000000000
0000001000040001000040001000040001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0880) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (fffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc00000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc00000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (08a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (008500214008500214008500214000000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc00000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003ffffff
fc0000000003fffffffc00000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc00000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc00
000000000000000000000000000003ffff) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (08c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000400010000400010000400010000400010000400010000400010000400010000400010000400010000400010000000000000000000000000800020000800020000800020000800020000800020000800020000800020000800020000800020000800020000000000000000000000000084002
100084002100084002100084002100084002100084002100084002100084002100084002100084002100000000000000000000000008000200008000200008000200008000200008000200008000200008000200008000200008000200008000200000000000000000000000000850021400850021400850021400
8500214008500214008500214008500214) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (08e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (8000200008000200008000200008000200008000200000000000000000000000000850021400850021400850021400850021400850021400850021400850021400850021400850021400850021400000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000400010000400010000400010000400010000400010000400010000400010000400010000400010000400010000000000000000000000000010000400010000400010000400010000400010000400010000400010000400010000400010
0004000100004000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0900) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000010000400010000400010000400010000400010000400010000400010000400010000400010000400010000400000000000000000000000084002100084002100084002100084002100084002100084002100084002100084002100084002100084002100000000000000
00000020033800ce0033800ce0033800ce0033800ce0033800ce0033800ce0033800ce0033800ce0033800ce0033800ce00008000000000000000000000840021000840021000840021000840021000840021000840021000840021000840021000840021000840021000000000000000000000000080002000080
0020000800020000800020000800020000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0920) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000000000000000000000000000000000000000000000000000000000000000000000f0f00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000003c3c00000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000420800000000000000000000000000000000000000000000000000000000000000000000000000000000000000000010820000000000000000000004000100004000100004000100004000100004000100004000100004000
1000040001000040001000040001000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0940) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0003fffffffc00000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc00000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003ffff
fffc00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0960) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (4184c2cb34070441af003c409ff0077c01df053fc01d110cfc21338d08c013e0047c01f3487f28030000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc00000000000000000000000000000003fffffffc0000
000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc00000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc00000000000000000000000000000003fffffffc0000000003fffffffc00000000
03fffffffc0000000003fffffffc000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0980) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (ec19ff040fc023f00cf800ff403d0085000000000000040200e00de0034401550007800d70071c01df1030c80cf0037e00df0037e00d340c7e001144444010f0047c00d10035000000000000000004000c1861c0035403110086480dd00d6420110036400dd00374c0d90037400d100e7440d190
444021d0007400d18035a0030000000000000480404020d84304801501076008580314801d0030484c52033400cd0033480c101074000100006201c0003480c1003320130000000000000c40040001d00354041b0286c0ef30016400110a74c04dd0077401d700fdc01d120064011130c44941d0047400d1007708
0300000000000006020cc001f007cc29b3) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (09a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (080056d0179401ed034c401e9036842135807b408ed017b401e19273401e1004b421218648401292b4b401ed8078809f00000000000000800c4000d10314004510034009800224008100b3400cd0033400c18033400c580000230500034030d2181420cd0032a80700000000000002005c42fdd8
e354004f2000c809160144004506bf400dd0037400d1003f400d12023401d100e1c091d2057484dd1030201b00000000000004001dc02df0034c02934054d00d300b6c00530037c00df8037c00d34037c80d60005c081f0085c8a1f0085c00df08350003000000000000040207c01cf003fc007f0a4f84093481dc
09ff003d500ff003fe00f7003de80fb002) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (09c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01e1027b401e988eb403f10073401a1004f621ed0079000100000000000004004c4004d08384806f0808c08bb202c400b1013ac00fd003b400e10432400eb002c440e1000b680a1400b420ed08388813000000000000042040d00170034c00430004c25d30834c00970031c01d70037c40d340f7
c00d31026c01d34047800971003c00df0037a01500000000000004600ac08fb003fc005f000bc08f6023fc003f143bc4cdf0037c00ff0037c00ff003fc04f710178001e022fc40df023db802000000000000006048c018d0171c00570163c018b0072c04030033c01cd00734a9c30973c09c70125e41c71001c010
f05c1c00cf007010120000000000000002) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (09e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000042040c02930164d009300a6c408e0024c00938023c009f2027c40970025c00932827c409f0264c01930124c01970027081000000000000004004bc041f0005d081b2007d20180007c10170087c001f8007c001f1006c001f00068021f0087c021b0207c001f0007001200000000
000006200cc137f8016c0b71001cc0057115c7017f0016c00578817e0051001704053001fc007304df4427300dbc005f001588170000000000000c2048400cd0036400cd00444008d0070408190032000c90033400c10033400c90161413c1017361bc1a483400dd08332812000000000000040000401ad007a401
7100e0400e500786012d807a641ed007b4) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0a00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (b70027c149f0027c409f0027c009f052fc00ad002dc14bf202fc149f0027b819000000000000080068c04130004c40130105c04170004e80130107c001f00074001f0106e00134007c40170106d00534004c00170004101d00000000000000a0404148140306008105614148500205008d053360
08d00234408d0523600811023400cc25204009900314018d002020100000000000000000604008100244008110254009500204009100274409d00274209d0026400910023400d5002640491002440495002420180000000000000000045019108e4400914024c809500244009500a74009d00274009d0027400911
0274029d14a54028b20254819d00262001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0a20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (020d00930027280500000000000000807032095a0264109181a44009511264229d00244009d00274009110274009100276909c0025480990035400910025a8180000000000000480586168d04226248d012040281012244491202040489002340081002340089a0274408d882140091002440481
0023a0120000000000000c4060483170140501130a445051740044011f12846011d0805c001100874001101474001d0005c001b0814405110007081c0000000000000c0060c05be002cc489f026cd0dc300a4c0883016cd888f002f600932567c009b00a7e00bf002e800b3002cc08b7402f80190000000000000c
0067c14bf0d27c14bf052ec34bf052fd14) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0a40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0030400c51031400c91060400c10033400cd0033400cd0033401cd80f3460c14142401dd0032a034000000000000000002c0573001ec005f081c48075201c40051815c4007100174005d00174805d0014c077d005c5006f005d0657d00100104000000000000040140c44130004c001f0046c001
71004400135004c00130007c801b00078401f0885c821f0404c181208868401f0005085400000000000004014fc00970425c08970023c00934025c009f2423c209f0025c009f2023e409f0127c199f0266d299f0226c209f40250057000000000000040114c329f0026c029f00644008300225008308244408b002
7400934027c809b04634839f2924c20930) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0a60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (c4038d0c68c1d11021b407ed01719815000000000000044108c29930054c09f3005ac09db0176d09df0267c1bff027fc09d3027fc09d31a74c0d9c027da4d73004bc09ff0077a802000000000000042152c001f4017c40df0020c00d722b6c80f70023c00ff2833800df0837c00df07b5c000f00
34c00170803c009f0035b810000000000000006043c01bb006ac55f7007840be7057d423e90048405e1007bc01ef007bc01ee0879c21ef207be01f3086ac01ff0078103400000000000000200340061207a408ec003d404ed0139504f90028400e1007b400ed003b400ed1138481ad843b4002d8088400ed203880
04000000000000000043401d900b2400d5) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0a80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (07c000f1027c00d71027c80df2034c00df2027c40d31037c00df0037c00df1137d829f1015c22170447c009f00370001000000000000040040400d34037c0efa12e4501f3247e402f50021400fd0037420d30037c00db4c7ce118e00b74019940474009f0035801c000000000000040008001810
012401cc00c2401c904f0446c10020400cd0033400c90033400c100704220c01404200900036009d00332006000000000000040010404a1110b400f9041c410c1a038404f50329000ed003b404e1013b400e9033840cad111b60429000b404ed0239001800000000000004015451da12176c05ef001ac49cb03784
09e301eac01d2027b465eb2173005e3007) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0aa0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (06dd04b6426dd013ed001b000749213a886c345709369003000000000000008042488092022400c10023450cd0934604d94131410cd0632618cd0333602cd243240c1108036460d0085404cd00b02030000000000000020004488514a12440c100e1600c50034400d90064480cd0037400dd0036
400dd0032421198937401110046401d50034200100000000000000220ec26111046c00d10005c80db0032d00cb40e5400dd0035c80dd0037420d50034403110c474131f00c14011d18362003000000000000040200c20fb006cc00f3001c900f3003cc00fb002cc00f7003fc00ff0837c20f1003cc50bb006be003
3000cc203f083f01810000000000000400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ac0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000689434c0cd00304084d0030600cd2032410c994304000d0132440d500334044d00014008d00011001c0843428c9203120130000000000000c0507401dd00744169d0874041dd0075406f30136c01d10135c01dd01374121700444019f00c44611c1107441d10037000300000000
00000ec00fc01df0074c043f003cc01df0076c14db0074c0133427cc01df127fc103d004dc01af050e4012b00cfc00f3003da8830000000000000ea007c0037018fc20cf000dc24fb073fc02ef10bbc00de0135e00ff0037808f7203dc062f2207c441f000fc801f21bfb8250000000000000a0000e104b0306814
f30295c0cf500b8680db002440aff10374) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ae0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (f90034400dba037400d72477400990064403818066c020d2017005f5003c201f00000000000004000fc00df0036c02330037808df2035c00df00344085f8037c00df1037c00df00a7c009b40a4c045f0017c00d308350827000000000000040607c00ff003fc093f0037d00ff003fc80d7003fc0
0f3003fc40fb003fc403f002fc04ff0005c003f124fc00f740390081000000000000040213c00df0034c031f0834c00cf0036c40db00344124f0032c00df0037c001f00c58009d00c5c025f0807c00db0035098000000000000000000f400dd00344c0dd2034480dd0035480d100304c0dd0035420dd0037400150
c444009500444001d0017420d900352803) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0b00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (011c01c30235201000000000000004200bc00df023fc2cff0035c00ff2237c00ff023fc04e30237c00df003fc881f202cc08b7203fc00bf2037e18ff423d280200000000000000005bc8dcf2072c87432033c01cd1071c05cf02749018d907340dcf0033c004f0123c188105a2c060d0003c40c3
0034001200000000000000001b401ed007b405a90078401ed0078405e1007852de9087b401e5807a41129006b649b1104a4013d005b481e50078080b00000000000008010f400cd0033410110033412cd0831420d520304108d0033400dd00334110906c140581014240a0d0003407c10030200300000000000000
214f400dd00374001b003dc00dd8034400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0b20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0014d005f0015c005f0015d016f0017c005f001440871205dc805f0c1f4077706ddc4053201520030000000000000c004b420cd0030481cd0032400cd0831400c50030401c10033400c10031400814471001c104b30058d08f0600c980312012000000000000040003401ed0078401e90270401f
c2079405ed1078401ed107b401ed8079521f19069411bc287b48165007d401e10179000000000000000004004f400ed0038400c50138400ed0038512e72038400e7a03b620e3003bc002b0028400e7200b440ab0018405eb003d1813000000000000042053c00df0034c01f30074c40df2034c00df0035c00df003
7880df00348400100458019f0007c00530) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0b40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (3400850523400c1082741489052020100000000000000420634009d002740a9d88244049d20254009100264009d00274009d00244109500274c49104274009110274009900242018000000000000000005c009c10274039d00244008d00244009100204009d20274009d00244039d00674409500
634239150234009160242001000000000000040043c009f3027c019f0026c009e0025c00930026c099b0027c009f0024c248f0227c809720a7c05960027c45930821001000000000000004004bc001f0007e10170804c001e0006c40070007c08170007c001700068401f0286c02172087c82192007c001f000500
1200000000000004000f4005d0014f127b) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0b60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (634001d00045070f0084d00160005c0f0f01444001f0147400170547608558007600110005c401b0046c021131c708180000000000000e0063c009f0024c15bf0464800bf0024c4d932025c00bf00a7c009f002f801bb002fc00b7002fe60b300a4c05b381e7a0190000000000000e6065c009f1
027c94bf0025d00af0027c14860527c00af1527c009f0d27414bf002b400af002fe80bb052f000972527381900000000000008006bc401f0007c041f0104c001f0005404130006d001b0007c201f2004904172007c00530107c40131007cc45b0107101b0000000000000000434008d00234148d05206008d00204
548940204008d00236008d20204148d003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0b80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (801f0005c061d1007c211f0807c021f0007c50130004005000000000000004014fc009f0025c10870025c509f0025c00970026c209f2027c80970027c019700e7c029f04e3c009b0a66c408f00250053000000000000040117c009f0026c009f8024c008c1024c009b0025c009d1827c209f0027
40a9100236409700e74009f1966c0091002720450000000000000600734009d30264289d0024400d500254009d20215009500274009400274409120a74409010254029d1027400d15025081c00000000000004805b4008d00226108d20204009d00204808924214208d21234008d01230008140264208500634008
d01224028100a100160000000000000400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ba0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000000043c01ef007ac012f007bc21ef0079c03ed057b881af08fbc01ef0068d0137186b4812d287bc81af207bc0163007c1030000000000000000003400e5003a410ed083b480ed0038600ed02384403d013b600ed8028491ed002b400e1043b450ad023b402254a38080000000000
0000040043600cd0032403c50033402cd0031400cd08330128d0833400cd10a0203c503b3401cd00f3404cd0037443c1003420300000000000000028034005700145027d00174917d00144007d801cc8267801f4405d021c4017d101f4057700df4017c00174007118142000000000000000040043c801f0004c00
1f0007c001f1005c800f0805c801720078) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0bc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (c50031601851033600c500014091900c34000d08434080584764000980352002000000000000040013404ed003b4002d033a448ed2038400e1003844ca1023b400e1080b48021022b4002c001b488ad2039400210339008c000000000000040157405ed037b4004d017940ded007ac00e5003fc8
9852837400e5000dc042b120b4226d262b4882f043ac002b0179105500000000000004210bc01ff0077c01ff007cc09cf007cc01f3007dc0d91007fc01fb0a4fc01f3026bc093c027fc09bf227cc89730075a042000000000000046053c00d70035c00bf0837c20df0037c12df01bfc0007003fc00df0026c001f0
027c401f1037c209f0037c001b3035a854) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0be0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (037001110034200100000000000000020f400d70037401dd0035401dd0835420d100304538f0036400d103c04811d01074a11980445051100370211500362083000000000000042203c00ff003fc017f003ce00ff003cc00e3083cc10bf103fc00f3001cc003f040fc003f08ecc003b003fc2013
00350081000000000000040007c00df0037c00ff0835c40df1037c00ff003f8029f0037c00df0005c009f00a7c011f00970129f2037c221f08350021000000000000042043c00dd0037c00df0036c40cf0034c00f3003c533d3203fc00d30017c01930467c019f0037c018d007dc8013083d200000000000000004
200b420cd00334060d0833400cc1032400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0c00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (007cc03c30074c248f0047c0037007dc001f007cc01df0074c0143004bc01f3007fc01ff00770003000000000000066007c00d7003fc043f1037c90bf00b7c00fb003fc08a7103ec00fb000fc003f100f8203b080fc803f203fc003f123f38a1000000000000080003c16df05b7c001f05344105
f00b4c02e140bce089f00b7c08d30014c001f0007c001d0004c001b0037c00130136180300000000000000804340ccd03334880d2131404cd09b1408c100b04809d0232440c140000000920024200d000044001003340005113020300000000000000a8007400dd00374049d28346215d1834400d10035408dd003
7400d108144419d20676011d1436401990) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0c20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (fc847f000dc00ff403fc00ff003d80050000000000000e2208d00934057c20530020c40d34054d081f00c7e0d070035e03570034c20df0834c10431843c00d10033c00d70037888200000000000004000c400513037400d18014400118034400dd00664405508374981d1036400dc00354005900
c4400d10837400dd0837880700000000000004004c414418533480c1813640401853041ccd0823480050037400050030400c50030600510005400c90133400c5003120140000000000000c600c400410037490d10514404d100344029d0044c49d50075c00170076c01dd1075421db0044481db0537401dd007708
010000000000000e040cc01511077c01f3) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0c40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (3c4216d2169485a9201c401e90069441ed806841da90078449adb17b401e9017a40979025e401ed217b401ed0178800600000000000008008c4825d0027400898070404d901a7400dd0020401090836400890033401cd0030480010102410c90033600cd0032a00700000000000002004c4869d0
2d5c015101844411900544015c01646235140344091d0037402c90036c035f1127c22cd0837400dd0034a0130000000000000420acc049f0057c01530126c011b1056ca55f08a4c00132036c485f0037c18df0036c07530004c00df0037c00df00350803000000000000060017c80bf025fc027f000fd00ff225fc
003d000dc70db003dc0037003fc00ff003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0c60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (813d007b401ed0079431711048001e1207b401ed0079000000000000000004684f400a1100b40021000c400e100084006100284008f003bc40ad2039c00ed0038520610018c00e1003f400ed00390813000000000000040043c00931007c80170824c00d00044d80130025d001f1036c00af0037
c00df0036c00530002f01cb0037c00df0035201000000000000006200bc085f032fc00b70011d083f0926c08ff022fc08f70031c201f203f800df003fc207f091fc00ef0937c08ff023db0020000000000000840c8d014f0163c058a8330c010b0163e01cf0160401cb03728051f0273c01cf0170c05430340c01c
b0033c01cf017010120000000000000820) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0c80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000042043c01930064c01930026c009e0024c00930024c089f0026c009f0027c019f0825c109b0267c00972027c009f0027081000000000000006004bc10370487c80190085f00170407c10170005c02170007cc81f0007c821f0004c001f1005c021f0007c001f0007001200000000
00000e201fc025b4097c02530016c00534094c065b091cc007f0014c016f0017c005f0015c0073401cc00534017c005f0015a80700000000000004005b40989000b40631000e440290008401591030400cd00334010d0031000cd0031403411110400c10037400cd00312812000000000000040013481a9284b401
21006e401390048401490868601ed20784) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ca0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (bf002bc00bf0027c14bf0027c00bf2024c00e7002ec00bf0527c009b0027b8190000000000000ac07bc20330002d001b0006c001f0800c041100044041f0004c041f0007c001d0007c401b0007e001f8807c001f0006b01e000000000000008053401a1902c400a90028400ad0068414c1002465
48d00216149d00234008d00236009900274008100234008d00202010000000000000020073400b1802e404b9402e400bd002c4089110344809d20244449500274009d00276309900a74009d00274009d0024a01800000000000008000f40a935360c009101a44048d00a45029b42207138d00254019d002740c9d0
0254008100624069500274809d00262001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0cc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (823ca09f0027a005000000000000040063400dd00276009d00247009580244009d0464404dd2024680982027400dc08274849918246009100274009d0025201800000000000004004b4148d85234148d01204108580254988d00214028d00204148d80234008d00214008100256209100236808d
0021a0120000000000000c60734811d08474011d0045401140044c071d00044221d000450f1d18074001d0007c001b0006d001009474001d0007081c0000000000000e0063c00bf082fca0af023cc00a200adc05af082cc25bf002c801bf2027440af0825480a30028c00b380a70009f1027aa180000000000000e
6067c14970525c14972527c948f0527c14) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ce0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (08724124c0034683451270400cd0033413890030405cd10304064900434034d0033640cd003228140000000000000600504007d001c8805d045c4037d001d41b7d001ed027d00174027d00144237d281440061109f4467d201f4005d0015a014000000000000042040c001f2004ca01f0004c001
f0004c00170084c00170007c481f0004c001f1004c221b0287cc01f1007c001f0005001400000000000002004fc009f0027c009f0027c099f0025c009f0027c518f0027c008f0027c209f0027c819f0427c109f4027c009f002480170000000000000e2017c009f8827c009f0824c06851825c498f20e5d139d082
4c049f0027c009f0025c809324a0480810) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0d00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (84052b20014850d117b400cd11798855000000000000040003c81b70277c01ff227cc01df207cc017f027fc0ddd027cc01af0077c09ff027fc0953004cc018f007fc09ff0077a000000000000000062043c008e20274009f0005d001f2026d805d8837c009f0037c00bf0035c00df0037c801f00
07c005f0837c00df0035b8100000000000000840449016f007ad01ef005ad016f0058c01670878401cf007bc01ab0878c01ef10784016b084bc816f117bc01ef007a1015000000000000082004403fd0408401bd002a4102d24294006d0038400ad803b400ad003a611fd003850030200f4006d023b400ed203a00
05000000000000080050401c50032040cd) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0d20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (07c825f2887c00df0097c805f2097c085f2037c00db2035c019f0037c409f2035c061f01d7c001f1037c00df003580010000000000000e2057c05df0035c00df02345005d1034c815f0c37409cd0034c018d20358209e0035c049100c44000c003ec00db0037a8350000000000000400134868d0
0234008d00804008508224004d00634028500334008d00304000d10304810900a04000d0033480cd003228040000000000000404034002d0129400ed01186006d12184006d003b480ed0138404bd0039400fd803940071020c5042d023a620e901390200000000000000046057409ed005b4088d006850da7036ac
002d122b4558b2173c85ad0b70c013d203) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0d40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (165d8db78065f00349021f2007e1c178837c08df0136b00000000000000000a1434904d3111480c100024048d01004000d0021442cd01314849d01b34b20982300061d00804040d0133400c9013022100000000000000208074809d0037404d100a04019d0224406dd1234401dd00344031d0037
4019d00344511d0107403150037400dd0834a0010000000000000802174021d0485ca1910014c014704d44e24d18254019d10354019d00374015900344030904044411d1037400d900362081000000000000042213c0077001ec01b3023cc007f005cd015f006ec80bf003cc00be003fc007f083cd0037204fd003
e003fc00ff003d08800000000000000600) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0d60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000c8043400cd003140209052640085003041051000340c850800682010480444011002404011000702011002400014003a010000000000000042017401df1076403d310044461500744048108544069b2245403180184c0a150246c081b02c44031102c6c0a132287080100000000
00000e800fc01df807dc003b0062c3c3f403400133204dc48a3410ec043b010cc0c33010ec8633000cc0432000cc0433010fa0030000000000000e2017c001f030dc24bf0085d08a70307c14bf002de0c3f1437c149f003fc001b213fc022b000bc843f10b7c00f90e3fb8050000000000000ac403c0c1f0286c68
934124c0a1f0304c22df02a64069f05344) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0d80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (d10032c82db0c06400110027c009104444201b00a2c015118a4400110014201300000000000004200fc40df0034e00330025c12932037c00d30027c04d30002c02070020c00830086c02131224c86430820c820300910803000000000000040a1fc00ff003ec09d7002fc011f4037c00ff403ec0
0fb0447c41170465c019f0043c011f1067c007a04678011720150187000000000000042403c80dd0035c211b0166c01172030c40c302e5c22d73206c8a134224d08930286c0a131224c02534224c0a131097080000000000000002201f400d50037000910064418950034600d100954029d0405410190006420150
4064100980044001500064101910058803) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0da0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (070e00d70037a01500000000000006400bc08fe023ec28df023fc00f9113dc00ff003be411f0037c0cff0017c0075013cc00ff001f80897001fc28d7002db80200000000000000404bc01cf0171c08c30171c01050171c00430033e01031032c00c40010c004b0131404c90012c009b0010408cb
4160101200000000000002001b401ed017960961c17c405ed927a401a1007e405290078400e1045b409690379401e9025a441b90658409e9426880060000000000000a011f400cd003340001803140315803140001003264a114070500c14050700494431520c9d49240a894090780c98022a00700000000000000
004f400dd00344009102a04139a203c400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0dc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (14ded21730016c0073021cc457b0014500570094c02515014d00530096405530094d00570015a8170000000000000c204b400cd0030440c10062481cd0032413d100b2400552030400c50036420c10030500c141b2440c90030400c10277281200000000000004000f401ed0078441e9086e4414
14072401f1207c421690078401e5007a401e10079401e0007a4a1e10078481e50079000300000000000006204f400ed0038c00434028400af003ac00e1803ad00774038400c50032c00cb0030400c0203ac00ea0038400c1003188130000000000000e0047c00df0036c01330024c01330276c00c3c076c0053003
4c21d30034c01d30036800db2034c01d30) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0de0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (9634a5252b614ad052b414a1052820100000000000000280634009d0027440d1c2276849d00256009d1024404b5002f400b9102e4a0b102ac400b1052f498fd102c400b9003420180000000000000800074009f00274009b14236039d08e4c009d00244509180e34009f00276009540e14009100
674229d11a54009140262001000000000000082043c209f0027c00934067c019f20a5c009f0024c01970267c00950027c00930024c009300278419f0164c008b002708100000000000000c004bc001f2005c001f0485c08170005c081f0007c023f0007c001f0406c101f0005c00070003ca21f1407c001f000700
1200000000000006205fc005f1814d007b) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0e00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (704001f00074001341456571f0005c01130005d031520874021500c6c0b15028680f1c0087d02110284c1f1182c3181c0000000000000e2060d00bf9827c01934028e05b3402bc0093002cc19bb046bc119b04eac0393006cc099f046cc15bf006ec01930067a8190000000000000e6067c00951
027e00bf452bc14bf0027c14bf002a4149f1023e009b0527c149f0027c149a0823c208f2025c149f0527b81900000000000008c073c001f0007e041300074041f0105c001d0804c04350117c44131107404130104c04134107e041d0104c041b0104101d0000000000000000434008d0023434890023614cd15304
008d0020714a1052b414ad052a494a1052) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0e20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (20170804c00130c05c20132406c401f0a07e401720050814000000000000040157c009f0027c009f0427c028f4023c02974027c008f0426c00970027c009f0023c008f0027c10870421c009f00250855000000000000040014c009d0027c009b00a0450930027c01934026c009f0027440938026
c00930024c009f0026400971026c0091002520450000000000000600604009500274049100a54409d802540091202540095002740095802640085082608099002440091203460091202580180000000000000e80404008d00236238984204288100234148100224048d00234008100264048100206008c00224008
40022484916522a0100000000000000c60) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0e40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000004053c01ef007bc01eb0078c213b004bc0ded007ac0183004b401ed0068c09c30863889f1307ac00cb0030541f341781014000000000000020013400ed003b600e9483e442e9400b404ed003b610a9040b400ed000a60ce5002b444e50070402e90039604e51138800400000000
00000a0053400cd0033440c94070622c902c3400cd8032481810032400c900e4400c18233400c10232401c920b0600d14036a01400000000000000041340047001740051449ec017b001f4205d80114007b001a40051461ec0055009d4005b10dc44071001d4005500142004000000000000040153c401f2007c80
131084c841b0407c001f0004c211b2007c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0e60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (d500334128d0003400c50003400d90000400cd0002000098002400c900332806000000000000040000404ed003b404e94028418310218404ed003b404a90108400e10013400e9002a400ed0038400e90008400ed00390048000000000000062056c05ed0171c09eb422940145014ac8de7037ac5
3cf124bc05ed000bc00fb0328c60ec008a800e9023ac20e1203188150000000000000e0008d01cf0277c09f3006cc058b0240c11df0074c29f3024e809db005dc01f30268c01ff207cc81e3007cc31f7187fa002000000000000066043c00d70037c00d70037c00bf2007c06df0035800bf0006c00d30006c06ff0
005c48fb4034c20130035000dc0f35b810) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0e80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (036400d10034200100000000000008020dc00dd0037400d508e6c018f41c6c80d30036c819b0405400db0005420db0046c00d502c4c001d00c5440d5003600830000000000000c2203c00ff003ec10f3082ce033b014ce00ff003cd009300c4c80d70029c00f300afc00d7800fc09ef90fec80d3
003608a90000000000000c0005c00df0837c00df48b7c10970087c00df0036c028b0081c00cf0004c00ff0023c00ff00b3c02d70087c00c700330009000000000000062050d00df0037c42db00b4c01d30000c00fd0477c02db0004400db0027c00fb0026d00ff0034c00d30034400ff003da8340000000000000c
201a400cd003100bc94185400058012406) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ea0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (407cc0199002cc0037082fc001b007ee013f0077c41f3213cc01d3004fc00df007fc01fb0075a0030000000000000c4017c04ff01bfc00df002bc003f5b0fc08f300bfc049f0087e00fb180dc00fb000ec20ff000fc003f000bc00ff203f9805000000000000084003c16df0136c50d302264181
b0304444ef8134c14970004410d50017400f14007080f12006c001d0806c20d10a3e1003000000000000008841408cd0333604c500324040d0022400c1013260c090001404cd0002400c18000400c500004000d8000400c5803000100000000000000a8007480dd0037400d190f6480998024400dd0036401d5000
4400d10017400d10887400d100364101d0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ec0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (7c0077204fc00df003fc00f7403d80050000000000000e2208c40d18032c00d30034901934004c031c00674011b0036401570037c00d34035411db0013400d70037400d10037a80200000000000004000c400d10034400d10034401d500205489540234a31100314111d0037400d500354815d02
37400dd0037400d10835a003000000000000048040400c10036408c110304949120a0458090123400090033400450033400c50231400d90037408c50033400c1003320100000000000000c4404421d10134c03f10074c009315a44269b0427400110037c011d0077401dd00ffc41550007483dd0077401d1007718
010000000000000c800c541f040f4404f3) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ee0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1b401ed0078601ed0079009fd04384456d826b40521057b4a5ad027b401e90078405fd0058605e9827b401ed007a080600000000000008000f400cd02b0612cd00336208910204004c01234870500f34000d0373400c98033601cd8111400c58030400c50032202300000000000002004f400cd0
0f4400ed0830d00c50064401dd00364835108b74009d0077400d1003c4210d00d4400fd0037400dd0030a01300000000000004200fc00df0436d00df0034c00d30004c10072027c02171437c02df0037800d32033c0adf0075c00d70035c00d300350803000000000000060017c80ff003cd00df183fc00bb0667c
01db026fe0037003f840bf103fc20ff003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0f00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01f10079401e90178401fd0079401c11079401e10079000400000000000004204c500e1003b408ed0038c00f10928400f1003ac006d003ac00eb203b400e10131400fd0018480e10039c00e100399813000000000000042040c01d30037c0cdf0034e00d20004c01930024c001f2034c01530073
c40db0534c00df0015c09fb0073c00d30073a01000000000000006600bc08df0235c00ff003ec00450637c445f02268003f023fc00df083fc00d74477c00cf003dc08fe003fc08ff0035a00200000000000008604bc01cf0170c00cf0373e49099160d104f0a23c15070177605cf0173c01cb0933c01cf0031c05c
70270c00c7007210320000000000000800) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0f20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000042043c00930264d009f0024c009b2027c049f00a4c049f0067c009f0027c00910024c81930465c209f0027c209f0025081000000000000006004bc001f00878820f0005d881f0007c101f02068821f0007c001f0087c00170005c021f0087c001f8005c001f0005801200000000
00000e201cc00530017c005f0014c00712198d00734015c006f0014e02730017c005b5010c007d091dc005b4015c005340178817000000000000042058400c10037400cd0030411d104a0402c10073207cd0032419c91033000c90031409cd1874400c10031400c100332016000000000000040010401e1007b445
ed2078401e10148403a110214030d00784) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0f40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (bf052fc14bf0527c00a70027c009b2827c00bf1d3fc009f0027c009f1027a8190000000000000ac07bc00130000c445f1004d00134103c041f0104d041f1807c001f0007c00170104c00130005c841d0007c001f0006b01c00000000000000a0534008140304148d0020400810527414cd052041
49d00234008d0023480854520400c140234148500234008c002028140000000000000200734009100244009d0024400d102a7000dd08a44029d02a74409d01274009500244049100374009d00274009d0024a01c0000000000000800074009100a44029d00240009110ef4039d00a44219d00e74009f0127400910
0245008103a74009710274009d00262001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0f60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (027c009f0027a8050000000000000400624009480264009d002440891a0244209100264049100214049d00372809130244009d11274409c00254009d0025201800000000000004804b4008d0023402cd00216108120a07028125a04469101234008d00214008100a06009d01234028d00234008d
002000120000000000000460724001701424001d00044051041444071340c4424114107c005d00074801100845001d00474421d0005c001d0007181c0000000000000e0063c00bf00afc01bf002dc009300ecc07b3002cc06b300afe009f002dc4093016cc00bb022fc059f002fc009f002fa0180000000000000e
2067c008f052fc009f0027c14b7052fc54) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0f80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0032400d11234400cd0234400c10bf3480cd0273400c10033510c100f3460c90033400cd0032a0140000000000000200534007b041f402790016d0051005c4007d001c40065409f4205d08df48055081440571005f4005d00174005d0014a014000000000000042043c00130007c001f0004c021
30006c001f8806c001310078021f2007c00134005c80120107cc01f0007c001f0005081000000000000002004ec00970426c009f0027c019f0027c00870025c019f0027c409f1427c009f0023c229f0027c009f0027c009f002580130000000000000e2017c209f0027c009f0025c45930024400930224d0693002
74029f0025c00914024c008b08a74009f0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0fa0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (b40321204f40ded0033405ed0179101500000000000004250380173205cc011e007c801fb027c809ff226cc01df0247c09ff0077c09f3027fc017f0057c01df007fc41df027d2000000000000000062043c005b0007440db0035c08e50025c001f0015c801b0007c00df0037c00df2035c004f80
1fc00df2037c00df0035a810000000000000084047c016f106bc016f0078c01e3085cc01fd0058c0173007f601ef007bc01e3007380163405fc01ef007bc01ef007810110000000000000820074006d007b42069003a400f918284c06d003854265001a400ed003b400e5003a040e1045b400ed003b400ed283888
010000000000000800534404d00b3610cd) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0fc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (07c80570037e028f0037c00d700c7c0e9f0217c221f0007c00df0007c80d73037c025f0207c00df3037c00df003700010000000000000e0057c005b00364001d0034400f180b6d039700365121d0027605df0027400d9c037c0e5b4087c00df0837c00dd0035a815000000000000042013400490
0016000d0031401c961204430100404021d0003013cd1003400c90033400000907400cd0033400cd0031202400000000000004080348069211a408ad0038450f1000a400e5000a4642d010b404ed001b608e9093360061001b488ed003b404ed0239080000000000000004205740d41086fc07ad0033c01eb0a70c
016309ecc076d0043409cd0b6b40dc1817) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0fe0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00dd2017e04df003441613011740cdf18b7c00df0136a00000000000000000a0434044d81216044d20334c0c5001054081a1136100d0a00604cd0102418cd343040c010143400cd8033400c9033020100000000000000200074005db014401dd0037400d920b44148122334011d0007440dd0067
400dd8034400510047480dd0037400dd0034a0010000000000000802174005d0005481170035e00d74084420112004c011d1187c00dd00d7480dd1036d03050857600dd2037400dd00362085000000000000040213c007f102ec009f003d400f30010c0073402dc101f024fe00ff003fc80f7803cc0433001fc40f
f203fc80f7003f08840000000000000600) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1000) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000e8043600c14221402818802400c50001400c100016004d4012444c10132420c900024088d00324040500014600d0007a0100000000000000c2007401d100a5402110014424db0045c00d500544a1554004420d50035404d500454201d0074c00110003c81110017000100000000
00000e000fc01f3012ac0013000ec49f3184cc01f30049c014f4042c09ff027ac89fb000e5043f007ec0333104fc813b000f80030000000000000e0017c0c5f0307c08f7053cc02cf0707c081d0204c003f018fc18df048fc04df2037c001f020fc2cff053fc08ff0b3788050000000000000ac003c0a5f2316c00
5f00b7c0ed30184c84430127c2e1d01076) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1020) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (db0072e01510027400db00b7c40db1036e00d30034400512006e01118014205300000000000004200fc00d70026d08330307c08df0287c80d320e5e00570017c20d30636c00d30880d02df2035c00134084c40130005080300000000000004021fc00ff022fc81cf0017c00fb154d000ff007fc8
07b002fc00ff003dc00ff0847d003f003dc803b000dc0033281d0187000000000000042413c00d30825c81124046c00d600c4c00c32425c004f0056c00d30036c00db0286c011f0036c00170845c031f0105280000000000000006200f400d10025404902054400dd0807000d50114440550060400d52836420c10
4044148900364100500476011d20048803) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1040) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (005c0053004fa01500000000000006600bc00ff0227e00b3013fe00da100bca0ff033fc2c5f223fc00ff0237c00f7002fd40b3003ec00ba020f5002f4001b80200000000000000405b801c70560e05cf0aa3e01cf21c3c2dc32373405470073c01c30033400c501004009f0031c0011000141005
0000001200000000000002001b441e1026c4092d200b421e5814d401e9013a41561004f40de98079401e908ea001a1007840925804840931005c80060000000000000a010f400c500244004d0047404dd8003410c10133405450003400d108b7400c540004068d0031600050005401050806800700000000000000
014f400d102c4c01d10857400d10001c00) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1060) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (001fc005b061fc205f009ec006f01ddc005d0017c005bc8dec107f0016c0173001dc017303dda8170000000000000c204b400c90452406cd1033600c108f3480dd01b0500450035400cd0033400d10070401c50032409d900f1605c90073281200000000000004000f401e900ea5016d047b441e
0004f401ed007a4416d0079501ed007b401e9805a401fd007a401310049601710009000300000000000002204f400e1002c400cd101b400e1000b400ed0038440614038400fd003bc20e10030400e7083ac002b08084002b081d80130000000000000e2057c00d30024c405f0007c00db0003c00de0036c005f103
4c01df0037c80d30054d00cf3034c200b6) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1080) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (2614cd0023400852023400994d2000100000000000000000634009182204028d00254009120a74029d80244089520370409d30254809d22244008d002660091a030488dd00242018000000000000080007400914026c039d1025c899b00a04039d0026e019100270009f80244609d0026c029d10
2540095802540081002620010000000000000c0043c80930064c089f00e7c009388264029f00e4c01970027c009f0825c009f0064c009d0024c00938024c019f402308100000000000000c004be00170085c081f1007c00174007ca01d0005c001964064001f0005e401f1685c40170007c001f1606c481f100700
1200000000000006005fc005b10dec827f) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (10a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (734001701c0d17171146c011700074851300044201309434011d00474051c8005c011d0005c011121444001101c3181c0000000000000e0063c0093046cc21bf00efc82bb002fc02b3002ed00b340afc029f002fc009f0069c07bf0027c02930824c00b3046788190000000000000ee067c009f0
52fc14bf053dc149f282cc149f102fcc08f252fc549f0527c349f002fc14bf0025c14bf052dc80e7052f98190000000000000a4073c00130114c041f0105c00110007c001f00144a01700034201d2015c401f21144041f0006c20110000c001f4106001d0000000000000080434008105224148d05214008900234
00890022600c100234008500200008d052) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (10c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (001b0406c00134005c121f0004c02138807c001310050054000000000000040157c00970561c10971267c009700e7e00934027d809700e7c009f1027c009f0465c019f0025c019e1027d049f106500150000000000000c2117c009300a4c109f00274009f2067c009b0022c008304e3c009e0027
c009d00e7c188f0027c38934264c82934027200500000000000004a0634009500a44008588244009908a76009508244009100274809c00274009d0a27000dd08254009004204009102a1a0180000000000000680434008185204068d01a34408d20274008900264408101230808d04214108d80e24028d80234008
50420440810422a0100000000000000820) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (10e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000004053c01eb087ac217b407c401ff005b4016f004b4012f047b621ff0068c0ef31049c017f0078d15e5247fc01a941781034000000000000020011400e90008400e980da41121800b400ed10ab40029003b401e50028404e1045b5026d0038405f5613b400ac0138800400000000
00000a0053400c90072402c980f0403cc8233401cd00b3406cd0073400cd0220400c10031501cd0030400c5a033400c90032a034000000000000000011c0051045cc2071109e8237100db4447d00df63271045d40057001c40053001cc017d00144805300174304510140104000000000000042153c00130884c00
130404c501f0407c011f0107e00174085c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1100) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (9d00405000104f3400d90003420c900c24004d0030403c901324078900332806000000000000040003404e9020f6166d0008080a1128f6082d0208400314c3b420ed1019400e9000b6006d0039400f1003c400b901390018000000000000062055c05cb0043c00e7204940d4f0343648cd000040
921113a42ccf080b480eb040840c6d0038400eb063ac58ab057d08150000000000000e000bc41d3227fc05f70054c21fb0007a097f007cc0123007fe19ff025de41f3004cc0b6f007dc11fb007cc01a3027f2002000000000000064041c00d70037d00170007400378803c40df0027c00172134d00df2007c40f70
004c025f0037c20e34237c009706b5b010) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1120) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (034400910030a00100000000000008020dc00d10034412910056c00950184400190035c091a0077c00d90005c00d90606c035d8035400d1003540185003620830000000000000c2203c20f3603cc88bb003ac08b3100ce883f015ec0133007cc00ff002ec00ff0404c00ef003cc10fb003cc05b3
083f09a10000000000000c0007c00df0305c02df8017c029f28c7c021f0037c021f4036c00d70027c00ff0005c025f0037c20ff0037c009f01370001000000000000022053c00db08b3c01971034c00932003c009d04544000300b3c00ff0025e00fb0006d00df0035c10f300b8c0393003da83c00000000000008
2019400c90003601151a414001d0003400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1140) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (007e8012f0049c01fc087dc01df0047c01f30077c01ff187dc01ab8007c8147006fc01df007db0830000000000000c4017c06f700838143f020fc1407140bc843b210dc0217002fc04ff000fc00fb000ec003f003fc00e7003bc00bf02359805000000000000084003c04db0084c421b1004c021
b000442a1f1006cc61300aa400df0014c00ff00044003d0034400fb103c48093213e1001000000000000008041406c901845c04171024100d44005204982434280940a2408c90001400c900026400d0031400c980354009501302010000000000000020007600d900344001100444101900444105d000640219112
6400dd8014400cd00046011d0034400c90) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1160) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (ee00b30007c097f102fc00f7803d0185000000000000040203c00d70034c00da0034c111d0045c00cb0035400df01d7e20d32037400df0835c429b0147c03574027400dd0837208000000000000006200f000dd2034400dd00350019d0064400dd8035480dd0066400d92037600dd003700a1100
50450114027400dd0035a007000000000000040043400cd0830400c980314a01d0001400c80831400cd0803420c10033400cd0033600014012480050023480cd003320130000000000000c0407421d90074401dd00754011d0044401dd0074694d92057421db0077681dd0076401910804101510027401d7007700
030000000000000e200fc01f5087cc01de) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1180) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0b401ed007b481ed007b48df5015b401ed007b401ed017b405ed017b405ed007940131007841b21826b405ed0178001b00000000000008000f400cd0033400cd0071448110083432c52073400d58003400cd00b3400cd00304000100f2400810067400cd0030200300000000000000005f400dd0
037445cd2036c039901a7411dd8077440dd2027400dd04f3400dd00354805504d54020104f7400d70034280300000000000004001fc80df0037c40df1236c461f0427c20df1237c00df0027a00df0135c00df0037c001b2406c02130937c80df20350007000000000000040207c00fb003fc00ff803fc003f000fc
40ff003ec00fb801fe00ff203fc00ff003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (11a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01ed007b401ed00784033108ea401ad107f401ed0079000000000000000004404f400e90039c00ed0039400eb101b400ea0038400ed003b400ed003b400ed00394002b003840021002b400ed00390033000000000000040043c00df1037c00df0034c010f0007c00d22070d00df0037c00df0037
c00df0034c001b0026400934827400df0035301400000000000004600bc00ff0237c48ff023ec04db203fc00ff223fc00df003fc08ff0037400ff003dc001f003fc0018082fc08f50235080200000000000000004bc21cf0073a01cf0031c010f0243c01c70073c81ce004340dcf0171c05cf0071c210b0052c0d8
34027c05cf017000120000000000000002) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (11c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000040043c009f2027c01930167ca1914167c239f0164c809f1025c209f0067c009f0824c209b0a66c009f0227c009f0025001000000000000004004bc001f0007c801f0005c02130007c001f0005c001f0607c801e0007c001f0007c001f2047c00170887c001f0005001200000000
000004000fc005f0017c005f0016c017d005b4405320160005f009fc005f0017c005d0014c0063005ec407d005f4005f001520030000000000000c004b400c90031400cd1033401c921f3400c90032400cd1033000cd0033400cd0031401091070400190237400cd00312832000000000000040003401ed087b401
ed087a0036d20fb481e1007b401ed007b4) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (11e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (9d00268548f002fc609f102fc009f0026c00af052fc00a5152bc009f0027a0190000000000000c006fc001f0007c00134007c00178807c00570004c001f0005c001d0007c001f0004c001b1900c60130007c001f0004001b00000000000000a0434008d00224008140236008100234008d002150
08d00234008d00236008d00215009105224009180234008d002020100000000000000600634009d00274089100274889500a74009500240009d00254009d02a74009d80244009900a04039140274009d002420180000000000000000074009d00274009100234459300274c09d00654808d00274009d00274009d0
024420914026c039101a74409d00260001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1200) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (027c009f002521050000000000000280734009100274009990254009908274209180244009d08274009d00274009c00245849100255049180274009d0025281c0000000000000c805b4008100234008d00234208d00234008100214008d00234808d00234208500205009120214008101234008d
002100160000000000000c0063440110007400190007a001900074001100045151c00074001d00074001d0004480110bc7c001101474001d00060018000000000000062067c0093402fc00bd002fc00bf102fc00bbc02cc009f0023c209f002fe009b0027c008b436dc00a340af8009f0027b0190000000000000c
0067c009f0027c409f0027c40bb002fc00) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1220) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0063403cd0013409cd0032000c10033420cd10f3420cd2030440c180d34000d0076400cd003020100000000000000000034005d00134005d081f40179081f4017d001c0207500174005d269d8005d101448055001d40f61115f4005d0014a000000000000000040043c001f0007c081f2007c981
530c7c801f0006c001300868001f0007c801f2004c02130307c00131006c001f0804005000000000000000004fc009f6027c009b0027c809b1127c00970026c209f0227e809f0827ca09f0027c009f0263d409f0267c009f002500530000000000000401174009100274209d002740c9d0467c80910021c008f016
7a009f0027400970027c068b4425440930) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1240) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (040dc58418c0521087b400ed007118b500000000000004010bc01df007fc09b34867c09f30254c01af007c901ff1277c01d3007fc09d9007cc01f3205bc81230277401ff027da042000000000000046143c00de2037800df2027c001f0817c001f0037428df0037c00df0025c00df0037c00df04
05c00130003c00dd0035a054000000000000006053c21ef207bc81af206b48127006bc01af007ac01f3007a801ef287bc01ef0078c01e2004fc812f007a401ef00780010000000000000000003400ed003b600a900ab440a9801b4002d0028004e5107f000ed003b400ed8038500f560094002d003f400ed003800
00000000000000002043400cd0033400cd) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1260) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (87c20d70037c00df0035c109f2085c421f2026800df2036c00d78087c00df0035c00df0c97c021f0037c00df00350001000000000000000073c00dd1037480934033c52900c06c809d0035c20ff0477000db4027c00dd2036d01d10815420120036400dd0035a01800000000000004201b400cc0
0314008100230034500524000d0831400dd04f2420c91003000cd0032008c50030402014007400cd00312022000000000000040433480ed003b600e1012b40061828e400ad0039404ed033b400e9221f488ed003a404f1001940ca1103e400ed0139000c00000000000004205740dcf0373c00e101698054f03d04
020d0220505ed087a401c10b7b42dcd003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1280) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (04df0517c06df8236c96df409cc80110127c0add0334110100000000000000a053490cd11b36008151334000d13034000900a0484c90a3340cc50113600c10031406d500926040504224c0cd05302a30000000000000000007400dd0036400d102274819d08474009d1234400d10037440dd0077
400dd0036500dd0456502510067400dd1034200100000000000000060f400dd20374089100274011d00674001d0064400dd0037480d701c7400d30035420c12056c02050046400dd003400a3000000000000000207c00ff003fc00f3007fc803f002fc0437002cc40ff103f880ff002fc00fd003ec00f12018d153
3003fc00ff083d01810000000000000400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (12a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000e804f400cd1033480c10712400c91031488cd0032440c900124005188264210100324008d0031080c51002480090037a0100000000000000c200f401dd0074404d10083d01d100744160d0065481d100554011d00544011d2877cc997007402af10044400310077080100000000
00000e000fc01ff0076c09f3010ec01db007dc043f006ec01cb005ec013b007cc203b203ec84bf007fc04ff000ec0033007788030000000000000ea007c04ff8137c14ff022bc181f800bc143f002f90ccf213fe26f70503c16f3013fc00cb201fc921f000ac00ff0137a821000000000000004007c0edf04b6c02
930027c001d1487c021f0024c0cd70537c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (12c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (5d0036c01c10177e009d8024402d9103fc01dd0034601fb08144001d0034801300000000000004200fc00df0037c10d300bcc00d30134c001f0036c10d70117c005b0225c049f1035d089f0035c20ff0014d000f00350003000000000000060017c00ff003ec00ff024fc00f7003ec007f006fc0
0f7001fc00b7003dd00ef003dc019f203dc00ff0019c0017403d80050000000000000e2003c00df0037c00d200c6c00cb0031c121f1026c00db00528034300f2c00930036c019f2037c00c7c146c131b0036a00000000000000006200f400dd0835400d14003400d10035400dd0135600d108744039d00e64015d0
036408950034400d10046401190035a003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (12e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (802ca55f0037a01000000000000006600bc00df0035c48fb001fc28cf0331c00df0237c00ff423bc00df002fe80ef003ec00bf003ee10f3001ec00bf0235a00200000000000000404bc01cf0373c08c70150c01c30072c00cf0030459c70213400c98031c00cf00304008f0031640cb8011c200f
0072103200000000000002001f401ed007b401e5117a409e9007a4492d007a405e102594012c2078401a90079401ac0079489c902594012d307a08060000000000000a001f400cd0033400d54020404c182327041d0030403c900934000901f14828d20304008d0831448c920014800d0036282300000000000002
004f400dd0037c00d10426c00db00b4410) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1300) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (409ec00530016c03734017c4057005bc427b001ec027b1014c005f0016c005b105ac117f001788170000000000000c004b400cd0033400c101b7400c10033410c10033400cd6062424c10172440c50830401cd0030400c936b0452cd20332016000000000000040007401ed107b401e1007a401e
1007e401a1007f441e540df411e9047a403c91170411ed007a465c1005e4014d0079000400000000000006204f400ed003b680e10031400e10038400c1003b440eb201b000e10838520e708b8620ed0038008e14818408ec083998130000000000000e2057c00df0037e00d3002cc00d34035d00930077c20d3001
3c00db0070c01d30034f00cf0036c02fb8) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1320) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (34148d00214148985274348d002028140000000000000220634009d00264088100364009502244109920274249940264009d02274009140260249d20254309100274009d0024a01c0000000000000800074009700244069114255008101a04039d00274009b0024c008d20e7406911027c019d10
254009300274809d002620010000000000000c0043c009f0024c00930026c00971025c089f0027c009b0824c009f0067c05970020c018f0024c02934027c009f002508100000000000000c004bc001f0007c021f0005c001f0084c080f2007c001a4087e001f0005c121f0007c001f0007cc0075007c001f000580
1200000000000006005fc005f0017c0053) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1340) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (734001d0004d010505c450011400648b192005c801100074005d00174021700074401d000740b1100044411d0007101c0000000000000e0063c009f0024c02b3016cd00a3402fc01bd0025400b3002f8009d082ac01bf0067c00bf0026c27b70466c019f0025b0190000000000000e6067c00971
025c149f152fc00af002bc14be002bc8093403ec00bf002fc00bb0025c00bf002781497002fc14bf002780190000000000000ac073c001f0006c00134106c00170005c84192007c805b0006d001f0017c44130106c841d0805484134107c441f0006b01d0000000000000080434008580225008105216008120207
148d00234008900314008d002261481052) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1360) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00178104c001f0007c001e0006d001f0005c020f0005081000000000000004005fc009f0027c009f8067c009f4026c189b0125c009f20270829f2227004970827c839f0027c009f5065c009f00258013000000000000042017c009f0026c009302e4c00830023c139d0025c40920267e009d00e6
c019f20258019f0026c00970226c409f0027a8050000000000000620634009d00244009500a44009180274009980254209150274209d00274209100274009d0027440d100264029d802520180000000000000e804b4008d00224448102204009180274b48d80234208000214c08d00234028d00a14008d00234048
500664128d002120320000000000000c20) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1380) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000004053c01ef0078c01e30078c01eb0048c01ff007bc01e3005bc0165107ac81ed007be01af0078e01ff0079c01ff00780011000000000000020013480ed0038410e14821402692088401ad003b4006d002b08060107f4218d003b642ad003a411a1003c400ed2038800100000000
00000a0053400cd0830481d106f0400c90030402cd0033011c10033600458af25048d0031401cd0030440cd1031400cd0032a0140000000000000200534005d181440071009d5017b00dc40277001744275045b4007100dc4057d00174087d00144017100104005d0014a014000000000000042053c001f0004c00
130000c00130904c821f0007c08132187c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (13a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (4d00334200509234014982005014580334000d00324009111b3402dd00312016000000000000040003404ed003a484ed0018400a1000a400ed033b42821012f40c6d0238400f1003b4002d003a400a82c3f400ec10390008000000000000062057405cd0078c01bd0292c052f03c04092d007bc0
d65056b6156d000849865003b4002d023ac0ca0233b400ed003910110000000000000e000bc41ff207cc019f005cc09b30048c097f027fc69931067e897f007cc01e3087fc013f007cc09fb027bc01ff027d2002000000000000066043c00df0037d007f102fc005f0003c00770037c0093c023c205f0034c005f0
037c009f0034c009f2033c08df0835a810) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (13c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (035400dd8034a001000000000000080007400dd00374001140074011710c44011d1035c129500670805b01d44130d003744119003680b111034400dd003600850000000000000c2203c00ff003fc01b3115fc00b7024cc009f203fc00b3882fc8077001cc09bf0037c003f003dc005b003dc00ff
103f08050000000000000c0007c80df0037c007f02afc00170005c00bf0035c205f0027c845f9127c02170037c001f0037c029f0037c04df00370009000000000000062053c00df2036c005f1074c00930006d05df0037c00130023c035f00e0c00930037c051f0034c20db0033c02ff0035a8140000000000000c
201b400cd00304004d00164000d0002400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (13e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (2067e143b0034c0037000fc013f0076c61df050fc011900cfc01f3004bc01f30004c0033d87fa0030000000000000e6097c16df0537c003f010fc0c0f0307c081f0237c043f022bc085f000e0003f003f4003b003d80033003fc00ff103fa805000000000000084003c02df01b7c14930287c849
70304d049f0137c14132027c20550014c009f08364001f0035c001d0035c00df02b6a0010000000000000000c3404cd04334440100234080501004840d013140c4500234844980045000d90334010d0032400850034400cd203028100000000000000a0007400dd00374061100274019500044084d0037404190c6
74005500644009da0364011d0037400954) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1400) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (fc30ff005fc00ff0031d01df403d80050000000000000e0003c00d102c7400df00e760b1b10b0d01130047c011d0035c00cf00c74101b02c7480d241c3c00d30075c1a510037a8200000000000000ea00f400d50817400dd00674105124244115d04616011d0036420dd00c7408d10007400d111
37400d100c6400910035880300000000000006a043400c10203400c580234000100044000100034000d0031400cd0403400498103400c10007600c16003400010033a0130000000000000c0007401d500c7401dd0027403110034441170005c001da034c01dd0187400910007421d11057481d10006401d1807708
030000000000000e000fc01d3010fc41ff) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1420) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1b405ed016b401ed014b441e9427b401a9104b405ad017b409e9004b409e108fb405ed225b405e90258401ed0178800700000000000000000f400cd0103400cd00634020101f24028080c34008d0032440c94000400c10007400cd0103401c950107800d0032a00700000000000002004f400dd0
1334a0dd0227487db097d4024b00e74049d0077000d500a5c00d104f7402db084740bd124546004d0030a01b00000000000004200fc00df00a7c00df00a7e22d34024d07572387c101f0035c00d301065005b4087c00d30057c08d300a4c22df00350803000000000000062017c00ff003fc00ff002fc31bf0177c
00170805c203f003cd20ff000fc01bf000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1440) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (21e90052481fd0048401f900cc401f50042451610079000100000000000006004f400e10031400ed0038000c10038400a5001c400ed0038400e10038400ed0038520e10018500e12018c00e1403988130000000000000e2043c00d34016c01cf0034c00530234c00938004c019f0036c00cb0054
c40df0004800d30000d01d7081cd00414073a01500000000000004200bc08ff003fc08df023f488ff213dc007f002fc00df0037e20f70015c08f7103fc00fb8817c00d70a1fc00df003db00200000000000000004bc05cf0173c00cf05e3401830272c04470003c878f0470c0dc92054c01d10287c05cf8803c25c
b40404000f017010120000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1460) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000040043c00930063c20978164c05934264c05830063c499f0024c809f2264c009300244089b0025c00930062c008f002708100000000000000c004bc001f0087c401f0287c421f4002500140087d121f0807e001f0005d001f1487c02174187c001f0007c001f0007001200000000
000004005fc005101dcc005f001cd1b63105dc047f029c4867d8816c004b019ec206f201cc005b009cc4057281ccca730815a81700000000000008005b400c10471400cd0470420c104f14014d0050482cd0030400c101b2600cd02f0440c98050400c113d0400c100332812000000000000040013401e10078401
ed8078481e100f94614d80d8441bd807a4) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1480) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (ff052fc14af05274009f052fd14af053fc00af402fc00af052fc00bf0027b2190000000000000ae073c00134107c00150014c84531104c04530107c001f80044801f0104c00130004c00130015c00130106c441f3006b01d00000000000000804340081052340081002641485052041481cd2340
08d00214008905204009500254408900234008505206148d002020100000000000000220634009102374009500244809100245009102274009d00244009d00a44009100244009181274049102264009d002480180000000000000880074009104674209080e2c029500244209101e74119d00254009d20e4400950
1214068f08234069500244009d00262001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (14a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (4a041b930027a8050000000000000400634009d01b70009100274009502264409101224109d00274009105244049c1025400910025480d90024400910025881800000000000004804b4008900234008949234808521b240081c422414cd01234208120204408d002048081e02244089012040281
002328120000000000000c0063400150007460110107400154096c001100044001d00074001340044001d0005400111005ea01141c4402114005001c000000000000062073c0093802fc00b300afc40b780adc10b3042cc00bf08afc00bb002cd009f1028c00b3002ee00b344ecd05b3002fa0190000000000000e
6077c009e002fc009f052fc00fe0d2bc00) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (14c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01f4413cd41b74d2c104f1602d10073401cd80b7400c50071403410013080010071600cd0032a01400000000000000004340051415f40051401c5337f109f40271419c4007108574017d005f44071021f4016b009b06071001c4005d0010a014000000000000040053c00132042c80130a84c821
74087c0a1b1085c90130007c001f0007420130085c20132007c09130884c001f0005081400000000000004005fc00914027c009700e7c039f0827c018f0025c019f0027c009f0467c009f00e7c909f0527400970127c408f40248017000000000000040017c009900274009b0127403950066c08910426d0a9f802
74009300244008f00e4f009301264409b0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (14e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (8c094901585058d0128605ed0371881500000000000004001bc09d30077c01ff007cc49d30244c01d30053c017f027fc0993405dc09df0067c01de015c501bf007ef01ef1077a002000000000000064043c00df0037c00db20070009f0036c001700060001f0027c00df0017c04db0017c001f00
03c00df0026d40df0035a810000000000000006053801e3007ac01e7007cc21cf007bc01a3805dc8173407fc01ed087bc09e74059c21a3085bc01a3407dc01ee00780015000000000000020013420e12033600e50018401ad0833400e100284006100eb402ed009b40ce500db49068008b4006180a9400cd103880
050000000000000a2043400c10073400c5) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1500) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (17c00df02b7c40df0205c041f0a37e009f1086c0a1f0027c00df0007cb0df0405ca29b2486402df0027c08df00370009000000000000060053c00d300b7400df08a48139110a4c009900674001d0037400d18025460fd08354000f01c48000d00f6c00cf0035881400000000000004200b400c50
103400cd01874030000e54290100c3406052027480810981480cd02024004c10014004d06e4400cd08332806000000000000040003404e1083b400ed0009408218100480a9450e4006d013b640a10009604ed2009400ed200840c3d0828406ed00390008000000000000042057409e50243401ed00994058102e94
03ab014a44d0f206b485ab0351421fd184) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1520) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (a8dd0086c12ff0004d00930004c061308a4c34df07b6b001000000000000002043404cd2403444c500006420d012144409000260c0141a3010c90201486cd01004a481c1104904d0821504dd013022100000000000000a0007400dd0037400d180644119500644011d0407401150027440dd10c6
400cd0404421910474401d91126440dd1034a001000000000000080207400df0087400d520444011b00754811d00874d1110027400dd0045400dd0045413d51040401d70064440dd103620210000000000000c2203c00fc024fc00f3102cc00830c3ec008f064fc00330a3dc08ff0006c20ff009cc00f3200cc00b
3007cc00ff003f08010000000000000c20) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1540) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000068043400cd0033400cd8833400cd0031400c10033620090035600cd0003400c10813408c10002408c50033480c1008100130000000000000c2007401dd0077401dd1077401dd0077c01d50074481d52064400dd0af7429df42d7cc3d30046c03d702f744bdb00e7000300000000
00000ea00fc01ff007fc01ff007fc01ff007cd00f3007ac212b006dc01ef010fc04f3001bc00f3000cc24ff203fc80f3100f90830000000000000e2017c08f7050bc08df000f4063b822fc003e008fc201b0127c00fd0207e40ff208fe12af0087c1447042e800df003fb005000000000000084003c0adf0187a04
d302a4d061712a4c141d1107e121724a7c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1560) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (f100b2c11dd00a4400d11a84400d11126c00d90034400950034400dd2034a81f00000000000004000fc00df0035c00df0837c00df0034c10d70037c061f0034d04d34084c8093081ed00db00b4c008300b6c009b10250003000000000000040217c00ff003fc00ff003fc00ff003fc00cf043ec0
0fe08afc00ff00cfc00ff081bc0077006fc80d420ffc005f005d0081000000000000040203c00df0037c80df0837ca0df0035c00d30037c130b0061c80df1047c12d12017408d340c2c10d700f7c00d1004120800000000000000e000f400dd0837600dd0037440dd8037400d40035468d50024400dd20b7400d10
015480d10216448d50037400d101252003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1580) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (044c00d70815081000000000000006600bc00df003fc00ff0037c00ff0037d08fb013fc00fe022dc00f7003bc40ff001fc00fb003ed00ff0037c00ff002d280200000000000000404bc00cf0031c00cf0033c08cd0030c00c70331c00cf0032c00c30000500c34010400cf01a0c00c34032c40cf
0010003600000000000002001b401ed007b401ed007b401ed007b401e5043a609eda06a401f90078409410058401cd0078489e50270429ed1068009f0000000000000a201f400cd0031400cd0033400cd0030401c50030402cd0622400d10240400c10010400cd0000400c11032420cd2010202300000000000000
004f400dd0037400dd0037400dd8037c07) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (15a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0017c005f0015d005f1014c807f015140053001dc017b01dcc1b7349dcc017300dcc0377009da0030000000000000c204b400cd0033400c90033400cd0031400cd1031400cd0070400d104f1508c92060580c104b0412c14af0593cd20b12016000000000000040003401ed007b601e9287b401e
c0079609ed0078401ed0079601e12079621890058401810078401e100604038d0079000000000000000000204f400ed003b400e1003b400ed0038420ed0039400ed0038400f140304406140194006100385006100184206d00190213000000000000060053c00df0037c00d34073c00df0834c00cf0034c01cf102
5c00d30074c00d30010c00930010c01531) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (15c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (149481452341489052241481052000100000000000000000634009d00274009d80274009d00264009d01274119500a540099002441091002441091002740099043643091002428180000000000000800074009d0025c009d00274009d80244029d00676039100e4c809d00254029100254029100
274129900a440293202420030000000000000c2043c009f0027c009f0027c009f0026c088c2027c009700e5c009f0024c00930020c00930027c009f0024c009b042500100000000000000c004bc001f0007c00170007c001f0006c021f0007c001e1087c001f0206c00070407c000f0003c0a1f0107c000f000100
1200000000000006201fc005f0017c005b) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (15e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (734001d00074001720074001700045001d0006c4017000440117108f442110086c22114084c42110006c2a1d008700180000000000000e2063c009f0027c009f002fc009f0024c00bf002ec00bf002dc02bf0067c01930064d01930064c11931464c819f0077a8190000000000000ee067c009f0
025c009f0027c009f0025c009f0027c00bf002dc54bf002fc00bf002fc00bf002fc00eb082dc20bf403fb8190000000000000a407bc001f0007c001f0007c001d0006c051f0007400170005c201f0104c04134104c041301074041b0106d04130106001b0000000000000080434008d00214008d00234008d80224
14cd00634008120224208d052141481852) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1600) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0013000ec00130886c00130004c08130804c00030085081400000000000006005fc009f0027c009f0027c00970027c009f1025c009500a6c00970027c839f0122c408f0061d029f4022c899f08250a170000000000000e0017c009f0027c009f0027c009f0024c008e0826e009f0025c809f0827
c03930425c02930a24c029310a5c029f082520450000000000000600634009d00274009500274009500244009c002646095002540095002f420b1402f400b100ac400b1102f480bd083528180000000000000e804b4008d00234008d00234008d00204008d00224008d00216008d00ab483a100a9403a100a8400a
10069601ad20a100120000000000000c60) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1620) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000004053c01ef007be01ef007bc01ef0078d01ef204ad01af107ac01f10058d0143007ad01430072c01634052d014900700014000000000000000013440ed003b400ed003b400ed00385808d84384007d003a400e10052403e10020402e1003b400c100ba402e92078080400000000
0000000053400cd0033400cd1833400cd1030504cd00b0603cd09f2400d1c010401c10030401c14032401c10072401c8103220100000000000000204134005d00174005d00174005f00144007d025c42c6d109c4057190144005340144205100154404100144005140142000000000000000040053c001f0007c00
1f0007c001f0004c081f0006c001f0206c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1640) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (c52001483450003600cd04114020504234060500b24000900074040900b32002000000000000040403400ed003b400ed003b400ed0038400ed001b4002d001b400e504594002100334402d403a50009020b4002111390008000000000000062057400ed003b400ed023b400ed00385006f0a09c0
06f002b442eb001acc0a5102b404ab0038408ab102b400ab023900550000000000000e200bc01ff007fc01ff007fc01ff007cc21ff007fc01bf007fc01f3005cc01b3007fc01b3007cc01b3006fc01b3037db002000000000000046043c00df0037c00df0037c00d70037c00df0027c00cf0835c00df0015c00570
027c005f2035d005f8015c00570035a010) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1660) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (025420910014200100000000000000020f400dd0037400dd0037400d7003441091046740d9d10555014500274005b01074005100854005500174005100942883000000000000040203c00ff003fc00ff003fc00ff003cc008700cfc11bf083cc80f30227c1053001fc00730600c40732017c8073
081101a9000000000000040007c00df0037c00df0037c00df0037f021f08a7c021f0047c405b20a2c01df0283c01db0085c00cf0077c21df21950009000000000000040053c60df0037c00df0037c00df0034c005d0003c135d2027c00d700e5401d30017c23dd01c6c00db0077c03d304d520300000000000000c
001b480cd0033400cd1033400cd0030420) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1680) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (507fc01510064c20178874421eb503fc011b070fc00130247c0013004cc09b700ccc03770057a0030000000000000e6017c00ff003fc00ff003fc00ff003fc60ff000fc003f000fc003f002fc003f400fc003f000fd0037000fc003b681fa8010000000000000ac003c00df0037c00df0037c00d
f0834c00d70017c001f0014c00910027c001b0017c00130004c001b1005c001100168101000000000000008043400cd0033400cd0033400c100305004100034000d00004200500224008900024208100006008940274008500102010000000000000022007400dd0037400dd0037400dd0034404d500164001d046
44089100a5480990017400914084400998) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (16a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (fc0057080cc02b7000dc107700ed00850000000000000e2200c00d380444005b0026d01511024d03090034400db00334015f08c7c531d08c38931b0845c929720c6411570055280000000000000000000c400d12015608d90035401110004401910834440d100354119d80476011dc4474c11d80
45400c90462501810435a803000000000000048040400c11200424c9102204001000442019f8304a0c100336440d20034000d8007400090101400852002400c50023a0130000000000000c6004401d10585600d100654205b00644a1332036c01d90037c1451088740911100740115040450091210048401051308
030000000000000c020cd01d30104e6873) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (16c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1b40ded876a61185027a68d7d806960921c67840de5807b429e1205b68121006a40d29134940d610248405a14358801f00000000000008000f400cd00404010d80200425510224920d80b4403cd2033080000842402050043409090105040814000441410052a00300000000000002004f400cd0
2b6c80d700228809d0021c841202b440ec7103f0009103e54031102a4401516464545d14314400910000201300000000000004200f4a0df08a2820df0034c24970c66c801f4034c00df0037c009b4084c481f00a5c00130004c10d34004c88d30825080b000000000000060017d00ff00bfc00e540bec407f016fc
0013203fc40ff003fc00730003c3033002) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (16e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (03ed005b601ed007840129084c641e1004840369004d000100000000000004604d400fb0030400a1002ac006d082bc00410038500ed0838400ed001b4006d103840069000840061000c400b100388813000000000000040040c01d34014c00131035c004f0024c02534074d00df0234c00df1017
c805f0004c80034004c00d34806c00930037a01500000000000006000bc08dd023fc00ff0227d002d2207c02f5023fc00ff0237c08d7023dc20c7282dc0077021ec007f00174003f002db80200000000000008404be0dcf01f0c008f0230c21070042d0d4f2074505cd00734050302c2409440767c09092145c2d9
31000c05c3056010160000000000000820) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1700) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000042043c40930225e00930024c019b0064c018f0165e009f0024c109300a4c81800064c88830024c00930026c009300a7081400000000000006004bc001f0085c001f0006c101f0047804190007c401f00068201f0107e421f3287d40170806d401f1187c20174007001200000000
00000e201c88051225e400734010c027f1019c01770016c004f0015c017f01dfc137f10dcc0773009cd0463249c8097b01dda8170000000000000c0059040c130f2500c1a073401cd8032403c50030420cd1031401dd0037406cd0474413c901356004100545800904032816000000000000040010401f100fa401
8180ec483bd10694b165a07a601fd21794) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1720) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (bb052bc00ae0226c14af052ec00bb052fc00bf1529d14bf052fc14b7052bb8190000000000000ac07fc80138107e44131004d00134004c841f10054001f0284800130104504570004d04120804c00030005c801b0006101800000000000000a05340081052341481402042081802651489102040
08d81210008105214148500204148520204019500214018900200010000000000000020073000910423600810024400910024508dd20254829d00245409100244249502244109104244209110255008980202018000000000000080007400914065c009100254598116e6c209910644009d0024400914425402914
1e44009540a4c009509a54029140260005) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1740) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1a5c0593042508050000000000000000634009514254409102244909100264009100244809d00266009d00a440899002760095002a440bd002c400b10a25a81800000000000004804b4408110204028140200448900271828100244409c05a24809c10224008d902340085406b404b58139404a1
0027a0120000000000000c2072440151807497110004000172017c82114106d00114146c255d0004400190007442150548441110144401004143081800000000000006a067c00b3002ec84b1202dc82b3803ec04a340acc20b141644029f202ec00bd102fc11b70025c089308a7c289300afa0180000000000000e
0867c009f052de14bf202bc54bf002fc80) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1760) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0010201dd0070404c90070402cd0033400c902b3411cd20b3481cc2072400c10034400d180b2a0140000000000000200534005900dec005d201c402790a1c09373111c4017c201f40071009e4137d081f401750056c80515014400510010200400000000000004004300013148440a1f0004c3a1
f0004d001b20044081f0007c00130107c001f0487c2013400cc483b000cc22330185081400000000000006004e4009f00a7c828b0066d039700e7c218f0027d10930027c039f0025c008b1027c049f1125c40930265c039f002500130000000000000e0017c009100e6c06930060400914023c9b9300204008f002
2c008f0826ec49e0627412974027c09874) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1780) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (b405e10326c118b0168404db21d9881100000000000004210be01f30274c01f34058809520248c813b007fc0117027f401ff0367c21ff025fc09d5626dc0193006cd01f50057a002000000000000066043c40d70027c16d900174005b0007c201f0037c40880a36c00d70807c40db0007c001711
970005700151205f0035b810000000000000084047c01e30078d01bf0058d01fd2048c21ab407c5016f007bc01eb303fc81ed005bc016f0c5ad0173005cd01634078101c000000000000080007400e90432400ed0018400691088400210038480ad003b400e9203a080ed083b402ed043a440e1403a400e1043880
040000000000000c2053400c140746008d) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (17a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (86c40d81896c00cf0017c085b0287c20180027c809f0035c00df00a7c00dfa407ca05f1237c00df0037c009f008700010000000000000e0073c00d740f4409934014420d14042c0280080740017003fc0cff09a70009f0067403570273c61d300f4c119d0955a81400000000000004001b400c58
143403810050400010002480050035420015037400cd01430020500c34080100c24031911c04005904432806000000000000040023404e58118418e10118408a9020a40a21802f40025003b404ed012b404ad121b4c265800b48021060c4226d02090000000000000000042256405e1047fc0081055ad057b094b8
802b413bc8d011973c85ed016340567061) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (17c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (06df0387c061f0087c1e134087c88030404c001b00a2100000000000000000a843486c8018240085011345051040162201c0224000140b3406cd01034044d88034440100a740481212140081c4200030000000000000020007400d92220400dd0015400510444481110447400110037400dd0047
4019d00c744a1100274009100204449900302001000000000000082217400d10144c40d70016c004100c5441150067410911037400dd09474055d0047403110016c005140155011100860001000000000000040017c00f3007cc009f001c080f3000dc20b3000fc03332037c80ff202f8903f000fc0073001ed507
3001cc2033021f08800000000000000600) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (17e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000040040400cd0033600c10003400c90031400cd0020424cd1030500118007488c50000640cd0003480cd00a340005c21520130000000000000c2004401dd0077401d12207401dd00774019d0074480cd0074401950067403110044401d702c4409fd10c7401110097110300000000
00000e000cd01ff007fc01f3110fc01fb007fc01ff007cc09ff007cc21f3006fc0033000cc10ff000ec84ff000fc0033481f20030000000000000e0017c02d7008dc10b50a14c103e0507c402f012b80c3e0237c28db020fc1c1f050fc403f000ec423f2003c103f052fb8250000000000000ac007c02da4084d00
ff2115c00934084c2013228740e1109b74) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1800) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (9d0074402dd08b7482810067401514075403d51077425f522f4431d10450201f00000000000004200fc00df0037c00d3001dc00df0037c065f0004c05d70137c10170a27c08d30030c02c30007c00f71204d00df04140007000000000000040217c00ff003fc80ff0007c00ff003fc05bf003ec0
0ff003fc08bf022fc007b0277c15f70146c40ef0037e015b009d0081000000000000042210c00df0037800d30007c00db0037c035f0414c80df0034c01d30023c00174044c07df0087c00df2247c8317209520800000000000000e200c400dd0837400d10047400dc0037410dd0065400dd8034400950007480150
004400dd0035400dd00274189500152003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1820) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (004e01930005281000000000000006600bc00ff003fc00ff800fc00ff083fc28ff102fc40ff083fc00b7001bc00b7023d800ff003fc00ff023dc08f70239300200000000000000405bc00cf0033c00c30021c00cf0233c18cf0130c00c70033e000f2013c80c32232c90c300a3c00c70032c004f
0292001200000000000002021b401ed807b401e1004b401ed007b609ad0078401ed067b411a9007f401a902fb029c544db443e5005a401e9025c024b0000000000000a000f400cd0032400c10005400c90033603cd0330000d520b3603890133404010202403c10873400c10812412095012201300000000000000
084f400cd0037400d10027400dd0037403) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1840) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (005fc005f0016c0c73409bc005f0017c006f041dc057300dcc0b7f001fc005b201cc1173411d280300000000000004204b400cd0033400c10033400cda032402c10033400cd00334008d1161481c12070501cd0033400c908f0410c560352812000000000000040003401ed007b401e1087b401e
d007a401f108fb621ed807b4012d8079401e100f0623ad286b405e91449401e14059020000000000000004204f400ed003b400e14013400ed003ac0061001b400ef283b420ad2028500c180384004d801b490e14030500c100090013000000000000060053c00df0037c00d3004fe00df0034c01530013c00df007
7c009f0024c00131004c001f0037c0ef30) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1860) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (045481052141481852341481052020140000000000000000634009d00274209d00374009d00264019100a44008502244009d0024400d15034400914065400918027000910024201c0000000000000800074009d00274009d02674009d80274049500a44009d01645069d0025400910024c009110
2540691602740091016420010000000000000c2043c009f0027c009f0067c009f0026c009300e4c009f0064c039f0024c00930024c008500250009314234889340e508100000000000000c004bc001f0007c001f32c7c001f0007c021f0487c001e0087c001f0006c000f4403c001f0003c02070007c0018008400
1200000000000006201fc005f0017c0053) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1880) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (734001d0005c001b42c74001d0004c005d1007425170005c0051000c4025302844021d000448a1d20844025b40c5101800000000000006a063c00bf0027c009301ebc009f0024c00bf002fc80bf002ec00a30024c05930164c119f0164d019f0064c159301efa81900000000000006e067c009f0
027c009f053fc009f0027c00af102fc549f0023c00bf002f800bf002dc40bb002fc009f003fc00bf453f1a1900000000000008407bc001f0007c001f0117c001d0006c00130004d00172004c001f0004c04130104d04130105c04130107c04130102001b0000000000000080434008d00234008d05234208d00236
008510244818d00204008d002141480052) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (18a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (011f000ec0033008fc0033088fc203f008ce003b0105081000000000000004205fc009f0027c009f0027c009f0027c949f2927c10970025c099b4027c48870063c008f1165c008f0027c918f40210813000000000000040017c009f0027c00930063c209f0026d009f01a7c009f0026c039710e4
d009306e5c069f01a6c009f00a4c089310a522450000000000000600634009d00254009902274009d80244009d0827400950035400d501ac400b1402c520bd103e440bd102c500b9007520180000000000000c804b4008d00234008141234008c00224008d00234108d0023400c5002c402a10029400ad00aa400a
d00a8400a100a120120000000000000c60) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (18c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000004053c81ef207bc81e3007bc01ed807bc81eb0068c01750068c01ad004ac01230043c01230053401ad00484014b00780014000000000000000013400ed003b420e9001b400e5803b400ed203a503a1245a401750038400c9003b600e5007b400ed0038400e120bc000400000000
0000040053400cd0033400c10013420cd0033681c90c30402c40170400cd08024a00102030000120036000d000044209203220100000000000000004134005d00174005b04df4005780174806d211c48370005e8007f8110c005100174045500174205d20144005100dc2000000000000000042053c001f0007c00
130187c001f0007c281b0004c00170004c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (18e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (891ab34004500024118d0063400cd00a04008d00634604900f04000104072802000000000000040403400ed003b400e1000b400ec003a480b1003f40069093a404ed001b4102d001840069001b400a90400502f5103d0008000000000000062057400ed0239c08e5020b400ed103ac806b001b48
0670008408ad022b420ed0128402ad023b428eb023840061032900550000000000000e000bc81ff207fc01f3004fc01ff027cc09a2007fc817f016cd0dfd005fc013f005cd017f004fc0133004cc01bf02792802000000000000046043c00df0037c00df0037c00df8037c209f0025c00bf0013c009f0037c00d74
037c80df0027c005e0037d009f00113810) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1900) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1b5440910a14200100000000000000020f000dd0037400db0077440dd0034451c301e1c409f80d7c0ad104934011d01174005d0087e001d00444009100c4008b000000000000042203c00ff003fc00f300f7c00ff003c418f3067fc213f002cc01f3402dc11ff042fc009f043ce01ef007cc0073
082d09a1000000000000000007c00df0037c00df0013c20df0037c08df0087c00bf0095c4a5f0217c421f1297c0a5f0297c009f0c87c08c700b50801000000000000042053c00df0037c00d30457c00df0036c03530097c009f0006c03cf0067c00df00a4c009f0027c005b0074c001700b420380000000000000c
201b400cd0031400c581c3400cd00324a2) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1920) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (006fc011f806ec013b004bc010b000cc00ef00f4c043f090dc2413000ed0011004cc0137005ba00300000000000006c017c00ff003fc00ff001fc00ff003ec00f70039c003f100dc40ef000fc003f000fc003f000fc203f000ed003f000db901000000000000084003c00df0037c00d20017c00d
d0835d00d32037c001d0034c00d31035c00dc0037400dd0035400df0035c00c300060001000000000000008043400cd0033400c90003400cd00304004100114000400036005100074000c00034200c18114008d00014804180002010000000000000000007400dd0037400d12007400dd00354005100374081d007
4600518034406dd8037400dd08254a45d0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1940) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (7c001b0025cc02f022fd207f003d80070000000000000e0008c01930026c230d00674031d0964c011b00074031b0044c00dd20345001f00c6c011340e5c1a170144d01178053a80200000000000006200c403510137403d501354411d0065401910435403110065400d420344021d04470011504
40100110034441510065a8030000000000000ea0404008109264000d80234000d0020400010003400091000480cd00304021d000240001000140005000042055a017a0100000000000000c00044091100254019f0037c011d8025400110047c01112005400df01354231d024740911000448021004440111006708
010000000000000e200cc04b34260c012f) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1960) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1840de9006e4117d00784612d006b40121007d405200048405ed387848121004940569084850921007c40f31026880060000000000000a009c4808111624030d04f14080d10034031188816020109c4600cd00306000110414000512c14000100b1401094192a00700000000000002004c400cb0
172c00dd00f4c419703274219300b1420510034400fd12b45004100244209100e5430150030413032144a01300000000000004000cd02d320248245d1027c201f00a7c58138334e12130234c40df0035c00530385c021701a4c12134314c02530035080300000000000006001fd009f687dc00bf007fc003f002dc
803f40cfc003f0007c00ef003fc041f000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1980) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (05ed007b4416114536036d80e85432d0068401b100f9000300000000000006204c500e1003940061203bc00ed0029ea021203b4402d0008420ed003b400e1401b420ed00294104d201848061002988130000000000000e0054d00c74030401430033c001f0027c001b08338001f1006d08df0037
c205b2057c205f1026c041f0034c00434043a01500000000000006200bc207f003fc00ff033fc0867002fc80b7003fc003f001fd00ff203ec089f1236c48570a2fd6c7f200bc0cee00059002000000000000000048d05830072c000f0461c890f0263c00014101515834340401cd0070c29014011c1f074301c010
30b71d0ccb00b010120000000000000208) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (19a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000c2040c00970067c08970027c85912024c01938866c00930064c00970027e009f8026c08934066c009f0026c009f046708100000000000000c084bc801e0205c00170007c031f2107c001f0387c041f01048001f0087c84171487c001f0407d800f0007d221f3087001200000000
000002205cc0873401ee2079405f4807c089fc047b085e4107f0819c005f0017c0371001fc436f105cd017f01dc8616300dda8170000000000000c2048409d10037401c900354c0cd02f1600d100b7481cd02f1400dd003742ac180b3431cd80b1412cd0180409812043281200000000000004000c401e1107e403
6900ff4112d806b40128207e401ed00796) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (19c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (bf002fe40bf0d2fc08870527c40bf002fc40bf052fd54bf002fc00bd102fb81900000000000000c070c04171007c00170007c00118004400130016c00514104c0a1d10074441da106c24133106d041f0006c005f0016b01c0000000000000080424549100236008940636008d002260199002460
08125254048980234148d8520414810d204148d00204008d10202010000000000000020060440950227402950027400d54c644089122264809122344009d00274009d82264009181225089d10e6421dd0224a018000000000000080006c009100274039302e740597a0e2ec39b00e44088101e54409103274009d0
1244049100644019d10e44039d08e62001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (19e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (165c039f00a7a8050000000000000620634009d00344809100254509501374809d08244149500a54009d00244049d80274009128e44009500245209d22a5a8180000000000000ea0404009d00204009100264009100274008d00204008102200028d20204c08d0023400810020502dd08214009d
0023a0100000000000000c0073d005d8804420114505c401f01174145d0014480150587c071f20044005d00074201141440874f00044205d0007081c0000000000000e0060d80bf002cc20b3402cc80b100afc00bfa02cca0a3212cc079f002cd00bf002fc00b204ecc07bf102dc00bf002fa0180000000000000e
c067c20bf052f800f7852f400b2052fc14) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1a00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01f3401d500f0421cd24a1400412070440c100b1600c9c072401c50136500cd0220407cd0072a01400000000000002005050041101c4a36d0099c007100184807d009c40061441c40071041c40041009c4037d005c40067029c4036d019c8014000000000000042050c00130804c001f08074381
42404c221f0005c00130044c00130105c00131604c82170206c01171004c0a1f01850814000000000000060057c029f0a27c019f00a7c099f0827c029f0067c019f0163c00970027d009f0127c509f6026c409f00e7c089f002580150000000000000e2014d009d0024d08914026c02910867c009d02a4d029318a
44008f8024c029f1167c049208244899d8) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1a20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (b411a0127810d7d0000481ed024988150000000000000e0000d01e3027cc01c3025bc0933031fc21f3004cc415f0054c01ff0174c05ef014f405f320f0c01d6024cc094f025fa000000000000000062043c00cf0007c408d0017c805f1007c001f00174001f2007c08df0017800d70001c009f29
85d20d70027c200d0035b810000000000000000054c21e3007cd01ef205bc0127404cd013f0049c0163007c505e3405dc01eb006ad01e7006ac01ef0048d016f00481015000000000000020014400e10058400fd1438400a120b84032d8008410f11038404c10058480c9805a6118d2008400e10028400fd002880
050000000000000a0050400c1423040ecd) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1a40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (07c00df0897c06db0206c08d702b7c401f0417c28db0207c00df1007c00dd00078821f0107c089f0037d0adf10a70001000000000000062054d03c32814443c958274c09900d3c119900544835d3804cc0fd0024c42dd00b7c811311e4508d600f4c408f23f5a8150000000000000c2010413c58
241409050001411890083412414890401091001440dd0000404cd00034000108645004d24404014d10032804000000000000040000414e1003c404f9000f600e9000f4086906084427d0208404ed8108488ed108b402218228604e52438404fd0139000000000000000006205450dc5215d40d6b0002c056101474
056f114a90da90151041cd1158505cd210) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1a60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00df0387c46df010740a13092ed06df0094c041f1916b000000000000000008042590dd21804041d80024101954074100d0410450dd0400518dd0103400cd21014040100304060da0104509d04002030000000000000020004400d900044039d00444415900474019d00154215d2044400dd0447
400dd8407403112076501dd08444819d0414a001000000000000080206c00d57080c021d01c7c010900c74c11d1457c410d01c5400dd08c7420dd0087e031118445409d1cf44271d00a620810000000000000c2200c00f3009cc007f000cc8073140fc803f021dc007f040ce00ff280fc40ff114fc0033402ed00a
f003cc003f00ff08800000000000000c00) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1a80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000e8043400810003404810000400090c004900101004a48d11024244d0813404c9c2014900141037060d6037400cd00b3a0100000000000000c2007401910823430111034404110104404018004e004101144041d0504408f105044041b0104406010027401dd00f7080100000000
00000e000fc01b3004fc2133004cc0333004cc0133024cc0933024cc893f004cc0df3000dc0033008cc0833206bc81ff003fa0030000000000000e6017c10d70085d003f040fc30d704074201f0013c102f110f804cf220fcdcdf0207c8c1f10afc0c3f1d1fc003f000790050000000000000ac000d04db0884c94
1f2004c009380074801f20154005f0a844) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1aa0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (934065401dd009740250029540ff361b400ed1003449bd10137440d1003ca01300000000000004200fc00130107c01970004c109f0424c05930066c009f0107c04530214c40d30114d02130034c025b0037c00d34035080300000000000006001fc013f40ef4093f503fc09b70a6f809be826dc0
073001dc003f000cd00d7486ec01df0124c01f3002fc00ff103580070000000000000e200bc00134047c21132004d019b4064d0191c0645001f4006d001f0007c00dbe085c03130047c025f0023c00df0037a80200000000000006200f404910027400910030400190004400110006400dd10164005c0817500c90
501418c900136181d0027400dd0035a803) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ac0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (027c00df0037a01500000000000006600bc01ff003fc08ff283dc087f021fe0877821dc00ff003fc00f30037c00ff000fd08ff403dc0877222fc08ff023db80200000000000000404bc00c34013c20c70006c005f0210c08430214d008f04a3c02cf00b4c04c90020c08c30022d00cb0033c00c1
0030101200000000000002001b401e1007b40161027b4016d02584096102584116d027b401ad4069401e1025040921007a60129406f401e1023882060000000000000a001f400c1009740045004240b5d02144025100144001c20674209d4060400c90030480010482400990163400c10032a00700000000000002
004f4001101a740b9109354039d00e4501) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ae0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0014902474095d425f6097c40530016c00530015c005700dcd0073009dc42730457c005f0014a8170000000000000c204a400490034480c11030400c50031400cd0033400c10036400d10032400cd01f4400c14033407d10077680cd0033281200000000000004000c40171005c401e50048401e
50079401ed007b401a1006e401f1007d425e50078411e10479603e1007b401ed0279000300000000000006204ec006b0838400610038680e10038400e1003b400611038400a1002ad02eb2030400c11032c0081002b400ed017988130000000000000e0054c01530014c01570004c00d30034c01d30077c0013002
4840930024c12d10034c00d30054c00930) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1b00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (14148c05214148100234008d05202210000000000000020063400b148af400b14028400b1002b408bd002c500a5402e600b109204808940244028d04345029100a74009d1024a0180000000000000800074009100e74129100244039b00a70029d00e44869100244079144e45079101e55009d02
e54429140a74009d002622010000000000000c2043800934167c04930224c059300a7c019f0164c009300a6c04930024d449b0124c129f0024c009320e7c809f202708100000000000000c004bc103f0007c021f5087c101b0406c10130407c021f4085d021f4007c00190207d021f04068001f6007c001f000700
1200000000000006205cc22530014d8057) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1b20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (734001140406015111454051700474051d014440113004444111004ec031b08c2c031141c6c0f1100474001b0087081c0000000000000e0063c0093402ce02b3022cc00bf00afe02bf002cc02b310afc22bf40a4d179b0265c0393026cc87b3022fc00930167a0180000000000000e6067c008f0
523c149f0527c149f0527c349f0527c149b0d23c148f0523c149f452fc14bf052fc14bf452fc009f0027b8190000000000000ac073c00330007ca0030010d00031003c000f0000c00171016c00111004c440b0104c441f0904c04130003c001f0106b01c000000000000008043400a1402b400a10028401b9006b0
01ad8068600a50028400a1002841481052) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1b40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0013000cc0033000cc00330404c00130407c001f00050814000000000000060057c009f0427c00974027c009700278009f0427c00930025c49974a67c009f0067d00974163c00930067c009f002180150000000000000e2017c009340244828b0024c009f00274009f0024c009f4025c00960027
c40974225d029b0126c009f4067c009b0027a8050000000000000620634009100204009900214008510274409c002440094002000081002a400b9402e403990026404891123400990025a8180000000000000e80434008105205049901204108d00234008d04205058d012140481002b420a501a9602a900a25008
d41236208900a3a0100000000000000c20) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1b60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000004057c01634248c81f7406fc0123404bc416f005b40167006ac012f0258400c3007bc0183005cc8145407fc01ef1878101500000000000002001740061001a4302100bb410e100ff400a9002a400a5001e40075401c400e5003b400a50038450e100ba400ed0038800500000000
00000a0053400414090403c50073400c100f3403cd02b3401d58032481cc00e04801140074005102f0406c50073400cd0032a01400000000000002005340071001cc0871401f40371001dc057900de41271001d41177069440055001450055005c44370001f4405d0014a014000000000000042053c00130004d02
170047c10130407c101f0007c10130005c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1b80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1120204000d00034000100144001104004034100c1402cd8043400cd0033282400000000000004000340061000c40021008f40029000b4002100294007d042b400250228500c59039490a10409600e5843f400ed103902000000000000000620574006b001940821020b40025109b4082100a980
02d001b400254018400e1013840ca1021c404e3018b400ed023988150000000000000e0003c01730058c01b3004bc01f3004fc0133006ec016f007fc01b3086cc8133004cd0973007cc01f7007fc01ff027fa000000000000000066043c005f0005c003f0027c00ff0029c00fb001fc003b4009d002b00a3c001f4
0048005f0037d00df0037c00df0035b810) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ba0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (037440dd0034a0010000000000000802044004102f2c8a1101b34021b0844400dd00140138100c441b554064400150004420510075401d90087400dd003620810000000000000c2200c007b402cc00b3002fc0032000cc007f001cc01b3006c401f3005cd00f30030d109300dcc200f00cf800ff
003f08800000000000000c0007c805f0097c227f0037c0237000fc00bf008fc83bf009fc027c0027c00df0036c009f0022830d00037800df00370001000000000000062057c0e5102b4c00530177c001b0037c00d30814c009f0007c00d72014c00171005c835302e5c02974077c20df0034a8150000000000000c
20134034900014001100034000d0007400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1bc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0048c2c33010f8013f004cc01030046c013f0074800ff004cc00f78526c40df0048c0153405ba0030000000000000e6017c0077c03fc003f003fc003f000fc003f000fc803f000ec003b101fd0037000ed007f000fc00fb000bc40ff003fb8050000000000000ac000d0053002cc00030027c001
70000c001f0000000534025d00910020c00db0034c40934004c00df0007c00df0036b0000000000000000080404004140324000100174000900004000d0000400110011400040050400cd0031400802001400cd0003440cd003020100000000000000200044205100b44101102074141512044401d200400451050
1400850a24400190805400410024404dd0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1be0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (fd00ff0007c80df083fc01bf001d80050000000000000a0210d01134042d081b0044c43131885c031f08c45018324424211d2034000db00c5c00d51082d01dd0034d02170097a82000000000000004001c400910866480990c54610d506074611c1044411111065403150035420d11235400d120
e4011d50834424910235a80300000000000004004044481000240c0900045040102016008d80006000120064000d1c30400c90101420d56022420cd0000000d50003a8130000000000000c400440a91000443211004440c1520c74011d0844441110007c001f0137c40f10405401f100e44209f087440151005700
030000000000000e010cc08b30048c001b) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1c00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1a40df9214c40d49004e48da90f7b40d2d814c485218168485a10879405ed0058405e14368741e1007b405e1006c800f00000000000000000c4129902004130100024510900c04008d08c04110500014030500b1400cd0004400c10821401d1040340a490032a00700000000000002004ec11db0
224400db0012c10df00f3c009104044829111a44019100b4400fc00340cee54145403d118b7409012000a00300000000000004200cc00530804c0a5b0e04c029300b6e02970186c40970127c4e979434c00df0414c00db0084c10db0237c00db00050803000000000000062017ca97f002dc00e7003fc036f0437c
003f200fd40bf000fc00bf003fc40cb002) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1c20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01ed0078509ed00fa445e90070441e90078621e10869000100000000000004404c400e1003c400c12038400c1083ac40a1200ac00ed003b400e90838494fd003840ce12038400f10038500a108398813000000000000040050c00131064d009b0050c40d60044c00830000c009f1027c805f1036
c86de0034c20d92034c00f01070c000b0033a01500000000000004200bc80ef002f408ff201fc28ff093fc04230009400ff002dc00ff0036c08ff023fc10c7003fc0856403fc087f200da802000000000000006058c0dcb01e0c07c30112c0d5b087051f8d2040d11050345485d50375505cf26e0c01c32061c314
30003c05cb00e000120000000000000020) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1c40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000042040c009f00249039f00e4c019f0027c80970164c819f0066c099f0866c00930624c858b0264c109f0064c04930427081000000000000004204a8421f0007c06130487c021f0007c10170007d001f0007c021b0085c000e2005c021f2187c02174c87c01170007001200000000
000004001dd0d7341dcc037f14dcd1b77041ce127b42dcc086d02df0057f80144005f009ad007b00981057b20dcc00734119a817000000000000040049401d154f040add0070403c101b2441c102f2448cd2073424c90030420cd00f2480c102b04235902f06004100232812000000000000040001401410078481
ed005c401e50078401a9004c401ad00fb6) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1c60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (bf202fc00af052fd14bf0527c549f452ec008f002fc14bf202fc00ff002f98190000000000000ae078c041f0005c441f0004d041f0105c00170004d001f2004e401f0006cc4130014c041b2104c04570004c80130006b01d00000000000000a850414cd00214148da0204148d052050081002448
08d8020400dd00204148100264148105325148900204019140242010000000000000020070400dd01254109d04244088d202540095a0b44249d22244009d0a26680910824422990024408950024500d18024a0180000000000000000045089d10244819d20244079d06e44008100e04009d04a44428d01e4420910
066c019100a6c409d03a44008120260001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1c80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (024c018f04a788050000000000000400606069502254849151254009100656609100654209021374029c00244009d02244809101244c09900245809d0125a8180000000000000400484208500244808110244808100634008900200009100230848d00214008d00214008100264008d20244009d
0023a0120000000000000c4060440150105420510015400150007c405520054005115064001d20044001c0007c00110806c0f0900044001d0007081c0000000000000e0070c20b3022cc00b3002cc00b2002f400ab002c400a3002fc42bf002dc009f002dd00b3002dc0db7002cc00ff002f80190000000000000e
2077c14bf0d3ec34bf002fc94ff002bd00) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ca0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (4070501c10430461c100f0605dd0474404cd1030440cd0432401c140715a0dd84e34898da032a01400000000000000004340375005ec037104184097b011c4017102d86117d119c42375049ec005d109cc2371205ac117d0c9b6007d0814a014000000000000042043c02130604c02130404c021
32002c001b4204c821f0004d02134004c001f0087c04130207d041f2007c121f0085081400000000000004204fc018f0067d009f0067c008f4027c239f0827c289f0066c009f1427c008f0067c808f0026c03970027c099f00258017000000000000040014d03972064c03930024c0a9300274039b04a4e409344a
7c0b9f0025c009f01e5400914066506972) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1cc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0401c10028401ed027b400ed0031801500000000000000001ac09df007cc09ff0174c25ff1075c01b3004dc012e0057c015f037c009df227d469f61068c07ef0077c093f007fa002000000000000062043c009f0017c009f0003c00df2015d809720034001f1007c00530017c00dd0004e00df08
03c02de2037c001f2035b010000000000000086043c01e3007cc01c30078c81f30070c01e30048501ef0058c01f9007cc89cf205ae01c30849d01ef087b401af00781015000000000000082003402e5001a410e10028402e91018011a1000c4003d00384516c105a40ced001a442e1002a440ed803b4002da03880
050000000000000c0043406c008f4406d1) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ce0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (158009f0087c005f0427002cf0197808994107c001f1407c221f0086d00de0007c020fe087c04df1037c005f043700010000000000000e0052c019f0074c22df0ca5c03dd0096403d709e1c30dd00e74c09f0006480fe02a5c00d50804d03df0037c02df2c35a83c00000000000004000a4a28d0
8d540c0500c148d0d12426818500004050520430000d0002440dd1040440011040441cd20736860c00332806000000000000040c024046d04387006d0009480ed811a600b502090002d0c1b4062d110a404ed0819404250608418ed0e3b630ad00390008000000000000044056c1d8d13514ace7016940d0d03438
0481200048d2f104b4050d185a845cd141) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1d00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (461f1484c08e30a04c8c1b0885c0ab30137c02df00b6a0010000000000000020430028509025000d80204a205c1034008100040040d04834060d0301484c10046504094200404c101376a04d003020100000000000000a00054019104044188d00e4410d500174409120444011500474031d0044
600d14044402d900c5521d100376019d00348001000000000000080217621950816c211d00c44001501c74009100456210da0c74031d1945400d10842c201308c44679104b34875d00362009000000000000042213c10b3067cc20df280cc02311209c10f3000cc00bf080fc403f000d800f3000ec08d32009c00e
3057fc00ff003f08010000000000000620) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1d20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000040043400c142024088d0033400cd0033400cd0033400cd00334000500034048101074204d0223400cd00314009d0033a0100000000000000c24074231300c45035d1077401dd0077401dd0077401dd0077400d10077441d114774015d0077401dd0874400dd0077000100000000
00000e200fc147b1108c043f007ec01ff007ec41ff107fc01ff007fc013b004fc0933404fc017f012fc00ff007dc01ef007fa0030000000000000e2017c08bf04074003d008fc061b020fc24ae050bd281c010fe063f2007c06ff010fc0c13000fc881f021fc147f053f9805000000000000086003c02130404c08
1f0104c06030a87c8893408448e170187c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1d40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (dd00f7400dd0037421dd04434001d0037400d10024400fd00344009d0034a01300000000000004200fc08f3009cc40af0037c0cdf0037c10df0437c00df0037c041f0037c00df0087c00d30024d00df2036c009f00350803000000000000042217c0037005dc01ff003fc00ff043fc00ff003fc0
0ff003fc09f7100fc00bf013bc00ff2027c00df003fd01ff003d8805000000000000040213c18520096c851e1036c00df0036c00df0037c00df0037c04110037c20530007c01de0027c00df0035c008f0037a00000000000000006201f400990116408dd0037400dd0037440dd0037000dd0037400d10037400514
0374185d0077400dd00344089d0035a807) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1d60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (034c009f0037a01400000000000006200bc00bb000fc00ff003fc00ff883fc00ff083fc00ff003fc003f003fc007f000fc003b003fc00ff083fc00bf003db80200000000000008404bc00c74020d00cf0233c00cf8233c18cf0233e40cf0033c54cfa0038008f00b3e00870020c00cf0232c008f
0030181200000000000008201b4012510684014d007b401ed007b401ed007b401ed007b4012d007b421ed004b401250078401ed0078401bd0078000600000000000008000f4024500204000d0033403cd0033403cd02b2400cd0033403c904834000d0033400850020400cd00324008d0030200300000000000000
004f409510010400dd0037403dd01b7403) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1d80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0017c005f2017c405f0017c005f0015c005d01d7e01530016c027f0014c005f0014c015f001520170000000000000c004850781427050acd1033400cd0033440cd0033400cd10334000d0043400090004401cd2032400cd00304008d00332836000000000000040000401c100704018d007b401e
d007b401ed007b401ed0079401ed007b401e1007a4017d0078405cd0078401bd0079000000000000000004604c4002100384406d003b400ed003b400ed003b400ed003ac003d000b480ab0008400ed003ac02ed0038500ad00398033000000000000040050c01530074c001f0037c00df0037c00df0037c00df003
4c01df0037c00530036c005f0034c01df0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1da0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (84009d05234148d00204009d002020100000000000000200734109d04345109d00274009d00270009d00274009d0027410b1402c400a9002d4009d00274009d00264009d0024a0180000000000000800074029d10a44029d00274009d00274009d00274009c00274039110a14409500244008d00
274009d00244008d00262001000000000000042043c009f0024c109f0027c009f0027c009f0027c009f0027c45930165c00930025c109f0027c009f0026c009f0025081000000000000006004bc081f0407c000f0007c001f0007c001f0007c001f0006c003f048fc083f000fc081f0007c001f0007d081f000508
120000000000000e201cc0373089cc037f) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1dc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (704083700045021d1005c003d00074401d00074001d0006c051d30074010100444401d0285c021d00074001f200700180000000000000e0060c019f0064e119f0027c009f0027c009f0027c009f0024c00bf002fc029300a6cc09f0177c049f0027c009f0027a01c0000000000000e2067c00bf0
02fc00bf0027c009f0027c009f0027c009f0027c149f2027c14970527c00af002fc009f0027c14af0027b81d00000000000000407bc041f0104c041f0007c001f0007c001f0007c001f0007c00330815c001b0801c001f0107c041f0806c001f0006b81c00000000000000a0534148d05204148d00234008d00234
008d00234008d0023400a10029400ad002) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1de0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (081f0304c00130006c001f0007c001f0004c401f0005081400000000000006004fd04871025c039f0025c009f0027c009f0027c009f0027c009f0027c009f50278009f0025c009f002740196002508170000000000000e2014c029f10264039f0027c009f0027c009f0027c009f0024c009f0027
c04930026c008f0027c009f0027c289f00252005000000000000040060400b5006e4009d0025400bd002f400bd002f4009d00264009d00274009100204009d00254009d00274009d00252818000000000000040048401ad026a401ad0023400ad002b400ad002b4008500214108d00214048100224009d00234028
d00234148d002100120000000000000c60) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1e00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000004040d01c34052d014f0079c012f004bc0129004bc01ef0078d01ff0078c0de305fec01ed007bc01ef0078c01fd007818140000000000000020004c26120f8482ed003b400ed003b420ed083b400ed0038400ed0038609e10138540fd003b400ed0038405e50038800400000000
0000080050401410072401cd00314080d0003408090203400cd0030411d98020400c15032400cd0033400cd0030500cd0032a0100000000000000204104005300144005d00174005d00174005d00174005700144027d009c4005300144005d00174005d00144005700142010000000000000042040c00330004c80
0f0007c003f040fc003b000fc001f0004c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1e20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (8d0023400cd00305015d12b0401d100b0402cd0033400cd0030400dd00312802000000000000040003401ad00884000d003b4006d002b40065001f400ed003a400ed0038402e5003c400fd003b400ed0039400fd003900000000000000000460574182d002a400ad003b400ad001b408ab002b40
0ed0038c08fd2238400f10638408ed003b400ed0038c00ed0239001500000000000004240bc013f006ec01bf007fc097f026fc0973031fc01ff007cc01ff007cc01f7007cc01ef007fc01ff007dc01ff007da006000000000000042143c00d70017c005f0037c00df2037c80df2037c80d70037c00df0037f02d70
037c00cf0037c00df0037c08d700359810) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1e40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (034400dd0036a00100000000000000021f400dd00155005d00374045700674025d0117400dd00344119c1035000d10034500dd0035400dd0035400dd00362081000000000000042213c00f7001cc007f003dc00b7005fc00bf002de00ff003c800ff003cc00f30030c00fe003cc00ef003cc00ff
003f0880000000000000042007c805f0077e05cf1037c025f0027c02530097c00df0037c04df0037d08df0137d00df0037c00df0035c08df00370805000000000000040053c015f1036d01df0037c009d0017c00970027c00df0036c32dd02f4c00f700fcc08cf0177c00df0035c00ff0035a0140000000000000c
001b4108d00004000d00334008d0013400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1e60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (084fc0123118e40137104ec092b2104c041f007ec009f003dc013b0068c01ff0a44d01fb007f80030000000000000e2017c00bf000fc403f103fc0037000fc003f000fc00ff003ec00bf001fc00f7003fc00ff003dc00ff003fc00ef003fb8250000000000000ac003c00970004c001f0035c00d
70037c00df0031c00df0035d00dd0034c00f3103cc00df0036c00df0034c00df0036180000000000000000a0434000d80217008d00334000d88034000d0003420cd00314008d1071400c91034400dd0033400cd0031400cd003000300000000000000200074001500240009d0037400dd0137402dd0037600dd003
5401d90074400d14034400d91036400dd0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1e80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (fc0073022fc00f7020dd40ff003d80050000000000000a2203c03d300464015f0a030435100c7c51050840c0b1b00c40111f0036c00d760354091b0060c00df0086c40df0037a80000000000000004000f401195045440550035200110c45421118435420910024000dd00364009108344009500
24520d51406400dd003580030000000000000400434208901864001d0017400010087400118020004112000402050032408c10231430112024400cd0102400cd0033a0100000000000000c6007481d18087e80510005c815101844011b00054249112444431d0074403f100ba884014064400c70004401dd087718
010000000000000e000fc01e3008ce417b) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ea0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1a401e0004b409e10a4b4916102db401298a4e401a18070401ad017b405a10278409e9016c405e901cb401ed007a080600000000000008008e506c10ac3400d0008021101c0034000d00424031104404030904b1452c50030400010062500dd0003600cd0032200700000000000002004c413910
0936115140368015100d30079384b4485d1013448bdd2037400c1403cc20cb4c24400dd08a7440cd0034a01300000000000004200cc20930195c02530136c025800d7c901708b6c301340b2c008b0037c01970030c00d34426c80df0027c00df00350803000000000000060017c00f72007c057b004dc037f0016c
003faccdc01bf415fda55f003dc02bf003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ec0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01ed0078401e50378601e1046e501e1086a401ed0079000400000000000004607fc00e1200a400e1180d42061001b400a1000e420a18033c00ef2038500e1043ec00ff0028c00fd002b400ed00399813000000000000040040c20d32006c814b0004c015f0003c001f0004c00135067c80df0036
c909f11b4c00931026d00d70007400df0037a010000000000000062009c00ff001f800ff002ee00770a1fc00778039c00bf023dc00ff123fc00ffd23dd08ff012fd08ff020f400ff003da8020000000000000840dac00c24083c00c30004c00034213c040e8022d060320d041d4b2571c01850230c01434022c85c
f0343c00cf003210160000000000000820) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ee0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000420c0c10934067800930666c099340a6c80970026c089f20e4c048f0024d01831024000910167d009f0027c009f0025081000000000000006084bc401f2087d00170007c00170007c0a1f4405c20170187c041f0006c40170007c001f0007d401f0007c001f0005801200000000
00000e201dc8077421ec827b00d84027f029fc027f045c5497b011f6077d0016c01772014e0673105ec0053041e4005f0017a81700000000000004004b420c10274410c902b1650c94277431c100b244ac908f1401c50030488810036406cd0030440cd1473400cd00332012000000000000040211401e50050411
f900684216d005f64169004a401f9007b4) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1f00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (bd152fc14af003ec80bf0025e00af0524c94ba002bc949f052f8009f0027881900000000000000c076c00130107c00130006c00110107460570006c401f0104c041d0014c04130107c00172007c001f0007c001d0006b01d00000000000000a85050081052340081002740081853340081002050
08d05205148d10204148905234008550244008d00634008d0020281400000000000002007240ad12227401d1c026400d100274089504226009da0254109d0224400918027500c500275008d01274009d0024a01c000000000000080004c018101e74019100674079b80e64039102244018d24244009d10644cc9b1
026c009140204009d00274009d00262001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1f20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0a34009f0027a8050000000000000400600009500f440095c22740291013346099006346099203c404bd002e4419800244069900244009100274009d002520180000000000000480494009100205848180274809100236008d6023420890828580a5002a4029100204008100214008900274008d
102100120000000000000c607040015000440411050440011000344011250344011200c4001d00065001b00844151100045151100174001d0007181c00000000000006a064c00a3402cc02b7002cc00f8002fc00b7002fc00b10024800971024801b90566d008a4029da08b002fc00bf0027a0190000000000000e
8067c00ef052fc94be052f800af052ec00) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1f40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (8370400c90231440c10072400c500804050d04c0402c50030520cd0030400d50333400cd0032a0140000000000000200104007140dc4005c009800361005c41371165c511710416c005f049540465401440071011840071281f4005d0014a014000000000000040040d02132484c001f0004c001
34105c00132084c00172406c000f0004d04132000c421f0004c00174087c001f0005081000000000000006004fc039f0027c019b0024c19934027c19970027c039700a3c409f1025c009f3027d409700e5c009f0267c409f002580130000000000000e0015d028100a0c2c930127903932127c109d4127c079b402
4406970024c00920024c038b0025d009b0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1f60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (c40dd1004a401dd0518405ed0179181500000000000006000cc09eb205fc01f3206cc0127437b041f2007cc81e3007fc09f6007cc01cb0274c15db8069c09ff007cd01ef82752002000000000000062042c009f0017c009e0036900070035c00cf0115420df0035c00d70827e001f02b7c30df80
07c92df0017c00df0035a810000000000000084045c0162005cd01bf0078c01290079c01e3447ac01f70078d01ef8878c01c70378e81ef0068443e5005fc01ef00781011000000000000082825420a11098602ed003941029203a401e1401a401e11032402cd0039620e50130484f14008404e1001b400ed003888
01000000000000080051018c120f0401dc) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1f80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (27c32970017c08df0025c12170487c82df1017c0a9f0037c00470015c08d70035c00df0005c20df0007c00df003700090000000000000e2058d20cb0097403d30026500551436493d164f4421532037c01df0036d01db403ec03fb0005c00ff00a4d00df0035a8140000000000000400186008d0
0834069902f64080800054010100b4507952273401c90032400091036504c00242400cd8480400cc00312026000000000000000820620e9601b400a1003a0003d130e40ae1003c420b1023f6106d201e400f1003a450e0012f400ed0008484ed0039000800000000000004605444ca5250b420ab00ac40429033bc
02210298406e5200f40ca1027040de1917) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1fa0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (02df0fb0d4017013c42efb0104d02f70007c44d72136b00100000000000000a8404009d9002400856021400114003400050002400814230520cd0930698058431620c10100706cd0203460cd00302010000000000000020004411950055404958046602110037400d50037421510234400dd8624
48a150034420c90204400c50047400d50034a001000000000000080294cc39f20c1d01910074400010087601150097e01910034406dd0035421110035400d10480480dd01c7400dd00362085000000000000042014c00f7240c801b1043cc0033223fc0333057c420730408c18bf003cc00e0003cc00fb000ec00f
f080fc00ff003f080d0000000000000600) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1fc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000048043420cd0033400cd0033400cd0030420c90003400cd0033400cd00334004d0a034200108076220d00834008d0033a013000000000000042007401dd2077401dd0077401dd0074401d10027400dd0077403fd0027409dd00c74291100e74031d08c74099d0077080300000000
00000e000fc01ff107fc01ff007fc01ff007cc01f3002fc01ff007fc15ff007fc443f000fc0433052fc003f000fc443f007fa0030000000000000e0815c00b90809c40bb003e4003f800fc403b001be40bf110fc143f0107c043b403fc0cff4a07c02df110fc48df023fb8050000000000000ac004c00d70005e20
970016d0013200742011003d400130034c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1fe0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (c10077400dd0037400fd00274095d0037400db0013400dd0037400dd0034a01b00000000000004200fc00df0037c00df0037c00df0037c00d30237c00df0037c00df00b7c425f0037c00930897c009f0027c009f00350803000000000000040217c00ff003fc00ff003fc00ff003fc00f70033c0
0ff003fc00ff003fc01ff009fc007f103f402bf001f802ff003d800d000000000000042203c00df0037c00df0037c00df0034d00db0177c00df0037c00df0077c0a5f1037c00d340f7c009f0037c029f0037a8000000000000000e200f400dd0037400dd0037400dd0034400d94077400dd0037400dd00e74105d2
027400d100474005d00374109d00358803) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2000) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (074c219f2037a01500000000000006400bc00ff003fc00ff003fc00ff023fc08ff203fc00ff003fc10ff001fc08ffa03fc00ff021bc00ff003fe00ff003db80200000000000000404bc00cf0033c00cf0033c00cf0333c00c30a33ca0cf0833e80cf0033e008f8003cc0030083e028f2003c00cf
0030101200000000000002001b401ed007b401ed007b401ed007b413e1007b401ed007b401ed005b401ed005b40129005f4016d024b6016d007880070000000000000a001f400c90033400cd0033400cd0033401c10073400c90033400cd01b240a0900034000100034004d0003400490032a00700000000000000
004f400dd1037000dd0037400dd0037400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2020) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0017c005f0817c805f021fc005f0017c005b011e5807b011ec86730099c027b009cc107f2815a8170000000000000c2048400cd0030400cd0033400cd0033400cd00b3480dd8033400c10017401c170f2544c14811500c962f0513cd00332812000000000000040000401ed007a401ed007b401e
d007b401ed007b401ed007b401e9007a481e110624818100414018900604018d0079000100000000000004204c400ed0038400ed003b400ed003b400ed003b400ed003b40ce30019440e12018600610038400611018440ed00398013000000000000040050d01cf0036c01cf0037c00df0037c00df0037c00df003
7c00d30034c014b0064c01d30024c01530) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2040) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (36148105274148da5234148d002020100000000000000000634009d00274009d00274009d00274009944244209d00244009100672009d04274109944274109d84274109d0024a0180000000000000800074009d00274089d00274009f0027400950026c809d00245009b01674009d00a7c029100
a74029d00a74429d002620010000000000000c2043c009f0027c019f0027c009f1027ca4930220c009f0024c00938027c009f0027c009b0027c009f0027c009f002708100000000000000c004bc001f0007c001f0007c001f00074001f0007c001f1007c000f4084c081f0105c001f0306010170107c001f000700
1200000000000006201cc005f0016c005f) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2060) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (734001d00074001d0005c001d00074801120474251d00045021d104440037008740a11028740a1d00074021d0807081c0000000000000e2063c00bf0027c00bf0027c009f0827c20b3687fca09b0024c1597802cc019f0067c459b0167c059f0067c159f0027a8180000000000000e6067c009f0
027c009f0027c00970027c4097052fc149f0027c009f0d2bc00ff002dc00bd403fc80bf002fc00bf00279a1900000000000008407bc001f0007c001f0007c001f0807c001b0104c001f0004c44110007c441f01074041b0107c041d0107c041f0806a01c0000000000000000434008d00234008d00234008d00234
018d05224008d00204148980234148d152) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2080) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (001f2004c02330005c00130084c00130804c001f0005001400000000000006205fc009f0027c009f0025c009f0027c409b0263c009f0027c008b0225d08870027c00970827c099f0267c009f002500170000000000000e0117c009f0027c009f0027c009f0027c009700a7c009b00244009f0026
c019f00a7c02934027c829f00a7c429f002520050000000000000620634009d00274009d00254009d08270009504274809d00244209d0026400f5002f404b1002f400bd002f4809d0025a0180000000000000e804b4008d00234008d00234008d00234008505a34148900204008d0532442ad00eb401a1002f401a
d00eb401ad0023a0120000000000000c20) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (20a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000004053c016f007bc01a7007bc01ef007bc01e1005bc01ef0078c21ef0058d01834060d01830068501834060d018f0078101400000000000000001340065003b400ed003b400ed003b402e10433400ed003b400cd0038402a100c840321400c4032100c84032d0038800400000000
00000000536004d0033400cd0033400c90033401414033400cd0030400cd00324018100484812100084012100484012d0032a8140000000000000200134007700174005d00174005d001742071001f4805c0015c005d001c4005100144005100104005100144005d00142014000000000000042153c001f0007c00
170007c001f0007c20130007c001f0004c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (20c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (c92092400cd0033400c50167402cd00b3402c10023400cd0033402cd003328060000000000000400004006d003b400ad003b400ed003b400e10018400ed003b400e10009400ed003b400e1002b400ed003b440e5003900000000000000000661544006d003b400ed003b400ed203b408eb022ec8
0fd003b408e5003f408ed001b40061000b4006d001b4046d003988150000000000000e2008d017f007fc01ff007fc01ff007fc0173007cc01ff007fc01f3007fc01ff005fc0173004bc017f005fc017f007fa002000000000000046143c00570037c009f0037c00df0837c20df081fc28df0035c00df003fc009f0
027e009f0023c009f0027c009f2035b810) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (20e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0145005d0036a00100000000000000020f4005d00374099d0037400dd0037401d501d7400dd0035400d504574421d00274009100374009d00244009d00362001000000000000042203c007f003fc01bf003fc00ff003fc00f3055bc00ff003cc00f3001fc0037042fc10b3003fc00bf002cc00bf
003f0880000000000000042007c005f0037c009f0037c00df0037c00df00d7c20df0037c00cf2017c871f0047c811f0057c011f0147c010f00370001000000000000040050c005f0037c009f0037c00df0037c001380d4c00ff0037400d304d7c411f0047c01130053c011f1047c091f0035a8140000000000000c
00184004d00334008d0033400cd0033400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2100) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (004ec4133004cc013b000848033004dc00ff007cc34df0077c00d7008cc0033007ec61ff8077a0030000000000000e6017c006f003fc00bf003fc00ff003fc00ff001fc00ff003fc00ff001fc007f003f800ff003fc00ff003fc00ff003db8250000000000000ac003c005f0037c009f0037c00d
f0837c80d30017c00df0034c00d30017c00570037c00d34037c80df0034c00df003610000000000000000080434004d00334008d0033400cd0033400854013480cd0031600c500134004d00134004100174004d00104004d003020300000000000000200074005d00374009d0037400dd0037401110017400dd003
4600d100574005d00174005100574005d0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2120) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (fc00ff1027d009f403fc00ff003d80050000000000000e2000c05130040c011700c4c02034040d01132084c08130043c20dd0036c00df0037c00d60044c63030037c00dd0037a80000000000000006200c4215122374411d0104440112044411100005480110446400d50036400dd0837400d100
64411110037400dd003588030000000000000e80404004100224000d8000480010c04480014800440010007404cd0032400cd0033400cd0800400010033400cd0833a0130000000000000c200442111207dc001d0044401110104421130045401110044410df0074403fd0037480f12b84400110077401dd007708
030000000000000e000cc0123002cc0137) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2140) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1a40179047b4212d114b60921204b4012d064a40921107b401ed017944ded0078441ed0048409ad007b485ed0178800f0000000000000a001c4014150b34881d10434010100834010d040240b091043400cd0031400cd0031502c500054000d0033400cd0032a01700000000000002004ec104b0
03740b1d0007400111827438012054400d100a7400fd0034520fd0034432fb02e44119d0033400dd0034a01b00000000000004200cc40530107c421f0687c42170327c00139086c100b03a7c00df0034c00df0134c10d502054029f0037c20df0035080300000000000006081fd003f0065c003f000fd093f000fc
003f024bc009f402d040ef203dc00ef103) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2160) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01ed0078405e5007b481ed0078401cd007b401e10079000100000000000006004f40061402b400612808420ed000b400210018400ad003b461ed8038610cd0038492cd0038400ed003b400e1403988130000000000000e0057c00531003c00530040c818f2005c80170003c801f8017800ff0036
d8cdf0837c06df0024c005f0037c00d30073a01500000000000006480bc007f00bfc083f0b0fc003f000fc0033c80dc007f003bc80ff023ec00ef003fe00f3222fc0cff083fc00ff003db802000000000000004048c08c34033c280f3283c100340074080d2802c024b0223c00cf0971805cf8071c01d70261c09c
f0233c01cf017010120000000000000200) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2180) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000c2043c00970020c609f0427400910267c029b0165c018f00e5c009e0024d009f0124c00830064c019f0024c209f002708100000000000000c004bc041f0207c021f5285d081f2187c001f0005c021f0207c001f0005c000f0007c021f0047c081f0007c001f0007001200000000
000006205fc027380df4197300dec4b7d041fc0175121d8087f021fc005f0014c005f0017c205d041cd087f0017c00430015a8170000000000000c204b482c104f3402d10072400cd00f349bc12030403cd00b3400dd0032460cd0030480cd0074401dd0033400c10033281200000000000004200f401e1005f441
61004a401bd006b40125104d411ed20794) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (21a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (bf802fc20af003fc149f0027c009f0527d949f252fd34bf0827d009f1027b8190000000000000a8077c00170104c001f0007c001f0017c001b01058041f0005c041d0004c041f0004c44130104c041f0004c001f0006b01c0000000000000080434008105204008d00234008d002340081052045
48d00304148d00204148d08204148105604348d00204008d00202010000000000000020063401950624621dd0067401dd00274309920356089d00254209d20246009d08a44009900344009d00244009d0024a0180000000000000800074209100e45079d01e74019b00a34029100205059d00244009d80244009d0
0a44069162645089d00244009d00262001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (21c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (027c209f002528050000000000000620636029500274109d12a640095042444ad104274219d00246809d80264009100240809d0024401950027420950025a8180000000000000e88434008100234048d00234008100205209000a34838d002140c8d80224808101314108500204048980234808d
2023a0120000000000000c20734401510874041d00064201400044001100074801d00040071c00044021140445011d0004603170007400171007081c0000000000000e0067c00b3052fc02bf002fc00b3002cc00b3013bc04bf002dc069f0024c15bb00afc00bf002cd97ac202fc00bf002f80180000000000000e
20e7c00bf002fe14bf202fc80bb052fc00) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (21e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (2070601c90973608cd00f0543cd08b3400cd0033400cd0435491c100f0480c90033400cd0032a03400000000000002005348051041b4817f061c4217b001f4827510d841a7d029f4805d28174805d001ec0371005c4407100174005d00142014000000000000042053c02134007c80121086cc01
32087c10130204c001d0887c001f8007c001f0004c80102884c42130007c001f00050814000000000000020057c039f00e7c009f0026c009f00a7c419f4627c009f0027c008f0025c008f0027c408f04e7c00970027c809f002500170000000000000e2007c02930027c009f10e7400930020c028200e7c019f10a
5c409e0026d009b0027c009f01244048b0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2200) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (c4012c1020009cd107b400cd003988150000000000000e000bc41f2007fc01bb004fc01b3005fc0933025f8457f027dc41ff0074c01f3007cc019b007cc09df027fc01ff007fa002000000000000064043c00df0007c005f0001c008f0007c001b4007c001f0027c00df8037c80df0036e005f08
07c00970033c00df8035b810000000000000004057c01a30063c01a30048c01ab405fc01230078c010d007bc01ec087bc41ef0079c01434068c41eb207bc01ef00781014000000000000020017400e1003b410e9004c511a9009b400250018001ed203b400ec083b400ed003b410e100f0430e9007b400ed003880
040000000000000a0053400c10073441c1) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2220) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (07c00db0027c021b0807c009f0017c221f0007c065f0006c00df0037c00d700a7c009f00a7c00df0037c00df00370001000000000000062073c00d100674001f0267400d10057c21034ce7c039f00e5c00ff0034c00da0024d00df002440adf0037800df0035a8140000000000000c201b406c10
1c34004d0243408810043418000143423090080400cd0032440c900044001902c04009d0033400cd00332806000000000000040003400a1042b400ad000b400a1041b40020301b4542d0119420e50038400e90028420250028400ed003b400ed00390000000000000000062057420e1402b402e9200b400a1201b4
4820030b4026c1678441ed0272c0de1401) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2240) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00df05b7c06d32005c009f00844009f0037c02df00b61000000000000000008043480c100234000d00036008100005000110034404d0103404cd01b3406c122005d00d00804108d0133402cd00b00810000000000000020007400d100a74811d00674009104444011920474005d0067400dd0037
400d100654109d00c44819d0037400dd0036a001000000000000080227420d120a74211d14474009100404031100474081d04c7c00dd3037400d111445889900c46009d0037400dd003620010000000000000c2007000b30221c103f000fc00b3001cc00360023c013b042fc00df003f800d7080dc00ff042cc00d
f003fc00ff003f08800000000000000c00) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2260) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000e804f400cd0032400cd0033400c10830400c16032400c500304005d0033408c10010414c90030404c10130404c90433a0100000000000000c200f401dd1074400dd0077401d1013440ef10130444c100744015d0077403f10010400d10435414d10134480d10137100100000000
00000e000fc01ff003cc20ff007fc01f3027cc09f3426cc09f7007ac007f007ec05e300dcc01f3007cc01f300fec03f3007ba8030000000000000e6017c00ff002fc003f100fc00bf200bc003b000fc003f0005c02df003f008de010fc902b000fc10bf00b7000ff003fa8050000000000000ac007c40934027c80
1f0007c40930004c00134007c401b2507c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2280) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (f142b4481d100734004d0034520f100774015d00574015d005740b511054a01300000000000004202fc00df0037c00df0037c00d30034c08d30034c08d34137c005f0034c20d31077c015f0057c055f0055c015b00550803000000000000060017c00ff003dc00ff003fc00ff003fc00ff00bdc0
0ff003fc007f003fc00ff007f80977025ec097e025dc0977001d80050000000000000e2003c80df0036d00df0037c00d30034c00d30076c00d70036c065f0036e00d34234d015b4054d01534054d015b4017a80000000000000006200f400dd0036400dd0037400d10034400d10036400d100344011d0037400d11
014400d90035400d10034400d90035a007) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (22a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (044c011f1017a81400000000000006600bc00ff003fc00ff003fe00ff803fc08f7023dd00fb803fc00ff823fc00ff000fc08bf022fc08bf822fc08bd003d380200000000000000404bc00cf0033e40cf0033c00c34035c80cb4232c00c78133c20cf0030d00c30203c008f0023c008f0021e488b
0030181200000000000002003f401ed007b401ec007b401e12079121c9067a401e5007b4016d0878409e1004b401ad006b401ad006b409a1407800060000000000000a005f400cd0133400dd0033400c11035402d90036504d542334804d0030400c148074049d80274029d01274029901b4200300000000000002
004f400dd013f400fc0037400d103b5489) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (22c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0017c005b3014d4053009cc00534017c017f0014c005f0094d02574094d02534094d025f009428170000000000000c204b400cd0033400cd0033400cd0031400c546d0500d10033401cd1030400cd00204002110084002100084002d00132016000000000000040007401ed017b405ed007b401e
90078401e1007c401e1407b401e50078429ec20684a12100484812120484012d0059000000000000000006204f400ed003b402ed003b400e50039514f50038500f1403b4206c3038510cc00284402100084002100086802d001990130000000000000e0057c00df0237c00df0037c00d34834c0cd30030800d3083
7c007f0034c02df3024c01170044e01130) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (22e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (b401ad006b401ad006b401ad002020100000000000000200634009d00245009d00274009104200409021325009100244009d00244209d002f400bd002f400bd002f400bd0424a01c0000000000000800074009d00244409d00274009040a54069054644519114214809d00254009802e74029d00
a74029d00a74029d00a420050000000000000c2043c009f0024c008f0027c00930264d05835064d05934024c008f08254008f0027c089f0167c009f00274009f002508100000000000000c004bc001f0007c001f0007c00130006c821b0007c001f0007c081f0007c001f040fc101f1407c101f2407c101f040500
1200000000000006205fc005f00176005f) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2300) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (734001d00074051d000740011094c51f0340544051100074421f00054001d00474011d00474011d004740511014500180000000000000e0067c009f006fc039f0027c009300a4c019300a4c0093402bc059f0024c05bf002fc00bf002fc20bf022ec00b700afa01c0000000000000e6067c009f0
027e149f0027c009f0527c149f052f8149c0023800ff0027c809b0527c149f0527c149f0527c149f0527b8190000000000000ac077c001f0104e041f0007c00130000c04130004c00134004c041f0004c041f000fc000e0003c000f0003c000f0006b8180000000000000080434008d05204148d00234008100214
d48100204008100214148d00215148d006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2320) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (001f0007c000f0007c801f1007c001f0007c00130005081400000000000006005fc009f0027c009f0027c00970027c009f54a7c00940427c019f0025c009f0027c009f1027c009f002700097002508130000000000000e2017c009f0027c009f0027c209b4024c809b00e4d009b0023c0a9d0026
c009f0027c009f3027c009f0026c809f002120050000000000000620634009d00276809d002740099082c400b100284208900374009500274009d00274409c00274009d0027400d9002528180000000000000e804b4008d00a34028d0023400890128400a90838510a900234088d00224028d05234548d05234108
d01234108d012120120000000000000c20) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2340) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000004057c01e3007bc05ef007bc01e3005ed0163007cc01f3007bc01ef007bc016e006bc01af006bc01ef007bc21e3005c1814000000000000020017400e1045b404ed003b400e1009a400e10038400e1000b400ed003b0006d003b400e9003b4026d00bb422610018800400000000
00000a0053400c10073400cc0833400c10166502110080401014073400cd00334204d2673400cd09f3400cd0033401c10012a01000000000000002005340051005f4005d00174005140d450651401458651001f4005d00174007d009f40c7931df4017c005f40071401c2010000000000000042053c00134007c00
1f0007c0013000cc2433408cc10330207c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2360) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (dd0012400c10010400cd00304204d00034000d00034000d00034000d00312802000000000000040023400e90028400ed003b400e1001a4002d002a400214018410ed00384006d041b4006d001b400ad002b400ed00190000000000000000062057400e10018400ed003b400e100a85006d061840
0e10218500ed02384006d100b400ad00ab4002d00ab4082d001900150000000000000e000bc01f3006cc11ff007fc01f3405cc01bf006cd0133005cc01ff007cd016f205fc017f007fc01bf206fc01ff005d2006000000000000066043c00df0013c00df0037c00df0425c009f4007c001f0027e00df0037c005f0
027c001b0027c005f0017c005f0035b810) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2380) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (117400d10016a001000000000000080007400d10493420dd0037400db0094483910062c131100e7400dd00374005d00070001d00874031d00c740a11406220810000000000000c2007c00f34017c00df003dc00f3422cd0873055cd00fb402fc00df003fc007f040fc00bf000fc047f005dc0133
011f08800000000000000c0007c40d70017d00df0037c00df2015c421f0025c021f40a7cc0df2037c005f0037c80df0017c029f0027c029f00070805000000000000062073c00db4014c00ff0037c00d38026c00df0016e00d30020c00df0034f405f10b7c00df1017c80df0017c009f0015a0140000000000000c
205b400c90010400cd0033400c10022400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (23a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (004bc003c120f80123001cc0133000dc00f7007fc0033000cc003e000c8003b000ec0037000fa0030000000000000e6017c00ff001fc00ff003fc00f7001fc00ff003dc00ff001bc00ff003fc007f000fc003f000fc003f000fc003f002fb8050000000000000ac007c00d30007c00df0035c00d
34020c00030004c200b0017c00dd0037c005f00174005f0017c005f0015c005300161800000000000000008043400c14013400cd0033400c90010400410076480c10013400cd10334004d00234008d80234008d00234008100000010000000000000020007400d18007400dd0037400d1002061091000460809085
7400dc00374005d00b70005d0037402dc0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (23c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (7c009f200dc00b70077c01af00b180070000000000000e2208d015a20678009b10c5c01170045c030140f4481034045440df4033c63130040c01070446c070f40c6c60173047a8020000000000000e200c420d920674089940c4441d510254031001b6401910844400d980374111100e44031d00
664011902b4408d10005a803000000000000040040400091023480891001440814041400111836400111005640c900334000100004000500024000d0002400050003a0100000000000000c2004401d10027480910004440550204401110016401112044400d020774011100445011d004440111004440111004708
010000000000000e080cc003b000fc01bb) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (23e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1b009ed086b405ad024c10979227a40135014b601210358509ed0079401a10079401a10a69403a1004b42161007880060000000000000a001f40305000140085088440541014060b050093411018901503cd003341a050001680010001400010003400010002a00700000000000002084f402db0
066c0f9b0044407db2436c01110033412910150401fd0035c23910124424910024400910037404d10034a01300000000000004200fc84530224c00930e84c409300348401611b7c00130017c08de0837c029700a5c429310a4c02934083c025300b50803000000000000060017c2267002bc00b7000fc00ef00d8c
103f2875c003f0017c10c7003fc00bf200) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2400) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (09cc0878501cd00784c1c10073441e10070401c10071000300000000000004204d400412038400e5000c400e5003040021001b480210018400ed0038400ed0038400e1083b400e10038400e100398813000000000000040050c00130024ca0972004c00030026c000b0077c00174002c00df0034
c005f0024501534077c00590034c01d30007a01500000000000006600bc20fb002ec04bb000fc20ef003fc803b012f800fe011dc00ff003dc00ff003ec08ff083ac20e7003fc00ff003db80200000000000000404bc10070025c00970000820c30014c04053033400014191c00cd0033404c74011c60c34011c08c
300334028340b010120000000000000200) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2420) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000c20c0002834424d21970164c00830126c409f20e7c09930664d039f0024c208b0027c209f0024c00830027c0093002708100000000000000c004bc001f2007c00170205d001f0101c001f2207c081f4007c001f0007c0c1f0407c0c1f4007c081f0607c041f0003001200000000
000006209ce0773445cc455f205ec0072009ec487b005fc0077409ac005f0014c017f001cc0172029fc0873009c40373009da817000000000000042049412c10034401cd04b2486c5083262bc10433601c10270000dd0030402cd00b0003c102f3401c14070509c143f32812000000000000040000401610070541
ad006a411f1107a40129007340165005e4) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2440) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (bf253fc00ff402fc549f0025c20bf002fc00ff102fc00bf002fc00bf002fb8190000000000000ac07ac04130114c00130004c04534106c001d1107cc0114104c241f0006c241b2107c241f0104c04130107c04134106b01c000000000000008043514890520400d800245148105214009d0d2340
08105244148d00225148d05634148d052051481452341481052020100000000000000200624009140644089190247009100a76069d00a74409100a44029d00264009d00274009d1024401910427410910424a0180000000000000800044009b00244018b10605029100e54028d00a74109100a44039d00244009d0
0274409d00244009100a34029100a62001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2460) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (024d029700a7a8050000000000000620604049130264009500254449528a3488910827400b1042c420850027003b1046c401bd002c782b1052e404b10225a8180000000000000e804a400810522410c121644018110236808904a3400a102280c0cd0023402a100a8400ad0028400a100a8403a5
00eba0100000000000000c207040211000040015100540e11400760051408740031008010a1780074023100844021d0014480110004402110087081c0000000000000e0060c10b1042cc00b300acc0cb3003fc20ab012bc00934124c06bf0023c01930064c119b0464c11930164c01970067a0180000000000000e
4064c00bf0d2fc94ad052fc14bf052e400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2480) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (4030400c10070410c100f748329080b402c900114004d0833400c10071400c10072500c10072a0140000000000000200504227b001c54071001842171005e41271021f40151015740271001c4015d0017480510014400510010400510014a014000000000000042050c0a172004c00134004d011
20a86c40130087c101b00c7c001b1006d003f0007c02133007c00130004c00030001081400000000000006005fc108f4125c409f80a7c009b04e7c819f0827c009f2123c509f0027c009f0023c008f0127c098f4025c019f006580150000000000000e2014d04932166d00839064c008380674c29b0027c0a93102
4c009d0027c61934064d039f10e4400930) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (24a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (b428ad302b448615228400ad002988150000000000000e0000c0d72017cc4133007cc01f3087cc01b3006f409fb2079c09ff805f4013f007fc01fe006fc01f3006cc01ff006fa000000000000000064043c401f1017c001f4037c00df00255201d0007840df2017c001f0016c405f0007c209f00
34c001f0017c001f0015b810000000000000084054d01874048c4173006cc41f3007ec01e1406bc01eb107bc81eb805bc816f005bc21e34079c01a34052c414340501015000000000000080014400290038440610038610e1403a401f100bf490e1403f440e100594114d002b400a100f14404100b8400a100b880
05000000000000080050403c53034410c1) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (24c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (07e041f0035c00170a97d00930695c0a9f00a7c06172027c42df0017c00df0427c401f0097c005f0137c118f017700010000000000000e2054c06834074c041a0024c0a9340f4e01910027c13d100f5c00dc0016c02df00774425f1097c00d301b4d01df00f5a8150000000000000c20106a1410
1d64810c18344208d00804000000c3000c094704001400134060d10c34048d11234020100400020d0003080400000000000004200060c613708400298028410e10010600b1440b44121042d440ed001a4012d041b400ed002b400a1000a4006d0209000000000000000006015448c6101385002521384002100385
04a1112b40ae10038420ef011b4002d022) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (24e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000f0015c009b2017c00534007c009f00044005f0006b00000000000000000804040001403240009801300001c003400050023400c100304000d20114008d00234010100034204d00205008d00202010000000000000020005401110034481110027401510422401153067404d104145061d0015
4009d0037400510087400dd0024400dd0024a001000000000000080204c211104b6c870b0e974079122474471111c7401d100344401d0015c12dd00074801100134001d0014c001d00162081000000000000042201c20930024c8033006ec0093803fc10b70403c01f60178c01ff001fc00fb001fc0073001fc10b
f0016e005f001f08800000000000000600) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2500) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000e8043400cd0032404cd0033440cd2033484cd0911584d11030420c5a027402cd00b0408dd0030406cd1833400cd0033a0100000000000000c2007401dd0074406dd0077401dd0077401dd0074411d10874400d14077403f700fcc03ed0075406fd2077481d70077080100000000
00000e000fc01ff007c418ff007fc01ff004fc033f08ccd0133487cc01b3007fc81ff007cd41ff207cc8cff007fc01ff007fa0030000000000000ea015c603f103fc002f201bc00bf000fc002b800f4003b100fc003f101dc00bf000fc003f000fc003f000fc003f000fb805000000000000008001c00130024c00
131026c40d10006440170807480d14034c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2520) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1d0004000111030484dc00e440bfd0afc40bfd0034400fd0037400dd0034a01300000000000004200fc00df0037c40df0037c00df0037c00df0834c80d30236c00df0024c08df0234c08df0034c00df0037c00df0035080300000000000006001fc00ff003dd00ef003fc00ff003fc00fe001e40
0cf603fc08fb0c3fc20d7003dc00fe183fc00ff003fc00f6003d80070000000000000e200bc00df0036c00df0037c00df0007c001f0025c00130034c02d700f3c00df0034c00df1034c00df0037c00df0037a80200000000000006200f400dd0036400dd0037400dd00074001d0025400111034480d500f7400dd2
036400cd0035400dd0037400dd0035a803) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2540) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (037c00df0037a01500000000000006600bc00ff003fc00ff003fc00ff080fc003f002fe003f483bc00ff0a37c10ff02bfc08ff203fc00ff803fc00fe003db80200000000000000404bc00cf0033c00cf0033c08cf0233c00cf0010c40c38232c20df0630c00cf0030c00cf0030c00cf0233c00cf
0030101200000000000002001b401ed007b401ed007b401ed007b441ed8078501f12078403ed2078501ed0078501fd0078401cd007b401ed007880060000000000000a001f400cd0033400cd0033400cd00034000d2000400010072500dd00f0400cd2030400cd0030400dd0033400cd0032a00700000000000002
004f400dd0037400fd0037400dd0007400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2560) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0017c005f8017c005f0097c205f1015c217f01dec20530815c805f0014c005f0017c005f0015a8170000000000000c204b400cd0033400cd0033400cd00034000d01034000d10324415d8017400c10031400cd0030400cd0033400cd0033281200000000000004000f401ed007b401ed007b401e
d007b401ed007b401ed0079411ed005a405e10179609ed0078401ed007b401ed0079000300000000000006204f400ed003b400ed003b400ed003b400ed001b400ed203ac00fd201b488e141b0500cd0038510ed003b400ed803988130000000000000e0057c00df0037c00df0037c00df1007c001f0827c801f003
5c00df0016c04d30134c12df0034c0cdf0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2580) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (04148d00204148d00234008d002020100000000000000200634009d00274009d00274009d002f400bd802f400bc0826001d900245009100244009d00244008d00274009d0024a0180000000000000800074009d00274009d00274009d00274009d00274009d00244219000244009142645099d00
244009c00274009d002620010000000000000c2043c009f0027c009f0027c009f0027c009e0027c009f0026c009b0824c00930020c808f0024d009f0027c009f002708100000000000000c004bc001f0007c001f0007c001f180fc203f000fc003f0007d011f0107c000f20064001f0007c001f0007c001f000700
1200000000000006205fc005f0017c005f) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (25a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (734001d00044050100074001d00044051101444015d00044011d100f4021d02874020d00044011d00074001d0007081c0000000000000e0063c009f0024c1193002fc009f0024c08930224c229f082dc02bb0027c019f0067c019f0024c199f0027c009f0027a8180000000000000e6067c009f0
027c149f0027c009f0027c149f0527c149f0027d34bf002fc009f0027c809f2027c349f0027c009f0027b8190000000000000ac073c001f0007c041f0007c001f000f8001f0007c401f1006c001b0004c04130104c041f0004c040f0007c001f0006b01c0000000000000080434008d00234148d00234008d002b4
00ad002b400ad002040181002441481152) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (25c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (061f000fc003f000cc003f0004c001f0007c001f00050014000000000000060057c009f0027c008f4027c009f0027d009b4027d009f1027c009f0027c009f0027c009f0025c008f0027c009f002580150000000000000e2017c009f0024c00b30027c009f00a4c06960024c009f0025c389b0227
c009f0027c009f0026d009f0027c009f0027a0050000000000000620634009d00246009100274209d00e44018500604218d08244409d002f400bd002f400bd00264009d00274009d0025a8180000000000000e80434008d00205108100234008d00204008500204208d0021404c9002b602ad002b602ad00224048
d00234008d0023a0100000000000000c20) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (25e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000004057c01ef007ac03ef006bc01ef0078c0ff7017dc09ff0878c81ff004bc012f005ac016f0078d01ff007bc01ef00781015000000000000020017400ed003a400ed002b400ec0038404e5223940ced2028400ed00bb400ed003a501fd0038408ed003b400ed0038800500000000
00000a0053400cd1032400cd0023400cd0030500c45031500cd0030502dd00434410d20024000d0030480cd0033400cd0032a0140000000000000200534005d00144005d04134005d00144005100144005d10144007d00574045d10144005d20144005d00174005d0014a014000000000000042053c001f0004c00
1f0007c001f0084c02130004c201f2004c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2600) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (d900b5422d100224005d0062400850021400850032400cd0033400cd00332804000000000000040003400ed0038400ed003b400ed0038400e10038408ed003a400f990184006100184006d003a500ed003b400ed00390000000000000000062057400ed0039400ed023b400ed0239418eb063949
0e30228448ed042ac02a500b9402e70038400ed083b400ed003988150000000000000e0003c01ff007cc01ff007fc01ff007cc41f300fcc01f70078c01eb025cc0173004cc013f007cc01ff007fc01ff007fa000000000000000066043c00df0035d00df0027c00df0037c02db00b6e04df0027c00df0037c00df0
025c009f0037c16df0037c00df0035b810) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2620) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (037400dd0034a001000000000000080207400dd0034500dd0077480d90036c00db0036800dd00354059d0196c025b0086c021d0034400d90037400dd003620810000000000000c2203c00ff003cc00ff027fc00ff003c800f3103d800ff003cc00ff082cc20930834c00df003cd00df003fc00ff
003f08800000000000000c0007c00df3037c00df0037c00df0237c44df0137c64df0035c06df2017c024f0093c024e0035c00cf0037c00df00370001000000000000062057c00df0034c00df0037c00df00f4c03f320fcc83ff0036c46db0024c20930824c009f0836c00ff0037c00df0035a8150000000000000c
2013400cd0031400cd0033400cd0931402) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2640) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000ec003f0068c0123804cc4133104f0813f007cc10fb043cc003f087fc01ff007ec01ff007fa0030000000000000e6017c00ff003fc20ff003fc00fb003ec00ff003ec00ff003fc00bf080ec403f000ec403f003ec00fb003fc00ff003f98050000000000000ac003c00df0034c00ef1037c00d
f0035c00e30038c00ef0034c009f0034400d10034400df0034c00ff0037400dd0036b000000000000000008043400cd0030400cd0033400c90033400c90032480cd0831400cd00034400900134004d0030400c90033400cd00302010000000000000020007420dd0034400cd0037400dd0835400d00034400dd013
4401dd0034400d100244009d0034400dd0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2660) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (7c008f003f440fd003fc00ff003d8005000000000000042202c02131896c09930044c019d0004d121110144001b0c444809f2036d00d300349011f0036c00db1037c00df0037a8000000000000000e200d411c504226809100346015d00344005040044025900044001d0036400d110344039c00
37400dd0837400dd0035a803000000000000040042400c100024008100304004d00304001100004000908004001d1032414c105306400d0032400c98033460cd0033a0100000000000000c2005400d500244019108244011d98640015100046404120044001d0074442f140bc4011d0077401dd1077401dd007708
010000000000000e000ec0073000cc01a3) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2680) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (18411e9807a401b1006802129006c401e10368401e900f85096d0078401ed027b4892d007b401ed007b401ed007880060000000000000a000c4044112324068100174030900214008181e44119968364064d0830400dd00774000d0033400cd0033400cd0032a00700000000000000004c4039b0
2744058120744015b00944244100544415100044818d8034460f1007c4209d0037400dd0037440dd0034a01300000000000004200cd02932004ca0970077c24138c15c201f8214c421320c4c089f0034800d342348221f0037c00df0037c00df00350803000000000000040217d003f421dd00bf00a7c008f000fc
007f001fd0077124dc88bf003dc00d7003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (26a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01ed007a405e1437a601cd107b601ed007b401ed0079000000000000000004004c400810033420ad0038400ad0008400e10038500e10038d00fd0038410c10330400ed083b400ed003b400ed00398813000000000000040050c20130037c209f0816c809f00044018b0030d00930834c80df0034
c08d34136c01df0037c00df0037c00df0037a01400000000000006600bc08df4235c009f40358085f0077c00d30927d00d70037c205f0037d08d30034c00df1837c80df1037c00df0035b802000000000000004058c00d34036d008340338104b0031c04814124c108b11368005d0a30c80cf0033c00cf0233c00c
f0033c08cf003010120000000000000200) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (26c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000c2041c02970067c01930064c008f0027c05938224c00930024c099f8024c00930027c009f0027c009f0027c009f002708110000000000000c004bc000f0087c001f0005c401f040dc02171285c801f0005c831f0005c001f0007c501f0007c001f0007c001f0007001200000000
000006201cd0c71421fc015f001c5207f0096500534056c005340108005f0016d00530016c027f0017c005f0017c005f0015a817000000000000002058403c10277008cd22740040d0092400c00872400d10032400cd0032500c11030429cd8833400cd0033400cd00332813000000000000042000601e1007b401
ad00784110d205a401a1007e401a1007a4) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (26e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (9f2527c149f0527c149f0027c349f0527c20bf0027c209f0027c009f0027b819000000000000080079d04172107c00130104c045f001fc00114004c000100005001d0004d04110107c04170007c001f0007c001f0006b01c0000000000000000405148905234008905224148d002b400a1002840
0a1486c600ad00204148145234148d00234008d00234008d002020100000000000000000614009521274809101a44c49d012f650b18038500b1002c4008d00246008142234009500274009d00274009d0024a0180000000000000800044079304674889b0066c029f00a74019b21a441b9102e44069d0024500910
0674809d00274009d00274009d00262001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2700) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (027c009f0027a8050000000000000620614009100344049d04374089500264009140204009120305008100264008100274209d00274009d00274009d0025a8180000000000000e88484028140a04008501a34428d002340081042040091202000481402241081c0a34028d00234008d00234008d
0023a0120000000000000c20714064109844001109064001f00070001100044241105044041140044011100474225d00074801d00074001d0007081c0000000000000e0060c06b301acc00bb51afc04bf002fc00ab002ce08ab002ee02ab002cc119900efc059b0027c009b0026c009f0027a0180000000000000e
2067c14b5052fc80bf052fc00b72027c00) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2720) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (30f14c0cd00b0400cd0470403cd0070521c90032400c90063400cd0033400cd0033400cd0032a014000000000000020012c817100df40071021c4007d009c4107d009c4866d001c40a71101040051011f4405d08174005d00174005d0014a014000000000000042051c0a130087c00170085d001
f2404e001f0204c901f1404c081b0005c00130007c001f0007c001f0007c001f0005081400000000000006005fd048f4063c00930262c019f0067c00970027c00974025c00970024c00970023c449f2027c009f0027c009f002580170000000000000e2014d01934364d008700e7c109d822742093082450093202
44009300269009310278039e0027c009f0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2740) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (b400ed003b408ed003b400ed003988110000000000000e000ac01f20a6f401b3024c501f3085bc29be107fc01ff027fc01f34078983f7407f801ff007fc01ff007fc01ff007fa002000000000000044043c409f0037c401f0017c005f0007c201f1037c00de0037c80d70030c0ad705a7c20dd00
37c00df0037c00df0035b810000000000000004051c01e34073c01a3405dc01af00685012f0078d01ef2078c01eb087ad05cb407fc01ef007bc01ef007bc01ef0078101400000000000000081240061043b4102100b8401cd00b8401bd1038480fd0438400f9003a404e9103b400ed103b480ed003b400ed003880
04000000000000000451500c104f3440c0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2760) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (05c005f09a2c001f0086c021f8137c021f20a7c801f0087c00df2037c00df0027c20dc2037c00df0037c00df00370001000000000000042052c0a5340374210306d44104100f7401190836081df1037400d38030d00f50837c8adf0837400dd0037c00dd0035a8140000000000000c201a442d10
2924010188154214500934010d00024811d0007400010030440c14833400cd0033400cd0033400cd00332806000000000000040002400e1003b400a10018400a1061b61029002a4102d000b400e10038400e5002b400ed003b400ed003b400ed0039000000000000000006215450861032a410214309400ef003b4
0cad321b400ed023b088210238420f1002) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2780) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (001b0034d00fd883fc00df0037c00df8837c80df0036b000000000000000008040400414020420010003400050023400080004500014000420012030400cd0033600cd0833420cd0033400cd003020100000000000000200044805100254811140454425501074001100b4402d10034642c90034
400dd0027600dd0037400dd0037400dd0034a00100000000000008820c4329102b444711a0c6c0011404340f130000422110884601114034420dd1077400dd0037400dd0037480dd20362081000000000000042200d02930075c00330014804b1006fc0033015cc08f3023dd043b003cc00ef012fc20ff003fc00f
7203fc00ff003f08800000000000000c00) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (27a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000040043400cd0033400cd0030410c15432590c12010404853320408490033400c90030400c11032408cd0033400cd0033a0100000000000000c6007401dd0077441dd0075406f101bc406f500e4418151401001110076401dc007440ef503bc406fd0077481dd0077180100000000
00000e010fc81ff007fc01ff007cc14f3052cc14f3151cc20f3003cc64f3407fc01fb007cc0cf3122cc0cff107fc01ff187fa8030000000000000e4017c20bf001fe003f000ee002b000fc0036000f8203f080ec203e003fc00ff082bc00ff003fc00ff903fc80ff003fb8050000000000000ac000c00922015d00
110015c40970007e00134004e201300044) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (27c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (fb04c6c00d00017400dd0033400dd0034480f10034401fd0037400dd0034a01300000000000004200fc00df0037c00df0034c00d31024d00d310b4c82130027e021f0037c00df0034d00d34024d00df0037c00df00350803000000000000060017c00ff003fc00ff003fc00fc0029c00df04cbdc
09f024bc006d003fc00ff003fc00df002dd20ce003fc20fe003d80070000000000000e220bc00df0837c00df0034c20d32036c00d30074c2b570474c4a9b0037ca0db0034c00d30036c00df0037c00df0037a80000000000000004000f400dd0037400dd0035400c10126480c500a4400451815000910036400dd0
834500c50122480dd0037400dd0035a003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (27e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (037c00df0037a01500000000000006200bc00ff003fc00ff003fc00ff083fc08ff023bc207f523f400bf083f400fd003fc00fe003fc10ff083f800ff083db80200000000000008405bc00cf0033c00cf0030d00c30020e20c30200d028302034004d0833c00cd0030400c30024c00cf0a33c00cf
0230101200000000000008201b401ed007b401ed007a401c91260401e9227a61921026b4012d027b401ed0078401e10268411ed007b401ed0078800600000000000008000f400cc0833400cd0030400c10030440c10000481c11013400cd8033400cd0030400c10030441cd0033400cc0832a00700000000000002
004f400dc0037400dd0036c00fb0034400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2800) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0014c005b0056d00530096c015b00d4c01430017c005f0017c00530014c005f0017c005f0015a81700000000000004004b400cd0033400cd0030400d94022400c506624640910c0408010033600cd0033400c50060400cd0033480cd00332812000000000000040013401ed007b401ed007840de
9007a409e1005a401c940f8401e1407b441ec207b405e10478505ed007b401ed0079000300000000000004605f400ed003b400ed0038414e10238408c50c10400a1102840041003b400ed003b408e5043048ced003b400ed20398813000000000000040043c00df0037c00df0034c04d30824c04d34124d0153001
6d00933073c00df0037c0cd30124c04df0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2820) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (04148145205148d00234008d002020100000000000000200734009d00274009d002440091802460081002f408b90028620dd00274009500244009140204009d00274009d0024a0180000000000000800074809d0025c009d00244009b0026c809101274009100244009d00274009d00244009100
245819d00274009d00262001000000000000042043c009f0027c009f0024c00930020c009360a3c009b5024d009f8027c009f0024c00830024c059f0027c009f0027081000000000000006004bc001f0007c001f0007d00170205c001f008dc4837010dc103f1007c001f0007c001f0007c800f2807c001f000700
120000000000000e201fc005f0017c005f) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2840) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (734001d00074001d200440515404142f11029440f1540555001d00074001d00054151102444110d00074001d0007081c0000000000000e0063c009f0027c009f0024c05931164c0d93016cc05b32464c05bf002fc009f0024c05930264d01bf0027c009f0027a0180000000000000e0867c009f0
025c009f0027c149f052fc149f0027c949f05238209f0827c009f0027c149f052fc148f00274009f0027b8190000000000000ac07bc001f0007c001f0004d04031100d0413210f4041b0104c041d0007400170004d04131104d041f0007c001f0006b01c00000000000000a0534008d00214008d00204148905224
1481052b494a1a528414ad00234008d002) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2860) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (801f0007c001f0004d00130004c00170007c001f0005081400000000000006004fc009f0027c009f0025c008f0265c009e0027c049f0123c408f0027c009f0027c008f0023d009f8027c009f002500150000000000000e2017c009f0027c009f0026d00970026c009340e0d00930024c099f0027
c009f0025c00934024c008f8027c009f002528050000000000000400634009d00274009d00264009500274009102244108500254409d10274009d00254009101244009d00274009d0025a81800000000000004004b4008d00234008d00224128505a24008100204708144205038d00234208d202148c810020428c
d00234008d0023a0100000000000000c60) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2880) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000084047c01ef007bc01ef0078c07e30478c03e34048d01c308f2401cf007b401ef0078505c14170501e7007bc21ef00781014000000000000082007400ed003b400ed003a404c1003a400c1243a400e9a03a400ed003b400ed0038404e10138400ed003b400ed0038800400000000
0000080053400cd0033400cd0030400c00034400d10050441810032400cd8033600cd8030120c100304408d0033400cd0032a0140000000000000200534005d00174005d0016c00510016c0051009ec045b001ec005d00174005d00144005110145c07f00174005d00140014000000000000042043c001f0007c00
1f0004c00131004c00130104c00134004c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (28a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (c50102422c912b060ccd0033680cd0031400c10070400cd2033400cd80332806000000000000040003400ed003b400ed0038400e10430400e1021a400a9023a000ed003b600ed2038400e10038508ad003b400ed00390000000000000000042157400ed003b400ed0239400f100384c0f5003840
0b1203c404ed003b400ed0039400f1003c400bd083b408ed00398815000000000000042003c01ff007fc01ff007cc03f3007cc03f3006cc03f300fcc01ff007fc09ff027cc03f300fcc03ff007fc01ff007fa002000000000000062043c40df0037c00df0037c02df4237c02df00038029e00b7c00df2037400dd2
037c8adf02b7c02960037c00df0035b810) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (28c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (037600dd00368001000000000000080217400dd0037400dd0034400db0037400d14044421db0034400dd0037400dd0034400db0037400dd0037400dd00362081000000000000042213c00ff003fc00ff003cc00f3003fc00f32014c01b3003cca0df003fc00ff003cc00f3003bc00bf003fc00ff
003f0880000000000000060007c00df0037c00df0037c00df0037c00df0a35c90872433c80cf2037c00df0037c00df0037c209f2037c00df003700010000000000000e2057c00df1837c00df0034d00f3003cf20f300c2d05db403ec02df0837c00df0034d00f3417cd00df0037c00df0035a81400000000000004
2013400cd0033400cd0031400c14030400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (28e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (214338504214338514614018500214518124214008404220028910614008500214008500214000000000000000000e2017c00ff003fc20ff003fc00ff003fc00ff080fc00bf203f800ff083fc00ff003fc00ff003fc00bd003fc00ff003fb8050000000000000ac003c00df0037c00df0034d00f
3003fc00f30014c00f3003cc00dd0035c00df1834ca0f1003fc00ff0037c00df0036100000000000000000a043400cd0033400cd0030400c90033400c10830580c94030400cd2033600cd0030500c90033400cd0033400cd00300010000000000000020007400dd0037400dd0034400c10033420d1022440891003
4400dd0035000dd0034400c110374019d0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2900) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (220104004010100404000100004000000000000000000000000040001000040cc1023040001000042c010320400010800c1880000140c0204100240200004008100004000100000000000000000000000008000200108000200238004600338020e00028004220818000a20108100204c2802460
00080002000080002000000000000000000000000008440211108440211108444211808444e11038444221118444a211084442051286446210084402110084402110000000000000000000000008000200008000200208000a00408008a00028008201028068220208008200218808a20008000200008000200000
0000000000000000000008500214008500) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2920) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0008000200008000200108004200828020a00408020a2080800c600508908200618804a000280002000080002000000000000000000000000008500214238500214208520e14018514614028500204c0813822420810022442ad00e2401850021400850021400000000000000000000000000000
0010000cc00230000000000024400010004000200004000100808c2011002c0200000000000000000000000000000000000000000000400010100400010100400010c00404810010414010a00404420100904810910024000020400810000400010000000000000000000000000010000420010000400010000400
0108c0402010000410010880420010c824) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2940) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (8800a00500404a20910c04420800400a100004000200000000000000000000000008100004000100004328124e04200138804400128004228120a24400008a24a209088244001006040001000040000000000000000000000338400210008400210038418a10408404210108414210e18c0ce201
08424c10018c3020000840ce10008400210000000000000000000020000800ce0023800ce0013800820072802ce00808000600008008e20808804208238024e20f3800ce0033800ce000080000000000000000000008400210108400210008404010418404610028400220008404a10208204210128c28e1000840
0210008400210000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2960) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000000000000000000000000002583c2c2c025a401980358421840002402643cacfcb2c0264026400000000000000000000000000000000000000f0f000000000000000000309080800000100010f09080800000100010f08080800000104010c0000000000000000003c3c00000000
0000000000000000000000000001010400000001080009020000000001080009010400000000080008000000000000000000000000000000000004208330000000000000000110004000100000c00100000020120010c00100124e0080000400000000c40000000002010820000000000000000000084000100004
0001010842441010040481050042401093) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2980) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (ffffbc0000000003fffff7fc0000000003ffffffdc0000000003fffffffc00000000000000000000000000000003fffffffc0000000002fffffffc0000000003fffffffc0000000003dfffdffc0000000003fffffffc00000000000000000000000000000003fffffffc0000000003fffffffc00
00000003fffffffc0000000003ffffdffc0000000003fffffffc000000000000000000000000000000000000000000000000cc2014141000000000cc4024448000000001115448dc940000000000000000000000000000000000000000000000000000000000200808000145400004200028080145400150016001
6003796fe9780000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (29a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (04208828200000000000000000000000000850021400850021400850021400850021412850c230508524e10018500234008500614108404a10908404210000000000000000000000000000000003fffffffc0000000003f7f2fbfc0000000003fbfffbf80000000003fffffffc0000000003ffff
fffc00000000000000000000000000000003fffffffc0000000003f8edf6f00000000003f77ffffc0000000003ffeffffc0000000003fffffffc00000000000000000000000000000003fff6fefc0000000003fff7fefc0000000003fffffffc0000000003fffffffc0000000003fffffffc000000000000000000
00000000000003fffffffc0000000003ff) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (29c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00400010000400010000421010c000030800004000100004000100004320008c00030800c04000000000000000000000000040001000040001000040001000040001010040c030110008c10000400030000400010300504010010500c10000000000000000000000000800020000800020000800
0200008000200128004204808024a00008000200008000600208004a04908004204000000000000000000080000844021100844021100844021100844021112844c211508c64e15018440211008440611338444a15d085542110000000000000000001000008000200008000200008000200008000200018004204
208010e00028000200008000a003380006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (29e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (10840021032840c210818c10a10000000000000000000000000800020000800020000800020000800020011800ce04008824604008100200208000200318804200d28120e04000000000000000000080000850ce14008500214008500214008500214308400e14128528a1400850021410850021
0028500214218c00a10000000000000000000100000000000000000000000000000000000000002000c000930000000000000000000000000200104c041001200000000000000000000000000000400010000400010000400010000400010120404010130c04024000400010000400010110404814130400c14000
0000000000000000000000100004000100) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2a00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000400010000400010000400010000400010020c34830920410010400400010100400014100424010800c004148000000000000000000000000100004000100004000100004000100004010108000200900000000000000200100004220838004c2000080000000000000000000000000084002
10008400210008400210008400210028400a14d08400210008500214008400210108400210008c20614c00000000000000000020033800ce0000800ce0033800ce0033800020010802ce00028008a20b3800ce0023800ce00138024200338800600008000000000000000000000840021000840021000840021000
8400210328d04e30928410a10008400210) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2a20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (8003f8040000000000000000000869412000816a000400000000000000000f8000000000000000000000000000000000000003d01580c8026403fe6400000000000000000271b66b6c019bfd9bfc000000000000000000103000000000000000000000000000000000000308080800000100010c
00000000000000000308080800000100010c3c3c00000000000000003000000000000000000000000000000000000101040000000100000800000000000000000102000000000200000800000000000000000c20000000000000000000000000000000000000000001480402002002080010000000000000011010
0000010920404108200000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2a40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000003fffffffc0000000003fffffffc0000000003ffdffffc0000000003fffffffc0000000003fffffffc00000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003efffffdc0000000003fffffffc000000000000
00000000000000000003fffffffc0000000003fffffffc0000000003ffffbfdc0000000003fffffffc0000000003fffffffc00000000000000000000000000000000000000000000000000000000000000000110881840800000000000000000000000000112244544100000000000000000000000000000000000
0000000000000000000000014860094802) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2a60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (8c2023a808ea023a808e8023a818ea023a808ea023a808ea063a808ea022a200000000000000008403b020e8083b000e40839020ec0a3b000ec0039008ec083a020e00a3b028ec083b028e8083b028ec0a3b038ec082a3000000000000000000000000000003fffffffc0000000003fffffffc00
00000003f7fff7fc0000000003fffffffc0000000003fffffffc00000000000000000000000000000003fffffffc0000000003fffffffc0000000003ffeffffc0000000003ffff77fc0000000003fffffffc00000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc000000
0003fffffefc0000000003fffffffc0000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2a80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (031080442012a300000000000000008c01800060001008040201008060081800040201800060001800060001800040201800060001800060001800060002a3000000000000000a8803a804ea0130886ca01b0806ea013a884c221ba884e2013a804e2013a80cc209b8804e2013a804e2013a80ce
a012a200000000000000000401a0006a003a10068401a10068003a100e8401a00068001880060041800068001a0006a001a01060021a0006800001000000000000000204012010480410010e8043a0104804100106804120104804120104800120004804120184804120184804120184804001000000000000000a
8803a808ea0230808c20230808ea023080) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2aa0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (4004100104004102104004102104004100100004100104004100104004100104004100104006a200000000000000008480800820030800020000800020020800020000800020000801c200608008200208008200108000200608008200200100000000000000088402a00ca8032a00ea803aa00e
a803aa00ca80baa00ea803aa00ca803aa00ea803aa00ea803aa00ea803aa00ca803801000000000000000a8800a814280428814aa052a8142a0d0a814a2050a8142a050800022010a81ca2050881428040a8142a050a81c2a052a300000000000000008c010804420a18804620118a044201108046201108044201
1080042011080462031081442001080442) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2ac0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (32010ca0c32010c80432010c804001000000000000000000030000c00010000400010000c00010000400030000c00030000c00030000c00030000c00030000c00030008c000000000000000000000a88030810c20410810620418010c20410810420430810c20430810c20431810c20430810c20
430810c20430910c2042a200000000000000008c01b000680113000ec003a0006e00130006c001b0006c00180046c001b8006c001b00068011b0006c001b0006c002a300000000000000008c01a8006e001a8026a009a8026a009a8006a009a8026a009b8006f009a8026a009a8026e009a8026a009a8006a00aa3
000000000000000a0c8010010400410210) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2ae0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (02880188006a801aa006a801a8006a801aa006a801a20060001a20068001aa0068801800068801aa006a801aa006a2000000000000000088018812c20c98832620418810600498812620498812620430812620498012620498812c204188106204988126204aa200000000000000008c010010c0
0410010400410010400410010400410010400430010400410010400410010c0041001040041001040042a3000000000000000a8801a8106a041a8206a041a81068041a8006a001a80062041883062041801062041a810620c1a8106a041a8006a042a2000000000000000004032010ca0c32010c80432010ca0412
010480432010c80432830c88432010c804) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2b00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (018e4063b018ec063b018e8063b018e4063b018ec062a200000000000000008803a818ee063a808ea0239c08ea0638808ea023a818ea063b818e8063a818ea063a818ee063a818ea063a018ea062a2000000000000000a8c02b018ac0621018840620018ac062b01884062b018ac062b018ac062
b01884062b018ac062b018ac062b01aac062a3000000000000000004002012080480032000c00010080482012000482012080402012080482012000482012088402010080482012080480000000000000000020800a01828062a018a8062a018280608018a8060801828060a01828060a018a8060a01828060a018
28060a0182806001000000000000000a88) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2b20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000a8803a800ea003a900e8103a840ca003a800e8403a800ea003a800e20038800e21038800e2003a800ea003a800ea002a200000000000000000001a0186a061a0186a061a0186806180186a061a01868061a81868061a0186806180186a061801868061a01868060000000000000
00000880012010e8041201048041201048041203048041201048043a010480412010480412010e804120104804120104804000000000000000000a8803a818c2063a01aea063a818e8063a81aea06ba81aea0630818ea063a818ea063a818c2063a818ea063a818ea062a2000000000000000088039018e8063a01
8ee8639018e0063b018ee863b018ec0638) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2b40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (40001200042001080042001080042001080042001080042001080042001000000000000000000a8802a030a80c22030a80c2a030a80c22030080c22030a80c2a030a00c2a030a80c2a030a80c2a030a80c2a030a80c000000000000000000a8800a81028040a80028000a800aa0c0a81028000a8
102a040a01022040a81022000881020040a81022040a81022042a200000000000000008001081042041085040041081062041081040041081042041081042041081042041081042041081042041081042042a200000000000000008801801060041805060041801040041801060041801060041801060041801060
041801060041801060041801060042a200) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2b60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (02b0002c002000000000000000000000030800620030880c20030800c20030800c02030080c20018800c20030800c20030800620030800c20030800c20000000000000000000000001b000e800130806c001b00064001b0006c001ba006c003a0006c001b0006c001b000e8001b0006c001b0006
c002a100000000000000008801a8006e001a8806a001a80067001a9004a001a80068001b8006a001a80068001a8006e001a8006a001a8006a002a2000000000000000a880010100404000920424812920005210120424a101004040101004040101004040101004040101004040101004042a20000000000000000
0000800420010080420010800420002000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2b80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (221308846220108844221180846261188846221188046221188846201188046201188846221000000000000000000000010002400090002c000b0002400198002400090002400a1000240009000a400010002400090002400090002400000000000000000000000001a8316a0c528116a045a811
6a0c7a8114a045a0396a0c5a831620c588316a0c5a831620e5a8396a085a8316a0c400000000000000000000032028ca0a32028c80a32028c80a32028c80a32828c80a32828c00a32038c80a32028ca0a32028c80e32028c80a000000000000000000000030002400090002c000b0002c000b0102c000b009ac002
10002c002b000ac0003000a4002b000ac0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2ba0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (3a004ee093a804ea013a804ea0100000000000000000000002b00cac032b00cac032b00c84032b00cae032a00cac032b00cac032b00cac032b00cac032b00cac032b00cac03000000000000000000000002014080502014080d02214008502014080d02014080502034080502014080d02014080
d02014080502014080500000000000000000000000810428410a10420410a104a8410810428410a10420410a10428410814428410a00428410a00428010a004284100000000000000000000002a880a80022880822022880aa20208800a202a080aa2028080a2302a800a2202a880a0282a888aa002a800a220000
000000000000000000018884622110884c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2bc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0027e909fa426490992426492ffa4264909924be5f0997c27e92fffcbfff09fa4bfff0997cbe5f2fffcbfe909ffc000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000009fbf27
efc9fb727fdc9ff727edc9fbf27edc9fb72ffdc9fbf27edc9fb72fedc9fb727fdc9ff727edc9fbf2fedc000000000000000000000099b5242d490b424ad092b4266d090b5242d098b425ad090b5242d890b4252d091b624ad092b4242d090b5256d00000000000000000000003a804ee013a824e20138824ea013a
804e20138804ea013b864ea213a804ea11) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2be0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00048043a010480412010480412010480412010480400000000000000000000003a818ea023a808ea0230808c20230808ca0212808ea023a808e20230808ea0210808ea023a808ea823a808ea02000000000000000000000039028e40838800e00838020e00838028ec023b828e40839028e40a3
9020e40039800e00838020e00839000e40800000000000000000000000863721edc863121ec487b1218c48637218c4863727edc87b727ec49fb727ec49e3121edc9fb727edc9ff7278dc00000000000000000000009ff727fdc9fb727edc9fb72ffdc9fb727edcbfbf27efc9ff72fffcbfff27fdcbfff27efcbfbf
2fffcbff727ffc00000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2c00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000000001080662011000242009080242009082242019001e420110826420198806620110006420090802420090804420100000000000000000000001800040201802060001800040201800060001800860001800060001008040201800060001800060001802060000000000000000
00000000038804c20138084e20138844420938804e22128004e20138804e20530824c22138084e20138804e20138884e201000000000000000000000018008600018000620018900625018958600418008600018010480218100600038100620018800620018000600000000000000000000000001201048041201
048043a010e8043a010680612010480412) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2c20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0620018000620018800620018800620018000660019800660018800620020310000000000000000c001102040031000040001000040001000040001000040001000040001000040001000040801000040021000040020310000000000000000c00800220202080220018800620038800e2000880
0a20000800a20028800a2000080022001880062003a0000200000310000000000000000002800ca0072002ca0032800ca0032800ca00b2800ca0032800ca0073800ca00b2802ca00b2800ca0072002ca003003100000000000000000008815a2074881120044801120064801922054881522054881d22016881da2
0548815200448011200648815220540000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2c40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (041880062042a2020000000000000000030010c00430034c20c30010c00430830c00430010c00430010c00430010c00410010c20430830c20c30010c004000020000000000000000030000c00030004c00010000400010000c00030000c00030000c00010000c00010000c00030000c00030000c
000000020000000000000a88030810c20431810c20418832620c98812c20430810c20430810c20418812c20410812c20c30810c20430818c2042a2020000000000000000419000640018000600138804e2013800464001900064001900064003900064001100060011800460011900064002800800000000000000
0c01880862001800066001980066001980) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2c60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00608018000608018200608018200608018080638018e006080182006080182006080182006000120000000000000a88428800a20020000800020800820020000a20028800a20028800a20002800a20028800800020000800028800a2002a2020000000000000000018810620430810c20430810
c20430810620418810620418810620418810620418810c20430830c20c1881062042800a0000000000000000010010400410010c00430810c20430010400410010400410010400410010400410010c00430010c004100104004280020000000000000a8801881062043a820620c180306004188326200088106204
18810620418810620018800620c1881062) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2c80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (3a018c20630818c2063a818ea062820a0000000000000208039018e4063a818e00638018e0063a018e40639018e40639018e40639018e40639018e00638018e00639018e406080020000000000000000038808e20638818e60639808e20239808e20638818e20638018e00638808e20638808e60
639818e60638818e206280000000000000000a8802b01884062b018ac062b01884062b018ac06ab018ac062b018a406210188406ab01aac062b018ac062b018ac062a20200000000000000000020100004028100804120100204020300804020100804020100804000100004020100804020104804020100804000
120000000000000000008018a006080182) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2ca0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0180104004980326004100104004980126004980126004180126004980126004980124004100304004980126004280020000000000000a88038801c21078801e20050801420078801e20078801e20068801e20078841e20078801c20070801c20078801e2006a200000000000000080001801860
061a81862061881862061881860061801860061801860061801860061801862061881862061801860060800200000000000000080120104804ba012e8043a010e804b2012480492012480412012480492012480492012e8043a010e804920124804000020000000000000a8843a818ea0630818c20630818c20638
818ea063a818ea063a818ea063a818ea06) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2cc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01004040105004042181004050101404052101004042a20200000000000000000080042000208042001080002000080048001080042001080042001080040001200042000080002000200042001000020000000000000000028030a00c20010a00c28030a00c28030800c28030a00c28030a00c2
8030400c30030a00c28030a00c30010a00c000020000000000000a88008810a20808030200400030000808010220408810220408810220408800224008810a00c28010a00c0881022042a2020000000000000000010810620410810420410810420410810420410810420410810420410810420410810620418810
6204108104204280020000000000000080) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2ce0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000030020c00810038400a10020400810020c01a30038c02a30020c01a30020c04830128400810020400830020c0080000a0000000000000a88030801c20051801620058801620058801c20070801c20070801c20070801c20070801620058801620070801c2006a20200000000
00000000019000640098002e000b8082e020b8000644099002640099000640099002640099002e000b8002e0009900064002800200000000000000000188006200188006600198806620198006200180006200188006200188004200188006600198006600188006200280020000000000000a8800101004052101
0040401054040701010840401010040401) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2d00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0a22228980a22202880a23020802a220a08a0a02028080a00028880a2202a2020000000000000000018884622018804620130880c220308846221188846221188846221308846221108046220188806220188846221280020000000000000000010000400110000400230004c001300004002100
00400210000400a300004000180004001100044001100004000280020000000000000a88018830620c18838620c18810620418810620c18838620c18830620c18810620c38818620c18830620c18830620c2a2020000000000000000430028c00ab000ac20ab082ac24ab0928c00ab002ac00ab0028c00ab002ac0
0ab012ac20ab082ac20ab0008c00a00002) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2d20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (2d094b525ad400000000000000000000038804ea0138804e60939804e60139804e20138804e20138884e22138824e20938804e60139804e60138804e201280020000000000000a8802b02ca40b2b02cac0b2102c040b2b02cac0b2b12cac0b2b02ca40b2b02cac0b2b02c840b2102c040b2b02ca
c0b2a2020000000000000000002014080d02814080d000140805021140805020140805020140805020140805020140005000140805020140805000000000000000000000008004204108104204128104a84108104200108184204108144084108104204108104a04128104a041081042041000020000000000000a
88028880a200a8080a0222008080002000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2d40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (7efc9fb727fdcbff72fefcbfff27efcbff72fffc9ff727edc9fbf27edc9fb727fdc9fb727edc0000000000000000000000be4909fa4265f0997c264909fa4bfe92f97cbfff0997cbfe92fffc27e909924265f09924264909fa426490992400000000000000000000000000000000000000000000
0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000009fff2fedc9fb727fdc9ff727edc9fbf27edc9fb72ffdc9fbf27edc9fb72fedc9fb727fdc9ff727edcbfbf2fffc000000000000000000000092b5252d090b424ad092b4242d090b5242d090b425ad
090b5242d090b4252d090b424ad092b424) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2d60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
71c2000c000040408004000c0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000bfb727ec4863721edc87b121ec487b7278dc9fb727edc9fb727edc87b1278c4863721ec487b121ec49e3727edc00
00000000000000000000bfb727fdc9fbf2) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2d80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2da0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2dc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2de0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2e00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2e20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2e40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2e60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2e80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2ea0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2ec0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2ee0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2f00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2f20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000071c2000c000020408004000c0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2f40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2f60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2f80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2fa0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2fc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2fe0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3000) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3020) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3040) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3060) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3080) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (30a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (30c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (30e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3100) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000071c200
0c000060408004000c0000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3120) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3140) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3160) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3180) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (31a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (31c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (31e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3200) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3220) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3240) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3260) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3280) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (32a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (32c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000001c2000c000010408004000c0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (32e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3300) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3320) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3340) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3360) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3380) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (33a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (33c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (33e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3400) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3420) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3440) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3460) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3480) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff0000000000000000000000000000000069da00008000000c020000008005000ca00000008001000c000000000000000000000000000000000000000000000000
00000000000000000000000000000000000000000000000000000000000000007002000cc00000008001000c4e7500008000000c0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (34a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0001) TDO (0000) MASK (0000) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'serase' instruction. 
SIR 8 TDI (0a) ;
RUNTEST 37000 TCK;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) SMASK (ffffffff) TDO (f5034093) MASK (0ffeffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) TDO (00) MASK (00) ;
SDR 16 TDI (4000) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'usercode' instruction. 
SIR 8 TDI (fd) TDO (00) ;
SDR 32 TDI (12340004) SMASK (ffffffff) TDO (00000000) MASK (00000000) ;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) TDO (00) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'usercode' instruction. 
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) TDO (f5034093) MASK (0ffeffff) ;
SIR 8 TDI (e6) TDO (00) ;
RUNTEST 50 TCK;
SDR 32 TDI (00000000) TDO (12340004) MASK (ffffffff) ;
//Loading device with 'conld' instruction.
SIR 8 TDI (f0) ;
RUNTEST 110000 TCK;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) TDO (f5034093) MASK (0ffeffff) ;
//Loading device with 'ispen' instruction.
SIR 8 TDI (e8) ;
SDR 6 TDI (34) SMASK (3f) ;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) SMASK (ffffffff) TDO (f5034093) MASK (0ffeffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) TDO (00) ;
SDR 16 TDI (4000) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fdata3' instruction. 
SIR 8 TDI (f3) TDO (00) ;
SDR 6 TDI (3d) SMASK (3f) TDO (00) MASK (00) ;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) TDO (00) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fvfy3' instruction. 
SIR 8 TDI (e2) TDO (00) ;
RUNTEST 1 TCK;
RUNTEST 50 TCK;
SDR 6 TDI (3d) TDO (3d) ;
//Loading device with 'conld' instruction.
SIR 8 TDI (f0) ;
RUNTEST 110000 TCK;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) SMASK (ffffffff) TDO (f5034093) MASK (0ffeffff) ;
//Loading device with 'ispen' instruction.
SIR 8 TDI (e8) ;
SDR 6 TDI (34) SMASK (3f) ;
//Loading device with 'conld' instruction.
SIR 8 TDI (f0) ;
RUNTEST 110000 TCK;
//Loading device with 'bypass' instruction.
SIR 8 TDI (ff) ;
TIR 0 ;
HIR 0 ;
HDR 0 ;
TDR 0 ;
TIR 0 ;
HIR 0 ;
TDR 0 ;
HDR 0 ;
SIR 8 TDI (ff) ;
SDR 1 TDI (00) SMASK (01) ;
