// Created using Xilinx iMPACT Software [ISE Foundation - 6.3i]
TRST OFF;
ENDIR IDLE;
ENDDR IDLE;
STATE RESET IDLE;
TIR 0 ;
HIR 0 ;
TDR 0 ;
HDR 0 ;
// Validating chain...
TIR 0 ;
HIR 0 ;
TDR 0 ;
HDR 0 ;
SIR 8 TDI (ff) SMASK (ff) TDO (01) MASK (03) ;
TIR 0 ;
HIR 0 ;
HDR 0 ;
TDR 0 ;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) SMASK (ffffffff) TDO (f5034093) MASK (0ffeffff) ;
//Loading device with 'conld' instruction.
SIR 8 TDI (f0) ;
RUNTEST 110000 TCK;
//Check for Read/Write Protect.
SIR 8 TDI (ff) TDO (01) MASK (ff) ;
//Loading device with 'bypass' instruction.
SIR 8 TDI (ff) ;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) TDO (f5034093) ;
//Loading device with 'ispen' instruction.
SIR 8 TDI (e8) ;
SDR 6 TDI (34) SMASK (3f) ;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) SMASK (ffffffff) TDO (f5034093) MASK (0ffeffff) ;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) TDO (f5034093) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0001) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'ferase' instruction. 
SIR 8 TDI (ec) ;
RUNTEST 1 TCK;
RUNTEST 15000000 TCK;
//Loading device with 'conld' instruction.
SIR 8 TDI (f0) ;
RUNTEST 110000 TCK;
STATE RESET;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) SMASK (ffffffff) TDO (f5034093) MASK (0ffeffff) ;
//Loading device with 'ispen' instruction.
SIR 8 TDI (e8) ;
SDR 6 TDI (34) SMASK (3f) ;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000000000000000000c4000000000000000054fba80000000000000000000000000000000000000000000000000000000000000000000000000000000000000000d53ff0000000000000160400000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000c480000000000000001200400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000c480070da000a0002000c800000008001000c000000008004000c900000008001000c638000008003000c6dfc01008004800cb0000000800680
0ce00000008001000c66aa9955ffffffff) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0000) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (b814000500014000500014000500014000500014000500014000500014000500014000500014000500014000400048ff0000000000000420000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000004800000000000000054ffc000000
0000000000000000000000000000000000000000000000000000000000000000000000000000000000015bff0000000000000d2ff80000000000000000000000000000000000000000000000000000000000000000000000000000000000000000015bff0000000000000140028000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0020) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (839b0834c80c500c64209708c5c009f0045400dd0037a80200000000000006200f400d00024502958036510110524400110404404d14035483110034400d000c7400d10444400dd0014500dd1035a8030000000000000c8043440c114204400120034004100324020100a2400801016400080030
602c50c02484c52301404cd2001400dd083322100000000000000c2007401d1038440a55228440a1102c4c435100c440a4102f5d00111074483f19385c00570084420dd00c44211d0077080100000000000006800fc01c30106c04330104c0038000ec003b0006c041301104212a0075d00f72006c093e0a0dc89a
f0d05c81ef1875a0030000000000000163) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0040) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000a001c400c501004050900824058d00c04098d10034001100124019d8033629c900420000500c44809d8051400cd0032a00700000000000002004c400d50034400d104744015d1036c415d0815402d30034401dd0032c41f90065408d180e4400d10165400cd0034a01300000000
000004200cc00d30034c0a030490c22cf80b2c025f00b2c50932026c209f0034c00ff0026c28d70c84820d60827c22df0035080300000000000006001fc00ff201fc03ff0065c811b045fd60ff109fc017f011fc00bf003ec00ff0029c40fe0007c00ff0a46c08ff103d80070000000000000e200bc00d24010c21
930e37c0b1340c6c120b4096c921120124) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0060) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (e11020400cd001ac00a38038504ed803bc00e3080ac00f10818400ed003988130000000000000e2057c00d30014c20932034c00970027c00930004c00de0814c00950874c84df0007c00930804c00978054d00cf0037a01500000000000006600bc00ff016fc0057800dc08ff203fc08afa03ec0
8170034c64bf0236c1be91037c40fb0237900ff001dc88ff003db002000000000000004048d09c70164d094b4142c014d0110c458f0072c25032352c518f0173401cb8762c00d51440c45c70141407cf02701012000000000000020018401e5004840d49014a415ed144a40d6d816900129c07d40dad017b001e92
068641650048409e10159409fd01788006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0080) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (024c109f002708300000000000000c004bc001f000fc12170087c001f0087c001f0007c041f3047c801f0007c000f1007c02172007d001f04064001f0007001200000000000006005f400530054d015b40945045f0115c01534114cc55f0494c0f6f2014ca05f001e40071429ec0057005cc036b
0015a8170000000000000c0049400c80230422c90274406cd0470404c10870401cd0072400c10030400cd8275412c90a76400d102a1489cd0033281200000000000004000f401e18078403a90078401ed0879403e10078401e50078401fd0078481cd006a401e10052421e50060441e90079000300000000000006
204fc00eb001c400f108384008d0808500) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (00a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0114c44131116c84132105d041b0105c405f0804c04120106420172105c001f0104c001d0006b01c000000000000008043400814528414a5dd28514a04528414e1452b094a105255009d0021014890522440853d256208d05205008d0020201000000000000002206340091002c400a5012c404b
1022e480b1002d400b160254409d04244009100264229520254409d00644009d0024a0180000000000000800074009121a44069140644019100e4401910026c009900214229d20a54419b01264029504644009d00244009d002620010000000000000c0043c00932020c80920464c00830062d02830020c098b202
5c249f2924c02930426c039300a4c009f0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (00c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (44009500244809500664009d0025a0180000000000000e80434008120334968584a36168110a17028d00a04068d00a64009d80204028101207008d00224049180f24808d002300100000000000000c20734001181c7403110145c01110804c001d0006c831b0086c051d0007c001511444001710
044011100845001d0007081c0000000000000e0063c00930f6fc01b7016fc05b3006dc01af006cc03b70064d02bf0028c05a380acc00bf002ec0897006cc00bf0027a8180000000000000e6067c009f0527c149b0533e149f0027c60cf0026c149f102fc94af002bc009f0d2fc14bf052ed14bf082fc00ff0027b8
190000000000000ac073e0013010cd0417) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (00e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (534007f001c40173501d50471001ac0261401440571001540465011c5007104df40379085e4a07c00144804d2014a814000000000000042053c40130084c00132084886130287c02130004c201b0085c00131404c880b0487c421f2087c001f0005c021f00050014000000000000060057c009f0
023c249b1561c009f0065c059f0027c109f0127c019f0827c409f0127c209f0a67c019b4021d059f002580150000000000000e2017c009140a7c04971027c02934125c019f0424e029da162c019f0024400910124a2c9f04a6c08810026c029f0027a0050000000000000620630009104274009480254349121240
009d0126410918026404dd002542095802) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0100) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01c3034cc01d3024ec09bfb25ec19d10068c01cf0277a800000000000000066043c00570007d80130005c809f1006d00171033c02374037c00c70837c40970017c001b9806c00ff0825c00cf0035b010000000000000004057c0163006cc016e0042c01b34043c01290078c01814071c01eb0078
401e3404bc0167207bca1ef0069c81ef007810150000000000000200170006d000840385800a401e1000b500a90078500210039400fd8048400e1003340269000a420ed003a480fd003880050000000000000a0053420410420500cc02b2403c104c340c890030401918031500c90000400c10065404d58633400c
d8033400cd0032a0140000000000000200) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0120) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000620574005f0166c0bd100b7c80db4084c508142b64019101b6c01cb0004400d900244018d00a6c01f10030101cd0035a0150000000000000c20114204d00124035900472028920c04008100b24009101f24098900024008144845080d04c4400d14022006c50033200400000000
00000400034046d003a404611009400a9000840481013a428a1223e404f9010c424e90d084003d140a4e4e1002e400ed00390000000000000000062057c056f0138411cb050f614810c0850181097ac15a1007ac0d814348c41cb00484802d0140c39d1022a50dcf017988150000000000000e0003c415f207cc21
f3105fe01b3004cc01931074c8fb3017ec) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0140) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (8d033048c8101b240495230048889830040011448140cc10220400dd003020100000000000000200074005d00044109102a7603d101b45039d0034411951035400d90084400910004451110444400d11225400dd003488010000000000000802074005d01c6d081d10774031160404019d0034c0
1d14036c231720014009f2014403170045400d1c025400dd003620810000000000000c2203c007f056cc01fb003fc10fb0044c00b78034d20f3003dc433b224cd02d3100cc0033000cc00f3802dc00ff003f00800000000000000c0007c00570085c021f2437c00170107c84df0037c02bf4033c82d72005c80cf0
035c021d1807c00df0225c08df00370001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0160) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (010000cd0033a0100000000000000c2007401d10134400dd0034410dd0077441d90875401d71046c811900154401690014004d207448911002c400dd007708010000000000000e000fc41f3027cc031f0249c00ff007fc81ff007fc41cb0046c20330046c21270044c017f0075c203f003cc01fb
007fa0030000000000000e4017c027f000dc001f812fc04bf000fc04bf013dc249f0131c00370103e8cbf0103c80270007c04ff002fc28ff033fb8050000000000000ac003c0a5f00a4c068b0027c0adb0004c069f0434494a305b5d181b0404c04930504500139084416d188a5e08dd2a36b00000000000000000
8043404490082612050a23400818800492) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0180) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0224c00d304b7c00df0a36c02d7144680a5f00a7c00d70085d001b1137c001f1013c00df0035080300000000000006001fc00f7083dc027f205f400df002fc00ff283dc00ff00afc00f3401dc01b7091fc807b203dc209f001fc00ff003d80070000000000000e200bc00db4036d00dd0035c40d
f00f7c00d70034403870006c19170852c241108c45035f20374431f0494c00df0037a80200000000000006200f400d820364c09d0134400dd0477400d90035441d4a0064809d10675044c20900235d0036083910014540cd0035a8030000000000000e8043420c92032400cd1131608cd1033420c58030480d5080
64000d00004600108004801c00334800d0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (01a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (fc0c380034c28f7009b408df003db80200000000000000404bc05cf0033c07470092c00c34233405cf0272c034f4242d05cf02c1c0d874153c0c8f8372c8d830413c05cd01701012000000000000020019405ed007b409e5026a501e1067b405ed017840dfd02595254d90f8401f1014840d2900
7960725086f409ed097880060000000000000a001f400cd0037440d58032420d100f3400cd0072001c900806000d080140a0511434210d02f2429010053402cd0032a00700000000000002084dc00dd0037440d50034400f110f7480dd1074404d02021440cc14644c9d3043553b4900f440185101740add0034a0
1300000000000000200fc80df0037c00d7) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (01c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (4b400c5003140d29808b600d14030440cd003048ac50832402cd0af3489c10031481c11033012c12450400d10033283200000000000004000f401ed0079601e11077405e1045c601ed2079401fd004e441ed007b401e100fc443ad0878401e50458401f10079000300000000000006204f400e70
038400eb083b404e10038540ed0038400e7003ad00ed003b400e110395006a003b400a10818400e3403988130000000000000e0057c00df0036c01930037c00f30074c01cf0035c21d32002c209f0037c405f0012c205fa837c40971014c80d30073a01500000000000006400bc08fe023fe09df003dc98df023bc
00df083fc00f30019c4cdf003dc00db003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (01e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (109d80270009580274849d05264029508a44009d0024a0180000000000000800074009d0827400950ca54009d10e74009100234009f002440187202441b9300e44808900e440381902540e9d102620010000000000000c2043c009f1027c00930060c209f2267c00930127c00970025c299f0625
c809101668809f8067c05970264c019f002708100000000000000c004bc00170006c001f2407c201f0187c801f0007c821e2407c0c1f0007c12128c05c101b0886c021f2083c02170007001200000000000006205fc005d0015c0051245740053001cc005f00158097d001ac427f085f421616098c017d1014c057
500dc400530015a8170000000000000c20) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0200) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000e0063c009308a440293002c81793002f800b3002dc00b3102dc21b320abe82b2002fc80bf802cc40b351ecc08bf002fa0180000000000000e6067c009f8527c949f0527c149f102bc009f4027c00af002fc80a7152fc14b3052ec14bb202fc00bc052b814ae0027b01900000000
00000ac073c001f0007c00230004c041f0007c00130007c00170005c041f0807e20170007c000d0007c04158904c001d0006b01c0000000000000080434008d0023000a5002c4148d0023400814023400cd00304148528204009d40654019d00204148105214008d002020100000000000000200634009d0027400
b1022c5009d00a74009100274049500254) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0220) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (9f2027c149f0024c808f0067c90975065c20970427c009f0ce7c309f002580150000000000000e2017c00994025d049b00a2c009b1027e40910027e03950027d039a11e342a9b862110b9920245058700244009f0027a8050000000000000620634009d00214008d002650089002740095002643
09900274289922356109980244009d08244089900a64008d202588180000000000000e8043400892121400892422400890023400819023400850027502c900234808905256508900224008501a04048d0023a8100000000000000c20734001100404051f00544031b0017420150006c801f80055005b3047c05150
0444255f0006e201b00c6c011c0007001c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0240) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0584893700780015000000000000020017400e90138008ed0408624cd080b400e90038500a80009480a5003f642ed0429502e5b028410010030720ed003880050000000000000a0053400c10030400c900c0420cd01c2420c92070500800013400850033442c98c11520dda030404c50034600c5
0032a0140000000000000200534005300140a075081c4005d011b4005900584106b0299c2071245fc607d001c4817f841c40271401c4027d0014a014000000000000042053c40130004c00130084c001f1087c001b8204c021b0005d01130085c021f1004c041f2004c02170084c00170005081400000000000006
0057c00930026c059f0565c009f0127c20) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0260) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (020c420e98229480e1092a44225009a080ad093950461083b45029022f40021013850c2c09390000000000000000062057405c1007ec05e12949489e1028b401c10372d0da50048505cd017ae01d5026f4043d41eb4c90b057c4055d017188150000000000000e0003c41d32674c09f30244c49f
3424dc01f34074c0d830056c09af0974c09f3a0d5c4137007fc01332074c017f0077a000000000000000066043c00d7003fd14f7001781cff0007c00df0037c008f2003c00cb00354809f01a4d00df2027c001f5007c061f0035a810000000000000004057c01e30278c01fb004cc81ef104ac01e90878c01a3005
bc01a70039c01eb1069c117d0078501271) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0280) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (44015120c44010100474011d003620810000000000000c2203c00ff003fc00f70207c20f30c4ec00ff013ec00b7200dc4432083c501f3002cc8037000dc4037044bc403f003f08800000000000000c0007c00df003fc04ff03a7c20f70087400df0827d00de0045c429f1097c425f00a5c005720
87c005f0827ca01f10370001000000000000062057c00d3403c521f30064c40fb04c1c00d14036c928710e6c0b9d03b541bd141e5c42510023807d15024c809f0035a8150000000000000c2013400c10030401c1c001400c98003600c1002242105000240bcd00764010409e36040900230130900a04000d803328
04000000000000040003404e10038410e1) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (02a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (17c02ff00bfc04cf000fc02df000bc08df05abc1437210bc0097121cc861f00afc003f010310c1f022f4241f233fb0050000000000000ac003c02df003fe14f70107c84e30006c0edf20a6c52152785c18951335e001b00bc500310404c2a110127414370136b000000000000000008043486cd0
13340cc90403444c90813400cd00226008d480550485801162c0141a042001830040001412300c0d0b302010000000000000020007400dd1037400d50087400d10207400dd20364019500c5402950075406890050611016044601110227411150034a001000000000000080207400dd0037440db1083400db20c74
00dd0067c019f0041500072044c0315016) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (02c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00df0037c20df4246c0b0b0033c425314e7c20db0061290000000000000006200d400d10037400d10875401190106400d900364a05c2037420d90037400d10016480150007482d10067400d19005a8030000000000000c8043400c10033420c90020400090003484c11024480550033600cd0033
420cd4202408490003420192027440c92003a010000000000000042005c01d1a077400d10035421150006400fb0076c011d0077401dd0076481d10414401910846d01530867421d1084700010000000000000e800f401d1007bc21fb002cc0133000e002f30064c01bf007fc61df007ec01db000ec0439204ac014
7806bc21da004380030000000000000e60) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (02e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000a001f400c10030401c580876000582c0400c118004008d0033400cd0831440c5c0214490d08414424c1023400c14202a00700000000000002004fc00d300b5c03d910e74130102c4500f11123e001d0036400dd1037400d10426e4a1d0684402430163400d100c4001300000000
000004200f400d30135e04df00e7c46172080c00d7a0a5a001f0037c00db0035c00d70803d025f0025c845b0027c00db0005080300000000000006001dc00ff183fc00ff5427c0037004ec40ff00afc803f003fc00ff003ec00ff004dc81b3082ec0973082fc00ff424d00870000000000000a2003c00d10033c40
db20e4c031b4087c00d30464c09078037c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0300) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (eb00284002d0839c80ed003b440e11022c00e1002ac4063882b400e1000988130000000000000e2057c00d30075c00d90037800130044c04d30024c000f0037c00df0035c00dd0025c00132831c205f0023c00df0043aa15000000000000066009c28d70037420f31037c007f022fc84ff0223c0
80d0237c20ff1037c40ff201740436000dc087f0037820f30205a80200000000000000404bc09c34130c8dc78003c00c51200684c103614050f0173c0dcf0371c01c700c54064f0a41c814f0033c4dc303d0181200000000000002001b401e90079611ed005b40121224040dc1436d4053d217a405eda07b481e10
07840d89010c44171104f405e103c88806) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0320) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (027c209f202700100000000000000c004bc001fa087c00170207c00170487c001f0007c001f0005e001f0007c20171406c380f0007c40130c07c001f0087001200000000000006205fc00530015e005102df4227108dcda05100d9c006f0017c005f0015c005f01dd40171001d51176009bc005f
01dda0170000000000000c004b400c10033400d16033092c94070400d910e06000d0031400cd0033480c90070542c12000403450833400c104c3201200000000000004000f401e1007f401e18073441e9a0d8429c160ed5433d007b601ed8079401e90059501c1046f40165007f401ed0049000300000000000006
604f400e1403b400e1103b42029003c448) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0340) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0107c205f0116c041b0007c001f0007c001f0007c00150105c045b0005c00178007c801d2006101c0000000000000080434008d00205008985224008d85204148908204009d00224808c00234008185214148500256009508234008d002000100000000000000200634009d00a44069d0137400d
d20364009940274009d00276009d0027480950625404992c274029500274009d00e428180000000000000800074009d00244029901634009d20e44609300244009d00274009d00274009b80645839502a040b8502674009d206622010000000000000c2043c009b2024c81970027c009e1226c809b4e27c909f082
78409d0027c009050200019b0465810970) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0360) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (52809940354829140274409900a588180000000000000a80404408d00224048909240409100e04148500244009d00236808d18234008d002040281002744085002740085002300100000000000000c60704001d2004501050284c40150006c031f2006ca01c00074001d00074001103c44401b08
05e00110017400130007081c0000000000000e2060d00bf802cc02b3022ce80b300acc3497002cc00bf0027c409f002fc009f036ce05b3002ec00b7002fc0097002fa0180000000000000e6067c009b202bc9497252fe00bf052fd1497002bc80bf2027c009f1027c009f252ec00b7902ec00ad102fc209f002fb0
390000000000000ac073c001b0004c0017) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0380) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (5340047001cc0071305f4407100dcc005198544205d081644051081762051419c5106f225c40a71041a4005100182104000000000000040053c001f0104c001720c7c001f0006c001b4285c001f0007c00130007c00171007c02160007c00130087c001b00850814000000000000040057c009f0
025c00970025d109f0823c008e0026c099f0027c009f0027c009700e2c409f10a7c039f1027c009701650015000000000000048014c009d8826c009b00a4410810024c209500a0c138f00274009f00274409f012410f9104624019702a7c009700a428010000000000000600604009d00266008d20a4608d500666
0095d0a64409d08274009d002740090802) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (03a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (09df027fc09d3805dc01ef0072d01f7005bc01da007fa802000000000000064043c20d70037d00df0003c80d72007c00f72021c00cf0036c00de0033c00d30004c009f0010f40cb0003c20df0001b810000000000000004053c01ee087ac8125205bc01e7005ec03f0007a401ef007bc01e3007b
401e3004cc01c70879c01e3004bc01eb10481014000000000000020013400ed0038410e1009f640e18098500e1402e440ed203a020e1007b400e40028400ed043d601e1c00e400e1000880040000000000000a0053600cd0232401c58037602c521d2440c11072480cd0033600c10033400c901b0411c500f1448c
184c3600c90032a0140000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (03c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000062053e40df0020c00d100d7c005b00a4400f100b0c00dd0037c00dd0036400d100f5c10df0074840471083c00d30275a0140000000000000c201b400cd0000400c14c83442c10342400d480e2502cd0033400cd0833000c10c50403050202400c10083400c900c3280600000000
0000040003420ed112844421001b608e90008400c1872c480fd083b40ced003a424e10318520690028642e5010b400e100090200000000000000060057401ed0368401db005f40de3000ac01e5006ac49cd0073481ed0071c05ef4d50404e70272c04e1014b40dea004988150000000000000e400bc21ff106cc01
97905fc09db006ec01d32378c09ff107fc) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (03e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (cd0025000d900b3602cd0133604c9c100480019406500d1042340cc9830028100000000000000a0007400d10867400950447401510064400d10836480dd1037400dd0037440d10805430910116601d52067400dd0034a001000000000000080207400d101e74121710c7403910445400d7026550
0c3a037420dd0035c20d300414011140c2c05d51147400dd000600830000000000000c2203400f3002fc053f001fc10f3000ac00f3003ec50ff203fca0fd103f880f300c5802e3003ec20f5000f820fb800e00800000000000000c0007c00df00a7c001f0057c809f0007c80df0427c00df0037c00df2035c80df2
827c065a1425c4adf0487c40df02060001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0400) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (023400cd0033a0100000000000000c2007401dd00c4c031f02d44031102044035504854039002c7c0191004c401150044441172045e011b4067401d7807708010000000000000e000fc01ff010cc0413000ec04130809e0007010c0443b090cc0113100ec4111100cc013f0045c0113006fc01cf
007fa8030000000000000e2016c00df00a7c00370807c40bf000bce8f73627c08c70237c06ff0e35c04f79307c203f010ec84af2027c04ff2103a805000000000000080003c06d30027c12178d07c00530004c00d30036c8adc00b7c06df0037c38d1a305c00110206c0a970027414dd0404100000000000000000
0043412c14023482059003410814001404) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0420) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (2080c92d320a4c84130ca4508db0003c00130005c08db40b6c061f0805c00170024c00df0035000300000000000006001fc00ff0006c0197926fc219b024fc037f00b7c019f00ffe80bb001dc057b107ed80b7000dc003b022fc00f7003d80070000000000000e200bc00df0245c00160126c004
700654320380618015b40d4c01034042c0357c0c5c1b1f04c4401010027c00dd0037a00200000000000006200f400dd08255941d00344065540b4400d500054081104074011504464009509054009d2044501950027420dd0035a0030000000000000e8043400cd0221428c5000244885000150881308140801080
04001100064009580016001d0022020012) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0440) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (ec8cbf083ec009f0a2fc88db0235b80200000000000000404bc21cb0370c01cf4140d0d830100c01814271c050b4373c8d014041423cf05f3c088f0261c0d070260c05c90070101200000000000002001b001e5035841d6d015044929085b511210349401e1824a401a520484cbed6b734452901
4b6592d0068401e9007880060000000000000a001f400c900100000d00006000120555010128910000924234a0011001480cd40c36030c0c816530d0020500c90032a82700000000000002004f400d70024401c103f4480db0425c01d18034421810126411150014403cb4a724078d01264019d0020480d90034a0
1300000000000004200fc00d34024c02d3) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0460) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (4b440c51032449c550f241bc90072543c10272400c00873421050032401c10272533cd00f1401c52070400cd8033281200000000000004200f441e50872401e10468681e18073481e5007a401e500784113920cf600e1807a401ed28694413d1468401fd0079000300000000000006004f400e10
01840001003ac006b003840061001c400c1003ac80a5001a480e10030480ad00184002f0028400ed003988130000000000000e0057c20d32054c00170074800420035c00de0055c815f2030c01130081000c31004c008f2004c001d0024c01df0037a01500000000000006600ac08db087fd60f3a01fc04bf001dc
089f0026c0c77091bc045f12bbc28cb023) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0480) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (449100266849105245089d00245209100274029d0024a0180000000000000800074009d0024405932124c008100644059d00274209bc8274209100244828100e44018d03a4c139009234029d002600010000000000000c20430009f0024c058c0025c049b04204188f0027c109320e7c409ba026
c01930020c409f0064c029b0167c059f002708100000000000000c004bc001b000dd021b0406c02178005d02170184482170486c001f2001c001f4185c201f09065021d2087c001f0007001200000000000006205fc00574016c08572014c8053e1d5c07550096c075701d0c2173001dc257000dec127f11ddc106
d00144405f0015a8170000000000000c20) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (04a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00000000000006a063c0093016cc21b7146c905b3016cc11ba05ecc25b3816cc00b1016e400b3416bc00b3002ec00af002fc00ae0027a0180000000000000e2067c009f0827c00970021d009f1526c008e0527c809b182fc00ef482fc00bb002ec00bf182dc80af602fc00af0027b01900000000
00000a8073c001f090cc041f0105c641b0105d041f0117c041509074401b2106c00130104c001d0004c00130007c401f3006b01c0000000000000080434008c0528714a10d28414e14529494ad052b414ed0523400815520401914520400cd08204008100234008d902020100000000000000200634009d102c400
bd122d400b1012d580bd803f601b524274) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (04c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (970027c908f0026e809f2465c00971123c449b0067c039f0067c009f102582150000000000000e0017c609300a4504871024602870266c10931125492910864c03830064e00912427493912063c109f00674009f0827a8050000000000000600630009104244049506266009d0024580d5002542
09142266089121a4402d180254009569a54009d22274009d0025a8180000000000000c8043400818a204808500204428502224008121214828110a04009140a0420810a234808580254009d00234008d0023a0100000000000000c2073400110004408111086d005b05d4c021721c7e001b0806c00112804400130
0878001520056801d00074001d0007081c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (04e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (07ac016f00781015000000000000020017400e50018400650008400a10028400e10008400e1240b600e5443b44121082b402a1a018482fd1038401fd003880050000000000000a2053400cd00104014120c060e890274409c18820403c18411448c108f0403c900b36458100305135d04b240ccd
0032a0140000000000000200534005700184c474309c40373409c52161061d50171009b4005f001d44661009f40271041c4007d109c4017d0014a014000000000000040053c001f0084c12130284d0213c484c001b8080c4a130007c40130080c10130107800190084c421f8004c801f0005081400000000000006
0057c009f4027c009b4421c889b0067c00) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0500) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (200a04ca9200a482e1210a00021100a404a5233b40461422b408bd0338014e920194006d0239080000000000000006205740dcd061140d2f0782d2ca1410cc09eb0b42c45000141401e105734412501614222d0158c05ed08304012c017180150000000000000e0003c01ff025c441136248e0db
2004cc89eb116cc89530044c69ef0375c496b1274d81bf0076809eb027cc092f007fa000000000000000064043c00df0017c001f0021d009f0027c20572027c00df4007440df0035c80050807c00974031c009f0037c405e0035b010000000000000004057c01ef0058d01430048c21891070c21c14060c0183004
3c41e10070c006b406bc81e30878c41ed0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0520) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (4483090067410910060c005900362081000000000000082203c00f3001cc007b0a4cc009f014cc00ff007784033154fc00fb2075c007f00248803f002fc00fb082fc007f803f08800000000000000c0007c00df0015c01df0085e029b0294c80d71097c02df1005e0c9788b5c42170424c269f06
16c00de0037e00dd00370001000000000000062057c40df02d6403d302c0e24130056d12c34416c04930084e01d70ab5c200301264409f0064881d92175400df0035a8150000000000000c2013400cd00934000d00024058101c06014900024130100214008180324000540434000c00304278d28105004d003308
04000000000000040003400ed001a40661) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0540) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (17c00df001fe022f001fc40fc000fc02df00870022b048bc0c9f000fc0017120ee002b273f4849f000ce045b2037a80500000000000000c003c06d34214d061b2204d02dd2004c029f0087c02110107c0e9a4185842570305c001d00b5c069b0087c145d05b6a000000000000000008043618c10
0105080d00014028d101060cc981834068d300764481860141205080148019081341281023740c0903302010000000000000020007400d100144031900044119d0094584dd8207428910805620dd018544155a0c74019d00754449902374001d0034a001000000000000080207400d100104014f00454438d80044
00dd04f74055f018340891107140117204) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0560) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (035f0031441d30857c00df0836c005b0037c00d30035208000000000000006000f400d10034400151ab5481d100354111d00444809500054419d8835401912025420d50036601910037400d1003528030000000000000e8053400c10031600858034480d100214000509004008500120804d0031
400014807400cd8132481993033400c1003120100000000000000c0007401d12034441110037c209100244001b0004040d10055c01111075401931285c41d70034481510877401d1007501410000000000000e200fc01f30878c00120019c2193006cc001340ccc01e3005b80117007dc0093000bc21fd20f6c016
e407fc01db007f90030000000000000ee0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0580) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00000000000000200f400c100314200840d2401cd04a10080980024808100134000d0072400850043400cd01b0400010133400cd0030206300000000000000014f400d10237000d12270c00cd2475402100816c40932155c009d00b4c138102b2c00d91074400050cb3400dd0030a01700000000
000004000fc00d30037c00c31036c08df0025c06192086c209b0017c60590037c809f0017c00df8036c40130037c00df00350007000000000000040217c00ff003fc02fa003fc00ff107ec8009400fd80fb601f800b3043f51097025fc00f7203dc007f003fc00f7403d0181000000000000040003400d34031d00
5710d4403d30221d01150140c09c503524) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (05a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (e10808400a1001b400e1003ac80ab000b400e1003eca021003b400e1003900130000000000000e2043c00d30034d00120006c00df0037c00530007c00950013c00d70071c40b30007c20db2074c01170033c00d34073301000000000000004200bc00df023ec0077003dc08ef203ec805a0016c0
0b3003dc20df083dc0897102f800fb023dc001f003bc08df2235200200000000000000604bc05c34173c058b0472c07cf0031e0d0b0266c0183005340bcb1673c05070143400cd2570420032173401cf0070003200000000000000211b405e1827b40969437a601fd006940125034a405bdc05f4412d327a405a10
4484c1e9007845125027b401ed00780002) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (05c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (067c009f0025001000000000000004004bc201f0087c581f02848001f0007c401f4004400170207c081f0006e061f2007c401300068061f0007c001f0005001200000000000004205fc0053001440261005d4017f005f40373005d4005f009bc09750015c0469001dc00500015400772813c0053
0015a0030000000000000c004b400c10030440c101704125d027740ed104b1400980493401c12033400890067420c10033480010033400c100332012000000000000040003401e1007860181c079603e9087a4016140ed401bd805b041e50079401a900c8421e1207b68135007b401e10079000000000000000006
405f480e1003c400e14008420fd003b400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (05e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0104c001608058a4110005e00172007ca01d0004504150907e001f8807c00174007c00170006001a0000000000000080430008140215148505206808d00230148140210008500274008920304149185224008900234808500224008d002000100000000000000000734009100244009542245889
500a54189100254009500276209d20244089100274009d002760295002540095002420180000000000000000174009301a04809111e04619b40e6c019b00205009100674009d88e44119108264009d20274029102664809d00252801000000000000042043c209300a4800930064c00930164801932024c409720e
7c009f00a4c019700274009f0025c00930) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0600) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (74009520274009d0024000910025201c00000000000004804b4008101204028101234048d00234028104256848d00234208d00234028d11a14008908276808d102040081002100160000000000000c0073c001120454401180474011d00074121101568811d80074201700044001d01574001391
474001d00044001140070018000000000000068073c0093022cc01b205afc88bf022fc04ba2024c029b102f4009f002dc85bf00edc0093022fc00bf002cd00bb402fb0180000000000000e6067c00971526c00bb052bc14bb052ec14bf452ac34ab002fc00bf2027c00af4d2bc809f852fe00ab00264009f0027a8
19000000000000006073800130004c0417) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0620) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0340051001c40053441c40f7f00dc52175001f0007b841f4005f031ec107d009f4805d081c4037d885e6804d08112900000000000000042053c00130104c420b4004c001f0104c44131087c001b40874001f0007c001f0087c801f0006c021f0007c001f0005001000000000000004214fc009f0
027c009f05274019f0a27c24970066c009f1267c449f0025c008f0827c80934027c119f2027d009740240053000000000000040117400934020c129101e3c009f30278209102a1c009d00274109f0027c049d08a5c80990023c1b9f0024c009100252005000000000000042061400910035400914027474dd00274
0091c0274219c0c274809500244049d002) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0640) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (09ff0256c01230065c01f32077c093f024fc01ff007d2942000000000000066043c00df0037d00d71027c00df2006c00170837c00fb0023c80df2017c000f200fc80df0005c808f0006800df00352814000000000000006053c01e3407cc01e3086cc81bd0049c0173017fc81e1006bc01ed005b
d412f004bc21ec006ac41ad304b401ef00780010000000000000020013480e100b8400c90028401a5009969165003b400edd06b420e5001a6002d140b000ec000a4112d041a480ed003800000000000000000a0043400c10071400c100f05018d0071403c108334a0d50023400cd00934040d8143400cd0a224030
d1443400cd003020100000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0660) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000062053400d30037c07d18236c62d04115c041349bd840f30023c38dd0014c08113005e00d50007c001f0003800d700352810000000000000042009400c14001402c50023000010043411011074400d112e3402cd081350a040093020c10003400440023400cd0031200200000000
0000000003404e1022b604e1002a60031880d400210339408f1212b008ed0118400610029400e5003b4042d100b088e502390004000000000000040057c05c10021c0de5022140c21000b40561017040dc1006344ded00c3423250053428e01b4b40967802300ded1171101500000000000004201bc41f3206fc01
d3007cc092b0249c0973047dc39da8067c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0680) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0100b0442c18821604dd01904068d2b03400cd00034c4498022406c919300810000000000000000007600d10077480d10064401d51046603110034400dd0024400dd0116404190027400d90417620198047400dd2834200100000000000008020f400db1063400d504f1501c904c2401110034c8
0d10025400cd0095401070243400dd0807400910047440dd803420830000000000000c2203c40f3002fc10fb0034c20f3000fc4033803ec20ff222cc00ff001fc413b0447c00f7000fc00bb000fc80ff003d08800000000000000c0017c00df0037c00df10b5c04d70087c021f0137c00d30437c20df2015c021f0
007c00df4007c20171007c00df08350001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (06a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01140081803000130000000000000c6414441d10037400d10076401df0007401d100754011500bc441d10057421dd00444141c2067412110004401910d3700030000000000000e000cd01d3007dc01f3007cc01f3004fe01db0064e0133043cc01d3005bc01db004dc003b006fc201f000cc0193
4877a0430000000000000e4017c2cd3112bc0cff010fc10b3000e4181d0231c02ef022bc14df011f00017210fc00ff0d8b80857212fc04df2237a801000000000000006003c0ed30027c08db00a4c00d70006c041121b4c26df02a4c36df2436e901b0527440db0197c201b2207c12dd0236000000000000000000
8043404c94233004c50224400dd1006400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (06c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0037e00df0806c20dba4b7c00db0037c04df0117c00df0804c8e174124c101310b5c009300350027000000000000040217c00ff003fc10ff403dc00ff420fc00ff003fc00bf203ac00f7001fe80ff200fc007f203fc0013404ed80ff003d00810000000000000c2210c00d3c031c00d30030c00d
30013c40db00b1400030035800cb40d7e00db10458831a0077c031b0084c20930033218000000000000006800c400d10837400d10036400dd4407400d10a35401154035300d10857400dd04445011d08674031d3d24480910035a0030000000000000c0040400c10031400c10836580c10005600c90035400d1153
1400d90013440c9300140019802340c090) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (06e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (4c2463002bc08bb0237c08b70235380200000000000000404bc2dcd0033c45cf8233624cf0000c09c30452c41c30277e45c700d3c4dcd0363c260d04e0d01074215c85890174001200000000000008201b401ed0a7b629ed047b401ed004c405e9217b40525027a435e1005f405e5035b10d7d23
6840125027f409a94078000b00000000000000800f400cd0033403cd0173401cd0000400c10072000010033001c500d2600cd14834400900a0480050215480890830200300000000000000004f400cd8077401dd00b7410c50004500db007740097183e403d10413480df0c044004180344131002f7400c1803428
1f00000000000004200fc00df0337c08df) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0700) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (4b400c91030400cd0031440c10ac7400c9001340bcd2033400cd04b3400c92473404c10290403c10034401c920312832000000000000040003401e10078401ed0078401e9804f401e1105b401e1127b081ed004b401e1007f40331487c411a100f8403a10079000000000000000004004f400e34
03c420ed0039400e1000b400eb003b400e7143f400ed002b400eb0038400600038420b10838400e300390033000000000000042043c00d20036c01df0034c01cb0027c00d300730401b01b7c20df2017c00d20855800030070d019b0034c00830035281000000000000006200bc40df0837c28ff0037c00f70009c
60ef0013c001f1137c00f70017488ff003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0720) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (289d00274409d22a46209500e74009d00244009d0024a0180000000000000800074009100a34239d00e7452933024c009d09a74029500234519906a74009d00e54039d00674139100a44008500222003000000000000040043c00930027c099f0167c21970026c009f00e7cd09b0027c419f0067
c409f2024cc58f0027c25972424d00970825083000000000000006004bc00170007c001f0007c021f0407c001f0007c02178007c001f8007c001f02048021f0107c921f4007c0017000500120000000000000e001fc00530014c005f8014c005b00df40043115fc41738017c005f01dfc0051009f40273009cc007
3009cc0153001528230000000000000c20) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0740) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000ca060c00bb00acc00bb002cc20bb0027c00bb002cc00b300e7c00b7002fc80b3002dc11bf002f400b701ee400b72025b0190000000000000e2067c009f0527c34bf002fc00971529d009f002fc00f34527c40bf002fc809f002ad14bf002fc34b70d2bc00b30523301900000000
000008607bc00134007c400f0017c00170004c001f0007c005b1107c001d00074001f0004c04173007c04170114c001f0006001b0000000000000020534008100234008d00234008100227008d00234008d15234008900234008d0021414cd08234148105204009d00202010000000000000020073400910427402
9d80274089d00246009d00376809180274) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0760) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (970025d439f0827c00970267c00930c25c008f0027c409f0067c009f002400170000000000000e2414c009b00204009b0020c009b01274009303e6c00830027c009e8067c009301a59429f00e742d9702e6c00970021204500000000000004206040091002440081002740095002540091203644
09500274009d1027400990025580dd22a560091042740091202428180000000000000480484008909204008900204008904274008110264008191a34008c00234408970214008900234008580a648081052120120000000000000c2070500110144515110007900150147e001340044001519c74001f00074001b0
005c825d0007c801109c34001140470018) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0780) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (279c01e5017c00100000000000000020034006100a8400ed0038580e1013b400e5001b440e90138410ed041b401e400b9002ad000b400ad4039401e1003c00000000000000000000534004180f0440cd2032408850033000c10813400c90030407cd1973400cd08d1701cd1333444cd40b1400c5
0030201000000000000006001340069009c4007d005cc0a61001300055009b44171081c4027d205c4005700984007d001f4b075401840051201ca000000000000000042043c001b0404c301f0206c40170007800120387c4a134000c801b0004c001f1004c101f0087c001f0104c00172005001400000000000006
004fc009f0027c009f0025c009f5127c80) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (07a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (003940421003c424e1001e42cf5013b4c0e1003b480ed00296042d05084a02d001b480e98939008c0000000000000421544256b0068d014b0179c0527023850de1054ac4dcb00734056b0373401ed07404483d0942c1da1067b401e1017d0075000000000000042108c4173227cc09d30279c011
3007ad01c30a58c01e3267fc89d3207fc09df007dc0d7f0074c019f007fc09da147db002000000000000042143c005f0027d009fa035c004f2237c00de0013c00d710b7c408f0034400c71036c009f00074201580b6e00cf183da014000000000000004043c016b007ccc17f007ac0165007fc21e3005bc01eb027
0400eb007b881ef1079c01ff105bc012f4) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (07c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (74a1192047403150487c40d14034288b000000000000040213c007f003cc083f001cd007b003fc00f3001cc0173003fc003f003fc00f3103fc1033801cc001300b7c80f3283d0081000000000000040007c005f00b7c00df00b7c00571037c00df0017c06db0037c009f0637c00df1497c001f01
07c041f0007400df00350009000000000000040050c005b0034d40932035c800301fcd40d05016410c7003fc40910077400df0861c259d20704009f0277c31db203da0100000000000000420184004900204001980314000d01f0400c10052402cd9833420090833440cd10404020d2042602110093400c1003500
2200000000000004000050469003840471) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (07e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (17c004f00a3c142f0025c007f003fc04ff0b174581f0637c883741b3c88f70f07c0037020dc083f0205c18ff09b7a8a10000000000000ac003c5c5f0104c041f0414d045b2037e04d18114c0413003bc065102b7c8cdb21a7c40111184c0a13001fc46d301b4000300000000000000a043400450
1205104d2130610490037418c50314400891033486412123404c94003400095203440050902400c1223020300000000000000200074005d00e44009d0074403590037400d10854400950033423d10477480d900e74811900c6403112833400d10034200100000000000000021f4005700744009d01f46035b00334
40d5207049b5b2037403110073400d1005) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0800) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0400010000400010000400010000400010000400010000000000000000000000000800020000800020000800020000800020000800020000800020000800020000800020000800020000800020000000000000000000000000084002100084002100084002100084002100084002100084002100
084002100084002100084002100084002100000000000000000000000008000200008000200008000200008000200008000200008000200008000200008000200008000200008000200000000000000000000000000850021400850021400850021400850021400850021400850021400850021400850021400850
0214008500214000000000000000000e00) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0820) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000850021400850021400850021400850021400850021400850021400850021400850021400850021400850021400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000400010000400010000400010000400010000400010000400010000400010000400010000400010000400010000000000000000000000000010000400010000400010000400010000400010000400010000400010000400010000400010000400010000400000000000000000000000004000100004
0001000040001000040001000040001000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0840) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000040001000040001000040001000040001000040001000040001000040000000000000000000000008400210008400210008400210008400210008400210008400210008400210008400210008400210008400210000000000000000000020033800ce0033800ce0033800ce0033800ce00338
00ce0033800ce0033800ce0033800ce0033800ce0033800ce00008000000000000000000000840021000840021000840021000840021000840021000840021000840021000840021000840021000840021000000000000000000000000080002000080002000080002000080002000080002000080002000080002
0000800020000800020000800020000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0860) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000000000000000000000f0f00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000003c3c00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000420800000000000000000000000000000000000000000000000000000000000000000000000000000000000000000010820000000000000000000004000100004000100004000100004000100004000100004000100004000100004000100004000100004000100000000000000000000
0000001000040001000040001000040001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0880) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (fffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc00000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc00000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (08a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (008500214008500214008500214000000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc00000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003ffffff
fc0000000003fffffffc00000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc00000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc00
000000000000000000000000000003ffff) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (08c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000400010000400010000400010000400010000400010000400010000400010000400010000400010000400010000000000000000000000000800020000800020000800020000800020000800020000800020000800020000800020000800020000800020000000000000000000000000084002
100084002100084002100084002100084002100084002100084002100084002100084002100084002100000000000000000000000008000200008000200008000200008000200008000200008000200008000200008000200008000200008000200000000000000000000000000850021400850021400850021400
8500214008500214008500214008500214) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (08e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (8000200008000200008000200008000200008000200000000000000000000000000850021400850021400850021400850021400850021400850021400850021400850021400850021400850021400000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000400010000400010000400010000400010000400010000400010000400010000400010000400010000400010000000000000000000000000010000400010000400010000400010000400010000400010000400010000400010000400010
0004000100004000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0900) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000010000400010000400010000400010000400010000400010000400010000400010000400010000400010000400000000000000000000000084002100084002100084002100084002100084002100084002100084002100084002100084002100084002100000000000000
00000020033800ce0033800ce0033800ce0033800ce0033800ce0033800ce0033800ce0033800ce0033800ce0033800ce00008000000000000000000000840021000840021000840021000840021000840021000840021000840021000840021000840021000840021000000000000000000000000080002000080
0020000800020000800020000800020000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0920) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000000000000000000000000000000000000000000000000000000000000000000000f0f00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000003c3c00000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000420800000000000000000000000000000000000000000000000000000000000000000000000000000000000000000010820000000000000000000004000100004000100004000100004000100004000100004000100004000
1000040001000040001000040001000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0940) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0003fffffffc00000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc00000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003ffff
fffc00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0960) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000fc01ff804ac04fb007cc01df0137c01f30074c09ff0277c012f0076c013f007f8213f207fa0030000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc00000000000000000000000000000003fffffffc0000
000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc00000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc00000000000000000000000000000003fffffffc0000000003fffffffc00000000
03fffffffc0000000003fffffffc000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0980) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (fc003f003fc01ff003fc003f003d0085000000000000042203c00df0037c00d70007c00dd0967c00df2836c00df0037c00d30034c00cf2037c231e0037c035f0036c001f0035280000000000000004200f420d50837400dd2027400dd0047620dd0036400cd0037400d90034400dd00374011d90
37408dd00344001d0035a803000000000000040043400cd0833480c50031410cd0803408cd0032400cd0231400c10032404dd01334000d00334000d0032400cd003328130000000000000c0007401d70077400d70007404dd0046c03dd0074420d700f7401db0074400dd10374211d0077400dd00744011d007500
030000000000000e210fc81ff207fc61df) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (09a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0b405ec007b401e1004b401e1006c401ed007b405e9007b485ed0178449e9017a401bd0078401ed80784072d0178809f00000000000000000f400cd0033600c10003400c10020122cd0073400cd0033400cd0070400cd04334008c08304004d00714090d0032a00700000000000000005f400dd0
037411d10167400d10424c41ed0837401dd003f400dd03b040cd120b44801d043440b5d00344020d0034201b00000000000004201fc00df0037c40db0135c20db1026c04df0037c00df0037c00df0035d00d72035c821b0034d011f1237c00df08350803000000000000040207c00f7003fc20f70087c00ff102c4
00ff003dc80f7003fc00ff003fd00ff003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (09c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (81fd0078401fd007b4036d0078611710078441ed0078000100000000000004004f400ec0038400e1a018c00f90028406e1003b400ef0138400fd0038400ed803a400a90038480eb003ac002f00398813000000000000062043c00df0034c20d30003c01df0025d00f3c037c00df0035c01df0036
d01df08378809f0034c00530070c000f0037a01500000000000006200bc08ff303fc88d7202fc00df022dc88cf093fc00ff063fc00df003fc00d7023dc003b0037c00ff003fc082f003da80200000000000000404bc05cf0833c25c34031c00c34020c11cf0673c11cf1073c05cf0171005df0177c000b0370c215
f0031c05cf017000120000000000000001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (09e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000042043c009f8024c00920027c009f1066c83830027c009f0027c009f0167c009f0027c009f0164c219f0066c009f0027081000000000000004284bc001f0007c00170007c001b0007c001f0807c001f2007c001f0005c001f0006c001b0007c021f0007c021f0007021200000000
000004000fc005d0014c005b021dc005f009dc40714017c205d2015c205f0014c005d0017c007f0014c00730014c406d2015a81700000000000004204b400cd0030440d90250500cd01b0480c10033400c50030440cd3030440cd003342109a030524d900324000500332812000000000000040003601ed8078401
e9407c401ec0069441c1007b401ed08794) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0a00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (9b20234149f0027c209f0827c14af0527c00bf0027c14ab0024c00bb0027301900000000000008006bc001f0004c00074107c001f0006c041f0007c401fa107c001f0007c001f0007800171004c001f0006c001f0006101d0000000000000080434a08d00204008585234408d002241485602348
08d85234208d08334008d00230008d0020400890022400cd002122100000000000000400734009500244029580374009d01264409c00674019d00274009d00256209d2827400d50024400dd00264019d202420180000000000000000174009d0024502910ee34809d00244509100234209d00274009d00a74009d0
0274009d006450c9902644019d00262001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0a20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (027c038f002528450000000000000420634009c00244008120244009d00646009120254009990274a09d00244009580354109588254829900264089d0025a81800000000000004805b4008d00224148105226148d10204209120236048908226008d00206049d01204009d00234148900235008d
0023a0120000000000000400634001d0004d011320d4c411d2006d02114005c811b00870001d00064011f0045420170007c01110006c005d0007081c0000000000000ea063c809f2024c20bb046f8009f003cd11b3002fc02b304674409f002ec08af0a2cc209d002f400bb002fc00af0027a01900000000000006
4067c009f0027c14bb052ec149f002dc00) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0a40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (8053400cd0073410cd00336004d0033600c500324068d0063400c50060403c144404030d1032a014000000000000028001c005d001440071245f4005d101743063001f4007d00174205d015ec027d195f40059001c4007100194007d0014a004000000000000042143c001f0004c00133007c801
f2007c801f0007c301f0007c001f0904c001f8107c40172204c32130204c001f0004081400000000000006214fca09f0025c10971562c009f0027c209f0025c009f0023c809f0027d009f2027c04970027c44970027c109f002500170000000000000e8117c009f0026c009340a64009f0064400908023c0093202
6c009d0026c408d08244838f00274009b0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0a60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (ac20eb026bc000b03484150d2371883500000000000004010bc41dd2074c41fe0355e09ff027ec09334074c09c70277c09ff0077821b30064c01f2106b4017301504012f0077a002000000000000040151c00df1037d001f4027c00df0037c00120027c005f0837c20df0017c009f2007c00df00
27c007a0003c001f0035b810000000000000000043c01ef007844171106fc05ed007b4812f007bc016f007bc01e7007ac01ad006bc01e70068d017308485012f00781014000000000000002001480ed0038400a1802b408ed00bb40029003b4026d003b400ed003a600ad000b400e900284036500094102c003880
04000000000000000043400cd0030408c5) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0a80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (07c00df0035c02d72487c00d60837c00130037c027f0037c00df0027c809f1017c00df0027c001f0007c045f10370001000000000000040043c00dd0034520dd0095400fd0074c409f6030400550037c00dc0027c00530034d04d300274111300008031f0035a83c00000000000004000b400cd0
0324008d8034600dd00604200d8822400c10033400cd0803680090022400c900216051900005030d10332826000000000000000013424ed003a404fd2419624ed0c384002d0138608e5033b400ed003b480a10128400f1023b4006100084042d82390008000000000000044157405cd0378d0da7017ac85f70228c
05014172c0de1017b485cd00eb40d0b016) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0aa0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (08df0717c505f0284c80d500a4c40530426c2e1f22b4100100000000000000a043410c90133490080000484cd002340401a4b34044d31324c0cd010340c0d0101400d184204c90501204000d003020100000000000000a8007400dd0037402190004500dd00374011100374035d0037400dd0047
4205d0104400d500244011100664101d0034200100000000000000020f400d90037441531164e00dd0827401114027401170036400dd00574139d0015400c120604015524444000d0036200b000000000000040203c00ff003de0373426d400ff096fc0033003fc003f2037c00ff003fc057f003cc00f780acc007
3080ec28bf203f09a10000000000000400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ac0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000680404008100004000100004004d00024068d08304c0c10032404cd2033400010427420450001600c58801400c9201120130000000000000c0406c40812004400110004c001d00044161700744011a0076c40dd0074c011d012444011004440afd2044480c00007000300000000
00000e800cc01930044c21370046c413f904ec80370074c01070037549ff007500035106ac007f1049804fa200dc81fb200d8903000000000000068807c04fe00bfc1007020ce00df002fc100f002bc1c3725be808df000fc041f030bc00ef2527c043f102fc8c1f033fb805000000000000080003c8adf8137c80
1b9004414dd8827c141301b7c025d00b74) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ae0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (9900b4425cb047cc00df00344014b0876c21511234421f89410493d12904201700000000000004000cc02df0064c05d30074c01d720378009f0034c00d30437c00d30035c02174436c035380a4c00d34005c04d31094000b000000000000040607c00ff026fc80ff003dd00bf003fc08ab283fc0
0fb0031c00fe003cc091d007dc0053000ed00d3000fc00f7060d0081000000000000040200c10d34064d00d34034c609d0036c011f0034c00d31037c00cf0035c02170276c01570081c20db0045cc0db00c7208000000000000006000e4c09108044c01100044004d0804480152034400d90036400dd0037500550
026403510425480dd1054480c904012003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0b00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (004c20d3000d301000000000000004200bc013f001fc401f020fc007f100fc003f023dc80db0635860ff0234c28330137c007b0025c22f2101bc08ff42393802000000000000000058d050f0350d011b0144809550007c0dd70872ccdc14171c80d10177c090f0830880450102405c50281c05c1
003000160000000000000020184092d025840d21834840921084800929807a661280078409e9007f401a9057a48965446e50dedb048481e1204c005f00000000000008001c4041d011440219040461005004242005813271201083141bc1003341908003440055104220cdd0101402c10000280300000000000000
285c411dd0064401d24074521db0434405) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0b20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01d6c025f0014505710013c00740019c005100174236340544227f205dcc07f005cc0053401d20030000000000000c2049409510032401c90072406dd0970406c1103340bc10031500c12033413c1003540ac504f0400cc82b0600d100352032000000000000042000401618078401e1007a601e
d0078081c1087b401e5817d421e9007b4012190f84014c2069605fd1048401f10071000000000000000004004d40071003ac00eb003ec00ad0038c00e1403bc00e12138400f3003b400a3a03d400670028d06ed0818420e140090037000000000000040040c00532074c80d32034c809f0036c01330037c00d3103
0840d10073c00132034c005f1026804cf0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0b40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (05148500206148945204c18945202010000000000000020060408bd002c080a10028400bd89274109124274109110254109d0025408d9022641095002541099002442195402420180000000000000000045009d0024c029300a44029d002740091e0274409509a64838d00244009100644ab9504
a14019122645009101a62803000000000000040040c019f00e4c089300a4c429f0067c00939227c08931027c089f0025c009b0024c01830025c05870020c00970025001000000000000004004bc023f0487c101f1407c001f0207c401f0005c301f1084c2217000780a170007ca6170a860021e0407c001f000500
1200000000000004000cc00535094c0753) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0b60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (60c041101044241f01034041d0507401130007400130004c011140044021300044051b00044011508844011309c700180000000000000e4060c02a300a8c02bf00afc02bf102fc81bb402fc60b7416bc00b3802ec05b1102ed53b5202ce07b59068c02af01edb019000000000000062067c149f0
525c14970527c149f0527c14b7202bc00ff0027c949b0027c20bf052fc14bf002fc5497003fc14a6452fa819000000000000080068c007f0000d00034004d000f0007c04138007400110107c001f0005c241b2006c44170005c041b0904c80170104001b000000000000008040400ad0038481a10068401ad002b4
148100234008505204008d0020414d1203) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0b80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (801f0007c0e1f0006c401b1084c20130484c00130105001000000000000004014dc609f4027c10978027c049f0027c01976027c00970022c00970027805930425c008f2125c009b0023d009f20e10013000000000000040114d00930024c009f0027c019f002701b970023e02970027c00890026
811971020c83952166400950024c809340252045000000000000040070400c100304008d0037400dd0827000910027484911025400990024000954034414910826200950124400c100a5001c0000000000000400584048121205848d21234048d082341285c0274008500a34108900224028c08244208500226068
500a06208110a120160000000000000c40) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ba0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000000040d01eb4079c01fa4078c01f3006dc01e90078c01ef0048401ff1079421ad087bc81f10079c0003406ac01e340580010000000000000000000600f1043d410e11479401e1006a411c50038401f95009600ed00396007d242b440ed003b44361008a410710038000000000000
000000004040bc900b0400c100b1400c14831031c90030520cd10004298d0031401cd10f150cc10671400d00072641c10030201000000000000000000040073201d40071201dc83710016c007f001c4407b015d44b7d001040369005c4427f201a50871101c40071001ca800000000000000040040c04130105c00
1b0104c0c130204c021a0004c201f0804c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0bc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0da0124000108214009508324810928014011981b14400d90834201100112022000000000000040013424ed001b404a9022a400a5002f6447d923a480f4110f400ed083b4162d002840025241b4000d000f480a50919008c000000000000044155801ed023b40dcb08184884b02294070d037840
5e54148400af103a40003020b404b3237840801210b02901005d107500000000000004210bc09df007fc01f3007cc01f70078c014f0074c29fb024bc01bf027fc053c006c801b7207ec0177004bc49950255a002000000000000040053c001f0027c005f0835c20df0827c00df0017c000f1027c00ff0034c004b1
004c00db0030c801f0805c201f0591a814) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0be0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (085424911454a20100000000000000020f4001300874021d0047c03150022c024720074001b00044081d00364511d0087c019540774011d88054021500c42083000000000000042203402f3023fc00ff00dfc037380acc403e022fc00ff005cc00b7183e4003f808dc00b7003dc003700ccc0173
00190089000000000000040007c00df0097c029f8025c02970025006df0035c00d70084c009f0036c00130887c00d20036800520007c021f00e50009000000000000042043c04df0037c20d31036c00d700374119d0036c20d70013e009d8037c039d0014c1b9780b3c00df0e47c20d72054a01000000000000004
00094130d0007400090802500090023403) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0c00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0007c24ff102cd00330067801df0077c01ff0077c01f11276c02fb022bc00330134c403c2077a0030000000000000ea007c1c3f000fc041f250ec043f002f80437a00fc740f0107d20af013e8143f800fc803f02238043c000f80c3f020f98a1000000000000080003c041b0007c4e1f00834020
10024c081d02a7c06df17044009702b64001d0005c40150015c02170004c0213001e20030000000000000020434040140834100d2001408050026410850432410c9010040088003340008000240080002744209000146205010000300000000000000a8007400190027414550037400d100254089d8037480dd618
44229520374011d20054019100774011d1) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0c20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (fc00ff003fc001f0037d00ff003d80050000000000000e2a8bc00d3103441b9100b7c20df0267c410300a7c01d70037460df0037c00d30036d00dd0027405510034c001d0036a88200000000000004000f480d90030500510407460dd002740115c1a74409d0037400dd1037400d10030400d508
274011000340209d0036a80700000000000006804f440c11030442010003400cd0023481010007400c50033400cd0031440c06030506cd01334000140304088d003100140000000000000c600f4c1db2134402510007409fd00244811100374019d0077401dd0077401d10134402ff12a74001102bc403dd107708
010000000000000e820fc01d30a74c4033) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0c40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (3f401ed827b4a9210248481ed027a40d2d1179409ad007b445e9027a405ed0278001c1026840125907b401ed0078800600000000000008000f480cd00334290101c2400cd00720230920534008d0033400cd8033400cd0030400d10020401c500334008d0032a00700000000000002006f400dd2
037420d12814400fd0026c03550061c209d0037400dd0036420dd0035400f1403445153203f440cd0034801300000000000004200fc00df0037c108b4016c00ff8024d50130007c00df0037800df0037c00df0034d00f300368305f003bc425f00350803000000000000060017c00fc003fc20ff4a33c00df002cc
205b106fc03bf003fc00ff003fc00ff003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0c60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01e9207b401e90078405e50078401c12070401cd0079000000000000000000604f440eb103c40031002ec0ae4003ac00e12038440ad003be80e3003b400e1003c400c1083ac80a10138400ed00390813000000000000040043c00d00034c001b0067c00f38074c80938816c019f0037880d70073
c00d34036d1cf30024c00d5213cc009b0035201000000000000006200bc40ff003fc48d7003fc00ff003fc0037003fc089f0237c00ff0237c80ff0037c00ff022dc08fb06bfc48bf023db00200000000000008404bc0dcf0173c0dc30562e0dcd0432c950b0557c01cf0073c09cf017340dcf0170400c30070c00c
70073c038f007010120000000000000828) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0c80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000042043c00930024c018f8025c009f0024c059300674009f0027e209f0027c20930026c008300a44049f0024c009f002708100000000000000e004bc001f0007c001f0006c201f0007c02174007c001f0005c001f8007c00130005c401a0007c01190007c000f1007001200000000
000006201fc805b0014c007b061f400510114c096b001ac005f0017400570017c005b0014c20530154c10710014d037f0015a80700000000000004005b400c90034410c00030400c52032403c980304008d0033400c10033400cd0030400c14032421d57034418cd00312812000000000000040813401e92078601
e1406b445e0106054369845a441fd007b6) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ca0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (ac052b800af0027c009f2027c009f2d26c149f052bc34bf0527400bb1027b8190000000000000ac07bc00130004c041d0107c041f0114c04130007c001f00076401f0007c00130007c04130105c04170104c041f0006b01e0000000000000080534008588205148d25234148d052141481802744
08d20234008d20234008140214148105215148105205148d002020100000000000000200734009180244009d02a74009d01244029140a74009d08274009d00274009100234009110274009500244009d0024a01800000000000008800f40095002440c9d88e5c009d10654019102e74009d00274009d0827400910
0244209144e14019100244009900262001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0cc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (020c0393002788050000000000000420634009d00244069100334009100644219502244089520274209d0827400990024400950025400910024406910025881800000000000004004b4008d0c204008115234028101304208541306008d08234808d002340081052071081843340c8104a040081
0023a0120000000000000c20734001d0044d071140d74a01b0a84500114116c801f0005c801d00074001b40444070501c4c1511410442a114007001c0000000000000e2063c009f0024e13b3046fc0193c22cc10b300a8d00bf00274009f002fc20912024c15930568c25b34164d05b3402f80180000000000000e
6067c009f0d27c34bf152de009f052fc00) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ce0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (8030400c11432401c00434400cd0033400cd0033400c10030400c10090402018031600c5003320140000000000000200534005d001440071081c48055409c50073001c5204d1015c205d201740055001ed005b401f88071001c4204d0010a014000000000000040043c001f0004c80191006c201
30004c041b0004c201f0007c001f0007c40132006c00130006c02130004c00170005081400000000000006004fc209f0027c008f0127c009f4023c009b2827c009f0025c009f1027c009f0027c008f0466c328f0027c019f002580170000000000000e0017e409f0024e019310e74409140244848500e44009d802
74009f0027c00910020400930221d04930) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0d00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (c400e120434a3210038515cd11798055000000000000040003c01df007cc41f70878c05f7427e401064074c85e7027fc09db007fc09d3027c401f3004fc2993007cd01cf0277a000000000000000060043c00df003f4005f2005d00df2025c400f0005c00cf0035c00df0037c20df03bfc06ff00
35c801f4036500df0035a810000000000000084047c01ef02f8c413b184cc01c3006ac01236058c01ef007bc01ef007bc81e1237cc49e300784013301f1c01c7007a00150000000000000c2007460ed0038400e19038401e5003040231003c480ed103b480e9003a600e5813a408e8001b410210139400ed003a08
05000000000000080053600cd0030509c9) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0d20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (07c20df003dc024f0007c00c200c7c0e1f01a7c00df0037c00df0037c00d7003fc00ef00d7c0e5a0033c40df003580010000000000000e20d7c00df003ec01951074400df0054420010024510df0037c00df0037c00db003cc40f3005740257003c980df0037a815000000000000040013400cd0
033408048802000cd0026400010054401c10033400cd0833600c14030400c08007403058030443cd00332804000000000000040003400ed003a40021060c60ce900284002174184cced003f424ed203b404e91138400e1000b404a50038404ed00390a0000000000000004625742ded083940985003ac04c1033ec
0d01037ec01e3017f40dcd007b405c1007) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0d40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (02df0537404db89bcc00f11225e14530037c16d70bb6a00000000000000000a043418c500b06040d1001400c40022606051323408c50033634cd00b2400c584b1440c12113604414032406cd01302010000000000000020007400d10831400910231400d10865683110465400dd0037400dd0037
400d10030400d50455401110037400d58034a001000000000000080217420d50034404570005400d50166c01150846440df0037400dd0037400d50035420d500e5c41512037400dd00360081000000000000042213840f3003cc42b3083c800db002cc0033080f400ff003fc00ff003fc00fb103cc80d30027c007
30037c10ff183d08800000000000000600) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0d60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000e8043400cd00324048d02204104d0031400d100024000100334000d0031440d943004201d2133444c51007401150033a0100000000000000c2017421df807440a5108c44045d0074401d500444015500764011d2075401d521844011d1134404f1004443410007f080100000000
00000e000fc01ff007cd0813000cc017f007cd01e3004ec010b0077c013f007cc01ff220dc013f0a74c28f7004fc213b103fa2030000000000000e2497c04ff203fc2407050fc40ff002ec003f402eca8df0737c10ff0137c16ff0137c00ff2325c007f043fc04ff0b3fa8050000000000000ac003c00d300bdc1c
9300b5e2ad30025c101344a5c00dd00b7c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0d80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (dd0007e050d2032c001d0034400d90007403c10836e04f1010144210003c201300000000000004200fc00df0035e001f0090c005f0035c08df0004c249f0034c001f0034e40df0007c0cd30034c00cb0004c20170075080300000000000004061fc00ff003d809b7481fd007b003ed00fb004fc8
03f003ec023f003fc00f6880e0023b203dd00ff000dc003b68310187000000000000042003800dd0036c011b0094c014f0035c00c34102c099b0037c021f0035c20db24c4c131f0036c20d704c7c680f1034080000000000000006201f400d50036400d900644015d0035400d501044005518374021d0035400d00
040100dd0836500d1c044400152035a803) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0da0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (010c001b0577a81500000000000006600ac00ff003fc40df003dc005f003fc08df000e808ff003fc002f003dd08cb001fc08fb083fe08d7010a88c17063db80200000000000000404bc05cf0031c058f8132c801f0433c01cf05404070f1f70cc80f0032408cf0803480078376408db1001c0517
0070101200000000000002001b405ed00794056d004a4096d8078401ed014b48d6d207a4013c007a401e9004b401e4407a40bf9114d11721007880060000000000000a001f400cd00314091d00024004d0873426cd00404820d20306000d0032400d51003682051032400c908014010d8032a00700000000000000
004f400dd0035e019d20145005d02f4c00) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0dc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (205d401630011c00590059c006f0017e006f0017c005d105fc867d0816c005350dcc016b0015a0170000000000000c204b400cd0030401c50031401891031400c90271411cd0033408cd8832400cd0b33406c41033400c10030680c14033201200000000000004000f401ed00784016d04794033
10079401e9804c401fd007b4012d007b401ed807a401ed007a401e100d8481210078000300000000000006204f400ed0038400c7082bc006b00394a0eb00094002d183b4002d003b480ed8029c00ef0039c08c1181840031213180130000000000000e0047c00df0036e015b0024c00430031c01d31005c808f003
7c001f0837c00df0005c00dd0036c8adb0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0de0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (14008d00204148500265209d052020100000000000000000634009d00274029c0034400d501274009100240029d00254209d00274009100274089d202650295002640095002420180000000000000800074009c00274229c2025400911065c07994426c009d20254009d0026400910026c829d00
244829506204049d002628010000000000000c20434009f0027c009f1024c10920027c099b0025c029f1167e009e0027c40930022c419f2024d45932064c8297002700100000000000000c004bc201f0007c101720474001f0087c001f0407c081f0007c041f0007c001f8005c021f2005c00070407d0b1f000700
1200000000000006205fc005f1016dc77b) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0e00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (734001f000452b4d2207c40124004400130004420110005c005d0005c00110144c00174144d22110004400110007081c0000000000000e2063c009f0024c09bb0164e0093002cd00bb202ec00ab002fe008f002f400b78025c00b300a5c01b70029c00b3416fa0190000000000000e6067c009f0
027c14bf002fc14ff4027c00ab002bc00bf0026c80bf0026c209f052ec00fe0527d949f002dc14fd00271819000000000000084073c001f0007c041f0104e00170007c001b8005c801f0807cc01f00074001381074005f2004c04170006c00170106001d0000000000000008430008d00230148d15214409108314
408100260208d00214009d082340081c52) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0e20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (40130807cc0170007c06130006d0c1b2005c1a1300050814000000000000040057c009f0027c008c0127c009f0027d40970127c259f0025c009f0025c009f9861d009b0027800970027c009f00250015000000000000040017c009d00244009b14e44009b0020c408b84a6c118b0027400970027
c00950227c408b2021c009f282544093202108450000000000000600630009500246009d0827444910024400918034440d100254049c20274009108a4404940024400990034684910025a8180000000000000e80434008d08204048d0820400982020400990026400d9002340085002344085042240099a1234088
d3061440910222a0100000000000000840) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0e40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000d3c01ef0078d01630078c05e7085b401270079401ef0868401e6007bc01ef817b001af017c401ef004ac016100701010000000000000022811400ed0038402e15071404f1803b49021003e4406d242b401f5107b400e5003b600ad03384204500af420658028800400000000
00000a00d3400cd0030401c18030400c19013404c58030484cda030400c50031400cd8033400cd0030402dd0032402c10072a014000000000000000411c005d2014c40710815c4061491f40071101ae627d0013c0055001740057001748275001ed0171005b40065011c2004000000000000040153c001f0004c04
131886c02170807c801f4087c001f1804c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0e60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0500f140305003360bcd0033400c100b04ab0d08344000924834060100232812000000000000040003404ed013b604252138614e5001840821003c4043d013a400fd003b404e50038448ad00381042d200e4002108290088000000000000062057421cd007a401a70278401f1a2b9c070f017148
56f0b7b400ef007bc05ef403d40aad003840529032b40b01412188150000000000000e000bc09df0277c09b70274d19f70058c01320274c011f0074c01ff0277c09f714fec09ef907cc4133626bc013b006fa002000000000000062041c00df00378005f0837c01cf0013c00130033c001f0827e20db0032c20d70
0b7c20970037c001b30070401f2025b810) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0e80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (045481198024000100000000000008020de00dd003640c9d2034500c512d54031500444481d0064580dd0034c00dd0037403971036c001100c040301202600870000000000000c2201c00ff003fc10ff103cc00f3085cc4137049dc013f022c400ff003cc00ff043fc10bb203cc032b000cc0073
103f08a10000000000000c0007c00df0836c029f0037c10df0815c821f0827c04df0025c00d60835c00df0035e009f0835c00170087c08170027000d000000000000062053c00df0037c01d70034401f70010c00011170c068d0034c08cf0037c80d501be5029d003cc40932006cc1530831a8340000000000000c
201b400cd003340a050030403c10013400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ea0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (005ec01b3003d801130027c0133003fe01df004ac01d3025d489f10a7fc01d7027fc61f3007fa0030000000000000e6017c00ff003fc0c1f023fc80dd001fc260f018bc242f032ec00ef00bec00df003fc00b7013ec420b480fc021b402bb805000000000000084001c16df0537c0c5f2134ed4d
30014400171215c141f8025c00db0134c14df003fe009f0034c001318044481302269003000000000000000041406cd01324040d8930404d5001140c01012042cdd01a1480dd0031604c910324408d02334040100046040510202014000000000000000005400dd00374005d0034400d100044081520354009d802
5400d90035400d500360019d0034410101) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ec0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (fc09f5002fc00ff025fc09ff403d80050000000000000e0208c121a0435c939f10c6c2093a035c07071027c01110037400df0056c00d90215c01d30823c02d34057c01d30037a80200000000000000200d4805500154245c0037484910034401951017410190037400dd0067400dd00370005900
37400911037480510005a0030000000000000480406005900114024d00076008100b04008500034000100b3420c58010400c90135604410175400811133404410007a8100000000000000c0005401570045c031100474219920f44801142274011b05b7601dd0047401d581136a4d11837400d10037410d0007710
010000000000000ca20cc0193200e8003b) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ee0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1b401ed006e44105005a481fd007b40569016b6016d007940de4004f401e1014a423ad00594056d01eb401ad007a000600000000000008000f4100d00a06210500820038d00b34004c0023404090033400c10003400c1c1074208922104124d00274008d0032202300000000000002004f4024b0
0f2821c120a04019d10bf40a9104676111d003dc06d52027480d108774015d20654469d08574075d0000a01300000000000004000fc00930eb5c08d71315c249f2176c80139027c001f1037410db0097c00db0077c015f0026c409c0057c045f00050803000000000000060017c097f013d401b3021ec01bf003bc
003b0023c087f003bc00fe002fc00f7005) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0f00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (81ed007b401ed00684012d00484013100484012d0049000400000000000004204f4406d00384006d0028680e700b8420710129c20e1113ac20ed003b400ed2008480ad1008440610008400ad00399813000000000000042043c001f2034c005f0816c009f8834c00530224c0003023cc01cd0037
c00df0804c019b0006c01530044c019f0037a01000000000000006600bc00590033c04bb0221d00ee003fc80350117c805f1237e00f70837c20f70227c003f201dc003f0327c003f0005a80200000000000008604bc014f0221c41878213c108d0033c010d41434010f2173c85c303f3c0dc30163c040f00104051
f0223c440f000200320000000000000808) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0f20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000040043c159300a4c208b1065c00930224d00934061c489b0025c039f0826c009f0067c049f0026c039f0027c009f0025081000000000000006004bc0a1f0205d001e2105e08170005c02170405c10172006c021f0007c001f000fc001f0087d001f2c07c801f0005801200000000
00000e001fc017d20dcc887d009ec016f001ac097340dcc136800144005f00dfc005f0014d005d0016c00534094d005d0017a81700000000000004205b401cd04f2400cd00b2480c500325005142e1442c90037400cd03f3400cd00204002d00084002100080002d000b20160000000000000400134016d0078401
cd244a481fd117a4036100604012920784) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0f40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (bf852fc00bf0521ec09e002fc409b0527c149f0527c148f0527c149f0027a81900000000000008c07bc00531114c041b0805c00110104c00510105c001b0105e001f2004c001f000fc000f00074001f0003c000f0006b01c00000000000000a053600892520714810024400814d2560081252040
09185234008d202340089806b401ad002b400ad206b401ad002828140000000000000200734009000244049902356189100247049101254009900274009d00244009d012f400bd002f400fd012f400bd0024a01c0000000000000808074029b00204219514e04439100654209101ec401910027c059d0827400990
0e74229d11a76009d00a74229d00262001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0f60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0274029f0027a805000000000000040060400990025482950427480910825400990025400950027480d530254009d00254209108264009d20274809d002520180000000000000480484019902234028d00234008100214148111236408d1c234408d00234008d00234008184244048d04234008d
00212012000000000000046070400110005c001f1007c001180844845b0585c801f81c7400170005ec01d0555c01518946c011d01474155d0017181c0000000000000e0060c80b3012bc21ff802bc00b3056cd00a8046fc00bf0467c00bf002fe009f002fc82b3103ec82bf802ee00bf0025a0180000000000000c
a067c40bf102fc00bf002fc20af0027c14) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0f80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00f1404cd0030002d18075401c18030404c10033400410030400c50030400dd0072411cd0032a01400000000000002005042061209f4407f109f40277005840375205c49871001f41273201740071011c4207100584817d001c4037d0014a014000000000000042040d10132007c40111187c001
70244c02134407c601300078001b0805c00134086d121b0104c081f0004d021f0085081000000000000006004fd05974921c089f12654839f4026c139f2a65c029f0827e00970227c009f0025c009f4827c099f0027c009f00e580130000000000000e2014c029b0067e819d00e7e00913025c009301274419d002
7e009d21e76409f00a7c829000245009d0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0fa0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (34042d2368d04fd03784006141791815000000000000042503c0171027cc019e036da0197025c809d3035cc0d7f027fc01df027cc095f017fc21ff0074c01ff007c401a3007d2000000000000000062041c00870027c00df0017c00570837c805f0021c004f0237c00d70033e005f0027c205320
15d008f0007c005f0035a810000000000000084046e012b407bc81a3006bc01af0078d0163006bc01e1007fe01e1207bc4163005ec0177405cc01ed005ac017f0078101100000000000008200640079001b602e900fb4506d3038662f1043c40171017b400e9807b420610078411a590b8400fd00a8411ed003888
01000000000000080052400c98b3340081) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0fc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (07c009f0016c808f14b7c00178085c125b0037c221f0035c22d70037c005f0117c009f00b5c005f0807c209f003700010000000000000e20d7c091300765809f04b5c10978022c424b11744000f083fc009f00f45005e00f7c00df0024c00dd0034d00d30035a815000000000000042093402090
0214008d00834404908124004d00654180d00350000d02304804d00334000d00004209d00004804100312004000000000000040803444a1213a600ad00294002d121a40469132a08c7d003b448ad183840465141b400ad0118480ed2008400b1023d000000000000000004205701deb067bc2dcd094b40d6b22084
09fb005dc074d1871c096700704096d00f) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0fe0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (061d01b7c165f0797c00934104c0a9f8027c009f0436b0000000000000000020424041521217048d8133404012004644d18c004001104334884903334044931134000124014c00d04134000d013028100000000000000200044039100650049d00374019110444025904545011908354019d0037
4005d0037600d101004119d04374089d0034a001000000000000080216c23450064000dd0cb74011301444495100654a11100374035d00374005d00474005104f54031d00074801d00362085000000000000042210c00f30030c00bf00afc00bb0024c017b202cc003b103fc803f043fc007f011fc0073006cc00f
7003fc007f003f08840000000000000600) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1000) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000a8042410cd0033600c12132400190033404c10035440110006400cd8a034a0c10303480090007460818007400010007a0100000000000000c2004424dd0037441d500354011d0077410d500354019f0045c09d110c7401df0c84c01110047441910045c011b1047080100000000
00000e000ec01ff007fc41d320fac010b007fc01db807cc012b804ec04eb000fc01d3100fc8131004bc0183004fc2113004fa8030000000000000e8017c12df00a6c02af0037c083f100fc0c3f1107c8c0f0c378023e0237c146f0807c003f000fc003f0007c003f0033a80500000000000008c000c00530025c0a
9f0427c001140045081b0284c081b0135c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1020) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (d30036c008116c4440e10ae7400db03c64009100e5480d500a74031b0004205300000000000004200fc00df0037c00d30035c005f0037c20db0834c20570085c0cdf00a7c00d30006c82170924c009b0187c041300c5000300000000000004061fc00ff003fc80ff083fc203f003fc00ff003fc0
0bf014fc00ff0807c00ff0004c00b3000fc02bf600fc0037400d0087000000000000002012c00df0037c00d30036c021b0037c00db0035c025301c2c20df80c3c40d104c7c0a1b0cc3c019303c3c01138145200000000000000006200c400dd0037020d50034400190037400d500354019d0005400d10047420d90
847490995067440910005411190045a003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1040) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (004d008c0027a01500000000000004e00bc00df023fe48ff003fc08bfa03d408de40378407f200bc10d7101fc08df203e808bf002f800f7001bc001f0011980200000000000000405b405cf0073c00c30471c058f0033c05c38076c4b060041c44c70542485c14003600870001c1d8b0113c0901
0000101200000000000000001b405ed007b401e10178405bd0079415e1007a40531104c401e10a4b401e1004b421210269405bd005b42921404880860000000000000a000f401cd0033400c104b54020d0033404c10836400050081403c50042400c1080748004224141389109248b010006a80700000000000000
004f610cd03f7400d1083440e4d2035c21) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1060) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (4015c516fa814c00530017c18731018d80578418c005d801fc1a7b09dfc01570098c017f049da8170000000000000c204a400cd0032400c50032405c90031400c100334a2c10830400c120b0400cd88f7400c120f3400c141a040add1073281200000000000004000c401f9007a601e12079401e
58078481f1207b401e1008c401e40878441ed00fb641a9006b411a50468401ad0079000300000000000006204cd00e50838400e5003ac20292039400f5003b440210008404e52028000ed0029c80a3002b400a42008400ad002988130000000000000e0054d01d30034d21c30035c000f0034c41d34037c0053800
4c00f70002c01cf10254009b0027c20972) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1080) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (2400810033420814022400d548202010000000000000000063404958123440910026400dd00274009100276489500244089140374009100274009900274209100274009506242018000000000000080007400914065c009141204029d10274009110224009104240049101274009741660809100
6342191006448391002220010000000000000c2043c00930067c00930026c809f0027c009300270a1970165d008b0027c009301678209b0627c289b2a25c0492002708100000000000000c0049c02170005c001f0087c201f0007c821f0007c821f0107c001f0c85c001f0405c80170087c021c4087c521d018700
1200000000000006205cc005b0016c0053) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (10a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (714011300474001100454201d2807401110007400530007002110007c001b00174801900074001b0007600110807081c0000000000000e0060c28b3422fc00b300a8c00bd0027c82bf0027c00a3102fe05b7002ce00b3002fc009b002fc00b3102ac00b7002fa8190000000000000ee067c14af0
52dc009f0521c00bf20274149f0563c00bf002b4808f002fc0093052f400ff003bc00bf0039c00bb002fb8190000000000000a4073c00170003c00130006c405d0807c805310074c0570005c041b0107c00130107c001b0007c80530017c00150004101d000000000000008043400c100216008140224008d80234
408140226008100244148105236408d052) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (10c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (001b0087c801f8887c02170886c001b0407c181f01050014000000000000040157c00970027c009f0025c049f0027c009f5027c009700278009b0825c009f0123c41970067c149b00274209b00650055000000000000042014c00930023c009340208058f0027c209f00278219341a7400970024
400930065c039b0027c019100a6401978267200500000000000004a0614009180274c09100254009d20274009180270019112264009582a7400990827044990226440d57027404950025a0180000000000000680404048181274008189204008da0234048d80234408120234088508204809188214008900234008
10023440851023a2100000000000000c20) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (10e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000004053c01ab007fc81eb20794016f007ad01ff41fd401ed2079401aa0079c01ec004b401e7087b421eb084b4a12f00581034000000000000020013400290009400e9003b6102d203a601e18139401ed103a411c80829000e8003b400e5202a410a1001b4802d0c28800400000000
00000a0453406590033400c94171403cd8032603cd8035700cd21104c5c98171400dd04b3600c506f3401c808b2402cd0072a13400000000000000001340671289dc005b049fc0b7d001441073001ee907d001ac80710199c005d211f4005100da60171015a4037f18982804000000000000042153c00130407c00
131005d021f0004c041f0004c101f2085c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1100) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0100374910d1033400c10023400c508c240bc104604010188804000180032816000000000000040800404a9003f408e950296202d0238404e1113b600251039400e1002b408ed0008428fd8028610a1420d40039030d0048000000000000060056c05810003405e701204042d00384012b0371c0
5cf0473628e106a1c00ef200ac08ef01784082b080ac2923014988150000000000000e4008c41a3007fc29d3406de012f007cc097b407fe89d30075c01fb006fc81ff007ec09ff0364c09e30048c8131004fa002000000000000064043c00974007c00dd4835c800f0035c007e0036c00df0037c00d70001c00dc0
007c00db0013c409f0806c001600159010) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1120) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0844411d0104200100000000000008020cd13810067400d13063c0e1d00374011b0035c00dd10e7887df00e4c00dd0144480d50077c031188804011d004600830000000000000c2200c08b3412fc00f3403ce013f003fe00b3003dc00ff003fc00b70027c00ff880cc40f5003fc0037024cc403f
200f08a10000000000000c0007c829700b7c00df00a7c121f3037c009f0035c00de1137c20d31425c00df0187c04df0027c009f0187c881f08270009000000000000062050c609b4037840db2035c000f0034c0091403fc12d708358009140e7600dd0164400cd0120c019100044008b0425a8340000000000000c
201a400890007000c540204020d1030500) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1140) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (040fc04d3010fc200b600dca439404fca11b000dd01da010fc143e0007c003f010fc143f007f00030000000000000e2017c029f010bc08ff412bc003f103f4081f0131c283f00abc00f7012ec04ff080f880ef022fc243f100ec0c0b0203b805000000000000080002c02970085c08d300144021
f0037408c30135c0c1f11b74001f00a7822dd2004600d7002742215200444e1f08061003000000000000000840402810093404c182234020d0033400090631620cd0231600cd20a0402c90000540d109314020100004240d210000100000000000000a8006400950095440d100f44001d8037408510037420d910f
64819d1067400dd1864400d50477481952) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1160) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (fc017f00dfc887f005fc003f203d0089000000000000080a00c02930026c02cb0017c00d340b74051300058209300d70075f0104d00d304474421d0047c011f0107c041f1037218000000000000006200e414d10034480998227400d100114011104344005180474219d0024400dd00374145d00
b74001d0237400dd0035a803000000000000040040600912026420d90003400c102034000100814181100034204d0000400c502234008d00234808d12234008d103120130000000000000c0004c41d10864401d3006740af10005c411108b0406510015c001d0044401dd00d74035d0ad740b5d00d74035d007709
030000000000000e210cc81b3407ec01db) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1180) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0a441fd007b009610153601c100484032509785097d017b405a9015f405e9045a401ad096b481ed034b4216d0278080b00000000000008000e422850023440412042601c101c160009c083409051005401090003400cd04c34000d20034000d00034000d0030200300000000000000015c4034d0
22344191027143af10c944001509144004d0467c029b02a7400cd00a5c005d00374001d1037480dd0034201f00000000000004001cc41960037c019b0014c00f74087c011b01164005f04a7c0ed31207c80df0027c409b00a7c029f00a7c02df00350007000000000000040605d11bf097fc00f7003fc00fe20358
003f000bc40b7003d4803f022ec00ff020) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (11a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01e90073401e50070401c100d0401c98071403c1887d080000000000000004084c400e1082940061003ac00e10030400650028400a7003b020e1003b400e1003ac00a10038440e10028400a100390033000000000000040040c00934074c00431024c1df30034c401b0024c00970017c20d36067
c00db0074c01132054c811300648019320752010000000000000046009c00cf202f820b7201dc04fb003dc00ff203fc0c6f003dc08df023bc00df001dc00ff002fc00df021fc407f003d280200000000000000004ad01872073c474344c2c81c301a1c014b1143ce5070361c254b8163c01cf1043c00cb0143400c
d0153c000f027010120000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (11c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000040040c119f0024c08930023c829b0024c90830464c82830166c019f0024c009f0827c009d0027c009f0027c109f0025003000000000000004004bd421f0205c201f4286e021f0007d80172087d90172687e52171007c00170007c001f0007c001f0007c001f0005001200000000
000004000c40161001ec1b73009ec0053401cc0177401cc0377001f0027900dfc005f021c40071001c4007b021dc0073401520230000000000000c2048408c100334008101b2400c10474408c500304284580b700bd90ef3000c942f0500c14030500c140b0500c100312832000000000000040000401a1a06a481
a10062641c10468401e5047840165007b4) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (11e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (a5052bc34a7052c454bf002fc009f002fc00bf802fc00bf002fc00bf002ba81900000000000008006cd001f1004c80134107c041b1104c04180914c441300045001f01045001f01074041e81074841f0107c041f0006001b00000000000000a0404009500205808105216348505224948d052241
48920334808d85204008d05234148d05234148d05234148d002102100000000000000208604009d30a44009102276109920245a4992a204a099003540a9d16244009d04274309d0427410dd04274109d1424a01800000000000008000444f970024401810125c02950026c01950026c00994065c429d20654008d0
0a74029d00a74029d10a74029d00a62003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1200) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0a6c0b9f002720050000000000000080724009160274089d08364009120214009128246049d21274829100274009d002f488bd082f401bd082f400bd0025201c0000000000000480584409100276808d80234108004234828500204028d01234108100234808500eb403ad026b643ad00ea403ad
00210016000000000000040062c001340074005d0084002112885c425111844051d20174001100074001d008f4001d00874001d00074021d000700180000000000000e4064c80b3002fc00bf056dc11b3046fc84b505ecd03bf022fc00b3042fc80bf0067c059c0167c059f01678059f0027a8190000000000000c
0067c00a3102bc40bf002fc149d052fc00) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1220) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (3072481c90030400c121f4401c51070681cd00b340041006044125004844125204a4012d0010213000000000000000200040061449b40171045e4017342dc50575149c4007d019c48a7d06df4007030144005910144005100144405f00142800000000000000040040d12130407c001300058011
30286c80130006c201701848001f0007c001b080cc40190006c00131004c001f0005001000000000000004004fc04970967c009c0425c408f0165c029f08a7c209f00674089f00e3c009f0027c019f0027c009f00e7c009f00250053000000000000040014c13930027c009f80274809341274009700644118d00a
74819341674009700a7c029d00a7c029e0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1240) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (34006d031b4056d01134006f00110015000000000000042108c0161407fc419f007cc017f017dc01bb027cc09bf0277c01fb1277c017f0277c217f225fc097c105fc017f005da842000000000000042153c804f0033c00974824c001b0025c000f0db5c009f0807c005f1037c00570007c009b00
25c009b0025c009700359014000000000000000040c81e7007bc21ab0070400fb0078c41a3407cd01e70058d017d107b881634040d018f4060d01874062d018f00790030000000000000040000410f1103b400a9007a490650020401254018682cd0018403e9003b4406100e84032500ca4032520ca4032d001800
00000000000000000440443c5a033449c9) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1260) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (07c02d30087c009d0225c000f0027c10170891c00df0087c061f0097c005f0067c411f0047c011f0047c411f00150001000000000000082062411d80067c0a9c28e4c409f0027c031b00d6401cf04a76011f89e34005c1067c031f00474011b0047c011d1015201800000000000004200a4114d0
0736008508e04000d00327020924525208d04434000d08034004d0013402cd0433420cd0033400c500312802000000000000040e7240069043f41cad02284006d853b604a9513a480ad011b4102d010b40c6d011b400e5103b482e91039400ed0039011c000000000000042056c01410033425af00101203d003ac
9d2104d043cdd02434212d00734056d007) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1280) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0a100007c405fa117c00df02b5c00d700b7c40d320b6010100000000000000a841444559033450812222600011013610012410600d5008540415031344c4d01b36404d00134104d009340041001020300000000000000080064845d84774089d0066441150033480111015400910444451110067
4805d20374005d0015400550017440511014200100000000000008820d485871067401932066c251b14274071100d45409500c140305a1d74205d00074009d00274009d00274009100322183000000000000002204e41ff282fc00bf042cc003700afc2233025c900f3080ec4033142fc007f080fc10bf082fc00b
f002fc40b3203d00810000000000000400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (12a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000e804f400c10030404094032494454831400cd1032480cd00114405d0201400cd0432600112030400c10033420c06833a0100000000000000c200f401d5007440a1b02444489902b45080c0075c01dd00545015d258540bdb11b8c0111007cca1f10234401d0203f180100000000
00000e200fc01db0078c0231010cd843b013c408150074c21ef204ec017f010ce24f3053ec013b003ec00eb113ec00930037a0030000000000000ea007c105f053b804b7202f4043f201fc100f0017c04bf0a0dc081f018fc465f031fc40ff003fc00df003fc00ff453f30210000000000000a400ec145f10b7c0e
9d00a440a150037c20116209c089109846) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (12c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (dd0034c314704a5c00c151e5401f5403e40dd1023d400f5037c500c1003ca01300000000000004000fc00d30c34c025300b4c10570034c04ef0035c005f0005c88d32185c00d30036c02574030c00cb2034c10d340310803000000000000060017c00f7003fc091f0a4de491b0037c05bf083fc0
1fe242cc10ff2025400cf003bc02b7483fc00ff4036c00df003d80050000000000000e0003c00d31034d015b2046c011f0035c001f003641a5f8945c01df18c5c00d70036c20036034c00db4037c01930037a80000000000000006000f400d500344109940864009500344005d8035460dd00756015d0047400d90
034410d10034480d10831441d10835a003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (12e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (035c011f4437a81000000000000006600bc40df0037c00ff0231c08ff043dc083f2035c04d70037e006f1237e18fb003ec00fe403f888f7843fc0c77303da80200000000000000404bc01c34030c0d030032c004f0032c0d8f82714218b0371e00411201c00c30833400854470508c34030c074b
0172103200000000000002001f405e1047a40de1407a501e1827a4092d017a40de50159481718059501e5827b489610071449e50078405e941720a060000000000000a201f400c1003041b9100024011d083640a0d0031610880001400411041409c14033403010070408c14070448091032202300000000000002
004f400d100f2c0391028049313003c500) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1300) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (401cf02732014c11770012c007f091d4036f019fc00771014c13753015c60570014c057f1817a0170000000000000c204b400c90030401c10032430d54034400dd003048dcd81716038d20b1600c100304d2c50031440cd10364004500332016000000000000040807441e90078403610078401e
10878601e5007a461ed0079402fd805b401e50178401f50179409e501784012d0279000400000000000006204f400eb0038400c30032c00c5013c400cd0038400af0039620ec0039c04e3023c400eb04b0404eb207ec00e1013988130000000000000e0057c00d10030c01d30004c00934034400570036c000d002
4e01cf0017c00f7023cd21c70135c10c30) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1320) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (34008565215148505234148105202814000000000000020063480912027484910424400d100245029100244049d00260409d04354009110274029502255029001a7460910024a81c0000000000000800074009500274039108a54109100244029100254048700240029102e44099100274029124
a45009420a742091082620010000000000000c2043c00930027c00930022c05930024c02930024c019f0a27c14970061820870021c02911020c00930027c0093002100100000000000000c004bc001f0007c02170005d021f0007c521f0007c021780074421f0107820170007c001b0806c20090807c0019000580
1200000000000006205fc405b0010d0173) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1340) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (7340013000450311008440311408440f4700044001f0006440110004d001501c78001f4086c421d01c6c00114043181c0000000000000e0063c0093082cc07bb016cc05b30564c07b3102ec80b7002cc00b7002c841b36567c00b32c6cc51bf006ce01b310e7a0190000000000000e6067c009f0
027c14bf402fc14bf0527c14bf5027800bf202fc00b3152ece09a1527c20bb8026c009f0527c00af4527a8190000000000000ac073c00130007c24532106c04130104c04130004c001f0007d005f2105c84134105c80151105c84130107c04133102b01d0000000000000080434008590234148105214948145204
148140214009500300009d8521414840d2) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1360) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (401f2004c40171003c801b0100c80130107c06130005081000000000000004005fc009f0024c109f1426d059f0027d00870024c01978e65815976824c009f0025c009f0027c008f0027c088700218013000000000000042017c009b0026c049b04e1c01930024c8397002680e8701e4c018b0026
c00933027e04910026c009f10244079b0027a805000000000000062063400910027400810235400810024404d590274809d20264209900b54009100274049520264009d102458099082520180000000000000e804b40089402240c8910a14928100206008500264008d00225008920224028104234008100224008
d24a04028900a100120000000000000c20) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1380) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000004053c01e30048d01b30060c01b3007a801ad007bc01ad007b4016d007ac21e50473c0163406ad014b224bc01e325f81011000000000000020813400e90088400e9102a400690332400e5003b4006d003a400bd002a410f5003b400e100a2500ad0043442254138880100000000
00000a0053400c10000402c10020002c10036400cd0037406cd22b3600cd21f6411c10033410c13072405c90043421c11032a0140000000000000000534005b02980007b105ec2a7b00144007fa0174027d801c4067d819c48365001740075001c4117501df400750014a014000000000000042053c00130004c00
130284c08130004c001fa007c481f00054) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (13a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (190032412850441409c502054008518374030900004000940005c00100352006000000000000040003400e1000a410ad02bb40021203b408a1003a428bd2108400fd030b408ed00394006100081442100084002110310208000000000000062057441e10248c01490178429a1093c401e3017845
d05117148ca71148c01a7203b4006b00204052b003849521213908150000000000000e000bc01f30048c095f027dc81d3207cc09db0278c096a007ae09ff805cd09df007dc01f71068d0913087cc0913207d2802000000000000066043400df1003c401f0827c203f0035c401f0037c00df0035c00cf1025c00cf0
ab7c001700259001721070001f4835a210) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (13c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (473400110034a801000000000000080007400db0c705011340e6c021b00345021f0037c0a408152d40d180c545b9100354451110c44011160c7446151036208d0000000000000c2283c00fa00ccc01d3002cc1013003cc095f803cc4037002dc0173380cc01a3283ce10330028c0003100fc1073
003f00050000000000000c0007c00df0037c009b00e5c0a7f0034c12970035c02592295ca2d70084c02df00374001a0087c021f0087c021f003700010000000000000620d3c00d34006d01df002340313403fd00534036c039f0026d20cd0aa7c00df003dc31070024c00130034c0053003da01c0000000000000c
201b400c14000407091012402010037600) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (13e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (004cc01b3004ac2136004cc00334037c01f30077401ff0074c02ff107ce00f3012fc21fb007da0030000000000000e6017c14db0207c803f00a7c003f003f8403f0335c041f0187c00ef0087c002a003fc0033050ec0837000fc0c2f013fa805000000000000084003c12df4104c12db0124c041
30034c105d13b4c1c150385400518004c9011203c40017008444013400bc061300beb001000000000000000043400cd000040c0101224140920304088581334000101144008100014000140316000d40015000900334020500b028100000000000000a0007400dd40044244920644180110344005d003441015086
400a1160446005108346011500e4403190) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1400) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (fe00ff003ccc0cf424fc20ff083d80050000000000000e00005011f08a7c019a0041c11932467d13150814403131033c80d30037c00df0034c00df0036000d11003c00df0037a8000000000000000e800c4019d0027420d10065401950a24421111224420090037400d10037400d52035400dd00
37440d10015420dd0035880300000000000006a0404088d0023400890005600810003600050030540011833400c10033400cd1030406cd0032400c10213400cd003320130000000000000c00044869d00674d49305044219500644a0111064420130037401d10877401d72075402fd2034400d100a5c21dd007708
030000000000000e200ce08bf006fc01bb) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1420) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1b485ac0068401b9106b40121026c4012103684010d037b405ed017b405ed087a681c9007c50de1007f601ed0078800700000000000008200f4138c00c04418d84c32010120814101900414010d0033600cd0033400cd0032540d90871403c98033400cd0832a00700000000000002004f4115d1
0a4400d904274208101a0501130071403dd203f480dd0033400dd0034400ff04b4406f10017400dd0834a01300000000000004000fca05f0124c109f0027e029301a7c881b0215d061f0037800df2037c80df0034c00f30934c04db0017c00df0035082b000000000000060017c002f00efc03f5200e810bf006fc
003f103fc0437003fc00ff403fc00ff303) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1440) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01ed0078401ed0079401e10079405c1405f401ed0079000100000000000006604e400a10038420e3283ac0031003942061003a40061007b400ed0038400ed003ac06f1003ad00e1001b400ed003988130000000000000e0043e00931006c00d30066c211300508001f2052c0017007fc00df0034
d01cf0035c13f30035401d30013c00df0037a01500000000000006280bc48ff023fd48cf103fc005f423dc0497113b400be203fc08df023fc40df003dc08ff0037c18fe001bc00fe003db80200000000000008004bc058f04a0c10cf0003410030211d011b21b1c1a0f0073c25cf2173c81cca272d00cb1035c0dc
b0113c48cf003010120000000000000800) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1460) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000042040c85932164d009f00678149d0067420970464c118f0067c009f0027c009e0027c20970227c00972427c009f0027081000000000000006004bc021a0007c021f0007c221f0007c0a170206c001f0007c001f1007c401f0007c001f0007c201f0007c001f0007001200000000
00000e205fc03760458d057b041cc0073449cc087500dfc047720174005f0014c005f001542053001550051001fc005f0015a81700000000000008005a48cd54070400c10432602c101f1401d11033480c10033400cd0030400cc0030400c16030600c00097400cd00332812000000000000040011401e5106c401
e9406800371007c601f5007f4012500734) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1480) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (ef082fc54bd0527c009d0827c009f0027cb49f2527c149f252fc809f0027b0190000000000000ac074d04130004800070003c001f0006c001f0004c041f01074401f1007c001f1007404170003c04170107c001f0006b01d00000000000000a0506148108254008d00206008d00324208d802201
48d05234208d00234008d00234148140234148105234008d00202010000000000000020070400d108244a88502b70029d02264409d202454a9d02274009d80274009d00274009500234049540274009d0024a0180000000000000808044059509254049d00a5c029d00644469d1266c029d00276009d20274409d0
0274409101674019100274209d00262001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (14a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0a7c809d0027a8050000000000000400604249100254009510a34009c00246889100244609110274209900274009c00245009d00324009900274009d0025a8180000000000000488484608100204009500234008d90214508100250148140236008d20234208d10224108900235068900a34008d
0023a0120000000000000c20704001100154201140074001d2006e001100044605103874001900074001d00044051105444031101974001d0807081c000000000000062064c00b3002cc00b3002fe00bc002de80b30029c90a300afc009f002fc00bf0026c1193002d027b300e7c009f0027a0190000000000000e
0067c14bd402ac14bc052dc00bf002cc94) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (14c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0173405cd13b0480d56050426d90233400cd0031400cd1030440cd00b1405d10033400cd0032a0140000000000000200534807d01d9c017401df40179209c40171601cf0071001f4005d00174805d10144005d005c40175001f4005d0014a014000000000000040043c001f0007c00130807c481
f0806c02172086e001340074a01f0007c001f0004c001f0107c00134087c001f080508140000000000000600cfc409f0127c249b0127c249f0827c109f54e7e829f0823c009b0027c009f0025c00834025c00974263c009f002580170000000000000e0014d009340a4c408700274059f06e550391246140093002
7c009f0027c009f0026c009900274009b4) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (14e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (9400e1516c40051007b400ed0079881500000000000004000bc895f0074c09e30a74c01ff027cc01762271c03d30177c01f34073c09fd1076c03f3006dc01f70273c01ff0277a802000000000000060043c001f2016c00df0027c001f2025c964f0015c02570827c00df2837c00df003750aff08
25d20df0237400df0035b8100000000000000040c78016f107bc01e7007fc01ef0878d016700584016b086fc01ef0079c01ef0078401cf8079cc1f3097fc01ef007810150000000000000220074802d0039490e5203b400a90028410e1141a49069803b480ed803b400ed0038400ed0438410e1013a400ed003880
050000000000000a2053418dd01f3426c4) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1500) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (07c031f0025c001b0015c001f0027c001f04d7c0a5f0837c00df0037c20df8037c80fb00a5c00d70037c00df00370001000000000000062073c015f00b6d00d90474c039d00a6411130055002d34037c80d34837400dd8034ca0f1083750097083ac00dd0035a01c00000000000004005b4000d0
203448110c034020d0102450110820442110027440c10033400cd0031400c500064c0090033420cc003320060000000000000400034042d022a404390018410bd022a604612139100e1812b400e1113b480ed0138400e1030b400a5033e400ed013900080000000000000460574050d2179403e3497d4212d020ac
0d81137840160037b401c1017b405cd017) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1520) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0adf05b7c2adf21b5e80e70104d02934137c00df043630010000000000000080424640911007840d80034240d0001401010110490414423404cd0933400cd04b1400c52122500410c37400c901300010000000000000020806441592014400dd1027401991066401111054400d10027400dd1037
400dd0035400d50904501910037400dd8034a801000000000000080a154111b11c04021719874931d04454411154d041b5500274c0dd00374c0dd0034400d500e4c01d52037080dd003600210000000000000c2014c8023063cc08ff117f430b3000cc0033001cc11f3a227c00ff003fc00fd003c940e2007cd00a
7403fc00f7003f00010000000000000c00) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1540) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000068043400cd9033400cd0030404cd0030400cd0013480410523414cd01104020d81004000501004a4910125400cd113320130000000000000c2007401dd1077601dd0074404dd0074c01dd0057400410207400dd84044065d0104424011404d00832020404f70037100300000000
00000e800fc01ff007fc01ff007cc09ff007ec01ff005fc0933010fc01ff004ec023f124cc09330048c03b300cdc48ff127f20830000000000000e6015c303f080fc0817020fc000f900ff0c1d009fd207f0d2fc08df053fc08dfa13ec00ff0a05c143c003f000ff003fb0050000000000000ac006d141b0404904
1f8007c109b2006c0c210014c00e100a7c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1560) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (c104d54009102a540add0024400510aa4480d50034400d10034400f00034a01b00000000000004200fc00df0037c00df0034c04df0037c00d34414c1293003cc20df00358002700a5c42d30034c809b0034d00db10350003000000000000040217c00ff003fc00ff003fd00ff103ed00ff001fc2
03f0003c40ff000dd00df200fd05fb007dc02f7003ec10f7003d0081000000000000042203c00df0037400df0034c00df0034c00df0017c01130017c00dd11d6c009f00c4c011644c4c81830001c00df003520800000000000000e200f400dd8037400dd0034400cd0035400dd0017483d14047400dd08664101d2
064442152200400d91225400dd0035a003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1580) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (004c06d30035281400000000000006600bc00ff003fc00df003fc20ff003fc00ff0019c00d78007c24ff003fc2037003fd28ff0837c00ff083dc00f7103d3a0200000000000000404bc20cf0233c00cf1030c08dd0033c00c30012c004b0020c04df0011c400f4185c88c70830c01cb0032c81cb
0834183600000000000002001b401ed007b401ed0078401ed007b401e1025f411e9004944ded0068409690068409e5027c70da1227a605c90278009f0000000000000a001f400cd0033400cd0030501cd0032480c100d2403092000400cd0000500090000600151000400892002000d81030202300000000000000
004f400dd0037400dd0034412dd8037400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (15a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1017c005f0017c0053001ec0273001ec0053029e4127101ddc037b049ec10530458c00530015a0030000000000000c204b400cd1033400cd0033600cd0033400c9001340bc11873400c148b2505c92071508c941b6701c90072400c1c8352016000000000000040003401ed007b641ed007b401e
d0079401e1005a401e100fa401e1007a401a1006d401e9007a001e10078449e10079000000000000000004204f400ed003b400ed003b400ed003b400eb001b400e14011440e10038400eb1038400e10838400eb103ec0cc110390013000000000000060053c00df0037c00df0037c00df0037c00d30012c0093101
cc40d30034c00b30824c00130004c01db0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (15c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (240085802340081802641489002008100000000000000000634009d00274009d00270009d00274009908254009100204008d042441081002041081142763091102640091042428180000000000000800074009d00274009d00274029d00274009300604008f40245009100a2c02914026c429508
a74829140244409110e420030000000000000c2043c009f0027c009f0027c059e0027c00930265c00930024c40970024c00931024c80938027c00930024c009b016500140000000000000c004bc001f0007c001f0007c001f0007c001f0007c301f0045c601f0205c001f0406c04170005c001f1007c000f000500
1600000000000006201fc005f0017c005f) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (15e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (734001d1005c001d2006c55190004400190005c853700454c51500444011a0046c01170144401110156c010d004100180000000000000e2063c009f002dc009f0024c00bf0024c00bb2028c00930564c009300a4c01930025c00930024c009300a4c159f0027a8190000000000000e6067c009f0
827c209f0027c149f0027c009b002fc14bf052fc1497152fc14bb052bc14bf252fc14bf0d2dc14970527881900000000000008407bc001f0007c001f0007c001f0007c001b4005c00130104c000f1000c04010004c00010003c00030006504134002001b0000000000000000434008d00234008d0023400cd00234
008500344009d052060089202641481402) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1600) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00130086c02031006e80134084c40130086c00132005001000000000000006005fc009f0027c009f0027c009f2027d009f1025c05970027c009f0065c019f0067c03970025c009f0026c008f002500130000000000000e0117c009f0025c009f0824c609f0824ca09b2825c039308a5c009306a6
c009104654079304a6c009300a5c009f002500450000000000000600634009d80254009d0026000890024400998025402a500ad4a0b4002a406b91128400b5006e401a1206b440bd102528180000000000000e804b4008d90216008d10204048d0020400898021510a10d29410a0002a51ca10529414b1042a4b0a
14029414ad052920120000000000000c20) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1620) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000040d3c01ef007be41ef087bc01af007bc01e3006ac017b407ec01f9405cd0171407c50173085ed0073407ec01e308480010000000000000000013400ed003b400ed003b400e5003b400e1405f48069009a6906d00b9402e90098402e50438423e100bb400610078000000000000
00000020d3400cd0033400cd0033403cd0033400c12432000490076400dd0070401c90870401c10036401c10072000c1003220100000000000000200134005d00174005d101740877001740043045fc80710014441550015400590014400410054c005100154205100142000000000000000040053c001f0007c00
1f0007c081f0007c00130004c02330004d) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1640) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (c500314825d01834000d02c54010d008640e1500024001900674005100032002000000000000040003400e9403b400ed903840025003b400e5003940d7d002b400ad00094102d022940031058b400290029404e50809004c000000000000062157400e10039c05ed0239400bd003b40de1037944
57d000b4882d0029400bd2c0bc40a502684289b042ac0541317900150000000000000e000b401f3007bc09ff027cc013f007fc01d30074c217f086fc01bf006cc01bf006ec01b3226dc01b3006dc49d70a75a102000000000000046043c80df0037c00df0037c60370037c00df0027c00570015c00510016400560
0144005b0017c005f00359005f4005b814) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1660) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (4044009d0034200100000000000000020f400dd0037c00dd003744b1d0037400d914c44429108174005b00144005b0816c005500144005140954001d00042883000000000000042202c00ff003fc00ff003dc003f003dc00ff025ce18b7403fc00f3041fc2063003cc0073001cc4073001cc489f
000d00a9000000000000040007c00d70035c00df0037c823f2037c00da0087c8a9f0213c005f0037c40df0417840df0035c08df0896c001f00350001000000000000042053c00db4037c00df0034c005f0037c00d74035c009f0077c40df08b5400df0075c21d30033c40db0215c0097003520380000000000000c
201b400c90031400cd00316000d0033400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1680) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0004c0123000fc012f0004c04170077c01ff0077c01b38046c01bf001c4012f0076c01f34077a0030000000000000e6017c00ff003dc08df003fc003f003fc08fb023bc409f000fc003f000dc203f100fc002c0087d0036200f8003f000f88410000000000000ac002c00df0037c04df0835c401
f0035c04df0134400970027c00930005c001f0024c00170001c02190000c129d0c020001000000000000008043400cd8033404cd80334000d8033400c9003055081000340009202040089000240085012440289000152c0d01300810000000000000020007400dd0037400dd00374105d8037400dd003441091002
74009100245009d0024400951025400990) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (16a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (cc00bf001fc00ff003fc00f7003d00850000000000000e2202c430a0041c831340c44010300c78030d0044c42170037600df0037c051941454008d01d6d011f2037c00db0035280800000000000004001d403d00465418c100454019510444a11d20444001d8033400dd0037421d908654889900
544015d0037400d90035a8070000000000000488424009908057c20180004000180024000d0040148050433400c500324008900015009d00124001d0033400c90033a0130000000000000c60054049110454941105054011505044011d80444164b0137001dd0077401d100044019900746815d0077441d1187708
030000000000000c010eca9cb0044c0437) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (16c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1801565214a4092d014e431fd064840521034840ded017b401ed197a405b5124b401e504584096d027b401ed0078800f00000000000008000c4500d20c24200820c54000d04c00030110024489d1033480cd80334008189070408c09524030d0033400cd0032a00700000000000002004c460170
2e6c02db0214c019d00040441b01c4e029d0037600dd0034400d58817400914054502cd0037400dd0830201b00000000000004200cc005f0005d04170005c009f1085810170404c069fa036c80df2035cc0932007c00934014c181f0037c00df003508030000000000000600164007f002e001db001fc003f000bc
203f0807c0873003fc00ff003fc00f7000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (16e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01ed007a403f90059401b1004840131007b401ed1079000500000000000004604c400ad0038500c1401b420e1400b400211838420eb003b400ed003ac00eb000c400e10018400a1003b400ed00398813000000000000040050c40df2024e00d30007c00d30006800130011c00930077c00df0034
c01c24005c80930014d00430073c00df0037a01100000000000006000bc003f103dc40f90019c08ffa20ec883f021f80c7e023fc00ff0035c00af2007c00fb0109c807f023f020ff023db802000000000000084048d014f2763d19cb24c1c230f0200c050541424034d0173421cf0273c058125074408f0040c000
f0173c08cf007010120000000000000820) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1700) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000042040c00932124021960020c209b1624e05930064c009f0027c209f0027c00970064e00930062c119f0027c009f0027081000000000000006004a8461e0405c06070087c001f0087c081f4187c020f0007e801f0007c001f0087c001f4007c021f0807c001f0007001200000000
00000e201dd027f00dec007b09dfcd073041fc2173009dc02730017c005f00164007104dd8005302dc400730017c005f0015a817000000000000040059400cd0872480c90473425c180f7445c102f0510c90033400cd8032404c14194400c082d0508c10033400cd00332812000000000000040001411ad10ea403
e90043401e5105b601210079401c1007b4) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1720) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (bf002dc14b71527ca09f0027e00bf052fd20af082bc40bf0027c009f0027b8190000000000000ac07cc40130005d04174104c00172100400130114c041f0003c001f0007e80170004480110104e001f0007c001f0006101c00000000000000a05240081002101485852048085052040081452051
48500234008900234008100204009505204009d00224008d00200010000000000000020070414910025658958224408940034480d001244009d20274809d00276009512244009102244009d00274009d00242018000000000000080006c01812c204039511245018141a47418100a0c04970027400990027480910
1e440085002450e8d00274009d00262001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1740) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (027c009b00250005000000000000040060400950464440851225400910060400dd05344088100276009500240209906266009d04256009d1027400991025a0180000000000000080494008508204808180614808540214008d38204508584236208d08204008900265009502244008d082340089
0023a0120000000000000c60704001580044001500055001502040801c0004401510147000170004d001b0d464001f00855001d0007400114007081c000000000000068064c20bb002cc00b1052cc20a3082dc00ae242cd11b70027c009f0824c0093102cc00930968c00af002fc4093402fa8180000000000000e
0067c34af402ec94bb052fc00bb053fc80) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1760) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00b1403cd02f0400c90230410cd1035480cd2033600418093600c10230402cd0033400cd8032a8140000000000000200504017d08d85067d201c4087c001d4006b201c480772015c4057001740071421f40055001ed906d00164005d00102004000000000000042040e001f0804c32170107c001
f0005c2a130106c081f0005c001f0007c02130207c00130086d001f00070401f0005001400000000000006004fc139f1027d039f0063c409f2427c049f0827c009f0027c009f0025c009f0025c209f0025c119f0027c0097002500170000000000000e201550187a024c04920025c728700a5c059f00a440397102
7e009d0024c068b00a0c00850a20c099f0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1780) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (8400eb0102c0d2d003b400ed00398815000000000000042008c0d5f806cc0dfb027ce4163007cc01bf004fc09f7067dc01df027cc015f024dc01f3006c5094f007fc01ff007fa002000000000000062141d005d0005c00df1805c409f00168001f00254005f013fc80d78037c005f203fc00df00
07c005f1036c00dd0035b810000000000000084046c217f004ac01f7207bc01ed0078c41a31068c01ff0379c01ef007bc0161005fc01e100684216d207bc01ef0078101c0000000000000820046006d00aa600ed043a402ad0839500390040400650039600ed003b40061a01b480e5000e4002d003a400ed003880
040000000000000c005200acc04f2681c5) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (17a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (27c021f0135c181100b7c021700b7c8a1f0007c000f003fc20df0037c085f0197c00df0087d001f0037c00df003700010000000000000e00504005e04f7402d70934d215300349000f0487c1197003fc20df0036c0a5f09d5c24d30494d041d0037800df0035a81400000000000004005a4011c0
0c34030544446004980840110d81426000d0037420cd00314024c00b4401c900c25050d0033400cd00332806000000000000040c204442d000b604350238410610238400bd800b40065113b404ed003a4007d0009400f1002c6043d003b400ed00390000000000000000042046c1d6d0809428d14ab84004300284
880db10b429ad007b405cd0179c014d017) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (17c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (06df00b5c14534186c80db12845001f20b7c00df0036900000000000000000a0424080108036000180024024160014000d0000510850130404cd81b2404410311400d100024000d00b3400c980302010000000000000022004421510227408d100044415104144011d8004400d11037400dd0037
400510044400d910044011d0037400dd00342001000000000000080216c13112013407112247c050100854031d2024440150035c00dd0037400555145400c10486c054d0037440dd00360001000000000000000014c0073101fc01f3203cc103b0624c003f00acc08b3003fc00fd103dc0073000ec00fb0408c007
f203fc00ff003f08800000000000000600) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (17e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000068043400cd00234000d00014000100034240521224044d00034000504014140d8020400150015400cd0003008cd003100130000000000000c2017441dd00674019d00444541105074001d0004c001d00774015101004401d004440111105440bcd0047403dd0537000300000000
00000e800fc01ff006fc810f004cc0133004fc093f0a4cc031f004fc0137004cc013f004dc01330055c04ff004ec84ff207fb0830000000000000e0017c4c2c400fc003f050fc003f100fc102f110fc101f01b5c3cfe2237c506f1207c00eb000bd083f103fc40ff043fb0050000000000000ac004e04131207e0a
134080c021300044401f0284c0053023f4) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1800) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (d300f7401dd00b7403500117401918437401c40290410fd0107020fd0034281f00000000000004200fc00df00a4d005f2097c019f0424c01db0077c01df0607c001b0897c019300b7c02d30014c00df0087c00df10350007000000000000040617c00ff026fc00ff081ec49bf026fc40ff001f84
0bf003fc107b001f849bf224ed103b401ec00ef000fc00ff003d0081000000000000042203c00df0427c005f0015d01934067c40df00169009f0007c00170015d019f00c4402160055c00df00c7c00df003720a00000000000000e201f400dd00274009d04054401100074001d80244005d00374005524044401c0
034442d50614400dd0447400dd00352003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1820) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (047c00f30035a81000000000000006600bc00ff005fc08bf022fc087f021fc083f002fc007f023fc00f7002fc0873013bc00ff002bc80df021fc90df023d280200000000000000404bc00cf0010c010f0023c084d1010d05130067c054f0203c088b0023c084900a3c10070460d04cf0203c01cf
0170001200000000000002001b401ed0058401bd006b4096d005840521004b4052d007b401e9006b4296d017f489a5016c401fd024b401ed0178004b0000000000000a001f400cd00104000d00234105d00944840129036001d00434098900674005904a2480052060411cd0003400cd0030200300000000000000
004f400dd0024400dd00174019d81a4401) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1840) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (4054d02534094c05530157c025f0013c004f0054d0251005cc037b40dbc005702df800532015280300000000000004204b400cd0013441c10230400c10032403c10073400cd0033400cd0234400c90072400c500f3400c11073480c100352812000000000000040003401ed005b40161007c401e
18078481e1007b401ed004b401ad0078401e100fc403f9647f40de520cf401e10079000000000000000004204f400ed001b400e10038400e5803ac00f1401b400ad083b400ed0038400eb003ac00a5000b400e1001b404e1403d8013000000000000060043c00df0017c00530070c01d30074c00d30017c009f000
7c009f2034c00d30074c019b0023c00d70) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1860) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (24008100244148d002341485002000100000000000000600634009d002f400bd002f428bd002e400a10028400a5002f400f1502c4008d00274009120244009d002740091002420180000000000000800074009d00274009d10274039d00a44829100a44079100644009100244029d10264069100
244809d002740095002620010000000000000c2043c009f0027c009f0027c019f00e4c04930024c42972225c029300e4c009f0027c04934024c848f0027c0093002508100000000000000c004bc001f000fc001f0007c101f0407c101f0007c101f00074001f0087c101f0007c321f0107c001f00078001f800500
1200000000000006201fc005f0017c0553) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1880) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (73400110004c001d0005405150143c050d01545011d00044801100444011d100f400118016e0a1d00074221d294510180000000000000e0063c00930024d00bf0020c00b3002fc00bb102cca2af002cc00b300adc02bf0027c00930024c219f202fc119f0227a8190000000000000e6067c009f0
827c009f0027c549f0525c149f05274949f0025c009f0527d149f002bc40af002fd209f202b4409f0527b81900000000000008407bc001f000fc001f0007c000f0802d00134000c40170007c40532004c000f9007c00132004c041f0007c04130006001b0000000000000000434008d002b400ad002b401ad006a4
01a10068500a1003a400a10038401ad002) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (18a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (10170007c101f800fc003f008fc10370004c00130005081000000000000004015fc009f4027c009f0025c109b4025c009f0027c009f0026c20950025c009f2027c44930124c408f0167c009e00250813000000000000042117c00930022c009f0027800930027c809b00a4c009f0025d008b0027
c809f0927c139d00614009d00a7c009f182501050000000000000620634009100244009d0027000d500274009d9024404dd10254009940224009d012f600bd002f500bd00a74009d3025221c0000000000000e804b4008100224008d002341081042749089a4204208d00214009900234008d082b480ad002d400a
d00334008d082120160000000000000c20) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (18c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000004053c01ef005bc01e3407bc00730058c816ba05cd012f007a501e70049c016d004bc01e7100bc816f007ac81e3417c0010000000000000000013400ed001b400e1007d4002500a9001210468410bd003a400fd002b430ad003b600e1007d400ed002a481c10178000000000000
0000000053400cd0013400c10033403d101f0400c80070603dd113248acd00f1401dd00034000540030000d3032040c1083220100000000000000000134005d001f400410014c0575009940472005c4017d015c0017d061f4037d00174205120158005d001400051001c2000000000000000042153c001f0007c00
130004c00130004c30134084c441f0004e) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (18e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (050030500050003401010800400cd00330120500b20000d00a0400dd00332012000000000000040003400e1001f400ed00384202100284002d001a40825008f614e1100f648ed000b410e5000c404fd2028400ed00390048000000000000062157400e5021b400ed1038684250209404070830c0
06100bb400630839c08ed083b400eb403ac05690028401cd223100950000000000000e200bc01f3005fc01ff007cc04b3007cc01bf007cc0173007bc05f3027be09ff104fc01330048c09b70268d09ff007d3002000000000000046043ca0df0017c00df0036c003f000fc003b102f0203f0035c008f000fc003f0
037c00170031c009f0025c80df02753810) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1900) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (024400d12034200500000000000000220f400dd0014400dd0036c001b00474001908074021100d34031109834401d0485c001d24844009d2024400d500302883000000000000040203c00ff001cc10ff003cc02b300dfc02bf080fc0033002fc0033000fc003f117fc00ff063ec006f016cc00d3
003d00a1000000000000040007c00df0317c00df0037c407f008fc007f008fc02ba001740097000dc003f0207c00db0007c20d20627c00df00350001000000000000040053c00d30097c00cf0034c00d30004c00df0006c00d70167401934017c001f00374011500b4c001600e4c00de003d20380000000000000c
001b400c50053402cd0030440050005400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1920) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (104ec0123000cc013e000c800f3c27fc80df007fc0013000cc00f3005bc011f003fc013f007f80030000000000000e4017c00ff001bc00ff003fc003f000fc003b050fc003f200fc803b000fc403f100dc003f010dc081f002ec06df013f8841000000000000084003c00df0014c02df0036c000
30003c020f0087c02030007400514007c001f0037c80df00b6c80cf0024c06d308b60005000000000000000043400cd0010508dd00324000900034080d00034a2c100174404400374000d0003420cd00824044d0021502d500b00010000000000000000007400dd0014400dd20364000100874021d0187400d1006
7411d100374061d80374001d00364009d8) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1940) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (6c00cf20afc00ff0037c01ff003d80070000000000000e200ac11410c83c02d12144c010702c54010f0044c00d10030c40dd0037c13170044c00db4117c011f1037c019f0037880200000000000006200c40111003740a9120474019500054119d0044520d10034400d500374411540c5680d100
374819d00374245d1035a8030000000000000e80426441108034008190004009500016000d0000480c10130400cd043340c059000400c900374218d20334000d0033a0100000000000000c20044641108c54819100454411110444019d0044400d30134500df0137492112044500d300574015d007f4015d207700
010000000000000e000ec2913040cc01a3) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1960) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1b40de9806844135006840121004a441a9004a441fd007a401ed0278405690049501e1006d403e1007b401ed807880060000000000000a001f4044102800010d0002402010181400011050440dd2030400dd0031425090002400c140034010100f34010d0032a00700000000000002004f4005b0
0b440ac70460411910010c809b1026c00fd0036c00fd00b4400110053c20f10013c0151007f40bdd0034a01300000000000000200fc03530424d02df0826c069340c7c20130a24c20df0036c00df0035c00131884c00d31637c08934137c889f0035080300000000000006081fc007f011dc21ff002dc203b0006d
00bf0007c00f7403ec00df0c3fc001b201) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1980) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (05e1003b600650048401ed007b401a9017b4016d0079000300000000000006204d540610038400ad003b400ed0008460e1000b420e7003f422e1003e400ed1019400e7002b400e10133c002d003980130000000000000e0054c005a0034c00df0017c001e0005c001d0013c08d30037c00d34037
8011f2804c08df0017c00130537c00df0037a01500000000000006400bc00fc003bc08bf003fc00be001dc40ee000fc80ff0037c00ff283fc08f70017c00ff0a0fc807e2437c08bf0035ba0200000000000000404bc09430110c108f0232c00831281c00010010c00dd0130c01cf017143d494742400c3022340dc
30533c08cf123000120000000000000208) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (19a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000c2040d40934264c089b0267405930120c00970127c00930027c809f00e4c049f0164c00930127c029300a4c809f00270810000000000000080049c001f0083c501f2407c121f0387c001f0807c20170007c001f0006c021f2407c00170287c40170083c061f1007001200000000
000006205ec017b08dcd026f009f4617f009dc127b065bc00510017c00530017c027f009cc005f00dfc067940174276c0015a8170000000000000c204b418c103b0400cd22f304acd20f0444c100b3400cd0037400c10032404dd8271400d504134074900314030d0033281200000000000004000e401690078403
e5007b401ed0049441a9007b405e1007f6) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (19c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (af002ec08970527c889f0526c14bf002fd149d002fc40bf4027c00bf202798190000000000000ac070800534114c001f1007c40130104c00170107c0a130007c0a1f0004c045f0104c04010005c40130104c401e0006a01c00000000000000804050081252040095002240081652050091052348
48100234048d00204148d85224148100274208105204008d002020100000000000000200606009120245009d0027400d100244009500274009140274009d04244009d0024400911025440910024508dd0024a01800000000000008000440a8100244309100624849121a44808100274009300274009d00a44029d0
026c0091c4a34119504e44139d00262001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (19e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0254019f0027a8050000000000000620614029591274009402a70109909a64189900260009120274009400244009c85264008500374009908244109d0025a8180000000000000e80406008500234008510234808900a34008500e24108100234108100244008d20214008d08224808100214009d
002320100000000000000c20714001120074001100064201b00840801b0006c0113814740b1500045001da086c021f00074a01a00046801d0007081c0000000000000e0060c00b2402fc00b3002ec00bb012dc00b6012dc11930227c0194202cc00bf046dc119f002ec00b3002dc00bf0025a0180000000000000e
4067c14af202ac80a9002fc00bf002fc00) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1a00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0073600c50230400c14071480cd0033400c500f4403cc01f3400cd01234208900234018d0032a0140000000000000200504027b005f40279011dc0071409cd0161001c4007d001fc405d021c58271009f4805d009f61171045f4136d0014a014000000000000042050c00130387c101f0007c001
30106c42120404c801f0007c401f0004c10170087cc01f0007c031b0045c061f00050814000000000000060057d109b0023c859b4026c31970021c00970227c40874027c009f0027e058f0825c009f00e7c409f0023c049f002580150000000000000e2014c028641e74129500a340a9ac0a748297002340091002
3c00930024c049d00e5c009c0126418930) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1a20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0400fd00784082100484086d017988150000000000000e0000c0973015cc011e106cc01cf205cd0197025dd01ff007cc01df027fc01df015dc11ff0064d013b4048c09bf007fa000000000000000064041c00db0027c00180025c005b0001c00ce0026c88df0037c00df0017c00931027c00df00
27c20df0037c201f0835b810000000000000004056d01ff105bc012f106bc21670058c01e10079d05ef007b403ef0058441ff107bc4def006b401ab0063c01ef00781015000000000000020016402ec103340229002b41065001e430e10431404cd8039404ed0098402a50473400ed040b400a1002b4006d203880
050000000000000a0052443cc0033400cd) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1a40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (07ea2df02928001f0027c12570005c509f0007c00df0837c40df0007c029e3215c00df0037c02d700b7c13df00370001000000000000062054c00d320555911d20a6403dd82d6504970047420ff203cd20ff0027c059d0097040fd2450410410015d001f0035a8150000000000000c2011410950
181480051ca04810d0842423810040400cd0030000cd0003606058002000cd14a04070100004200d08332804000000000000042000408f1821d4042d822a4906d801a604a5001a404ed0038604ed010b440ad919b400ed8028400310009680ed02390000000000000000060045405352a5c4272f0368c8b2f05095
0da5054ac05ed0b78425ed005300d2f015) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1a60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (04df10078481f0387c00f79114c205b2014d00df0436b0000000000000000088404100804034100104274100d00006108d3103010cd0133426cd14034100d0003400c504104024100104001d21302010000000000000020004403d104474001501274205d04564489d0047400dd0837440d520c7
4439d0087400d50044411d90474410dd0034a0010000000000000802044019b00c7c0b1308634401d20444008d09c7600dd0037400dd00c74011d2005c40d100d4483d100f44030d103620810000000000000c2200c00b3101fc0137006fc423d001ec00bf000fc00ff803fc00df000fc203f015dc00f1001cc00b
b0028c09ff003f08800000000000000c00) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1a80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000e8040400c10033400c10032400cd0033480cd8831404cd20334000d0032400cd00034004d0102484418107400c50033a0100000000000000c2004401d10037421d10837401df0077401dd0054461dd00774015c00fc400cd0044405dd2074421d10c77421dd0077080100000000
00000e000cd01f3407fc01f3007bc01ff007fc01ff807cc09ff007ec012f047ec01ff004dc093f224cd0913404ec01df007fa0030000000000000e2017c149f1005c80271027c003f900fc00af0203c00cf00b7806ff0507c043f2305e00fb001fc046f0217c002f103798050000000000000a8000c06930107c04
178127c801f8816cc49d0007400dd0037c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1aa0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (d500d7480dd00340809100fc400dd00274801c00074001d0007403dd0034a01300000000000004200fc00d30037c00d30237c00df0037c00db08a7c00df0035c00170036410df0007c00db0037c00d70037c04df0035080300000000000006001fc00ff403fc00ff003fc00fb003fe00ff002ed0
0fd003fcc0ff0c36400ff002cc007f000dc207f000b800ff003d80070000000000000e2008c00d24037c80d30037c00dd0037c00dd00a5c00cf1036c015f0036c00df04c74009f0036c00830036c00df0037a80200000000000006200c400d10033400d10037400d50037400dd0115400dc00374019d0835440cd0
0676008d0036400914037400dd0035a803) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ac0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (034c00df0037a01500000000000006600bc00fb423fc00ff003fc00ff023ec08d70033c08ff083fc08df003dc08ff002fea8bf023fca8bf803fc20df2035b80200000000000000404bc20c70037c00c30033e40cf0033c40c704b3c00cf0231c00830432c08cf0023c084b0003c05470803c0dcf
0030101200000000000002001b401e5007b401e5007b401ed007b001e5005f401ed0078401710078409ed004b609ed007b409ed007b41ded007880060000000000000a001f400c50033400c10077400cd0033400c501b3400cc0031418014072400cd0003600091803400050003401cd0032a00700000000000002
004f400c102b7400d50077400dd0037400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ae0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0017c005f0017e205304dcc005f0017c057f00159005f205cc02530195c425700d4c004f0015a8170000000000000c204b400c11037400cd0033400cd0033400c904f0400d50031402c50032400c80332406010800400110000540cd8033281200000000000004000f401e1007b401ed007b401e
d007b401e1886c401ed007b401ed0179401ed0068401e10079401e500f4481ed0079000300000000000006204f400e1003b400ed003b400ed003bc00eb0038400e70038400e705bac00f9002ac00710008400610008400ed103988130000000000000e0057c20d30037c00df0037c00df0037c00d31074d00df003
6c01cf00b5c00df0024c01934074c00970) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1b00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (3420ad2029440a508294008d002020100000000000000200634009101274009d00674009d00274409d00244209d0027430d100265048d0027400b9002c000b100284109d0024a0180000000000000800074009541e74809d04a74009d00274009d02e4400990025c039101a44019d00274009d20
254209500254099d202620010000000000000c2043c00934067c009f0027c009f0027c809f0024c409f0027c02930226c019f00274409f3024c00930024c009f002708100000000000000c004bc001f0087c001f0087c001f0005e001f0006c801f0006806150083d001e0007c003f040f0103f040fc001f000700
1200000000000006205fc00534017c005f) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1b20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (734001100474001d08474001d0007c001d00044450d00074001b00044810d00044051b0144c251300474001d0007081c0000000000000e2063c00b3002fc009f002fc009f0027c009b0028c009b0827c00b3046ac00bb0024c00930024c009300a7c00bf0027a0180000000000000e6067c009f0
523c809f0527c009f0026c009f003bc148f2025c00bd4027c149f002fc149d05278148f0d27c208c3027b8190000000000000ac073c00130007c001f0007c001f0007c401f0004c001f0007c00130106c001f0007c003f0000400130804c401f0006b01c0000000000000080434008100234008d00234008d00230
008d00305008900214008105204008d082) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1b40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (02131006c001f0004c00130007c00130007c001f00050814000000000000060057c009f4027c009f0027c009f0025e209d00a7d009e0027c019f04258009f0025d099f0025c099f4027c009f002580150000000000000e0017c00934027c809f0027c009f00278409b3064c008b00278069b0024
c009b00e6c019b1024c019b0027c009f0027a8050000000000000600634009100234c09d00270009d00274009d00244009d00274089900245008d25264008900224008100234009d0025a8180000000000000e80434008105234008d85234008d00234808d00204108d80234008900214148900224108984205d08
900234008d0023a0100000000000000c20) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1b60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000004057c01e3407fc01ef006bc01ef007b801e3907ac05ef0079e01e3106ae81ef0878c11fb00ffc01e300ffc01ef00781015000000000000020017400e1041b400ec081b400ed103b400e5006a400ed083b400e50019400ed0038400e9013b4a0e1013b420ed0038820500000000
00000a2053400c14012400cd0053440cd0033400c18072500cd003300ac10072400cd0030500c94033400c14033403cd1032a01400000000000002005340051001f4005d241f4005d001740055065c4007d00170887501d94007d001440051001740071001741b7d0014a014000000000000040053c00130107000
1f2007c001f0007c00130004c001f0005c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1b80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (c90071400dd2033403091021400d900b3602c900b440add00b74000d00332804000000000000040003400e1002b404ed002b600ed203b480e10138400ed103b600e10029400e1003f400ed0039408ed023b428ad01390000000000000000062057400e1020b405ed821b400ed1039c01eb057940
ded023b4102b0009408fb023b49ce92078688ed043b40bed017988150000000000000e0003c01f3004fc89df005fc09ff327fc01f30258c41db027fe29f3007dc01f3007ec09ff00f540bff00ffc01ff227fa200000000000000066043c00df05b7c00df0027c00df0037c00df0035c1edf0037c00df0037c00df0
037c0ed721b7c0adf21b7c205f0035b810) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ba0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0374845d0034a001000000000000080207400d122f3480df0003400dd0037000dd0035400d90037401550034404190036400d50834480d588374031d003620810000000000000c2203c00f3001fc00f3000fc00ff003d480ff041cc00ff003fc00730177c08bf003fc00f3083cc20f3083fc41ff
003f08800000000000000c0007c00df4097c00df0097c00df0037e80df00a7c00df00374069f00b3c025f1077c84dd1137c10df0137c409f10370001000000000000062057c00d30017c00df0017c00df0037e20d308b4c00fb0037c01930035c00d30237c03ff21fd440ff10ffc00df0035a8150000000000000c
2013400c10023480cd0033400cd0031400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1bc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (084fc011b050ec5417087f801ff007fc03d3407ec0113004ac09f35060481b3003dc01f700ffa0030000000000000e6017c00ff403bc02ff001fc00ff003fc20df0037c02ff003fc803f003fc003f003ac00fe223fc00ff003f0001f2237b8050000000000000ac003c00d3003fc00d30007c00d
f0035c20df2414c04ed0037c00570037c009f0037c00f3013cc0ae3003fc1c1f0036b000000000000000008043400c10003404cd8013400cd0033410cd0121000c90033400051010400491033600c50030540c508334040d00302010000000000000020007420d10087400d10097400dd0037400dd0444400dd003
7411950096500dd0037440d00034400d90) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1be0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (fc00ff002dc00fb1433c083f082d800d0000000000000e0210c010102278021300c0c400f0006c08030037c00df0037c20d30032c241300c2c00d000e6c09d30035c00570047a80000000000000004001d4411520174001504445001d00b5490910037480dd0037400d10034404d10204400d510
e6420c5003451081053588030000000000000400404001104034000500046001d0002400010033400cd0033404c10036610010006404016432410c12231504c50133a8130000000000000c400549495813f4411500444811d08c4403110077401dd0077400d11074c04111044480df0124400c1043441491013700
030000000000000e020cc0123002fc0113) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1c00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (19401e9017a4052d10484012100484056d047b405e90078401e8017b40529014a429ed037d569e1007a4016d0348800f00000000000000000c4830519774460d00c14000100015000d0073400cd0030520cd0031400194003401d51415405c14030402cd0072a00700000000000002004d4a2db0
1764001d0644402110034413dc8073400d90034420dd0037400d122a740adb0185441d1007c4191d0280a01b00000000000004200cd0c570827c0a1f0087c07134686c065f0037c00df0034c00df0037410131007c281300b4c00d30234c025f00050803000000000000062017e00ff0027c053b600ec443f023ec
01db043fc20ff003fc00ff003fc013f404) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1c20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01e1007b401a9006e401355848401f5037840171004d000100000000000004404fc80eb0428400a1002a40021003b040ed003b400ed003b400e10038c8061102ac00e14038400e1413c4002100098813000000000000060050c001141a49008b00230401b0037c00970037c00df0037c00d34037
c20130060c00d70014c00d76034c00830817a01500000000000006200bc247f021fc007f090d4402f203bc00ff003fc00fb003fc00df003fc00d7000fc00fb003fc28df023d900bf003da802000000000000006058c41474153c010f0141c0f030933c45cd0a73c01cf0030c01df0073c090a0143c00070041c18c
30070c00df047000120000000000000028) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1c40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000042041c08970664c089b0264c09930123c219b08a7c009f0027c009b3064c019f01644029b0024c409b0020c009300a7081000000000000004204b8021fc807c86170286c021f0007c021f0007c001f0007c001f1006c12174207c021f0007d081f0087c001f4007001200000000
000004001fc0271405cc027b00db4056b031f4197f0017c005f0017400510017c106b00dec4077021c441474014c1373065da81700000000000004004b426c802b4480c981b2413c100b3602cd8833600cd0033400c10031403c929b2400d10094401c100305041100832812000000000000040003481610070401
a9006b44129007b081ed007b401ed007b4) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1c60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (be002fc009f0026c1497802bc14bf103ec14ab052fc14af2525c54bf052bb8190000000000000ae079c001f1114d001b0004d005301074041b1007c001f0007400134005c001f0015c001b10005001b0106c80130006b01d00000000000000a0d070081252048081002040091452341481402740
08c00214008140246009d002160081302048181052240081002020100000000000000200714009d0024400d980244209104274289900274009d00274009102254009d0035400992064480994026410912820a018000000000000000004c058180e44048124e4c409100e76049100234409d0027c009101e054e9d0
0245529108246009101a45229540262001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1c80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (024c0a830627a8050000000000000400614019508204049930374889101246019d00254009d0027400910027401910827401915d2c408a1002c510b1402588180000000000000400484009100b04409100234408120224018d00234008d0023400810821480810023400818d29484a141a8410b1
0827a0120000000000000c40614001500144001b10074001100144001d0007c001f200741511000760051880740011004c4010100c0401110547081c0000000000000e0070c00f3002c840b1002fc80b2002ec00bf002fc009f8027c0093002dc20b3002fc40b30025c089300e4c0093002fa0190000000000000e
20f5c14ef052fc80bf002dc80ff402bc80) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ca0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (90f3481cd00b0503cd0073400cd8033420cd00b040fcd0033600c90034500c90034600cd0472a014000000000000000042c0261021f4127d009b4027d22dc4036d111f4005d00174005d00194227d105b4427700144805520145005d00d0a014000000000000042040c02132007c101f1607c2e1
f0082c101f0007c601f0007c001f0406c021d0087c021b088cc003b000cc003f0005081400000000000004204fc109f20e7c019f0167c019f6025c009f0027c00970027c009f0027c009f1067c109f0067c009f0027c009f10258017000000000000040014c029340e4500830067c03912026c009f00274009d802
740093c025e00914267c069340e5501930) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1cc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (04006b013b405eb013052ce100318815000000000000040418c84730078c012f024fc09ff207c801ff006fc01ff007fc01ff0277c0dff0264d016b00fdc4df3007dd09f1005fa002000000000000060043c001f2037c001c00074401f2035d20df0007c00df0037c00df0037c005f2807c001f01
a3c805f4815c005f0005b810000000000000086040d01734073c012b004bc21ef2078501cf006bc01ef007bc01ef0078d017f004bc81eb0068c016b4058c017f0078101500000000000008200240261283b4002d000b480ad00b8410ed000b400ed003b000ed0038401ed009b400e5003c420e5003a600ed041880
05000000000000080040441c12833400c9) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ce0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (16c085f0027c001f0207c069f0123c8c9f0007c00df0037c00df8035e001f8085c00194297c009f0026c889f005700090000000000000e0050c01530074c411f00474039f00f4442df0007400dd0037cc0ff0037c001f00c6c07160095c00930025c039342b5a814000000000000040008401010
2460010d00034210d08406030d1001400cd0033400cd00114080d01420820d08a3409490015444510023280600000000000004000040271002c4003d800b440ad0428400ad002b400ed003b400ed201b4862d030a4007500294406130194206100190008000000000000044054401514212c902d0003418ad02184
086d1003c00cd023b401ed0171c016d244) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1d00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0adf0006ca81f0184c40170003c04134206c000b0002b00100000000000000a8424040142404030910024000900034030d0a02408cd0033424cd03324041d008140015801762489082040081002020100000000000000a00064831100344011d0047403190037404dd0047400dd0037440dd2836
4011d00c4401150017400910126404990000a0010000000000000802144030520044800900474031103464001d04c7440dd0037400dd00254470d00454870141034001100044401100462001000000000000042210c0073021cc203f000fc00b3005fc005f000fc00ff003fc00ff00acc003f000cc5031140fc053
30046c013b00bf08090000000000000620) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1d20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000040040410810400600010033400cd0033400cd0a30400dd0000500dd0033420c520b3424090832400cd20204080d0033a0100000000000000c6404444830104404010037401dd0077401dd007c401dd0074403ed0077001d100bc4011102e44091d02444421d0077000100000000
00000e000cc01b3004cc0933407fc01ff007ec01df0174c017f002ec11ff007fc01f3407cc0833001cc24ff003ec00df0077a0030000000000000e2015c001f000fc003b140fe0437080ec003f210fc04ff083fc08df030dc4c1f130fc003b040fc0817410fc003f042fb805000000000000006002d1c131084d02
1f0007c2a1b4007c021f0007c00df0037c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1d40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (dd02bf40edb00f4413fd0037400d104bc400db80d050b8104d4500dd0034a01300000000000004200cc041f0164c05970037800df2037c00df0037c20d301b6c10df0036c00d30030c025742a4c22530124c021f00350803000000000000040217c0137026fc09bf003fc00ff003ec00ff003fc0
8ff0035c00ff103fc00fb0434c03e704fdc009f014fd051f003d8805000000000000042210d08134064d01930037c00df0036c00df0034c07cf00e4c20df0037c20d72037cc31b4446c095f24b6c04df0037a00000000000000006001c400990004400110037400dd0037440dd0034500dd0074480cd0036400d50
0374409900064001d1014500dd00358807) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1d60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (011c00df0037a01400000000000006200bc01ff021dc007b003fc00ff003fc00ff023fe08ff883fc02ff003fc00ff10bfc00fe008fc887f023fe08ff883d3802000000000000084048c08cf0012c01470037c00cf0033c2dcf2073c05c304b2c00cf0033c00c30030c00d50070c08830201c010f
93701812000000000000082018001ed005a40565007b401ed007b401ed007b405e90278401fd007b401e100784096900604196142607012d0178000600000000000008000c502dd1096502550077400cd0832480cd0233400c10072402cd0033400c1083040001009040181101140edd0030200300000000000000
004c4041d00e4403910137400dd0037400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1d80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00178005f0017c005f401fc0077041cc005f0017c00530016c06730294d03534295c005f001520170000000000000c804b400410030400c10031400cd0033400c500334308104f3400cd0033400c90034403d100604060102404901d00332836000000000000040003401610078401e5007b401e
d007b401ed037b401e50072400cd007b601e18078400e910d0021e10079401ed0079000000000000000004604f400610038400e10039c00ed003b400e30333400e1003b400ed003b400eb0138500e30039000c100284803d003980330000000000000c0053c00530074c00d70037c00df0037c20d320b7c00d7003
4c0adf0037c00d31236c41930084cc0132) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1da0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0414818538414a10528514ad00202010000000000000020073400bd002c4008144234009d00274009100274209100245009d0027400910124400d5802c406f1012e4009d0024a0180000000000000800074029d80e45039100a74009d00274009b42678019100244009d00274009184e40809140
a45039140a44199d102620010000000000000420434029f0164c09930227c009f0027800930063c04930020c009f0027c00930024c00920164c01930026c819f0025081000000000000006004bc103f0407c101f4007c001f0007c001b0007c801f0004c000f0007c001f0007c241f400bc082f008bd083f000508
120000000000000e201fc02535094d8257) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1dc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (73401171446c05014145c001d000740011008f400510285c020d0007400130044407110004500110004d011d000500180000000000000e0063c08bf102cc00b3022fc009f0027c00934067c00d70067c019f0027c0093816cc0393016cc05b3016ec03bf0027a01c0000000000000e2067c149f0
527c149f4527c009f0027c00970025c00bf402dc009f0027c009e0523c14bf0037c809f0027d149e0027b81d00000000000008407bc003d0000c80030003c001f0807c80130107c00130104c041f0007c0011410444407010cc04132116c041f0006b81c000000000000002053401ad0068401a100234008d00234
008905234008105224148d002340081052) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1de0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (003f0007c001b2006c02134086c80132005c0c1f0005081400000000000006004fc00971027c00970025c009f0027c009e0427c019f00614009f0027c00970423d008f0121c048f0427d648f002508170000000000000e2017c009f0026d009b0027c009f0027800930027c499706a7c409f0027
c009b0026c1b934066c879301a0c019f002520050000000000000400634009500264008900214009d002740091002f400f1002d400fd0027400910024400910026400914124502dd0025281800000000000004004b4008d00324108900234008d00234008100af400a5002b402a500234008985a26068100a24228
100a05028d182120120000000000000c60) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1e00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000004040d013f0058d0163006dc01ef007bc01e10058c016f0048c012f007bc01e3003cd0de30068c21c34079c01cf0078181400000000000000200040325000b410a100bb400ed003b400e1003c401fd0038401fd003b400e10078404c10030500e14030500ed0038800400000000
00000404504058d0030401c14031400cd0033420c120004000d04804000d0033400c140f0400c15020540415050401cd0032a01000000000000002001040077001d40271005f4005d00174005140104005d00145005d00174005104dc40051429c41071419c5027d00142010000000000000042040c001f0044824
130047c001f0007c0013000cd023f008cc) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1e20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (c908034128d0850400cd0033400cd0802400c900c050bc140f050acd003128020000000000000400034006d001840065000b400ed003b400e100334006500284002d003b400ed0038408f10008404c10030404cd00390000000000000000046057400ed0028402c12019c00ed003b480eb021b40
0cb0218408ed003b400e7003ac10eb0510409e1043840ded0039001500000000000004040bc01ff007cc01f7005fc01ff007fc01fb006fc0133006cc013f007fc01fe007cc41e3106ce0953407cc09df007da006000000000000042143c001700158209f0027c00df0037c00df8023c008f8037d00df0037c00d70
005e08df4027e40df0037c00df0035b810) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1e40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0b4001dd0036a00100000000000000021f4121d10045001101a7c00dd0037400d500274001d00254021d0037000d50085400d144e4401d140744039d0036208100000000000004221340937001cc047300afc00ff083fc00f3001bc00ff0214c00df003fc00f300bcc00f3002cc00a3013cc00ff
003f0880000000000000040007000bf002fc02bf0025c00df0037c00df0037c0a5b0127d220f0037c00d700b3c00df04b3c04df04b3d12cf00370805000000000000042053c2cdf0034d00d70027c00df0037c00d31007c029701d4c00df0037c00df0034c49f30074c02132074c00df0035a01400000000000004
001b4834d0000400011017400cd0033400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1e60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0009c087f004cc013710cdc81fb807fc843b0186c14310040c00f3006ec003f007cc2133004f80030000000000000e2016c807f000fc143f103fc00ff003fc44ff050fc043f000fc003f003fc00f7000fc40ff0109c00ff002fc0cbf013fb8250000000000000a4003c00570014c02430023400d
f0037c08d300b7c4adf1034400df0037c00db0004c00f30206c04931034c0cdf0234180000000000000000a043400cd0060400810811400cd0033400c580134004d20014000d2033400cd0801400c14012510c140305040d003020300000000000000a8007400d50074400c10007400dd0037400d100264009d003
4408d90037400d90084400c14216401510) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1e80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (fc40ef026dc0027003fd00f7417d80050000000000000e0201c0008003750f13c045e23d70474c01c704f5c00d900378631b0446c03170844c33930466c051f0034c011b01f3a80000000000000004000d402190004600510045518dd28144005d0037400dd0036001150047401150044401d108
374819500344145908058003000000000000048041400594033400c12003400458830501c50135490c90032424090082410052800400c150244800d2030400590007a0100000000000000c20054a0014006e80110045404dd1074450d30036004dd0074418112184406110045421d1102540117003440111004718
0100000000000006200cc0133201ce003b) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ea0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1a40124244a681218249001ad0078409ad007b401ed0078401610158401650148429e9035b401e9007b403a1006e080600000000000008008c00105801341b4100035000501f1400cd0033400c100306000500046021d8882410c501214020d0033600810002200700000000000002204ec21114
046801d14004402dd00f4484dd0037400dc003448a9512844229503a1c45db20334029902f7480810034a01300000000000004000cc025318b5c00d70007c06570034c009f0037c40db0037d021f0086c041b0027c00d740f5c0c9f0037c01d300b50803000000000000060817c09370083c802f280bd01cf022fc
09f300cac00ff803de40030004c001b400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ec0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01e50c5b40165107d4c165307c401c9207e4916d0449000400000000000004607c4003500214807b00184008d0038400fd003b440e9003bc006d203b600e12008480e10018400e100385002d00199813000000000000040040c00131034c80524000ca19f0014c005f2037c80df2076c005d0017
c001b8005c01ed0036d00d300344009f0037a01000000000000006080bc08bb003fc007f001ec00ff003ec08fe003fc00ff003ec0077023dc687f023d420ff911f604fb023fc00fe0029a8020000000000000840d8c10c720b1c00530083c00070621508df0003400cb0032a0b078140c094f0162c00470125c090
f0433c00c3003210160000000000000820) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ee0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000042041c00972024c00930467c089f04a4c089f0027c009f0024c029200234049b1527c01930066c15932024d039f0425081000000000000006004bc001f2487c000f0005c001e0085c0c1d0007c00170007c041f0087c00124287c021f0887c28170005c061f0005801200000000
00000e201cd0073009cc437b0058d2a7d04d6c035f029760057001640277021fc0077005dc0d7f015ec017b4016c007f00dfa817000000000000040048409d5003560fc902b0400cd00405030d0042400c9003140bdd0033412c58870403410854420c900364024d00d32012000000000000040210501e10078401
f9004c401ad007a401ed00fb401e5007a4) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1f00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (9f0527c149f0023c14b9252fc34bf002bc80bf0529c40bf052bc00af082da8190000000000000ac075cc0170106d041301078241f000d4001d0007c00570004c04170105c84130017c04130006c04130004c001f0006301d00000000000000a052580890d22454800527414cd0829600ad002b40
08d8020514854523495859023414894030414c10820600dd8020281400000000000002007140095012640891c0274809d00ad400bd022f400950024600958025400d100354189102264009100244409d0024801c000000000000080006c869b09644109502274219d00a55018d006740a9d00244059103e7400950
8a34039b20a4c408141a44008d00260001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1f20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (024c029f00e7a8050000000000000400614068d44254009d04664029d802440a9d0c274809d00274509d00a64029180274469900264829d00244189d02a5201800000000000004004a4348943214008d00224408d88204008d0433404cd00214208d00226008108234808900224408d04204008d
002100120000000000000c60714040505046821d00845031f00044001d01474211d20074001d000648011001744a1115464201d01444001d0007181c0000000000000e0066c00b3412cd18bf042ce12bf002cc00af802fe08bf0025c00bf102cc00bb502fc21b3402cc11bf002c800bf002fa0190000000000000e
0867c14bf052dc94ff002f414bf0027c14) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1f40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0073400cd0232402cd0033400cd0011403c98273400c940704014910f4640cd0033410410032a01400000000000002001142071009c0017d285c40571009c4027d0015c8277001c44071009f42173085841371509c4057d089f401610014a014000000000000042041c00170084c121f2005c820
70086cb21f1007c101f0805c42134007c1a130884c1013c604c031f0207c42130005081000000000000006004fc01970962c218f0025c00978627c009f0067e009f2027c109f2425c28870027ca1972065c008f0427d019f002580130000000000000a2016e009b00e55089d206642a9f04e4d008d0a674009d002
5c009d00244439302e74209b02645029f0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1f60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (8408a3017f404cd006b40a6d0079181500000000000004000cc01e3907cc0573106fc01bf006fc01ff006cc01bf0257e09ff087fc89fe0061c0db3887fc01ff0277c09be02752002000000000000062043c001f2037940de0027100571003c80df0035c00d70017c00570017c005f0003c009700
37d404f0817c209f0031a810000000000000084045c01674068c81ef006bc01cf207ac41ef007bc01ef1859e01fb105fc406b0048501a9007cc01ef007bc016100781011000000000000082825400a1a030400cd0438400e90078402ed003b400ed001840361a05b4016114084a1c90038400ed003b410a1007888
01000000000000080051400c5c130009cd) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1f80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (27c00d72233c22870225c00df00a5c081d0435c005f0017c081f1087c001b0007d039708b7c009f00a7c0a9f003700090000000000000e2058d00d150244839b08a0c2a5d00e4c495d00b64605b001742a1d1367c289a0464c01db003740edf0027c015f01f5a814000000000000000058400180
1304130d14624025d80414828d88a64001d00134230d00c26020000404208913774010d00074120d04f1200600000000000004002041071002861c490028600ed0028400bd042a40029011b4802d000b618215008486a9c13b600ad213b480ec08390008000000000000046054404ab013c404650a2a414ad05294
02fd0028400ac025b4054d001b60841834) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1fa0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (021f0887c82130184c209b8127c02130007c00df0036b00100000000000000a040501c500304000d80244418d0001400810030401cd00134060d00036020113005008930214230100036200d80302810000000000000020004400d524654411500246041d0447600d90074400dd00174311d0447
411110064400990077480510047608dd80348001000000000000080214480d140d44451b00644011d08444220100244001d00174031d20474231110404249b0175c011141474001d003600a5000000000000042014d03f2000dc00b200e4c203f042e40573002ec093f081f80034080fc0033000cc098b003fc09f
3002fc00ff003f08050000000000000600) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1fc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000048041400cd0030404cd0033400c142124080100b0402090031400c102334100c01004008d00434008d0103404050437a0130000000000000c2007401dd0074618fd0037401d50064501d5083440391007640bf500bf405d70077401dd2477440dd1177401d10177080300000000
000006800fc21ff207cd44ff007fc01f3001cc8433010cc006b087ad01f3017bc213f00cec013f004fc013f00cfc0937004fa0030000000000000e0817c40f9803fc403b002fc803f800e800bf802dc003f089fc021f050fc803f020fc40be12054003f420fc003f023fa8050000000000000ac004c00d74025e20
130024c000fa007c009b8824c000d1017c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1fe0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1b000440f5101f3400eb20fec00dc08174015d00244235d0007600510004a01300000000000004200fc00df0037c00cf0037c00df0004c00c30034c009f0037c00d70434c021f0027c009f0015c089f0837c809b0035080b000000000000040217c00ff003fc40ff003fc00ff0139c201f003fd0
03f003d080ff003fc02f7001fc00f8002fc01ff000fc007f00318005000000000000042203c00df0034400df0037c00d30046c00d30004c00cb2036c80d30037c021f1024c081f1017c811f0037c00970007a8200000000000000e200f400dd0034400dd0837400d50026400d50004400d10036400d50037410dd0
0776005d00374045d0037401d15005a803) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2000) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (034d01d30007a01500000000000006400bc00ff003fc00df003fc00ff008fc48fb020f428df003fc02fb803fc083f082f4003f0816d003f023f420bf000db80200000000000000404bc00cf0033c00cf0033800cd0030c080f0030c080f2033e80c14830c00dd0213c10cf0221c0ddd00034004b
0030121200000000000002001b401ed007b401ed007b001e50048409ed0070409b1427b421e1007a4212c006b401ad0059409ad007b409a1027c800f0000000000000a001f400cd0033400cd0032420cd00304000d01845004901f3600c10234400cd08124414d00204334d0003400490002a00700000000000000
004f400dd0037400dd0037400df0034500) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2020) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0017c00530114d03534014c20570015c005f0014c005f0017c005f2014d005f0214c00530015a8170000000000000c204b400cd0033400cd0033400c10020408010004402450031400cd00304001500034000d00004001d02804000140032812000000000000040003401ed007b401ed007b401e
10058401e10078401a50079401ed0078401ed0079401ed8078401ed0078401e10079000100000000000004204f400ed003b406ed003b400e10010400210030480254038500cd013850027000b400ada808400ad000840031103d8813000000000000040053c00df0037c00df0037c80db4124c00c30004c00c3207
4c08df0634c00df0037c005f2034c005f0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2040) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (b400ad0028400ad002b400a9002820100000000000000000604009d00274009d002740091003c480b900ae484980424424910864420bd002f400bd002c500bd002f440b90028a0180000000000000800045008d0027400bd00274009100244019100644018c0026c009100244409d00274009d00
244079d002740091002620010000000000000c2040c009f0027c009f0027c00930024c05930166c819f0024c01830020c009f0027c009f0024c089f2027c0093002708100000000000000c004bc001f0007c001f0007c0017040bc102f108fd103b2006c001f0007c003f004fc803f000fc003f000fc013f000f00
1200000000000006201fc005f0017c005f) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2060) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (734001d000441f1d01474001100854021118d44021d1007c42150045c011d0047400110047441130044801110157081c0000000000000e2063c009f0024c019f00a7c0093046cc11b3066cc11b7002cc01b301ecc089f0227c00b30237c02b30024c0093002788180000000000000e6067c009f0
027c149f0527c009f0027c00970527c409f1821c009f05270149f1527c009f0527c34cf0527c54974527b819000000000000084078c001f0007c041f0007c0013010cd041b0106c045f0004c04130104c002f0007c005f00044001f0007c001b0006b01c0000000000000000404008d00234148d002340081c5284
54a94528414ad0022514814520500ad082) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2080) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00030207c00130004c04130007c02130804c00130085001400000000000006205fc009f0027c009f0027c009f4023d008f4027c049f0027c009f0021c009f0027c00914027c00974025d009f412500170000000000000e0017c009f0024d009f0027c009300e4c009300e4d01972026400930024
c009f0027c009d0027c00930026c0093006520050000000000000600634009d00244009d00274009100654009112244009d00254009500254008d00274009d002340091002042081282188180000000000000e804b4008d00204008d00234008000605808141204008500224028100a00048d01234018d0123404c
005224d4810423a0120000000000000c60) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (20a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000004053c016f0079c01ff00fbc01e34070c81c14078c01870058c01a30073405e1037cc01ab837fc016b017cc11f3017c1014000000000000000013400650038400ed003b400e1003a400a900b0400210078400e1001b424e1417a401a9013b400690138408e10138800400000000
00000404534004d0031400dd0032400c102305008141b05124500f0700c14073400c10030401884033400c94030500c14032a0140000000000000200134007700144005d0017400510056c005b105c40071061c40051001f400511816c117300174007100144005100142014000000000000042053c001f0005c00
1f0007c00130004c80132000c80070004c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (20c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (cd00524420d00124008d0017403c900764008d00b74424900b6402c100b328060000000000000400034006d003b400ed003b400e10038408c1021a400ad002b400a90033400e100ba402a1003b400290038400e5003d00000000000000000622574c06d003b400ed003b400e10638410a7043841
82d0038400ef0019c08ea003ac002f063b4184b063ac18e1063988150000000000000e000bc017f007fc01ff007fc01f3007cd01bb005cc016f004fc01e3007fc33f3047cc0133047fc01f3047cc01f7047fa002000000000000046043c00570037c00df0037c00df0037c00df003fc001d0813c008f001fc06db0
037c20870837c20770537c06df04b5b810) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (20e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (037400d10036a00100000000000000020f4005d0035400d10037400db0024401db00f6c101d0015400d10097420d50836c01840037408510037400d140362001000000000000042203c007f003cc00f3403dc00f30024c89f20034c05bf001cc08e3000fc70f3003ce00b3003f8017b003fc00f3
00330880000000000000040007c005f0037c00cf0037c00df0023c04c701b1c444f0035c80d70095c80df4037c409b2137c005f0137c04df01370001000000000000042053c005f0037c00ff003fc00d340e4c03d300f6d03df0037c00db0017c51f3213ec859300ffc09db00fcc03f700fda8140000000000000c
201b4404d0033400cd0037400c10130402) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2100) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000cc013f000fc0433012cc0137092cc083b104cc013b400780037104dc80f35004c06ff0077a0030000000000000e6017c007f003fc00ff003fc00ff003fc00fb103fc003f181f800ff401fc00f7003ec00ef003fc007f003f800ff003f98250000000000000ac003c605f0034c00d30035c00d
30034c00d70034c009f0024c00d10017c00f9003840093003bc4a5b003bc00e3003e10000000000000000080434004d0031400c10033400c90030500cd80226004d1031400c18013400cc0832420450833480410033400c1003400300000000000000200074005d8034420d10037400d10234400d5a4654005d000
6400d10297400d91034408110037400d90) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2120) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (fc0017005fd00df0827c00ef003d800d0000000000000e20004018308b4c010d0486c010f0027422170075c410709165131b08c4ca18200c6c111f0005c00d210c0d00df0037a80400000000000006200d4089148c54211d00374019d0037400d52064400118016401100444528d502044010901
b4420d10064400dd0035a8030000000000000e80404008120004011d00924001d02134084500a14000506364020921004401108024800d0005440c10500402cd0032a0130000000000000c20054819120454011d00e54019d1047481110044401d10194646110404400d5480c40a110004400f10004406ec107708
030000000000000e000cc00b3000cc012f) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2140) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (18401a1284a4213c0048641ad005b48161105c401e8005f4016d0069409f508c84092942e8549e50158509ed0078800f0000000000000a001c4028100734010d08006000900034008800004000900434800d0405400450200427090042404d51000400cd0032a00300000000000002004c400d10
c304411d00b44809d0037420d1083040091041340b1d00a440ed14084401510130402f12024500fd0034a01300000000000004200cc049340b5ca81f06044411f3036cc05b0034c019b0036c001f00a4c009700804025310a4c00d34084c00df0035080b00000000000006001fc00df2037c003f003dc80bf008fc
823b001fc02ff025dc002f002fc20ff004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2160) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (616d0078401e540d24014d007f401c10078605e10079000100000000000006004f400e10038480ad201b400e1001840061001b400e1001b420ed0028400e14408500210039490e14038406f1003988130000000000000e0057c009300344000f0007840131064c21970007c00130011e201f2006
800db4084c80170037c0cd21024d02d30073a01500000000000006480bc00ff003dc083f023fc20af203fc00ff001bc0067001bc00ff023ed20eb031fe0077483f800fb003fc02ff003db802000000000000004048d00830933c200f2030c280b2003c228b0080c204b0003c1d4f0021c004720c4d100b0154c80c
721f0c00cf007010160000000000000200) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2180) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000c2040c00831024d049f2027c009e0427c009b0027c009b0064c009f0024800910026c00930024c02930426c009f002708100000000000000c004bc021f2a03c081f8a07c001f0005c001f0007c101f4007c121f1087d00170005c00170207ca20f0007c001f0007001200000000
000006205fc0053509cc897f005f40b72009ec8076001ac00710659c027f865ec087f00da4007f209fc0073001cc00534015a8170000000000000c204b449c104b0542cd007340ac14032580c15253480c18053400dd0030402d904b24b9c924f5400c100b0600d10033281200000000000004200f401a11070421
2d006b441e10062401810042401e1005f4) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (21a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (bf002fc00bf052ec14bf052ec54ab052fd94bf052bc149f052bc149d0027b8190000000000000a8074d04130104c001f0107e201f0107c041b0107c201b0105c041f2015d00174106e04132004c04130104c041f0006b01c000000000000008040414805d204009d05234018d152341481252740
18105250148d00214008505345148140204948105204148d202020100000000000000200604089100244809d00a7600dd04274109944674009902254209d80254109508664018180665009900204009d1024a0180000000000000800044049120244008d00a74809d00a74229100a74009100645469d0ae4500911
0244809100244509140245009d00262001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (21c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (ae4c009f002528050000000000000620634019121a740191002c404bd802f440b1542f400b180264029140274009012244419900244009104244009d2025a8180000000000000e80434028100a34008100e8400ad00eb481a1802f480a500a24008100274148100204848928214128144204108d
002320120000000000000c207360211008742011400c4001d10076021100874801100444001100174811113c44011105405031101405071d0005081c0000000000000e0067c44b3a12fc40b10064d009b0167c51930467c009f00ecc00b3002fc00bb036cc22b3002dd01b30466c159f002fa0180000000000000e
2067c00bf002fc00bf002fc80bf002fc00) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (21e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0063400290049401290009400290055403c100f0681c500f2701d91077400c1a034400cd0032a01400000000000002005340571281f40151081740051001440051001340051449440271421c4027b001c40071041c51071601c4005d00142014000000000000042053c00130007c0013000fc021
21004c00132085c00134085c02130004c10174184c901b1087c84130084c400f00050814000000000000060057c109f4823c409f00a3c419f0127c019f0027c04970d65c188f00e7c009f0063d00974167c008f0025c009f002500170000000000000e20174019110678009300a4c058f00e740b930027c449744a
6e01930023c009341a4d059b2165c80931) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2200) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (8000b9032440161013c440fd003988150000000000000e000bc093b006fc01bf207fc0937005fc01730048c0137027dc09df017fc0553086cca3b3027cc01c300fec03ff007fa002000000000000066043c001f1027c009f0007c20d72026c40970033c00d70007c405f0017c001b4005c065760
37c80d780b7c8adf0035b210000000000000004057c01234073c01a34043c41ab4061d018b8079c21ab0859e0073807cd01774062c81eb007bc01e30178d05cd107810140000000000000200174006100ab402a000ab4206900c940329400f400690010403e10098603adc42a410092038600c91238404ed003880
040000000000000a0053402c54071400c5) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2220) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (07c021f1027c089f0067c205f0047c011f0047c285f0057e021f0007000170023c041700d7d028f0037c00cf003700010000000000000620134041b02a7c008d1067c311700c7441174040c030602d1e321f0447c81d363e4c10930234c609341fed00fd0035a8140000000000000c205b001010
0e34068c0913420cd00b3402c10131403c100a30040c008340a1900004019900b0480010070420cd0033280600000000000004000342029002b400ad001b608a5803b400e5003c408b5083b4046d0809480610200500a14838400b12038400ed0039000000000000000006205740021062b408ad003b4086d011b4
0061000940061032f4050d815b40121016) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2240) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0e1f0104c04174184c00b308a6c501300bcc00ff023610000000000000000080434000140224409520334004d10134004148044005108374000d044041001a4a0400810080404010230400cd003000100000000000000200074821100254649d20374001d00176005100044201100374031d0044
410150464421912022523915036400dd0036a001000000000000080207400110026c81970007400dd0027400910034400d150474011d1844402110044441514194401112034400dd003620010000000000000c2007c03330228c01bf100fc90bf042fc10b3003cc10b340dfc003f140cc3277400cc00f3017ec203
30438c00ff003f08800000000000000c00) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2260) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000e804f400cd0032400110033400cd0033400cd0033402cd0033400c910776005d0003420cd10025100d00305000d0033a0100000000000000c200f401dd0874500510037401dd0077401dd0075c03dd007440bf120744411d0003001dd00044051d00744001d1077000100000000
00000e000fc01ff007cc0173007fc01ff007fc01ff007fc00ff087cc01f3006fc0177800fc41ff000cc003f007cc003f007fa0030000000000000e4017e003f002bc00b7081fc00ff203fc00ff083fc80ef402fc4c3f2007c003f1007d80bf000fd003f003fd00ff003fb0050000000000000ac007c00130024c00
9e8017c809f2037c80d30034500910837c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2280) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (dd0034440fd04f440bfd2bb748b114077400d00034400dd0034401dd0034a01300000000000004202fc00df0034c005f0037c00df0037c00df0034c00df0834ce8cf0037c285300b7c00d300b4c028f0034d0ac700350803000000000000060017c00ff003dc007f002fc00fd003fc00ff003ec0
0df043c020d7013d8003f213f800ff00d5c01ff003fc81df003d88050000000000000e2003c80df0036c12530037c80df2037c00df0037c40df0037440db2073c1347a187c00df0086c081f0034d031f0037a00000000000000006200f400dd0036400114037400dd0037400dd0035400dd0037500d910364011d0
007600dd04264025d00344081d0035a807) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (22a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (034c001f0037a01400000000000006600bc00ff003fc003f003fc00ff003fc00ff003fc20ff003fc20ff083fc007f003fc00ff023fc24dfa03fe08ff003d380200000000000000404bc00cf0030d001f0033c00cf0033800cf0030d00cf0830c88cf0233c00c30033c00c34210c00cfa030c08c7
0030181200000000000002003f401ed00784016d007b401ed007b021ed0078409ed0078581ed207b401a102fb401e102785058d0078409ed007800060000000000000a005f400cd00304004d0037400cd0033400cd0030400cd00f0400cd0033400c10203400c100004000d0030404050030200300000000000002
004f400dd00344004d0027400dd0037400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (22c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0057c005f0017c005f0014c005f0017c005f001cc426b045fc0055501cd807f0014d037f001520170000000000000c204b400cd003050fcd0223400cd0033400cd0030400cd1031420cd0090480c90073400c50371409dd0030403dd00332816000000000000040007401ed0078401fd007b401e
d007b401ed0078405cd007b40ded0079461f9007b401e50078481cd0078403cd0079000000000000000006204f400ed0038400ed002b400ed003b400ed0038602ed1039c94ed0038480a10033400eb0031400ed0838400ed003980130000000000000e0057c00df0034c01df0037c00df0837c00df0034d00df003
7c22df0034c00c34007c00d30024d005f0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (22e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (34008105204348d1020514cd002020100000000000000200634009d00274009d00274009d00274009d00244009d80244009d08264219000274009100240009d0024400dd0024a0180000000000000800074009d00274009d10274009d00274009d00254009d2266c009d00244009046e74009140
245009d00245009d002420010000000000000c2043c009f0027c009f0027c009f0027c009f0024c008e0064c009f0026c00930427c00930024e009f0024c029f002508100000000000000c004bc001f0007c001f0007c001f0007c001f0007c001f0005c000f0407d10172003c801b0002c901f0007c041f000508
1200000000000006205fc005f00144027f) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2300) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (734001d00074051101474001d00074001d000450a1d000d4021d00045000100474001b00c410b1d0004c031d000710180000000000000e0067c009f00274009b0027c009f0027c009f0024c259f2024c05970037d0097006fc00930066c079f0024c03bf0027a81c0000000000000e6067c009f0
027e14af052fc009f0027c009f0027c009f0027c009f002fd20bf052fc009f052fc14bf1027c14fe1027b81d0000000000000ac077c001f0007e001f0007c001f0007c001f0004c441f0804c041f1006c00130907c001301044241f0004c041f0006b81c0000000000000080434008d00234008d00234008d00234
008d00214148d00224148d006040091052) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2320) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (003f000cc00330007c00130004c021f0004c021f0005081400000000000006005fc009f0027c24970027c009f0027c009f0025c008f0025c408f0265d00970663c009f0021c049f0025c049f002500170000000000000e2017c009f0027c009b0023c009f0027c009f0026c009e0026c00971425
c0f9b4067c00990264c059f0024d019f002528050000000000000620634009d00274009900274009d00274009d00264009d002f400bd002c400b904274009104244408d0024400cd002500180000000000000e804b4008d00234108904274008d00234008d00224008d002a408a50029420b944a34008945a04008
d00205068d002100120000000000000c20) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2340) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000004057c01ef007bc07e3007fc01ef007bc01ef007bc01ef005bc012f0068c01630073c01e3017cc09ff0078d01cf00781814000000000000020017400ed003b404e1033b400ed003b400ed003b480ed003a400ed0038500f1003b400ed0138408ed0038410ed0038800400000000
00000a0053400cd0033400c10033400cd0033400cd0033400cd00034000d10004520142b3400c10030400cd0030413cd0032a0100000000000000200534005d00170005100174005d00174005d00174005d00164005d001442041009f4005f40144005d00144007d00142010000000000000042053c001f0007c00
130007c001f0007c001f0007c001f000fc) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2360) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (cd0033400cd0023400c50011403010087400c900b0612cd10304001d10312802000000000000040023400ed003b400ed003b400ed003b400ed083b480ed001b4002d042a414f1201b400e90038400ed0038410ad00390000000000000000062057400ed003b400ed003bc00ed003b400ed003b40
0ed00bb408ef023840861072b400e10638401ed0038400ed003900150000000000000e000bc01ff007fc01ff007fc01ff007fc01ff027fc09ff804fc013f004cc0db3027fe41f3007cc09ff007cc01ff007d2006000000000000066043c00df0037c00df4037c00df0037c00df0037e00df0827c00df0017c209f0
037c20df0237c06df0037c005f0035b810) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2380) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0364005d0036a001000000000000080007400dd0034500dd0037400dd0037400dd0834400dd0007453110844500916247400d10035400dd00344001d003620810000000000000c2027c00ff003cc00ff003fc00ff003fc00ff003cc00ec003fc03f300fcc0073002fc00f30034c00d7803cc13ff
003f08800000000000000c0007c00df2037c00df0037c00df2037c00df0037c00df0017c421f2026f10df0117cc0d70033c00df0037c029f00370805000000000000062073c00df0037c00ef013f400df0037c00df0037c20df0027c00dd0290c431340f7c00db227cd07ff0034c00df0035a0140000000000000c
201b440cd0033400cd0071400cd0033400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (23a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (408dc14b3040cd043f007cc013e007fc01ff004dc41b3004ac0123004dd013b004fc0133004fa0030000000000000e6017c00ff003fc00ff003fc00ff003fc00ff003fc00ff000fc003f000fc803f000fc00ff003fc00df103fc003f003fb8050000000000000ac007c00df0034c00df0037c00d
f0037c00df0034c00df0837c20d31034e00c34003c00d30034c04f70034c000f00361800000000000000008043400cd0030400dd0033400cd0033000cd0030580cd0013400010024400510003400c10031430cd10304000d00300010000000000000020007400dd0034400dd0037400dd0037400dd0034400dc202
7400d10014400810437600d08034400cd0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (23c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (cc00f7401dc8077043fc19bf003d80070000000000000e2208c001308c0c001100c5c019b0284c021f0034c009d0037c00df0085c08100010d001f0496802134037401974037a8020000000000000e200d4005500444081106134009904344009d20344101d0837400d90137420950024400d910
06450510007400110005a8030000000000000480404280100004201101834008900004000d0030400190033400cd00036208100004001d0006400110003400040003a0100000000000000420054031505044011188874039100c44091c00745015d9077401d90047400950064441d1000442051200340011200708
010000000000000e000c40433104c04123) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (23e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1b41129084a401310278401e10058421eda07b4016d007b401e1004f401e58068401f91069401e1244840561004880060000000000000a001f40101014040201004140681400050a0d00334000d0031400c10003713c500c04020100634008500c6400410086a00700000000000002004f403db0
006c038113f4401d102b0400dd00374094c0037400d100364011101b4405c100504804100344019102f4a01300000000000004200fc04130004c0c9540b5c08d30095c06db0037c425f0037c00d30084c00134114c90120616c00170036c019300750803000000000000060017c09ef000fc203f0067c09f74067c
084f083fc00ff003fc00fb007fc013f083) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2400) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01e90c7f40161085d4212d007b401ad1878401ed0079000300000000000004004c400e50818400210030420e10030400ed0038400ed003b400e1003b440610038400ed003b400ed2038480ed00398813000000000000060052c00431014c80130014c01930036c00870034d019f0037820d30077
400530011c201d0036c009f0034c00de1037a01500000000000006400bc007f000fc003f023fc00ef023ec08ff003fc00bf003fc00ff0038c09fb002f400f7022e800fd000fc247f000db80200000000000000404bc00430404c00020221c04c30020c024d00334108f0033c00c30031c10d71000d00030227d089
72202c0053400410120000000000000200) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2420) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000c20c1c00930064c00930026c00930026d019c0027c009f0027c009e0024c60930266c009f0024d00930124c0893822708100000000000000c004bc0a1f0887d02170187c001f0003c000f0007c101f1007c40174007c033f0007c401f0007c001f0407c001f0407001200000000
000006209ec0163015cc0769445c5515304dec0c7f1016cc27f0017c005b021fc005300554a04f00576605f01d4d425f01d5a817000000000000042048413c50170411c900b0001c14470402cd0030400cd0033400c90033600514230600cd2233400cd0070446dd10732812000000000000042002401718058401
b90078401c1007a401ec207a403ed007a4) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2440) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (bf2027c00af0027c009f0029d149b2027c008f0525c549f0525c149f0527b8190000000000000a8079c04530004d00134106c045301144045f0007c401f00078201f0006c00370006e001f0004c40134006d00014006b01c000000000000008040414814020400918d23414810d204148d002340
08d10230008d0022500ad4028400ad002a400a1106a401a1906820100000000000000200634009100344839180234009102244809d18274009d18274009d8036401b5402e404bd00ac600a1002a400b18020a018000000000000080004c009106a04039103a74029140a460a9d08274129d30274009d00244059b0
4204109d10a4c009108e44229100a60001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2460) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (826ca0970027a8050000000000000620604209d00264429980274809101a74009d00254069d8027400910527400d91027400910026420810032440810021a8180000000000000a8048400cd00225008900230808100234008d00206009d802240081002341489002304081002340081092240485
0123a0100000000000000c20704801d00044001100060001100074005d00054801d1007000110007481110007400114144400110044491010947081c0000000000000e0060c00bf002cc20a3002fc00b3002fe00bf0024c00bf0027c0093002f800b3002bc00be00adc0092022ec00b7022fa0180000000000000e
2065c00bf0d2bc00af052fc80bf002dc40) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2480) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1873400cd0070400cc0033443cda833460cd0011422c50073400c100b7640c100f0404cd01f0201400000000000002005040071209c42071109f4027d001c4027d00174007d00174805d001b4007b001b41171041f40051081c4047d01dca014000000000000042050c2013200441a130087c0c1
f0844d061f0007c001f0007c201f1085c00130107c50131407c801204068401f8005081400000000000006005fc149f0425c819704e2c009f0023c009f0027c109f0027c009f0027c10976027c009f2025c009f5025e009f102580150000000000000e2014d018f04a6c8a8b44a7c0893402740a9e0024c008f002
7c00934027c009b0027c00930027800930) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (24a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (b482a101a8400e1122f08061083d88150000000000000e0003c0132005cc0d22137f449ff007c841ff307f841ff007fc09f3025f408f3025fc09f3207cc13f7037fc05f7007fa000000000000000064043c000f0007c00170037c005f2037c009e0037c001f0037c00df0017c009b3817c40df00
17c82df0837d009f0015b810000000000000084054d01e3405cd012b407fc01ef0878c01cf007bc816f007bc01ef1059c41e7005bc81e3007fc01e3407cc01ed00781015000000000000080014400b100d84203900bb440ed00b8401ed103b410ac003b400ed001b400ed009b400e1403b420e100b8400ed003880
05000000000000080050402c10070401c9) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (24c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (07c201f3917c009f00b7c009f0024c100e1037c409f0037c80d72017c821f0007c005f00a7c08df0097c00df002700010000000000000e2057853536094c019111b7c219f0aa64109f0037c01cf0037c00db4097c02934006c10d30024c00f70033e00d70035a8150000000000000c20130a3010
0805010520834010d00425010d00336014c1033400c901d2600010003402018000500c00003400110003080400000000000004240340021001861421013b480ed002a4006d003a410ed003b420e9141b00861209e40061603c408f5091b084e50029000000000000000006005740821001848825028f410ad06184
08ed003b4086d003b400e1001b450e1130) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (24e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (40df0017c001200174801b0005c00f30007c00130006b0000000000000000080424010100074a00910004000d00004000d20324000d0033400cc00134000100036000d0001400c1600450001400020100000000000000200064801100474001100304011d04646019d28344009d0037400dd0017
401912047624d90045400c10037402910410a0010000000000000802044001101c34101b02844871d00444071d3036c001d00374c0dd00174011104d34211d2044500d10084c001108062081000000000000042200c1063001fc8533040cd00ad000ec409f003cc027f003fc00ff001fc10b3001fe11bf182cc00f
b222cc087300bf08800000000000000600) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2500) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000e8043400cd0033400cd0033400cd0033400cd0430400c14213400c11201008c10433400cd0032400dd0033400cd0033a0100000000000000c2007401dd0075c01dd0077401dd0036489fd09bc40bf540e7401130004400010133421dd0074480cd0077481dd0077080100000000
00000e000fc01ff007fc21ff007fc01ff207fc04ff053cc24f3411fc10f3003ceacf3007ec61ff007cd01df007fc01ff007fa0030000000000000e2015c003f000bc003f000fc003f000d9003f203fc003f003fc00ff001bc003f000bc403e000ac00ef000fc403f000fb0050000000000000a8002d00130007c00
138004c001f0004c001f00348009d0037c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2520) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (fd007f400fb046454e110035002912037400dd0034501dd0037000dd0034a01300000000000004200fc00df0037c00df0037c00df0034d00df0037c00d30094c20d32000d03530077c00df0034c40df0037c00df0035080300000000000006001fc00ff003fc00ff003fc00ff103f4a0df083fc0
0ef48ebc02172004c20bd003f800ff003dc00ff003fc40ff003d80070000000000000e200bc00df0037c00df0037c00df0037c00df0034d00d30197c00d26334c02530836c00df0036c40cf3037c00df0037a80200000000000006200f400dd0035400dd0037400dd0036400dd0034400d40827400190037404111
037420dd0036400dd1037600dd0035a803) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2540) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (037c00df0037a01500000000000006600bc00ff003fc00ff003fc00ff083fc00ff003fc22fb021bc00db503f6007f003fc00ff203fc00ff003fc20ff003db80200000000000000404bc00cf0033c00cf0033c00cf0230d04cf0433c08c70820c08070800c00830033c00cd0030c09cf0233c08cf
0030101200000000000002001b401ed007b401ed007b401ed0078401ed007b421ed0058481e5164940161027b401ed007841bed007b401ed007880060000000000000a001f400cd0033400cd0033400cd0030400cd0073400c500604210501f0010910037400cc0830400cd0833400cd0032a00700000000000002
004f400dd0037400dc0037400dd0034000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2560) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0017c005f0014d00532017c00534097c045300d4c07530017c005f0014c005f0017c405f0015a8170000000000000c204b400cd0033400cd0033400cd0030400c54033400c104634440140c6446190033400cd0030500dd0033400cd0033281200000000000004000f401ed007b401ed007b401e
d0078405e1037b40de100db401e100f0461e1007b601ed0078401ed007b401ed0079000300000000000006204f400ed003b400ed003b400ed0038608c50533484e10413400e1080ac00fb103b400ed0038400fd003b440ed003988130000000000000e0057c00df0037c00df0037c00df0034c0cd30137c02d3412
7c00130034c00130077c00df0034c00df0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2580) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (34008d00204008d00234008d082020100000000000000200634009d00274409d00274009d002440091002050091242c486f1442c400dd00274009d00244069d00274009d0024a0180000000000000800074009d00274009d00274009d00244009000640009100e45039002a45009d00274009d08
245039d00274009d002620010000000000000c2043c009f0027c009f0027c009f0024c00930224d00930224d01930024c009f0027c009f0024c419f0027c009f002708100000000000000c004bc001f0007c001f0807c001f0007c000f0007c000f000bc002f010fc403f0007c801f0007c021f0007c001f000700
1200000000000006205fc005f0017c005f) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (25a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (734001d00074001d00074001d00474021509c44021102945025145d44431b2045c001d20074151d00074001d0007081c0000000000000e0063c009f0027c009f0027c009f00a7c019301ecd0593006cc11b3016dc01b3002fc009f0027c00bf0026c009f0027a0180000000000000e6067c009f0
027c009f0027c009f0527c009f0527c009f00274009f4527c149f0527c009f0027c14bf0027c009f0027b8190000000000000ac073c001f0007c001f0007c001f0004d04134104c0413410cc84134104c841f0003c001f0004c001f0007c001f0006b01c0000000000000080434008d00234008d00234008d00204
14810520414810528414a14528415ad006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (25c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (20134484c080f0207c001f0004c001f0007c001f00050814000000000000060057c009f0027c009f0027c009f0027c009f2023c008f0427d008f4021d009f0025c009f0027c109f0027c009f002580150000000000000e2017c009f0027c009f0027c009f0827ca0934024c009340e0c239300a7
c0b930827c009f0027c009f0026c009f0027a8050000000000000620634009d00274009d00274009d002740095002440091022440891a1265029900216009d00274009d00274009d0025a8180000000000000e80434008d00234008d00234008d012340281032040881002040081123253281a4234008d08234048
d00224008d0023a0100000000000000c20) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (25e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000004057c01ef007bc01ef007bc01e3007c801c3007fc01ef1068c81c9007c4016d005bc01ef0078d01fd007bc01ed00781015000000000000020017400ed003b400ed003b400e9027a401e9003b400ed8008600e940384a085002b400ed0038483ed003b400ed0038800500000000
00000a0053400cd0033400cd0033400c10030400c10063600cd02d05814900b04c0cd04f3400cd0030603cd0033400cd0032a0140000000000000200534005d00174005d00174005b0016c005b01174005d001c4047b001c5007700df4005d00144827d00174205d0014a014000000000000042053c001f0007c00
1f0007c00130004c00130007c001f0004c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2600) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (c14033420c14150402c500b1449c10037400cd00304200d0033400cd00332804000000000000040003400ed003b400ed003b400e1203b4a0e1002b400e10010400c5113b40061003b400ed00385002d003b400ed00390000000000000000062057400ed003b400ed003b400e1213f404e1002f40
0e10018418e10639c08e1023f400ed0238482ed003b400ed003988150000000000000e0003c01ff007fc01ff007fc09f3907fc01f3007fc01f3204cd8173137ee01f3007fc01ff007cc01ff007fc01ff007fa000000000000000064043c00df0037c00df0037c00df0037c00df0427c20df0827800df4037c009f0
007c20df0037c00df0037c00df0035b810) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2620) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (037400dd0034a001000000000000080207400dd0037400dd0037400db0034480d12037480d00034401d14074000950007400dd00374021d0037400dd003620810000000000000c2203c00ff003fc00ff003fc00f3003cd00e300efca0f2403cc20f30034c0063001fc00ff003fc00ff003fc00ff
003f08800000000000000c0007c00df0037c00df0037c00df0037c00df0027400df00b7c04991031c109f0027c00df1037c001f0037c00df00370001000000000000062057c00df0037c00df0037c00d3003fc00d30037c00d301b0c030702f6c00d30037c00df0034d40df0037c00df0035a8150000000000000c
2013400cd0033400cd0033400c14037400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2640) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (007fc01fb083ec8cf7003cc00b3043fc04fd007ec8036000ec01fb002dc08f2032cc02f3007fa0030000000000000e6017c00ff003fc00ff003fc00ff003fc00ff002fc00fb000fc00ff082fd00ff003fc00ff003fc043f003fc00ff003fb8050000000000000ac003c00df0037c00df0037c00d
30034cc0d3403fc00d70004c00d14004c00530037c00df0037c2a0f0037c00df0036b000000000000000008043400cd0033400cd0033400c90030400c10033600c50000500810020500c50033400cd00334000d0833400cd00302010000000000000020007400dd0037400dd0037400d10034400d10023400d5050
4401511474400d108374a0dd2837408dd0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2660) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (4d10ff0077c00cf40a7c20f7003d8005000000000000042200c011300c6c094f0037c00db0037c80d74034c80901037c00d70037c031f0444c00db0065c00d30034d00db0037a8000000000000000e200c401950044402dc0037000d14037400d18034400910833400dd0034411990066400d101
20400d10024420c90035a803000000000000068840480010002680cd0033420c90033404c10930520c1453342cc5083340c0d0000400c90021500c1813040cc94033a0100000000000000c2004401d50004420dd0037401d1007740cd106bc49efb10bf452cd0074412110004c00d10024c20f103bc402e1207708
010000000000000e800cc0033000ec007f) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2680) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (18401610078401a5007b401e50078401e90070601e5027b001ed0078691a5406b401e10078499e93268501e1027880060000000000000a001d4800102d1403050033400cd0030400cd0030400850033600cd0831484158007400d90021401c92030440c10032a00700000000000002004c480d10
0e441bd101f7400df003c400fb003cc0091403ec00fd1034441910027402d10034401f10034460f14030a01300000000000004200dc00134187c00d30437c00df0034d00d32034d00c34034c00df0835c029300a7c20db0037c40d34020c00d300350803000000000000040217c00cf0023c20ff003fc00ff003bc
00df003bc00df0037c00ff003fc0017100) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (26a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0dcd0078401c4107b401e50079405e10078405e10079000000000000000004004f400612038400a1003f400e100b9400f50039488e50230404ed0039400e3003b000e0003e410c12238412f120398813000000000000040053c00130016c00920037c00d30035c08d302b4c04934335d00df0034
c01950037c00d70027c4ed30124d04d30033a01400000000000006600bc001f0225c00db4037c00df0237c08df00b5c009b0036c00df0237c009b0037c00d70035c20d60a37c80df0031b802000000000000004049c00030081c00970037c00cd0030c00cf0030c00c30033c00cd0031c04050813480cb4131440c
b3220c00c3003010120000000000000208) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (26c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000c2040c00830264c00920167c00970020d40930024c00930024c009f1025c08930024c01930820d05930024c0093002708110000000000000c004bc001f0487c00170007c001f0007c001f0807c00070001c001f0007c02174407c021f0005c001f5007c001f0007001200000000
000006201fc1073609ec037b0017c00534014c00530014c00590017c005f001450c75009fc00560055c40534114c00530011a81700000000000004204b40001003441bd98037400c10031400c500314208d0032400cd0030402c900b3420d10232480c10824400c14033281300000000000004200340121004a401
c9407b401e10170401e10170401c9017a4) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (26e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (9b2525c14bf4526c149d0827cb4bb052fc14be052fc549f0d2fc349f0027b819000000000000080078c04134100c04174017c00170104404120106c44132104c041f0007c24110100d00130104c04130100d04110006b01c0000000000000000424148105204148500234008105204148d452241
48105214148d00234148905204008145206148105204348100202010000000000000000060400d104245109580274009500244008110225209180245008d0027410910020400910024440811824400810024a018000000000000080006c009100e44009100674009100244009b20244009100244009d00274019b0
82440f9100244019140244209150262001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2700) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (224d00930027a8050000000000000620604009100304009140274009100254008900254008508204009d0026410990026400990127420991024400910025a8180000000000000e80484008103204808100234008980a04008901205048104205048d00220008100a21009940a340489052050481
4023a0120000000000000c00704001105004281104074001100854031140c548b1501444031d00064001300844051100874411140c4483110007081c0000000000000e006011493013cd08b3002bc009b0124c17930664c0993046cc199f002cc00bbc174c42b3a167c08b30464c199b002fa0180000000000000e
2067c00bf052fc14bb0527c009f0027c94) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2720) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0073400c90030400c10034420c10022400dd0833600dd0033400c14030401812030400cd0032a01400000000000002001340051005c40471045f4005100144805100145005b00544005d081740877181740271101c4805108144005d0010a014000000000000042053c00134105c04130005c001
b0004c00130804c00134004c201f0007c221f2007c20130004d00130804c001fa805081400000000000006005fc008f4027c099f0427c009f0023c00970027c019f0027c009f0025c049700e1c30970027c00970023c0087002580170000000000000e2014c09934264c12930023c009b0024c009b4024c0893402
4c009d0024503910126c40890823c009b0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2740) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (c48060023ec00bb0138408f1003988150000000000000e000bc01f3007ec01b7007dc01ff007cc01f3107cc03f340fcc03f3407bc09f3067cc01f304fcc01f3007cc03f3407ba002000000000000046043c00df0017c005f4037c00d70037c16df03b7c02dd00a5d02df00374009719b7c60df00
37c069f07b7c62df0035b010000000000000000053c01e30079c01c30079c01eb0078d05f34370c01f3106ac43ef007bc21ef1d7bc01e1107cc09c3417cc07fd00781014000000000000000013400e10438400e1003b480e1003040ce12138448e90c22400cd003b402ad083b410e10038603e10038500ed003880
04000000000000000453400c10071401d1) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2760) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (07c04d700b7c22570035c00df0037c00d70037c00cf2837c00d70037c82170037c029f0037c009f2037c00cf00370001000000000000042053407d34076c0b9f0035c00dd0034c20f3003cd00f34034900fb00374849b00bc80095407c400d30c7cd00f30035a8140000000000000c209b481c90
154401490013400cd0031400dd0030400c50030400c960334030911b4520000072400c92030420c140332806000000000000040403400e1042a4008d400b400ed0038400e14038400e10238400e9003b400280038400b50438500a10830400e1003900000000000000000620d7408e1023c49061201fe00ed00394
80e5203c498f5003c400f1003b048a14a3) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2780) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00ff0037e2013003f40013883cd00f3003cc00ff0036b000000000000000008043400c140304004d0003400cd0030400c1a032400cd0020400cd0033440010033400010030400c10030580cd00302010000000000000020007400d180345049d8065420dd0034400d54030440dd0124400cd0037
403916837421910032404810030500dd3034a00100000000000000020dc00d100844075d0077600dd0034500d10036c00dd0074400dd1837403110037407110034420d14034400dd08362081000000000000042203800f3014ec01af003fc00ff003cc00d3003cc00ff007ec00ff003f810b3003fc0033003cc80b
3003cc00ff003f08800000000000000400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (27a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000040053600cd0033400cd0033400c11130410c10133404c10530410c900224848004204108d04214048941204c48d2133a0100000000000000c6407401dd0077401dd0077401d102bc40cd525bb444d50138400e10424414410916c241c01045001100045001d0017080100000000
00000e000fc01ff007fc01ff007fc01f3023cd44f3152fcc3e3052cc10f30068d0133084cc4137084cc0933024cc093f025fa0030000000000000e4015c00ff000dc007f000fc00ff003fc00ff003fc00ff082fc00ff083fc003f003fc202f003fc00bf103fc00ff003fb8050000000000000ac003c00d34024c00
9f0007c00df0034400f3003cc00ff002ed) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (27c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (fb0034420d24036c20f10024400dd00370819d0867001dd10e74039d0074a01300000000000004200fc00df0037c00df0037c00d34037c80d30024c00d30024800d30024c009f8827c019f0067e11df1067c019f00750803000000000000060017c00ff003fc00ff003fc00ff003fc00ef00afc4
0ff102fc80e7002dc007f001e8093f0a4ec0077024fc193f001d80070000000000000e220bc00df0037c00df0037c00d34034800d31077c00d30034d00db4266c80030004c011f0045c205b0044c011f0017a80400000000000004001f600dd0037400dd0037400d10830400d50027400d50124400d92026400d14
0336a09d00254008900204408d0035a803) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (27e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (054c00534857a01500000000000006200bc00ff003fc00ff003fc00ff003fc00ff003fc28ff023fc02fb005fc20ff003fc80ff0a3fc08bf023fc08ff203db80200000000000008404bc00cf0033c00cf0033c00c30033c20c3a02080ccb0220c04c70110d008d0823c24cd02334008f0033c08cf
0030101600000000000008201b401ed007b401ed007b401e10273401e900684a1e10a6a401e5405c4996d085b4016d025b4012d005b4096d0058800600000000000008000f400cd0033400cd1033000c10033480c10034500c80034400c520144810d00034005d00134020d04934024d0012a00300000000000002
004f400dd2037400dd0037400d1003f400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2800) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0017c00530017c00530015c205f5054d005b0016c80530014d00534017c05534014d00530015a81700000000000004005b400cd0033400cd0033400c50033400d10063400dd0060400c90012400d92034400c02037401c10030400c100332812000000000000040003401ed007b401ed007b401e
1017b405e10473401ed00f8405e9005a501a10068681e1007b401e10078401e10079000300000000000004604f400ed003b400ed003b420e50cb3440e10a3b400e50430560c100185006b001840061001b40061001840061081d8813000000000000040043c00df0037c00df0037c00d301b7c08d301a5c40d3012
4c4ad34010c40130004c01530017c00530) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2820) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (b401a10068401ad0069401ad002020100000000000000200734009d00274009d0027400910020400914024400908024400814838400b1462d400b1002c400ad002c400ad0224a0180000000000000800074809d00274009d00274009b0826c409100244009b00240009180244099100e74029140
a44039d00a54029d00262001000000000000042043c009f0027c009f0027c00930024c00930024c00932020c00932024d00930067c00938024c239f0024c049f0027081000000000000006004bc001f0007c001f0007c001f0007c001f4003c80160007c0017200dc801f0087c801f0007c201f0007c001f000700
120000000000000e201fc005f0017c005f) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2840) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (734001d00074001d00074001101474071105c54010100c14011101404010140440115b1456c015b00544015d0057081c0000000000000e0063c009f0827c009f0027c00934067c01930064c029300e4c0793402cc02b3022cc00b3002cc00b3002cc00bf002fa0180000000000000e0867c009f0
027c009f0027c009f0527c149f052f4149f052fc349f05274148f0527c149f0d27c149f0527c149f0527b8190000000000000ac07bc001f0007c001f0007c00130104c04130104d00131904d0411200c400130001c00010000d001f0000c000f0006b01c00000000000000a0534008d00234008d00234008905224
14810520400890520454810028400a1002) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2860) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0013c004c00130904d02134084d02134084d02134085081400000000000006004fc009f0027c009f0027c009f0027c609f2065c009f0261c008f0027d009f0027c009f0427c009f0027c009f002500150000000000000e2017c009f0027c009f0027c00934027c80934226c80974026c00930020
c00830024d029300a4c029300a4c029f00a528050000000000000400634009d00274009d0027400910027400910023420910027420910024480910820440c900224008900204009d0025881800000000000004004b4008d00234008d00234008104a34328120a24448501a24468104204258100604008101204108
104205108d0423a0100000000000000c60) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2880) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000084047c01ef007bc01ef007bc01e301f8d03f341fcc47eb01fad03f101e8c09e3085c40179005c40173005cc0173007c1014000000000000082007400ed003b400ed003b400e90130405e1013a484e1003a484e10128400e180a8400a10428440a10028400a10068800400000000
0000080053400cd0033400cd0033000c10034440c12030420d92032400c10020601810020400c900f0480c12070480d10032a0140000000000000200534005d00170005d00174005b4014400510016c80732016c2051201c40471501c6007b801c40071011c4007100142014000000000000042043c001f0007c00
1f0007c00130004c00130004c00130004c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (28a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (c90031420c12030400c101224c0c10812440190030400d10037400dd00372806000000000000040403400ed003b400ed003b400e10838400e90031400e10838600c1002a408b1021c40061003840461001b4006d00390000000000000000042057400ed003a400ed003b400e1293c400e1043842
0f1053cc24e1002c400a1001ac00ab083c401b1003f400ad00298815000000000000042103c01ff007fc01ff007fc01f300fcc01f3007cc03f300fce01f300ecc01e30058c21f3207cc09d3407fc01ff007fa002000000000000062143c00df0037c00df0037c00df00b7d80df05b7d02df48b7c16df20a79049e0
017c001f0007c00df0027c00df0035b810) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (28c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (034400d10036a001000000000000080217400dd0037400dd0037400d10037480d10034400db0834400dd0024401c11011400d10005400d50025400d500362081000000000000042213c00ff003fc00ff003fc00f3003fc00d34038c00f3003ec00ef002cc25b3001cc03f3001cc0073001cc0073
003f0880000000000000060007c00df0036c00df0037c00df0037c00d72036800df1035c00df1065c419f086fc22df0027c409f0027c009f002700010000000000000e2057c00df0037c00df0037c00d3403cd80fb403dd00f3403cd00f350eec00d30024c60d30034c00d30037c00df0035a81400000000000004
2013400cd0033400cd0033400c10030400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (28e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (e1400850021400850021410850cc14008d34214009504214828908a34018500a34230920610000000000000000000e2017c00ff003fc20ff003fc00fe003fc00ff003fc60ff003fc00ff082fc00bf101fc00ff003fc00ff003fc00ff003fb8050000000000000ac003c00df0037c00df0037c00d
3083fc00d3003cd00f3003cc00ff082cc80f30014c00c10034c14530014c00530036100000000000000000a043400cd0033400cd0033400c14033440c18830400c90830580cd0020400d10015400c140314048500314008500200010000000000000020007400dd0037400dd0037400d10033480d10034420c1003
0400dd0824440912014400d10030400d10) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2900) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (020100804220308004200108800000000000000000000000000040001033040001000040001000040001002040441091000c02011060401050041c830100800000000c24014000000000000000000000000800020000800ce00008000200108000200108004200008820220008008200d2800040
0118a04a0011a028e04000000000000000000000000844021100844021100844021110844021110844461180884420100844c611128444621138044a11d08444e110000000000000000000000008000200008000200008000200008000200008048a00008858220008004400008028a0023800060022882ce04000
000000000000000000000850021400850c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2920) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000800020000800020021800020000800020032800c20050880c20090880c220628008e0013890c600218830e040000000000000000000000008500214008500214000500214008500214218d28214008108214008908a2c008500214128800e1400a50061400000000000000000000000000000
00330000000000000000000000000000000000100820c00110004000030000400900000800400010c04000000000000000000000000040001000040001000040001000040401002040c010910020810510414010921430010110404810d00404c14000000000000000000000000010000400010000400010000400
0108004010108c04220900804020108004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2940) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0800810100024020a29434210900514a10900424c10800000000000000000000000010000400010000400010020400010820402810c204600100804c0011002412810c204a00018604200120800800000000000000000000000840021000840021000840ce10008408e10338c2ce10908400e201
08824210b2840ce10508408e10508000e10000000000000000000020033800ce0033800ce0033800ce0033800ce00138020a0033881c200938028220038008e00138924e0071800ca00008000000000000000000000840021000840021021840021000840021031840ca10608424210208004a00938414e2003890
4a10128400e10000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2960) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00000000000000000000000000000000000000000000000000000034042c10001a581a41a03e402800c27fc181a689a09c0002640264000000000000000000f0f00000000000000000000000000000000000030a080800000100010f0a080800000100010f090c0800000300010c3c3c00000000
000000000000000000000000000000000000000000000100000000000100000900000000000100000901000000000000000800000000000000000420800000000000000000000000cc0000000400003002cc00100020c0010080006072002cc0010010cc00100024c0490820000000000000000000004000100004
0001000040021000040421003842421090) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2980) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (fffffc0000000003fffffefc0000000003fffffffc0000000003fffffffc00000000000000000000000000000003fffffffc0000000003fffffffc0000000001fffffffc0000000003fb7bfbfc0000000003fffffffc00000000000000000000000000000003fffffffc0000000003fffffffc00
00000003effffffc0000000003fffbfff80000000003fffffffc000000000000000000000000000000000000000000000000000000000000000000cc2844281000000000cc1448141000000001129416144c0000000000000000000000000000000000000000000000000000000000082808080001400150002020
2001000141502040204802e801c9000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (29a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000080002000000000000000000000000008500214008500214008500214108500214210500614008d08210238404230418424a30008500210008500214000000000000000000000000000000003fffffffc0000000003ffff7ffc0000000003ff7efffc0000000003fffffffc0000000003ffff
fffc00000000000000000000000000000003fffffffc0000000003fff7fffc0000000003ffff7ffc0000000003fffffffc0000000003fffffffc00000000000000000000000000000003fffffffc0000000003fffefffc0000000003fefffffc0000000003fffffffc0000000003fffffffc000000000000000000
00000000000003fffffffc0000000003ff) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (29c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00400010000400010000422010c4040200000202101004000208000240001000040001000040000000000000000000000000400010000400010000400010000404010130408810010000014100400034800518c00000400010000400010000000000000000000000000800020000800020000800
020000800020001800060080803c204208004200818110a240080002000080002000000000000000000000800008440211008440211008444211108440211138440211828c54e11138444a11118444a310084402150084402110000000000000000001000008000200008000200008008200208000200228000a00
41880ce203380006002288086000080002) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (29e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (118414e20008400210008400210000000000000000000000000800020000800020000800020000800020010810460012802820012800ca04a28024e000080002000080002000000000000000000000800008500214008500214008500214008500214308400210118430210218408234108508e1
4338500214008500214000000000000000000100000000000000000000000000000000000400012000c000010100004100004000410128c000000000000000000000000000000000000000000000400010000400010000400010000404010130404810400c20010120504810410404020000400014000400010000
0000000000000000000000100004000100) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2a00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000400010000400010000400010000400010130534814500504024820434c308004340109004000100004000100000000000000000000000000100004000100004000100004000100004230008004200108804810108800800008800e0010000400010000400000000000000000000000084002
10008400210008400210008400210038404a10108420610428404230408400210108400210008400210000000000000000000020033800ce0000800ce0033800ce0033800ce00108104e00b28104204b3882c60022800c60033800ce0033800ce00008000000000000000000000840021000840021000840021000
8400210308408a1471840421401850c230) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2a20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (6c07e8116109412001e96ad17800000000000000000000000000000000000f8000000000000000000000000000000000000001a04a75ac019bfc02667aaa5df4019bfd9bfc000000000000000000000000000000000000103000000000000000000000000000000000000308080800000300010f
080c0800000100010c0000000000000000003c3c00000000000000003000000000000000000000000000000000000101040000000000000900000000000200000800000000000000000000000000000000000c200000000000000000000000000000000000000000114800500010400020810c0000012040400000
0000000000000108200000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2a40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc00000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffdfc0000000003fffffffc000000000000
00000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc00000000000000000000000000000000000000000000000000000000000000000113201014100000000112841880100000000000000000000000000000000000000000000000000000
0000000000000000000000000148284801) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2a60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (8c2023a808ea023a808ea023a808ea023a808ea023a808ea023aa08ea022a200000000000000008c03b020e8083b000ec083b020ec0a3b020ec003b028e4083a020e40a3b028ec083b028e2083b028ec0a3b028ec082a3000000000000000000000000000003fffffffc0000000003fffffffc00
00000003fffff7fc0000000003fffffffc0000000003fffffffc00000000000000000000000000000003fffffffc0000000003fff6fffc0000000003ffff7ffc0000000003fffff7fc0000000003fffffffc00000000000000000000000000000003fffffffc0000000003fffefffc0000000003fbfffffc000000
0003fffffffc0000000003fffffffc0000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2a80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (011081442010a300000000000000008c01800060021008040201008060001800040201800060001800060001800040201800060001800060001800060002a3000000000000000a8803a804ea0130886ca01b2806ea013a8848221ba884ea0138804e2073a80cca01ba804e00138814e20d3a80ce
a012a200000000000000000401a0006a003a10068401a10068003a100e8401a00028001a80068001800868001a00862001a00068001a000680000100000000000000020c01201048041a010e8043a0104804100304004120304804120104800120104804120104804120184806120184804001000000000000000a
8803a808ea0230808c20230808ea023080) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2aa0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (4004100104084100104004100104004100104004100104004100104004100104004100104006a200000000000000000480800820030800020000800020020800020000800020000801c200208008200208008200108000200208208200202100000000000000000402a00ca8032a02ea803aa00e
a80baa02ca80baa02ea803aa00ca803aa00ea807aa00ea803aa00ea803aa00ca803821000000000000000a8800a81428062a814aa052a8142a050a814aa050a8142a050a0002a070a814aa050881428040a8142a070881c2a052a300000000000000008c0108044200188046201188044201108046201108044201
1080042011081c62031081440001080442) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2ac0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (32010ca0432010c80432010c804001000000000000000200030000c00010000400010000c00010000400030000c00030000c00030000c00030000c00030000c00030008c000000000000000000000a88030810c20410810620418810c20410810420430810c20430830c20430810c20430810c20
c30810c20430110c2042a200000000000000008401b000680113000ec003b8006c00138006c001b0006c001a0046c001b00064001b0006a011b0006c001a0006c002a300000000000000008c01a8006e001a8026a009a8026a009a8006a009a80262009b8006a009a8026a00988026e00988026a009a8006a008a3
000000000000000a8c8010010400410010) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2ae0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (02a80188006a801a2006a801aa006a801aa006a801aa0060001aa0068801a2006a801808068801aa006a801aa006a2000000000000000088018812c20c98832620418810620498812620498812620430812620498812620498812c004188106204988126204aa200000000000000008c010010c0
0410010400410810400410810400410010400430010400410010400410010c0041001040041001040042a3000000000000000a8801a8106a041a8206a041a0106a041a0006a001a8006a04188306a041881062041a810680c188106a041a8006a042a2000000000000000004032010ca0c32010c80432010c80412
010480432010c80432810c80432010c804) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2b00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (018ec063b018ec0639018e0063b018e4063b018ec062a200000000000000008803a818ee063a808ea023a808ea063a808ea023a818e2063b018ea063a018ea063a818e6063a818ea0639818ea062a2000000000000000a8c02b018ac0621018a40621018ac062b01884062b018ac062b018ac062
b018a4062b018ac062b018ac062a01aac062a3000000000000000004002012080480012080400010080482012000482012080402012080482012080482012080402010080482012080480000000000000000000000801820062a018a8062a01828060a018a8060a01828060a018280608018a8060801828060a018
28060a0182806001000000000000000a88) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2b20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000a8803a800ea003a800ea003a100c2003a800ea403a000ea0038800ea003a800ea003a800ea003a800ea003a800ea0028200000000000000088001a0186a061a01860061a01868061a01868061881860061a81868061201868061a0186a061a01868061a01868060200000000000
00000000012010e8041201048041201048041201048041201048043a010480412010480412010e804120104804120104804000000000000000000a8803a818c2063a81aea063b818ea063a81aea06ba81aea0630818ea8638818ea063a818c2063a818ea063a818ea062a200000000000000008803b018e8063b01
8ec063b818e4063b018e40639818e4063a) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2b40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (4000120004200108004200108004200108004200108004200108004200100000000000000000000002a030a80c02030a80c2a030a80c22030080c22030a80c2a030a80c2a030a84c2a030a80c2a030a80c2a030a80c000000000000000000a8800a81028040a9002a400a000aa0c0a8106a000a0
102a040801022040a8102a000a81028040881022040a8102a042a200000000000000008801081042041081042041081062041081062041001042041081042041081042041081042041081042041081042042a200000000000000008801801060041801060041881040041801040041801060041801060041801060
041801060041801060041801060040a200) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2b60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (02b0002c002000000000000000000000030800620030800c20030800c20030800c22030880c20018800c20030800c20030800620030800c20030800c20000000000000000000000001b000e8001b1006c00190006c001b1006c001b0006c003a0006c001b0006c001b000ea001900064001b0006
c002a100000000000000008801a8006e00128006a001a8006a001a8004a001a8006a001b0006a001a80062001a0006e001a8006a001a8006a002a2000000000000000a880010100404010120404810920405210120424a101004040101004040101004040101004040101004040101004042a20000000000000000
0000800420010000420010800420002000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2b80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (229308846220108844221188846221188846221188046221188846001188046203188846221000000000000000000000010002400090002c000b000240019800240009000a40021000240008000240001000240009000a400090002400000000000000000000000001a8316a0c528316a0c5a811
6a0c7a8114a045a8316a0c5a831620c588396a0c5a831680c5a8316a0e588316a0c400000000000000000000032028ca0a32128c84a32028c80a32128880a32028c80e32828c80a32038c80a32028ca0c32038c80a32028c80a0000000000000000000000300024000b0002c000b0002c000b0002c000b000ac022
10002c002b000ac0003000a4002b000ac0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2ba0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (3a804ee013a804ea013a804ea0100000000000000000000002b00cac032b00cac032b00c84032b00cac032b00cac032b10cac032b00cac032b00cac032b00cac032b00cac03000000000000000000000002014080502014080502014000502014080d02014080502014084502014080502014080
502014080502214080500000000000000000000000a10428410810428410a104a8410a10428410810428410a10428410818428410a00420410a00420010a004284100000000000000000000002a880a000228808a2022880aa20228800a202a988aa2028080aa2028800a2202a880a0a02a880aa002a800aa20000
0000000000000000000188846221108a4c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2bc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0027e909fa426490992426492ffa4264909924be5f0997c27e92fffcbfff09fa4bfff0997cbe5f2fffcbfe909ffc000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000009fbf27
efc9fb727fdc9ff727edc9fbf27edc9fb72ffdc9fbf27edc9fb72fedc9fb727fdc9ff727edc9fbf2fedc000000000000000000000099b5242d490b424ad092b4266d090b5242d098b425ad090b5242d890b4252d091b624ad092b4242d090b5256d00000000000000000000003a804ee013a824e20938824e2013a
804ea0138804ea013b804ea113a804e219) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2be0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01048043a010480412010480412010480412010480400000000000000000000003a818ea023a808ea0230808e20230808ca023a808ea023a808ea0230808ea0238808ea023aa08ea023a808e802000000000000000000000039028e40838800e00838020e80838038ec0239838e40839038e40a3
9020e4803b800e00838020e00839000e00800000000000000000000000863721edc863121ec487b1218c48637218c4863727edc87b727ec49fb727ec49e3121edc9fb727edc9ff7278dc00000000000000000000009ff727fdc9fb727edc9fb72ffdc9fb727edcbfbf27efc9ff72fffcbfff27fdcbfff27efcbfbf
2fffcbff727ffc00000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2c00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000000001080662031000242009080242029080a42019000642011080642019880e620110006420090802420a90804420100000000000000000000001800040201800060001800040201800860001800060001000060001008040201800060001802060001802060000000000000000
00000000038804c20332084e20138804421138804e2213800ce20138824e20930824c22138084e20138804e20138884e201000000000000000000000018008600018000620018900624018948600418008600018008600618100600038100620018800620018000608000000000000000000000001201048041201
048043a110c8043a010680612010480412) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2c20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0620018000620018800620018800620018000660019800660018800670020310000000000000000c001102040021000040001000040001000040001000040001000040001000040001000040801000040021020000020310000000000000000c00800220202080220018800620038800e2000880
0a20000800a20028800a2000080022001882062083a0000200000310000000000000000002800ca0032002ca0032800ca0072800ca00b2800ca0032800ca0033800ca00b2802ca00b2800ca0032000ca003003100000000000000000008815a2056883120045801120044801122054881d220542805220768815a2
0548815200448031200448815220540000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2c40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0c1880062042a2020000000000000000030010c00c30034c20430810c20430830c00430010c00430010c00430010c00410010c20c30830c20c30010c004000020000000000000000030000c00030004c00010000400010000c00030000c00030000c00010000c00010000c00030000c00030000c
000000020000000000000a88030810c20c31810c20c18832620c98812c20430810c20430810c20418812c20410812c20430810c20430818c2042a2020000000000000000419000640018000600138004e0013800464001900064001900064003900064001100060011800460011900064002800800000000000000
0c01880862001800066001980066001980) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2c60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00608018000608018200608018200608018200638018e006080182006080182006080182006000120000000000000a88428800a20020000800020000800020000a20028800a20028800a20028800a20028800800020000800028800a2002a2020000000000000000018810620430810c20430810
c28430830620418810620418810620418810620418810c20430810c2041881062042800a0000000000000000010010400410010c00430010c00430010400410010400410010400410010400410010c00430010c004100104004280020000000000000a8801881062043a820620c188306204188126200188106204
18810620418810620018800620c1883062) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2c80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (3a818c20630818c2063a818ea062820a0000000000000208039018e40638818e00639018e00638018e40639018e40638018e40638018e40639018e00638018e00639018e406080020000000000000000038808e20638818e60639808e20239808e20638818e20638818e20638808e20638808e60
639818e60638818e206280000000000000000a8802b01884062b018ac063b01884062b018ac06ab018ac062b018ac06210180406ab01aac062b018ac062b018ac062a20200000000000000000020104004028100804020100204020100804020100804020100804000100804020100804020100804020100804000
120000000000000000008018a006080182) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2ca0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (018010401498032600410010400498012600498012600418212600498012600498012400410010400c980126004280020000000000000a88038801c20078801e20070801420078801e20078801e20078801e20078841e21078801c20070801c20078801e2006a200000000000000080001801860
06108186206188186206188186006180186006180186006180186006180186206188186206180186006000020000000000000008012010480490012e8043a010e804ba012480492012480412012480492012480492012e8043a010e804920124804000020000000000000a8843a818ea0630818c20630018c20630
818ea063a818ea063a018ea063a018ea06) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2cc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01004040009004042101004050101404052101004042a20200000000000000000080042000308042001080002000080048001080042081088042001088040001200042000080002000200042001000020000000000000000028030a00c20030a00c28030a00c28030800c28030a00c28030a00c2
8030400c30030a00c28030a00c20010a00c000020000000000000a88008810a24808030200400030000808010220408810220408810220408800220008810a00c28030a0040881022042a2020000000000000000010810621410810420410810420410810420410810420410810420410810420410810620418810
6204108104204280020000000000000080) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2ce0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000800030020c00810038400a10020400810020c02a30028c00a30020c01a30020c00830038400810020400830020c0080000a0000000000000a88030801c20051801620058801620058801c20070801c20070801c20070801c22070881620058801620070801c2006a20200000000
00000080019000640098002e000b8082e020b8000644099002640099000640099002640099002e000b8002e0009900064002800200000000000000000188006200188006600188806620199006200180006200188006200188004200189006600198006600188006200280020000000000000a8800101004053103
0040400054040701010840401010040400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2d00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0a22028880a220288c0a22020802a220a0880a02028080a00028880a2202a2020000000000000000018884622018804620118880c220308a46221189846261188846221308846221108046220188806220188846221280020000000000000000010000400110000400030004c001300004008100
284008100004000300004000180084001100044001100004000280020000000000000a88018830620c1883862081a810620418830620e18830620e18830620818810620c38810620c18830620c18830620c2a2020000000000000000430028c00ab000ac20eb082ac24ab0828c00ab002ac00ab0028c00eb002ac0
0ab002ac20ab082ac20ab0008c00a00002) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2d20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (2d094b525ad400000000000000000000038804e20938804e60139804e60139804e20138844e20138904e20138824e20938804e6093b824e60938804e201280020000000000000a8802b02c840b2b02cac0b2102c040b2b02cac0b2b02cac0b2b02cac4b2b02cac0b2b02c840b2102c040b2b02ca
c0b2a2020000000000000000002014000502814080500014080502114080502114080502014084502014080502014000d00034080d020140805000000000000000000000008004004108104204128104204108104200108104204108104204108104204108104a04128104a041081042041000020000000000000a
88028880a200a8080a0202008080002000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2d40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (7efc9fb727fdcbff72fefcbfff27efcbff72fffc9ff727edc9fbf27edc9fb727fdc9fb727edc0000000000000000000000be4909fa4265f0997c264909fa4bfe92f97cbfff0997cbfe92fffc27e909924265f09924264909fa426490992400000000000000000000000000000000000000000000
0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000009fff2fedc9fb727fdc9ff727edc9fbf27edc9fb72ffdc9fbf27edc9fb72fedc9fb727fdc9ff727edcbfbf2fffc000000000000000000000092b5252d090b424ad092b4242d090b5242d090b425ad
090b5242d090b4252d090b424ad092b424) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2d60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
71c2000c000040408004000c0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000bfb727ec4863721edc87b121ec487b7278dc9fb727edc9fb727edc87b1278c4863721ec487b121ec49e3727edc00
00000000000000000000bfb727fdc9fbf2) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2d80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2da0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2dc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2de0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2e00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2e20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2e40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2e60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2e80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2ea0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2ec0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2ee0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2f00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2f20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000071c2000c000020408004000c0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2f40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2f60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2f80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2fa0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2fc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2fe0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3000) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3020) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3040) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3060) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3080) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (30a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (30c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (30e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3100) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000071c200
0c000060408004000c0000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3120) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3140) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3160) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3180) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (31a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (31c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (31e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3200) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3220) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3240) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3260) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3280) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (32a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (32c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000001c2000c000010408004000c0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (32e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3300) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3320) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3340) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3360) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3380) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (33a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (33c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (33e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3400) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3420) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3440) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3460) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3480) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff0000000000000000000000000000000069da00008000000c020000008005000ca00000008001000c000000000000000000000000000000000000000000000000
00000000000000000000000000000000000000000000000000000000000000007002000cc00000008001000c7c2700008000000c0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (34a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0001) TDO (0000) MASK (0000) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'serase' instruction. 
SIR 8 TDI (0a) ;
RUNTEST 37000 TCK;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) SMASK (ffffffff) TDO (f5034093) MASK (0ffeffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) TDO (00) MASK (00) ;
SDR 16 TDI (4000) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'usercode' instruction. 
SIR 8 TDI (fd) TDO (00) ;
SDR 32 TDI (12340001) SMASK (ffffffff) TDO (00000000) MASK (00000000) ;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) TDO (00) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'usercode' instruction. 
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) TDO (f5034093) MASK (0ffeffff) ;
SIR 8 TDI (e6) TDO (00) ;
RUNTEST 50 TCK;
SDR 32 TDI (00000000) TDO (12340001) MASK (ffffffff) ;
//Loading device with 'conld' instruction.
SIR 8 TDI (f0) ;
RUNTEST 110000 TCK;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) TDO (f5034093) MASK (0ffeffff) ;
//Loading device with 'ispen' instruction.
SIR 8 TDI (e8) ;
SDR 6 TDI (34) SMASK (3f) ;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) SMASK (ffffffff) TDO (f5034093) MASK (0ffeffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) TDO (00) ;
SDR 16 TDI (4000) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fdata3' instruction. 
SIR 8 TDI (f3) TDO (00) ;
SDR 6 TDI (3d) SMASK (3f) TDO (00) MASK (00) ;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) TDO (00) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fvfy3' instruction. 
SIR 8 TDI (e2) TDO (00) ;
RUNTEST 1 TCK;
RUNTEST 50 TCK;
SDR 6 TDI (3d) TDO (3d) ;
//Loading device with 'conld' instruction.
SIR 8 TDI (f0) ;
RUNTEST 110000 TCK;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) SMASK (ffffffff) TDO (f5034093) MASK (0ffeffff) ;
//Loading device with 'ispen' instruction.
SIR 8 TDI (e8) ;
SDR 6 TDI (34) SMASK (3f) ;
//Loading device with 'conld' instruction.
SIR 8 TDI (f0) ;
RUNTEST 110000 TCK;
//Loading device with 'bypass' instruction.
SIR 8 TDI (ff) ;
TIR 0 ;
HIR 0 ;
HDR 0 ;
TDR 0 ;
TIR 0 ;
HIR 0 ;
TDR 0 ;
HDR 0 ;
SIR 8 TDI (ff) ;
SDR 1 TDI (00) SMASK (01) ;
