// Created using Xilinx iMPACT Software [ISE Foundation - 6.3i]
TRST OFF;
ENDIR IDLE;
ENDDR IDLE;
STATE RESET IDLE;
TIR 0 ;
HIR 0 ;
TDR 0 ;
HDR 0 ;
// Validating chain...
TIR 0 ;
HIR 0 ;
TDR 0 ;
HDR 0 ;
SIR 8 TDI (ff) SMASK (ff) TDO (01) MASK (03) ;
TIR 0 ;
HIR 0 ;
HDR 0 ;
TDR 0 ;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) SMASK (ffffffff) TDO (f5034093) MASK (0ffeffff) ;
//Loading device with 'conld' instruction.
SIR 8 TDI (f0) ;
RUNTEST 110000 TCK;
//Check for Read/Write Protect.
SIR 8 TDI (ff) TDO (01) MASK (ff) ;
//Loading device with 'bypass' instruction.
SIR 8 TDI (ff) ;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) TDO (f5034093) ;
//Loading device with 'ispen' instruction.
SIR 8 TDI (e8) ;
SDR 6 TDI (34) SMASK (3f) ;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) SMASK (ffffffff) TDO (f5034093) MASK (0ffeffff) ;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) TDO (f5034093) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0001) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'ferase' instruction. 
SIR 8 TDI (ec) ;
RUNTEST 1 TCK;
RUNTEST 15000000 TCK;
//Loading device with 'conld' instruction.
SIR 8 TDI (f0) ;
RUNTEST 110000 TCK;
STATE RESET;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) SMASK (ffffffff) TDO (f5034093) MASK (0ffeffff) ;
//Loading device with 'ispen' instruction.
SIR 8 TDI (e8) ;
SDR 6 TDI (34) SMASK (3f) ;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (400280000000000000000000000000000000000000000000000000000000000000000000000c400000000000000000054ede80000000000000000000000000000000000000000000000000000000000000000000000d53ff00000000000000016020000000000000000000000000000000000000
00000000000000000000000000000000000c48000000000000000001210000000000000000000000000000000000000000000000000000000000000000000000000c48003102000a0002000c800000008001000c000000008004000c900000008001000c638000008003000c6dfc01008004800cd0000000800680
0ce00000008001000c66aa9955ffffffff) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0000) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (074401dd00770801000000000000000e000fc00ff007fc01ff007dd54120704c013b4806d04230058c08fb004bc01ff007cc01ff007da003000000000000000162dc1c000480010000500014000500004000500014000500014000500014000500000000000048ff000000000000000420000000
00000000000000000000000000000000000000000000000000000000000000000000480000000000000000054ffc0000000000000000000000000000000000000000000000000000000000000000000000015bff000000000000000d2efc0000000000000000000000000000000000000000000000000000000000
000000000000015bff0000000000000001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0020) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (401f0036c065408f6c00df04c7c00df0037c00df003508030000000000000006001fc00ff003fc00ff003ec08bf109fd013b000bc403b143fc005b002fc00ff003fd00fe003d8007000000000000000e200bc40df8037c20d70034c00134165c819f0125c00570174d00df0047c00df0034c00df
0037a8020000000000000006200f400dd0037400dd0034400c10005406150205406954874411450067420dc0034400dd0035a803000000000000000e8043400cd0033400c50030410c10001400150011400050836402cd8003000cd2030400cd00322010000000000000000c2007401dd0077401dd107048611219
55011102c5409110074406511047001dd0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0040) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (600bc00ff003fc00f70037c08ff023dc482f023bc48d70935c80970027c00ff003fc08ff003db8020000000000000000404bc00cf0033c00c72233c05c71156c280f0350c208d0820d048b00a3c00cd0033400cf003010120000000000000002001b401ed007b401e9047f40121027a61929037a
44169117c40121804f401ed007b401ed00788006000000000000000a001f400cd0033403c501336060500024014d43800238850a0620890003400cd0033400cd0032a0070000000000000002004f400fd003740cdb00774029100044000b00c6c538108b04605100e3480dd1037480cd0034a01300000000000000
04200fc00df0037c00d70037c80170022c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0060) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (007c001f000700120000000000000006205fc005f0017c005f2014c007f009cd816f429dd007303989007f045fc005d0017c005f0015a837000000000000000c204b400cd0033400cd0030603dd04307130140b3400c588e2400dd08f1400cd0033400cd003328120000000000000004000f405e
d807b601ed00784916d00704e12d3079411e1106c403ed106b481ed007b401ed007900030000000000000006204f402ed003b400ed0038400e1003840021003840045203ac000d0039c00ed003b400ed00398813000000000000000e0057c00df0037c00df0034c40512024d001f2020e20d38024c409f0027c00d
f0037c00df0037a0150000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0080) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00134107c04132005d041d0007c001f0007c001d0006b01c000000000000000080434048d00234008d8031534810521400c10d20614c908604148d00234008d00234008d00202010000000000000000200634009d00276009d10254069900254209100a67009100654049d00274009d00274009d
0024a018000000000000000800074009d28274009c00244009308250009100e44029b00244469d03e74009d00274009d00262001000000000000000c2043c009f0027c049f01244109b0027c04930127c05832025c009f0027c009f0027c209f00270810000000000000000c004bc001f00078021f0087c8012000
3c081f0000c001f0007c821f0107c001f0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (00a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (20604009d0027400bd003c4009588254049102244409d20244208d00344009d00274009d0025a818000000000000000c00405028d0023600ad20284c48501a16409120234228d00244068d00224008d00234008d0023a810000000000000000c00704001d00074003d000440b112045480110084
4001120144011d10044001d00074001d0007001c000000000000000e8060c019f0027c009f0026d29b329e4c20a30569c21a7002ac07bf002ec00bf0027c00bf0027a018000000000000000e4067c089f0027c009f0026c14f7052fc00af002fc40ff002bc14bf003f4009f0027c009f1027b81900000000000000
0ac073c001f0007c005f0005c040b0905c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (00c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (03b400ed00388005000000000000000a0053400cd003362a2d20c84a3dd2833441810040400850cb1481cd83e3420cd2833400cd0032a014000000000000000200534005d00174015d00544107d0016c056b131ec0170015c4047d001f6004c00174005d0014a01400000000000000042053c001
f0007c041f0106c001f0005d42130004d01170007c061f0087e001f0007c001f0005081400000000000000060057c008f0027c009f0027c109b0163c209f0063c009300e7c089f0027d009f0827c009f00258015000000000000000e2014c009d0027c009f0024c88944025804934067c008f00e2d059f0026c009
f0027c009f0027a8050000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (00e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (02b581034a08d022f5046d812a400ed003b400eda039000000000000000000062057400ed003b4016f01484012d217bc08ab0048605e10178607ad004880ded017b441ed00398815000000000000000e0003c01ff007fc01df107cc011f0274d01a30244c09f74278c01bf026cc01cf0277c01df
027fa00000000000000000066043c00df0037c00df0035f005f003ec009f0005c20dd0015c205f0037c80df0037c00df0035a81000000000000000000057c01ef007bc01ef0078d01cd017bc01a38048d01a79079d014f007b401ed007b401ef0078001500000000000000020017400ed003b400ed0438400ed033
b500b9000a402e10038600ed103b400ed0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0100) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0204500dd0037408d100344001d00345818b0340405db26454439d0057440dd8037400dd00362081000000000000000c2200c00ef203fc0177014cc018f003e000bf004ed00f3003dc218f001fc00ff003fc00ff003f0880000000000000000c0007c00df8037c029f00b5c10df0237c03530404
812d700a4882dd10f7c40df0037c40df0037000100000000000000062057c00df1037c80dd0036d00df82bcc23175007d00cf41f3c02df00f6d00df0837c80df0035a815000000000000000c2013400cd0033600c580322024d00b34408d12e34cbc931434124d0400400cd0033400cd0033280400000000000000
040003400ed003b441ad813a480ed02384) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0120) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (047401dd10770801000000000000000e800cd01ff007fc01ff0074c08f58b0cc01bb0068c041b0004c043f2107c0c3f007fc01ff007fa003000000000000000e6017c00ff003fc803f0087c5c3f08bec00bf050fc00df4087c001f0207c08ff023fc00ff003fb005000000000000000ac000c00d
f0037c04d60134c049f0037c009f0496d14d30105c14170105c00dd0037c04dd0036b00000000000000000008040400cd0032410c181345440d00b1400191100400c9c1056040d0003600cd0033410cd0030201000000000000000020004400dd0037402d520306081d80374031c0006681510015444150865400d
d1037400dd0034a0010000000000000008) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0140) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (819b0025c025b4294c9093c0b4d0c1f2105c00df003508030000000000000006001fc00ff003fc00fd003cc00df000fc00bb182dc00df112e8005b20cfc20ff000fc00ff003d8007000000000000000e2008c00df0037c00df0035500d58104c839700625021b1085c825700c7c02df2067c80df
0037a8020000000000000006200c400dd0037400dd0035400d520347c39d18774200900254005510374805d0077480dd00358803000000000000000c0040400cd0033400cd0831402c108006009505274004940015028504b3400050003400cd0033a010000000000000000c2004401dd0077401dd0074ca6df03b
4401db00254481b200448311018740e1d0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0160) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (400bc00ff003fc00ff003fc2cfb123dcc02f113e40037402dc04f5021fc00ff002fc08ff003db8020000000000000000404bc00cf0032c01cf0071c11c58142c200b2061d05c320e2504810140c058f0041c05cf003010120000000000000002001b401ed007b405ed017a401e51173409a1007d
44921014240da912504050d014b405ed00788006000000000000000a001f400cd0032400cd0030403d5104248289202164081004640b0110044010d00a3600cd0032a0070000000000000002004f400cd0037400dd0036c03fb805540b81003440fd100744024b80344025d0027400dd0034a01300000000000000
04200fc00df0036c00df0037404df2a10c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0180) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (087c001f000700120000000000000006205cc005f0017c005f0016c0057001e44477005fc407b00dcc007f009fc467f001fc005f0015a817000000000000000c2048400cd0033400cd0032400c500f2440010031431d908f4500cd01b4401cd0073400cd003228320000000000000004000c401e
d007b641ed0078425e400fa4812500eb403e980f8403ad0063401ad00cb401ed007900030000000000000002204c500ed003b400ed0038504f0282ac00a1000cc20c10838400e30038c40ed000b400ed00398013000000000000000e0054c01df0037c00df0036c08f70024c01970024c20930035c00530025c40d
f0037c00df0037b0150000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (01a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (001b0006c04174104d041121044040b0007c001d0006a01c000000000000000080434008d00234008d00214148915214008108216348d4d20414c10520534cd00334008d00202010000000000000000200634009d00274009d00256088120276069900b2420d58024488d10834408d800274009d
0024a018000000000000000800074009d00274009d00244019b0125c239100e55879b04644009100244039d00a74009d00262001000000000000000c2043c009f00278009f0024901930163c019b0526c059b1164c01934024c21890027c009f00270810000000000000000c004bc001f0007c401f1005c0011018
7c001f0084d42174406c00021007c521f0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (01c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00634009d00274009d00244208500234089d02264408900254209101244109d00674009d0025a818000000000000000ea0434008d00234008d002040c8501226009d01215008141234028180a10028d00234008d0023a010000000000000000c00734001d00074001d00044071180454001d0156
c1e1b12844001105d44151d00074001d0007081c000000000000000e2063c00bf0027c009f0024c07b104ecc80bf00afc01b3422ec05a32865885bf002bc009f0027a018000000000000000e6067c008f0027c009f0026c149f252dc00ef052fcb4bb052bc00af352fc14bf002fc009f0027a81900000000000000
0ac073c001f0007c001f0005c041301038) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (01e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (05b400ed00388005000000000000000a20534004d0033400c90033423c101324330d00f0483c56470400c9083240bc00473400cd0032a014000000000000000200534007d00174205d0015c1171009d4437d001c40375041c53371001440371191f4005d0014a01400000000000000040053c001
f0007c001f0007c00130004c0a1f0884c00131084c10130006c92130087c001f0005081400000000000000060057c009f0027c009f0027c109b0165c009f0427c159f0122c028f0063c898f0027c009f00258015000000000000000e0017c009f0027c009f0024d00954026e408f00655019344e7c079340e5c009
f0167c009f0027a8050000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0200) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (10290019402e900994106d0439400ad042f400ed00390000000000000000000600574006d003b400cd0038501c14064c042d0172c60610008480ad0178430410023400cd00398815000000000000000e0003c017f007f841ff007cc01131275c012f2275c01f3005cc41ff0275c01ff004fc01ff
007fa00000000000000000062043c005f0036c00df0037c209f0035d000f0027c209f0017c00970037c001f4037c00df0035b81000000000000000000057c016f007bc01ef007bc01e3407ec012f1068d01c72058401eb4072c4143205bc01ef00781015000000000000000200174006d003b400ed0039400e1002
b0002d8438450e50030400e91238400a10) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0220) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (02074005d0037400d900374021103e5458050987c021518444519d0034403dd0047400dd00362081000000000000000c2203c007f003ec00ff003f400d7146bc41b3020cd05730004d20bf003ec05bf002ec00ff003f088000000000000000080007c005e0037c00df0037c005f1007c025f0017
c43d710328028e0037c025f0027c00df0036000100000000000000062057c005f0037c00df0034c40d300d5c011f0151c00db08b5c029f003dc801f0087800df0035a815000000000000000c20134004d0033400cd00304008102d04010d01126201900015068d00304001101c3400cd0033280400000000000000
0420034006d003b400ed003840021a11b6) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0240) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (077401dd00750801000000000000000e000fc04ff007fc01da000fca1d30036c01af08c4c41bb004cc02f3407fc01df0077c01df007fa103000000000000000e2017c007f003f804ff093fc143b010fc403f088dc003f250ec00af043fc043f043bc04ff003fb805000000000000000a8003c005
f0036c08df0237c16134107800130384d02074085c009f1536c008f001644adf0036b000000000000000000080434004d0033420c900334044106014201400275080500014008d89304084d0813400cd00302210000000000000000200074005d0037400dd80374221108154001100244109d40554019d0036402d
d0476480dd2034a0010000000000000008) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0260) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (059f0027c069f0406d004f0037c00df0037c00df0035000700000000000000060017c00df003fc00ff042e000fb0036c00b9400fcc0b7280fc019f003fc00ff003fc00ff003d0081000000000000000e2083c00df0037c00db0117c00d730378819f01c4c839f0404c05d30035c00df0037c00df
003521800000000000000006200f400dd0037400d10007200dd2835401150876421911014428110037400dd0037400dd00352803000000000000000e804f400cd0033440c90007434c520b34005501206049d0030406410031400cd0033400cd10312010000000000000000c200f40add0077401d10007440db20f
4401951002c30d30844502912077401dd0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0280) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (600bc00ff003fc00ff8a0bc08df2037c603e0125c00bf011b4003f0037c00ff003fc08ff003d280200000000000000004048c00cf8033c89c69343c05c70571c200f0063c63970252c004f0173405cf0073c05cd023010120000000000000002003c401ed007b401e1136b605e1127b409b1236a
405ad034d401ad017b405ed007b405ed00780802000000000000000a001c500cd0033400c50002400c4817000089a026402850883421cd0033400cd0033400cd003020030000000000000002004c400fd0037400d100a3000d1007bc038100244000f000151a1d0033400dd0037400dd0034201700000000000000
04202cc00df0037c20d70017c80d70037c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (02a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (007c001f000700120000000000000006205fc005f0017c0053115ec00570016c0363405dc0163011cc00730014c00534017c005700152007000000000000000c204b440cd0033400c50023400cda0314028110214228989c2402c12030400c12033400cd0031281200000000000000040007401e
d087b401e18053401e5a07a511a1846d411b1004c021e10078401e1007b401e5007908000000000000000006204f400ed003b400e5002bc00e500b9400a10029400ab200a800f14038500e1003b400ed00390013000000000000000e0057c00df0037c00d3001ec00d3007ec409b0822c00930040c00d30070c01c
30073c00d7003520100000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (02c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00530006c001f0007c24170007c001f0007c001f0006001a000000000000000080434148d00234008505244609d85214208140206009d10215348d00234008d00234008d00200010000000000000000200634009d00274009110240009d00244009100224049d30270008900274009d00274009d
00242018000000000000000800074009d20274009501201008d09e54019100244019906a45019d00274009d00274009d00272001000000000000000c2043c009e0027c00932425c089f0224c04970026d009f1067c29970027c009f0027c009f00250010000000000000000c004bc001f0007c001f0004ca015008
7d061708058841f0007c181f0807c001f0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (02e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (20634009d0027400910020400c92024401990c244008904374009500274009d00274009d0025281c000000000000000e804b4008d00234008180205048c08a04009909264448980254028d00234008d00234008d00210012000000000000000820734031d00074001147c44010c0084c20110144
501110006c411f00074001d00074001d00070018000000000000000e0067c139f0027c0093016cc28bf0068400a308a2c08bb002cc03bf002fc00bf002fc009f0027b018000000000000000e6067c009f0027c009f052fc74bf2023c00ae052f814a9002ec94bd1027c009f0027c009f0027a81900000000000000
0ac077c0e1f0007c00130105c005f0104c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0300) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (03b400ed00380004000000000000000a0050400cd0033400c91080481c51613601c50030422cd20b0402cd0033400cd0033400cd08302010000000000000000200504005d001740057009c40275005d4136100104197d029c0827d00174005d00174005d0814200400000000000000042050d001
f0007c00130684c00130005c10170004c001f0084d100f2807c001f0007c001f000500140000000000000006005fc009f0027c009f0027c109f0025d80974127c02970126c009f0027c009f0027c009f00250013000000000000000e2017c009f0027c00934124c409f2024c509b40a6c879b0821d109d0027c009
f0027c009f002521050000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0320) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (08b9013d400b5002c40069003f400e9003b400ed0039000000000000000000062057400ed003b400e10010405b501f8482a5077ac004b2210542750377400e1003b400ed00390095000000000000000e000bc11ff007fc09f3005cc89b3027ec01a3107cc01f70078c0173007fc01fb007bc01ff
007d200200000000000000066043c00df0037c00db020fc005f4015c00df033e7001f0027c001f0037c00df0037c00df0035281000000000000000004054c05ff007bc01eb404cd0167005bc01670578e81bd2028c01bf007bc01ef007bc01ef0078001400000000000000020014405ed003b400e50028402e5405
b400e1013c4006d00784102d003b400ed0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0340) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0007480dd0035c00df0045c80950044423850032c00cf80c44009d2037400d90036400dd00342083000000000000000c2007c00ff003fc00f3040fc03b390ccd00f3003cc08ff000dc00bf003fc00fb003fc00ff003d008000000000000000080007c00df0037c00df008fc02d74085c42d7003e
800df01a7c08870037c00df0037c80df0035000100000000000000062073c00ff0037c00d3000cd00d90002c10db003dc19d50824c41db0037c00db0037c00df00352010000000000000000c201b400cd0033400c142545200d00224218d00334030800004414d0033400c10033400cd0031280200000000000000
040043400ed003b600e1001864429023a4) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0360) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (077401dd00751801000000000000000e000cc01b3024cc093b323fc143b0049c012b053dc423b007fc01ff007fc01ff007fc01ff007fa003000000000000000ee017c00ff003d400f3000dc1c1f8c03c00bf04b38002f0d0fc00ff05b7c04fb003ec04ff003fb8010000000000000000c007c00d
f0037c48d31281c46110025c0093003c4481d8085480df0137c2adf00b742add0036180000000000000000008043400cd0031480cd4001404458c20400852136400150000400cd0833480cd2232400cd0030001000000000000000020007400dd8037400d100c54005108254019180344101d3065400dd0037600d
d0037400dd003420010000000000000008) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0380) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (801f2037c005f1237c00df0036c00df8037c00db0035080300000000000000060017c013f026fc00ff103742159020f40133003cc00ff283fc00ff203fc00ff003fc00ff003d8005000000000000000e2028d08134064d00df0037c2c1f1481c134f2035c035f0835c20df1037c00df0037c00df
0037a8020000000000000006200c4009100044001100364009508074041d0837428910037440dd0037400dd0037400dd0035a003000000000000000e804c4148100004000d01334508d00236800d8c31408040431480cd0033400cd0033400cd00332010000000000000000c200c4008100044000122b640611084
7d019101b4406910137041dd1077441dd0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (03a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (600bc01ff021fd081f003fcc0db1005c20360037c20ff003fc20ff003fc00df0037c00df003da80200000000000000004048c00cf0010c60070130c01c30043d100f0173c0acd0833c08cf0173c00cd0033c00cf003210120000000000000002003c403ed005800129007844d65094e4092d017b
4212d007b401ed217b441ed007b401ed007a0806000000000000000a001c500dd00944001500344104140924000c10374001d01b7400cd0033400cd8033400cd003220030000000000000002004c4001d0064409db003c07151010440a1f003f400dd0037400dd2037400dd0037400dd0034a01300000000000000
04202cc011f0464c01db0034d00132105c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (03c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (007c001f000580120000000000000006205fc02534094c035f0014c2071005dc027f0017cc17f0017c005f0017c005f0017c005f0017a817000000000000000c204b400410030500cd0031433c18141402010033400d50033400cd0033400cd0033400cd00332036000000000000000400074016
10078401ed0078421a1c0496013d0073411ed007b401ed107b401ed007b401ed007900040000000000000006204f400610038400ed01b9400c100094002121bb48027003b400ed003b400ed003b400ed00399833000000000000000e0057c20532074c00df083cc40939001c001b0877c00170037c00de0037c00d
f0037c00df0037a0100000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (03e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (001f0105c041b0007c001d00074001f0007c001f0006b01c00000000000000008043401ad0068401ad25205148900244009d05204148d00234008508234008d00234008d0020281400000000000000020063401bd022c4088900244089000274089d00256009905274009d00274009d00276009d
0024801c000000000000000800074829d30a44029d20244009b04a0c058d00244009d00274009f00274009d00274009d00262001000000000000000c2043c009e0064d419b2024c01830025c009f1025c009f0027c009f8026c009f0027c009f00250810000000000000000c004bc103f0407c181f00074ca1f020
7c0c1e0007c001f00078001f0007c001f0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0400) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (2063400dd00244008100244408d00274019d20244009100234409900274009d00274009d00252018000000000000000e804b4008d04204108103204028d4027400dd01a24228101234008c20234008d00234208d00210812000000000000000c20734011d01444050300c4401050016c201d0144
4171308474001c00074001d00074001d0007101c000000000000000e0063c02bf002cc00b341e4c03bb202ad80bf21e6c219300afc00970027c009f0027c009f0027a018000000000000000e6067c149f0527c149f0527c54bf002fc00ae0527c14ff05278209f0027c009f0027c009f0027a81900000000000000
0ac073c003f0000d000b0104c24530007c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0420) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (03b400ed00388001000000000000000a00534018d0031401cd08304a0c940d0000050030400cd0033400cd0033400cd0033400cd0032a01400000000000000020051c1a7d045c4107d001441170065bc0061001440057101f4005d20174005d00174005d0014a01400000000000000042053c001
f0005c001f2004c001a0004c921700078001f2007c001b0007c001f0007c001f800508100000000000000006005fc009f0427d10970023c109700e6c009f0027c01875027c009f0027c009f0027c009f00258013000000000000000e2017c009f0024c00930024d049f00e7c049f0026c4a930027c009f0027c009
f0027c009f0027a8050000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0440) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (003d0038400c9012b408ed013b404ed013b404ed0039000000000000000000062057408ad022ac0dad03784850121705162d003050de1425b485ed0173401ed017b401ed00391815000000000000000e0003c01ff007cc81ff1475c09730279d013f047cc01d30277c01df0077c09ff007fc09ff
007d200000000000000000066041c001f0007c009f003fd205f0027c000f0035c08ff0017c00df0037c00df0037000df0035a81000000000000000004057c212f0859c016f0078c01eb0078401270078d01cf006bc01ef007b401ef007bc01ed0078001100000000000000020015420ad0028600ad0938400a1402
f480210070404e5001b400ed003b600ed0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0460) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00044005d04c44091120344005b0862c021d0034400d10887440dd0037400dd0037400dd00362085000000000000000c2200c087b005cd0075003cd20f3102fc003f003cc00e7120fc00ff003fc00ff003fc00ff003f0884000000000000000c0007c00ff003fc00ff0837c009f40a7c021f1035
c00d70027420df0037c00df0037c00df0037000100000000000000062057c065f0014c00df003dc40d300a55010d003cc00f90037c00df0037c00df0037c00df0035a815000000000000000c20134051d00024000d00344091101304078d1032412c90017400cd0033400cd0033420cd0031200400000000000000
0400034002d00184046d013940081443d6) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0480) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (077401dd00771001000000000000000e000fc81ff007fc21f3005ec003b090e88027010ec002f000ed0c3f030cc147f007fc01ff007f2103000000000000000e6015c007f000fc001b023fc461f0127c002f203fc02ff080fc00ff003fc08df0037c02df003fa805000000000000000ac002c005
b0014c94470134c8a930527c001f00b4c04d78103c14dd0537400df0537c00df0036b00000000000000000008042500cd002040485a0305000943264004d0230504c10523404cd0333480cd0133404cd0030281000000000000000020006400d90135410c500344005104674841d0034400d500b7400dd0037400d
d0037400dd0034a0010000000000000008) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (04a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (02d710a1c00d30025d02d34404c00cf0037c00df0035080300000000000000042217c00ff103fc00fb081fc001f0417c003f1055c03bf025ec00b72077c2077003fc00ff003d800500000000000000000003c00df0037c00d78017c040b0896c221700c6c469f04d7c009f3074d005f0037c00df
0037a8800000000000000006201f400dd0037400d50015400550d24414518915400110025402551224400dd0037400dd00352003000000000000000e8043400cd0033400c5001160049808240845c48248005022118c0d0080404cd0033400cd10312010000000000000000c0017401dd0077401d1451542b15104
4403110195c0b110844484470004414570) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (04c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (600bc00ff003f800df021cc09db2027cc8fc0237c007f0b3bc20ff023fc005f0037c00df083db802000000000000000060dbc00cb0033c00c32815c01c74c41c00870172c00030311c00051150d024d20334a0cd023218120000000000000000011b401ed007b001e02059411a10179401e10168
619e90368449e183484014d007b401ed007a00060000000000000000008f400cd0033400c040154828100e14128500225114140414001580804004d0033400cd003220030000000000000000004f400dd0037400d10094422530091422430014c009b0420000d000a440add0037400dd0034a01300000000000000
04200fc00db0037c00d30417c045f1094c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (04e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (007c001f000580120000000000000004005fc005f00174005f001cd005b4055500530016c265b4050c03530217c025f0017c005f0017a807000000000000000c205b400cd0033400cd1010400c903f0402c100b0511c1003048ad100f3600dd0033400cd0031201600000000000000040003401e
d007b441ed0858481e90079403e500e2441e144704016140db401ed007b401ed007900040000000000000006004f400ed003b400ed0018400a10030620810038400c1801840081083f400ed003b400ed00391813000000000000000e0043c00df0037c00df0014c00930025e001b48468005b2014d001b4037c00d
f0037c00df003520100000000000000004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0500) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (241f2107d041301054a4172114c841f00074001f0006b01f000000000000000000434008d00234008d0023414a13528514ed8529414a10528414a185284148d00236008d00202814000000000000000000634009d00274009d01a5402b5a42c400bd003f460b1402d400b5812c4009d00274009d
0024801c000000000000000000074009d00274009d00e6c038100e04009d0025c048120244009310e45419d00274009d0026200100000000000000042043c009f0027c009d0024c02970264c108f0027c02930225c10970024c029f0027c009f002508100000000000000004204bc001f0007c001f2087c0237000
7c02170107c021f0107c00170003c101f0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0520) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (20634009d0027400950023421d90226004992a244c29180a44048502274009d00274009d002520180000000000000004004b4008d00236008521234808980224008910214008100a04068d0ca30528d00234008d00200012000000000000000c00634001d000740011404740a1110844025105c4
42a1100044011701574055d00074001d0007181c000000000000000e0073c209f0027c0093022fc01b3446e411bb0d65c21b6406cc039f206fc01bf0027c009f0027a019000000000000000e6077c009f0027c009f0526cc08f0037d009f0525c009f0027c14970527c149f0027c009f0027a81900000000000000
086073c001f0007c001f0005d04372104c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0540) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (03b400ed003a0801000000000000000a0043400cd0033400c100304004908b15838100364d0490061400c14033411c90033400cd0832201400000000000000020403400580015c0051095c4017d001c413650014e0061041040051201f4107d10174005d0014a01400000000000000042153c001
f0007c00134004c381b2104c00130084c42130085c00130007c001b0007c001f000508100000000000000004215fc009f0027c009b0827c00971860c10971027c019f1267d01970027c409f0027c009f0025801300000000000000040017c009f0027c009700274019b00a6c009b0925c4a930024c009d0027c029
f0027c009f0027a8050000000000000004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0560) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (802d213a454e9013240ce10118400ad013b400ed0039000800000000000000000057400ed003bc05e10279405100163404ad0172c0fe10069401e100604052d007b405ed003918950000000000000004001bc01ff007fc01f10074c017b027fc01bf107ec01cd0274c09d30264c09bf027fc09ff
007d200200000000000000066043c00db0037c00df0022d005f0007c808f203dd80d50023c18df0037c005f0037c00df0035a81000000000000000046053c01ef007bc01e30048c016b0069c01a3017e401eb4079c81c30053c01eb007b401ef007a101100000000000000020013400e90039400e0003d4010da02
8400a50338402c90028404e100fb4006d0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0580) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (020f400dd0037400dd06544010b0045493cb0834403910224440db00844189d1037400dd00362085000000000000000c2203c00fb003fc00ff005cc007f002c430f3043ec00fb007dc00c70048c00bfa03fc00ff003d0805000000000000000c2017c00df0035c00df0097c001700a7c00df0037
c10df2025c08df0117c00df0037c00df0035800100000000000000060053c00df0037c00d30034c125b0227430df217ec00cb4032d02f340b4d00df0037c00df0037a81c0000000000000004200b400cd0033400c10021427090a836038d08b6481c10422405c100b04001d0033400cd0033201600000000000000
040003400ed003b444e101084043820234) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (05a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (077401dd00770001000000000000000e000cc01b34048c810f004ec21130047c01ff0047c01eb007fc09fb00ffc01de0075c01df007fa003000000000000000ec017c00ff003f408df000fc041b1107c00bf0435d00ff002fc02ff040f8801f0237c02df003fb80500000000000000086003c00d
b0037c00df0000c145d0385c40930136c40db1135c00f50500d040d0037c04df0036b00100000000000000000043400cd0033404cc040050c850401420890430410c12420624c101004104d3133600cc0030201000000000000000000007400dd0037400dd00244015d20c5601911836401d90035600d506244005
d0037440dd203480010000000000000008) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (05c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00d304d6c04d34036d00d72037c20db0037c00df0035080300000000000000062017c02b7201fc00bd001fc00f3126f800fe004f420fb003fc00fb003f800ff003fc00ff003d8805000000000000000e0000d128b0000c409f0086d00d74067c00df0047c00cf4037c00d34037c80df1837c00df
0037a0000000000000000006200c4009900344211d00144201c0007400d90504200d50033480d50037480dd0037400dd0035a803000000000000000e80404009900244001d0000400050001400cd0011400c50431604c53133400cd0033400cd0033a010000000000000000c00044009100144001d085442011000
3401d90044401d11137424c10037401dd1) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (05e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (600bc497f003fc0877403bc041f0217c08f78302c00ff023dc00ff0037c00ff023fc00ff003db802000000000000000060c8d085720208054f0363c25070153c08cb0051c00c30034c0dc70373c01cf0173401cf003018120000000000000000001840961005840579007f40125015b421e9006b
649e10078401ed987b421ed017b405ed007800060000000000000000008c4004500c0441480022404150117400c94021602c10030401c40037400cd0033400cd003020030000000000000002004c4009120f441a800017484d50067400d10086c00d10034404dc0037400dd0037400dd0034a01300000000000000
04200cc10974624c00970007c00d30067c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0600) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (007c001f000508120000000000000004205cd00530014c805f2014c07534095c405b44d84804f20174005f0017c005f0017c005f00152017000000000000000c2058400551036440cd0032401c11837420c10071400cd0033400cd0033400cd0033400cd00332816000000000000000408104216
10068401ed0068441e10079401e1007c601ed207b441ed007b401ed007b401ed007900040000000000000006004c40077001ac00ed083aca0e1003b400e10028400ed003b400ed003b400ed003b400ed00398013000000000000000e2040c005b0804400df0024c00d38837c00db8024d00df0037c00dd0037c00d
f0037c00df0037a0100000000000000004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0620) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00130005c001f0007c00530017c001f00074001f0006b81c00000000000000008040500e1002a400a1102c441a5006b400814824440cd102340081c0234008d00234008d0020201000000000000000020060408b1602e00aa1003c408a502274009102250009d00a74009180234809d20274009d
0024a018000000000000000800044019129645009108204029500e74009104a4c009d00e74029100274009d00274009d0024200100000000000000042040c01930164c00930024c41910067c40930025c099f0227c00930167c009f0027c009f002508100000000000000004004bc00371007c411f0007c101f040
7c001f0406c001f00074001f0007c001f0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0640) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (2060400d510244008d0824400c188204009101266009500334008508274009d00274009d00252818000000000000000480484008181204008d0020400898c234008100264008521304008d01230808d00234408d00212012000000000000000400605010510044341d2004404130104c00110804
4001100444151700474001d00074001d00070018000000000000000e0070c02b100ac840bf0025c08b3002fc0093002ec40b320afc60bf00afc009f0027c009f0025a01c000000000000000e6077c149f0521c149f40270149f0527c009f2029c808f0527c949f0527c009f2027c009f0027b81d00000000000000
0ae070c00334006c00030004d00070003c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0660) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (03b400ed00388004000000000000000a00404034d40b0402cd8032525c92872600cd8013403c100b060bcd0073400cd0033420cd0032a01000000000000000020042d107100dc41077001440371511f4005f01dcc0271009c0027d085f4005d00174405d0014201000000000000000042050d041
30004c001f0004c40170007c001f0105c08130104d041f0007c001f0007c001f000508140000000000000004205fc809f0427c109f0827d009f1425c009f4025c109b0024e00970427c009f0027c009f2025081700000000000000040014d00824120d009f0025c009b4027c40900c22c00874027d009f0027c009
f0027c009f002520050000000000000004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0680) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00ed21284c0ad022b4006d000a400ed003b400ed003900000000000000000004005441831403ad00fd0432c89bd014b440ed02684842d202b4008d0371c00ed003b400ed0839001500000000000000040018c0333207cc01ff007cc05ff007fc09ff826cc01bf006fc01ff007fc01ff007fc01ff
007d200600000000000000066043c02d30013c00d70035400c79037c00d70035c008f0015c009f0037c00df0037c00df0035b81000000000000000006050d01ef2078d01ff007ae01ef007f401ef0079c01a1405cc01ff007bc01ed007b401ef00791814000000000000000200124006d043c440e5803a410f9003
b400ed2038400e10038400ad043b400ed0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (06a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0204401d114634071d08374021d01c7400dd0446c011d028440e5d01d7400dd0037400dd00362081000000000000000c2280c0173003fc25ff003fc02bf010fc00ff001cc003d204ed017f095fc00ff003fc00f7003f0880000000000000000c2017c005f00a7c021d0037e025f20b7c00de0097
d029f0037e005f0007c00df0037c00df00370805000000000000000200d0d03530074c00df0034d00df0035c00dd0414c008f0037c005f0006c00df0037c00df0035a014000000000000000420084128100424400d00324000d1003400cd00204000d00234001d0001400cd0033400cd0033280200000000000000
040000400a104084082d02384086501394) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (06c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (077401dd00770003000000000000000e010fc81ff007fc01f30006c0133007ec083f004ec411b4046c29130043c01ff007fc01fb007fb103000000000000000e6017c20ff002b8443f013fc401f0407c00ff0d27c002f000fc003f0187c04ff003fc00ff003fb80500000000000000086000d00f
30027c001f0037c161f0007c20df21a6c001f0006c001f1285c00df00b7402d700369800000000000000000000404000140234080d22334860d0403400cd04224000d20104028d0123608cd00b3402cd00302010000000000000000a0004404010077400dd0037400dd0037400dc00664039d00144009d8025400d
d0037400d50036a0010000000000000008) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (06e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (02d70017c2a1f0017c22d78486c01df0037c00df0035002f00000000000000062017c00ff303fc00ff025fc0077001dd05ef0c3c010fb000dc817b402fc003f003fc00ff003d0081000000000000000e0203c00df8037c00d340668014f44d7c04d70857c450f0046d011700c78015f0037c00db
003521800000000000000004001f400dd0037440d100254011d2074500110047401d510724049518670519d0037400dd0037a00300000000000000040053400cd0033400c100004401d2025444051003400050d124800d0003400cd0033400c910310013000000000000000c4007401dd0077401d102d540115207
444e112864441d11024c041110474019d0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0700) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (200bc00ff003fc00ff003ec002f003bc48ff001f8007f083fc00ff002fc08bf003fc00ff203da8020000000000000000605bc00cf0033c0dcf0151c17030071c08130753c294b02534834503e2c058f0033c0dcf023000120000000000000000201b401ed007b401ed015b4013901794092d007b
6296d027b441e1214f40dad007b401ed0078000b0000000000000000001f400cd0033400c900004110009304000100d2000492cd34201520024008d0033400cd083020030000000000000002004f400dd0037400dd0422c835b0031420dd00834419d0187400d000a34011d0037400dd0834281700000000000000
04200fc00df1037c00df0825c405302b5c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0720) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (007c001f000700120000000000000004001fc005d00174005f401c50e7b23d9f0177001dc0173009dc037f001cc007f0017c005f001520230000000000000004004b400cd0033400cd00b0400852073418cd00516814962d0400cd8e726008d0033400cd0031201200000000000000040003401e
d007b401ed0078601a8007f4a12580d9443610059603fd0078401ad807b481ed007900000000000000000000004f400ed003b400e1201048065003ac000d00384a0610018400ed002ac00ad003b400ed0039001300000000000000042043c00df0037c00d30064c015b0034d00170014c80432015c008f0024c018
f0037c00df0035a0100000000000000004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0740) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (041f0004c001340004801f0007c001f00074001f0006001b0000000000000000a0534008d00234008d85214008100204148d80224009900254008d20234008d00234008d00200010000000000000000200734009d00264009d00274809500245009d00244009904244808d80254009d00274009d
0024a018000000000000000820074009d00274009d0065c0e9101a44809d04e6c048900e16009d11a74009d00274009d0026280300000000000000040043c009f0027c009f00e7c019f1166c008d2165c42930624c009f2027c009f0027c009f002500300000000000000004004bc001f0007c00130107c401f008
4e001f0006d00170087c041f0007c101f0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0760) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00634009d00274009900266889900254409d11254009501254008d02244429d20274009d102520180000000000000004804b4008d00214008100326018808225048180254009101274048d00205009c20234008d00200012000000000000000c40634001d00074001b0286c00110007e43150015
4001500444011d00044001c00074001d00070018000000000000000c8073c009f0027c0093006ec00b3002ccd39b002cc00b310aec029f802cc00bf0027c009f0027b019000000000000000e0077c009f00274009f002dc00a7202bc14bf002f400b7052fc54bf002fc40bf0027c009f0027b81900000000000000
0ae07bc001f0006c001f0107c00170006c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0780) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (03b400ed0038000000000000000000080043400cd0033400c10833400c12031400dd8133451cd6030200cd0823600c90033400c500302130000000000000000000434005d00174005300174187120584005f001f09271001d4005d021e4015d00174005d0014280000000000000000042043c001
f0007c00134007c00174085c021f0007c00170006c421f2007c021b0007c201f000500540000000000000004204fc009f0027c009f00e1c00974127c04970067c029f0026c049f0027c809f0027c009f0025005700000000000000000017c009f0025c009319e6c028901a4513932021c01830023e139d04a4c008
f0027c009f002720050000000000000004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (07a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00e5192b600ad000b400e9110b418ed003b400e50039018c00000000000000044057400ed003b400c1003bc01450770434ed01c348067003b440e1036bc208d003b400cd003900150000000000000006051bc01ff007fc01f3007fc01db0070c01ff9077c29ff107f801f32067c01ff007fc01f7
007d204200000000000000062043c00df0037c00d70037c00df0033c40d73027c00d52805c04dd0026480df0037c00df0035285400000000000000086043c01ef007bc01e30073c01e50079c07ff106bc81ed004ec89ff084bc01e9007bc01e70078003000000000000000082003400ed003b400e1003b400e100b
c400ed002b400e9003940ced042b430ed0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (07c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0217400dd0037400dd10274001504e4d00d300474001d0604400c90467c00dd0037400dd0036088300000000000000042293c00ff003fc00ff2037e0073403cc00d7200fc027f003fc10fb002fc00ff003fc00ff003d008100000000000000062017c00df0037c00d70025e029e0017c00ce01a7
c0697200fc80df10a7c04df0037c00df00350001000000000000000e00d3c00df0037400d30877600df0070d83ff0963c10df2877c80f34227403df2837c00d7103520180000000000000004000b400cd0033400c90423420050070405cd00034000d0683689c120a16018d0833400cd0031201200000000000000
040003400ed003b400e1462b400a5613c4) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (07e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (077401dc00770803000000000000000e000fc01ff007cc0133083fc009b0046c21fb002fc01ff007dc01fb0074c01fb007fc01ff007da003000000000000000e2017c00ff003fc24ff012fc543f003dd00f7010fc343f010fc10fb0239c54bf203fc04ff003fa8810000000000000008e003c00d
f0037c28df12a7406130eb4c00d70706c021f12b7c00ff0117402dd0037c00df0036a00300000000000000002043400cd8033400cd0023430053114400c100034000d0000440dd11b34008d0033448cd2030281000000000000000028007400dd0037400dd0077434d12074400d58066410dd0035400dd0077400d
d0037400dd1034a0010000000000000008) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0800) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (84df0077c00d70037c00df0037c00df0036c00df0035080300000000000000060017c00ff203ec107f006fc20b7002dc00f7102b800ff003fc00ff003fd00ff403fc00ff003c8005000000000000000e2003e00de1035c11030237c219b6143c80cb0177c00df0034c00db0030c00d30037c00df
0037a8200000000000000006000f400dc0835401540027403993047400d90077400d98037400d10034400d10037400dd0835a803000000000000000e8043400cd10314001100246008d8507400c90023600cd2032400c90030400c10033400cd00332013000000000000000c6007401dd007444055002740191200
5401d10847401dd0877481d10074001d10) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0820) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (200bc00ff003fc003b0137c083f832fd08e3012b800df8037e00df0237c80ff003fc00ff003db8020000000000000008404bc00cf0232c00070237815872167c00c74023c00c30033c20cd0173c00cf0032c20cf003010120000000000000008201b401ed007b40125803b405ad0168501e5016f
601ed087b401ed097b401ed807b401ed0078800f0000000000000008000f400c90032008054072403852003602c10023400c10032400c90033400cd0032400cd0032a0070000000000000002004f400dd0037401d1068300b9f0024442d10037400dd0037440dd0037400cd0033400dd0034a01b00000000000000
04200fc00df0036c02130007c029f10a7c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0840) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (007c001f00070012000000000000000e205fc005f0014c1273001c40873295cd0041139fc005f0016c005f0017400470817c005f8815a817000000000000000c005b400cd0032407414015403451172600c10073480cd0033400cd8033400cd0033400cd1033281200000000000000000013401e
d007840121005060181807e401e11073401ed007b401ec007b401e5007b401ed107902010000000000000006604f400ed003ac0021003900025002ac00e1003b600ed003b400ec203b400ed003b400ed00398813000000000000000e0043c00df0034c01132034c01132000c00d14037c80df0036c20df0037c00d
70037c00df003780150000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0860) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00134106c001f0007c401f0007c001f0007c001f0006b01d0000000000000000a0534008d20234008945234148100244008555234008d00214008d00204008d00234008500202010000000000000000200734009d00274029904274019500245049102260009d00274009d00274009d00274009d
0024a018000000000000000800074009d00274039100a74009100204049100274809d0025c009d10244009d0027400970026200100000000000000042043c009f0027c08930167c40973824c00932023c009f0027c009b1025c009f0027c009f002708100000000000000006004bc001f0007c001f0407c081f400
5f001f0007c201f0007c001f0007c001e0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0880) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00600009d0024444850aa24019c0a244009d20a74009d00274009500274209100274009d0025a818000000000000000400484008d0020404c501204008d00204208d00224008d00236008d00234008900234008d0023a012000000000000000c60705001d00045241142c6c025d01444001d2207
4201d90074001710074001100074001d0007081c000000000000000e0064c00bf0024c02b7026cc14bf08a4e20af012fc009f0027c009f002fc00bb002fc009f0027a019000000000000000e2067c009f0027c14b7052fc00bf052fc0089002f8609f0027c009f0027e409f0827c009f0027981900000000000000
0ac077c001f0007c000b2107c84570004c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (08a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (03b400ed00388005000000000000000a00534004d0030520c12070401c4003240dc50233400cd0033440cd8011400cd0033400cd0032a014000000000000000200534006d001440071201c402750014c00630015c005f00174005d201d4005d00134005d0014a01400000000000000042043c001
f0804c041300048241b0086c80170087c001f0007c001f0005c001f8007c001f000508140000000000000006004fc009f2027c019b0027c008e0027d009f0067c009f0027400970027c009f0027c009f00258017000000000000000e2014c009f0824c13970024c019d01e44009d0226c209d9827c009f0027c009
b0027c009f0027a8050000000000000004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (08c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00a9002b408ed003b404e90118404ed003b400ed00380008000000000000000420544006d003841de1016b4a961037ac0821032b485ed223b401e11158409ed017b405ed0039881500000000000000042008c017f107cc09d7026fc04d71474c81b3026ac01ff007fc09fb0058c09cf0277c09df
007fa00200000000000000062043c005f0037c20df0007c00d71831c00978827c80d70037c00df0017c00cf0037c00df0035b81000000000000000004047c016f0078c01f3405cd01a7107ac01a7807bca1ef007bc01ef0059421ed007b401ed00781015000000000000000220074006d0038400e180a840245087
e400e91071400ed003b600ed0018401ed0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (08e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (02174005d00354801140f44525b0037403110037400dd0037400dd0017480dd1037400dd00362001000000000000000c20174007f003cc52f3025cc05a2043fc0033017bc00ff003dc00ff001fc00fe003fc00ff103f0801000000000000000c0027c005f0036c001f00a7e015f2036c00970137
c00df0037c00df2017c00df0037400df0037000900000000000000062050c005f0035c03d70037e039700394009b0437c00df0037440db0014d00df0037c00df0035a814000000000000000420185004d00314021142034128100b36000900e3400cd0033400c10010400cd8033400cd0033281600000000000000
0400604006d003940425000b400a5413d4) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0900) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (077401dd08771901000000000000000e000fc01ff007fc01f3530ec638f0271609b31206c803a204c400334274d08ff007fc01ff007fa003000000000000000e2017c006f003fc003f0235c4cbb003bc002f483fc48df003fc00df0517c00ff003fc00ff003f3005000000000000000ac007c005
f1034c04030112d04970737c00130037c00df0037814dd1597c34df0137c14df003630010000000000000000a0434c04d003141101102240c0d4937400010033440cd0033404cd0913444cda533404cd00302010000000000000000200074005d0034400d10422440950037431910037600dd1037400dd0017400d
d0037400dd0034a0010000000000000008) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0920) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00d33087c225f1027c04b30287c00df0037c00df0035080300000000000000060015c00ff003fc00ff2086c003f003fc10fb5816d022f000e4803f002fc80ff003fc00ff003d8005000000000000000e220bc00df0037c00d20007c011f017440b570047c105b0441c011320e0c00df0037c40df
1037a8820000000000000004001f400dd0037400d404254011d0075402d501054001100654030100f4400dd8037400dd0035200700000000000000040053400cd0033400c188234200d2130400d52003680098505510010014408cd0033400cd00310010000000000000000c6405c21dd0077401d503854249d382
7c04d10114414112004404110031442dd1) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0940) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (200bc00ff003fc00f30037c0077001d440e5010fc805f9237c001f1227c50ff003fc20fe003da8020000000000000008405bc00cf0033c00cf0031e010f0473e00cb41c3c448da013c400341634a0cf0033c08cf003210160000000000000008201b401ed007b401ed8458421b9017e651f9007b
4012d806b40161016b401e5107b401ed007a08060000000000000008001f400cd0033400cd00110129d2073601c940274128d0103000410123400cd0033400cd003220030000000000000002004f400dd0037400db0294024110034c02c100274009d0027442110027428e70037400dd0834801300000000000000
04200fc00df0037c00d30001c00170c35c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0960) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (007c001f00058012000000000000000e201fc005f8017c005b001fc9273409cc0173601cc017d101ccc27f00ddc005f0017c005f0017a8070000000000000004004b400cd0033400c1a0334240114b3406c90670404cd00b24020d0ae1500cd0033400cd0031201200000000000000040003401e
d007b401e108cb601212078601f16058511ed08790010d2049405cd007b401ed007900000000000000000004604f400ed003b400e1402948023a03ac20e100304003d002ac006d0828405ed003b400ed0039181700000000000000040043c00df0037c00db1004c001b0037820d30024c00df00244007f0024c21d
f0037c00df003520140000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0980) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (001f0105c441da0044041f0007c041f0007c001f0006b01e0000000000000000a0534008d00234008d4522400910825600950d204348d10205148d10334148d10234008d00202814000000000000000200734009d002740095012448a9504244109d10a14069d01a44069d00274029d00274009d
0024a01c000000000000000800074009d00274009b01e6c038100214088100a44029d00244009d10a74039d00274009d0026200100000000000000042043c009f0027c00910020c01972024c00990265c419f1064c019f0427c089f0027c009f002508100000000000000006004bc001f0007c001f0105c0217008
684a170007c000f01870120f00860001f0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (09a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00634009d0027400900126408bd82be600a901ab602a10228404b180284008d10274009d002520180000000000000004004b4008d0023400818821410ad212b414a9032a680a18028412a104284108d00234008d00210012000000000000000c60734001d00074001140c2c253d0144605194544
5091304404011100445011d00074001d0007101c000000000000000e0063c009f0027c009204ecc009f0235d20832164909930024c21930024c11bf0027c009f0027a018000000000000000e2067c009f0027c009b053fc14af052fc14ab052fd94bf053fc14bf052fc549e0027c009f0027a81900000000000000
0ac07bc001f0007c00171100c00170800c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (09c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (03b400ed103a080100000000000000080053400cd0033420c50376504cd0070601c10072601c10033489d120334008d20334a0cd00322014000000000000000200534005d00174005b00dc801712015c215100940085104546805100576115d00174005d0014a01400000000000000042043c001
f0007c401b0084caa330006c00130084c021b0105c02134007e801f0007c001f000508100000000000000006004fc009f0027c009f0027c209fb865c04970464c04970027d809f1027c009f0027c009f00258013000000000000000e2017c009f0027c00914025c078f0027411931826c019140a4c309341a4c009
f0027c009f0027a8050000000000000004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (09e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (08610509414c10208408ad00284002d013b400ed0039000000000000000000046057400ed003b401e5015c405ed0058410b140e840520205c6057d0148400ad117b405ed0039181500000000000000040003c01ff007fc89d2004ec01df1264c01b30264c01bb227cca9ff026ec01bf0277809df
087d210000000000000000062043c00df0037c00db0017c00d30015c009c0015c00570035e00c70017c205f0837c00df0035a81000000000000000084047c01ef007b801e7106ac01ff407cc0163405ed0171887b641e3207f4016f007bc01ef007a001100000000000000082007400ed003b000ed0038400ed00d
b430f100ba402e1001a40079041b480ad0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0a00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0217400dd0037440d10484004c140454121100e44001302744035106044185d1037400dd0036208500000000000000042213c00ff003fc00f300acc02f3225ec00730025c083b003cc1373045ec01ef203fc00ff003d088400000000000000060007e80df0037c00d70607c029f06a5f225f0032
004c72007c801f30a5c025f0037c00df00358001000000000000000e2057c00df0037400db1096c019f00b2d01c308f5d01d34024d809f0830d20df0837c00df0037a81500000000000000040013440cd0033400cd00104418d00124128104414024104844208d00004000d0033400cd0031200400000000000000
040403400ed003b404e9012a415bd002a4) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0a20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0c7401dc00770001000000000000000e000fc01f3003fc00330054c81a3000fc01fb002ec001b0006c01df0857c0123050f821ff007fb003000000000000000e2017c40ff003fc00ff0007c0caf500fc003f000fc08170207c081f0307c007f003fc08ff003fa805000000000000000ac003c00d
f1037c44d34124c08930b86c00534405ca0934104c00134016c80cf0137c00dd0036b0000000000000000000a043400cd2033410c134004000154254401121904440101004040109a44404d1433404cd0030281000000000000000020005400dd0037400d10000420110026400910a15480910024530810036400d
d0037400dd0034a0010000000000000008) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0a40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (08df0186c069b0082c00df04b6c40930103c00df003508030000000000000004021fc00ff603fc80bb027fc00b80047c00f7002bd24a6004fc00ff003fc00bf027fc00ff003d800700000000000000042003c00d30037c03134034c00970057c00db0066d039b4606c00df0067c019340c7c00df
0037a8000000000000000006200f480d10837401d51415521950ab7400dd0444410590007400dd0297421110037480dd0035a803000000000000000e8043400c1003340041001440085c033400c90003400011003000cd2003420010003420cc2033a010000000000000000c2007401d1003748195005540091200
7421d50064400554007001dd2047401100) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0a60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (600bc00ff003fc20ff002fc00b3003fc00f3c039c00f7019fc80ff002fc08ff023fc08ff003da8020000000000000000404bc00c3003780d4f0271c058f0073c00c39040c1dc54057c09cf0452e9d830173c05cf003000120000000000000002021b401e1007b405a50858405bd116b601e50068
589c1825b401ed0178505a10143405ed00788006000000000000000a001f400c100374000900905239c6622407c120a0501c50193400cd00c2412810003400cd0032a0070000000000000000004f400d1003f40a9703a04039000b7402d101c4402d10407480dd20e44409108b7400dc0034a01300000000000000
04200fc00d34037c225f00b5c0c934033c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0a80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (487c001f000700160000000000000006205fc005f0017c427f3198c2057401cc0053015fc86770017c0059009fc027f01dfc005f0015a813000000000000000c204b400cd0033412cd00a1401d100b4580c13033500c50273400cd01f3403cd0073400cd003228120000000000000004000f401e
d027b421ed2079403a19078401e10043401e5205b401ed046b401ad007b401ed007900030000000000000006204f400ed013b4006d0039400b12038400e14838480b1003b400ed202b400ed003b400ed80398813000000000000000e0057c20df2037c001f0034c00970015c21cb082c400970087c00da0037c009
f0037c00df0037a0150000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0aa0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00534105c04130103c40112004c00154107c001f0004301c000000000000000400434008d0123414810024400c94523400890521414810523400850034400c595234008d00202010000000000000000000634009d0027400d108a4080954827400910025604914127620910024504d500374009d
0024a018000000000000000800074009d20245129100244829b00274019b21a44309100674009500a04018101274009d00262001000000000000000c2043c009e0024800831024c009300a7405930921c00831037c00930024c10910023c009f00270810000000000000000c004bc001f0007c021d0107c021f048
6c021f0084c501b0043c001f0087c081f0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ac0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (20634009100254019d0024000914864400950134400d500374009500244209140274009d0025a818000000000000000e80434008104a14038d00204248184624808d08216908101234008da0264008110234008d0023a810000000000000000c00734001101445021d0004404110984400110084
4061540874001300044001100074001d0007001c000000000000000e0063c20936064c04ff002ec02a1053ec40bb252c814b34623c009b002ec80a3002bc009f0027a018000000000000000e6067c009f0224c00bf202fc34bf052bc009d003ec14bf6527c009f102fc00bb002fc809f0027b03900000000000000
084073c001f2287c04134004d00170117c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ae0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (02b400ed00388004000000000000000a0053400cd0030403cd0021441c108f1401c10032001512877400cd0870502490023400cd0032a014000000000000000200134005d00140027d041c48373001f4117120dcd007104974005c009840261041b4805d0014201000000000000000042153c001
f0004c001f0405c10131c05e201f0084c00130907c001f0104c00190007c001f0005081000000000000000040157c009f2022c108f0127d239f4023c009b0422d249f4037c00930127c109f1427c009f0025001500000000000000042117c00930025c029f01a4c80830026c008b40a5c81910227c009f0026c099
306e7c009f002528050000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0b00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00610208644ed022b400e9019b000e5293b400ed0039000000000000000000062057400ed003b410c1221850f9301e4420210140488fb241f408e101eb444c186b3400cd00398015000000000000000e000bc01ff047fc01f30258c059b4274c01f30244c0d7300ffc01fb0873c81f7035fc01ff
007fb00200000000000000062043c00df0037c005f0016c001f1807c005f0025e00df41a7c00dd00178009f4827c00df0035a81000000000000000006053c01ef0178d01ef0849c81e30051c016f404ac81f3807bc81ed0058c01eb006b401ef0078001400000000000000022013400ed0138602cd8019410b140a
b400210420610e1133b420ed0098400f10) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0b20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (020f400dd0034519512050401412085c04530084401550087480dd00576019180e7480dd00362081000000000000000c2203c00ff003cc2063001cc0273001fc04730001c2073001fc00ff001ee40b3802bc00ff003f08a0000000000000000c0007c00de0037400da08d7c40df24238001f00c7
d8a490897c00df0097c02d70427c00df0037000100000000000000062053c00df003fc02574054c80d31175c005360d4c005d0a9fc00db0897cb1d70827c00df0035a834000000000000000c201b400cd00334014500104210128804404101804008d0087400c112434408120f3400cd0033280600000000000000
040003400ed003b402e5021849c2103095) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0b40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (437401dd00770101000000000000000e000fc01ff007fc01d3004cc03839060883370044c413b80ccc003300efc039b0067c01df007f9003000000000000000e4017c00ff003fcc43f111fc487f110dc0027210dc843f050fc00ff010fc00bf082bc04ff003fa80500000000000000084003c00d
f0034c00930214c2a530187c20122305c08130087c02df02074029140a7c02df0034000000000000000000000043600cd0030428815014484d14ca1400006402400450013602cd0403408c12223402cd0030201000000000000000000007400dd10344009900d5400d10047420110005481518017440dd00474a3d
00867400dd0036a0010000000000000008) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0b60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (20df0227c28134026c00d700b7c00db0027e00df0035000700000000000000062017c00ff003fc00ff812fc01ba002dc0036003cc003f216f080ff002fc00f7023fc00ff203d0081000000000000000e0003c00df0037c00d3c0c44019444e38011d08e5c931d00a4c85d34127c80db0027c00df
103520800000000000000006200f400dd0037400d10015408950074501410051501152814541910007400d10037400dd00350003000000000000000e8043400cd0033400c11400484952437400cd10016040d1130414918123404890023400cd00310010000000000000000c0007401dd0077401d1010548091012
4c041304144141f1105404910027400d31) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0b80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (400bc00ff003fc00ff0038c089b0237c087f0017c0867021cc00bd0023c00f7023fc20ff003d2802000000000000000060cbc00cf063380cc70161c04c70153c60cf0bd1d058b01f4c0d8d0063c01830377409cf003000120000000000000000001b401ec007b001e1027d405bd407f4116d025b
441310249429e90b6f405e1017b405ec007800820000000000000000008f400cd0033420c500014139500134014d81114019900114068d00a7480810037400cd003020430000000000000002004f420dd0037400d110304029b02a740a1d0067c00110025c13cb83b740dd14037400dd0034281700000000000000
04200fc00df0037c00d700b7c289308b78) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ba0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (007c001f000500120000000000000004205fc005f0017c005b001ec007b041e40077085c4007300d8c007581df4105f0015c005f00152003000000000000000c205b400cd0033400c108304008908e1600452050001012080483911033401cd0037400cd0031201200000000000000042013401e
d007b401e9087e481b9007a401f50c58491a1807840385807f401ed0079401ed007900000000000000000006084fc00ed003b400e34038080a1003fc0061401c400210008c00e1002b000ed003b400ed00391013000000000000000e2043c80df0037c80d30056c01930074c01530814c00db0016d40970027c00d
f0035c00df003520100000000000000004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0bc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00130017d00034002804130004400110007c001f0007381b000000000000000080434008d00234008d00234018d80234008900254009180261148140205008500234408d00200010000000000000000200634009d00274009d00374009d022760291022740a9102a64069100204028120274009d
0024a018000000000000000000074009d00a74009d08274099d0025c029b00e15038118a45839108244029100274009d0024200100000000000000042043c009f00a7c009f0027c019f0065e889308264019b0424c01930524c0093e027c809f0025001000000000000000040049c001f0087c001f0407c0817048
7c081b1106c00170287c301f8007c001c0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0be0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (20634009d00274009d2027421b10028444a10128488a12438440a1082c4008520274009d0025281c0000000000000004804b4008d00214008d0023444a14428410a10128414a10128404a105284148d00234008d00212016000000000000000c00634001d00074001d0557481310140505510044
50111004450b1310445011705474001d0007081800000000000000068073c009d002fc009f003f8029b00248809200a6e00830224c09930024c00bf0027c009f00272019000000000000000e2077c009e0027c009f052bc14af052dc94af252fc54bf052dc14bd9d2bc14bb052fc009f1027b81900000000000000
0e8073c001f0017c001f0007c001f0817c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0c00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (03b400ed00380004000000000000000a0043400c50123400c50020481c10070520c10030402c10073409c940b44008d0033400cd083221100000000000000002004340051019f400510814400513054440510015c025100174005100954605d00174005d0814200000000000000000042053c001
70007800170084c00318004c02130006c04110987c06130884c001f0007c001f000500100000000000000004205fc009f0027c009f0167c009f0167c209f1065c019f4227c08970567c00970827c409f0025001300000000000000040017c009f0025c009f00a7c00930024c029340244409100a4c07934124c009
f0027c009f002520050000000000000004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0c20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0865023d640fc04184c0a9001840871003f000ed0039000800000000000000040057400ed002b400e53a2450df1006e400e1004fc808c03204a0010142c00ab203b400ed003900950000000000000004001bc01ff006fc09f3006cc41f9106ec01f7027dc01eb126cc09f3025cc01f3047fc09ff
007d300200000000000000064043c00df0023c00df1027e005f4017c409f0035c201f0037c00571023c000f0037c00df1035381000000000000000006053c01e7006bc01e7086ce01712078c0173007cc8163407fc016b0078c012f007b441ef2078101400000000000000020013400e1006b400e10268503e1043
8420e10009400b100bb440a9002d402ad0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0c40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0a07400dd0c67400d100245801160815021d0884d001100e15005906c741b5d0037400dd08342983000000000000000c2203c00ff002fc00f2002cc4033046c4227f208ec0337012cc007f046fc01ff003fc00ff083d0081000000000000000c2017c80df0027c00df2027c00930096c0a1f0005
c20df2097cc0970097c025f0037c00df0035000900000000000000060053c00df0027c20d301e8c118340d7409971835010df0094d0dcb40b4c11d3047fc00df003520100000000000000004200b400cd0023400c401e04010100930229102334079d3450400090082600090033400cd0033201200000000000000
040003400ed002b600e1002846521043b4) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0c60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0444011d00770801000000000000000e000fc01ff000cc0127002ccc07b002cc012b004ac00bb100fc8033286dd003f004dc013f007fa003000000000000000e6097c80ff001fc14fb002cc0c1f0207c003f02058003d000fc003b0307c046f043bc04ff003fa80100000000000000086003c00d
e0007802d742a7c00170225c005f0284e48170204c028f0323c00df003744adf00360001000000000000000000c3400cd0023400c50023408d180044000901024004100054081981134084d1833400cd00300010000000000000000a0007440dd1867400d50027404d506054109d00b4430552004400dd8037400d
d0037400dd083420010000000000000008) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0c80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00570206c025f0004d021b22b4e02af0227e029f0035080300000000000000060017c00ff000fc303e808fc827c006fc037b001fc80970017c003f400fc089f002fc80bf003d8805000000000000000e2083c00df0044e03070025c205b0064c035b0042c039a0043c011320e5c029f04c5c011f
0037a0000000000000000006200f400dd0474403190095400518a204401500445015900474231180504009d00446011d0835a803000000000000000e804f400cd00004201d00314414920204201908404004980034000104315008d00016000d0033a010000000000000000c200f401dd200450119200548071002
44211500444219100074011101044003c0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ca0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (600bc20ff023fc08df921dc02171027404fe0007c00f7000dda8bf223fc41db0037c00df003d38020000000000000000404bc08c30304c688f0812d11072166c04c70042c00cf0100e488b0170440cf20334028f003010120000000000000002003f401e104584197d085a40101896a40d71034a
401a10c4a5098d0148501ed00eb403ad00780006000000000000000a001f400c000404010c08124c00500624264d81824a18901c140089a020400cd00034210d003020030000000000000002004f400d040545015c001410b4100b6c06418056c0f0108744801d02e44009908e74538d0034a01300000000000000
04202fc20d30494c001f04a4c005f0334c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0cc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (207c021f000708120000000000000006205fc005f00dcd017b405cc90630056d0175005cc0073209cd027b00dee017b009bc0e7f00152037000000000000000c204b440cd04f0403c90054405c51033440c106b1402c104b4411c90230510c10033422cd0033281600000000000000040007401e
d8478481a914584012140fa403e5105c40161505861178007a451e9007f441ed007908040000000000000006204f400ed0018480a10818500f5103d400611019400a1001c400e1400c400f3403b400ed10398013000000000000000e0057c00df0014c81930014c40130064c01470044c40930014c00130026c009
38005c005f0037a0100000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ce0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (001f0004c24114104c04130005c045700074001f0005201c000000000000000080434008d0523000c945215949d15236008d00304148125314349580204148500234008d00202010000000000000000200634009d00274089181a54109d0d24600dd0024400d10024400910031400d585274419d
0024a018000000000000000800074009d00274029b00644029d00e74009d0ae4c058100654008143e44038120676059d00262001000000000000000c2043c009f00a7c809300244009f0027c099f0024d14931164c00972425c08970467e009f00250810000000000000000c004bc001f0007c0e170087c021f288
4c001f108784a1f2287c00170007c021f2) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0d00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (2063400990924500910125400d502234109500254c0d100247009106244009d002740a9d00252818000000000000000e804b4008101a04009105204148d0423400818021602c115205008900264129d00230808d0021a012000000000000000c20734001b00844005100854a2130107400152005
44011029450a1100044045da0074001d00070018000000000000000e0063c009300acc00a3042cc10bb0c2ec00b3802dc00b3002cc00ab002a800be002fc00bf0027a01c000000000000000e6067c009f052ec00af052ec14bf252fc00bf0039400ed052fc00a9052fc14bb003bc00bf0027a81d00000000000000
0ac073c001f0117c00130101c041f0105c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0d20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01b4006d00388004000000000000000a0053400c10070400c15871503d506b2401c10cf2400c902b3440c50071401cd00f3410cd0032a01000000000000000028053400550b5fe0261029ec2271289f0137104d8c007d225c40051109c44c6d041f4117d0014201000000000000000042053c001
30084c1a130805c40134007c021f0084c031f0805e00070105c021f0187c021f000508140000000000000006005fc009f0063c019f0023c10930066c109f00a7c038f4023d029f0067c819f1267c009f0025081700000000000000042017c00930424c09934024c009e4066c02912065c02930824c019b00e2c0a9
d00e7c009f002520050000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0d40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (002d01194542d010b408e9021d404ad1589408250039000000000000000000062057400e100084052b156940dc10be34802d034040d2d0758435e10160405ed034b4072d00391015000000000000000e000bc01f3005cc01a30060c89b7017fc893d105dc051f0056c09cb0275c09ff006dc01b7
007d280600000000000000066043c00df0037c005b0037e00db4027c40164013c001d0005800df0037e00df0007c001f0035b01000000000000000004053c01e3007c001634079c01e7086bc81a3005a501af004b401e70079c01cf107b401ef0078181400000000000000020013400e5001b0007500b2502c5003
340021a01c4400d001a480f180bc400ed8) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0d60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0007400dd0044400512c354025b00174871d0344483110004500db0847c73cd14c74811d00360081000000000000000c2203c40ff0004c4973417cc03f10077c0035140cc0801000cc00f780edc00df083fc803f003f0880000000000000000c0007c00df8097d02df0405ca85f08b7c001f0295
c021f0c17c10cf2017c409f2007c105f0037000500000000000000062053c00d343b4c04c300e4d80d70077c401f0095c099f10d6d81db0cf58119f1065c04970035a814000000000000000c201b400c100c0401090073400d112274200d00804010d0884400c101440018c08434010d0031200200000000000000
040003400e1001840471023c406a5032b4) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0d80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000800020000000000000000000000000000850021400850021400850021400850021400850021400850021400850021400850021400000000000000000000e6017c00ff000fc001f201fc085b1197c003e0107c403b000fc42ff000bc009f0007c081f003fb00500000000000000084003c00d
f0005c54530514c02c74117c00170504c14170504c00d50585c049f0007c041f0036180000000000000000000043400cd00000040141015024d0a334000d0300724054100404c101834500d14036840d00300010000000000000000a0007400dd00d5410d100004005502374011d10144001500d4400d504354011
d00474019d003680010000000000000008) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0da0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0400010000400010000400010000400010000400010000000000000000000000000000100004000100004000100004000100004000100004000100004000100004000100004000000000000000000000000000400010000400010000400010000400010000400010000400010000400010000400
010000000000000000000000000008000200008000200008000200008000200008000200008000200008000200008000200000000000000000000000000008400210008400210008400210008400210008400210008400210008400210008400210000000000000000000000000008000200008000200008000200
0080002000080002000080002000080002) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0dc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (20033800ce0033800ce0033800ce0033800ce0033800ce0033800ce0033800ce0033800ce000080000000000000000000000084002100084002100084002100084002100084002100084002100084002100084002100000000000000000000000000080002000080002000080002000080002000
080002000080002000080002000080002000000000000000000000000000085002140085002140085002140085002140085002140085002140085002140085002140000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000040001000040001000040001000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0de0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000003c3c000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000420800000000000000000000000000000000000000000000000000000000000000000000000010820000000000000000000000040
001000040001000040001000040001000040001000040001000040001000040001000000000000000000000000000010000400010000400010000400010000400010000400010000400010000400010000400000000000000000000000000840021000840021000840021000840021000840021000840021000840
0210008400210000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0e00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (fffffffc0000000003fffffffc0000000003fffffffc0000000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000f0f000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0e20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00000850021400850021400850021400850021400850021400850021400850021400850021400000000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000000000000000000000000000003fffffffc0000000003fffffffc
0000000003fffffffc0000000003fffffffc0000000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc000000000000000000
0000000000000003fffffffc0000000003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0e40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1000040001000000000000000000000000000010000400010000400010000400010000400010000400010000400010000400010000400000000000000000000000000040001000040001000040001000040001000040001000040001000040001000040001000000000000000000000000000800
020000800020000800020000800020000800020000800020000800020000800020000000000000000000000000000840021000840021000840021000840021000840021000840021000840021000840021000000000000000000000000000800020000800020000800020000800020000800020000800020000800
0200008000200000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0e60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (800ce0033800ce0033800ce0033800ce0033800ce00008000000000000000000000008400210008400210008400210008400210008400210008400210008400210008400210000000000000000000000000008000200008000200008000200008000200008000200008000200008000200008000
200000000000000000000000000008500214008500214008500214008500214008500214008500214008500214008500214000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000400010000400010000400010
0004000100004000100004000100004000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0e80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000042080000000000000000000000000000000000000000000000000000000000000000000000001082000000000000000000000004000100004000100004000100004000100
004000100004000100004000100004000100000000000000000000000000001000040001000040001000040001000040001000040001000040001000040001000040000000000000000000000000084002100084002100084002100084002100084002100084002100084002100084002100000000000000000000
0020033800ce0033800ce0033800ce0033) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ea0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0003fffffffc0000000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000f0f00000000000000000000000000000000000000000000000000000000000
000000000000003c3c0000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ec0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (003b004cc24ff004dc4133087fc01af007fc01ff007fa043000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003ffff
fffc0000000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000000000000000000000000000003fffffffc00000000
03fffffffc0000000003fffffffc000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ee0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (2217c00ff803fc00ff067ec00f74c77c813f003fd10cf021fc80ff182fc48bf003fc00ff003d800500000000000000000403c00df0034c00df00e5c00c34285c120a0075c00df2005c019304e3c019f0037c00df0037a880000000000000000aa00f400dd0035400dd0005400dd08a5444510045
400dd0434604950077400dd0037400dd0035200700000000000000068053420cd0030410cd0001400c10101420c90801400cd0001400011037400cd1033400cd00310050000000000000000c0007401dd0075404dd0214009d70635401110045408dd0044400d500574019d0077401dd0077180100000000000000
0e000fc01ff007cc01ff020cc04f3110c4) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0f00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (037800df003da8000000000000000000604b400cf0033c10c304b7404c711435048f0151d00cb2012c404d0162400cd0233c00cf0032101200000000000000020019401ed007b401e1805b44de9025a40d0d0158401e9b86e4497d104b401f5007b401ed007a08060000000000000000000f400c
d0033401d100c3412c510034000d0051421c948024075d0222400cd0033480c9003220030000000000000000004fc80dd003740ad10007600fb40e6c185b1140405f103b45049d006540adf8037480dd003480130000000000000004200fc00df0037c00d34087c00d70201c02db0014c00d71024c001b0024c00d
f0037c00df003508030000000000000004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0f20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (4573009cd005300dc40a7b635e4005f0017c005f0017a806000000000000000c204b400cd0033400c90030400c10070643c900d2400d901f050a012863400cd0033400cd0031201600000000000000040003401ed007b401e9087a485c500f8481a118d8405c1003840129006f401ed007b401ed
007900000000000000000006005f400ed003b400e10030464e1501c420eb1038402e10038400f1000b400ed003b400ed08391811000000000000000e0043c00df0037c00d32066c00f30007e00030070c00d30030841930062c00d70037c00df003520140000000000000006e00bc00fe003f800df023fc10df020
7c043b1213c08f72039c006e012dc08df2) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0f40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (20434008d00224008d8522414896522414cd88206148d00234808d00234008d00234008d00202814000000000000000000634009d00274109909240009100214409d80254029d8427402dd01270009d00274009d0024a01c000000000000000880074009d00264029d8066c019b08e7c0b9d0064
4229d00a74019d08674049d00274009d0026200000000000000000042043c009f00274009b0024c04830227c008f0e24d04960027c089f0027c409f0027c009f002508100000000000000004204bc001f0007c00170007c001f0485c301f0005c00170287c001f0007c001f0007c001f0005801200000000000000
0c005fc005f0017c0053529ec005380ddd) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0f60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0274009d102520180000000000000004004b4008d10204049101f16028564234008120244228900240108d00634008d00234008d00210012000000000000000c00634001d00044051141474021501c34021500145071110044451d00074001c00074001d0007181c000000000000000e0077c009
f0024c02b301efc01b3056fc31bb002cc89bb102e800af002f800bf002ec009f0027a019000000000000000e2077c009f0026c149f052fc0097052fc00bf102fd349f202fc14bf002fc00bf2027c009f0027a81800000000000000086077c001f0007c40190104c04130115d041f0004c041700074c01d00074a01
f0007c001f0006b01f0000000000000004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0f80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01cd00224070d00b14034d08234108d0033400cd08322014000000000000000000034005d00174017f081ec287100df41a790017c807d121c4087d10574417d00174005d0014a01400000000000000042053c001f0007c001f8046c001b0405c021f0007c001f0085c021f0007c001f0007e201f
000508100000000000000004205fc009f0027c009f0027c009d0067c059f02674809f08e7c449f0827c029f0027c009f00258013000000000000000e8117c009f0024c40930027c00970467c039b0020e009b0162d108e20a7c019f0026c009f0027a805000000000000000420634009d002450091806242095092
34309510244008108244409d00274009d2) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0fa0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (2057400ed003840d2f1448409030433618eb056050dad016844bbd026040da1017b405ed003910950000000000000004001bc09ff007cc01bf0274c25af807fc09f3086ec01df0076d015c1a64c01a3027bc09ff007d200200000000000000066043c00de1037c00df0027e201f0007c009ba035
c805f1807e001f0027c009f0037c00df0035a81000000000000000046053c01ef007bc41ed0868c612ba079c01ef006ac016d80794412f187bc01af007b401ef007a101100000000000000020013400ed003b47065083a40341280b600e9802b0022d0028402bd142b410ad003b400ed003a080100000000000000
0a0043400cd0033601dd90304034902314) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0fc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (037480dd00362085000000000000000c2207c00ff003f40073100bc0037804dc04f2002ec09af002fc11ff043cc00bf003fc00ff103d0805000000000000000c2017c40df0035c021f0017c405b4487c825f0027c001f0025c02df0037c009f0037c00df1035800900000000000000060073c00d
f0036d00dd0054d005300c7442d12062c009f20a6c00df0034500134037c00df0037a8140000000000000000204b400cd00324008500406000100874840900704004d84c04000d80a0680810033400cd0031201600000000000000040123480ed003a400ad0338400a1020340061812c4846d05394342d0138404a
1003b400ed003900080000000000000004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0fe0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (012b3046c2133405bc0133004dc041f1a47c01df007fa003000000000000000ea017c00fe003fc021f000fc441f100de203b04338003f000fc023f01afc00df0237c08df003fb805000000000000000a400fc80df0037c04430137c44954007c80130026c008f2007e201f12b4404dd1037c04df
0036b8010000000000000000a043480cd2032404018543418010a334200d14205500d0c434008d01214104d0933404cd0030201000000000000000000007400dd0037406d11037400950437402910026400dd20474041d10644815d0037480dd0034a0010000000000000008020f400dd203740211000740011028
5c011b00344131d0047081dd00356078d8) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1000) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0013c00ff002fc00ff40fe400330021c0033000f800bb00dec007b000fc01ff00afc80ff003d8005000000000000000e0003c00df0027c00d20cf5c01174066d011700c4c23070055c00130045c2b9f0007c00df0037a80000000000000000060007440dd0037400d440176031d04664011d0045
0069500054305500404105d8037480dd00358003000000000000000e804f400cd0423400c120014201500226000520004001500016005124410000d0003400cd0033a010000000000000000c200f401dd0137401d50016c00030864401112045c0001105446151210440b1d0107401dd0077180100000000000000
0e200fc01ff006fc01d3000cc21132024c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1020) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (23f408ff003da8020000000000000000404bc08cf0023c05c70247c050b0863c820b8141c018340405054d2053c01cd0163411cf003210120000000000000002007f401ed007b405e5414b40529006a04135034b70125085d605ed804b401ad315b681ed007a0806000000000000000a201f400c
c0023440c500425000820030060910414400400104020d01434058d0443600cd003220030000000000000002004b400dd0027400d10497c040b1024000060042c409400214014f0407411cd0177001dd0034a0130000000000000004002fc00df0027c00d70111c101300a5c021b0204c2013002640c5f0007c009
f1017c00df003508030000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1040) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (057e08ddc207b041dc00730a5fc5277035fc005f0015a817000000000000000c204b400cd0023400cd00f1410c546b3401cd01b1412c901f0480c102f3480c100b7400cd0033201600000000000000040007401ed006b401ed007a6013520794012d9449441e9207d40161104f661e5807f401ed
007800840000000000000006204f400ed002b440ed003948021103bc00210809400b10818520e1400b400e1003b400ed00399813000000000000000e0057c00df0027c00df0036c00130837c001310048419b0050c01170047c00d70033c00df0037a0100000000000000006600bc00ff003fc08fb081cc285f103
50003f0806d00fb000cc88e50917c80ff1) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1060) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (80434008100274008185224009105234008180274008d00234008d00234148540234208d002028140000000000000002006340091002740091c4244429100254349500374009d30274019d02254009400b74089d0024a01c00000000000000080007400910023400912066c03910023442950823
4009d00274839d01e74009102274009d00262001000000000000000c2043c00934027c00930160c44930167c00920167c409f10274209f0067c00910067c219f00250810000000000000000c0043c001f0007c001f1087c00190085e041260079a0171007c421800074901f1007c001f0007801200000000000000
062057c005f0457c005f065ec0267005dc) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1080) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1344009d00252018000000000000000e804b4008144234208111225008920204008110224249d08234208108234008100244008d00212012000000000000000c2073400110147400112285400032084400114004c044d00070001110074001108005001d0005181c000000000000000e0063c009
30027c0093422ed08bb042ed20a7002c442df202fc00b3002fc00b3002cd00bf00278019000000000000000e6067c009f052fc009f052fc14af402bc00fd402bc14bf082fc00ae052bc00bb1d3fc009f1027a819000000000000000ac073c00130007c40134104800130915c00170017c001f10070005f0007c045
70007c001f0006b01d0000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (10a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (02cc8032400c94033641c102b0513c9c2f3401cd0832a014000000000000000000534005d00174205b001ec0f7d00d844076005d480410015c00714a1c4077100df4007d0814a00400000000000000042053c001f0007c00134004c821f0885c1a1f0006c00130007c00130004c00170487c001f
000508100000000000000004005fc009f0027c009e00a7c00970267c009b0266c009f0067ca19f0227c209f0027c009f0025801300000000000000042017c00930027c00930026c429b1064c00810062d009f26274209140e7c099300a0c008f0027a905000000000000000620634009100274009100a150ad1242
46019100a44089d00264089100a3400914) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (10c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (2057400ed003b400e10630401e10a6b406210368430dd03334000d01604106d013b400ed00391815000000000000000e000bc01ff007fc09f3007cc09e3426f40130006c911ff027fc09bf027cc012f007fc01bf007d200300000000000000064043c00df0037c00df2037c001f0025c001f0807
c02d70031c801d1037c40540007ca0df0035a81000000000000000004053c01ef007bc01e3006cd01af2069c412f004ac0de9007b40123007cc01e9007bc01af0078101100000000000000020013400ed003b400e9403a400ad04384007500a8444e9287f402210038401c9003b402ad0038880100000000000000
0a0053400cd0037440c15430520dd14714) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (10e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0054209d10362085000000000000000c2203c00ff003fc00f1406cc103e002fc003f000cc10ff803fc0073416ec2023123cc02ff083f0907000000000000000c0007c00df0037840df00b7c001f20a7c21170007c80df0037c001f9097d421f0337c80df0037000900000000000000062053c00d
f003fc00d340644835324664091b0085c00fd0037c045f0474c011f00f7c008f0035a856000000000000000c201b400cd0273400c10074501510ce3400090300401dd08334050d24440014d00c74008d2031205600000000000000040003400ed003b440e10008514f1012a400292009400ed003b6802d00184003
d103b400ed003900080000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1100) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (08fb003cc20930004c0103002fc01ff007fc01ff007f8003000000000000000ee017c00ff003fc00fb051fc545f0023c403f0b03d04ff003fc00370187c103f110fc80ff003fa805000000000000000a4003c00df0037c02d74080c86dd13a7c001f0384c4afd00b7462130206c20130284c889f
0036b00100000000000000008043000cd0033482cd1812510cd04036000d0100400cd90b34020901004200140014808d00302810000000000000000a0007400dd0836400d50504400dd20470011d0444400dd0037604110836423190004400dd0034800100000000000000080007400dd0837400db40b6c001d01e
74831d0044580dd00376071b0104401110) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1120) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0607c207f083fc00fb0037c423f0037c00d70037400a61047c08bf0037c00ff003fc00ff003d088500000000000000040200d005b0037c00db00f5d001d2034c40db00344819920d5c211344e3c00d70037c00df003521040000000000000004000c600110037400d500e54021d2034520d10035
411dd0204402d12077400dd0037400dd0035a8030000000000000004004c400090633400c904054401d2030402c92030400c80801040010003400c50033400cd0833a014000000000000000c000c4005101bf401d103255011da074442d32075401150045100111077401dd0077401dc0077000100000000000000
0e440cc217b003fc21fb0024c013f803cc) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1140) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (03fc00ff003d38020000000000000000004bc000f0033c05c30823c95030533c00c70771c0583014140583422340dcf0073c01cf003018160000000000000000006f4016d007b405e100fb501216178401e18278415a5096840d71006b401ed807b401ed007800060000000000000000000f4005
d0033400c12023501000473481d508714108181e1401110823481cd0033400cd003020030000000000000000207f440dd0037400d110f3c0001007cc08f110b8400d101a2c03d10037601dd0037400dd003420130000000000000004001fc00df0033c00d30075c02131035c48d70135c00db4095e4e5301a7c08d
f0037c00df003508030000000000000004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1160) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (805b4014d0371241d4007f021fc005f0017c005f001520170000000000000004004a528c90036400c908b7531c98033400d92030401c10430402cd2273400cd0033400cd0033281200000000000000040002401f90078401e9006c41131827a405e90070401b14059411fd007b021ed007b401ed
007900000000000000000004404c4006101b2c00e1103bd002b0138402e101b8420eb0020000ed082b400ed003b400ed0039801300000000000000040040c01430034c01cb0020c00130036c00d3003cc01830035c21cf0027c00df0037c00df0037a0100000000000000004200bc003f023fc08ff003fe842f403
f040fd003fc08a3021fc08fe002fc00fd2) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1180) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (20434008585234008125604008105206148585234948105234008105334008d00234008d002000100000000000000000006340091802742091002750891422560695c0a74449005354809500274009d00274009d002420180000000000000008800f40095002f4009b00245008104e44009500a7
40191206740a9108a74809d00274009d0024200100000000000000040043c10930027c00939567d00932063c00910023c1093c022c019300a2c099f0027c009f0025081000000000000000040049c00170007c00170007c001f0084c00170087d0a1f4086c321f0087c401f0007c001f0005081200000000000000
0c000ee037b4014c005b099c50173001ec) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (11a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0274009d002528180000000000000006805b4118d05a34208950267409988244108d00205008c08204108110234008d00234008d00210012000000000000000c20634051d08c74001103c3c405100044070d008440a1100842051b02874001d00074001d00070018000000000000000ea067c009
f0167c00b3036ed00ab002cc35bf056ec05bb246cc40b3016fc00bf0027c009f0027801c000000000000000e2067c14bf0527c009f4d2fc00af1023c549d0027c00bf003fc14ff402fc009f0027c409f1027b81d0000000000000008606fc00130107c00110107c00130105c24072907c04510105e00532107c001
f0007c001f0006181c0000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (11c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (05c100716014d0030403c124334008d8033400cd0032a010000000000000000000004005d0017404510019c806b809845075021c40679029ef0a71001b4005d00174005d0014210000000000000000040040d001f2007c00110087d001f2004800132205d061f0002c20130007c001f0007c001f
000508140000000000000004004fc019f0027c009b0427c019f0427d009f0027c048f00a7d249f0067c009f0027c009f0025081700000000000000040017c219f0027c009b01a6c009b00240009f0024d129f20a4401810027c009f0027c009f00252005000000000000000420734249d002740095402760491202
44a0cd00244409100344a09902a74009d0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (11e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (2057404e1003f4008142184058d00004602d0162c88ad2208400b312585408d0033400cd003900150000000000000004000bc01f3007fc09b30069c41cb2274c21bf2064c016f027cc01bf0270c01af007fc01ff087d200600000000000000046053c00cf2037c00df1027c009b20169809c0005
c004b0017c801f0037c00df0037c00df0035a81000000000000000004040c85ef007bc41e34059c01ad2059c01e34079c816f0058501f0007bc81af007bc01ef0079181400000000000000000000409fd003b600e100b9500b50019400650060600fd0418002a00813400ad003b400ed0039880400000000000000
040440400cd0033401c10871400cd82914) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1200) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (037400dd0036208300000000000000040604c00f0003f002b1001ce983b000cc08df002cc0033200fc01b3442fc00bf003fe00ff803f0880000000000000000400a7c80d70033c009f0476e081f2827c021f00a5c121f1107c04df0035c009f0037c00df0037080500000000000000040043c80f
b003fe209300b1c030e0001cc01f10245801d01c4c12d701f2c009e3037c80df0035a0140000000000000004200b400c950334208140814008d00100001c000240a4d08704030108f2480cc1033400cd0031280200000000000000040433480e9003b440a1000d444ad01194086d01284007d0238508a5003e400a
d003b400ed003900000000000000000004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1220) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01b30804c8127000cc04b32046c0833030cc013f007fa003000000000000000e2207c80fb003fc04bb000fc063f0d2fc403f000dc00bf012fc043f022fc14ff013fc34ff003fb8050000000000000008c00cc00d70037c0a97008440e1a2184c005f0e86c0a930227c00130027c029f0237402dd
0034180000000000000000002040500d530334008510954000004205000d01034408910034084101174808d0033400cd0030201000000000000000028004400d500374009500244021994644001d00464019100454085100774009d0037400dd003420010000000000000000020c400c140374209110254031100e
44429d04c5c530b00c3407110167400dd0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1240) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0017c20ff003fc00ff040fc81b70032c00ff000bc003f0802d08af024f440af4c1fd017f003d8005000000000000000e2007c00df0037e40d70407c099b0034c20970044c41170445c02930442c2b1300c4c014f0037a8000000000000000006200f000dd0037400d5112740099401640095a045
411112045410d10004500d101b44345d0035a003000000000000000e804f400cd0033400c100034408900214408500406400588014008100060240000004801d00332010000000000000000c200f401dd0077401d5004740091001e400950045480111044409910044404110b800015d0075180100000000000000
0e000fc01ff007fc01f7104bc01930226c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1260) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (03ed00ef003da0020000000000000000404bc00cf0033c00c30223c1d830362c008f1340e00094103c088d0762c081f0010c008f003210120000000000000002007f401ed107b401ed004f405a98b5b409ad076a62979284b605ed08684212104694016d007a0806000000000000000a001f400c
d0033400c100c34018102a24128c00816801981830018d24c24020d80004000d003220030000000000000002006f400dd0037400db00434019b4037431dd22844871001c741bdd1004419d100344005d2034a0130000000000000004200fc00df0037c20d30207c00930137c009f3004d04130007c02df8086c001
b0020c005f003508030000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1280) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (457300ddc0173089ec53737c5fc637310ddc056f0017a817000000000000000c204b400cd0033400cd00f3401d502f0441c151f1501c122f0423c59033407d10030401cd0033201600000000000000042207401ed007b401ed006b411a51078481a180d944361107a481f1007b403210471401fd
007900840000000000000006044f400ed003b400ed000b400e30030400e10039520611038400e1002b4406140380006d00399813000000000000000e0057c20df0037c00df0007c20934534c00939040c20138052c20c31047c001b4835c000f0037a0100000000000000006400bc00ff003fc00fb0027c00ff021
fc20bf820dc80d58017e0c5e0137880ff0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (12a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (80434008d00234008d00204018125244009d0d215008d052053489002045481c5304009d00202814000000000000000200634009d80274009c80264809101265119d00244008d20a4400990224010d100215009d0024a01c000000000000000800074009d00274009d06a44439100240018d20a5
0089c0aa440499002450a9100244009d00262001000000000000000c2043c009f0027c009f0066c05932024c009f08e4c019f0064c028f0065c019304e5d009f00250810000000000000000c004bc001f0007c001f0007c00110487d001f00874201f6407e321b0087c00170087d001f0005801200000000000000
06201fc005f0017c405f03dfc01572018c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (12c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0240089d00252018000000000000000e804b4008d00234008d00236048120234308d20204049d80224809188217028528200408d00210012000000000000000c207b4001d00074001d00074001140874001d22954001d00844205100144221100044005d0007181c000000000000000e0067c009
f0027c009f002f408b3042dc00bf002cc22bf042e400bb002dc00b7002cc00bf0027a019000000000000000e206fc009f0027c009f002fc14bf452fc14af002fc14bf002fc40b9102bc14bf052f420bf0025a819000000000000000a8077c001f0007c401f0006c00132114c001f01148800f0104c041b0015c041
32105d001f0006301d0000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (12e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00c14070408cd0231413890232400c540b7400cd0832a114000000000000000200134005d001740051401f08375109c4017102ddc807d105c4036d205850371001f4004d0014a20400000000000000042153c001f0007c20130087004130806d01130004d001f0004c081f0044c02130207c001f
100508100000000000000006015fc009f0027c009f0067c219f1023c009e0025d059f1027c209f0027c109f0467d009f00248013000000000000000e2017c009f0027c009f01e7c21932027c009f0024c118e09268609342a5c0b9703e48019f0027a805000000000000000620634009d00274009d012740891002
76209d00674009d1234444910824442811) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1300) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (2057400ed003b401ed0048405350358c24270548401e70248405a0037802df1005840ded00391815000000000000000e010fc01ff027fc01df006dc095b01544216c0344e0dff026cc01b30278c45d70074801cf007d200300000000000000064143c00df0037c00df0023c205f1035c00170005
c40df0006c800c0035c408b1037c00df0035a81000000000000000004057c01ef007bc01e3007bc01630070e01332048c81ff0049d01eb207ac21e7007f401ef1079101100000000000000020017400ed003b400e1044f610e50038491690443440ad0009000ad003a410f5003b400ed1038880100000000000000
0a0453400cd0033400c10473401c103304) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1320) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (004500dd2836218d000000000000000c200fc00ff003fc00f3120fc0036003cc0033000cc007f102c8893f013cc02fb0098c00ff003f0807000000000000000c0027c00df0037c00df0004c029f40a4c02570406410df0285d209f0904002570027c20df083700010000000000000006215bc00d
f8037c80df00d6d859b21f4d115f0060d005d00a6c028300b7d85df21f4c80cf0035a81e000000000000000c211b400cd0033400cd01c24200521e44011510c1500c510024190100c341109c400509cd0031204600000000000000040463400ed083b480ed042a4802900284003d000845ced8b8a40420160f4886
d1020400fd003900080000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1340) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (182b0604d8c3b170e80c336304c0c7f807fc01ff007fa003000000000000000e6417c00ff003fc08ff4007c143b452bc003f030fc02d71206c280f0007d883f108fc20ff003fa005000000000000000ac107c00df0037c00d31107c961700a4c00130b84c204f2125c401f03044001b0004c44dd
0036300100000000000000008143420cd0033404c10443404851402400014100404c501014009d0400400018000410dd0030081000000000000000020007400dd0037040d110074119500f40011980444184d21277109d1034410890434400dd0034a00100000000000000080407400dd0037400d1000340111006
6c13112044401d700c44021d2104403110) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1360) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0017c00ff003fc09bf0036c0123123dc00b340c7c41df027ac117f104fc007f003fc00ff003d8005000000000000000a2200c00df0037c11134023c001b00e6c029700c44801b0817c021116c4c125d0037c00df0037a800000000000000000e200c400dd0037400512035404d90402511150034
404d18425644d100304009d0037400dd0035a00300000000000000040040400cd0033400410033410c91082600458030444098003400810030546cd0033400cd0033a010000000000000000c2004400dd0877489110a6448c1045844861101844aed101a440c5123044021d0077401dd0077180100000000000000
0e000cc00ff007fc2432212ec04170804c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1380) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (03fc00ff003da8020000000000000000404bc00cf0033c00c30033c0d872772c04cb4540d1a830230c02832043c284f0033c00cf003210120000000000000002001b401ed007b40121006b401210242601790248409211a4c4090101534012d007b401ed007a0806000000000000000a001f400d
d00334008100230130510527001800044821102c00020140c34014d0033400cd003220030000000000000002004f400fd0037400910037406d100144021120f4449d170f40825104374108d0037400dd0034a0130000000000000004200fc00df0037c00130027c40d70084c065301b4c021b8496d02030cb7ca2d
f0037c00df003508030000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (13a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (02531895c40573054c02530097c135f0017c005f0017a8170000000000000004204b400dd003040acd8032401c50172602c103f0409c90030402c901b14478d2833400cd0033201600000000000000000003605ed2078401ed806b061e50038480e10071401fd047c701c1086b441ed207b401ed
007900040000000000000004204f402ed0038400cd203b080612030400c100384407b000d480e1003dc00ed003b400ed0039981300000000000000040053c00df0034c01ff0027c00530074c01930035c00570004ea0d34027c00df0037c00df0037a0100000000000000006600bc00ff003fc087f003fc01bf002
dc00f71a0fc08970231c009f2017c803f0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (13c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (80404148d00234148d0d20414a10528494a10528534a14528534a185286148d00234008d00202814000000000000000200604009d00274009d0024400b5002d402b500bc400b182ac404a1802c6029900274009d0024a01c000000000000000800044009d00274009d0024481910124c039100a4
c019300e44029100244039d00274009d00262001000000000000000c2040d009f0027c009f0024c24830020c18970024c69930860c11930164e029f0027c009f00250810000000000000000c004bc001f0007c041f0007c80380085c000f0003c20070007c0a170003c000f0007c001f0005801200000000000000
06201fc005f0014d417f0017c25576954d) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (13e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0274009d00250018000000000000000e804b4008d00204028100a3608a10428400a11528400a10928484b182284088d00234008d00210012000000000000000c207340b1d0004400110007417310044515114044c011141d6c070585d45175d00074001d0007181c000000000000000e0063c039
f0024c0193007fc05930464c11930464c139304e4c17930164c05bf0027c009f0027a019000000000000000e6067c149f0027c00bf082fc349f0525c149e0525c149f2527c549f0527c14bf0027c009f0027a819000000000000000ac078c041f2007c841f2104d04374105c04174104c24130104c045341045041
b00074001d0006b01d0000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1400) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (21c12072402c100f0401d9c0344028d0033400cd0032a014000000000000000000504005d001740051201c420510a14400510014c025102945295b0096c025d00174005d0014a01400000000000000042050c001e0007c8013c004c00330004c22131004c10130004c02130484c101f0007c001f
000508100000000000000004005fc009f0027c008f0027c089f4027c089f0264c008f0027c009f00e7c019f0027c009f00258013000000000000000ea017c009f0024d01934023c5093a0a4c01930024c00930024c10910024c439f0027c009f00278805000000000000000620634009d0024408912227400f100b
8402a108a9502b1012a4a0b5002c4048d8) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1420) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0057400ed003b405ed045a449a90078492ad2178519e1025c405312558c85ed007b401ed00391815000000000000000e050bc01ff007fc09df005fc099f1365481be0264c89f3026cc09b3027cc099f0077c09df027d200200000000000000066143c88df0037c00df0011c00db2037c005f0837
c001f0027c00de0007c005f0037880df0035a81000000000000000084050d05ef007bc01e1405ad01f3407cd0173405ec01c3405cc016b0078c010f007b401ef0078101100000000000000080010405cd003b400e1001a403e500b8402e100b84606108b8410e98012400ed203b600ed8038880100000000000000
0c0050400cd0033400c10012421c120704) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1440) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (036440dd0036208500000000000000042283c00ff203fc10f9001f4413f001fc01bb021cc08f3001fc0133002cc003f003fc00f7003f080500000000000000060007c20df8037c00df0016c065d2086c005f0087c321f2037c00db00b7c02df0837c00df00370029000000000000000e20d3c00f
f0037402df0017c055f0115c00db1034480934034d10d34864c00df0037c00df0035a814000000000000000c201b400cd0033422cd00174018900504204d0830401910c00400410044509cd0033400cd0031200600000000000000040803400ed003b400ed101b441ad1009400690108400e10108408611038080b
d003b404ed103900080000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1460) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0033004dc01130046c41171804c0033004cc003f007fa003000000000000000e6017c00ff003fc08f30017c083f000fc003e118f8081d0207c021f0006c006f023ec08ff083fb80500000000000000086003c00df0037c00df0417c081f0487c208b1184c00434807c00131c80d101f2037c00d7
0036b00100000000000000000843400cd0033400cd21174004d03224000100805040101134040503154044d0032400cd00302010000000000000000a0007600dd0037400dd00174045d01274009910204101100234009101044184d0037400d50034a00100000000000000080207400dd0037400d100174021d00c
742b1101844021100274089504e44435d0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1480) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0017c00ff003fc00fd003fc003704efc109b080dc017b400fc24fb080fc00bc005fd002f003d8025000000000000000e2003c00df0037c00df0037c091f4063c01170c47c43170042c03170044c13132414c011f0037a8000000000000000006200f440dd0037400dd0037480990027401150046
686150c47410d500c44211141144011d0035a003000000000000000e804f400cd0033400cd18314008da0274800580034800500064000510004000100164010d1033a210000000000000000c200f401dd0077401dd0077421912027421110000400510047421d100044001108044001d0077180100000000000000
0e000fc01ff007fc01ff0077e01a3006fc) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (14a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (03fea47f003da8000000000000000000404bc08cf0033c01c7037081dcb0060c084f0263e0d0f0343c054f0043c15071377c0d4f003010120000000000000002007f601ed007b401ed0078403bd00684096d234b4056d254b4056d004b40561006b4452d0a7a0806000000000000000a001f400c
d0033400c500304018900a044a0c00074831c00c34114c01874211500a34000d017020030000000000000002004f400dd0037400dd00344039d01e44009006274921d0047410dd004740b91019340a9d0474a0130000000000000004202fc00df0037c00d70034c201b0824d00132087c061f0487c421f0287c001
70117c001f003508030000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (14c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0363189ec017f209fc056f035dc0a7f005cd0b7b0015a816000000000000000c204b400cd0033400cd1033400c51030413c10271448cd0230401cd2871401dd0170609d90033201600000000000000040207401ed007b401ed107b41161086848341806b481ad007b4017d08796a3cd007840149
007900840000000000000006204f400ed003b400ed003b400650028520e10809c006d0038c8061401c400ed1018040e100399a11000000000000000e0057c00df0037c00df0037cc0530064c0053c006c401f2015c00030014d001f0004c00130033a0100000000000000006400bc00ff003fc08ff003fc00ff022
fc0873402f8003f121fc24ff013fc047f0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (14e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (80434008d00230008d00234008d20204148500334018d20204008105204548100244948100302814000000000000000200634209d00274009d00274009d02245089520234009d8024700910524400990c27484910224a01c000000000000000800074009d00274009d00274049d04e4427914027
0029d00244919110e45069100a05069100222000000000000000000c2043c009f0027c009c0027c089d2064d409200a7c899f00a4c04930022c409b1266c009300250810000000000000000c004bc001f1007c001f2007c861f00864801f4104e411f0485c80120006a801e0207c02174007801200000000000000
06205fc005f0017c005f0017c03732414c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1500) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0274009d00252018000000000000000e804b4008d00234008d28214008d85234208d21204008d20214409515236108124234248d00210012000000000000000c20734001d00074001d00044001d20054021b00044805110144001140840061101074065d0007181c000000000000000e0067c009
f0027c009f2024c00bf082cc10b3022cd02bb002cc00b3242ec90b3002fc12bf002fa018000000000000000e6067c009f0027c009f0027c00bf152bd00bb052f814bf002fc00bc252fc14bf252fc94bf5027a818000000000000000ac077c001f0007c001f0007c001f0004c84170003c001f2014c00134104c041
b0007c04130006b01d0000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1520) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (08c848f3486dd21f3200cda073006c50074541cd1032a114000000000000000204134005d00174005c001740271405c5037140df4077d045b4237c001c49179041c6807d045ca00400000000000000042053c001f1007c001f0007c021b1804c84130807c001f1087c181f08c6c80171086c001f
280508100000000000000006015fc009f0027c009f0026c009d0465cc18b04674049b10e7c009b00e7c038f0527c249f00258013000000000000000e2017c009f8027c009f00255008f0a27c089f04e4e019f0065c18871423cd3934127c039f0027aa05000000000000000620634009d00274809d002540a9d002
7400dd8220440950024500958024400918) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1540) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (2057000ed003b400cd003b4a30d08414002314f04886d000850821014b4008d0400400dd00a91815000000000000000e000fc01ff007fc09ff007fc015f8144e01330275c29ef027cc01f70257041ff007fc01ff007d200300000000000000066043c00df0037c00df1037c00170007c00170037
c001d1017c409f0804c405c0007c005c0035a81000000000000000004057c01ef007bc01ef007bc016b007cc0123007fe41ef205bc01af104bc01f70058c217f1079101100000000000000020017400ed003b400ed003b40229047840009043b4806d903b400ad00b9400e91018403ed00388a0100000000000000
0a0053400cd0033400cd0833005c920f00) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1560) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1474071d00362185000000000000000c200fc00ff003fc00ff003cc0039000cc0003007fc003f000fc223e0004c60bd200fc103f001f0807000000000000000c0007c00df0037c00df0037c021f0017c0c1309a7c0a1f0007c029a01078009f0005c0a1f00b700010000000000000006211bc00d
f0037c00df0037c0a0f0054c411310b5c011f0804cd3d70477c059f1065c039f0035a85e000000000000000c211b400cd0033400cd00334000d10414020100344000d018045105a0434101d00006030d8030204600000000000000040123400ed003b420ed003b40029040840021033d6083d0c08400a5000b400e
d02194082d002900180000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1580) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00370104c143b020cc1633110ec045f0077c01db007fa003000000000000000e4017c00ff003fc00ff003fc183f110fc403f1dbbc843f040f80027000fd043f050fc843f003fa804000000000000000ac007c00df0037c02df00b4c001b0504c001340b7c001b00074421f0584c081f0087c081f
1006b00000000000000000008043400cd0033402cd02324000d03005000509334080d20034020503004200d28036000d0020281000000000000000020007400dd0037400dd80344011d00464011182374031900474009d06144031d08474019d0034800000000000000000080087400dd0037400dd0036c011d09c
44031540d74411d04c74861700044811d0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (15a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0017c00ff003fc00ff002fc03972945c005740c7da89f2057c02df2057c017f003fc00ff003d8805000000000000000e2003c00df0037c00d34022c019b4106c021f1844c019b19d45021342c680b5f0037c00db0037a0000000000000000006000f400dd0037000d10024400192036490090034
400d102244421100940105d1037400dd0035a803000000000000000e8043400cd0033400c10026444098132458cd0c10404490080404010402414cd0033400c90033a010000000000000000c6007401dd0077404d100ac41a11020440611032441211018440211031444a5d0077401dd0077000100000000000000
0e000fc01ff007fc09d3072ec00132186c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (15c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (03fc00ff003d38020000000000000008404bc00ce0033c01c70365c090b1241d14c34440d05030170d0dc34063c258f0373c01cf003018120000000000000008201b401ed007b421e1166940569295840da1016840121024840121016b405ed007b405ed007800060000000000000008000f400c
d0033400c52021493590801400010000402010024400c100e34030d0033400cd003020030000000000000002004f400dd0037400d1002c406d108344805108f4489d10024407d106374245d0037400dd0034a0130000000000000004200fc00df0037c00d7002dc40d318b1c02d30131c08434104c12034023c92c
f0037c00df003508030000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (15e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00531094c00531017c025302155005f0017c005f00152017000000000000000c005b400cd0033400d90023425cd0030489c1067442fd10033409c142f14208d2033400cd0033281600000000000000040013401ed007b401e90b6b401e90028480e1203848161047b401e11079001ad207b401ed
0079000400000000000000066047400ed003b400e10423400ed1038400c10018400e1001b440e1101c000cd003b400ed00398813000000000000000e0043c00df2037800d300efe20db1064401130814c20d30037c00d30014c001f0037c00df0037a01000000000000000062003c00ff003fc00ff002ec0137021
fc04bf002f908bf0a3fc003f002fc88bf1) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1600) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (a0534008d00215008d0520414a10d28414a10528414e10528534a145285148d00234008d00202010000000000000000200734009d00254009da024408b1122e400b120ac404b1002c402b1002c4028d20274009d0024a018000000000000000800034009d00244009d00244019101e44529120e4
4029100244029100644429d10274009d0024200100000000000000042043c009f00248009f2024c01830064c00930164c409340e4c00830224c009f0027c009f002508100000000000000006004bc801f0007c001700078803f2482c220f0007c001f00038101f0002c001f2007c001f0005081200000000000000
0e205bc005f0017c005b4017c075b00945) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1620) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0274009d002528180000000000000004004b4008d00204048101a7400ad0428500a1812b410a1452a412a580a84008c08234008d00210012000000000000000c60734201d000450101084741f3102d46351142c740b1102c45051105405175d10074001d00070018000000000000000e0067c009
f0024c089380ebc01930066c31932b67c01930064c01931064c15bf0027c009f0027a01c000000000000000e0063c009f0026c149f052fc549f0d27e149f0527d34df2527c349f0d27c14bf0027c009f0027b81d000000000000000ac077c001f0005c001f0904d04330106e04134100c04030100c24132104e041
f0007c001f0006b01c0000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1640) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0bc90830603c90032408c800374098d0033400c50032a010000000000000000200534005d001440051001c4025b52544025108944825100144005100974015d00174005d0014201000000000000000042043c001f0004c20134006c40370884c20130004c10130184d00134107c001f0007c0017
000508140000000000000006004fc009f0027c009f0027c809360a5c189b0667c409f0225c009b0027c209f0027c009f00250817000000000000000e2017c009f0024c809140234409f20a44139301a7c09930126c00974024c809f0027c009f00252005000000000000000400634009d0024400910027408bd203
84a0a1002b480b1002a4a0e590ac4418d0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1660) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (6057400ed003a400e10133445212178408b14058104cd0010404810170418ed003b400ed003908150000000000000004000bc01ff027f043f3207fc013b027cd01b3027cc01bf007dc01f3125dc01ef007fc01ff007d200600000000000000066043c00df0037c08ff0035c40d71027c00d70037
c00172035400170037c009f0037c00df0035b81000000000000000004047c01ef1078cc1e34078d01ff006cc00fb004cd01fb4072c0079086bc012f007bc01e70078181400000000000000020007400ed0038500e11038443e900b8400e900384036900ba401a9003b680ad003b400ed0038800400000000000000
0a0053400cd0030480d12030425cd08704) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1680) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (037400dd00362081000000000000000c2017c00ff003cc00f30231c80b3015bc017f0004c20f3020cd02ff012cc007f003fc00ff003f0880000000000000000c0087c00df0036c40ff0027c44df1095c8e170027c104f0086c00570007c901f0837c00df0037080500000000000000062073c00d
f0037c20f34037405db0016c015300b4c00dd0284d04d32075401df0037c00df0035a0140000000000000004001b400cd0032400c180334014102424000901904020d0884407114070403cd0033400cd0031280200000000000000040023400ed103b400e1903b48569020a4002102086002d02286004106094006
d003b400ed003900000000000000000004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (16a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01e3184fc003f004fc01be000cc01b3004cc017f007fa003000000000000000e2017c00ff003fc14f7002dc021e0987c003f1205c003b900fc143f0907e047f013fc00ff003fa805000000000000000ac007c00df0034c02f302b7e62132303c205f1204c480502244029f0b02c085f0237408df
003610000000000000000000a043400cd8030400c100214060140230008d8000580c5c0104000d04004005d0033400cd0030081000000000000000020007400dd1034400c10037420110027618dd90344009584344009d0096000dd0037400dd0036a00100000000000000080217400dd0034400d30025c099100d
74821d0224c801120844435d00445190d1) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (16c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0017c00ff003f400ff003f400ff183e400fb000fc00bf000f810fe009fc00bf400fc00ff003d8007000000000000000e2023c00df0037c00df2037c00d34031c619620c3c2b1f0046c049f0484ca0830004d00df0037a8000000000000000006200f400dd0037400d90036400d10035408d40447
4101d2046400dd00045005100344005d0035a803000000000000000e804f400cd0033400cd0033400c000314008500076004d0002600cd00004004100304004d0033a0100000000000000008200f401dd0077401d90076440c511344019108474413d1047021dc00444219110044005d2077080100000000000000
0e000fc01ff007fc21ff207fc01f3027cc) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (16e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (037c005f4039b8020000000000000000404bc00cf0033c00cf1030805cfa171c80cf2152d08cf0012508c38243c144f0033c0843083012120000000000000002003f401ed007b401ed007a445ed3178481ed81da411bd004a421f1004f401ad004b4016100788006000000000000000a001f400c
d0033400cd0030004cd00305038d08024004d00024008100034108d0007400510032a0070000000000000002006f400dd0037400dd0036805dd08340038c014440add0124403d140974015d02b7401d10034a0130000000000000004200fc00df0037c00df0034c00df0235c18df0084c40df0404c08d30447c005
f0037c01d3003508030000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1700) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (017b989bc487f149f4007f125fc00430017c025f0017a817000000000000000c204b400cd0033400cd0032400dd0033400c909b3428cd10334004d2073400414033400dd0033281200000000000000040007401ed007b401ed0078601ed207a611b9185b401ed007a401e910fb40161007b401ed
007900030000000000000006204f400ed003b400ed003ac00fd0839400ab001b410ed001b400ed003b800a1000f400ed00398813000000000000000e0057c00df0037c00df0034c00df0034c40c32007c405f2007c009f0007c00930047c40df0037a0150000000000000006600bc40ff003fc00df003fc08df003
7480bf2215000af021dca8ef020bc815e0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1720) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (80434008d00234008d00224008c00306008580204148d08234808c0520520ad0029400cd80212010000000000000000200634009d00274009d00244109d00244249520654049500374249d8024410b5206f4049d0024a018000000000000000800074009d00274009d0026c009d00e4504810824
5079d01a74739d00640439d10e44439d00262001000000000000000c2043c009f0027c009f0024c089f08a4c01910024c009f0167c309f38a4c029d00264009f00250810000000000000000c004bc001f0007c001f0007c401f0805c021f0087c400f0c87c021f0085e003f8087c501f0005801200000000000000
06205fc005f0017c005f0014c005f0016c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1740) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0274009d0025a818000000000000000e804b4008d00234008d00206048180236209d006040085002b600a5102b4008511234148d0023a010000000000000000c20734001d00074001d0004404068007c0017200440017000f4001100974205121074041d0007081c000000000000000e0067c009
f002fc009f0024c82b3002cc00af002cc14bd0027440970527c00a7022fc00bf002fa018000000000000000ec067c009f0027c009f0027c149f0527c80bb002bc80bf002fe40bf002fc809f2526c149f0027b8190000000000000000c077c001f0007c001f00048001c0004c00174015c041700074001e0914c203
f2017c001f0007b01c0000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1760) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01cd1033401cd0383602014000462c00af4402cd0032a014000000000000000200534005d00174005d0015c0371009c48277001d5006d009741951001451171001c4007d0014201400000000000000042053c001f0007c001f0004c041b0004c041f0006d081f2007e00130606c10130104c041f
000508140000000000000006005fc009f0027c009f0027cc0970025c009e2027d18970267c489f00238009b0127c409f00250015000000000000000a2017c009f0027e009f0024d00930027e098f0064c019701a7c83970a67c00970167c009f0027a805000000000000000620634009d00274009d00244008d002
740095023440295002f442b1802f421950) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1780) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (2057400e1003b405ed0079401dd0151c0c2d225040b6107dac01e1075341d2d035840dfd00399815000000000000000e000bc01f3007bc09ff0074d09ff025fe093f207cc01530276c01de8277401ff027cc01ff007fa80200000000000000064043c00df0037c00df0037c00578005c201f0007
8001f0027c00572026c001f8017c009f0035b81000000000000000004057c01ef007bc01ef007ac01e3405ed012e005bc016f007b401e3007ac4121407cd01ff0078101400000000000000020017400ed003b400ed0039402e010ba4222504196804d803b480e90831401f10018401ed0038800400000000000000
0a0053400cd0033400cd0032400c181f64) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (17a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0474031d00362081000000000000000c2007c00ff003fc00ff003cd003f005cc6137001c5006f0a1fe04ff005fc1033802fc003f083f0a80000000000000000c0027c00df0037c00df0035c029f0035c081f0497d005f00b5e12970037c025f0007c421f0037000100000000000000062053c00d
34037c00df0036c009f0037c010f1114c00532074c00d71077c015f1020c001f0035a814000000000000000c205b400c10033400cd00334008d00014010d00404060101f2528c104f34000d10004000d0033200600000000000000040023400e1003b400ed003a484ed211b6002d221843061c13c400b5013f4002
d01084006d003900000000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (17c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0cf3023fc00be013dc00f7003cc00ff007fc01ff007fa003000000000000000e6017c40ff003fc28df003dc101f0607c00330307d002f000bc282f030fc021f0007c081f003fb805000000000000000ac007c00df0037c04df0534c101f0104c00172305c441f0137400df0333c041101074041f
0036900000000000000000008043400cd0033404cd01306048c00014000901034300d1433480cd00334200184074040d0030201000000000000000020007400dd0037400dd00344038d01044001d08054081d00274025d81274105180674111d0036a00100000000000000080007400dd0037400dd0034c021d004
545a1b0287c001d0077422dd047744211c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (17e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0017c00ff003fc00ff003fc81ff001fc00f7003bc04ff0837c00db4437c00ff003fc00ff003d8005000000000000000e2083400df0037c00df0036c00df08d7440d30037c00970835c80d70034c00df0037c00df0037a8000000000000000006200f400dd0037400dd0034404dd0057400dda037
000dd1034420d50034480dd0037400dd0035a003000000000000000e804f400cd0433410cd0332410dd8433424c923334008500b1400c50030430cd0033400cd0033a010000000000000000c200f401dd0137404dd013c4045d211740add00b7401dd0074449d102f440edc0077401dd0077180100000000000000
0e000fc01ff007fc01ff0b3e801ef005ac) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1800) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (03fc00ff003da8020000000000000000404bc00cf1033c20c72a31c04ce0891c00cf0071c54830731408c14073400cf0033c00cf003210120000000000000002003f001ed007b401e5007240139004d401ed8179601a11078401e1057b401ed007b401ed007a0806000000000000000a001f400c
d0033403c501314048d42c3413cd0031503814031402c10033400dd0033400cd003220030000000000000002000f420dd0037418d151fec07cb0805c03fd003c403d102bc413e000bb480fd0037400dd0034a0130000000000000004200fc00df0037c00d3103fc40d70435c28df0034c10931835c50d3b037c00d
f0037c00df003508030000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1820) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (005b1016d055f2013480436013c005f0017c005f0017a817000000000000000c204b400cd0033600cd0031603c50041440c900334018d8033400c10033480dd0033400dd0033203600000000000000040007441ed007b401e50979783f1205f425e90172401ad907b405e1007b401ed007b401ed
0079000400000000000000062047400ed003b400ed0038400e5900bc04e10179400ed00bb403e1217b405ed003b400ed00399833000000000000000e0057c00dd0037c00d7063cc20c30807c28f20234c80cf0037c00d30033c00df0037c00df0037a01000000000000000066003c00ff003fc00fb083fc00ff201
dc80ff103ec00af023fc00ff043fc10ff1) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1840) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (80434008d0023401814522500910026494814520414810520414c105204148d00204009d00202814000000000000000200636009d82274009100e44009120244429180a04089904254009921245809d00244009d0024a01c000000000000000800034009d00674009100a6c008121a2c02910024
4119102644489100e46009d08245009d00262001000000000000000c2043c009f0067c009b0026c009b40e4c03830024c008b2065c009b0024c009f0024c009f00250810000000000000000c004bc001f0007c001f00028041f0007c20174005c001f0087c001f4087c001f0007c001f0005801200000000000000
06205bc005f0017c00570015d8071815f0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1860) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (8274009d00250018000000000000000e804b4008d0128500a10029504a14129406ad072a4208120220808100234108d00234008d00210012000000000000000c20734001d004c4151147c46811109545071d004440a1512844001110074011d08074001d0007181c000000000000000e0067c009
f0224c20930164e088000a4c039d0166d01b2086ec91b3446fc119f0027c009f0027a019000000000000000e6063c009f0527c149f0527c14bf252bc149f0527400bf0027c809d0027c949f0027c009f0027a819000000000000000ac077c001f0007c001b0104d00130004c84130104d041b21054241b11144e41
f0004c001f0006b01d0000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1880) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (032100c85050d0410481892020400c90033400cd0032a01400000000000000020053400514614400510014c0151101440a5100144236d00dc60863015c5005100174005d0014a01400000000000000042053c00130004c00130006c001b0004c00131004c001f2004c00130004c001b0007c001f
000508100000000000000006005fc009f0027c009f0c26405971067c209f0427c419f0027c009f1027c009f0027c009f00258013000000000000000e2017c009f0024c009200254059302a5c009f8026c00910022c00932023c009f0027c009f0027a805000000000000000620634009d002c400a10028480a1002
8400ad00244089518244009108374009d0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (18a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (2057400ec000b40861001840829454b4086102474012d0148405212170405fd017b400ed00391815000000000000000e000bc01ff004fc0133006d84deb024ec01b7024f8091f0256c09470261c19ff007fc01ff007d200200000000000000066043c00df0027c001b0027c201f0007c009d0027
c004f0017c001f4037401df0037c00df0035a81000000000000000004057c01e3006cd01b7405cd012b207cd0173406cc01ef10585016b0058c05eb007fc01ef0078101100000000000000020817400e1006842225008841031100c4222180c84026d1418402010030401c1007f400ed0038880100000000000000
0a0053400c100e86012500c81122900084) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (18c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (037400dd00362085000000000000000c2007c00ff007fc00fc001449033023cc006b014e820fd000fc807b023cdc0ef003fc00ff003f0805000000000000000c0007c00df0037c029f4005c02df04b7c001f0087c485f0007c005100b7c00df0037c00df0037002100000000000000062073c00d
f0037c00534006c021b80c7c00170007c010f0026c009f0031c00ff0037c00df0035a804000000000000000c201b400cd0013400410032402110047480c100274000d00304200d0030400cd0033400cd0031200600000000000000040023400ed005b400a1003a704f1803f400e5012f4042d003a4086d911940cf
d023b400ed003900080000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (18e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (09334034c4033210cc003100ccc890f0107c01df007da003000000000000000e6017c00ff001fc00ff003ec00ff0033c00ff01b4c007f002fc027f412dc80df2237c00ff003fa805000000000000000ac007c00df0017c00df0034d00d31034c00db0137c045f0d27c04530726c14df0037400df
0036b00100000000000000008043400cd0003400cd0011400c145305004101b14344d2003404410122404cd0033400cd0030281000000000000000020007400dd01074105d0025610d184044009908374015d0067421510026400dd0037400dd0034a00100000000000000080027400dd087742b9d002442bd108b
4480910104c015d04474415130f4420dd0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1900) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (2017c00ff003fc00fc803f400ff203e8803f403ec109d02268419f082fd203f1077c00ff003d8005000000000000000e0003c00df0037c00df0837c00df0035d11132035c01110004e88130cc4c011f0447c00df0037a8000000000000000002200f400dd0037400dd0837400dd0035401110035
401110415510d10210601dd3227400dd0035a003000000000000000e8043400cd0033420cd0033040cd00316000100354140100004020151004008d1803400cd00332010000000000000000c0007401dd0077401dd0077421dd087440411003c400112ac54231128004041d02c7401dd0077180100000000000000
0e000fc01ff007fc01df007fc01df0074c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1920) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (03fc08ff003da802000000000000000060cbc00cf0033c01cf0873c8dcf0072c00030370d078b1060ca1830162c0d830171c01cf003210160000000000000000001b401ed007b401ed007b405ed007b439310270405a1047850161a17a40d71015b401ed007a08060000000000000000008f400c
d0033400cc0033480cd2832000110030002191000540011002400100201480cd003220070000000000000002004f400dd0037400dd0037400dd003540a9122f84c19102f0420d101b448ed10037480dd0034a0130000000000000004200fc00df0037c00df0037c00df0034c00134234c28932034c02430134c005
34097c00df003508030000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1940) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0673101cc2273015ec247f01ddc277f061fc005f0017a0170000000000000008205b400cd0033400cd0033400cd0031402c10030409c10432410c509b1403c90033400cd0033201200000000000000040013401ed007b401ed007b401ed0078401713278421a1787a601ed107d4017d007b401ed
007800040000000000000006004f400ed003b400ed003b080ed0039400e14538500f10030400c3003800061003b400ed08398813000000000000000e0043c00df0037c00df0037c00df1034c00130134c401b0014d00d70851c00470023c00df0037a8100000000000000004600bc00ff003fc08ff003fc20df003
5c002f0037e88ff423fc6cff0135d80fd0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1960) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (80434008d00234008d00234008d1022440804521414850521614cd00204808505234008d00200814000000000000000200634009d00274009d00274009c00244109100250008505254009d00244068d80254009d0024a81c000000000000000000074009d00274009d00274009c0026c02810164
4069100a04089d04e47409120274009d0026200100000000000000042043c009f0027c009f0027c009f1024c03931a604c2924024d819f00a4c809a0265c009f002500100000000000000004204bc001f0007c001f0007c001f0007c041f0087c52170085e020a20064241700034001f0005801200000000000000
04005fc005f0017c005f0017c005f2014c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1980) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0244009d002520180000000000000004004b4008d00234008100234008c00204c09501234408928226008120204408100204008d00212012000000000000000c20634001d00074001500074001d00044801520874021600074001040044000140045001d0006181c000000000000000e0073c009
f0027c0093002fc009f0024c80b385afc54b3102bc20b7002cc20b3082cd00bf0025a019000000000000000e6077c009f0027c009f0027c809f0027c14af0522c14bb102ec00bf052fc94fb202fc009f0027a819000000000000000ae073c001f0007c001f0007c001f0004d00132105d04170105c041f00044001
f0105c001f0006301d0000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (19a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (81c50073419c900b0440c941f6403d180f3400cd0032a014000000000000000200434005d00174005d00124005d081448061001f40171009c51170205c4807120df4004d0014a01400000000000000042053c001f0007c001f0007c001f0004c0b132043c80130384c00130006c00170387c001f
000408100000000000000000205fc009f0027c009f0027c009f2027c49970027c089f28e7cc89b0067c149f00e7c009f0025801300000000000000040017c009f0027c00930027c009f1024f01931027c109b0463c33970824d01930120c009f0027a805000000000000000420634009d002740095002700099002
46029d00270209510274009581a4400910) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (19c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0057400ed003b400ed0033005e91179424610049400830310426c1117300021008b400ed003918150000000000000004201bc01ff007fc01ff007fc01ff007cc0573425cc89fb825ec01e3807fc01f3005fc21ff007d200200000000000000062043c00df0037c00df0037c00df0035d005b1007
8405f0014000d71007400db0037c00df0035a81000000000000000004053c01ef007bc01ef007bc01ef007ac01f7405fc01e31858c01eb087ec81e34073c01ef0078101100000000000000022013400ed003b400ed003a000ed003a400e5e0ab400e1501a401c900b8430e5103b400ed1038880100000000000000
0a0043400cd0033400cd0033420cd00326) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (19e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0d2400dd00362085000000000000000c0203c00ff003fc00ff003fc00ff203cc80730114c10934414cd07300bec013b0017c20ff203f0805000000000000000c0017c00df0037c00df0036c00df0035c821fa001c40d70025c02d704b7c0cdf1417c00df0037000900000000000000060053c00d
f0037c00df0037c00df0036c06530036c04d30134c33db11f7c80c30017c00df0035a8140000000000000000000b400cd0033400cd0033400c900334110100034230148c0503890003403012203400cd0033201600000000000000040003400ed003b400ed003b404ed813a40c31090a440e18008400a9033b408e
1401b400ed003900080000000000000004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1a00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01f3007fc01f30066c0107407fc01ff807fc01ff007fa003000000000000000ec017c00ff003fc04ff043fc04d710b7c002c08874043f010fc843f6187c843f040ec10ff003fa80500000000000000006003c00df0037c0adf00b7c16dd01b4d00132006c081b0a84c02110382c001b0017400df
0036b00100000000000000008043400cd0033400cd0033408c51b31400054080700018020402c18004408110003400cd00302810000000000000000a0007400dd0037400dd0037400dd08344115100066084980f4440d10006424d90047400dd0034a00100000000000000082207400dd0037400dd1037400d7803
5403050144c101100c0540419400451110) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1a20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0217c00ff003fc00ff003fc40ff0036c00ff003fc00ff000fc003f003f400ff003fc00ff003d800500000000000000042013c00df0037c00df0034c00cf0037400d04037c00d14067c80070037c00dd0037c00df0037a8000000000000000006200f400dd0037400dd0035400dd0037400d00833
480d100c4400910037400dd0037400dd0035a803000000000000000e804f400cd0033400cd0030400cd0033400c10033400c10007400450033400cd0033400cd0033a010000000000000000c200f401dd0077401dd0075401dd2076401d10037401d10044001111077001dd1077401dd0077080100000000000000
0e000fc01ff007fc01ff087cc01ff003fc) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1a40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (037c00df0035b8020000000000000000405bc00cf0033c00cf0431c00c70033c00c34177c24cf0051c014f2033c00cf0033c00cf003010120000000000000002001f401ed007b401ed0078401e0007b401e5047b481ed01685013d007b401ed007b401ed00788006000000000000000a000f400c
d0033400cd0031500c50033400c10133400cd00714000d0073400cd0033400cd0032a0070000000000000000006f420dd0037400dd0034400d1003f400d10037400dd01804009d0173400dd0037400dd0034a0130000000000000004208fc00df0037c00df0035c00d71037c80d71037820df0c84c005f0037c20d
f0037c00df003508030000000000000004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1a60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (005b0015c4057005f400630017c005f0017c005f0015a817000000000000000c204b400cd0033400cd0030400c10033400c90033000c18413400810033600cd0033400cd0033281300000000000000040007401ed007b401ed0078541e11173401e90079401e580db40161007b401ed007b401ed
007900000000000000000006204f400ed003b400ed0038400e1403b400e1003f400e1001b40021403b400ed003b400ed00398813000000000000000e0057c00df0037c40df0034c00c10077400d30037c00d70072c00130073c00df0037c00df0037a0140000000000000006600bc00df0037c08df0037c00cf043
7c00db0237c00df0037c889f0037c00df0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1a80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00434008d00234008d0032400cd05234008540234008d10204009d00234008d00234008d00202010000000000000000400634009d00274009d00244009d00274009580a34809d08244389d00274009d00274209d0024a018000000000000000800074009d08274009d0026c009d00274009100a7
4809d01246019d02e74009d00274009d00262001000000000000000c2043c009f0027c409f0264c039b0027400920227c009f00e4c009f0027c009f0027c009f00270811000000000000000c004bc001f0007c001f0087c021f0007c00170087c001f0087c001f0807c001f0007c001f1007001200000000000000
06205f4005f0017c005d0014c004300174) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1aa0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0274009d0025a818000000000000000e804b4008d00234008100224008100a34008d05214008d00234008d10234008d00234008d0023a012000000000000000c20734001d00074001100044001110874001d00474001d00074001da0074001d00074401d0007081c000000000000000e0063c009
f0027c0093402ec00b00967c009f002dc009f082fc00bf002fc00bf0027c009f0027a018000000000000000e4067c809f0027c009f0027c009f0027c009b0527c009f302fd00bf0027c009f0027c009f0027b81900000000000000084073c001f0007c001f0004c001f0107c00171007c001f00044001f0017c001
f0007c001f0006b01c0000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ac0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (40cd0043400cd0010400894283400cd0033400cd0032a014000000000000000000134005d00174005d011c5036100174005d025f4005d04dc40871001f4015d00174005d0014a01400000000000000042053c001f0007c001f0044c20130007c001f12078001f0084c80130107c001f0007c001f
000508140000000000000004005fc009f0027c009f0027c109f0023c009e0027c009f0427c019f1027c009f0027c009f0025801700000000000000042017c009f0027c00930022e40930027c009f0025c009f0227c059d0027c009d0827c009f0027a805000000000000000620634009d002740091002440091402
74009d00276209d24274089d10274009d1) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ae0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (2057400ed203b400e1028b48ce1013b408ed1233400e5003b40421430b400ed003b400ed00398815000000000000000e000bc01ff007fc09f3024bc09f3007f401ff025fc09f3007fc0131025ac01ff027f409ff007fa00200000000000000062043c00df0037c00df0007c20cf4037c00df0007
c40df0035d000f0823c80df0037c00df1035b81000000000000000004053c01ef107bc81ef2048cc1e3007bc01ef204bc81ef0858c412b007bc01ef007bc01ef0078101400000000000000022013400ed003b400ed0028410e12033480ed283b680ed001a401a1004b410ed003b400ed0038800400000000000000
0a0053400cd0033400cd0070400c100334) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1b00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (037440dd00362081000000000000000c2203c00ff003fc00ff000fc01fb0037c00ff002fc40f2080fc013b001ec00ff003fc00ff003f0880000000000000000c0007c00df0037c20df4087c02df0037c20df0837c20d70087c00df0097c00df0037c00df0037000100000000000000062053c00d
f0037c00d30007c00d20037c00de0027400db00c7838d20003420cd0037c00df0035a814000000000000000c201b400cd0033400c10003400000033400cd0813400cd13f3400010003600cd0033400cd0033280600000000000000040003400ed003b440e1000b4a021683b400ed081b420e9020f44021001b400e
d003b480ed003900000000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1b20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01b30005c2033204fc003f0864c943f007dc01ff007fa003000000000000000ea017c00ff003fc00ff000dc20ff003fc00ff010fc00fb212bc503f001f800bf003fc00ff003fb805000000000000000a4003c40df1037c80df0007c00d90037c00df0007e00d740074801b0016e009f8037c00df
0036b0000000000000000000a043400cd0033400cd0003400cd2033400cd0203480c582034004100104008d1033400cd0030201000000000000000000007400dd1037400dd0047406dd2037480dda207600d500c74005900d64089d0037400dd0034a00100000000000000080007400dd1037400dd0007c01dd803
7400dd0427400d100e3408111054000dd1) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1b40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0017c00ff003ec00ff183fe00fb203ec81bf0017c009f002fc001f043fc00df003fc00ff203d8007000000000000000e2003c00df0037c00df8037c00df0037c019300c5c03130083c051e00f4d121f1035c00cf0037a8000000000000000006200f400dd0037420dd0037400dd0836408952044
4411121174419d08f44041d0034601dd00358803000000000000000c004f400cd0033400cd1033400cd00334048100854000100074008c00305100c2031400dd0033a010000000000000000c200f421dd0076401dd3877401dd00764109500c44001140074011d10744061d0034401dd0077080100000000000000
0e800fc01ff007fc01ff007fc01df0077c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1b60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (23dd00ef003db8020000000000000000404bc00cf0033c00cf0a33c0dcd0073c00838150c888b2026c088d0670c04c10036c00cf203012120000000000000002003f401ed007b001ed007b401e5007b401a905d8401a11078641a5107850de1407a401ed00788006000000000000000a005f400c
d0033420cd0033420cc203340081100040019000240b8d00f0448010032600cd0032a0070000000000000002004f400dd0037400dd0037400df08374199b00504069110f44209f00f454ad00034400dd0034a0130000000000000004202fc00df0037c00df0037c00df1837c00930094d049b0cf6c041f0034c00c
30034c00df003508030000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1b80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (815321dfc007f00dfc067f001cd86730017c005f0015a817000000000000000c204b400cd0033400cd0033400c50033400d90073404cd04b3400cd0050400c10037409cd0033281200000000000000000207401ed007b401ed007b041e1087b491e1005b411ad007b4012d0478481e1007b401ad
007900030000000000000006204f400ed003b400ed083b400e5003b400ab003b400ed003b400ac0038400f1003b400ed00398813000000000000000e0057c00df0037c00df0037c00d30073c00930003c001f0017c001f0034c40136037c00df0037a0150000000000000006400bc00ff003fc00ff0837c00fd003
fc00bf023f400de12374009f2a37c04ff1) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ba0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (80434008d00234008d00234008d00204008105205148d00334148d0020414c100234008d00202010000000000000000200634009d00274009d00274009d00244009100b4400dd00374049d11244c08140274009d0024a018000000000000000800074009d00274009d00274009d10245839100a4
4009d00274029d04e45019100274009d00262001000000000000000c2043c009f0027c009f0027c009f1024c05930660c038f0967c019f0424c02931027c009f00270810000000000000000c004bc001f0007c001f0007c001f0007c021f0807c001f0287c121f1007c121f00074001f0007001200000000000000
06205fc005f0017c005f0017c00531017c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1bc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0274409d00258018000000000000000c804b4008d00234008d00234008100204008120274128501304228520214008065234008d0023a010000000000000000c20734001d00074001d00074001500045001f00074061d80044005000145005b00074001d0007081c00000000000000068067c009
f0027c009f0027c0093002cc00a3002fc00b700acc84b70028c00b30027c00bf0027a818000000000000000e6067c009f0027c009f0027c009f0027c14bf003fc14ff052fc00bf002fc14bf4523c00bf0027b819000000000000000ac077c001f0007c001f0007c401f1004c40534104c845f0007c045f1004c041
30007c001f0006b01c0000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1be0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (02cd8431401c100b36038100b2008c93034600cd0032a814000000000000000200134005d00174005d0015c005d00104047d019844071101f6847b011804071001c4005d0014201400000000000000042153c201f0007c001f0007c001f00045001f0084c011b0107c00130084c101b0004c001f
000500140000000000000006015fc009f0027c009f0026c009f1027c909788a7c409d0067c118f0c26c019f0027c049f00250015000000000000000e2017c009f0027c009f0027c00930024c008380a7c009714a4d029700a5c02930027c019f00252005000000000000000620634009d20274209d002740095002
44089d00270049d8134404910225484890) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1c00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (205f400ed003b401ed117b601e501794026d006b401ad206b68560017840721017b405ed00398815000000000000000e000fc01ff007fc09df007fc01d30070c017f0267c09ff006fe01f3007cc29d36077c09df007fa80200000000000000066043c00df0037c00df0037c00df1037c005e0826
c00170027400df0005d00df1037d00cf0035b81000000000000000004057c01ef007bc01ef007bc01ed0078c016f0079d01f3406f401e3007ac01fb007cc01ef0078101400000000000000020017400ed003b400ed0039400ed00384007d0039403a1106b640e9003e400e10338401ed0038800400000000000000
0a0453400cd0033640cd0033400cd00304) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1c20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (037400dd00362881000000000000000c200fc00ff003fc00f7003fc00ff003cc0073002fc00b7242cc107f203fe0113003fc00ff003f0080000000000000000c0007c00df0037c00df0037c00dd1835c401f0007c109c1087c01df02b7c12df0037c08df003700010000000000000006205bc00d
f0037c40df0037c40d72036c005f00a3c039f00e7c81c342b4d01d3503fc01df0035a014000000000000000c201b400cd0033400cd0033400c500334001d03834410d0283400410080401010037400cd003320060000000000000004002b400ed003b404ed013b400e5013a4002d810b494ad000b424e10938014e
1013b400ed003900000000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1c40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (850ce1400850021400850021400850021400850021400000000000000000000ee01fc00ff003fc00ff00b7c14ff253fc0027030f8001e1207c085f0302c083f003bc08ff003fb0050000000000000008c007c00df0037c04d70137c32dd00b4c00130a87c04170004c045d1307404110137c44df
0036100000000000000000000043400cd0033410cd0033404c504324000500476100d09007044d0103400050433400cd0030001000000000000000020007600dd0037400dd0037400dd00346015100674111d0064404dd10c7400d10037400dd0036a00100000000000000080007400dd0037400dd0037400df903
6c011700474011d00444245d8086408151) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1c60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00000010000400010000400010000400010000400010000400010000400010000400010000400000000000000000000000000040001000040001000040cc1000040001000040001000040001000040001000040001000000000000000000000000000800020000800020000800020033800ce000
080002000080002000080002000080002000000000000000000000000000084402110084402110084402110084402110084402110084402110084402100084002100000000000000000000000000080002000080002000080002000080002000080002000080002000080002000080002000000000000000000000
0000000850021400850021400850021433) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1c80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0033800ce0000800000000000000000000000840021000840021000840021000840021000840021000840021000840021000840021000000000000000000000000000800020000800020000800020000800020000800020000800020000800020000800020000000000000000000000000000850
021400850021400850021400850021400850021400850021400850021400850021400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000040001000040001000040001000040001000040001000040001000040
0010000400010000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ca0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000000000000000000000000000000000000000000000000000000420800000000000000000033000000000000cc0000000000033000cc0000000000000000cc00108200000000000000000000000400010000400010008400210000400210000400210008400210000400010000400
21000000000000000000000000000010000400010000400810020400010020400010020400810020400010000400010020400000000000000000000000000840021000840021033840ce1000840ce1000840ce1033840ce1000840021000840ce1000000000000000000000020033800ce0000800ce0000800ce00
33800ce0033800020000800ce0033800ce) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1cc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000f0f00000000000000000000000000000000000000000000000000000000000000000000000003c3c00000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ce0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1400850021400000000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000000000000000000000000
000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000
000003fffffffc00000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1d00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0100004000100004000100004000100004000100004000000000000000000000000000400010000400010000400010000400010000400010000400010000400010000400010000000000000000000000000008000200008000200008000200008000200008000200008000200008000200008000
200000000000000000000000800008400211008400211008440211008440211008440211008440211008440211008440210000000000000000000001000008000200008000200008000200008000200008000200008000200008000200008000200000000000000000000000000008500214008500214008500214
0085002140085002140085002140085002) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1d20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000084002100084002100084002100084002100084002100084002100084002100084002100000000000000000000000000080002000080002000080002000080002000080002000080002000080002000080002000000000000000000000008000085002140085002143385002143385002140
0850ce140085002140085002140085002140000000000000000000010000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000004000100004000100004000100004000100004000100004000100004000100004000100000000000000000000
0000000010000400010000400010000400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1d40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000c20000000000000000000000000000000000000000000000000000000000000000000000000010820000000000000000000000040001000040001000040001000040001000040021000040001000040001000040001000000000000000000000000000010
000400010000400010000400010000400010020400010000400010000400010000400000000000000000000000000840021000840021000840021000840021000840ce1000840021000840021000840021000000000000000000000020033800ce0033800ce0033800020033800ce0000800ce0033800020033800
ce0033800ce00008000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1d60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (fffffffc0000000003fffffffc0000000003fffffffc00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
00000000000000000000000f80000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000010300000000000000000000000000000000000000000000000000000000000000000000000003c3c0000000000000000003000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1d80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000000000000000000000000000003fffffffc0000000003fffffffc
0000000003fffffffc0000000003fffffffc0000000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc000000000000000000
0000000000000003fffffffc0000000003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1da0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (001800060002a300000000000000000a8803a804ca45ba804ea013208e4a01b28064801ba884ea013a804ea013a804ea013a804ea012a20000000000000000000401a00068001a00068003a00068511a00062601a0186a001a80068061a00068061a0186a0200100000000000000000004012010
480612010480412010680612018e80402010080412010080412010480412010480400100000000000000000a8c03a808ea02ba008ea023990acc02ba808c0823a048ea023a808ea023a808ea023a808ea022a30000000000000000008c03b020ec0a3b820ea083b808e20a3b028ee083b848e8083a020ec0a3b028
ec0a3b028e80e2a3000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1dc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (02100084182104004100104004100104006100104006a30000000000000000000480800820020000082002000840100800820210020020030801c20060800820062000060030010000000000000000000402a00ea8038200e88038200e8803aa06ea80b8200ea803aa00ea803aa01ea803a200ea
80380100000000000000000a8800a814aa070a8102a0c2a01428042a85408840a83028040a0102a070a81c2a070a83428042a30000000000000000008c01080462091080042001880c42041881440001080042001080842011080442011080442002a30000000000000000008c0180004020180006000109804020
1018040201802060001800060001800060) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1de0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (04032010c80c32034c80d328104a0430010ca0432034ca0c32830c80432010c80432010ca0c00100000000000000000004030000c00030004c00120000408030000400030004c00030000c00030000c00030000c00000000000000000000000a8c030810c20c31010c6042081060053081062843
0010c20430810c20430810c20430810c2042a20000000000000000008c01b0006c001bc0068001b80068001b000e8011b00068011a0046c001b0006c001b00068012a30000000000000000008c01a8026a00928026a009a8024e009a8026a009a0026c009b00268009a80268009a0026e00aa30000000000000000
0a88801001040041801840041001060041) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1e00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (048201208048010000000000000000000000a018a8060801828062801800062a01808060a01820060a01828060a01828060a018280600100000000000000000a8802a801aa004200188006a00108006a801880042801800062001aa0068801aa006a80188006a20000000000000000008c018812
620490812420490812420498812c20c108128204b0812620498812620498812c204aa30000000000000000008c010010400410010600418810420410010c00410810c00410010400410010400410010c0042a300000000000000000a8c01a8106a0412830ea0c1a00068041a8106a041a0206a0c3a8306a041a810
6a041a8106a0c2a3000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1e20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (010c80410010c80432010480412010480412010c80408200000000000000000a8803a818ea0610018c2063281ac0063a818c2063021ae20638818ca063a818ea063a818e2062a20000000000000000008003b018ec063b818ea061b018ea063b0186a063b018e8063a0186c063b018ec063b018e
8062a20000000000000000008c03a818ea063a818ea063a818ee021a818e6023a018ee063b018ea063a818ea063a818ee062a300000000000000000a8c02b01804062b818ac060101806062101804062b818ac062b018ac062b018ac062b018ac062a3000000000000000000000020120804820120a04820124804
82012080c0201208049201208049201208) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1e40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (8802a830aa482a03028043a9002808aa82028082a81028042a0302a042a8302a040a81028042a20000000000000000008801881062041881042041881442041881040041881042041881042041881042041081042042a20000000000000000008801001040041001060041001000041001040041
081060041001020041001060041801060042a200000000000000000a88032800ca0032800ea0032802ca4032900c84020000ea0030800ea0032800ea003a800ea002a20000000000000000000001a0186806128184a06180184a061a0186a06120186a061a81860861a01868061a0186a060000000000000000000
0200012010480412210400412010680412) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1e60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (003080062000000000000000000000000001b8006e001300048001b9004a001b000e8001b800e8003a0006c001b0006c001b000e8002a10000000000000000008801a8006a001a8006a00128006e001a8006e001a0006c001b80069001a80069001a8006e002a200000000000000000a88001014
0405018100404010100624810140405a181004040101404040101404040101004042a20000000000000000000000800020000800022000000020000800020002000020010800020010800020011800420010000000000000000000000002a030a80c2a010a80502014a8042a030a80c22010a80c2a030a80c2a030
a80c2a010a80c00000000000000000000a) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1e80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (880c22018880620118980622118880620118804622100000000000000000000000010006400190802400190002c20290006c0019000a40009000640009000640009000a40008000000000000000000000001a8316a0e5a0316a0c5a83968045a8316a045a8316a0e5a8396a0c5a8316a0e5a8316
a0c40000000000000000000000032028c80e12008480232808480232028ca4a32038ca0e32828c80a32028c80e32008ca0a00000000000000000000000030002c002900024002b001a4022b000240009000a40029001a8002b0002c002b000a400280000000000000000000000031800c600100004680308004400
308006200110a0620008800c20030800c2) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ea0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0003a804ea093a804e2013a82466011a004c4013a824ee013b004e8013a804ea013a004ee010000000000000000000000002100c840321a0cac032910c86032100c84032180cac032900cac032100cac032b00cac03000000000000000000000000000140005000140a0502014080502034080d0
003408050201408050001408050201408450000000000000000000000002a10408012a10428412a104a8e10200428412810428412a10420012a10428010a00428410000000000000000000000002a080a8002a880a8202a08088222a88088202a1c0a8202a000aa0028800aa002a888a8200000000000000000000
0000018880626018880622018980622018) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ec0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (edc9e37218dc0000000000000000000000009ff72fffc9fb727efcbfff2fefcbbf727edcbfbf27ffc9fff2fffcbdf72fffcbfbf2fffc00000000000000000000000027e92fffc26490997cbfff2f97cbbe909924be5f09ffc27ff2fffcbde92fffcbe5f2fffc0000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000009fb727edc9fb727edc9fb727edc9bb727fdc9fb727edc9fb727edc9db727edc9fb727edc00000000000000000000000099b4242d090b4242d898b4242d011b424ad090b4246d090b4242d89894
242d090b4246d000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ee0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (804e20138004e20138004a20138804e20138004e201000000000000000000000000180006000180006004188004060188086000180006006180006200180006000180006004000000000000000000000000120104804120104806120184804120104804120104804120100804120104804120104
8060000000000000000000000003a808ea023aa08ea023a80844043aa18ea823a008e8023a208ea023a808ea023a808ea0200000000000000000000000039020e40839020e40a39828e04239828e20839020e00a39020e00839020e40839a20e40a0000000000000000000000000863127ec48631218c48631218c
49a3121ec48631218dc87b127ec485b127) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1f00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0c0080082000080002002880028000a000220818000202809000220038800020002000020008031000000000000000000002800ca0032800ca0032800c800b2000ca0030000c08030000ca0072800ca0032080ca00300310000000000000000000008815220548815220548015200c4803522044
881122054881120064881522054803522054000000000000000000000001080c42011080042039000642009080642009080242019080242009080442011000442018000000000000000000000001800860001800460001800060001800060001880060001880060001800060001800060000000000000000000000
0000038804e20138804e20938014e22138) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1f20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0430010c00400002000000000000000000030000c00030000c02030000402130080c00030004c00030004c02030080c00030000c00000002000000000000000a88030810c20430810c244308104604b0810c20430010c20430010c24430810c20430810c2042a202000000000000000000419000
64001900064009980240001900260011980064009900060011900064001900064002800800000000000000000c01880062001880062001880066001880066001080062001000066001800060001880062002031000000000000000000c001000040001004044081102860021102040001800004081800040001000
0400210000400203100000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1f40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (018200608018200608018200608018200608018200608212000000000000000a88428800a20028800a20028000800028800800000800a20000800800028800a20028800a2002a202000000000000000008018810620418810620418010420418810c20410810620410810c204188106204188106
2042020a000000000000000080010010400410010400410010600410010c00410010400418810c00410010400410010400428002000000000000000a88018810620418810620018010e20898810620c1083062041a03062081881062041881062042a202000000000000000880030010c00430010c00430810400d
30010c20c30034c00430234c20c30010c0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1f60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (8843a818ea863aa18ea06ba018c0063a818c28611018ea0630818e206baa18ea063a818ea062a20a000000000000000088039818e40639018e40639018e20639818c80639818e6063b018e80639018e40639018e40628002000000000000000000038818e20638818e202b8808e20238808e6063
8818e20238018e606b8818e20638018e20628000000000000000000a8802b018ac062b018ac062b018ac06ab018ac062b818ac062b818ac062b018ac062b018ac062a2020000000000000002000020100804020100804020100a040201048840201008040201008840201008040201008040001200000000000000
0208008018200608018200608018200608) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1f80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (040881022042a202000000000000000288010010420418810421418810421410050620418810620518810421410850420410810420428002000000000000000000018012600410010601490010601498052400410012000480812601498050600418012600428002000000000000000a88038001
e20070801e2007a801e20078101c20070801c20070201e20078901e20078801e2006a200000000000000000000018018600618018600618018620618018620610018620610018628618018600618018600600002000000000000000a88012012480412010480482010400492012c8041201248049a012c80492010
480412012480400002000000000000000a) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1fa0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (082e28091002642091802e01099002640019000640028002000000000000000000018000620018800623018880661018080660018800622018800641018000620018000600028002000000000000000a880010100404010140404000148624010900404018100404010100404010100404010140
4042a202000000000000000000008004200108000200108000800108004200018000200008000208108004200108004200100002000000000000000888028030a00c28030a00c28030804428010a00d28010a00528010a04c28030a00c28010a00c00002000000000000000a880088102204288302240088302000
08800a00c28030a00c2883020000880022) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1fc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (80010000400010004400010004600010020400110800400010000400010000400010000400028202000000000000000a88018830620c18830621e98830e20e9887a600c18030620c18830220e88862620c18830620c22202000000000000000800430028c00a3002ac05eb012a4012b004ac20a9
000ac0429000ac21ab006ac00a30008c00a00202000000000000000a88030020c00830020c00a30020405e30068400810020c00810020405e30078c00830020c0080000a000000000000000a88030801c20070801c20070001460070801628050001c20050801620070801c20070801c2006a20200000000000000
0008019000640019002647099002401099) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1fe0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0138804e2010a00200000000000000088802b02cac0b0102cac7b2802cac0b230ac040b21a2cac2b0102cac1b2b02cac0b2b02cac0b2a2020000000000000002080020140805020140875021140a0d02094080500014086502014080502014080502014080520000000000000000000080008104
204128104200128004204108044a04128104280128104204108104204108104200100002000000000000000a88028800a22028880a20028a80803028880a02028880a22028880a00028880a22028880a2202a202000000000000000000018884622118880624198880420998806602018880622018a80620198806
6221188806221280020000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2000) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (fbf27edc9fb72fedc9fb727ffc9fbf27edc9fb72fedc00000000000000000000000027e90992426492fffcbe492f97cbe5f0992426492f924264909ffc265f0992426492f92400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000bfbf2fffcbff727edc9ff727edc9fb727fdc9fb727edc9fb727edcbff72fffcbfbf27ffc00000000000000000000000094b525ad496b4242d092b4242d090b424ad090b4242d090b4242d096b425ad494b524ad40000000000000000000008038804e20138804e2013a804e209
32804e60138804ea0138804e61138804e0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2020) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000030c2000c000040408004000c000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000009fb727edc9fb12fffcbfb1218fcbe3f21ec486312f8c4863121ffc9fbf27edc9e3727edc000000000000000000
0000009ff727edc9fb72fffcbfb72fefcb) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2040) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2060) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2080) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (20a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (20c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (20e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2100) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2120) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2140) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2160) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2180) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (21a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000030c2000c000020408004000c00000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (21c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (21e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2200) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2220) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2240) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2260) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2280) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (22a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (22c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (22e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2300) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2320) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000030c2000c000060408004000c00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2340) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2360) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2380) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (23a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (23c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (23e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2400) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2420) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2440) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2460) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2480) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (24a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (24c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000c2000c000010408004000c000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (24e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2500) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2520) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2540) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2560) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2580) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (25a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (25c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (25e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2600) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2620) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2640) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff00000000000000000000000000000000da8b00008000000c
020000008005000ca00000008001000c0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000003002000cc00000008001000c8cde00008000000c000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2660) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0001) TDO (0000) MASK (0000) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'serase' instruction. 
SIR 8 TDI (0a) ;
RUNTEST 37000 TCK;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) SMASK (ffffffff) TDO (f5034093) MASK (0ffeffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) TDO (00) MASK (00) ;
SDR 16 TDI (4000) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'usercode' instruction. 
SIR 8 TDI (fd) TDO (00) ;
SDR 32 TDI (ffffffff) SMASK (ffffffff) TDO (00000000) MASK (00000000) ;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) TDO (00) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'usercode' instruction. 
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) TDO (f5034093) MASK (0ffeffff) ;
SIR 8 TDI (e6) TDO (00) ;
RUNTEST 50 TCK;
SDR 32 TDI (00000000) TDO (ffffffff) MASK (ffffffff) ;
//Loading device with 'conld' instruction.
SIR 8 TDI (f0) ;
RUNTEST 110000 TCK;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) TDO (f5034093) MASK (0ffeffff) ;
//Loading device with 'ispen' instruction.
SIR 8 TDI (e8) ;
SDR 6 TDI (34) SMASK (3f) ;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) SMASK (ffffffff) TDO (f5034093) MASK (0ffeffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) TDO (00) ;
SDR 16 TDI (4000) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fdata3' instruction. 
SIR 8 TDI (f3) TDO (00) ;
SDR 6 TDI (3d) SMASK (3f) TDO (00) MASK (00) ;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) TDO (00) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fvfy3' instruction. 
SIR 8 TDI (e2) TDO (00) ;
RUNTEST 1 TCK;
RUNTEST 50 TCK;
SDR 6 TDI (3d) TDO (3d) ;
//Loading device with 'conld' instruction.
SIR 8 TDI (f0) ;
RUNTEST 110000 TCK;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) SMASK (ffffffff) TDO (f5034093) MASK (0ffeffff) ;
//Loading device with 'ispen' instruction.
SIR 8 TDI (e8) ;
SDR 6 TDI (34) SMASK (3f) ;
//Loading device with 'conld' instruction.
SIR 8 TDI (f0) ;
RUNTEST 110000 TCK;
//Loading device with 'bypass' instruction.
SIR 8 TDI (ff) ;
TIR 0 ;
HIR 0 ;
HDR 0 ;
TDR 0 ;
TIR 0 ;
HIR 0 ;
TDR 0 ;
HDR 0 ;
SIR 8 TDI (ff) ;
SDR 1 TDI (00) SMASK (01) ;
