// Created using Xilinx iMPACT Software [ISE Foundation - 6.3i]
TRST OFF;
ENDIR IDLE;
ENDDR IDLE;
STATE RESET IDLE;
TIR 0 ;
HIR 0 ;
TDR 0 ;
HDR 0 ;
// Validating chain...
TIR 0 ;
HIR 0 ;
TDR 0 ;
HDR 0 ;
SIR 8 TDI (ff) SMASK (ff) TDO (01) MASK (03) ;
TIR 0 ;
HIR 0 ;
HDR 0 ;
TDR 0 ;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) SMASK (ffffffff) TDO (f5034093) MASK (0ffeffff) ;
//Loading device with 'conld' instruction.
SIR 8 TDI (f0) ;
RUNTEST 110000 TCK;
//Check for Read/Write Protect.
SIR 8 TDI (ff) TDO (01) MASK (ff) ;
//Loading device with 'bypass' instruction.
SIR 8 TDI (ff) ;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) TDO (f5034093) ;
//Loading device with 'ispen' instruction.
SIR 8 TDI (e8) ;
SDR 6 TDI (34) SMASK (3f) ;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) SMASK (ffffffff) TDO (f5034093) MASK (0ffeffff) ;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) TDO (f5034093) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0001) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'ferase' instruction. 
SIR 8 TDI (ec) ;
RUNTEST 1 TCK;
RUNTEST 15000000 TCK;
//Loading device with 'conld' instruction.
SIR 8 TDI (f0) ;
RUNTEST 110000 TCK;
STATE RESET;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) SMASK (ffffffff) TDO (f5034093) MASK (0ffeffff) ;
//Loading device with 'ispen' instruction.
SIR 8 TDI (e8) ;
SDR 6 TDI (34) SMASK (3f) ;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (080280000000000000000000000000000000000000000000000000000000000000000000000c400000000000000000054ede80000000000000000000000000000000000000000000000000000000000000000000000d53ff00000000000000012820000000000000000000000000000000000000
00000000000000000000000000000000000c48000000000000000001210000000000000000000000000000000000000000000000000000000000000000000000000c48003102000a0002000c800000008001000c000000008004000c900000008001000c638000008003000c6dfc01008004800cd0000000800680
0ce00000008001000c66aa9955ffffffff) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0000) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (007401dd00770801000000000000000e000cc01ff007fc01f3587ec093b0240d09330406c4035000ec04b7004cc0173000ec01ff007fa00300000000000000012adc1e000400010000500014000500014000500014000500014000500014000500010000400048ff000000000000000420000000
00000000000000000000000000000000000000000000000000000000000000000000480000000000000000054ffc0000000000000000000000000000000000000000000000000000000000000000000000015bff000000000000000d66fc0000000000000000000000000000000000000000000000000000000000
000000000000015bff0000000000000001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0020) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (429b0024c069f0032c00d700a6c13530227c00df003508030000000000000006001fc00ff003fc00fb043ec00fe103fc003b004ac417f114f4a98f040ed087b042fc00ff003d8007000000000000000e2008c00df0037c00d70037d009f2034c83144046c07170926c21970841c00530147c00df
0037a8020000000000000002200c400dd0037400d500354305000344019521254084110044005000e5402d10067400dd00358803000000000000000e8040400cd0033400c508314044d21004a4150002400850013402c40805420c10023400cd0033a010000000000000000c2004500dd0077401d1003008051003
4400110084480510044403150044440514) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0040) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (600bc00ff003fc00f70037c00ff0234c08b3982ac041f1024e001b0023c08df0037000ff003db0020000000000000000404bc00cf0033c00cb2171c80d74343c881287d14859f0811ca4810402c08d30067c00cf003010120000000000000002001b401ed0079401e90678001ec037b449a5026d
4092d824940121006840961486b401ed00788006000000000000000a001f400dd0033400c940354019194474410501115000d8001400814042480510067600cd0032a0070000000000000002004f400dd0035c00d10034060df00344058500740105d0004400db0064441510027400dd0034a01300000000000000
04200fc00df0037c00d30035c0adf0235c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0060) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (207c001f000700120000000000000006205fc005f0017c00570016c627740dcd117f80ddc4473005ac027f0b5cd825f005fc004f0015a817000000000000000c204b400cd0033400c50032404c58470400c10031405c120b2404cd80f2400c941b3400cd003328120000000000000004000f401e
d007b401e5007a441f580fc601ad13f9501e1047a50d8d0078481ed4063401ed007900030000000000000006204f400ed003b400e14038400e10038400e1002d400a10018404ed002ac10f1003b400ed00398813000000000000000e0057c00df0037c00d30874d4193a034c019b2036ca0130024c009f0024c059
d4007c00df0037a0150000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0080) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (40160105c84434115c041d0007c001b0105c001f0006b01c000000000000000080434008d00234008d00236608d4023400c02520494810523414890023400c185204008d00202010000000000000000200634009d00264009d00a74069001a7420dd00a44009100254049d00274809940254009d
0024a018000000000000000800074009d00274009d02a74239f00a34009110ac42b9100a6c25a904a74419104644009d00262001000000000000000c2043c009f0027c009f0067c00930027c42974121c20930024d009f8127c04db0921c009f00270810000000000000000c004bc001f0007c001b0005c001b000
7c501f24044000f5105c0a1f0007c0e170) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (00a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (20634009d0027400918023428990024402d500215249108344409d08244009104274009d0025a818000000000000000a80434048d00234008181234148185224909504a14088120a04008d00206048542234008d0023a010000000000000000c20734011d00074001141070011b0044405114055
4961110844021d00044041115874001d0007081c000000000000000e0063c029f0027c009300afc00a3002ec40bb806dc04b3002cd51bf002c022b3012fc00bf0027a018000000000000000e4067c009f0027c009f0527c14af452bc14af052fd14ff1028400bb282fc149f452fc009f0027901900000000000000
0ac073c0a1f0007c001f0003c00131807c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (00c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (03b400ed00388005000000000000000a0053400cd0033420c96070401c50033441c004f0687c90071405cd0ab2580d14073400cd0032a014000000000000000200534005d001740051005c4007303df40070209c40271405c4606d001c40171045f4005d0014a01400000000000000042053c001
f0007c00130004d001b1007c601b1005c40172000d001f0804c12130087c001f0005081400000000000000060057c009f0027c009f0427c009f0027c009311268008f00a7c859f0667d449f0663c009f00258015000000000000000e2017c009f0027c00930027c01b1002ac40a520e5c229341a48019d0124c049
740a7c009d0027a8050000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (00e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00a9040940885003a4206d0138404adc12b400ed0039000000000000000000062057400ed003b400e10264445e1004ac01f121584058d007a431ed0078409b10767400ed00398815000000000000000e0003c01ff007f801f30a7cc01c30058421970a65c09ff007f805f7027c009f4006fc01ff
007fa00000000000000000066043c00df0037c00d70017c009b0007c00972007d00170036c408d0805c009f0027c00df0835b81000000000000000004057c01ef007bc01eb007cc03e740cfc87e3405dc013f0079c01ada07ad01f3007fc01ef007810150000000000000002001740ced003b000e90438455a5310
b410e10098602290431402fd103a402a10) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0100) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0207400dd0037400dd0046d129154d44829120e74615108b7c009102c04059540c7400dd00362081000000000000000c2203c00ff003fc00fb012c409b3001ec08b040afc107b143bc40bb007ec00b3002fc00ff003e0880000000000000000c0007c00df0037c00d700b5c00172055c00500435
ca05f0216c04df20b7c029700a7c20df0037000100000000000000062057c00ff0037c00db4036501174014c0f1f4021c07df1096c83df0034c009f0067c00dd0035a815000000000000000c2013400cd0033400c900024089900064029d20824238d80b24024d04105091901a7400cd0033280400000000000000
040003400ed003b400e9013a404b5008c5) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0120) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (077401dd00770801000000000000000e000fc01ff007fc01fb0877881f70336c00ff524cc08130245c03836057c015f0077c01ff007da003000000000000000ee097c00ff003fc00ff0104c00bb0107c08bb030fc0c1f0227c285f2807c021e4507c00ff003f98050000000000000000c003c00d
f0037c00db0604810910306c00970180c461b09274845b0d06c84970107c00df0036b00000000000000000008043400cd0033000cd8103604450500500442097482010101004c10010404050523400cd0030201000000000000000020007400dd0037600dd00954805500444001d0084406198107400d914164c11
550c7400dd0034a0010000000000000008) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0140) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (80db1087c041700a7c021300b7c10df0837c00df003508030000000000000006001fc00ff203fc00ff203fc00f9003ec00ef002cc24ff00dfc10bbe83fc217f003fc00ff003d8007000000000000000e200bc00dc0037c00db0034820d70037c00df4045c041700c5c059722f7c135d0037c00df
0037a8020000000000000006200f400dc0036000d11837400d50035420d11065400c140344019500074a45d2037440dd00358803000000000000000e8043400cd0033400c90030420c50133402cd08014800500054248500134804d0033400cd00332010000000000000000c2007001dd0076401d10037401d12b3
4423d10100880d120004049100574c15d8) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0160) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (600bc00ff003fc00ff0037c08ff083fc10e3002dc041f103fc28ff003b0007f0237c00ff003db8020000000000000000404bc00cf0033c00cf0272c05cf8175c25cb00e1d05151553c05c900d34114f0873c08cf003010120000000000000002001b401ed007b401e5007b415e9037a605e58048
4012101e840da1017f485ed007b601ed00788006000000000000000a001f400cd0033400c900b6400c90034010c90405702040042480990013403cd8033400cd0032a0070000000000000002004f400dd0037400d703f744bda003e800f10024402d100704049a0833400dd1037400dd0034a01300000000000000
04200fc00df0037c00df2036c00d52035c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0180) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (007c001f000700120000000000000006205fc005d0017c005f0017c005b0817c005e041cd0173601dc006b0013c015f0017c004f0015a817000000000000000c204b400cd0033400cd0033400c10033480c500f0702c10034401c11073419cd0033440cd003328120000000000000004000f401e
d007b401ed2079401e9807b481e5886c603c10079403f900db401ed007b401ed007900030000000000000006204f400ed003b400ed203b400e1213f400e14038400210038420e1103b408ed003b400ed00398813000000000000000e0057c00df0037c00df0837e40dfa237c00db0020c00130037c009b0513c049
f0037c00df0037a0150000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (01a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (84172004d04134000400130007c005d00054001f0006b01c000000000000000080434008d00234008d00214008155234348d00264148140204809140234008d00204008d00202010000000000000000200634009d00274009d02a74009000274809581244108104347029100274089d08254809d
0024a018000000000000000800174009d00274009d20e5c189100274249b0062d409110644a29108274009d00246009d00262001000000000000000c2053c009f0027c009f0867c01930023c00914064c88930164c18930037c01df0025e009f00270810000000000000000c004bc001f0007c001f2007c001b000
7c02131107c861f00c5c02170047c021f2) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (01c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (20634009d00274009900234009580244009880204108100a07089d18244109100274009d00258818000000000000000ea0434008d00236008921234008180224808904204188160214109d00204009900234008d00230810000000000000000c00634001d00074001141474001503c440a110054
4030101444855c00044401110074001d0007001c000000000000000e0063c009f0027c009300afc00b30b66c01bb402ad04b340bdc00bf002cc009b402fc00bf0027a018000000000000000e6067c009f0027c009f0525c009f4527c009b052dc14bf052fc54af4027c009f0027c009f0027b81900000000000000
0ac063c001f8007c801f0007c00134107c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (01e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (03b600ed00388005000000000000000a0053400cd0033400cd0073413491030483c56471421cd2032482cd8033404cd0833680cd0032a014000000000000000200534005d0015c005d00df4827b081458371215ee0971005c4016f08174014d00136805d0014a01400000000000000042053c001
f0007c001f0107c00130004c501b2085c00170004c041f0007c081f0007c001f0005081400000000000000060047c009f0027c00972027c009f0023c00870027c039f0127c009f0167c80df1027c009f00258015000000000000000e2017c009f0027c009b0027c20934026c209a00a4c02932065e01bf2024d0a9
b0027c009f0027a8050000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0200) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0021031850005080c5403900384006d013b400ed0038000000000000000000062047400ed003b400e30049400410039400810070519a1011841ca328384006d017b400ed00398815000000000000000e2003c01ff007fc01fb005dc01eb0474c01a34256c0133486cc09fb8078c03ff107fc81ff
207fa20000000000000000062043c00df0037c00df0007c00d7c837c00430027400971015c00df0037c029f0037c00df8835a81000000000000000000057c01ef007bc01ef004bc01eb007cc016700694812f204ed05fd007bc016f007b401ef0078001500000000000000020017400ed0039400ed042b41069803
8410e5183c490e9009a418a5203b400ed0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0220) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0207400dd0037400d108174035b00344279104a4900dd00344405d1037401dd0037400dd00362081000000000000000c0203c00ff003fc00f3427fc00730035c00a3020cc017f002cc08ff883fc007e003fe00ff003f0880000000000000000c0007c00df0037c80d70095c025d3037c009f0065
ca0da24b7c00170037c00df0837c00df0037000100000000000000060057c00df0037c40db0034c001f003cc00911004c0bd70434c0a9b0174c00df0037c00df0035a815000000000000000c0013400cd0033400c10007400c100355008104b04029500504831904305894d0833400cd0033280400000000000000
040003400ed003b400e98008400ed80384) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0240) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (877401dd00751001000000000000000e000cc00ff007fc01fb050ec301b403bc00130056c003f005fc017b030dc843b007fc01ff007fa083000000000000000e4017c00ff003fc00ff0207c947f233fc00bf233d400de203ac002f003fc806f2237c20ff003fb005000000000000000ac003c00d
f0037c00d300a3c02931035c08134010c165f2224c021d02b7c0a5f00b7400df0036b00000000000000000008043400cd0033400c1088340049123040081223040ccd00315290d10334004d01b3400cd0030201000000000000000022007400dd0036400d104274239100354019900100445d00a44009d0037408d
d0037400dd0034a0010000000000000008) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0260) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (065f00b5c421f0027c205b4086c024f0037c00df1035000300000000000000060017c80ff003fc00fb025fd43ae803f609db002dc005d0c1fc90bf014f8451f003fc00ff003d0181000000000000000e2020900df0037c00db04168015b4033c005344e6c891f1047c01db0085c221b0037400df
103520800000000000000006200c400dd0037400d520204101510344820160564308c2077411513024402510837400dd00352003000000000000000e804c410cd0033400c910005800908b25400104124000d0033420492121480490033400cd00312010000000000000000c200c404dd0077401d100a44239500f
4440911134480dd0077441110304428110) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0280) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (600bc00ff103fc00f3083ec086f2037c807f1217600bf003fc007f402fc20bf023fc00ff003d38020000000000000000404bc00cf0033c00c30241c000301714150f2051d110f02d3c0dcb01f2c018f2173c00cf003018160000000000000002003d401ed007b401e50261401a10178429ad0078
405eda07b44161024050dad017b401ed00780006000000000000000a001f400dd0033400c1410142b0140b04210d0c554810d0013402c900164078d0033400cd003020030000000000000002006dc00fd0037400d1045440211003c6035c012442a1d21274061103d4411dd0033400dd0034201700000000000000
04200fc00df0037c20db0095c86534135d) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (02a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (007c201f000500120000000000000006205fc005f0017c0053019dd017f00146027b009fe227f011fc017f0add402770017c005f00142003000000000000000c204b400cd0033400c50075450cd0030551d9101740fcd08d3445450234498dd0033480cd0031281600000000000000040007485e
d007b601e10069701e52370401a9045b421ec005b401ec205140125007b401ed007900000000000000000006204f402ed003b400e5a00040085003844081203b4006d101b400e210284006d203b400ed00390813000000000000000e0057c00df0037c00d30004c415b203cc00130017c001f0817c00db0015c001
70037c00df003520100000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (02c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (841340104241b2007400114106c040f00074001f0006101a000000000000000080434048d00216808105214148955204348180204148d3023400c005204148d80234008d00200010000000000000000200634009d00276009100a74209900254849150247108984274809190a65009d08274009d
00242018000000000000000800074009d0025c00910065c019b14a44059100e6c0a9d00274409100e45129d20274009d00242001000000000000000c2043c009f0027c00930167c84930821c00930165c019a0627e85938166c059f0027c009f00250010000000000000000c004bc001f0007c001f040680a16000
7c08174987c001d1087c0a190007c001f2) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (02e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (20634009d0027400910020408950027600dd10354049101270409152204009d00274009d0025201c000000000000000e804b4028d00234208104224288008234848d20215988100234408500a15828900234008d00212016000000000000000820734171d000740011034440056000451f1d0150
4035100174005141c44834d10074001d00050018000000000000000e0067c019f0027c0091006ec01bb0568c21bf38aec24b9102fc00b501edc07bb002fc009f0027a018000000000000000e6067c1c9f0025c009f052dc00b74027c14bf052f414bf202fc00bf453fc14bf0027c009f0027b81900000000000000
0ac077c001f0007c00134107c84530905c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0300) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (03b400ed00380000000000000000000a0050400cd0033400c90871400c900b2301d12070403cd049344a410970140cd0033400cd00302010000000000000000200504005d001740053005ec1065001ec8371441c0227d005f4037101dc4067d20174005d0014290000000000000000042050c001
f0007c20131104c901b0104c0a134485c860f0087c22134084d000f0007c001f000500100000000000000006005fc009f0027c009f00e7c009f0020c129f00e6c009f0027c109f00668199f0827c009f00250013000000000000000e2017c009f0027c00934166c01931027c059f0027820934023c08972865c239
b0027c009f002520050000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0320) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (80cd812a42420023d40061083840068213b400ed0039000400000000000000062057400ed003b400e50271408eb035140c6d0378c1d95061281841011084e010373400ed00390815000000000000000e000bc01ff007dc01f30264c0df30358c897f206ec211b025ec0166107e409334073c01ff
087d210200000000000000066043d00df0037c00df0017e20df0017c009f00168001f1017c00df0807c001f0037c00df0035381400000000000000004054c01ef007bc01eb0060c21cb0858801830049d01bd007b421e310484c1ef087bc01ef0078001000000000000000020014401cd003b400e1841a440e4041
a480218059402ed040b4006140204006d0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0340) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0084400dd0037400d10044c13db11c28031b02404131b21f50d3c180044001d0037400dd00342083000000000000000c2004d00ef003fc00f30144d90a3400dc092f004c42073013cc00f38044e087f803fc00ff003d0080000000000000000c0027c00df0037c00df0001c085f0087c821b0007
c068700a7c021f4183c12970037c00df00350001000000000000000620d3c00ff0035c00d34656623d10004413dd2876c02533070c49930994c049b0037800df00352010000000000000000c201b400cd0033400c54013503c18011631cd83b04010501124214110d0600190033400cd0031280200000000000000
040003400ed0039400e1000a604e1c2184) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0360) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (044401dd00771801000000000000000e000cc0173000ec003f0044c0123113ec006b100fc0195000cc0133000cc013b1840c01ff007fa003000000000000000ee017c00ff003fc00ff090dc20ef8917c003b0106c043f201bc047f210ec003f023fc00ff003fa8010000000000000000c004c00d
f0037c00d30504c02d00515d02170605d12530234448d100a44024d18b7c00dd0034100000000000000000008040400cd0033600c14322408c943124480921056868900014001120805888d0333400cd0030281000000000000000020004400dd0036440d10424641d10055080100005424518014001d162a44009
d8037400dd003420010000000000000008) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0380) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (32170c34c00d70447c03930007c009780a4c00df0035080300000000000000060017c007f00675088f003dc006f803cc006720c7c08bf001fc107f0401c303f002fc00ff003d8005000000000000000e202ac00534144c111f2237c00d30037c031b0047c419300c0c011300c4c130b0844c00df
0037a8020000000000000006200c4205102144005d0437401d51837401191817420d14844403110446441110844700dd0035a003000000000000000e804e400410000400050033400d10033400090013400810000400814802420891004400cd0033a010000000000000000c200cc015100444011d1075401d5027
c401510047401910005421512046401110) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (03a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (600bd006f003fc00ff8a7dc20df153cc00df2215800ef101fc2837021fc00f5013dd00ef003da80200000000000000004048c00430020c008e0972c82470b71c16c70352d01874087c08834003c00c503e2c20cd003210120000000000000002003c401710078401ec034a409ad0179401e9214a
401e9004b44929004b619a9002e401ed007a0806000000000000000a001c400410000400081032400c50031400c500826048500834000102436008d0002400cd003220030000000000000002004c411410034400dd0034402dd103c4019b0030002db00d74004100d7440990020420cd0034a01300000000000000
04202cc04534030d00df0004c5097083ac) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (03c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (007c001f000580120000000000000006205fc0073049cc01730655c02530011c117f01dfc015f209cd0473001f40a75401fc005e0017a817000000000000000c204b400414070509c1404840229c033466cd00b3408cd6270403010372440c108b3400cd00332016000000000000000400074016
10070401c10079421d10079601ad007b401fd004040121004b401f5006f401ed007900040000000000000006204f400610038400e10038c00eb8331400ed0018400e5a038400214808080a1002b400ed00399813000000000000000e0057c00530054c20530871c80d3213cc008f0004c01d78804c011300014219
72003c00df0037a0100000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (03e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (041f0107c00150106c00130105c00178807c001d0006b01c000000000000000080404009d05204148d0028400b10521494cd0523400cd85234008145334008900274008d00202814000000000000000200604019d04254309d202c400b104256009d04274009500264049100256809d00274009d
0024a01c000000000000000800045808d00a45029f00244409040244218d00674089f01674009140e749b9908234809d00262001000000000000000c2040c009e0024c009f0024c008300244859f0167c019202228009b2163c01970427c009f00250810000000000000000c004bc001f0407c010f0005c0417108
5e821f1184902150487c841f0085c021f1) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0400) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (2063400bd002c400bd222e484bc00254029108276c19500244009102274819100274009d00252018000000000000000e804b400ad00e8402a5002b400ad08a84008100a74408104204008140274008520274008d00210012000000000000000c20734003d00844225d00064001d0005402110887
4a01500044401100070005100074001d0007181c000000000000000e0063c009f0024c049f8027c00df0164c14b3012e400b3042cc00b3042fc00a7002fc00bf0027a018000000000000000e4067c00bf002fc00b70027d009f0826c00bf002fc00af052fc00ef002f880a7002fc809f0027a81900000000000000
0ac070c001f0104c041f100cc00130105d) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0420) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (03f400ed0038880100000000000000008053400410070401cd01b3400c50030580c10432601c9207349ac90032401c54033400cd0032a014000000000000000200534005180144005d009740051001441171005b4087f401f48275005840f7100174805d0014a01400000000000000042053c003
38004c020f2087c00130804c10131087c08134307c801b0486c22170087c001f000508100000000000000006005fc009f0267c049f0027c009f00274049f50678009f2023c039f1027c009f00e7c009f00258013000000000000000e2017c009f00e4d019f0427c069f1024400810326c00934264d018324a7c019
70123c009f0027a8050000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0440) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0429200b4042d1309404f1010f40869113b400ed00390000000000000000000620574006d032b424ad015b4012302734552d096240d65004842de1004b405a1407b400ed00390815000000000000000e0003c017f026fc01bf0057c09b20a77c0579036fc01570b45c01d04263c09db0073401ff
007d280000000000000000066043c001f0017c805b2037c005b5017c001e4023c005f0007c805f10074a01f0033c00df0035a81000000000000000004057c01214050d014f807bc01e70058c4123006bc016b005fc21eb204ac81e7007bc01ed00781011000000000000000200174006100f8402ed003b40265007
04004000bf4406d801b400650420621f12) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0460) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00074049d001440051c060400510041c071d00c74051101474011501c6401150037400dd00362085000000000000000c2203c00bf001cc0073002c500f300c7c813d002fc40330007c00fb100bc14f3003fc00fb003f0884000000000000000c0007c02df0177c11df0127c405700278821f0886
c02172917c015f01e7c00df0037c00df0037000100000000000000062057c00df20f7c41cf0127c01c34027c011b0967c001f0495403d10027802db0173c00df0035a815000000000000000c20134000d00034020d00534980100134070d88024890d00444108100834020124f3440cd0031280400000000000000
0400034012d000b6002d011b444a1091b4) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0480) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (047401dd00771801000000000000000e000fc01ff007cc012b0106c003b1848c01eb024ec001f182dd00bb024cc203f0047c01ff007fa103000000000000000e6017c00bf000fc003f030ec001f430dc001f0507c263f120fc08ad000e8083f013fc00ff003fa805000000000000000ac003c009
f0004c00130104c14930107c141f0587c00131107c84db0007404130537c00db0036b00000000000000000008043400cd00205a08103014040103214040d090360c01d003400c54402424850337400cd0030281000000000000000020007400dd10244009901044209100274041d00e7401110047401d900474809
10037400dd0034a0010000000000000008) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (04a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00df0407c0c1304f4d83db00b4c01d34007c00df0035080300000000000000042617c00ff003fc003f08ffc115f000ec00fb002c840ff0026c00df041fc00df123fc00ff003d800500000000000000040013c00df0034c081f2046c18470845c818b08c2c00df0464c13db84d0d019f0047c00df
0037a880000000000000000ea01f600dd0035410150034400943447401d500e5600cd00744019108644019d0437440dd0035000700000000000000068043400cd00304001d8322420858001600c900064000d0030400890004400cd0003400cd8031a010000000000000000c0007401dd007540195059442115004
6c81d110040081d08044001121044011d0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (04c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (600bc00ff003fc003f002ec0853820dc48df1035c00ff182fc20ff003fc20bf023bc00ff003da8020000000000000000605bc00cf0031c000f2361480071843c48cf09614011740206008f0100d08c30373c08cf003210120000000000000000001b401ed007a4013d014b41125027e489fd8258
405210268409a50068401219b4b401ed007a08060000000000000000000f400cd00314004d0005442050103403cd02c14210500204009d0080400018403400cd003220030000000000000000004f400dd0036c000d0036e02d1144045bdd00e4600d100f4001d70474400c10037400dd0034a01300000000000000
04200fc00df0035c221f000cc42df2007c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (04e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (007c001f000500120000000000000004005fc005f0017c036f01dec01770018c0773021cc217b089ac416b065fc0273805bc005f0016a807000000000000000c004b400cd003340c0c00f0406cd80c16024900b040ac11370405c95073409810173400cda031201600000000000000040013401e
d007b4012d005a4112580c8421e1006a40129006e47189207b021e110fb401ed887900000000000000000006004f400ed003b4002d0038500a50009400e1003c400c14038400a5003f680a1003b400ed00391813000000000000000e2043c00df0037c001f001fc40070004c40c36024d00db8022c00930077e009
30037c00df003520140000000000000004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0500) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (005708044a41301044441f0007c841300174001f0006b01f000000000000000000434008d0023400910522414812020420911020414c115344149d00234148100274008d00202814000000000000000000634009d0025400910024400950625504d521204288100245409c00274809101274009d
0024a01c000000000000000020074009d0826c00910826c009100e4402810866c039100a46099921e74289100a74009d0026200100000000000000040043c009f0024400930024c03870065c40970024d019300a4d019f10a7c019300274009f002708100000000000000004004bc001f0007c001f0103c8015040
7c06171007c861f4087c80170087c101f4) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0520) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (20634009d00244089508244029100254009180a05089128355009119224029100674009d002520180000000000000006804b4008d00224009914a04028d0024400910120614890c234049501236028100274008d00210012000000000000000c00634001d00044001101c4402150015400114044
4035101c440a1500574221100074001d0007181c000000000000000e8073c009f0026c009b0064c21bb0028c20a320acc35bb156ed08b710afc05b3002fc009f00278019000000000000000e4077c009f0026c00bf052fc00bf202bc00bd152ec14bf453fc14bb052fc80bf403b4c09f0027a81900000000000000
086073c001f0005c00134104c04570005c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0540) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01b400e5003a0801000000000000000a0043400cd0033640cd8030503c102424005d8033401c10074001cd02b24c08d8033400cd00322014000000000000000000034005d00174004d0816c187e881d4237d009c40071009ec004d189c4015d009f400570014a01400000000000000042053c001
f0007c221f0084c421b0106c0e1f0184c10130484c201f0484c021f0187c001f000508100000000000000000205fc009f0027c009b0023d008f0227c009f0027c408f1066c019f2027c289f4027c009f0025801300000000000000040117c009f0026c129b0424c099f0020c98910024c009b02e7c0e971027c009
30023c009f0027a8050000000000000004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0560) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (802d3129444290028520b5052a410bd032b400ed0039010800000000000000040057400ed0038400e1113b41d244342c472d0650407215278481e3135ec09ad017b400ed003918150000000000000004001bc01ff007cc01eb0877c09f31144c093f027cc01930064c01870044c098f0257c21ff
207d204200000000000000066043c00df0037c00df0a37c00df00076005f003cc001f0017c40df0805c40df0827800dd0035881000000000000000006053c01ef007be41ef0178c01c0504ad016f206bd0173406c501bd105ac01ef004bc01ef007a101100000000000000020013400ed003b400ed203a400e5080
94006d203b4022100b8402ed002a423cd1) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0580) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (020f400dd0035c00d10034418111083c009108644009300c44019100c7401dd1057440dd003620a5000000000000000c2203c00fb003fc00f30039c403f088ec00fb00ccc10971028c00b3006fe01fd003fc00ff003d080500000000000000082017c00df1034c00d70137c64c60987c86df00ae
d42c702a7c08970097c20df04e7c00df0035800900000000000000060053c00df0037d06db017fc03d701c4c11cf0295485d91274c41c712b6c81df0007c00df0037a8140000000000000004200b400cd0033411c920f34020140d24420d0055400090010005c908724618d0003400cd0030200600000000000000
040803400ed003b400f98133404e582084) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (05a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0740215d007700010000000000000006800cc00bf007cc0033033cc001f800cc001b0807c01fb000ec003b001ec0133001f8003f007fa003000000000000000e6017c00ff003d000ff203fc081f020bd080f080688237080bd88bf020fc00bf233fc00ff003fb80500000000000000006003c00d
b0037c40d30435c04160b86c049b0c85522178404c849301274249f0397c00dd0036b00100000000000000008043400cd0031400c1a1b06400100275449113014064909004249101136108d0003400cd0030201000000000000000000007420dd0037400d10835400d500864089920954c45509044049101b34449
d0467400dd0034a0010000000000000008) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (05c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (001f5317c00930207c02170035c041300b0d061f0035080300000000000000062017c00df083e4001f483bc00570030c00770256040bf0027c003f80bfc003f201fc001f003d8805000000000000000e0000d099f2036c00130035d061b08d7c850f2057c419b2146c011a0046c01032096c0a0f
0037a0000000000000000006200d4101d00355185110344049500f74011d4427608d100654c31104344011100644005d0037a803000000000000000c80404001d2032400013031400010013420050023020c900004800900324201168320800d0031a010000000000000000c00054019d0075c01110bb450015006
4481150007401d1206542010003c400000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (05e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (600bc48ff123fc087c063dc04ff0007e08260137c00ff003dc40fb023fc807e103fc007f003db80200000000000000006048d00cf0030d080f0372d01450050c04070363c0dc34340d15150171405434070c120f0030181200000000000000000018401ed00784092d017a401e1014a40531024b
609e5836840f6509705292104704016d007800060000000000000000000c4008d0030400090032411050000008000007400c108c04011570345020101104030d003020030000000000000002004c400cd003440a0d003c502d38076c0b5100574009542a04011501344005100644029d0034a01300000000000000
04200cc025f0034c2a1f1034c28cf8214c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0600) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0064001f000508120000000000000004205cd006f0015d026720144a273c45cf2867005dd4453001cc0277211dc017b3019c0b7f00152017000000000000000c005840dcd003150bcd0034409d50002402c504b7401c9027040ed1207048ad901b3489cd1033283600000000000000040810401f
d0079421e50178421e1105842165a449401b10058401c50079401698079401ad007900040000000000000006404c400ed00384006d013ad00e50008600610820440eb001840061043048021003ac00ad00398033000000000000000e2040d008f0034d00470834c00938812e80035004ca1930014da01721b5c201
22014c009f0037a0100000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0620) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (84171107c00150104c041f2106c80130105c041d0006a01c000000000000000080404149d00205149935204148005307148105334008d8d224148105306008505204148d10202210000000000000000200614009d00244029100244209502244189520274009500a44029d0026502d180355009d
1024a018000000000000000800044009d00244489b20244079110e44829120e74809b0022c039000a45039500244068d0026200100000000000000042040c009f2024c01972024c24930060c019740e7c009f2124c089b0122c08930025c089f802508100000000000000004004bc001f00068041f0007c101b008
5c021b2004c201f0107c001f0005c04174) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0640) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (20604019d00244049500240228121244629c22274009d0064480d000a64019101344089da0252818000000000000000480484029d00224828104204048180216008d20234008c00a04878583204009900235008d00200012000000000000000400604021d10044001703c440a151284cea1f1387
4001f0004424110186c140100844221d00070018000000000000000e0070c049f0024c00b30164c08b3082de00fb00edc009c112fc06b701acc00bb042fc10a70027801c000000000000000e6077c00bf0027c40bf1d27c14bf002dc00bf052f880ab002bc14bf052fc14af402bc00af0027981d00000000000000
0ae070d041f2004c04171104d040341048) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0660) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (021400ad00388004000000000000000a00c0400cd0030407c59030533c1b070522c500c3420c11030405dd0053402cd9033402c50032a01000000000000000000042c004d00145036320144067100dc40071099e02051009ed2471441d4016110984026d0014201000000000000000042050c001
f0004d02172004c421b0006c841b0105c40100904ca01f08835001f0c07c001f000508140000000000000004205fc009f1027e00970023c419f4421c22870027c00970027d849f1267c109f1067c519f0024081700000000000000040014d049f0024d0493202490a918025403990125e409f8125c01944064c049
b0127c669f002520050000000000000004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0680) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (862d080b638e190094c4e5001d4912509384082d0239000000000000000000040054400ed0038404a50134400f1024041aad285b60dc10120408010182c841b2942c00ad0039081500000000000000040018c01ef007cd21bb0c74c01fb005ec8def037fe01d3007dc8df7005bc013d0070421ff
007d200600000000000000066043c00cf0037800833036c00938005c00930006c00df0837c00534007c005b0026c009f0035b81000000000000000006050c01ef0078c4127207c801f34048401a70049c41e14078c81ef005bc016f007bc21a70078181400000000000000060012400fd0038410a50839400e4043
0400852842080e18472700440000410650) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (06a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0204400dd00354219100344061010464031100d7440d070514031120c54075502644911d00362081000000000000000c2280c00ef003cc0097103cc02f34003c00b1200fc00f30136c808b141ac2073002cc009f203f0a80000000000000000c2015c00df0835c019e0036a015a0185c201f0e13
800df0617c021f10a7c123f0227c121f00370805000000000000000600d2d05df0034c018fa03dc02df40c45419d0017c81d3e0b5c4f9701b55408700a0c028f0035a0140000000000000004200a406cd00324000500356060592804810d1093400c120004024100c04010901024090d8031280200000000000000
040002400fd00384002d02394086500086) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (06c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (013001dd00770103000000000000000e840fc01ff007fc01fb1004c80391042c803b006cc210b3087c01134227c01970047c01ff007fb003000000000000000e6015c00ff103fc0037133fc443f0b06c943b0717c06fb0d0fc203f010dd803f020fc403f003fa80500000000000000086002c00d
f0034c001700b4c42120087c02170187c0cd30087c00930084c02330304c00170034100000000000000000000042400cd20314008108b0402011082020044013400c100415080100a16081501005001d00302810000000000000000a0006680dd10344519d00344008920c7401950457420d900254011148744019
14004401950036a0010000000000000008) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (06e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0a175035f001310b6c00db0025c00d70227c00df0035000700000000000000062017c00ff003fc80ff20bfc0030146e409ff103fc003f0026c003f603fc00ff005fc00ff003d0181000000000000000e0203c00df0037400db0484c011b8cc6c211b20a4c801b00e6c01134067c88974207c00df
003520800000000000000004001f400dd0037400d100145219d0125480912221434112075408d10077400910437400dd0035200300000000000000048053400cd0033600c900044000d9002440190020420d90132400c10027020850023440cd2031005300000000000000044007401dd0077401d1051040133006
4480110025441110024400110133400910) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0700) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (200bc00fb003fc08ff2205c00a7000fc88f7300fc001d202cc20ff012fc88fa0037c00ff003d28020000000000000000605bc00cf8032c80c78142c91450b40c83d707e5405034061c09db0361c1dd70163c00cf003000120000000000000000201b401ed0079601e1014a40131024c401610368
40131216940d210268405e10a59409ed0078000b0000000000000000001f400cd0032400c504036000500404304d016140001202510219200148085014740ecd003000130000000000000002004f4a0dd0035c00d124f04019104a0422810034600010034018d10030400d11075c03dd0034285f00000000000000
04200fc00df0036c00d70024d002f0094d) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0720) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (087c001f000500120000000000000004001fc005f0017c005f001d4007f111cc12770159d1371609dd077b025fc045301dd4005f001520030000000000000004004b400cd0033400cd24244408118424128900b0600011360403014037400c14444400cd0031201200000000000000000003401e
d007b601ed00694212d8848401a5007d441310071401e80073601e10069401ed007900000000000000000004404f400ed003b400ed0008090210008500eb083840021002840020402b400e10018000ed0039001300000000000000040043c00df0037c00df000dc04290004c409f0032e01030035c001a0027c409
30005c01cf003520100000000000000004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0740) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (04474006c001121044005b2107c40134003e401d0006001b0000000000000000a0534008d0023400810d63414810020514852027400895d21420910d634208100234008d00200010000000000000000200734009d00274209d0824500951224404952626480910034400d928374809125274089d
00242018000000000000000000074009d0027400930025c119104e04029100e74409310257418100274809120e74009d0024280300000000000000042043c009e0027c20970025c03971024c00842067c00930020c089b20e7c09930067c019f802500100000000000000004204bc001f00078001f1007c8a0f800
5c201f24050101f0007c061f0207c001f0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0760) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00634009d00274009908245109910270109900214089508244009100a74009101234009d0025201c0000000000000004004b4008d00234808101a04028928225088900214208524246109001274648104234008d00210016000000000000000c40634001d00074001b40c0402150005697018144
40011a1c44051100470411100474001d00071018000000000000000e0073c009f0027c209301ecc05bb0028c05b3022cc00a71465c00b354efc08b3082fc00bf2027a219000000000000000e0077c009f0027c009f153cc00bf002bc14bb052fc00b7252ec14af0d2fc14bf052fc009f0027b81900000000000000
0ae07bc001f0007c001f0104804170004c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0780) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01b4002d00380000000000000000000800c3400cd0033400c100f0426810001407010332500c50031413c96130581cd8173082cd08302010000000000000000000434005d001640051a29c40373001c44671005c0004d001348661a0184045d001f0867d0814210000000000000000042043c001
f0007c00130084c00180004c021b00068021f8807c02134084c801f0207c101f000500100000000000000004204fc009f0027e00970023c09870465c02870166d209b0127c019f4267c099f0067c009f0025001300000000000000008017c009f0027c00918024d029b02220029941a5c279534e5d189320274009
344e7c009f002520050000000000000004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (07a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00e1070e400fd023c450a0002b480e9210f4802d0039001800000000000000046057400ed003b408e500494508511cb48c81015140de10038400ab032b484a1005b400ad003900950000000000000004001bc01ff007fc09f3026cc01bb0a43ea9b30062c01e71078c89bf026fc01f3024bc093f
087da00200000000000000062043c00df0036400df201fd209b0006c00574003420df0237c00974813c009f0817c005f1835b81000000000000000086043c01ef007bc21e14058c01a31009d01e3405ac01e7007bc01e94058c01bf006bc01af0079181000000000000000082003400ed003a400e100b801085840
d60061801c400fd213b000a9043c441ed8) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (07c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0217400dd0037400db520440395a2f44095104e2c80d980344258100c46008103c04011d0034218700000000000000042213c00ff003fc00f3045ec00b7044c000bb002cc00f7a03cc00b3044cd02b3044cc00bf003d008500000000000000062017c00df0037c00df002dc109f0007c005f30b7
c00d71037d00d20237c009702a78001f00350009000000000000000e0053c00df0037c00d300f6c008b04c3c02130ae6d2ecf237cc0bd380b74819900374008f083520100000000000000004000b440cd0033400c512874218500c360e912001401c100f44038d00e74898900934008d0031280200000000000000
040403400ed003b600e1012e400b9100f6) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (07e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0004811100370803000000000000000e000fc01ff007fc01fb083ec14fb0b36c003b0840c6133004cc81ff084dc012b004ec0073007fa003000000000000000ea017c00ff003fc00f70403c046f118e8003a110ec08d3003ec8429050fc54bf0186f00ff003fa861000000000000000a4003c00d
f0037c40d31036c0a150b05d0a1b2604d0cd508b4c00933082e02d320044001f083638030000000000000000a043400cd0033400c90400400850805600016116420dd0231408c500104009103244008d18300830000000000000000a0007400dd8037420d120366239120054101d0a04440dd1034501d18196420d
190244015d1034a0010000000000000008) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0800) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (201b2087c04530027028d71025e021f0887c02c30035080300000000000000060017c00ff003e000ff803ec40ff083ed912b140fa00f8024ec00fc145fc403f100fc019f403d8005000000000000000e2003c00df0037820db9037c00db1035c191f00c1c91570001c00df0141c010b04c6c0253
0837a8080000000000000006000f000dd0037400dd0835400c90035480950845201150005400d509244911108444a4912831a803000000000000000e8043400cd0033400c920b3600c900316000d0007600152805400c40821400190002400c10033a013000000000000000c6007401dd0077401dd00f4402d9033
4441110045001114044501d50064420110) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0820) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (200bc00ff003fc00ff8234d00ff2637c80a7201fe001f0207c00de0023c00170907800ff403db0020000000000000008404bc00cf0033c00cf0170e00d72275c108183d3c0d430803c08c34421400070042d02c3003410120000000000000008201b401e5007b401ed0379421e1017840921014b
4116d004b401e1006c409210848401a14078800f0000000000000008000f400cd0032400cd0030223c18831401000281423492003081c10041410050106403c101b2a0070000000000000002004f400d70037400dd003d40bf0403cc219120974428d0167401c1007445311000440c9101f4a01b00000000000000
04200fc00df0037c00df0036c08d71037c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0840) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0844000f40070012000000000000000e205fc005f0017c00520014c005b0014c0577889bc0b73205dc805b001ec877b049dc02730015a817000000000000000c205b400cd0033400c52030400cd0835461cd02f340a8100b3000c102f0403c901f5513c10037281200000000000000000013401e
d007b401e10070101cd8179421ed105b4c161046d401e9007e40129005d411c1087900010000000000000006204f400ed003b400e541b8426ed00394406d800b40061401b680e10038480310008400e100398813000000000000000e2043c00df0037c00d3007cc00db103cc80163007c00538040c00db0016c201
30002c00d30037a0150000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0860) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (04171005c001f0007400110015c001f0005c84130000301d0000000000000000a0534008d00234008905204148905204748540246008d002340089002040081c0304148140202010000000000000000200734009d00264409d082448291002400091c0a54849d00276209540254009d422568291
01a48018000000000000000800074009d00274009d0824c2b9a20244869108244008d02276059b002051a8100a44029100e6200100000000000000042043c009f0026c009d0024c01870024c028700a5c219f2067c04930024c019f0065d0093006708100000000000000006004bc001f0007c001f0807c401f100
7c001f0487c001f1107c021f2187c12176) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0880) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00634009d00274009d00244808d00254209500e7401950027400d1002440291202440291083188180000000000000004804b4008d00234008d02204128d1420600cd0823480850823400810020414c101645808100232012000000000000000460734001d00074001d00845071d01c5602172007
4a0150807400110004000110504408114000081c000000000000000e0067c009f0027c009f0164405bf1564e10bf202fc00b3002dc00b30028e00b30028c00b300afa019000000000000000e2067c009f0027c009f0025c149f0527400ab002fc80bf002fc409f003bc14bf052fc00bf0527b21900000000000000
0ac077c001f0006c001f0104904171104d) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (08a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01f4002104388005000000000000000a0053400cd8033400cd0031403c14030482cd80834028d9071400c18433402d10033601c104f2a014000000000000000200534005d00174005d001741a710016c207120ddc267d245f4057b001b40271045b40261201ca01400000000000000042043c001
f0007c001f1007c00130006c90130807c041f0087c10130087c921b0047c1813080508140000000000000006004fc009f0027c009f0027c009f1027c23872427c409f0827e009f0027d039f4127c039f00258217000000000000000e2017c009f0027c009f0024c009f00244069f08e7c339704a3e009340244829
12064c22932827a8050000000000000004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (08c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (4061812e4087100384042d1c3b4ee25011a410210019000800000000000000046057400ed003b400ed207340fa14278405650178cabcb03784012d016b48d61035040021020d88150000000000000004000bc01ff007fc01ff007fc01d3027cc09d70062c0173006ac097f017fc0975005ec81b3
007fa00200000000000000062043c00df0037c00df0037c005f223fc80572033c409f2037c009f2027800170007c201f4035b01000000000000000004047c01ef007bc01ef807bc21230978c01eb006bc01ef906bc01a2007b40123404b401e30078101500000000000000022007400ed003b400ed003b40061017
2440094c7d480ad002b400e9a02b400610) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (08e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0217400dd0037400dd00344225f0034402d14c7740a1d00264091d10f74131100445111d00a62021000000000000000c2017c00ff003fc00ff003cc083b0834c03d3042fc003f023fc203f083fc037b104cc008f00ff0801000000000000000c0007c40df0037800df0036c005f003685adf9035
c0c1f0035c229f20b7c001f00a7c001f4027000100000000000000062073c00df0037c00dd2037c4093003dc02c71132c21131824c409d2257c515712a6c01930034a81c000000000000000400db400cd0033400cd00334809180314014500b0402c902204000d00a3400010094511010013280600000000000000
040023400ed003b400ed803b600a109395) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0900) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (004401dd00771801000000000000000e040fc01ff007fc01ff1838c042b2104c00330003c0033040cc0033010dc047f000dc01ff007fa083000000000000000e2017c00ff003fc00ff8136c003701b7c007e233fc7c4f0236c080f0037c801f0716c803f000fb805000000000000000ac007c00d
f0037c00df0134c141b0234c14520327c045f0127c041d0937c241b0091c809f0036b0010000000000000000a043400cc0033400cd26315840d0130400d109374044d01224040c04334100141314000d0000201000000000000000020007400d90037440dd20344001c0835422d100674005d00374001d04774001
901b54019d0034a0010000000000000008) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0920) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (2a571084c005300a0c08df0020c408f00a6c10df1035080300000000000000060017c00ff003fc80ff003fc003f8846c01af207fc09df0837c006f027ec19bf083fc00ff003d8005000000000000000a220b400df0037c40df0034c200704e5c031309e78045708c5d00974044d001f0075c00df
0036a8820000000000000004001f400dd0037400dd0035400d402055385519174001142044809100044005d2054480dd0035200700000000000000040043400cd0033400cd0030400c51005602410012442040001408453620442cd1001400cd00310010000000000000000c6007401dd0077401df107540917120
44021502874431400240401501144005d0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0940) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (200bc00ff003fc00ff4035c09fb0017808fc401cc809f00278009b23178005e0026808ef003da8020000000000000008405bc00cf0032c00c70072d00c31151c08870173905814090c005b0334500cf0063c08cf003210160000000000000008201a401ed007b601e9817a4812102796092103cb
0096188684092003d84694d03e9409ed007a08060000000000000008000f400cd0032400c540324110900154038500074208000504010900000204d0023401cd003220030000000000000002004e4a0dd0037400db0178430d120e5c085124744805106b4500d100244049d0474404cd0034a01300000000000000
04200fc00df0037c00d70034c00d743b7c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0960) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (2c7c001f00058012000000000000000e201fc005f0015c405b2014540511094d065700d6c025b0094c01534094c0253105dc005f0017a8070000000000000004004b400cd0033400c94030400cd0170443d1017641bc0037540ac18030409c90024400cd0031201200000000000000040003401e
d0079601e92178401e10078401e580fa401c98058481f10070401e1006d401ed007900000000000000000004605f400ed003b400e100384002f403c400811020400e1003d420710038500fb0038400ed0039181700000000000000060053c00df0035c40d34234c01130026c80d71024c019b0014c01930004c205
32031c00df003520140000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0980) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (04530907c44150117c041f1104c04134104c001f0006b01e0000000000000000a0534008c00234008d0523494a1252a434a1652b014a1052b414a105285148105304208c00202814000000000000000200734009d1027480918827408b5022c480b1002f480b5022f480bd00684009100344009d
0024a01c000000000000000800074009d00274009f00234109184204029126a740091d0e74209140244809100645128d0026200100000000000000042043c009f0027c00930026c01970024e05930027c00970067c02990024c02930164c029f002508100000000000000006004bc001f0007c00170007cc037228
5c061f0085d001f0807c441f1407c100f0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (09a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00630009d00274009d0026401d10024410c80225420910025400950937400d100274409d002520180000000000000004004b4008d00234008d00224038180224088901214088104204208000234048101234408c30200012000000000000000c60734001d00074001f2004400144544c15014a44
4001401454051421444055101c74001d0007181c000000000000000e0063c009f0027c009f4028c21b3056cc05b300ecc21930c6dc99b3166cc13a304efc00bf0027a0180000000000000006a067c009f0027c009f0022c008f0535c149f05274009f0527c149b0537c14bf052fc008f2027a81900000000000000
08c07bc001f0007c00134106c84350104d) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (09c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (02b400ad003a080100000000000000080053400cd0033400c18072401cd00f04510530f2400c12010480912130040950063421cd1032201400000000000000020051c005d00174005f005840277015c71071001c4405182dc42575111c080710c5f4197d2014a01400000000000000042043c001
f0007c00130004c041f0101c02134181c02038884c12138085c08170007c001f00050810000000000000000200cfc009f0027c009f0025c809f00a5c00970066c019f0027c089f1060c009f4263c009f00258013000000000000000e2017c009f0027c009f0026d018320a6d099a0465d189344a1c049300a7d029
30027c009f0027a8050000000000000004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (09e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (880d242a480e54201700a10338604ad0039400ad0039000000000000000000046057400ed003b400eb1a60401a100c8c15e1226b421c30068401a1017ec81a10660400ad0039189500000000000000040003c01ff007fc01f30068c0193007dc0d5a0266c09fb127c809b7207e809b7007dc013f
007d200000000000000000062041c00df0037c00df0025c20df1037c005b1825000df1817c00df0807800da0007880df0835a81000000000000000084047c01ef007bc01e3007ad01ef007840127006ac01c1004890181006cd01e7206fc01ef007a101100000000000000082005400ed003b400ed80aa002c5002
8400e50432440e10430400e5001c480b50) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0a00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0217400dd0037400db08c4403c1c0144099100c7400d10115447c100074435500434419d0836208500000000000000042213c00ff003fc00f14248c00d92018000b3003fc90f3120e8409324adc10f30027c00ff003d088400000000000000060007c00df0037c00df0087c019f20a4c009728a7
800d30836e00de0293c02170037c009f00358001000000000000000e2057c00df0037c20d32004f00d10025e0a9f2076c83d72465c04d320b4c82df1075c00df0037a81500000000000000040013440cd0033400c90020410810103440190467489cd0cc54278108324008800004008d0031200400000000000000
040403400ed003b400e1102a400a185214) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0a20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (044d011108570801000000000000000e000fc01ff007fc01fb0037c04ff0136c012b084ec014f0105c01db0075c011d0044c0033000da003000000000000000e2017c20ff003fc00fb0207c083b0306c003f0d2bc14df28074001b00074000f0307800af003da005000000000000000ac003c00d
f0037c00d70204d00972305d041301b7c06d10107c04174105c449303b7c009f003630000000000000000000a043400cd0033400cd000044085010151041e423010c1c4214100504034100500234008d0030281000000000000000020007400dd0037400d50404401d51225400510477480d18025401550005401d
100774039d0034a0010000000000000008) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0a40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (001f0294c00510037c00df0635e001b0007c0a97022108030000000000000004021fca0ff003fc00ff1047400ff203dc00bf601fc007f0893c20ff003fc403f024dc03ff00558007000000000000000c2003800df0037c00db0057cc0df0036d011f00d6c455b0004c20db0035c05070104c0093
c1c788000000000000000002200f400dd0037400ddb207400dd2034601150044401510027400d10034401190006400500135a803000000000000000e8043400cd0033400c18023422c520b06000d8800400490002400c900315001500004001100232010000000000000000c2007401dd0077481dd1047002dd00f
4401150004480511247401d110744001d0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0a60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (600bc00ff003fc08f70027c08ff203fc8033012fc205f003fc48ff003f80c3f8307c207b003d30020000000000000000404bc00cf0033c20c32363e45cf1333805070364c05474752c01cf11714011f064340003002010120000000000000002011b401ed007b401e1036b465ed207800935027a
40d31027b401ed837a4012d904b4496188580006000000000000000a001f400cd0033400c080334c0cd14b2509040030480150042400cd00b14000d0443400014032a0070000000000000000004f400dd0037400d00007400fd083cc6b802292c20510037400dd00f2d001d00c740bc102b4a01300000000000000
04200fc00df0037c00d3c007c40df1037c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0a80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (307c101f440300120000000000000006205fc005f0017c0053409cc005f0013c417300584017b001dc00570015c407f50d8c077301dda817000000000000000c204b400cd0033400c10071400dd003148ac104305019903f2400c10032612cd00b0401c1003328120000000000000004000f401e
d007b401e10070401ec027a40131045c51129007b401e510795912d906c40101007908030000000000000006204f400ed003b400e12039404ed0039c40a14038400312033400e1003ac003100285006100398013000000000000000e0057c00df0037c00d30074c28ff203fc01130034d001b0065c00d700758001
38024c00130033a0150000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0aa0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00132015c001f0107c001f0804c00130016c04530106201c000000000000000420434008d00234008d05204148105234008120254208d85234208d00214009100264148005200010000000000000000000634009d00274009d00345209100a64209162350009d85374009d0024408914126408d1
0024a018000000000000000800074009d00274009d00244009102a74539100644009d00a74009d01a54008110645039142262001000000000000000c2043c009f0027c209e0024c09930067c059308244009c0867c009f0026c21930024c008300270810000000000000000c004bc001f0007c001f0307c001f108
5c041f0087d101700874401f0087c00111) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ac0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (20634009d0027400910024400950024400d100274888d00a74809100345088d0064440910835a818000000000000000e80434008d00234008180a24008110204008181264908d0023400811824400851021480c100230010000000000000000c00734001d000740011008441f158004420114004
4844d20074001140044005d1004422114097081c000000000000000e0063c009f0027c00930064c05b39d6cc00a308acc009e002fc0093002cc22bc002dc14b3052ba018000000000000000e2067c009f0027c009f002fc148f0827c20af053ad54bd002fc009f002bc14bf0029c40ff002fa81900000000000000
084073c001f0007c001f0104c04134107c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ae0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (8484006104088004000000000000000a0053400cd0033400cd00334054586b2400cd4802520cda0f1600cd0190407c08030480c118b2a014000000000000000200134005d0017400570017486710098c907300585005d801f4005d00dc40271039c40071289c201400000000000000042153c001
f0007c001f0807c80170004c04174284c421f1087c001f0204c00134004d22130085081400000000000000040157c009f0027c009f00a38008f0027c099f11248809f04e7c009f0027c019f0027c008f0461001500000000000000042117c009f0027c00934064d00902024d00832826d029f0067c00920020c039
70025c0893026528050000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0b00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (003d4199080f10003400ed801b400ad800b400ad0409000000000000000000062057400ed003b400e1017ad0087014bc080301534c5e1060b400ec0018000ad204b420210a098815000000000000000e000bc01ff027fe09f3013cc01b30840c41a30855c09eb004fc21ff2a5f801bf214fc41b3
004fa00200000000000000062043c00df0037c00df2037c005b0007d601f4026d72df8807c00df0017d008f0003c008f4005b81000000000000000006053c01ef007bc01ef007be4167404ac012f404cc05ed004bc01ef0058401a10048c01e30068101400000000000000022013400ed003b400e5003b40065001
0400b10008488ed00ab400ed0018410f12) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0b20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (020f400dd0037000d10037407d30142c02050886c60d10847480d90096c32dd10464009100c20081000000000000000c2203c00ff003fc40f71036001d3000ec0033100cd00f1000fc00ff025cc22ff000fc00fb000708a0000000000000000c0007c00df0036c00d70230c00df0087c281f0087
c00d70927c00df0014c08df0007c11530087000100000000000000062053c00df0037c00db0035c20d900044015b0015c02e340e3c00df0017c41df2107c03df4005a834000000000000000c201b400cd0033400c901b3420851003493010035484c100c3600cd00104078d00034008d01c3280600000000000000
040003400ed0039480e90139408a901084) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0b40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (075c01dd00770001000000000000000e000fc01ff007fc01f30078c0193104bc411b1061c41330059c403f000cc003f007fc01f7007f9083000000000000000e4017c00ff003fc00f72737c00f5020fc043f011ac0cdb010fc00fb011fc047f1506c20b4400db00500000000000000084003c00d
f0037c00df01b6c02d74286c00130294c2ef74007c08dd00244084f01874009b0006100000000000000000000043480cd0033420c98133448892802028156412404d50203480c902107004d0403480090000201000000000000000000007400dd0037000dd0037408950847460110454680d50045400dd00044004
d2447420998046a0010000000000000008) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0b60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00970805c08130116d02430044c001f0037c00df0035000700000000000000062017c00ff003fc00f4002fc10bf000fc20f7080ec493f083fc001f0107c03af003dc00ff003d0185000000000000000a0011e00df0037c00d20034c009b0247c219b20450029304f0d091f0844c009f0037c00d7
10372080000000000000000aa00f400dd0037400dd00254a895a404401990465442150854400914834500dd0037400dd0035200700000000000000068041400cd0033400c101204008800014800920214801120144024514a04080d0033400cd00310050000000000000000c0007401dd0077401d50525021d4203
44009100444011500550021401844501d0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0b80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (400bc00ff003fc00fb012fc08a30005c28af02364042f000ec00fb803f808fe003f800f7003d0802000000000000000060dbc00cf0033c40cf0260475870040d01072161c01030052c05c341f0c110f0073c00cd003000120000000000000000001b601ed007b401e5802c44db1014c409b1895d
40d39005d4156502486854d017b401e5007800020000000000000000008f400cd0033400cd00744208508044001504114004100d30078120144014d0033400cd003020030000000000000002004f400dd0037400d10ea47038100044459109604080b0495c00910014401dd0037400d70034281300000000000000
04200fc00df0037c00df0024c009f1805c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ba0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (007c001f000500120000000000000004005fc005f1017c40530016c217b015ac057b005ec4b73231dc007f189cc8a7f0017c005780152003000000000000000c204b400cd0033400c9002040089814040281023242901a052400c501b0402dd0033400cd0031281200000000000000040013401e
d007b401e1006a403b9004c401b9007a481310058481ed20785812d007b401ed007900000000000000000006004f400ed003b400eb002c400a10008440a1001ac0021001ac00630020400ed003b400ed00390013000000000000000e0043c00df0037c00d31036c009b0006e418b0050400130015c41910834c00d
f0037c00d7003500140000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0bc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (005f1004400134007c24110104c040f0005c001f0007181b000000000000000080434008d00214208948304009100234008d00214009100270948105205148d00234008500200810000000000000000200634009d002740099002148291c0274009d0024688912227484d100a04149d00254009d
00242018000000000000000000074009d00258009100244028300274019d04254078100634019100244419d0027420970026200100000000000000042043c009f0027c00931025c08970027c049e0624c40930027c80930264c009e0025c009f002500100000000000000004204bc001f0007c001f2007c8217000
7d061f0087d021f6007c001b4087c021f0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0be0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (20634009d00274009d02270009104275809110274009d0034422910424426dd00274009d0025281c0000000000000004004b4008d00236008d0123400812120600dd00214208d10604808141a044c8d10234008500210016000000000000000c00634001d00074001d0043400110547c01110017
4001d000451f1100445131d00074001d00070818000000000000000e0073c009f0027c009f022fc40a90028c88bf102bc00bf0028c01b3036ec01bf0027c009f0027a019000000000000000e6077c009f0027c0097052fc00a7052bc34bf002fc00af002bc14af5d2fc14bf0027c009f0027a81900000000000000
0ae073c001f0007c001b0005c00170007c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0c00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (03b400ed20380000000000000000000a0043400cd0033400c10071401c51026480010163401c101d14299d00b0510cd0033400cd80322010000000000000000200434005d0015c0051a01c4057b00144007524df4257b005c4007d201cc057d20174005d0014210000000000000000042053c001
f0007c00130004c00171084c21131007c04130005c001f8104c001f0007c001f080500100000000000000004205fc809f0027c009f0027c019f2a67c009f2127c209f0067c039f0063c008f0027c009f00250013000000000000000e8017c009f0027c009f00278089340e4c898f0021c1b9f02e4c019302a4c039
f0027c0097002500050000000000000004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0c20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0031022d4102d203b600a100120106d003b400ed0039000c00000000000000040047408ed003b400eb0761420e50063c04ab2d6a401cd03134848b0a228048d0173400ed003910550000000000000004001bc00ff007dc01fb0064c01fb0369501b3026bc41cf227fc41bb207cc01ff0277c01ff
087da00200000000000000066043c00df0036c00df001ec20df002dd003f1827c005d0817c40df1825c009f1037c00df0035b85400000000000000006053c01ef007bc01e14079d01e701eac0133006b401630049c01bd0878c018f007bc01ed0078101000000000000000020013400ed0039400e120f9401f9012
e40025000b400e908dc400ed0028400ed0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0c40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0a07400dd0037400d10047411df0025480050462c470300505935d0cc54009d0037400dd003421a3000000000000000c2203c00ff003ec00f1081fc80f7002ec1033002dc1033025cc00bf80ccc50bf003fc00ff803d0081000000000000000c2017c00df0037c00df002fc00572027c011f2027
c029f1097c12472097c005f0037c00df0035000100000000000000060053c00df0035c00d11054c01db1a69c03130027c009f0117820d1d156c025f0037c00df003520180000000000000004200b400cd0033400c90005400cd10a34020904a04004d00534088900024001d0033400cd0033200200000000000000
040003400ed003b400e1012c410f9072d4) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0c60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (8144001140270001000000000000000e000fc04ff007fc01f34436c00272a3cc013b004fc14cf207cca1f7004ec01730004c0137001f8803000000000000000ec017c80ff003fc00fb050bc00ef01a7c042d1427c28bf001fc003f000dc003f00bfc00ff003fb801000000000000000a6003c00d
f0036c00d70497c02951224c08534034c081b4214c089d0206c084f0237400dd0036380100000000000000008043400cd0033400c581234024541254000504224808100144000d08334a00d0133400cd00300010000000000000000a0007400dd0037400d50e17401d50024483112064481190014401dd00364005
d0037400dd0834a0010000000000000008) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0c80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (829f02b4c10f30134c08d302a6c01d34004d10178095000300000000000000060017c20ff003fc00fb203ec003f003f440bb202fc00ff003fc00fb000ecc0ff2053d813f10258005000000000000000e2003c00df0037c00d70036c2107a034c010f0885c00df0235c80c71047c868340d4c8907
4097a0000000000000000006200f400dd0037400d540354115d00354011512170c0dd0035420d58465000d102144001112218003000000000000000e804f400cd0033420c505304020d90b04001d8001400c90031620c50023400110800600150013a010000000000000000c200f40add0077401d100bd4031d00b
5441130047443fd0075400d10044401d10) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ca0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (600bc00ff003fc00ff003dc0857803fc20dd9036c04ff023bc80ff002bc88fe001dc007f402d38020000000000000000404bc00cf0033c00cf1170c48072376c9acf2361d01ca2033404d30023c088305e2c0815041000120000000000000002007f401ed007b441ec117a40961017b401ad10f9
42de9007a401e9004b401e1025b6016102680006000000000000000a001f400cd0033400cd083052a0110324010c0841402c900b3001c10083404c100e240305003028030000000000000002006f400fd0037400dd003cc0851003f40a9d00b0486fb01a6c00da02e3441d10a55453510064a01300000000000000
04200fc00df0037c00df0038c025f4036c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0cc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (303c101700010012000000000000000e205fc005f0017c20579014c826f0017e037b011fc005f5116c0057015f4016380dfc527700dfa817000000000000000c204b400c90033400c5403148acd0033411cd04f2400c90071480c50073403c12073403c143b3201600000000000000040007401e
d007b401e500704017d007b401ad007b601ed107a001e5206b401e1007b40124207908040000000000000006204f400e9003b400e105b94006d01bb400ad203840ec10039000e1402b400e1003f4006100319013000000000000000e0057c00de0037c80d301bcc004f0037c001b0815c20f30030c01d21027c809
34037c801f0037a8100000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ce0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00530005c44534007c201b0007ca0110107c00134106a01c000000000000000080434148d0023400810521414954d23400891024454810023400812021400c50523440c105202210000000000000000200634009d00274009540244009500234849020350009100a76089900254009101a7400d1
5034a018000000000000000880074009d00270009100244009100274839a0a204029100e34019100204009500e74009101a62001000000000000000c2043c009f0027c00938020c00920027c00970025c008b0166c019b0167440934027c0493002708100000000000000004004b4001b0007c001b0007c041e880
7c0a1f2005c02150085c00192407c181fc) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0d00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (20634009d00274009d00254049020204019d10254209100276009d8027004959027404994425a818000000000000000e804b4048d00236008d21a14008104204008d80216028508274008500254008101a34c485c4332012000000000000000c207340b1d00074001d00c04201308445001f0015
4201120074001b00174001100870001b11870018000000000000000e0063c039f0027c009f00e4c40b32464c20bf002cc21b7002bc02b7002b880a300afc02b7042f201c000000000000000e6067ca09f0027c009f0526800bb0527c00ff082fc009f002fc148f202ac00be052fc14bf052fa81d00000000000000
0ac073c0e1f0007c00110104d04172107c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0d20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (42a401e900288004000000000000000a0051400cd0833480c1003042acdc032608cd0131489c50033401cc00f12034900720110901b2a010000000000000000000504005d00174005100168207100174027d20dc40165009c48471101c48270285c40571009c201000000000000000042051c001
f0007c00134804c00130806c001f0006c011f0405c00170305c901b0106c021b088508140000000000000004005fc009f0027c009f0026c11974027c10971167c009e10a7c00938127c009b0263c019f4025081700000000000000042017c009f0027c009f9025d11831824c018f10e4840978063820970021c019
34027c849700a120050000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0d40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (8cad808b4802d0308460a5340a418e10538400751189000000000000000000062054400ed003b480e5007ec0521207340bad054340f2d1149405ad0148405214068410eb02090015000000000000000e0008c01ff007fc41f20274c012a0677c49ff025fc011f0046c09970246c09d34276c0167
034d200600000000000000066043c00df0037c00df0037c001308bfc001f0804c001b1004c00970806c00970025c00d70585b01000000000000000004051c03ff007bc01e304f8c01ef047ec81ae806bc016f004b401bf0069c01eb207ec417b105c181400000000000000020010405ed003b400e1417a4a00d103
b6a0ed809b50005240f601a9800d603292) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0d60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0004400dd0035c00d100344031a0037401170046c011d14444009b0000503858025413d140562081000000000000000c2200d00df003fc20f3003cd80270033c85bf000cc203b100cc08f3214c410f3807cc00f300170880000000000000000c0007c00df0037c40dd0037c8217003fc829f0887
c820d0285c009f0087c401f0081c10df40d7080500000000000000062050d00ff0037c20d7083c4061b483fc009d0047c001f2044d20d70006ca05340f49025700d1a014000000000000000c2018400dd0033400c500364010910336190d10434400d00014009d00404438104e0403d90001280200000000000000
040000400ed003b400e5013840629213b6) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0d80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000800020000000000000000000000000000850021400850021400850021400850021400850021400850021400850021400850021400000000000000000000e6017c00ff003dc00ff01bfc021f153f800170007c143f000fc08af020ec02ae090fc00ff001fb00500000000000000084000c00d
f0037c00d3023cc041701bfc141f17045121b0104c04911105c2091050040053001e180000000000000000000040400cd0031400c101304040905334040581004040c2400524810105404850301600c110100010000000000000000a0004400dd00374a0d140340031500374001d00c44081d01064009148854319
161944015100d680010000000000000008) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0da0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0400010000400010000400010000400010000400010000000000000000000000000000100004000100004000100004000100004000100004000100004000100004000100004000000000000000000000000000400010000400010000400010000400010000400010000400010000400010000400
010000000000000000000000000008000200008000200008000200008000200008000200008000200008000200008000200000000000000000000000000008400210008400210008400210008400210008400210008400210008400210008400210000000000000000000000000008000200008000200008000200
0080002000080002000080002000080002) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0dc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (20033800ce0033800ce0033800ce0033800ce0033800ce0033800ce0033800ce0033800ce000080000000000000000000000084002100084002100084002100084002100084002100084002100084002100084002100000000000000000000000000080002000080002000080002000080002000
080002000080002000080002000080002000000000000000000000000000085002140085002140085002140085002140085002140085002140085002140085002140000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000040001000040001000040001000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0de0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000003c3c000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000420800000000000000000000000000000000000000000000000000000000000000000000000010820000000000000000000000040
001000040001000040001000040001000040001000040001000040001000040001000000000000000000000000000010000400010000400010000400010000400010000400010000400010000400010000400000000000000000000000000840021000840021000840021000840021000840021000840021000840
0210008400210000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0e00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (fffffffc0000000003fffffffc0000000003fffffffc0000000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000f0f000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0e20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00000850021400850021400850021400850021400850021400850021400850021400850021400000000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000000000000000000000000000003fffffffc0000000003fffffffc
0000000003fffffffc0000000003fffffffc0000000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc000000000000000000
0000000000000003fffffffc0000000003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0e40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1000040001000000000000000000000000000010000400010000400010000400010000400010000400010000400010000400010000400000000000000000000000000040001000040001000040001000040001000040001000040001000040001000040001000000000000000000000000000800
020000800020000800020000800020000800020000800020000800020000800020000000000000000000000000000840021000840021000840021000840021000840021000840021000840021000840021000000000000000000000000000800020000800020000800020000800020000800020000800020000800
0200008000200000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0e60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (800ce0033800ce0033800ce0033800ce0033800ce00008000000000000000000000008400210008400210008400210008400210008400210008400210008400210008400210000000000000000000000000008000200008000200008000200008000200008000200008000200008000200008000
200000000000000000000000000008500214008500214008500214008500214008500214008500214008500214008500214000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000400010000400010000400010
0004000100004000100004000100004000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0e80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000042080000000000000000000000000000000000000000000000000000000000000000000000001082000000000000000000000004000100004000100004000100004000100
004000100004000100004000100004000100000000000000000000000000001000040001000040001000040001000040001000040001000040001000040001000040000000000000000000000000084002100084002100084002100084002100084002100084002100084002100084002100000000000000000000
0020033800ce0033800ce0033800ce0033) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ea0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0003fffffffc0000000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000f0f00000000000000000000000000000000000000000000000000000000000
000000000000003c3c0000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ec0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00bf086dc091f226ec032300efc09be0077c01fb087da043000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003ffff
fffc0000000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000000000000000000000000000003fffffffc00000000
03fffffffc0000000003fffffffc000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ee0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0617c80ff002fc01bf0826c08ba003ec209f200fc053f000e8003b000fc00bf003fc00ff203d800500000000000000040003c40d34086c00834003c028a08f5c01d700c5c021f0047c001700478039f0035c00db0037a8800000000000000006000f400d104140049101154109501116419d0064
4221d00c54000520c70811d0037400dd00350007000000000000000e8053400c10082404c180334849d01314009508214041d01034048541034040da031400cd00312010000000000000000c0007401d101944089100c4400d100344149d05004041d01044005101074001d0077401dd0077180100000000000000
0e200fc01f1018ec0ca30506c03bb20f8c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0f00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (03fc00ff003db800000000000000000008cbc80cf0021d00cb0160c288f1372c128b00d34810300054008d0413c02470071c00cf003210120000000000000000001b401ed0059411e9414a489b9937e40921044b40121067850175007b4816d017b401ed007a00060000000000000000018f400c
d00a540089000021a8d20324000900534010100300100c8137400450031400cd003220030000000000000000204f400dd00b4c00912036c839e003440a81002740e0142840051f00474009d0037400dd0034a0130000000000000004000fc00df019cc30d30034d001d24a4c02da00a7c22130085c001f1007c029
70037c00df003508030000000000000004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0f20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0073001cc4073201fc0063001c4057f0017c005f0017a806000000000000000c204b400cd0070400cd30705038981b16119902f5483490033409091071405cd0033400cd0031201600000000000000040003401ed007a401ed0078601b8107d401b1007c40331147f44121007c401fd207b081ed
007900000000000000000006205f400ed0028400ed0038400af0038600ab0019c006b003b4002b0039440ed003b400ed00391011000000000000000e0043c00df002ec009f0815080831035c00a30010c00130037400190020c000f0037c00df003520140000000000000004600bc00ff021cd08f7000dc488f003
dcc09f0037c00bf003fc003f003fc007f0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0f40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (a0434008545214148105215409948244148100206008100204209580245008d00234008d00202014000000000000000000634009502245029500250009500345829100a46028104204029120244008d00254009d0024a01c000000000000000000074009100a440081202500d9f00644039100e4
5009140a44039486e04529d00274809d0026200000000000000000042043c009100278009300244009300a4d03930565c009300a4c08938424c009f0025c009f002508100000000000000004204bc001f0483d021f0043c041f12065881b1007c061f0107c041f0207c001f0007c001f0005801200000000000000
04005fc005f01dec005f015cd07632099c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0f60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0274009d002500180000000000000004004b4008101a04048d9020534b1042d410a10468150a15428400a1a0285008d00234008d00210012000000000000000c00634001100c450b1d128440135014450f1141458211101445051009444051d0005c001d0007181c000000000000000e0077c009
3026c803bf0064c00910025c018b0024c00931026c029b00a4c028f0027c009f0027a01900000000000000062077c009b052cc54af102fc14b7152bc14bf052ec54ef153bc14bf052fc14bf0027c009e0027b81800000000000000084077c00170114d04174105c20172004c44134005c00130004d00110804c001
f2005c001f0006b81f0000000000000004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0f80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (20c10070603d50873400c10030412cd0032600cd10322014000000000000000200034005d005c4027d001c4804700d2c90510c9440a5130574835b0016c025d00174005d0014a01400000000000000042053c001f0004c041f0004c083f0104c00131405c42171087c001b0084e021f0007c001f
000508100000000000000004205fc009f4026c099f00678409f0027c609f02654009f0067c309f0067c049f0025c009f0025801300000000000000040417c00930024c018f1b24d129124a5c069b0864c42931226c209b4324c039f0027c009f00278805000000000000000420634009101205009c8024408b5122
c400a100384a0b1002840aa120284228d0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0fa0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (2057020ed0038404ad0159409e11871445ab2c606412929486097101cb4a5ed017b400ed003918950000000000000004001bc01ff007ed81bf2254e05e70854c09f2027cc21950074009d32277c0ddf1077c01ff007d200200000000000000062043c00df001fc00ff0017c80559037c201f8006
000df8017c00198037c80df2037c00df0035a81000000000000000006053c01ef0078d01ef0058d017f0078d0123904dd01f7006fc4161007c481ef007bc01ef007a101100000000000000022013400ed00b8402cd0018420ed043a420f1003860261009b410ad040a440fd003b440ed203a080100000000000000
0a0043400cd0030401cd0010401cd00704) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0fc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (836400dd00360085000000000000000c2207c40f304d8800ff0c1cc0873062ec20bb282fc11f3000cd007b041fc00ff003fc00ff003d0805000000000000000c2037c00df802fc039e8015c009f0005400592437c001b00b60849b1007c065f0037c00df0035800100000000000000060053c00d
f0086c01df0016c099300a7400d700f4c83d71831d05db6477c065e0037c00df0037a8040000000000000004204b400cd00804009d00134021160e74010d20044430901814011180e34034d0033400cd0033200600000000000000040123400ed0628400ad201a41131840b65475001c4b4250d2948ca8002b4806
d013b400ed003900180000000000000004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0fe0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (09130073c013b084fc0137084dc8033010fc21ff007fa003000000000000000e6017c40ff000fd00a70f1fc021f000dc28080103c263e008fc423f880f8007f013ec00ff083fa8050000000000000008400fc80d32005c00df1914c00130100e00db0597c04410104c009f04034005f05b6c00df
0036b00100000000000000000043400c100204008501105008146105241102074060508244444d10014144d0232400cd0030281000000000000000000007400d10405401dd8014400910414400d90017008d10834400dd20374105d1836400dd0034a0010000000000000008020f400d1005448717001440050408
4c060020a74009509944001c0017c42dd0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1000) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0013c80ff003fc00f70017c003f610e82136303fc01bc040fc003f000ec81f3003fc00ff103d8005000000000000000e2003c00df0035c00d30907c41170000c0c120033c089a0046c03170241c43120847800df0036a800000000000000000620074a0d50034400d10047601912434200590836
420dd0047023912085414116617400dd00348003000000000000000e804f400cd0031404c105834000510104040100336808d0002400050005488010303400cd00332010000000000000000c200f400d70534402e108974011100644841100774811d0047440140044430032d03081dd0075180100000000000000
0e000fc01ff007cc1cfb000fc011b000dc) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1020) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (13f880ff003da8020000000000000000404bc00cf0030c00c70053c01030253c0d078271c198f0163c2d0c0150c1dcf0171c00cf003210120000000000000002007f401ed0078403e1017b01129016340565027b4016d096b445a1c94840ded406b601ed007a0806000000000000000a001f400c
d0030020d108234030184834001500b04010d00834420d01004330c0a41400cd003220030000000000000002004b400dd0134400f120274239f34874915102b7400dd00874139b0154400d10237400dd0034a0130000000000000004202fc00df0034c01d71023c04172087cc25f0075c00df0207c04932884c02c
30021c00df003508030000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1040) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (a77e0013c037f005bc037700ddd277b01dfc005f0017a817000000000000000c2048500c50031400c50033400c90233404dd1033412cd0033403d183b1402dd4473400cd0033201600000000000000040004401ed0079405c100794812d206b4016d007b401ed0c6b611a52859401e9207b401ed
007900840000000000000006204c400f70038402e5003f40029081b40065903b400ed003b420a18008440c10033420ed00399813000000000000000e0054c01df0034c32d31027e801f0007c00538033c00df0007c60970044c00130017c00df0037a0100000000000000006600bc00ff023fc08ff801fcc0b5403
7c08739037c20ff003fc88be001bc24f30) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1060) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (80434008d00205158905234008c0d20500c100334808100214408d1060414c125234008d00202a14000000000000000200734009d00244009110234909d00244009d80264009502354009d00244009181a74009d1024a01c000000000000000800174009d00244809b20274229d08e44829580e7
4019101a45069d00644809100a74009d00262001000000000000000c2043c009f0024c00932027c809f0224c42972267c049780268229f0964c02930863c009f00250810000000000000000c0043c001700064000f0047c001e0487c021700878281f0007c921910064041300874001f0005801200000000000000
062054c005f0015d4053001fc057f08dfc) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1080) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0274009d00252018000000000000000e804b4048d0020406810320480c100a04008530234008d10204049d00204a08d00234008d00210012000000000000000c20734011d00444251100c44001120044005100074a01d00044041d00045205d00034001d1007181c000000000000000e0063c029
f00acc03b301e4d20a3486cc00ab002bc20bb2029c02bf002cc20bf002fc009f00278019000000000000000e6067c009f0527c949f052fc00ff002f814bf0027400bf282e414bf083bd34bf053fc009f0025a819000000000000000ac073c0a1f0004c04130107c001f0114c00170806cc0150005c001f2004c041
34107c001f0006301d0000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (10a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01c42032488c500f3400cd20714a0cd0073400cd0032a01400000000000000000053400510014402710016d086138dc40271001c4015100dfc817d201cc027108df4005d0014a00400000000000000042053c00130204c2c030004c02130085c12134206c00170187e001f0007c0c134007c001f
000508500000000000000004004fc009f0027d009f0067e049f1023c059b24270039e0027d809f0667c018f0467c009f0025801300000000000000042017c009f0024c00934664c039303248c08f4023c039908a5c028f00244229f0a27c809f00278845000000000000000620634009d002440091002040091002
41009100274829d02b46069d10244049d8) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (10c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (2057400ed003b4086d06734842103404002f016a4058d00234600d8020480812167480ed00390815000000000000000e200bc01ff006fc41bf0677e01330048c016f026cc0d9f014fc01bf007cc01f30277c01ff087d280300000000000000064043c00df0037c00df01bdc001f0004c005b0007
c008f0007c801f0015c00d38037c00df0035a01000000000000000004053c01e3007cc01630a7dc01634043c2167006ac01a7004b4016f0079c01ef087bc01ef007910110000000000000002001340ce10078480c1013a00031000b410f52028401a104794106d043a400cd947b400ed8038880100000000000000
0a0053400c14070501c14031400c186b34) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (10e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (007400dd003620a5000000000000000c0203c40ff027fc007f003fc1033124bc1933000cd05b3200ec107b002cc08b7012bc00ff003f0807000000000000000c0007c00dd0026c009f003f00a1b30868005f0085c009f0907c081f0037c305f4197c00df0037000900000000000000060053c00f
f0037c00df007f602171285c065d00045008f0457cc25f0270c13d354f7c80df2035a816000000000000000c001b400cd00334204d08734800502415020500026808d00034221d00405201000c3600cd0031280600000000000000040003400ed002b4002d113b4c02541094087d100a0d8bd310b4082d04384006
1031b400ed003900880000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1100) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0033010fc14130204c001f0117c01df0077c01ff087fa003000000000000000e6017c00ff002fc003f033fe043c0307c803f1a07c6caf010fc303f000fc243f120fc00ff003fa80500000000000000084003c00df0027c0017033fc08130007c08130304e04934206c80130284c88071207c00df
0036b00100000000000000000043600cd00234000d013340001420342001590044c911004420010004580010003400cd00302810000000000000000a2007400dd0026408950837481150087402518044680910046403110414400d50437400dd0034a00100000000000000080007400dd00674019d003740511000
7401110140400912040401114244410150) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1120) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0207c00ff003fc00ff0047c00170225c01ff007fc29ff408bc82df000fc00ff003fc00ff003d088500000000000000040203c00df1037c80d32286c03130066d03c32011c01030004d001f1817c00df0037c00df003720040000000000000004000f480dd0037400d5801441819040748a112e24
4001110244801d0097400dd0037400dd0035a8030000000000000004804f480cd2433400c114124408100024680100014000100004020d2e13400cd0033400cd0033a0140000000000000004600f401dd0137401d5138444e130245403110264403d103a44039d0187441dd0077401dd0077080100000000000000
0e040f441ff007fc01f30006c083b5106c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1140) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (237c00ff003d28020000000000000000404bc00cf0033c00cb0270d0d8f4562c15430170c05430151c05410177c05cf0173400cf003010160000000000000000016f401ed007b401e9806840de5225840981024a405e10170405e1216b405ed017b401ed007808460000000000000000010f400c
d00b3400c941a44004d0052400014000403010211400410033400cd0033400cd003020030000000000000000005f420dd0237440d10004400530a94401d10026c019102b4445d10027400dd0037600dd003420130000000000000004003fc00df0037c00d30084c02c71013c02d30004c58974035c108300b6c00d
f0037c00df003508030000000000000004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1160) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (045b0414d024b06d4c125101d7c005f0017c005f001520170000000000000004004b400cd0033420cd0034409c106f0403c10030400c100f0401c10067400cd0033400cd0033283200000000000000040003401ed08794a1e500784a1e90078400690078401c9007040181407b401ed007b401ed
007900000000000000000004404f400ed003b400ed0038480c3a030400810010400e10008400e11003420ed003b400ed0839883300000000000000060043c00df0035c00d400344015b2834d011b0054c001b0004d00130017c00df0037c00df0037a0100000000000000006600bc00ff003fc00f70077c80bb002
fc00ff003bc0849033fc087f423fc00ff0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1180) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (20434008d006340081052f414a1052a414ad0528414a50528514a105234008d00234008d00200010000000000000000000636009d022740099023f420b9002c530bd012e414b10028008b020274009d00274009d00242018000000000000000000074009d00274009100274009101204629d04e4
0009500640009100274009d00274009d0026200100000000000000040043c009f0067c009b0067c009b0164c158f0026c10930224c00930427c009f0027c009f002508100000000000000004004bc001f0007c001f000fc80170087c001f1007c021f0087c900f0007c201f0007c001f0005081200000000000000
04000fc005f0015e00570154d005b0014c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (11a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0274009d082528180000000000000004005b4008d05234008101224848040204008d00224208141214008d01234008d00234008d00210012000000000000000c20634201d00474001501c44071b00954221d0084402111dc44021d02c70001d00074001d00070018000000000000000e2067c009
f002fc009204eec1393046cc11af146ec31b3046dc51bf01e7c009f0027c009f0027a01c000000000000000e2067c009f0527c009f0527c949f0025c009f0027c009f0527c809f2d2fc009f0027c009f0027b81d0000000000000008606fc001f0007c001b010fc041b0904c041f0106c04130114c04134107c001
f0007c001f0006101c0000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (11c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (13c58101402c11036403010033400cd0033400cd1032a0100000000000000000000340051005f4005d009d520750018cc761205c51371001c4056100164005d00174005d0014200000000000000000042143c00130007cc0170404c80102486c80132285c90132086c84130086c001f0007c001f
000508140000000000000004004fc009f0027c009f0023c008f00e7c829f00e54288f3127c009f0867c009f0027c009f0025081700000000000000042117c009f0027c00930226c01911024c009f0126c03931165c009f0367c009f0027c009f00252105000000000000000420734009d002740095003440699603
54809d20244109120244109d00274009d0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (11e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0157400e1802b400ed0378404c5814850cc14143407ed00284002d003b400ed007b400ed003900150000000000000004000bc01f3006fc01ff007cd91f38046c09f30247c01ff007cc012f007fc01ff027fc01ff007d200600000000000000042153c00de001fc00df0017c41df0803800db0017
c00dc0017c004f0276c00df0037c00df0035a81000000000000000044043c01e3405fc81e70078805fb004ac01e74051c01c34072c01634073401ef007bc01ef0078181400000000000000042003400e1047b620ed8099440e51088400e50048400e1002850061217b400ed003b400ed2038880400000000000000
000043400c10073400c500f0400c900424) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1200) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (037400dd0036208300000000000000040207c00ff016ec00f3023fc00f3004dc00b70201c20fb200fc20f3003fc00ff003fc00ff003f088000000000000000040087c00d7009fc80df028fc00df0005c40d71827cc49f01a7c045f0037c00df0037c00df0037080500000000000000040063c00d
b4037c00df0024c00f10802c82db00a7423cf10944058f047f400df0037c00df0035a0140000000000000004200b400c90003400cd01e0446c50000604c90483423cd00145020d2033400cd0033400cd0031280200000000000000040233400e9000b408ed8128460e1010a680e9020b414ed02384082d003b400e
d013b400ed003900000000000000000004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1220) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (013f0847c003f000fc013308cec8073000fc00bf007fa003000000000000000ee207c00ff000fc00ff0087c00ef010bc00ef118de145f010fd407f253fc04ff0237c00ff003fb805000000000000000ae00fc00df0022c20d30087402d18505d02d72104e24db0087d0a5520b7c0adf02b7400df
0036180000000000000000008043420cd0013420c14183402c90300402418183494c100a0400410037420cd0133400cd0030001000000000000000028007400dd80b7400d10003400d10005691510404408d91416001548037400dd0037400dd003420010000000000000000020f400dd0087400d10897400db82f
4483c14005c01d122c4087515033440dd2) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1240) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0017c807f800fc00ff005fc453f101ec09ff010fc803f0007c01bf04eec80fa1053c811f003d8005000000000000000a20078005f0344c259a0497c441f1415c424f0047c05170047812930046c22530257c119f0037a8000000000000000006200f0005d0014501d1c2170c0dd80154001c0417
4019d844740411702540055c8874241d2034a003000000000000000e804f4204d00904001540174000da2034040980134000500024000100064001500034000d0033a010000000000000000c200f4015d004440bd100f74091c20444341d10074011d004744111110440051405f4019d0077180100000000000000
0e000fca17f010cc00bb142fc403f0005c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1260) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (037c00bf003da00200000000000000004049c104f0820ec80f9352c20872062820de13574050508028080f0202c208f0540c088f003210120000000000000002007d4017d007a4093d836f4096d8068041ed105b48d25846b4052d1048409ed0158401ad007a0806000000000000000a001d4004
d0020400090002400c500224094d00934010504830000d00424024d10004058d003220030000000000000002006c40a5d0036c00cb0013420dd0034400d002c740c91000701b1d002040ac500c44261d0034a0130000000000000004200cc005f0034c001f0096c001f9826c62db00d7c001f0086c001f0206c029
30184d021f003508030000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1280) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (827c815dc027f005fc0d7d025cc22730c1fc197f0017a817000000000000000c00484004144b0501450090500c140f1605cd04e0451cd0232600cd10f7526c90033402cd0033201600000000000000040204401610060451710050401810063403fd08596038d806b441bd104840181005b401ad
007900840000000000000006244c400610018400650018400610018400ed00084002d1828400ed002bc80eb041b400ad00399813000000000000000e2054c00430044c20432054c01d31056e014f0814d811f2005c21cf0004c80530093c009f0037a0100000000000000006400ad086f003ff282b0813c40ff003
5e40f3101fc28932026c0c1f2027c00c7e) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (12a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (80404009d05204548d05234148d05234208d00234148d85234008100214148515234148900202814000000000000000220604009d24240009d00274109d0427400dd022740a9d0027420910224400dd00a74009d0024201c000000000000000800045008d00a44009d00274029d00a7c009d00e7
4039d11674009104655059100a34129920262001000000000000000c0040c009f0024c008f2027c009d1026c099e0067c019f0127c00930064f088b0027c009f00240810000000000000000c004bc001f0007c001f0007c001f02068001f0007c021f0045ca01fa287d001f2007c001f0005801200000000000000
06001cd0073009cd0073035cc0073021fc) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (12c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1274019d10252018000000000000000e80cb400ad0268502a108bb403ad906b4018d01314228140a34408100215108500274028d0021a012000000000000000c207b4003d00844401508074021d1285c051700044021128874001100144065102974001d0007181c000000000000000e0067c009
f0164c05930167c019f0167c48a700adc04a3002dc00b7002fc14a3002fc00bf0027a019000000000000000e406fc00bf102fd00bf003fc00bf002d814bf052fc00bf002fc00bf652fc14bb002fc00bb0027a819000000000000000ac074c001f0104c041f0107c041f0106c001f0817c441f0107c001310045041
f0107c041f0006901d0000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (12e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (09418131448cd00f3600c110f05c0cd407340acd0832a01400000000000000020013404510016c0051001446051001442050601c52279001c46071461c44077005b4027d0814800400000000000000042153c00330004d03132084c00130004c00130004c001f2186880130004c021f6187c241f
080508100000000000000006015fc109f1127c409f0023c029f0067c009f8227c508f0023c049f4965c199f0827c009f00248013000000000000000e2017c009f00a4c02830027c039f00a7c00979065c139300e5804970025d0293c0e7c119f0027a90500000000000000062063400bd002c402b5122f420bd022
d4209504240219000e7420910030400810) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1300) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (20474006d0018400a1045340569005940371005b4010d0349c05eb0358005e127404002d00391815000000000000000e010fc817f205cc01a3025fc495f225cc01530277809fd007ec01f3007cc01fb007cd09bf007d200300000000000000066143c009f0027c000f4001c009300274005f0006
c009f0026c00cf0027c409f0017c001f0035a81000000000000000004057c01a3406090123404ad018f406090163207d401af006bc01e2007cd01af2053c01ef0078101100000000000000020017400a100ca40031400e4032d80c8401710059400a90439641e1003840065441b400ad0038880100000000000000
0a045340281104848021000a4012d00484) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1320) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1844071d003621a5000000000000000c200cc00bf082cca072002fc00bf082fc18bf040fc013f000fc01f3101cc00bb0618c001f003f0807000000000000000c0027c009f0047c185904278011b1047002df9087c489f04a7c011f0cb7c02974007c441f003700010000000000000006215bc009
f0044c00471063c031f0844c22d38087c02dd0064c01d30874c00831054c400f0035a81e000000000000000c211b4004d0030403851093406cd08314024100034050d3041440c900c070181004040b0d00312046000000000000000404234006d0038400b5031b404ed0138400612d0f404ad0428404f0053c41aa
14038440ad003900080000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1340) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (04330104c0633030e00036000cc007f007fc01ff007fa003000000000000000e6417c007f003dc00fb0233c08ff0b35c28bf020b4081f0207c02070802ca88d4403c403f003da005000000000000000ac104c005f0034c40d72337c40df12b7c009f03074061f0107c00db0c044209b0014c001f
00363001000000000000000081405004d0010400c500734004d8911424cd01034060d80034040901014008104005001d00302810000000000000000200044005d2014401d520370805d00174009d00474009d00e7654d900205819980144011c0034a001000000000000000804844008d0024c005100274009d202
5c009d04c740e1d00c7443110a84433910) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1360) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0017c007f202fc40fb001fc00770036c002f4a27d007f080ec293f0047c017f003fc00ff003d8005000000000000000e2203c005f0027800d71017c005f09a4402130904c00531087c81170044c0c1f0037c00df0037a800000000000000000e200f4005d0027400d500174889d4005704910034
020c14435450518234500dd2037440dd0035a003000000000000000680430044d0123400c5011748c8d1300400010210444810303420450200418cd0033400cd0033a010000000000000000c20074015d0167405d100574031741d44189100e440c1129b448b1100f44065d0077401dd0077180100000000000000
0e800fc097f026fc09f3425fc0c371304c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1380) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (037c00ff003da80200000000000000004048c004f0023c80cb0157c00c04160c02434060c0f130105c08cb0000c00df0073c08cf00321012000000000000000200186017d006b401e1095f401210a58601c11049409a14078419a928784016d097b401ed007a0806000000000000000a001c4004
d0023600c900134000108044004108004800101014128900405005d0033400cd003220030000000000000002004c4055d02b7400d10813400d18114400510034400d181140818104604005d0037400dd0034a0130000000000000004200cc045f0037c00db1017c80d30096d02530091d009b1091c02934024c401
f0837c00df003508030000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (13a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00570016d01534c54d205b00d1c065f0017c005f0017a81700000000000000042048500490273500c1c011501c50273406c10272408d100f0403c100324018d0033400cd003320160000000000000004000040161007f401e10059403ed007b403e5007a401090078403c98479401bd007b401ed
007900040000000000000004204c4006b0028400e1001848027003f420a10010400e10020420634018400bd003b400ed0039981300000000000000040050c01530024c01d30854ca0170027c00970854c00530024c40531011c809f0037c00df0037a0100000000000000006600bd006f002fc00ff0017c01ff302
5c00ff002ed00de0035c08c70037c40df0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (13c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (80434008100234008d0021414a10528514ad0528414b10529514a105287148d00234008d00202814000000000000000200634109100234109d0425510b1082c400bd002e400b50828410bd402c4009d00274009d0024a01c000000000000000800074029140274029d00a44829180244209d0024
c479340a540b8100244209d00274009d00262001000000000000000c2043c009300274009f0024800838024c098f0026c889b0024c009b0524c109f0027c009f00250810000000000000000c004bc001f0004c001f00068003f0103ca01f2005c401f0187c041f0085c000f0007c001f0005801200000000000000
06201cc00730017c0053001dc005fa097c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (13e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0274009d00252018000000000000000c804b400ad0129404a1002f423a120a86068d20a24048509a46008110a06088d00234008d00210012000000000000000c20734153d00474051125474171301c44071d0006417110046c8a1500844175d00074001d0007181c00000000000000068063c009
f00a7802930027c619310e6c89be0064c15b708ecc85b7006cc059f0027c009f0027a019000000000000000ec067c14bf052bc149f052ec149f4d27c149f0025c149f0527d009f0027c14bf0027c009f0027a8190000000000000000c07bc00030007c000f0801c04210904c045f0106c04171114c041f0114c041
f00074001d0006b01d0000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1400) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (03c10030700c100364038140e3400cd0033400c50032a014000000000000000000504007100144005300104005b009440375281444371041c40270015f4005d10174005d0014a01400000000000000042050c40332004c00131004c00138986ca4130004c00138004c06130487c000f0007c001f
000508100000000000000004005fc009f0027c009f0027c02970067c009f0025c189f0167c839f0023c009f0027c009f0025801300000000000000042017c009f0025c00934027c00934324d009f21a4d01978824c04830124d029f0027c009f0827a80500000000000000062063400bd006f400b1002f480b9002
44048d01264108120267009500244009d0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1420) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (20574002d000b400a10360481a10048407fd007b441cb0278489e1017bc01e10077400ed00391815000000000000000e050bc013f006fc01b3106cc8193225c409df0377c09fb026ec09e7027bc01f7007fc01ff007d200200000000000000066143c00df0017c00570017c205f1025d405b1037
c00df0015c409f0817c01df0037880df0035b81000000000000000084050d01f3407cd0173405cd01710071c01430078c01c1407ad01814053c01ef007bc01e700781011000000000000000800104036100d8403e100b8403e10028402e50070410e10032410e1003b408ed003b400ed0038800100000000000000
080050401410070401c10070421c120356) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1440) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (037400dd00362085000000000000000c2280d00ff003fe007e801fc0053203ac003f203c80121001cd21a3c03ec00ff003fc00f7003f0805000000000000000c0007c005f0017c00d70037c44df0027d009f0037c04174127c00df02b7c00df0037c00df003700210000000000000006a0d3c005
f0037c00db4034d01d301755289f00b7c221309d6c00d50022410f70037c00df0035a81c000000000000000c201b4008d00034200900004000140004428d04b340b090014400c104b1400c10033400cd0031200600000000000000040003401ad002b40029410c410211019600ad303b44021202a400e5083a480e
5003f400ed003900080000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1460) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00bf005cc041f0806c201b0904d00134063c01fb007fa003000000000000000ee017c00bf000fc003f0103c003f0107d003f043ec041b0206c085f0027c08df0237c00ff003fa805000000000000000a40008009f00274001d0d07c94110d10c001f0035c34170101c84d18524c04df02b7c00d7
0036b001000000000000000080404001d00034008d83234848103004104d143150cc58021480c10120404dd0133400cd00302810000000000000000a00044801d28276009d00274209108144004d0035608d50205414d12464400dd0037400d50034a00100000000000000088204400cd00174005d80174005b602
44091d1034407110184400919074540cd0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1480) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0017c80ff003fc00fe003fc29be102ec207f001fc030f002ec30fc011ec015f401fc00ff003d8005000000000000000e2000c00c34037c80df0837c121f00e18c94f82548231e00e5d0b1b0484c45030007c00db0036a8000000000000000006200c400d10033400dd1037680d504650409d0034
210dd00454001d20254049101b7460dd0035a003000000000000000e804c400c10033400cd00336020504214508d20105880900014080c2201400010023400c900332010000000000000000c200c401d10037401dd28774031501244049d00544031d10454031c0084441110877401dd0075180100000000000000
0e000cd01f3007fc01ff0877c20bb8024c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (14a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (137e80ff003da80000000000000000004048c00c30037c08cf0372c018f0961c85df2342c110f216340bcd8253c810b0063c08cf003210120000000000000002003c501e1407b401ec017a401ed0179405ed02db661ed084b401ec007b541a1807f401ed007a0806000000000000000a001c420c
10133400cd08324250d00c1100cd22525030d00826030d20c3441090023400cd003220030000000000000002004c400d10037400dd0036c265721e44205d003440bdd00a7412cd0874040d10033400dd0034a013000000000000000420acc00d30037c00df2034c22df04a4c185f0014c02df0327e02df03b4c089
b0887c00df003508030000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (14c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1175001ad0273005fc007702ddd4173619fc005f0017a816000000000000000c204b400c10033400cd0033413c10030412c5102340ac146f3602c550b5484c110b3400cd0033201600000000000000040207401e1007b401ed0079401710070481e5004e401e1007b401e500f1603a1006b401ed
007900840000000000000006204f400e1403b400eda03ac00610038480610018400c1002b400e50038600e1080b420ed00399811000000000000000e0057c00d30037c00df0034c00c34064e80534014c01d30023c201f2024f00934003c00df0037a0100000000000000006600bc00ef023fc08ff0237c0067003
ed04ff202c80cdf813fc00ff813ce40fc0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (14e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (80434008500234008d00205348c2520414810027414c105234548d8d204148100276008d20202814000000000000000200624209100234009d00244109d0224508d001a76089548374909120a44009110270009d0024801c000000000000000800070009501e74009c202440a9604e44128020e7
4029004634229f80244089100234009d08262000000000000000000c2043c009340e7c809f0024c809d0064c80932067c00970967c229300a4d81834025c009f00250810000000000000000c004bc001f0087c001e0006c021f0407d021a0084e841f0087018130086c001f0107c001f0005801200000000000000
06205fc00534017c005f0015c256124dcc) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1500) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0274009d00252018000000000000000ea04b4008100234008d08204c08900234008908204208110200808511214808100634008d00202012000000000000000c00734001101474001d2005000130087c201b00044001100844001b00045021140074001d0005181c000000000000000e0067c00b
200afc209f2024c00bb242cc10b3082cc80b3442dd20b7022cc10b3202bc009f0027a018000000000000000e4067c009f4523c009f2027c40b7052fc14af002bc00ff002fc00bb053fc00af002fc009f0027a818000000000000000ac077c00134007c801f0004c041f2104d04134007c84172107c04110104c241
300058001f0006b01d0000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1520) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (03c500b1400cd003050dc10073001c54033400cd0832a0140000000000000002041340071009f4005d00144057140dc02171005c40568201c42170009c4017110134005d0814a00400000000000000042053c20134407c801f0004c22132184c12170c04c001f0084ca0130401c40130007c001f
000508100000000000000006015fc009f0027c009e0027c048f0067c008f00a7c029b0462c088b00a64849f4227c209f00258013000000000000000e2017c00934027c009f0024d129b20e78109b04a0d00930265c00970824c058318678009f0027a905000000000000000220634009100274009d202440091252
7400980024480d500a5430dd0025600910) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1540) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (2057400a1011b400eda17940285817ac220708734112104a911820410ac8ce1017b400ed00391815000000000000000e000fc01b3005fc09ff027c801ab0876c017f1277c05b7006cc0df3007cc0da3007bc01ff007d200300000000000000062043c009f0597c00df2037c009f8026c004b0002
d00190807c001f1804c00db1037e20df0035a81000000000000000000057c01a3405fc01ef1078d01a3007dd01e70079c210f0068c0123407fc21a7007bc01ef0078101100000000000000020017410a1001b440ec0038400800419030f500bd4002900a8400c100ab41085003f480ed0039880100000000000000
0a0053000810217400cd0030410c100750) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1560) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (037400dd00362185000000000000000c200f400f3006fc40ff003cc20231034c8013067fc80330004c00339028c12ff203dc00ff103f0807000000000000000c0007c40df4027c20db0037c109c2097c025708b7e121a28a5c52070027c00df1037c00df003700090000000000000006217bc20d
30027c00df0034c939701f4c005f1033c83171822c811b06e4c11830237c00df0034a856000000000000000c215b400810017400cd00314010524a25000510034030500024030908424238110b3400cd0031205600000000000000040123400a1001b480e902384002581384086d813b48025000a00408002048ce
1463f400ed003900080000000000000002) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1580) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (c99f4504c0033010dc016f00bcc46ff006fc01fb007fa003000000000000000e4017c00bf003b400fb0335c103b032e9043d050fc261f000fc8037040fc84fe01b7c80ff003fa804000000000000000ac007c0093003fc80df02b4d00138325e08130107c001310844021140a4d029d0135c00df
0036b00000000000000000008043480814023400cd01304408d0001500091d03408010a205080000004089d01b3400cd0030281000000000000000020007444914107400dd0034421912065401510407621110864601110064420dd0037400dd0034800000000000000000080007400d124e7400dd2034c419f016
04210b10c74011100c44231300444019d0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (15a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0017c00ff0037c00ff003bc80f7004dcc037009bc10bf4a66da07f003fc00df043fc00ff003d8805000000000000000e0003c00db0037c00db0034c07d90006c03970484c60930064c055f0034820df0073c00db0037a000000000000000000ea00f400d10033400d10034401dd0124403110004
530510034401491834120d10067400dd0035a80300000000000000068043400c90333400c90030440dd0016400c105204100100104044d0130404cd0007400c90033a010000000000000000c2007401d105b7401d10074404d5010440411009440a4106044145c03b0408d10067401dd0077000100000000000000
0e200fc01fb013fc21fb083cc09d1924ac) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (15c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (23b800ff003d38020000000000000008404bc00c30233c00c30070405870241c11830074c01832140c05070771c01cb0153c00cf003018120000000000000008201b481e1007b401e10379529f1024c44db10178405610149605310379401e1417b401ed007800060000000000000008000f400c
10033400c14a70401850081400910000400010004501050171400c90073400cd003020030000000000000002004f400d1403f400d142fc41ac1120040011014440051103442611007c40ee10067400dd0034a0130000000000000004000fc00d30037c00d34034c62d70005c04930024c02434014c90570034d00d
b0237c00df003508030000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (15e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0465001dc0573001e8007f0814c0057001fc005f00152017000000000000000c005b400cd0033400c500300009104c2401810033403c10432400190030400c100a3440cd0033281600000000000000040013401ed007b401e1417b421b9684a401b10071401e10052403ec0878505e500fb401ed
0079000400000000000000066047400ed003b400e501b8400e1000c440a1003840081003810074407c403e1003b400ed00398813000000000000000e0043c00df0037c00d00036900092006c00870005c00934034c00d30234c00d70073c00df0037a01000000000000000062003c08ff003fc08ff003ac00af000
7c00af0237c08ff022ec083f023ec00ff0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1600) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (a0534008d05234008945215008d0824400980520414810d30400810530414cd00234008d00202010000000000000000200734009d00274009100254089522347429500245009102246029180244008d00274809d0024a018000000000000000800034009d00274009b46244019b0060422930024
c539110644439100245009d00676009d0024200100000000000000042043c209f0027c209300204019e1025c029f4024c02831065c159310e0c839f0127e009f002508100000000000000006004bc001f8007c001f10048001b0205c001f60808901f1081c00160087c021f0407c001f0005081200000000000000
0e205bc005f0017c00530017c0a7b001ec) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1620) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0a76009d002508180000000000000004004b4008d04a3400810020404b1812c404a18029606a14128414a9032b4008500234008d00210012000000000000000c60734001d01c7400118084c41310544501110044403110144505110d474091120074001d00070818000000000000000e0067c009
f0067c0093156dc02930824c029304e4447932674c00820167c09b7002fc009f0027a01c000000000000000e2063c009f0527c009f0022c14bb052f814b4053d814bf052ec14bf4527c149f002f8009f0027b81d000000000000000ac077c001f0107c00130105c20172004c80160114c04114104d00110104c040
d00074001f0006b01c0000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1640) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (41c980b1440c904f3480c1207349b8d0083400cd0032a010000000000000000200534005d00174005b00185105b20504005109d5c0451e0d45025b20170035d041b4005d0014201000000000000000042043c001f0007400130004c00300484c00190085c00130006c601b0007c201f0087c001f
000508140000000000000006004fc009f0027c009f4024d209f4067c499f4566d019f18a7c509f8027c009f0567c009f00250817000000000000000e2017c009f002fc00914024c0e8306e4c00930065c009300a0c009b4027c00972027c009f00252005000000000000000400634009d0027400910024400b1c02
c440a10038426e100ac404a1002b400910) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1660) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (6057400e1003b400e50271408e143d0404e5027840dc101100b84c29004000d0253400ed003900150000000000000004000bc01f3407fc01f30074c0def017ec01be007ec01d2005dc0dff106cc89ff0257c01ff007d200600000000000000062043c00df0237c00df0033c009f0003c00972827
c40572024c001d3027cc0df1007c00df0035a81000000000000000004047c41ef017bc01e30078c01bb0068d017a007dc01e9006fc0121407fc01ef084b401ef0078101400000000000000022007400ed013b400e90438400e9409c402e9002d680e900bb440f1009b4002d001b400ed0038880400000000000000
0a0053400cd0033400c109f04a0c900704) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1680) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1f7400dd00362081000000000000000c2037c00f34037c00f7007c48437007fc007b403cc081f011ec8173101bc00df001fc00ff003f0880000000000000000c0007c00df0037c00d700a5c485b01b7c02520284d2a9f0037c049e1097c001f00f7c00df0037080500000000000000062073c00d
38037c00d34032c024b0076c06d70095c21134235c01dd0834c009f0887800df0035a0140000000000000004001b480c12033480cd0033412c400404068501550011100806020800204004d0183440cd0031280200000000000000040023400e1003b400e1403a4c5f9072a48035001960ca10801004bd20384806
d010b400ed003900000000000000000004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (16a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (013f1a4c80153210dc213f000fc003b0047c01ff007fa803000000000000000e2017c00ff003fc00ff033ac043f01070042b0b0745c3f210fd042f110fc907f011f480ff003fb805000000000000000ac007c00d3003fc00d712b5800170502c0a131100c061f1287c00db4017c005f0117c00df
003618000000000000000000a043400c10033400c10131108110304400458300524cd0020408110a034000d0613400cd0030001000000000000000020007400d10033400d500154101502064008500046005d1027448d90027400dd0057400dd0036a00100000000000000080217400d10037400d106344001100f
04921122a45021d0114500010107400dd0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (16c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0017c013f024fc007b203fc00be282f4a5bf082cc947c0077c503d00e70201f000f400ff003c8007000000000000000e2080d081f0044d12570034c519f8474c03df24f7c245320c5c050b00c7c211b1447c40df0037a0000000000000000006200c4009d0024400154034001598234400cd0217
400d106304011d10b7448dd0047400dd0035a003000000000000000a804c4048d04204001500300545d0030490c900334504107014001808034000d0003400cd0033a010000000000000000c200c4008d0104421110134000190034404dd20344244120844011d22074801d0047401dd0077080100000000000000
0e000cc23bf004cc01330274c012f084cc) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (16e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (a3fc00ff003db80200000000000000004048c10cf0033c008f00709004f0160c06974565c05431033c080a402040a0d9343c08cf103012120000000000000002003c401ed105b401ad00784357c015a42164027940de1014b601211258409ad214b401ed00788006000000000000000a001c500d
d00134008d00746130d02b0409cd0071409512ac36000900804020d0303400cd0032a8070000000000000002006c40b1d02e74004d02f4400cc02b6c0bd322b4023d100f74339000f4607dd00c7400dd0034a0130000000000000004200cc001f0067c005f0235c02df0094c025320b4d00d34487c021b0e14c449
f0097c00df003500030000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1700) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (07531197c8077449fc267b0a1ed027f049fc005f0015a817000000000000000c204b400410033401c10030502dd204749105018748f852073426c102f0406cd0073400cd003320120000000000000004000740161007b401e100780416d007b441e10077401f5107a401690078401cd007b401ed
007900030000000000000006204f40061101b400e100394006d003b400e50038500e1003304061003c600ad000b400ed00399813000000000000000e0057c00530017c00d30034c001b1037c00d10014400c30037c001b0036c009f0007c00df0037a8150000000000000006400bc01ff023fc00bf023ec245f003
fc00db8136c08ff093ec80bfa03fc28bf2) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1720) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (8043441a1002f400a500201e0812028420a51038400d155220808105224148d90234008d8020201000000000000000020063408b101af4009100a04109161ac420a4022c4009100234009802244029d04274009d0024a01800000000000000080007402914063000950064402902064544910024
4008104e64869100e6c829d10a74009d0026000100000000000000082043c00930067400930125804930c24ca5930064c02930667c029b0024c048f00e7c009f00270810000000000000000c004bc903f0087c001f4007c101f8007c021d00844821b0007c001f2083c001f0487c001f0007001200000000000000
06205fc02534017c055300144227b14174) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1740) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0674009d0025a018000000000000000e804b4048d0033400810124400810c21480c180204208d002240081092340c8d00234008d0023a010000000000000000c20734211d0157400110040400514106c001100144405d0017440110006c121f00074001d0007181c000000000000000e0067c02b
f00afc009340acc00b3002cc40b3082cd00be002fc00b3022ec20ff002fc009f0027a818000000000000000e6067c149f0527c009f052ec34bf0537c149b0527c54bf052ec00bf052fc14bf202fc009f0025b819000000000000000ac077c00330003c00131000e0003200ce00174004d00132107c001b2114c041
f0007c001f0007301c0000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1760) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00cd63b0601c9c0f3481c910f0003dd2033400cd0032a0140000000000000002005041871001f4005140dec0271021f4007120dc40271045f62871109c4c17d225f4005d0014a01400000000000000042050c001340c7c00130004c00131007c01130084c84131087c28130106e121f0087c001f
000508140000000000000006005fc009f0027c009f0027c089f0264c009d4267c499f04e7c099f0020e05971027c009f00258015000000000000000e2017c009f00a7c00930020d009320e1f029200a4c039f08e6c029340e7c409f04e7c009f0027a805000000000000000620634009d002740091002440081082
74868100204008d80274109121a7402dd0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1780) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (2057402ad000a400eb00e9481ed214341d610773421a1015b405eb014b4292d047b080ed00398815000000000000000e000bc017f007fc09f32074809ff2377401f3017fc0dd34277c09d30277c09dc0277c09ff007fa00200000000000000064043c001f0017c00df0007c001f0027c00930027
c00570037c001f0015c000f0027c00df0035b81000000000000000004054c0133005fc01e30058d01f3406fe41ef007cd01fb007f401e3407ed016f007bc01ef0078101400000000000000020014401a1004b400e110aa402e100bb400ed0038602e9307b400e10098402fd00bb440ed0038800400000000000000
0a00d0503810033440c18130405c100f10) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (17a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (043440dd00362081000000000000000c2007c027f003cc00f3003cc00ff216cc887320bfc04b3009ce40f3400cd003b002fc00ff003f0880000000000000000c0087c02ff000f800df003fc00de2c27c00d70117c06df02a7c42d7c083c061e0107c00df0037000100000000000000062073c0cd
f0037c00d30034c53cf00a7c20db28b7c53d300f7c03c381c7c011f0827c00df0034a814000000000000000c201b4030d0002400c900014100d02034001900024010104074010921034011d0083400cd00332806000000000000000400234002d003b440e12018424ed000b42ae9131b604e10123412e901034146
d090b080ed003900000000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (17c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0837010cc0c11058cc0033000cc003f0017c81ff007fa003000000000000000e6017c007f000fc00ff030fc081e030fc001e0407c863f000fc403d008fc083f130fc20ff003f9805000000000000000ac007c005f0034c00d32310c040f1284d10130803c80134504410130104c041b0387c00df
0036300000000000000000008043400cd0040500d110225001d010050401440344c010100624000000404018007400cd0030001000000000000000020007440dd0074400d1003040a1c00244009184234105108344101104444011900e7400dd0034a001000000000000000800074005d0004400c15206c031c102
4010110007400110106d0b110044403110) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (17e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0037c00ff003fc00ff003dc507f011fc88174807d000f68cfd433f1165d003f001fc00ff003d8005000000000000000e2003c00df1037c00d140349014d8057c02170084c22d30804c00134086c8a1f0207c00df0037a8000000000000000006200f400dd0037400d100344015d2087490d90430
410510824410010406430dd2417400dd0035a003000000000000000e804f400cd0033400c100304245d118340ccd02204460101304124105824164d0493400cd0033a010000000000000000c200f401dd0077401d100744005d04874041905144041110044461100a44028d3197401dd0077180100000000000000
0e000fc01ff003bc01f31076c096f010fc) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1800) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (23fc00ff003da8020000000000000000404bc00c30433c60cf0971ca00f0170d04830460c0d030110410d14420c00430177c00cf003210120000000000000002003f401e1027b421ed017b40175066840121415860da10070409e10878401a1007b401ed007a0806000000000000000a001f400c
140f3400cd00314030d01204210100c0403010204405812054480012033400cd003220030000000000000002004f400d1003f400dd0832c01170054490510ad4480510aa4621910ad4408010037400dc0034a0130000000000000004202fc00d30137c00df0034c2a5f0014c02530094c0ed30034c02d30094d031
300a7c00df003508030000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1820) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (025340d7d08534015c00574014d10510217c005f0017a817000000000000000c204b400c14033400cd003340481007240bc102f3403d10831400c50270402c10067400cd0033201600000000000000040007401e1017b401ed007b40121c07a481e1107b483e10059401e50078401e1046b401ed
0079000400000000000000062047400e100bb400ed003b400e1002c480c1002040081203c420410030400c10003400ed00399813000000000000000e0057c00d30077c00df0837c80130024c00d31064c40d50004c80130014c00d30007c00df0037a01000000000000000066003c00ff083fc00ff023ec005fa07
fcc09f0037d04ff403fd00ff082fc08ff0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1840) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (80434008d0523400810023401810539614ad1d28654a10528534e10528414a105234008d00202814000000000000000200634009d0027400918027404d1002f402ad242c602b10038400b10028400b100274009d0024a01c000000000000000800034009d00274009100234819b40a44039d0024
4029141a44009146245589140274009d00262001000000000000000c2043c009f0027c00930027c009300224039f0264c009b0024c10930064c11830027c009f00250810000000000000000c004bc201f0007c001f00078081f200dc101f04848001f20069000a0087c021f0007c001f0005801200000000000000
06205bc00530017c005e0017800710456d) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1860) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0274809d00252018000000000000000e804b4008100a34008d0020430a10028402a10529450a11028482a100a85528d05234008d00210012000000000000000c20734001100074001d00045053917c45171100c45071103d44411100444051d00c74001d0007181c000000000000000e0067c009
3416fc009f802c4009b4864c21931464c95930364c039360e4801bf0467c009f0027a0190000000000000006e063c009f0023c009f0027c14bf0526c149f0537d149f0527c149f0527c149f852fc009f0027a8190000000000000008c077c001f0107c00134007c2011010fc041f0104c24132104c04112904c841
30107c001f0006b01d0000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1880) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00c10036001c10070410c10070480810033400cd0032a0140000000000000002005340051001b4005d001f4015300d440251001440151085448351a0544005120174005d0014a01400000000000000042053c00131047c801f2007c08330004c02130186c00130084c08119004c00130087c001f
000508100000000000000006005fc009f0027c009f0027c049b0567cb19f6966c049f0063c059f2227c429f1027c009f00258013000000000000000e2017c00930027e009d1824c009b4024402930825c019308a4d009300e4c009f0127c009f0027a805000000000000000620634009100274009d0024440b1802
8494a1202d4a0a1413c462a104284008d0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (18a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (2057400ed001b400e90258c19fd016054db10054411a1054b411a1204c441ed157b400ed00391815000000000000000e000bc01ff004fc21ff2054e01ff1074c0df3005dc01d31077c25d72264c099f0277c01ff007d200200000000000000066043c00df0017c00df0017c001f0817d605f2007
4001f4007d005f1027c005f0077c00df0035a81000000000000000004057c01e3407bc01ef085bc012b4078c0143407ac01430078c01e10078c01c340f3c01ef0078101100000000000000020017400e10093400ed001b400e10090480a10030410a10080480410410400e1017b400ed0038880100000000000000
0a0053400c10073400cd0013420d928704) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (18c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (033400dd00362085000000000000000c2007c00ff003fc00ff001ec0371222cc012b10fcc03f3209cc08b3001fc02d3003fc00ff003f0805000000000000000c0007c00df0017c00db0017c00df3017d02980023c845f40334401a0091c061f0037c00df0037000900000000000000062073c40d
f0037c00dd1016d21df01a4400d70c24c00d102f7c019340365801e007fc00df1035a814000000000000000c201b400cd0013400cd00104861d0144400c500004001100c30011111a24024d1033400cd0031200600000000000000040063400ed000b400ed001a4012d2118400e5033840c61093b40061003a400e
d023b400ed003900180000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (18e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (81036046c81b7004cf01f3402cc0033004fc01ff007fa803000000000000000e6017c00ff001fc00ff011fc001b010f4201f0307c9837800fc003f000fc007f043fc80ff003fb805000000000000000ac007c00df0007c00df1396c14170d04c141b0334c24834000c14530017e00d30037c00dd
0036b00100000000000000008043400cd8813400cd0410404954320404010100404090420584810403610010437400cd0030201000000000000000020007400dd0007400dd0016440950024400590004400911024400d10827430110037400dd0034a00100000000000000080007480dd0017400dd001440151001
451a110844507530014420114107403515) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1900) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (2017c00ff003fc00ff103ed400f0066c03fd093dd21fb080e800ff006fd102c008fc00ff003d8005000000000000000a0003c00df0037c00df0035c1a1f0067c02130104c01970240480c30064c01131147c00df0037a0000000000000000006200f400dd0037400dd00354209d0227400d10014
424d5a005400d10234441911007400dd0035a003000000000000000e8043400cd0033400cd00314000d0021620011800420958004400d10024400014003400cd0033a010000000000000000c0007401dd0077401dd00744001c1827601110004421910044401d11024441110847401dd0076080100000000000000
0e000fc01ff007fc01ff007cc001f102fc) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1920) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00bc00ff003da8020000000000000000604bc00cf0033c00cf0070c0d831461c47cf8370c01cd00c3c85c38261c19434343c00cf003210120000000000000000001b401ed007b401e40078001a100696493d0168401b98b4b43de0036f40d21094f401ed007a08060000000000000000000f400c
d0033400cd08305228101e14100d00044108c0403400c10021401010183400cd003228030000000000000002004f400dd0037400d60034011d100b4403dd00b4405c9019740ad10973402910003400dd0034a0130000000000000004200fc00df0037c00df0034c06134026c081f0164d009f1087c00d30025c009
30087c00df003500030000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1940) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (007f011dc0463085dc00534858c037f009fc005f0017a817000000000000000c205b400cd0033400cd0033428cd0075433cd84b0481c10070400c58a30501cd0273400cd0033201600000000000000040013401ed007b401ed007b401ac0069621fd8079401e110cc401f10070403ed007b401ed
007800040000000000000006004f400ed003b400ed003b400ed1029400ed0038c00e10038520e520284806d003b400ed00399813000000000000000e0043c00df0037c00df0037c409f0024c01cf0015c40c34841e01d10024c001f0027c00df0037a0100000000000000004600bc00ff003fc00ff003fc00bf023
4ca0ff0237c00eb002fe20ff023bc00ff0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1960) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (80404008d00234008d00234948105234008d00205019d00234408145244548d00234008d00202814000000000000000200604009d00274009d00274809101a74009d04244049d00a74029105244209d01274009d0024a01c000000000000000000045008d00274009d00274089100674009d0064
4439d00a74009100645019d00674009d0026200100000000000000042040c009f0027c009f0027c40956027c089d1164c019f0627c04930064c888f0067c009f002508100000000000000004204bc001f0007c801f0007c001f020740a1f0085c001f0087c001f0007c101f0407c001f0005801200000000000000
00005fc005f0017c005f0017c007f0055c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1980) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0274009d002520180000000000000006804b4008d00234208d2020485990422400818427400cd00234808504a04028540274008d00212012000000000000000c20634001d00074001d00044061241854401501074401d00174001101044801108074001d0007181c000000000000000e8073c009
f0027c009f0024c12b1052cc00bb802fe00bf002fc00b7002cc00b3002fc009f00270019000000000000000e6077c009f0027c009f0027c94bb052fc00bf052fc40be282fc00af052fc00af002f4009f0027a819000000000000000ae070c001f0007c001f0007804130107c005f0004c001f0007c00130104cc45
f0007c001f0006b01d0000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (19a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (888d0073406cd0aa04904100b3401cc1233400cd0032a014000000000000000000434007d00174005d20174016ba0df4006d14db4027d029ec0271221f4047d001f4005d0014a01400000000000000042053c001f0007c001f0007c21130407c211f0187c801f1084c08134207c801f0107c001f
000508100000000000000000205fc009f0027c009f0027d049d00e5c409d0127c009f0027c009f40e3c048b10a7c009f0025801300000000000000040017c009f0027c009f0024e019b0026c029301670009f0027c00970024d01970063c009f0027a805000000000000000420634009d00274009d002440091002
740a950027408dd1067600910024402952) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (19c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00574006d003b400ed0370018332142c02ed13685050d00134884107244088d0343480ed003908150000000000000004201bc017f007fc01fb0074801f3206cc09ff007c9014f227fc0137027dc09ff0047c01ff007d280200000000000000062043c005f0037c00df0037c009f0007c00df2007
c001d00374004f0807c001f0007c00df0035a01000000000000000004053c016f007bc01ef007be01a1007bc01ef007bc816f0078c0161005fc212f806bc01ef00781011000000000000000220134006d003b400ed003b410e90423400ed002b600ad003a40161403b400ed001b400ed0038880100000000000000
0a00434004d0033400cd0033401c100774) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (19e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (003400dd003620a5000000000000000802034007f003fc00ff003fc00bf022fc13f3000de0033001dc0073400cc0313806fc00ff003f0805000000000000000c0017c005f0037c00df2037c00170227c025f0887c681f00b7c025f0027c041f0207c00df0037000100000000000000060053c005
f0037c40db0034d0b934034c47df0044c009f01f3c00570065c068f0067c00df0035a8040000000000000004008b4004d0033400cd00304000910024024d06c04000d80134004100044030d0003440cd00312806000000000000000400034006d003b400ed0038500a902284006d00084243d80bb4006510194c02
d100b400ed003900080000000000000004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1a00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (21b3000dc01df0306c00130104c041f1807e01ff007f8003000000000000000ec017c007f003fc00ff033fc243f0183c246f0307ccc3f001fc047f010fc043f440fc00ff003fa80500000000000000006003c005f0037c00df03b7c089d03a7c08530005c0a170295c08530204c88110107c00df
0036b001000000000000000080434004d0033400cd10334800d0003400498b06404014013480410000401010403420cd00302810000000000000000a00074005d0037400dc00374519d0027480d100474011500b7401510044440910207400dd0034a001000000000000000822074005d0037400dc00374811d804
74805b04c2401112257487d104c4401112) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1a20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0217c00ff003fc00ff043fc00fb003fc10bb1165c00ff00afc023f206fc702f0097c00ff003d800500000000000000042013c00d30037c00df0037c20d20037c818340c7c00df1966d019b4044c041f00c7400df0037a8000000000000000006200f400d10037400dd0037400d58034401952002
400dd2014400514924504dd0c07400dd00358803000000000000000e804f400c10033400cd0033400c18033440810203404dd0182400091090402cd0203400cd0033a010000000000000000c200f421d10037401dd0077401d50074421911424414dd001440b51a0e44121d0057401dd0077080100000000000000
0e000fc01f3003fc01ff0077c01f34077c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1a40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (017c08df0035b8020000000000000000405bc00c30037c80cb0573c45cf0072c118309e0c05d30165c030b0753411c34053c00cf003010120000000000000002001f401e1007b401ed817b405ed007a40da11978401e1815a419e9025b40521017b401ed00788006000000000000000a004f400c
14037400c900b3400cd2032400810090444d14001400090003400010023400cd0032a0070000000000000000004f400d1003f400dd0037400dd0032c80112094444d10026c890b0023401110027400dd0034a0130000000000000004202fc00d30037c00db0037c00df0036d00534194c40d300254029a3097c001
308a7c00df003508030000000000000004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1a60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0867005c0005f091c40361221cc047b001fc005f0015a817000000000000000c204b400cd0033480cd1031400c9803040a010234440dd0030403c108b0407d900b3400cd0033281300000000000000040007401ed007b401ed007b401e9087a481350078481ed0078441e190704c1e910734c1ed
007900000000000000000006204f400ed00bb400ed0039e00e15038500a10038480ed0018400c30038400c1003b400ed00398813000000000000000e0057c00df0037c40df0037c00d31076c00871014c00dd0014100db8024d00d34067c00df0037a0140000000000000006600bc00df0037c00df0037c00df003
7c008f0027948df003742ccf0213c00df0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1a80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00434008d05234008d00234008d0022400810522400814522414c145205548d85234008d00202010000000000000000400634009d00264009d00274009d08244209902a60009100245089002344009d10274009d0024a018000000000000000800074009d00274809d00674809c0026c019100a4
c06910024c009100644009d00274009d00262001000000000000000c2043c009f0027c009f00a68009b0024c029b1064c40930020c40932024c009f0027e809f00270811000000000000000c004bc001f0007c001f0007c00170007c001f0007c021f0407d0e1f0003c00170407c401f0007001200000000000000
06205fc005f0017e005d0017c005b0016c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1aa0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1274409d0025a818000000000000000e804b4008d00236008d00334008d80205008911a34808108a36088d22224028d00a34008d0023a012000000000000000c20734001d02c74001d00074001d08054001940c74050105c54021d0084c075d00974401d0007081c000000000000000e0063c009
f00e7c009f002fc809f102c800a100eec08b30067c85af016cc03bf0167c009f00278018000000000000000e6067c009d0527c009f0027c009f0023c80bf052de949f2d2dc00bf202fc14bf002fc009f10279819000000000000000c4073c001f0106c401f0806c001f0004c001b0102d00030104c841321044041
f01074001f0006b01c0000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ac0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (428d86b4406c190304b185102040ac18033400cd0032a014000000000000000000134005d00174005d001f4005d001ec2b61005c401710014c027100546027140174005d0014a01400000000000000042053c001f0007c001f8007c001f1004c001b4084c20130004d00171204e12132087c001f
000508140000000000000004005fc009f0027c009f0027c009f1027c23972067c409f0023d009f30a5c028f0067c009f00258017000000000000000ea017c009f0027c009f0027c209f00244119200e7c00932027c008f0066d039f0867c009f0027a805000000000000000620634009d00274009d00274009c002
54009801a74009140a57009d0026400dd0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ae0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (2057400e1003b400e1004b408cd025851c8d10534012d0138406e10028404e1097f400ed00398815000000000000000e000bc01f3007fc09fb104bc21ff0854c09af0177c45ff047dc85e3207cc0173027fc01ff007fa00200000000000000062043c00df0037c00df0007c20df0017c001b1007
c80de5037d20df2022e009e2037c00df0035b81000000000000000004053c01ef00fbc01ed206bc81ef0858d01af2840d01634170c01e70078501c30073c01ef0078101400000000000000022013400ed013b400ed000b440ed101a582358038491e10138402e10069400a1807b400ed0038800400000000000000
0a0053400cd0033400cd0433620cd28104) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1b00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (037400dd00360081000000000000000c2203c00ff0037c00ff000fc40ff001ec00f2214bc4533903cc30e30577c05ff003fc80ff003f0880000000000000000c0007c00df0037c00d74007c00df2015c201f0037ca0df0037e409f1023c00170037c40df0037000100000000000000062053c00d
3503fc00d90007c00de00165019d1237c209f203dc22914174500db4037c80df0035a814000000000000000c201b400c10833400c11003440cd10120418d10134400d027440bc120e0400c90273400cd0033280600000000000000040003400e1003b420e1200b400ed021a480ad003b4006d803944ce100384006
9003f400ed003900000000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1b20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01ff1074c003f000ec013f007fc01ff005fc01ff007fa003000000000000000ea017c00ff003fc00f70007c10ff341dc04bb230fc821f2d3fc10ff9d2dc443f0337c00ff103f9805000000000000000a4003c00df1037c80df8187c80dd2016d0a978327c861120b4c00d140b742a0f0bb7c00df
0036b0000000000000000000a043400cd2033400cd0743480c5041240095010340c012032480c108214a00d2033400cd1030201000000000000000000007400dd0037000dd8047400dd0016681952027400910034401d100374401d0037000dd8034a00100000000000000080007400dd0037400d70047400df801
4c41014007401d14036d43518065c031d0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1b40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0017c00ff003fc00ff003fc40fe003fc10ff083fc001f080f8103f003fc10ff001fc00ff003d8007000000000000000e2003c00df0037c00df0037c20df0037c00de0035c031f20c6c401f0037c00df0017c00df0037a8000000000000000006200f400dd0037400dd0037400dd2037400dd0035
4111d00476081d0037400dd0017400dd2035a803000000000000000e804f400cd0033400cd0033400cd8033480cd00314001d00026800d0033400cd0013400cd0033a010000000000000000c200f401dd0077401dd0077401dd1077401dd00754011d00474011d0877401dd0057401dd0077080100000000000000
0e000fc01ff007fc01ff087fc01ff0077c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1b60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (013c00ff003db8020000000000000000404bc00cf0033c00cf0073e80c78173c08cf9270c0d0f0203c000f0033e50c30153c00cf003010120000000000000002003f401ed007b401ed007b401ed117b409ed00785052d024b4292d007b401e1415f401ed00788006000000000000000a001f400c
d0033400cd0033400c50033428cd20704090d00830020d0033403c10013402cd0032a0070000000000000002006f400dd0037400dd0037400dd8037440dd2c3400b4d1187006dd0037403d10017400dd0034a2130000000000000004208fc00df0037c00de0037c80d70037c00dc0434c025f0487c009f0037c00d
30017c04df203508030000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1b80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (004f0017c007643dcc0f6f1014c0053001fc005f0015a817000000000000000c204b400cd0033400cd0033420cd0032440cd0033409c50070401cd0032400c10013400cd0033281200000000000000000207401ed007b401ed007b041ed007a421ed807b481250060421bd2078481e1005f401ed
007900030000000000000006204f400ed003b400ed003b400ed00384a0ed003b4006100384006d103ac00e1401b400ed00398813000000000000000e0057c00df0037c00df0837c80df0034c00df0037c00131014c001f0034c01c34017c00df0037a0150000000000000006600bc00ff003fc00ff0037c00ff023
7c08ff023fe281f0217c001d0037c00df0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ba0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (80434008d00234008d00234008d00204008d00204148105304009d00234008100274008d00202010000000000000000200634009d00274009d00274009d00247009d00a44049901344049d00270009144274009d0024a018000000000000000800074009d00274009d00274009d00244119d1024
5019120644119d00274009100a34009d00262001000000000000000c2043c009f0027c009f0027c009f0024c029f00a4c818b0060c009f0027c00930027c009f00270810000000000000000c004b4001f0007c001f0006c001f0005c021f0087c04190007d001f0007c001f0007c001f0007001200000000000000
06205fc005f0017c005f0017c005f1016d) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1bc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (02f4009d0025a018000000000000000e804b4208d00234008d08224008d80234008d10344008100214008d0023400a1002f4008d0023a010000000000000000c20734001d00074001d00074001d00074201140044021102944001d00074403140074001d0007081c000000000000000e0067c009
f0027c009f1027ca09f1827c00b3402cc10b3012cc40bb202fc00930027c009f0027a818000000000000000e6067c009f0027c009f0027c809f0027c008d082fc00bf002fc00ef0027c009f002bc009f0027b819000000000000000ac077c001f0007c001f0007c001f0804c801f0004c441b0104d001f0007c001
30007c001f0006b01c0000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1be0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (12cc04b3401cd0033401c100330004d0033400cd0032a814000000000000000200134005910174005d00174405d00174037d009f4857d005b4116148170005d01574005d0014201400000000000000042153c001f0007c001f0007c001f0007c001f0007c221e0287c00130007c003f0007c001f
000500140000000000000006015fc009f0027c009f0027c009f0827c00934027c008f0267c049c00274009f4027c009f00250015000000000000000e2017c009f0027c009f0027c009f0827c009f0020d119300a4c829b2027c40930023c009f00252005000000000000000620634009d00274009d00274009d002
74009d00240019140245009d0027400b10) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1c00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (205f400ed003b400ed1173801ed207b40523234b40701006b003a1827b4056103634006d00398815000000000000000e000fc01ff007fc01ff007fc09df227fc41530053c01b3027fc09f3027be0973006fc01ff007fa80200000000000000066043c00df0037c00df0037c00df0037c401f0017
c001f0007c001f0033c005f0017c005f0035b81000000000000000004057c01ef007bc01ef007bc41ee007bc01ef007bc01ef105bc0163007bc016f005bc01ef0078101400000000000000020017400e9003b400ed003b400ed003b402ad101b4006d002b400a1087b4006d003b4006d0038800400000000000000
0a0453400cd0033420cd0033400cd00334) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1c20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0154004d00362881000000000000000c200fc00ff003fc00ff003dc00ff083fc083f001cc003f0007e003f003fc00b3001cc00ff003f0080000000000000000c0007c00df0037c00df0035c00df0037c00171017c001f0007c021f0037c00970037c005f00370001000000000000000620dbc00d
f0037c00df0037c00df0037c001b0017c01034267e81934037c009b0033c00df0035a0140000000000000008201b400cd0833400cd0032400cd80334000100034070100434680100334004940034004d003320060000000000000004002b400ed003b400ed013b444eda13b4c429002b414a1050b40421113b4016
9000b400ed003900000000000000000006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1c40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (850cc1433850cc14008500214008500214008500214000000000000000000006c01fc00ff003fc00ff0034c00ff0137c423f030fc0c1f0007c001f0237c089f0203c007f003fb0050000000000000008c007c00df0037c00df0535c10dd2c37c241f1284d0c1f01074041d0037c00930204c00df
0036900000000000000000008043400cd0033400cd0333404c503334050d00004041d04034100d08334008100214004d0030201000000000000000020007400dd0037400dd0037400dd00374001d00c44011d00674419d2037406910024400dd0036a00100000000000000080007400dd0037400dd0036c00df203
74001d10544031d01c74231d8037402914) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1c60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00000010000400010000400010000400010000400010000400010000400010000400010000400000000000000000000000000040001000040001000040001000040001000040001000040001000040001000040001000000000000000000000000000800020000800020033800ce003380002003
3800020000800ce000080002000080002000000000000000000000000000084402110084402112184402110084402110084402110084486110084402110084002100000000000000000000000000080002000080002002180002000080002000080002000080086000080002000080002000000000000000000000
0000000850021400850021400850ce1433) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1c80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0033800ce0000800000000000000000000000840021000840021000840021000840021000840021000840021000840021000840021000000000000000000000000000800020000800020000800020000800020000800020000800020000800020000800020000000000000000000000000000850
021400850021400850021400850021400850021400850021400850021400850021400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000040001000040001000040001000040001000040001000040001000040
0010000400010000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ca0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000000000000000000000000000000000000000000000000000000420800000000000000000000000cc0000000cc0033000000000000cc00000000000330000000108200000000000000000000000400010000400010000400210000400210008400210008400210000400010008400
01000000000000000000000000000010000400010000400010020400010020400810020400810020400010000400810000400000000000000000000000000840021000840021000840ce1000840ce1033840ce1033840ce1000840021033840021000000000000000000000020033800ce00338000200008000200
00800020000800020000800020033800ce) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1cc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000f0f00000000000000000000000000000000000000000000000000000000000000000000000003c3c00000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ce0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1400850021400000000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000000000000000000000000
000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000
000003fffffffc00000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1d00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0100004000100004000100004000100004000100004000000000000000000000000000400010000400010000400010000400010000400010000400010000400010000400010000000000000000000000000008000200008000200008000200008000200008000200008000200008000200008000
200000000000000000000000800008440211008440211008440211008440211008440211008440211008440211008440210000000000000000000001000008040200008000200008000200008000200008000200008000200008000200008000200000000000000000000000000008500214008500214008500214
0085002140085002140085002140085002) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1d20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00000840021000840021000840021000840021000840021000840021000840021000840021000000000000000000000000000800020000800020000800020000800020000800020000800020000800020000800020000000000000000000000080000850021400850021433850021400850ce143
385002140085002140085002140085002140000000000000000000010000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000004000100004000100004000100004000100004000100004000100004000100004000100000000000000000000
0000000010000400010000400010000400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1d40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000c20000000000000000000000000000000000000000000000000000000000000000000000000010820000000000000000000000040001000040001000040001000040001000040001000040001000040001000040001000000000000000000000000000010
000400010000400010000400010000400010000400010000400010000400010000400000000000000000000000000840021000840021000840021000840021000840021000840021000840021000840021000000000000000000000020033800ce0033800020033800ce0033800ce0033800ce0033800ce0033800
ce0033800ce00008000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1d60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (fffffffc0000000003fffffffc0000000003fffffffc00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
00000000000000000000000f80000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000010300000000000000000000000000000000000000000000000000000000000000000000000003c3c0000000000000000003000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1d80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000000000000000000000000000003fffffffc0000000003fffffffc
0000000003fffffffc0000000003fffffffc0000000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc000000000000000000
0000000000000003fffffffc0000000003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1da0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (001800060002a300000000000000000a8803a804ca45ba004ea01329864201b29064a01ba084ea013a804ea0d3a804ea053a804ea052a20000000000000000000401a00068001a00068001a00060651a0006a501a0086a001a80068801a00068021a0086a0000100000000000000000284012010
480612010480412010e80612018e80412010480412010480612010480412010480600100000000000000000a0803a808ea02ba008ee823a808c0823a008c2023a018ea022a808ea023aa08ea023a808ea022a30000000000000000080403b020ec0a3b020e8083b308ea0a3b028e8083b108e8083b020ec0a3a028
ec0a3a038ec0a2a3000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1dc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (02104084000104004100104004102104006100144006a30000000000000000000480800820060000082000000840200800820110020020030800c20020880820022000060030010000000000000000000402a02ea8138200e88038200ea803aa02ea80b8200ea803aa01ea803aa02ea807a200ea
80380100000000000000000a8800a814aa010a810280c2a81c0a042a81408040a81028040a0182a010a8142a070a83428042a30000000000000000008c01080462011080042001882442001880442001080042001080042011080c42011080442002a30000000000000000008c0180004020188006000100804020
1009040201882060001800060001800860) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1de0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (04032010c80432014c80d32010ca0432030ca0432034ca0c32830c80432010c80432010ca0c00100000000000000000004030000c00030004c00120000400030000400020004c00030000800030000c00030000c00000000000000000000000a8c030810c20430030c60420810600530830620c2
0010c00430810820430810c20430810c2042a20000000000000000008c01b0006c001b400680019000e9001b000e8011b00068011a00464001b0006c001b00068012a30000000000000000008c01a8026a00928026800928024e009a8026e00928026e009a80268009a8026a009b8026a00aa30000000000000000
0a88801021040041801840041021060040) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1e00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (048201208048010000000000000000000000a018a8060a01828062a01c00062a01808060a018a8060a01828060a01828060a018280600100000000000000000a8802a801a2004280188006a80100006a801880062801880062001a2006a801aa006a80188006a200000000000000000088018812
620490812420598816420598816c20510816c205b0816620598816620598812c204aa30000000000000000008c010010400410810600410010420410014c00410810c00430010400510010400410010c0042a300000000000000000a8801a8106a0412030ea0c1a80048041a8106a05120246a0c1a8346a041a814
6a051a8106a0c2a3000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1e20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (010c80d10010c80532214480512014480512010e80400000000000000000000a8803a818ea063001842063a81ac4063a818c2863001ae206388184a063a818ea063a818c2062a20000000000000000008003b018ec063b818ea073b818ea063b01868063981ce8063a018ec062b018ec0639018e
8062a20000000000000000008803a818ea063a818ea073a818e6031a818e6033881ce6063b818e2063a818ea073a818ee062a300000000000000000a8c02b01884062b818ac062901806062101884062b818a0063b018ac062b018ac062b018ac062a3000000000000000000000020120004820120a04820120804
8221200040201208048201208048201208) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1e40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (8802a830aa080a03028042800028082a82028482a83028042a0302a042a8302a040a81028042a200000000000000000088018810620418a1042051881442041881042040881042041881042041881042041081042842a20000000000000000008801001040041001060051001042041001040050
003460041001060041001060051801060042a200000000000000000a88032800ca103a800ea01328004049329004a0932804ea0030800ea0032800ea013a800ea002a20000000000000000000001a0186806128184a0f1a83c600f1a03c6a0f1203c6a071a81c68071a01c68071a0186a060000000000000000000
0200012010480410010480412010680412) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1e60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (003080062000000000000000000000000001b8006e001300048001b8004a001b000e8001b800e8003a0006c001b0006c001b000e8002a10000000000000000008801a8006a001a8006a00128006e001a8006e001a0006c081b4206808188206a081a4006e002a200000000000000000a88001014
0405018100405010100624810140405a181004040101404040101404040101004042a20000000000000000000000800020000800022081000020000800020002002020010800020810800020091800420010000000000000000000000002a030a80c2a010a80422114a8042a030a80c22010a80c2a030a80c2a030
a80c2a010a80c00000000000000000000a) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1e80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (880c22018880620118880622118880620118804622100000000000000000000000010006400190802400090002c00a90006c0019002240009000640009000640009000a40008000000000000000000000001a8316a0e5a0316a0c5a8212a0c5a8312a044a8396a0e5a8392a0c5a8316a0e5a8316
a0c40000000000000000000000032028c80e12008480230018480232028cacb12008ca0e32a28888a32028c80f32208ca0a00000000000000000000000030002c022900024002b010a4023b000200009008a40028001ac002b0002c002b000a400280000000000000000000000031800c600100004601318044401
30800620011080620118800c28030800c2) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ea0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0003a804ea013a804ea093a9206e013a020e4003a804ee013b004e9013a804ea013a004ee010000000000000000000000000100c8c032980cac022900c8e022100c040321808ac0229008ac0201008ac022b00cac0300000000000000000000000002014000d020140a8c02014080500014080d0
001008050201408050201408040201408050000000000000000000000002a10428012a10428410210428600a00408402a18428412a10428012a10428010a00428410000000000000000000000002a080a8002a880a8202a18088202a88088202a080a0202a100aa0028800aa002a888a8300000000000000000000
0000018880622018880622018880c22818) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ec0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (edc9e37218dc0000000000000000000000009ff72fffc9fb727efcbfff2fefcbbf727edcbfbf27ffc9fff2fffcbdf72fffcbfbf2fffc00000000000000000000000027e92fffc26490997cbfff2f97cbbe909924be5f09ffc27ff2fffcbde92fffcbe5f2fffc0000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000009fb727edc9fb727edc9fb727edc9bb727fdc9fb727edc9fb727edc9db727edc9fb727edc00000000000000000000000099b4242d090b4242d898b4242d011b424ad090b4246d090b4242d89894
242d090b4246d000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ee0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (814e20138004e20138004e20138804e20138804e201000000000000000000000000180006000180006002188084050180006200180006002182006200180006000180006006000000000000000000000000120104804120104804120104004120184804120104804120104804120104804120104
8040000000000000000000000003a808ea023a808ea023aa08c6043a808ea023a008ea063a008ea023a808ea023a808ea0200000000000000000000000039020e40839020e40e39828e04239028e00839020e40a39020e00839020e40839020e40a0000000000000000000000000863127ec48631218c48631218c
49a3121ec48631218dc87b127ec485b127) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1f00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0c0080082000080002002880028200a000222019000200008000260038800020002000020008031000000000000000000002800ca0032800ca0032800cc00b2000ca0030000c00032a00ca0072800ca0032000ca0030031000000000000000000000881d220548815220548015200c4883520044
881122054881120004881522054883522054000000000000000000000001080442011080442039001642009080642009080242019080242009080442011080442018000000000000000000000001800060001800060001800060001800060001880060001880060001800060001800060000000000000000000000
0000038824e20138804e20938004e22138) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1f20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0430010c00400002000000000000000880030000c00030000c02030000402130080800030004c00030004802030080c00030000c00000002000000000000000a88030810c20430810c244308104604b0810820430010c20430810c04430810c20430810c2042a202000000000000000080419000
64001900064009900241001940260011900064009800060011900064001900064002800800000000000000000c01880062001880062001880062001880062001080042001000066001880062001880062002031000000000000000000c001000040001000044081102840021102040011800044081800040001000
0400210000400203100000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1f40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (018a80608018200608018a80608018200608018200608212000000000000000a88428800a20028800a20028800080028800080000800a20000800800028800a20028800a2002a202000000000000000008018810620418810620410810420c30810c20410810620410810c204188106204188106
2042820a000000000000000000010010400410010400418010600410010400410810400410810c00410010400410010400428002000000000000000a8801881062041881062001a81062009a810620c1003062041003062081881062041881062042a202000000000000000004030010c00430010c00430010c00d
30010c20c30034c00430034c20c30010c0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1f60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (8843a818ea063a818ea06ba81846063a818c20630818ca0630018c20692818ea063a818ea062a20a000000000000000000039818e40639018e40639018e00639818e00638018e80639818e0063b018e40639018e40628002000000000000000008038818e20638818e202b8808e20238808e6063
8818e20238818e206b8818e20638818e20628000000000000000000a8802b018ac062b018ac062b018ac86ab018a4062b818ac062b018a0062b018ac062b018ac062a2020000000000000002080020100804020100804020100a04020100804122100804028100a040201008040201008040001200000000000000
0208008018200608018200608018208608) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1f80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (040881022042a202000000000000000288010010420418810421418810421410050620418a10620518810429410850420410810420428202000000000000000008018012600410010601490010601498052400410812400490012601498050600418012600428002000000000000000a88038001
e20070801e20070801e20078101c20070001c20070801e20078901e20078801e2006a200000000000000000208018018600618018600618018600618018620610018600610018620618018600618018600600002000000000000000000012012480412010480492010480492012e80410012680490012e80492010
480412012480400002000000000000000a) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1fa0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (082e00091002642091802e0109800264001800064002a002000000000000000000018000620018800623018880621018080660019800622018800661018000620018800620028002000000000000000a88001010040401014040401014c424010900405010100404118100404010100404010100
4042a202000000000000000000008004200108000200108000820108004200008000620018000200108004200108004200100002000000000000000888028030a00c28030a00c28030804428010a00c02010a00528010a04c28030a00c28010a00c08202000000000000000a88008810220428a302240288302000
08800a00c28830a20c2883020000880022) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1fc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (80010000400010004400000004600210008400110800400010000400210000400010000400028202000000000000000a88018830620c18830621e98830e20488872620c18030620c18830620c98862220c18830620c2a202000000000000000800430028c00a3002ac05ab012a4012b004ac20ab
002ac0429000ac21ab007ac00a30008c00a08202000000000000000800030020c00830020c00e30020405a30068400800020c00810020405e30068c00830020c0082200a000000000000000a88030801c28071801c20070001460070801620050021c28050801620070001c20070801c2006a20200000000000000
0000019000640019802647099002401099) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1fe0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0039804e2010a002000000000000000a8802b02cac0b2102cac7b2802cac0b2b0aca40b2982c8c2b2102cac1b2a02cac0b2b02cac0b2a202000000000000000a880020140805000140875021140a450209408850201400e500014080502814080502014080520000000000000000000200008104
204128104200128004204108044a04128104280128104204108104204108104200102002000000000000000a88028800a22028080a20028a80802028aa0a02028880a22028880a00028880a22028880a2202a202000000000000000000018884622118880624188880420398806622018880622018a80620198806
6221188846221080020000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2000) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (fbf27edc9fb72fedc9fb727ffc9fbf27edc9fb72fedc00000000000000000000000027e90992426492fffcbe492f97cbe5f0992426492f924264909ffc265f0992426492f92400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000bfbf2fffcbff727edc9ff727edc9fb727fdc9fb727edc9fb727edcbff72fffcbfbf27ffc00000000000000000000000094b525ad496b4242d092b4242d090b424ad090b4242d090b4242d096b425ad494b524ad40000000000000000000088038804e20138804e2003a804e201
38804ee013a000e20138804e61138804e2) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2020) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000030c2000c000040408004000c000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000009fb727edc9fb12fffcbfb1218fcbe3f21ec486312f8c4863121ffc9fbf27edc9e3727edc000000000000000000
0000009ff727edc9fb72fffcbfb72fefcb) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2040) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2060) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2080) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (20a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (20c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (20e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2100) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2120) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2140) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2160) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2180) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (21a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000030c2000c000020408004000c00000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (21c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (21e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2200) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2220) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2240) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2260) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2280) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (22a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (22c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (22e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2300) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2320) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000030c2000c000060408004000c00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2340) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2360) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2380) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (23a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (23c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (23e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2400) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2420) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2440) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2460) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2480) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (24a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (24c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000c2000c000010408004000c000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (24e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2500) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2520) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2540) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2560) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2580) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (25a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (25c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (25e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2600) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2620) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2640) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff00000000000000000000000000000000da8b00008000000c
020000008005000ca00000008001000c0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000003002000cc00000008001000c89cd00008000000c000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2660) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0001) TDO (0000) MASK (0000) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'serase' instruction. 
SIR 8 TDI (0a) ;
RUNTEST 37000 TCK;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) SMASK (ffffffff) TDO (f5034093) MASK (0ffeffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) TDO (00) MASK (00) ;
SDR 16 TDI (4000) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'usercode' instruction. 
SIR 8 TDI (fd) TDO (00) ;
SDR 32 TDI (12340002) SMASK (ffffffff) TDO (00000000) MASK (00000000) ;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) TDO (00) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'usercode' instruction. 
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) TDO (f5034093) MASK (0ffeffff) ;
SIR 8 TDI (e6) TDO (00) ;
RUNTEST 50 TCK;
SDR 32 TDI (00000000) TDO (12340002) MASK (ffffffff) ;
//Loading device with 'conld' instruction.
SIR 8 TDI (f0) ;
RUNTEST 110000 TCK;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) TDO (f5034093) MASK (0ffeffff) ;
//Loading device with 'ispen' instruction.
SIR 8 TDI (e8) ;
SDR 6 TDI (34) SMASK (3f) ;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) SMASK (ffffffff) TDO (f5034093) MASK (0ffeffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) TDO (00) ;
SDR 16 TDI (4000) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fdata3' instruction. 
SIR 8 TDI (f3) TDO (00) ;
SDR 6 TDI (3d) SMASK (3f) TDO (00) MASK (00) ;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) TDO (00) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fvfy3' instruction. 
SIR 8 TDI (e2) TDO (00) ;
RUNTEST 1 TCK;
RUNTEST 50 TCK;
SDR 6 TDI (3d) TDO (3d) ;
//Loading device with 'conld' instruction.
SIR 8 TDI (f0) ;
RUNTEST 110000 TCK;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) SMASK (ffffffff) TDO (f5034093) MASK (0ffeffff) ;
//Loading device with 'ispen' instruction.
SIR 8 TDI (e8) ;
SDR 6 TDI (34) SMASK (3f) ;
//Loading device with 'conld' instruction.
SIR 8 TDI (f0) ;
RUNTEST 110000 TCK;
//Loading device with 'bypass' instruction.
SIR 8 TDI (ff) ;
TIR 0 ;
HIR 0 ;
HDR 0 ;
TDR 0 ;
TIR 0 ;
HIR 0 ;
TDR 0 ;
HDR 0 ;
SIR 8 TDI (ff) ;
SDR 1 TDI (00) SMASK (01) ;
