// Created using Xilinx iMPACT Software [ISE Foundation - 6.3i]
TRST OFF;
ENDIR IDLE;
ENDDR IDLE;
STATE RESET IDLE;
TIR 0 ;
HIR 0 ;
TDR 0 ;
HDR 0 ;
// Validating chain...
TIR 0 ;
HIR 0 ;
TDR 0 ;
HDR 0 ;
SIR 8 TDI (ff) SMASK (ff) TDO (01) MASK (03) ;
TIR 0 ;
HIR 0 ;
HDR 0 ;
TDR 0 ;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) SMASK (ffffffff) TDO (f5034093) MASK (0ffeffff) ;
//Loading device with 'conld' instruction.
SIR 8 TDI (f0) ;
RUNTEST 110000 TCK;
//Check for Read/Write Protect.
SIR 8 TDI (ff) TDO (01) MASK (ff) ;
//Loading device with 'bypass' instruction.
SIR 8 TDI (ff) ;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) TDO (f5034093) ;
//Loading device with 'ispen' instruction.
SIR 8 TDI (e8) ;
SDR 6 TDI (34) SMASK (3f) ;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) SMASK (ffffffff) TDO (f5034093) MASK (0ffeffff) ;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) TDO (f5034093) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0001) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'ferase' instruction. 
SIR 8 TDI (ec) ;
RUNTEST 1 TCK;
RUNTEST 15000000 TCK;
//Loading device with 'conld' instruction.
SIR 8 TDI (f0) ;
RUNTEST 110000 TCK;
STATE RESET;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) SMASK (ffffffff) TDO (f5034093) MASK (0ffeffff) ;
//Loading device with 'ispen' instruction.
SIR 8 TDI (e8) ;
SDR 6 TDI (34) SMASK (3f) ;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000000000000000000c4000000000000000054fba80000000000000000000000000000000000000000000000000000000000000000000000000000000000000000d53ff0000000000000160400000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000c480000000000000001200400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000c480070da000a0002000c800000008001000c000000008004000c900000008001000c638000008003000c6dfc01008004800cb0000000800680
0ce00000008001000c66aa9955ffffffff) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0000) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (b81400050001400050001400050001400050001400050001c00050001400050001c000500014000500014000500048ff0000000000000420000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000004800000000000000054ffc000000
0000000000000000000000000000000000000000000000000000000000000000000000000000000000015bff0000000000000d2ff80000000000000000000000000000000000000000000000000000000000000000000000000000000000000000015bff0000000000000140028000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0020) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (071740c7480d90046c41df00568411b00c4d81df0037a00200000000000006200c400c504044015d00454089d02374025d0037400dd0037441950017400d508e5403952045600110464403d9003580030000000000000e8040600c990204005d80004008d08234860d1033480c52030400050083
400c908034848d10434240180304204d0033a0100000000000000c2006c00d500044005d00054019d08274025d0877401dd0074620950097421df804540091084d40811004c4008b003708010000000000000e000cc01db1004c014f8044c018f086fc0c1f0077cc1df0074500bf100fea1fb004ec08bb400684c3
b4006c00bf003fa8030000000000000163) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0040) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000a001f400c100d04070d0040502c50023440090032400c90031400811222600cd004041398000069a5d00014009d0036a80700000000000002004f413d10016c009d0064491810037400dd0037400dd0035c00110027400d800e50a19b00145039d0035400d1003ca01300000000
000004200fc00db23a5ce85f0024c04970237c00df0037e00df0837c02130087c00df0205c805b1012c009f00b5c02570035000300000000000006001fd10fb0117d007f000fc00be006fc00bf003fc20ff003cc0027460bc00ff242ec009b0006c091f000bd80fb003d80070000000000000e2008400db0080c01
4d0144c019f2027c409f0037800df9034c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0060) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (ad083b400ed203ac00e1000b400ed002bc00a14031400210800400ab41b980130000000000000e0057c00d30014c00130047a00df0034c001b0037c00df0036c00db4004c00df1025c80d70cb6c01530085c00d30037a01500000000000006600bc00d71027c007f021f488df1037c00ff023fc0
8df0237cc0ff4a3fc40db002f6809f000de481f02afc807f4235b80200000000000000404bc0dc34371e014f2540c85878027c010b9373405cf1971d251308e7c81cf0120c518b10404014f0851c01470074101200000000000002001b401e1026a4053d005840df1907b405ed017b405ed0179419a1007b441e98
048401a90b484012d0849401a140788006) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0080) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (020d0087802308100000000000000c004bc001f0003c021f0007c00170007c021f0007c001f0007c001f5107c001f2407c021f0100c30110007d001f0007001200000000000006205fc0053401cd0173009ec815f201cc017b00174005f00168047b001dc005f881e40277001c4807fc19d05071
001588170000000000000c20cb400d102714109101b1401c90270406dd0033400cd0032413c100f7000cd00b14635100315028d8180401410033281200000000000004000f401e10078411712048483f5007841069007b401ed007a1216908d9441e5207a431450058401cd0059401610070000300000000000006
204f400e1003140021001d500e18038400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (00a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0005c00170800c041f00076001f2004c44530113c201340048041f0107e24551104c040fa106a01c0000000000000080404008545235008d00214009500205348d002340088002059489052340081002645491352361485252041481052020100000000000000200604029502244029d20e54909
020204029d00274009d10244009101274009108244009d20274049540244089d4024a018000000000000080004502910466c009d00e44808501a44009d00274009900244a1934027400910262c0e9120274019b002540091202620010000000000000c2040c04910064c049f2024100970024c059f1027e009f002
4c05830067c00930864c51980027c01938) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (00c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (54009001244029d0026440910025a8180000000000000e80404148123204008d95204009190274828d00214008d00204008900a34408d00234028588a15008d0023414810023a0100000000000000c20705051b4546c011d01454401101474071d00074001d100548f1141c74801d20044021b00
1400a1700845031183c7081c0000000000000e0060c20b30168808af002c800b300afe87bf00274009f1025d07a201efc009f003ad01b7017cc05bf0464c11b34367a0180000000000000e6067c349b052cc14af252ec80ad052fc14ac0027c809f0027c14a7052fc809f282fc54ff002fc14b9002fc14fe152798
190000000000000ac070c00170104c001f) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (00e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (5340177089cc027100df4207500184007d00174005d0017c0271099f40051005c4017d20574037120144a075001ca014000000000000042053c001b1006c00132285c40130a06c041f0007e001f0005404130087c00134084c821f0207c04170084c801b00050814000000000000060057c209f0
023c109f0027c019f6127c009f0827c009f3027e89870527c409f0026c298f1063c808700e5c009f002580150000000000000e2014c209104a448a8f0124c009300674009d0027c209f0024c069b01678009f0027c019500254029d01a7c0b810023a8050000000000000620604008180245029d80254049120274
249d00274009d00244009960230009d046) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0100) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (81d30b77481ff007cc29b90078c09bf007dc41f3007fa000000000000000066043c001f1027c00970027c00d71dadc005f0837c80df0035c00df1837c00d30017c009f0837c001f0837cc4df4035b810000000000000004057c01230078c01eb406dc016b406cc016d207b681ef0079801e3107f
c41ef0078c21ef087b401e71070c89eb00781015000000000000020017400a50028410b9007b400ed0028401cd003b400ed003b002e1403a440ed10dc410cd083b600610078420c1023080050000000000000a0053408c18130501c90471410d9812052acd0033400cd0031400c120b3400cd0930105cd0033408c
50030500c90032a0140000000000000200) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0120) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000062054520d32075402df20b5c00d90404c039f0037420dd0034c01d91277620d90020c039b10b54800d10f5487d0003d88150000000000000c20104000100e54808d0400020c900614118d0031400c520325398d0081000c580304051989b15400d0030400d10033280400000000
0000040000400210439400ad0109604f9022c410b5093b404ed0838400e9031b488e90238414a902394142c1439400e101390000000000000000062056c01b101e8500ad0168401eb0969404ed8879c05ef007ac09850467c09c720385410120384051c0138408c1007188150000000000000e0000c01f3027cc01
bf0065c09f3006cc01ef8277c01ff007cc) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0140) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (090833420cd04314a4018483004c150204040582204021d20b0408c100302010000000000000020007402951074501dd0474401dd20674081d0035400dd003548a5d01b7400d10066441950025401181037440d01834a0010000000000000802074005140444078d00644018d21f74c55d203740
0dd2035c00854086400d10854553110a344511f003440995003620810000000000000c2203c05f2102cc10bf083cc807f002fc007b083fce0ff003d40097002fc80f3243dc001d1079c003f003dc01b3003b08800000000000000c0007c025f01b6823df2067c489f089fc029f0037c80df8037c22d74013c60df0
017c82970236c001d0437c44df20370001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0160) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000520410037a0100000000000000c60074805d20c7c891700f74031d00c44095502d4c0b9b02544011b0045c01dd0106401510044440dd0a4448043403f00010000000000000e200fc015f1500c043f200bc001f0504c0035110fc041b0111c0133000ec81dd004ec0143804cc01df080dc017b
403788030000000000000e4017c101b0623c242f052fc2c8f0023c043f073fc1cdf0135c18bf310ec02df803e4881b502fe0817003fc24bf41b3b0050000000000000ac003c00970024c089f05b4d045f812fc821b11b7c06df1335c409f4187c8ad31034c0e1710a54021f88b7c02a313b6b00000000000000000
8043410052130400cd012040d9d8423422) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0180) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (04a4d12934304c02c382a4d08d38015c0ad10013c00d31004c001b00a4c00d34084c00570035000300000000000006001fc007f040fc041f001fc415f0877c00df020ec823f023dc403f0037c20ff10af841ff040fc00ff0006c007f403580070000000000000e000bc005f0004c025d04c74039
f0144d06978041c00030093c09120004c00cf0486c81510844500df00c4c03530037a00200000000000006000f4005d0017410d521274081c02044a01500b5400d90096402d841a5400dd002648411a064400dd0844403410035a0030000000000000e80434004d80104000d00834020d000040005002160041001
3400d10000400cd0403400011820400cd2) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (01a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (fc0c57022bc08de003fc401f02b5b802000000000000004048c015b4172900834051c89471070d00090143021090173c0dcfa273c11c30034e49430720505d30181c00470170001200000000000002001840560006a011290979629a52048401ed4152005a94d7d40bed405b405e9004a4006108
4848de104484016101f880060000000000000a009c4044900224208102c14424580b04000901c3484090473400cd0003402c1c4004104100c0480d10041480450072a80700000000000002004c4025301d4c414300344079100c4400d10024403d12075c02c10037408d50466c459100e0400d112e4500510438a0
1300000000000004000cc00530014c8653) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (01c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (4b40041003040dc900f2511cd01b3609c9007240fc10032420cd0433440c103b7492c50470400c92071013d10037281200000000000004000f401610870401e9884a403e1047b421e98073481c1004e600ed047b401e5006e6217d0078401e1005b511e14379000300000000000006204fc00610
028400c10032c40c5003b400e3403a400610038420ed203bc80eb0029400ef2038c80fb080850021113188130000000000000e0057c00530066c80d74044c00d30033c00130035c80530014000cf2027c00df0024c005f0006c41d30043420532037a01500000000000006600bc087f027dc08b7203ec207b003fc
0033021dc00a7203f800c32037c00d7003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (01e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (009500274809104244429920376009d1026500910024a01800000000000008000440f9d0064c099d02e44039702e44009f00a04028104214038b08234129b00e70829d0227400990ca54809104e620010000000000000c20404019f00a6c019f0024c03930066c009b1065c239b2926442970027
c03934126d429b1025c009f0026d8093016708100000000000000c0049c021f000fc02170285c22174007c10074485c021f4045e001f0005c021f0005c801f0087d001f00864801f4087001200000000000006205fc00738014d804baa56e03432053ca25b21554035304d64007d085fc005500de4026d11dc4005
313dfc0173001da8170000000000000c20) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0200) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000e2060c00b3086cc01b3016cc15b3016fc019b086ad11b60c68c00bb006f600b3102ce00b3202ec029f002a8028701efa8180000000000000e6066c14bf0027d009f0827c20971837c409f80278809f002bc00bf402fc809f452bc00af003fc549b082fd14bf2527b01900000000
00000ac071d001f011ce841f0104c44171114c841b01154841b0107c40150107c00110006c001b0017c001d0106c00014106b01c0000000000000080414008d0528014ad0528554e52528514ad8528414e105256019105634c08100206408d802340089052140081052020100000000000000200614408d203c442
bd0c2c400f5202c600b9a22d500b940254) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0220) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (9f0025e48874065c90930127c209f0225c049f0427d409f0027c209b002580150000000000000e0014d0083406040a8b0464c069340674069b0120c05952224c809f01274009301e64409900a48008f0026c72950027a00500000000000006006040091007444099006540895002742095182440
0918026401954025400d50837480910864400950e24608850025a8180000000000000e80406109100a05028940206208102234008902204808500224018d00234008104274009950204848d1822440850123a0100000000000000c4070405110004400510a05400150007408150004400130006480111205e00140
145400130804c051700044451b03c7081c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0240) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (078c05e300581015000000000000022016402e500934002c108a40021208b400e92088400290038401214c30641e140b94022d002b400e900d8408f0401080050000000000000a0052401c120506000d0882402098143400c1013048e850231622c501b3405c140f30000d20b2400c90970420c1
0072a01400000000000000805040075081dc097d001c4037100df4005b005c7017b201c4446240184007100194006d001b40071881c40051001ca014000000000000040050c00130904c081f0004c081b0083c00190084c421f0101c201f2085c081301074041f0006c40131006c00130201001400000000000004
0057c009f0027c40970423c118f2127c83) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0260) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (102b44625200b400e50808404a903394886d291b400e1002c406a901ab448e98809410e901010000000000000000060056c05af04584492100434472b0188401e53340405a7005848d090170c05e10128c8d28014b42def044ac05e1015980150000000000000e0000c418f2246c05130047c011
f0049041d70341c4990237580d6f117ec09fb106de89a30273c01f30065c0bfb027fb800000000000000062041c005b0004d009f1005c009f0023c00de20078009f1037c000f0035c00cf0007c400f0027420d71015d06df4005b010000000000000000056d017340584010e104ad810b104bc41e3084850187007
9c0067407bc01e1006fc21ad106ac87e94) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0280) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (2c00110043400dd09c5400d5084620810000000000000c2200c01b3141e001110047c2573844fc50d3014ce00b7203dc407f047fc09f3027dc03b1200fa00ff8855c00f8000f00800000000000000c0007c005f0015d06176003c2a1f60c5c40df0083c04178137c021b2035c40d74025c001720
27c00df0087cc0da10070001000000000000062054500dd08944201b0087c03172043c05d70405c829921f1c000f0c37c00d30035da00204e7080f30055401fb0025a0150000000000000c2010400050000420090b03401090002402c50000702850830400090052400c003c0540090043000c904c0401d5000628
040000000000000420000443d012841029) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (02a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (17c063f050ec403b010fc063f051fc02fb050fd0caf0029c1217010589ccb000bc101b080fc82df080fc08df07078805000000000000088000c28932486c54170587c24151007400d1448648c9585b5c045f0706402d32015480912107402dd0105404e70186a000000000000000000042400490
0034040d0202406054001440c50000004c182104240d0120444041002450050406602c98d00404c50100201000000000000002000440ac10047500150417600150207440d120074019500754035d0226480d1a015400d10c67400dd0105420d50064a001000000000000080206c001b0052c0c4b02474001500c7c
80d104c6c018b1074c811f0075c02d1004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (02c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (005710e5c030b1087d03032044c020144c3c531f0041210000000000000006000f400d52064640dd0035400d10076400d10037400d50037401950a154111110b5451190864408d10057401554045a0030000000000000c8043400cd0020608c50031410c10032402c10037400c10033401054201
400110007602010000400c100174000d1007a0100000000000000c2007401d7a000403d90074404d10074c03d10077401d100764019500544011120454031b00c4400111047441110047080100000000000006a00fc01fd806cd80ff0074d01f3002ec00e30073801fb007fc00030105c813f104fc4037050cc693
b004f82133004fa8030000000000000ea0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (02e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000a001f400c10020409c18030640c100a2402c514f0483cd0031400498b03481044802432010043401cd00434110d0802a80700000000000002204f400d30024401e10034000d18235411fb89f5401dd00314005b405640b150130404911067401dd0297401dc0284221300000000
000004000fc00d32066c00d30034c00d30036c10d78834c10df0035c00530083c2a170c07c02130027c0adf0097c001f1005000300000000000006001fc00ff002f800db043ed20ff0015c00ff603fc80fb403ec00ff0036c403b017ec403f2003d0137000fc003b000d00870000000000000e0003c00dd8164400
d70035400c34052c80c30833cc0db0037c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0300) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (eb103ac00ed003ac0060002b4006340384806d0018400e0003840021000980130000000000000e2054c21cb0033c00df0034c00d74004e00f30035c01cf0034c00472026c801b0036c001f0004900d30000d00130047a81500000000000006400bc00d74125c10df0033e08df002f400df2037c0
8cf0037c087b402ec08790239c046a0027c8cff0217c087f122db00200000000000000404bc01c31160c08c30070c0dd14062c04c50070c01cf0071c214b2243c85050232c05034403c0dcd0013e580f01e0101200000000000002001b401e900e8421e11578404e10379401e10079411ec01794017d224a405655
24840121004b405ed145b4092d03488206) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0320) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0e6c259f016700100000000000000c004bc001f0207e001f2086480170407d021f80068021f0006c00132087c80170005c001f3407ca21a0087c001f400700120000000000000600dcd005b005fc005f0014c005f005c4005100104805d0016c127700db40073005ad027d085c4007f011cc1367
011da0170000000000000c0048400c104f74a0cd0031400c100a0420c90032440cd00335274901f34124910f0405cd00f0400d5c4e0410c10033281200000000000004000c401e9007f605ed2878441fd20e8601e10878441ed007a48175a0d3481a1247e4038d0478401fc00584a1f5206d000300000000000002
604c400e1003b401ed0038400f50008426) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0340) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (4006c001b0106c041300074001f0005c04130117c001b4006d041f8107c80114016c001f0006181c000000000000008043400850023514818023500814531414850023400c98821614990520400d18020494cd05204808120244208d102028100000000000000200634009505256089100264009
980264909100274209d00254009100374009981a64009d8027422d120264109d00a42018000000000000080007400951066c008103204808500614029520274019920254008f20a54438100e44828d20244029180204439d002620010000000000000c0043c00920064400930864c009b0266c008311278059f002
5c009300e5e029b0466c009f0127c4293a) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0360) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (468a9d01a54809d0224440996425a8180000000000000e80434008140234008d282040485a0a04828520206009d0022402958020400d100216808d10234048c0020501910023a0100000000000000c20734001301474201f8004c01110006c001b00044001d0006c025f20854001500044001d10
07c811d0004400110007081c0000000000000e2063c20b380afc00bf002cc089f0068d01b70028d20bf202ec0585046cc00a3802d400ad102fc02bf082ec20bb002f80180000000000000e6067c009f052c8809f002cc149f003be008f902be00bf8027c00bf002fe40bd102b440bf082cc14af202fc80af202b28
190000000000000ec073c40170005c0413) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0380) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (5340057215f4117d06dc40071409d4007f809ac017d00154004101184427d901ac0075011c485791a1f4827d00582004000000000000040053c00132087c001f0006c001b0484030128004c841f2005c221f2185c021d2186d00172004c001f0007c601a0e850814000000000000040057c00970
027c009f0025d809f2027c009f2027c009f0027d009f0027c009f4267c019f0027c049f0825c419702650015000000000000040017c00910427c009d1024c009700604008500244008f0026c009423a4c448120254008f00a74049d0024c4883006528050000000000000620634009130230c09500240009100764
009900340009d00264809480254009500a) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (03a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0dd36241c0907124ec81d3006fc0d9f027f8215f0077a802000000000000066043c00d72013e00df0826c00d70037c204f2016c004f0037c20d30007c801f00164009a0023c005b0027c005f0035b010000000000000004053c01e3006bc01ef085bc83f30078c0161004bc016f2079c00e70041
c41ad0048401e34078c217f206bc016f08781014000000000000020013480ec003f400ed0029400e1003940065000b4026d0039401f500185207d0008400a50878401ed002b4106d003882040000000000000a0053400c100334008d08d3640d102d0400c104834034d0031500c508014060d2280404c100305008
c00b3404cd0852a1140000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (03c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000062053c00db0086d00d90017e20fd0435400510004d004b4036c02d301c54891320c048483e4e5c000f00a70135d0134a0140000000000000c201b400c10184400c10023400d18070000490010400490030600cd40014020184006038100a34004d01234060d0033200600000000
0000040803488e9022e404e9021f404ed003940461090840479023a708f1800940421862c404e100296002d8d2b4006d01390200000000000000062057c0dc10160c05e341eb42dc310304036b0148507010170405ef006bc0901420ad05810b6b405cd016b44d6d037188150000000000000e000bc09fa007cd81
b3026fc01f7007d8497b004ed0173027ac) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (03e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01c1204064980334d0c144024840900004828c00204401900034200d002028100000000000000a0007400d104054009d0224400d900774015941064015d1034400d10047482150c444019d00244081d00674231d0064a801000000000000080207400d10094440dd00d5400d30077c4305000140
1d91037400db04474801f00c54139d08654071d99664215d01e622830000000000000c2203c40f3220e808ee001cc00f30830c005b000ec007f003ec40e3040fc2437000cc10bf016cd007f802f4007f102f00800000000000000c0005c00df08b5e00df0017c00df0037c021f0004c40570037c10df2003c011b2
086c801f0127c021f00a7c425f00370001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0400) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (8044401d0003a0100000000000000c0007401dd13244045d0104484152137484dd0134510910127401d50047401dd2074c161548044015100044011d080708010000000000000e000fc01ff020cd497f020cc0833027fc80fb0258c01a300efc21db0007c01dc007ec84138048cc05b004cc011f
08478a030000000000000e6017c48df0602c02cf8113c00d7002fc001f00a3c004f0f35c00ee010fc023f000b54caf08a3c1c3e00a6c023f00bf2805000000000000084003c06d32007c00df0594c46db40a6c045b8286c925f00b4c08d10387448170004c029f2924c041d0927c841d03b6300000000000000000
0043402c14121704cd81a1416c988b2410) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0420) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00b7c41d340b4c88d38214c02df0027c28d70027c80df0037c12132017c805bc6044405f2805000300000000000006001fc00ff0407c007f0217c047f003fc10df101ec40bf603fc80ff0127c00ff283cc003f04bfc107f294fc033e000d80070000000000000e200bc00df8084c404f0094c45d
33077c60db0054c65c30067c00df0043c00dd0036c23110004d031b0080d011f00c7a00200000000000006200f400dd80b44005d8004540052463600dd1054401910067400d50007440dd00354111540244115120044025d0445a8030000000000000ea043400cd00104445d2000608010033610c9211048491002
7440c50003400cd0033448010000400598) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0440) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (d0087f003fc8877102f8006f0a2db00200000000000000004bc05cb0452c0d4b02e3c09430034c01c1415040d8d0263c09c71763c8dcf2033c89030173c25410144c0d0d0360101200000000000002001b405e40068501791a6b60fa1107b605e1007d4093d036b405e9437b401ed207a4412501
5b41561836942d6d014880060000000000000a001f400c900c24004981a3640010030400c101504048d00a3405c12043400cd0033029110007602412040441090182a00700000000000002004f400d710e4c0c5b09b74005113f5400f180554009d0343400da0037400d60037c009500374024100c54104d0944a0
1300000000000004200fc00d34024c8053) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0460) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (4b400c100234004101f0430dd0070420c92410413810003400c14033400c90033401c110f1403c98076403cd1873281200000000000004000f401e18049401610069403cd80f8485e508cc503b5006b401e9806a401ed007b40161047f6114d08ca4c16d0479080300000000000006004f400e10
02f40061000c400ad103ac00fb0018440a1002b400e31033440e9003b600a1003840063202c4406d081980130000000000000e0057c00d34045c80520005c00bf0034c08f700148008f3067c00d30006c00df0837c00110022c405710048015f0007a01500000000000006200bc08fb003fc006f0837c00ff001dc
00ff1117820bf002fc00db4037c80f7003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0480) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (249100374209d30276089528304009901376009d802480180000000000000800074009d012440a8b00e44809144a44079100e68018d80274039540274009d0027e279b04e6c009120274289d022600010000000000000c2043c009b0024c019300e4c82930064c01931024c849c08a7c00932165
e00970027800970a24c008b0067c009f006708100000000000000c004bc001f0187c001f4287c021f2187d02172007c00170307c021f04034001b0007c031f4186492172005c481f0006001200000000000006205fc0053011dc0073109dc037f001c4005600dcc8077001fc005b015e4005d0017c1173005fc017
f085ed0b7f001da8170000000000000c20) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (04a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000e0063c009341e4c029f0167c079fa0a4c11930a26c089b022dc00b3016fc809f2027c00bb40ace05bf802cc20ae022f88180000000000000e60e7c009f052fc54bf452ec14bf152ec149f052bc14bf052fc409f582fc009f0027c14bf252e800bf452fc00af252f881900000000
00000a8073c001b0104c40130115c04531005d04130004c001d0003c00130107c001f0007404174004c845b4007c001f0006a01c0000000000000080434008c05204009805215348100214148148624809d1023400c565334408d00214948800224d48100334418d00602010000000000000020063400990024702
9110214009922214088100600829d00a76) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (04c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (9f0227c009f00a6c00970067c009f0027c00834067c058f0167d019f026580150000000000000e2007c009380e44009f2227c009d86a440093c0e6c428b2161c00940227c009f0027c049f00a45039d2024c0a8f0067800500000000000006206340091002c480ad002f400bd802d400a120a940
0b100354009c40a64009d00244489902a04709d28244509d0035a0180000000000000e8043400818128404ad90ab406ad0128610a100284a0b900254008500234008d00224008d00206028d05200809d9023a0100000000000000820734001103dc5011d05d74211c00454051111454055101404201f0a864001d0
0044801101444001d00444001d0157081c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (04e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (078d012b404c1015000000000000020017400e120bc500e920d8421ed0098420e50018700e1203b600e1002b400ed003944085001a410c1047c450a980d880050000000000000a0053620c90874400c10870740cd1030400c94030622c1403340ec500a3020cd0030401c11231401c18070424c8
2072a01400000000000002005340053101445151001443b5d001450053201440151001748261009b0005d0015c1274005ec0071001c40370029ca814000000000000042053c0013008dc10131404ca01a0006c84130086c18130087c201b0607c001e0006c06130047c04170005c22130084001400000000000006
0057c009f0227c009f0067c049f2467c40) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0500) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (202c440f9140f400a50639400a1042b42421012b404ed003a40029480840068402860421810d0000000000000000062057405c100604048b0152c49cb007b408c11156c014b0173c07ef016b405e7003840d334332c21a0812450821224988150000000000000e0003c01d30064c01f33268c05c
30077c01f7027dd01530273c49fb026bc49df207dc41da827cc01cb086cc0d330257a000000000000000064043c00df0013860570007c801f0015c001b0025e001e2007c00d54023c00df00364001f1917c40d31013c60172005b010000000000000004057c01eb4058c0173407cc01ff0078c0139087cc01b3006
bc01ef006bc01ed007890163445dc81e34) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0520) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (64051100934011100454831500c620810000000000000c2203c20f30010c80b3115848231022cc2863009ec03f3107fc00b5002bc40ff003fc0033001fc80bf102ed1437000f08800000000000000c0007c00df0037f025f20b7e20db0187800970005c80df0005e005f00a7c00dd0035c021710
17c02170037c831f00970001000000000000062057c00d300b44009304746081b00e7c00d720e5219d300d3e009304a7800dd1037c0e1b625441a9b1124c02010455a8150000000000000c2013400c18100400590042422cc00974000104e20211904434800d41e3440c5083250300024240001044400001204628
04000000000000040003444e1214840061) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0540) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (17c46ff100fc143f0206c023b120bc043f4006c103f100fc061b0107c14ff003ec103f041fc0c3b500fc002f0009b0050000000000000ac003c28d32784d020342a5c4e170024c2253ab96c408347b7c82130797c42df0037800136019e061b20a6c4217a4863000000000000000008043404c50
120400813101520054101402814404010050106406410123410cd00324100100174260540a04020503002010000000000000020007400d100244029120a54100500b4402518027480110215401910467400dc08356011190d5483990066490110044a001000000000000080a07400d5001440b1100944001120854
00110180400550007403510067440dd203) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0560) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (20de0036c80cd0034c00db0335c050300c4c13870035218000000000000006000f420d1403042645ac14440d90464600dd0037400d90037000dd8036680dd0036480d16014000d10044401d1003520030000000000000e8053440c10430610c13034400c900254048d0031400c50031400c58032
400c90832480c91d01510110000420d5203100100000000000000c0007401d10134404d5003440cd94074440dd8077401dd0077441dd0034401dd0076401d5001440451008440091007710010000000000000e200fc81f3207cc4133224cc08f3007fc83af007dc01ff007de01df0074c01df007cc00db004cc011
30c0cc81972077a8430000000000000e60) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0580) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00000000000000200f400cd0033400cd0037420c580224009d0032400cd0033400cd8032405c52473080c140174024100054808502f0202300000000000000004f400d70035c00d50037440f54025400dd0035c00dd0036400d60475481d100f4431e10017403d18464400dd00b0a01700000000
000004000fc00df1037cc0d308a7c00d700a4c009f0037c00df0037c80df2034c20d71235d10d30037c1113c085c1a9700350807000000000000040217c00ff003fd21bf0137d20f7002dc01ff283fc00ff003fc00ff203dc80ff003cda0d7407fc05ff5007c00bf043d0881000000000000040003c00d11034cc0
d300b4c40c30061c099d0035c00df0835c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (05a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (a13039c00ed003b400eb203d400e3883a406e1003f480eb002c4a0ba083900130000000000000e2043c00df0034c00530017c00fb0027c00930073c00df0035c00db1076c41cf0836c00d30037c20d22005c20931871281000000000000004400bc00f7203fc65f70237c08ff2009c00bf0237c0
8ff003fc00df0235c00ef1039c08ff001fc00ff001f808ff023d380200000000000000604bc0dcf1073c098f0233c89c72022c818d2173405cf0073c01cf0072c21c60233441c30047c0dc100c1c05d70070003200000000000000011b001ed0179401ed026f601e5026f405bc2079405ed007a401e5027b455e10
07a601e1035b601610048405ad08780202) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (05c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (964c009f0125001000000000000004005bc001f0007c001f2007c801b4407c001f0007c001f0007c801f0007c021300048001f4207c021f2085c901f0005001200000000000004204fc005f0014c05514397c0053001d800510017c005f0015c20532016c805d2017c405102dfc8073045ed1063
0015a0030000000000000c004b400cd003548530180f400c90023400810030400cd0033400c90031400c52033600c118b3426d911364004900312012000000000000040003601ed0878601e1807b605e100ed401a1007b401ed0079401e10078601ed007b405e1007b621e1805a401e10079000000000000000006
405f400ed0039400e1103b402eb002b400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (05e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000c44130807c801f0007c001f0007c00170007c00110004c24170004d00110105c001d0016001e000000000000008043400810020400a100285148100274008500234008d2023400858023400890030614c900246408105206809d00202010000000000000000063400912024480b1002c4009
120274009d00274009d00274009111274209132265409508244009108254009d0024001c0000000000000000074009100244009500244409140234209710274009d00274009700274119b80204029b00204069144644899d00e42805000000000000042043c00930024c00930024c20830027c009f0027c809f202
7c00970067c08938024c03800024c08938) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0600) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (54009d982540091802644291002520180000000000000480494008904234108940204148100245049d00234008d10234808190236008d20226028d252340085002040081002522120000000000000c00634001101474051b00546031500044011f00074001f00074001700474601d2005c021d00
45c201b4056c11110007101c00000000000006a063c009300274009300a4d5593202cc028f002fc009f2027c0093022bc80bf002f001bf2027c00b7022cc00b3402f10180000000000000e60f7c009f0527c349f5527d349f102bc14b700274409f0027c00952527c209f0027c008ba52fc14bf352fd14bf002f30
19000000000000006073c00134004d0023) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0620) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (03400510014c005110174007b00145005d0817c205d00174005b001dc037d0b5ec2b7d00174017da15c69271015d2000000000000000042143c00130004c021b4087c00132084c001f0007c00150007c001f0207c4c1f3005800160005c241e1004c80172805005400000000000004005fc00970
027c84972027c009f20a7c209f2027c009f0027c20970427c409f0827c009f0025c009f08a7c089f40250013000000000000042015c009b4027c039ba0a44008301e0c008d0027c009d0027c009100274009f1027ca09d03a7c0495002440393002121050000000000000420634009900234909981204009500244
a09500274209508274009530374009d802) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0640) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (09fb087ec818f027fe41d3067b0815b007fc013300453002000000000000066043c00df003fc26f7043fe28df0033c08df0837400df0037c00db0035c005f2026e401f003fc401f0037d209700012054000000000000006053c01e312fccc1fb21ffc01e10078c01ef007b001ef807bc01e5007b
e012f007b421ef0179c01ed10784013700580010000000000000020013680e11138545e9093b480e10038400f91039040ed003a400e0003b6002d9038411cd203b450ad1038400a9002800000000000000000a0043600c11030400c10833440c10030400cd0033400cd0033400c50077400058073401cd8031402c
d003440715004020100000000000000004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0660) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000060053c00dd003fc01fc01bec00f70234c01f15037400dd0035c40d30036c001d0037400d023bdc869020e7c03510001201000000000000004000b400c50031401cd0430400dd0033401c50031400cd0033440cc00334000d18034200140774031908e3607010001280200000000
0000040003404ed003b610ed013a444e5903c400e1013b400ed0139404e1003a4842d001b600e9023d40021003b04021000d0004000000000000004057005c70071c04cd0378d25cf007ac00db4173c65cd0173405ec02794052d023b409e3a23340d2b0021c54214369009500000000000004201bc29df0a77c13
ff087cd01d54a74c81f3027bc09de1077c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0680) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (d90331646c50433412c908034040d00004040500316040d00234004101a020100000000000000a8007400dd0037400dd0034400d10036400dd0037400dd0037400dd00574011d00244301180344811d80e74415d0044200100000000000008020f400d70036400dd0035420d34030500cd0035c0
0d70037440dd00f7c531d1607c021580354811900d741351004420830000000000000c2203c20ff203f400f7003cc00f3003ec00ff003fc00ff003fc00ff003fc003f007cc03e3803cc10bf0417c0077000d00800000000000000c2017c00df003fc04ff003fc00df0036c08db0037c00df0037c00d700b5c001f0
097880d70837c009f12a5c021f00250001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (06a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (20300005200120130000000000000c6117401d70075401110054501d11055441d10045400dd2066414dd2077401d91506401110526c041d00c720011004701030000000000000e810fc01ff007cc20bb0044c00f7405ec01bb0040c01370069c01df0077c01f3004fc013b002cc013f010fc8137
184f30030000000000000c4017c14f700bec00ff0037c00e7003bc00ff0035c04f5013f800df0311c0c3f000fc0c3f243fe103b010fc047f408b8001000000000000086003c04df003fc00ff043c41ad30436c02dd05b7c12df02b7c02dd0317c0c1f880462c118034c141f02174085f0084000000000000000000
8043414cd00b2408cd8131404c12134408) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (06c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0026c40df8016c12d30224c00d31037c20df2037c80df0816ca2db0137c109708a6d00170105000b000000000000040217c00f7003dc00b7024fc80db005dc00fb108fc00ff207fc00ff003fc00ffc11ec1837226ac21ff0007c40b9000d00890000000000000c2213c00df0035c439b00c4d00c
72034c00cf0901c00070225800df0837c80d300834021b0925c011f00c7401170047218000000000000006000f400d50037401d98004500d50215418d50025400dd0026480dd0036400d11007400d100260085d26074411510458803000000000000068143400cd0031400d15004400c50014400dd1021400c5002
3400cd0031400c520074000900210501d3) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (06e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (ec6cff0004c08f50235c003f002d220600000000000008404bc01cf0873c028f82c0c71c90150c40c10350d0dd30373401cf1173c0dcd0313c09011007c0bdf2223c40170b40003200000000000008201b401e5007a401ad014a485ed084840579a07c405e9007f445ed017b425e9005b401e9a0
4f451a9024a6312d3148000b00000000000008000f400cd00334008d8000404c90010401c10410412090023420cd0033400cd01830010120c22030d0003000050082202300000000000000004f400d70036000cd0002c01fd0010510db8034482db0037600dd0037400d90496451db2434401c10bb64009c0000a0
1300000000000004200fc00df0037c00df) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0700) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (4b400cd0033407cd00c0540c582504014d1033420cd2030400cd0033600cd04b7490cd01f1403c0033444bcd82332012000000000000040003401ed007b4118d1048685ed0058402fd0049401ed007a401ed807b401ed007a411fd007a403e12060401390048002000000000000004004f400ed0
038400ed0008400e100184006d202b400ed0038400ed083b400e70019480ed203bc40e10008400ad00091013000000000000062043c00df0034d009f0006d08d30070c00d30005c201f2024c01df1037c00d70005c01c70037c005300054401e1005301000000000000006200bc00df0037c009f0007c00df021fc
044f0037e00df1836c40ff023fc60ff021) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0720) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00950025040950236400d50227404952224501950134a0180000000000000800074009700244009100254048d10245009d00274039d0025c009700274009101e74069110276049104244068d20a620010000000000000420c3c009f1025c009304248809f8424c219f2827c099f0027c00940025
c009b0827c43910023420930026c009f0025003000000000000006004bc001f0004c401f0205d021a1007c001f3007c001f0804c001f0007c00170085c221f0807c041f0087ca41e200500120000000000000e201fc005d0017c036f0098c005f00dcc8167a15d8407f2116d005f9017e005f811f8027f011e4407
1401cd207b201da0230000000000000420) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0740) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000e0061c009f0026c05bf0028c01a7002dc00af002fc08bd0027c00bb0025c0097002cc00b7106cc00bf002c402bf002bb0190000000000000ca067c00971027c00bf402dc008f202dc00af003ec74bf002dc148f2027c009b052fc40bb252fc14f9003dc14af002fa01900000000
000008607bc001f0005c04132007c241d0006c001d0007c001f0007c00170005c00174007c00170107400154104c80170006001b00000000000000a0534008d00204149140235148d08224408d00230018d002302085002300081a023000854522400850d264208d006002100000000000000200734009d0825400
9100276089d00264089d00274009d88276) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0760) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (9f0424c209700e6c209f0025c00970267c439f1027c209b00a7c039f002500130000000000000e2015c009f00268139702e4c008f2461c008f0065c039f0027c009f0025c00970865d03850026cc19700649008f006621050000000000000600634009d00244a49500244009930247009d006560
89500270c09d10274009100240109111244049180244009d2225201c00000000000004804b4008d00226009508205428d20274008d00214448d00234008d00234608508216009500a25008500204409da021a0160000000000000460734001f0004408170014d021b0004d001d0004c055700074151d0007c00130
0144001128844001100044451d10171018) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0780) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (06b4016930480034000000000000002001040ed0038600c5007d402e1003c5402508380117d103b410a90039400e5042b490a100bb480690c2b480e9105c0004000000000000000053420cd8031400c58032681cd30304034500b1421cd00334008d0030400cd0177401c100b5428dc2873483c9
40722030000000000000020411c205d00144004300154407300144007701dc4027d20174007d0015c005f001e44279085f4017d00db40171891c2000000000000000042043c001f1006c02130086cc01f0084c08170807c861f0007c301f0006c001f0007c461b1107c021f1187c8c130405001000000000000006
004fc00970027c00970064c00972165c18) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (07a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (063c400e9023c400a5033f408ad003b4002d003b400ed800b488ad082a468ad03094047181090008000000000000044057405cd2b70401e1017ac4dcb0032c052b114b405cd1373c0d3d037bc09cd020b40d0d004bc8d0d02e84b5210341109500000000000006450bc01ff107cc09e3007c80cf
a0078c09ab027bc81ff007cc011f0077c01dd0a5f809df116fc819f126c8095343452802000000000000062041c00df0035d40d30037c00570031c001d8035c204f0037c009f2035c00dd0006c009f0027c001f0827cc05700052010000000000000004043c01ef0079c01e7407ac01ef00784012700798016d007
bc01ad0078c21ed007bc21eb407dc01ef0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (07c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (46051d01470230500444121101422183000000000000042213c00ff003cc10fb203ec20fb403ec003f083ce187f003dc097f003fc00f3102cc0033000ec8033002cc0073000d08a1000000000000040007c00df0035c00d70035c02df0137c18192637c001f0237c425f0037c00df0227c129d20
87c821d00060461f13050001000000000000042053e20df0036505c902f4440cb21b0402050837c059da0774805f0037400df00634218d00024859f0461d21530085283800000000000004001b400cd0032400c940724404920f05000d00034019d00314200d0031400cd00034080d80014250d004140351880320
52000000000000040003404ed083a404e9) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (07e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (17c10df0335c02d70131e0cc7103ff481f2105c041f0037c003f0b3fc14fa000fc22371007c84370005c802f1309a1010000000000000a8003c02df11b4d00d38534c049b02b6c001f0eb440c1f8335c8e1f0337416d7000462e1b0006c181b4406c145102060043000000000000008043414cd1
230404d58335406c900365040d00005500d8c330100d0132404cd10044000d04056041989064040109042810000000000000020007400dd0034600d10034443d930365031d30344001d10356101d0037600dd0044401992044411990066404510844200100000000000000021f400dd0034c00d51031483d90036c
011d0034c045d00374005d2037400df004) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0800) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0400010000400010000400010000400010000400010000000000000000000000000800020000800020000800020000800020000800020000800020000800020000800020000800020000800020000000000000000000000000084002100084002100084002100084002100084002100084002100
084002100084002100084002100084002100000000000000000000000008000200008000200008000200008000200008000200008000200008000200008000200008000200008000200000000000000000000000000850021400850021400850021400850021400850021400850021400850021400850021400850
0214008500214000000000000000000e20) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0820) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000850021400850021400850021400850021400850021400850021400850021400850021400850021400850021400000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000400010000400010000400010000400010000400010000400010000400010000400010000400010000400010000000000000000000000000010000400010000400010000400010000400010000400010000400010000400010000400010000400010000400000000000000000000000004000100004
0001000040001000040001000040001000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0840) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000040001000040001000040001000040001000040001000040001000040000000000000000000000008400210008400210008400210008400210008400210008400210008400210008400210008400210008400210000000000000000000020033800ce0033800ce0033800ce0033800ce00338
00ce0033800ce0033800ce0033800ce0033800ce0033800ce00008000000000000000000000840021000840021000840021000840021000840021000840021000840021000840021000840021000840021000000000000000000000000080002000080002000080002000080002000080002000080002000080002
0000800020000800020000800020000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0860) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000000000000000000000f0f00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000003c3c00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000420800000000000000000000000000000000000000000000000000000000000000000000000000000000000000000010820000000000000000000004000100004000100004000100004000100004000100004000100004000100004000100004000100004000100000000000000000000
0000001000040001000040001000040001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0880) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (fffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc00000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc00000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (08a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (008500214008500214008500214000000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc00000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003ffffff
fc0000000003fffffffc00000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc00000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc00
000000000000000000000000000003ffff) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (08c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000400010000400010000400010000400010000400010000400010000400010000400010000400010000400010000000000000000000000000800020000800020000800020000800020000800020000800020000800020000800020000800020000800020000000000000000000000000084002
100084002100084002100084002100084002100084002100084002100084002100084002100084002100000000000000000000000008000200008000200008000200008000200008000200008000200008000200008000200008000200008000200000000000000000000000000850021400850021400850021400
8500214008500214008500214008500214) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (08e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (8000200008000200008000200008000200008000200000000000000000000000000850021400850021400850021400850021400850021400850021400850021400850021400850021400850021400000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000400010000400010000400010000400010000400010000400010000400010000400010000400010000400010000000000000000000000000010000400010000400010000400010000400010000400010000400010000400010000400010
0004000100004000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0900) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000010000400010000400010000400010000400010000400010000400010000400010000400010000400010000400000000000000000000000084002100084002100084002100084002100084002100084002100084002100084002100084002100084002100000000000000
00000020033800ce0033800ce0033800ce0033800ce0033800ce0033800ce0033800ce0033800ce0033800ce0033800ce00008000000000000000000000840021000840021000840021000840021000840021000840021000840021000840021000840021000840021000000000000000000000000080002000080
0020000800020000800020000800020000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0920) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000000000000000000000000000000000000000000000000000000000000000000000f0f00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000003c3c00000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000420800000000000000000000000000000000000000000000000000000000000000000000000000000000000000000010820000000000000000000004000100004000100004000100004000100004000100004000100004000
1000040001000040001000040001000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0940) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0003fffffffc00000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc00000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003ffff
fffc00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0960) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (013cc8cd30237c01f3007ec01df0076c09ff007fc09db207fc010b004f4041b0b09c81ff0077a0030000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc00000000000000000000000000000003fffffffc0000
000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc00000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc00000000000000000000000000000003fffffffc0000000003fffffffc00000000
03fffffffc0000000003fffffffc000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0980) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (fc50bf046fc001f000fd00ff103d0085000000000000042201c00d54085c03030034c00d70037c03d30297c00df0037c00df0036820d30877c031a04c74031f0044c00df0835290000000000000004000f600d50135406516036400dd4037411dd00b5400dd0034400dd0034400c140576a11d09
17411110044400dd0835a803000000000000040143444c52101484110030420c50133410c1a435400cd0033404cd0030424c100374000d00034180d0200400cc0033a0130000000000000c4107430d1033440451263ec0ef303bf404df2134401dd0074480d70074504d510574011d0047406110184401dd007708
030000000000000e210dc01d30304d893b) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (09a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0b401e1015a41d3da079409e9227b40169017f401ed007b405ed0079081e1025e405b5007c40521004b401ed0178800f00000000000000010f400c000024040d0034400d90031406090033400cd0033400dd0031420c50033402052003609013007400c50032a01700000000000000015f400d10
2e54011d083d400f1003f444d10033400cd0037400dd2834400d10c6140391013440b990007400c90034201300000000000004201fc00d300844821f003cd00d34033c02db0037c00df0037c00df0034c00de0035c019700b6c021b0007c00d30035080b000000000000040207c00fb2062d803f083fc00d30837c
40ff007ed00ff003fc00f7003ec80ff003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (09c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01ed007b401e9407a401ad007840145287b401ed0079000100000000000004004f400e100384002b233c40ce103b8400a14038e80ed0039400fd003b400eb003b480ad00384406c100b400ed00398813000000000000062043c00d30034c0013003cc05d20174c80930030c01cf0034c01df2837
c00d70072c001d0015c201f0007400df0037a01500000000000006600bc00ff021dc042f263fc38f70a3fc0077023bc08ff023fc48df0836c00d70a19c08db0039c089f403fc00db0235b80200000000000000004bc0dc304c2d048f0070c05cb0971c044b0163c05cf0273c05ce0371d01d72233c05870223c050
b0803c80c7017010120000000000000001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (09e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000042043c009b0024c00930023c009f0027c019f0027c009f0027c009e0827c809f1265c209300a4e059b0027c009f0027081000000000000004004bc001f8405c481f0005c001e0007c0a1f0107c801f0005c801f0007c801a0007c021f0006c001f0007c001f0005001200000000
000004200fc0053409fd00730016c00570014c437300dec005f0016c005f0017c0059041ec087f011c7107f001fc005f0017a81700000000000004204b400c10276481091032480c10030405c10274400cd0033400c90033400c104f34028d04f0005dd0373400cd80332812000000000000040003401e1007b401
b1417a621e50078420f1a07e401ed207a4) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0a00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (a7552fc009f0027c149f0027c149e082fc00bf202fc14ff053fc009f0027b8190000000000000a406bc001b0110c00530107c441d0107c00570007c001f0007c001d0007c601d0004c00130016c241b0107c001f0007101d00000000000000804240081052140095052261485052344085002340
08d00236008d00234008920205208900204148d05234208d002000100000000000000000634009102244009100276009d00274289540276009d00274009d00264009d0024400d100264009900376009d0024001800000000000000000640091c0e54428500274009f20274039700274009d00274009d00274009d0
8644048b00a05059d00274009d00262001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0a20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (027c009f002520050000000000000000724208da0206809910244808800244889180274c09d10254408d00254a091022741499002740891a0274209d1025a8180000000000000480584148101a04848925204148105225008900234008d00204048d00204009100274408998234008140230008d
2023a012000000000000080062c01170044c010140c44030f80c6c151701476001d00054011d00054850b00074001100174001121474001d0007081c0000000000000ca060c009180ecc02b3c464e11910464c00bb0226c00bf0024c029f00248229b102bc00fb082fc00b300a7c00be0027a8190000000000000e
8066c149f152fc54af2527c148f0523c14) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0a40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0030400cd9030469dd0033400cd0031400cd0030400d10071406cd8173407cd0033400cd0032a0140000000000000004034005140dec0175001ec807d081c4007d001f4005d00144005d0014c005500514607d009b46371201f4005d0014a104000000000000040043c001b2006c401300044001
f2004c001f0087c40170805c001f0004c00131205c021f0007c42190087c001f0004001400000000000004014fc00970025d40970027c409f0023c00974267c009f0027c009f0027c009f4067c00970127c009f0263c009f00250017000000000000040014c20911024d109900205009100264019b04e34009d002
4c009f8024400910027c029b2027c82930) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0a60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (b48527005b405210178405ed01798835000000000000040508c01d31064c09c34474c2bdb007fc29950073c09df0277c09ff027dc05f7007b805bf2077c017f0076d01e90a7fa002000000000000042053c10d31027c00df0036c42df0237c001b2037400df0037818db0035c00dd0037c008f20
07c0013283fc00df0835b810000000000000000043c03e3007cc01e33070c27ed2178c01ff00fb401ef0079401ff0078d15e32079c21ef007bc01af017f401ef00781014000000000000002003404e1041a43065003b404ed0038400ed103b400ed0038404ed003a408e5003c011ad00bb410ed023b400ed003880
04000000000000002043400c10170480d1) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0a80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (07c80df0013c065f0036c00cf0037c025f1137c00d60037c40df2035c40d78027c429f2c17c08130635c00df00370009000000000000040040c00f34236c129a403c500f1003f4045d01bfc60df0035600ff0037420f700b7c2597a43740b17007cd00db0034a83400000000000004200a400c10
0c2403810831000c900354400500f3400cd0030420cd0032400c902e3400151883040110074400cd00332866000000000000040010400e10512408f90938408e10033400ed083f404ed0039404ed013b428ed022f400a5001b484250338424e908390208000000000000040056c01f1014ac01234970405fb203bc
41a70373401e70178c05dd0070401f1003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0aa0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (06fd05b7c36fc2025c04134106c80170037420d705363001000000000000008041402c10083404199032404cd0030404090037630c91031452cd0931444cd0023400102405604010033404cd03302010000000000000000007400d100274009d8035400d10834690050037400d50035400cd0037
440dd0035441910106401152837400d50034a00100000000000000020dc00d14027c054d0037c00d70034422134033440d98035400dd0035c00dd0026c871181c0431110037400dd10362103000000000000040203c20f3003fc093f003c800f3003cc00f3003fe20ff003cc00ff203fc80ff267cc103b005ec003
70037c00ff003f08a90000000000000400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ac0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000040040400c90033400c100356888d0030400050121408cd00334009100074008d00b24408d0003408cd0000008cd200300130000000000000c0104401d32077401d108744161d20754019b0025403fd1076441118287404d300f64109d0044403dd0044403dd0047000300000000
00000e210cd01d34077c01d94075c001b807cc011f20e0d00d70074c00bf010f443a7103ec803f084d884ff084dd40ff004bb0830000000000000ee007c08ff020fc283f033bc24f7093fe003405bfc00ff00bf804df2535e94df082ec921f080ee161f10bfc08df013710050000000000000a6003c24f32197c04
1f0235d18f10234510d721b740ed702344) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ae0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (8301a4425ed20344008f02d2c00d5023b4019d0064c00fd03a4440e00084a81300000000000004000fc00db0037c00df0037c001f2037c80df1005c80ff1034c009f1294c40d30037c009f0024c08df0005c20db2005000b000000000000040207d00ff003fc00f7403fc409e003fc00bb103ec0
0ff803cc0097221fc10fd0035c80bf202dc00df116ec00ff00cd0081000000000000040210c00db0037840d30031401191034ca1978025800d70835d01d14057c05df1036c138f0047c00cd0104c00df008401a000000000000004000c400d100370c0d100344089d08354019d2025000dd0036461910806421d12
0364219d0846420dd0024400dd0c05a003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0b00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (027440d70041281000000000000004600bc08df1237c00ff023cc009f2237c00b7002ec06df1a36d00b7922fc00df003fc089f002fc08df202ec40ef0205280200000000000000005bc01cb0873c8dcf0071c058f0033c01062161c0dcf8271c0d8b1080c08c50933c288f0822c81cd0821404cb
1540003200000000000000011b401ed007b401ed00794056d007b407a001ed40dcd20796012d006a401e5107b409ac0468405ed0848581f101cc000b00000000000008210f400c90033400cd01f16121d0033400050825006cd0031430890040400c502b360c850402600cd0080484c98000202300000000000000
005f400cd0033400dd01344119d0037407) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0b20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0017c0b7f0013c107100dcc007d00174067f001fc70778816c2f73005fc007e201b80077009da8030000000000000c004b400cd0033000c11032400cd0033404852421460cd00334428d0227401550033402d91173000cd0033400c104712816000000000000040003401ed08796a1e9687b4416
d007b441a1e04c609fd087b401ad0041481ed017a601f1046f485ed046b405e50469000400000000000000004f400ed003b400e3003a400ec003b400a70038504ed083b400a5002b480e70039440ab202b400ed202b407e110190813000000000000044043c00df0037c00db0033c203f2037c80931020d86ef203
7c00b30007c20d78234c00c70047c08ff0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0b40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (04148d082343481c0254548d006000100000000000000280634009d00274009514276009100246009d802544a9d00254009900244009d10244809d003440891012440095002420180000000000000020074009d00274009500e3490910025491830060c038d002441a8200244009d01a6c409d04
674449101e54129d02242001000000000000040043c009f0027c40970a27e25952024c439f28a5c80972027c01931224c009f0224c009f0226800970024c40870065081000000000000004005bc001f0007c80178006c281f0007c02170a86d021f0807e10170007c041f2005c001a0887c021f2107c001f000500
1200000000000004000fc005f0015c005b) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0b60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (604001140074001140058051d80054001321445021b40044021b11c6c811d9086403171004508170016c0211280718180000000000000e4060d00b3402fc0093402ec09bf902cc80a24028c91b2402fc45b32decc08b7046ec29bf002dc05bd202cc35a3802b28190000000000000e2067c009f0
027c009f002fc14fb0027c40b6053dc009f0026e20f7452fc94bf0827454bf302bc009f002fc009f202f981900000000000000806bc001f0007e00172007404132004c001f0815c04170005c041b0104d001d21045041f2004c04110004c04170006101b0000000000000080434008d00234008500236148140214
0091c0204148d0020414810520400cd052) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0b80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (001f0004c401321068521f00048001f0004c841b0405081000000000000004014fd009f0027c009f4425c038f0025c009700e5d009b0024c008f0026c009f0024c018f10e6c00970427c008f00250813000000000000040014c00930027c00930020c029d0026c008140e6c00952025c829f0023
c109f0026c049d0164c009f0024c009100a52005000000000000040070400910027400910025400dd00274049100264009180254049900274009d0827408950024000dd21266009140a5001c0000000000000400484208100234008100240428d00226009104224409500214028d00234049d00224068d00204009
c102042085102022160000000000000c00) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ba0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000000043c01ef087bc81ef0048c01ff007ac01e508698016d007b401af084ac01234058401ad0069d016d105aca1ab00481010000000000000000003600e5003b400e9440a0102d003b400f50c3e40041003b480ed000b400311060140f510a9602cd140b440210008080000000000
0000000043400cd0833480cd00c0600cd1832404c5c1654324d28334b1cd08020008100b04028d2131205cd00b24038900f020100000000000000424034004700134205b001ec017d001540375001ec136280124127f001d41061041c42073805c0006900dd4107101582100000000000000040143c001f0007c00
1f0004c601f0004c281b0085c001f1007c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0bc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (c10421400490031413cd00816010900034114520824200802830004982012042000000000000040013400ed033b400e9020a454ad203b400e1402c440418039400ed000940031000a400ad000a60061000b004650909001c00000000000004005740def017b400e701c940d2d0878400e30239c0
d624239400cd02094083b0009c106710a840443000b4026b00c1005500000000000004250bc01f7007fc01fb0044c0db7007dc41ef107dc05778278801ef204cc01b2206ec81bf026c1016b405bc45f30a4da802000000000000042153c00d70037c00df0003c20ff0035c00d5003fc005b0036c8097080d4000f0
814c00cb0026c401b0005c00171005a814) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0be0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (444420140044280100000000000000020f400dd0035c00db0096c03170034441c10022e981900354038520004094100424121500c64011500c04001d00442183000000000000042203c00fb003fc80ff096ce103f003ec00fb012cc007f003dc0031022fc01734007e0233002fc297b000cc492f
000d0081000000000000040007c00d78037080df0085c021f0035c015b02a7802570037c009f00178405f0005c42150185c005700874a21f00850001000000000000042043c00d70037c00db2002c01c70037c02d140e4c00432035c459f022540cd32006c001f0422400512247c00130005205800000000000004
200b400cd0033440c510034228d0832410) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0c00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0007c1cdb027cc04130077c01d70077c00ff107f481f3004cc01315007c01ff0077c01f3007d80030000000000000e6007c02df20b5c04ff050bc000f00b6804fb8029d88db013ec00ff000fc0037000ec003f000ec0437900fc003f2603b821000000000000080003c02db0237c02df01044041
f0036c8adb10244065d0035448d50026c001b0007400170007c08130004c401721060143000000000000000043406cd0031408c915024161520306019100864064d0231400c508104001800034000508034200508044000d110000300000000000000a8007400dd0037400dd00044049d0036401dd0c244005d203
5483d504264009910c7400150067600111) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0c20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (fc2037102fc80ff003dc00ff403d80050000000000000e0a0bc00df0035c09971147c80d30034c25132037c00d70037c00d70037c00d302c44011b0047c80df0037c00d3003788820000000000000ea00f040dd0035500110233400d90035408114033400d10037400dd3037420d500054211900
67420dd8037400d10037a80300000000000004004f400cd1031400c15003400c18131458010033400c50037408c50033400c100004a0090813400cd0133400c1003120100000000000000c200f441dd1874400014007406fb1035446110537401d10076443dd0077481d54045421110027401dd0535c01d1007708
010000000000000e220fc01df0076c0097) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0c40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (7f409ed807840521025a429e9047b50dad057b405ed007b401ed8179441e9824a42169004a461fd007b405ed0078800600000000000008000f400cd0030402910043420c92037400cd0033400cd0037400c90030482c9002250b090454400cd0833400cd8032a00300000000000002006f400dd0
0344021102b448af100b4000dd0037400dd0037400fd0035402db0283c0b0144f6c00dd0037400dd0030a01300000000000004000fc00df0034c12d34295e00db04348200f0037c00df0037c00dd0034c04d70017c00130094c00df0037c00db80350803000000000000060017c20ff003ec013f4867000fd003fc
c0df043fc00fd003ec80ff003fc00ff400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0c60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (05ed1078401ed004a401a10050401e1007b401ed0079000000000000000004604c400ed0038400614030414e30038400cf003b400ed003b404ed0039440e10809400614038400e1003f440ed00390817000000000000040040d01ce1036c00830034c0cc14834c005f0037c00df0037840df2034
801c72002c00038014c01c30037c00df0035201400000000000006200bc48df0037c2c3f003dc20d70234c44bf003fc00de0837c18ff023fc48cf180bc0847212fc00df023fc08ff0235b20200000000000008404bc01cf0370c03c30363409db0037c01cf0073c05cf0373e01cf0370c01cb0083c010b20d4c01d
f0173c85cd207010160000000000000820) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0c80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000042043c009f0024c01836225c01930824c10930066c809f00278009f0027c00930026c01930067c00950027c009f0026081000000000000006004bc001f0005c04190007c02170006c021f0087e001f0007c801f0007c00170685c101f0187c001f0007c001f0007001200000000
00000e201cc005f0016c0077001cd007300145017d0017c005f0017c005d0014c005f009ac007300dcd00510017c005f00158807000000000000040058400cd0032403c50474400d10034689d50037400cd0033640cd1031400c980414024102b4600c10037400cd00312812000000000000040010401ed007a403
f540f8405f9207c4016d107b641ed007b4) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ca0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (bf0527c009b1027c00970027c009f402fc00bb052fc80910527c009f0027b81900000000000008c07bc001f0004c04130105c04111004c841380064001f0007c041f9007c00130006c00134105c2015a007c001f0006b01e00000000000000a0534008d0022414810520414c58030514c1402340
08900234148d0023400819025000d115234008d00234008d002020100000000000000200734009d002440a9100254009112244019101274009d00274009d0027400910066604d102254009500274009d0024a01800000000000008000f4009d0026c039104644089500a44009101e7400990027400970027404910
1654028101e74009300274409d00262001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0cc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (027c00930027a8050000000000000680634009d0024438c180754009900264008d00274009d08274009d80244009101a64009120274009d0027420910025a8180000000000000c004b4008d00204048141f16008800224628d01214608d00236008d20205208120224209104234008d042340081
002320120000000000000c60734001d00045011101854031b24444851d10434801d0007002190004400114006c005101c74201d00474c0114007081c0000000000000e0063c00bf0024c19b308adc59bb1028d83bf00afc009f00274519f0024c00b3082dc00a1056fc00bf0027c0093402da01800000000000006
a067c009f0027c14bf052fc949f052bc54) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ce0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (04364008104c0442c900f3400cd0033400cd00334114100104114100f3400cd0033400cd0032201400000000000002005340079001450171401d4807b101d44471091f4005d00174005d08174406b009940771101f4005900174005d0011a014000000000000042043c001f0004c08130004e200
30204c04130007c001f0007c201f0007c00130484c62130407c001b0007c001f0005081400000000000006004fc009f3027c009f0027c009f2825c009f0427c009f0027c009b0027c009f4066e009f6023c009f0027c009f402580170000000000000e2017c009f0824c80932025c809b0022c009f0025c009f082
7c809d0024c00930025e20832327c009f1) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0d00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (85014d0408501c1123f008cd03718015000000000000040000c017f107cc81f32176c21b3104c021770047809ff227fcc1df0075c01224858c096f005cc89e9047fc01ff007fa000000000000000062043c005f2035c00170024d009f0014c00970007c80df0037c20df0037c005f08034205f08
1fc00df003fc00df0035b010000000000000084047c016f007ac013b007e441330048d01bb007bc41ef007bc01ed007bc01e30048c4163405fc01ef017bc21ed207a101500000000000008200740069003a400e9003b400a9002b440e9407b400ed003b400ed003b41069103940071009b600e9083b400ec003a00
050000000000000c00534804d2832400c9) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0d20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (07c405f2035c105f1033c425f0027c40df1037c00df0037c00df2037c821f0085e015f0187c00d70037c00df003580010000000000000e2054c005f0036c01d10174400d90004d0bdf0037400dc0036400dd0035c80010080f035d00c44c0db103fc00df0037a835000000000000040010400450
03240301900240089800040a810003400c50033420c500334000100824104d2040400c80033400cd003328040000000000000400004006d013a6002162b844029110c400ad000b408ed013a404ed08396402104084046d0218424e9003b400ed00390100000000000000046254401670178514e1015ac01ab0348c
0863007f405ef017b405cf0073c0d01021) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0d40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0edf11b6c0a1f0006c14530097c1ed71837402db033620000000000000000080434004d04336000901836104188004080905b3480cd8131414cd803240401000040cd10003404c90233448c9013008100000000000000200074005d0037400910827418d90204414150007400dd0034400dd0036
4031d44466085100c7400d50037400dd0034a0010000000000000802174005c10374405300c4c02110001421590007400dd0035400dd0036c031100444050100d7400dd0036400dd00362081000000000000042213c007f103fc42d302564002b004cc016f203dc00ff003cc00ef003ec003f040ec0173181bc00f
f003fc00fb003d08800000000000000600) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0d60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000e8043400c10132400910036444c500304004904304048500004200d000040205000040001008240001c800402091203a2100000000000000c0017401dba036c00110034c00d10075401d501bc4128d02474091d08c54031d12444891100c440b130244402110087080100000000
00000e200fc01d39274c01bb026ac09d70074c013b053cc1497000cc043f050cc043f080cc0033000cc2433090fd00320907a8030000000000000e6417c084f0137c8437208cc100f0203c243f010fe22df0037c00ff873fc081f000fc045f150fc20df013ec00ff0337a8050000000000000ac003c0c5f02b7c8a
930187c041b0904d00070087c0cdd07b44) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0d80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (dd003d4205108244009101a54001100444000101a4404914107480140024201300000000000004000ec00df2135c80931834c00df0036c00df8035c00570025c04930124402070284c02130121c04930083c001b0021000300000000000004061fc00ff003fc00bf003dc00ff003fc10ff003fd0
07f00654018f1067c011f0047c411f0065c01970845d003308650087000000000000040003c00d10036c138300f6c00d70034c008b0034c00470224c089f1224c2a1f0284c0a124226c28830284c031b4225200000000000000006201f400d120365019140f4400d10035400d500304209d30074001d00054101d0
4044101100060001980044141d2005a003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0da0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (035c00d30077a01500000000000006600bc08f7023ec08ef423fc00ff0039c08ef003fc01bf001ec00571816c44f3023de28f2001ec0057203fc00df8015b80200000000000000004bc05cf0071c00c30350d09df2370d004d2031c05838011c044b0010404cf0030e48cf0810c804b0033c00cb
0150101200000000000002001b405ed0079401f101b8449e10478451fd0079405a1025860169a25940de1007a409ed085860169027b401e5025880460000000000000a019f400cd00b5400c18010600dd00704230d003140081c01050b4850d0500c94072509cd50d0501494133440d94012a80700000000000000
004f400d704b44189100b040fd10030c00) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0dc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (005cc005f0010c407b2015c037b0094c225b1094d00514015d00570894c02530815c80530095a8170000000000000c204b400cd00324028101f0400cd0032400c900335995901b0590c101b2420c00030420cd0032406c1c030400c14033281200000000000004000f401ed007a601b12078401f
50078401e91970401690078401e92078401e10078001e52079601e10079401e10039000300000000000004204f400ed0038500a14038400ed803ac00eb023bc004b2030400c1a038c00c10030400cb003ac00e12038500c1203d88130000000000000c8047c00df0834ca1930034d21df2036c008b02b5c0053103
6c81db8030840d30037c01d30834c40c30) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0de0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (b414ad0528474a5053b414a1052820100000000000000400634009d08274909940a7400990026600950024400b1002e408b5002c480b5202f408bd142c408bd083e400b1402420180000000000000800076009d00a74029f0023401910024d058120254009100270139503256009500674009502
2447291406540091002720010000000000000c2043c009f0027c10930a67c489f0824c35970024c40930027c41910064e00910163c00910024c009300a4c0083002708100000000000000c004bc401e0805c081f4207c021f0007c021f1003c003f0003c021f8081c400f0005c401a0483c020f0083c401f040300
120000000000000620dfc005f0016d2373) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0e00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (734001fa044401570047401190004c001f85c4c0f1510074001e00874401b0a86c0a1c0806c021300844431147c7081c0000000000000e0063c009f88aec82b300abc48bf002ec00af8164d01921167c05b39c6dc11b7006cc01bf006ce15b7046cc35934067a8190000000000000e6067c009f0
527414af652bc14af0025c40bf0527c149f2027c009b1027c009f8027c00970023d209b0021c349f0d27b8190000000000000040734001f0817c801b0007c405b0806c00170104c04314107c04174104404170107cc41f0904d04170106c04130104101d0000000000000088434008d00234008d00234008100204
00810521414a1052b494a51529414a5052) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0e20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00170006c00110004c00131005c041f0007c401320050014000000000000040157c009f0426c009748e7c009f0027c009f1027c008f0027410950026e009f0027c808f0026c808f0022d009f202500150000000000000c2117c009d0027c02830063c009f1026c008d0026c80930027400910025
c20950024c009f0025400970025d009300252005000000000000062063400950025400d50027400990024604d508246409500274809d10274809100264009d80274009100254a091002180180000000000000e80434008d21236048101234048d80224008d02224108180a34028108274408500204008d80a14808
c002101081002200100000000000000c20) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0e40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000004053c01ef0078c8133006bc01ef0068441220173445ff087ae81e71078c81e32063901c34079c01eb2073411e300fc1014000000000000020011400ed041a410a1843b4002d802848035037a40ced103b480ed0038601e5803b410e50073422e9803b60ce50138800400000000
00000a0053400cd00f0400818033447cd0060507c10033600cd8032400c502f4400c10233401c10633400c90433000d10032a814000000000000000011c205d085e88071021f4047c00144407510144207d08174717d029cc0055205040157009f42371015f4405520142104000000000000042153c001f2006c90
130007c001f1206c88130805c001f2002c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0e60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (058035422cd0033400050003400c500204008100034200d1002440cd00372846000000000000040003404e1010b60461012c60021202841c290139600ed013a404c10038400e10022000818023488ed8828508e501390008000000000000022057401e1026b4012f027140d2b103bc0127087d40
ded037960725000bc20e50028c04e1211b00d6c011ad40eb117988150000000000000e000bc09d30267cad530274c01d31268c890302f4c03df0074c41f3207ec01f3106cd41fb207fc01ff007e841f308ffa002000000000000066041c00df001fc003f4027c00ff00248001f0135006df1037e00df0035d00cf0
034c00de1037c00932037c46df0835b810) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0e80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (436400d10034200100000000000008820f400dd00444820501f6c009d1026403110035400df08344a15b01d6440d10066c0095000544a150204400d1183620a30000000000000c2203c00ff007cc00b3803cc41bf202fc9937003cc00cb0039c00730017c00db00acc00e3821cc8173201ed00e3
003f09a1000000000000040007c00df000fc029f01b7c001f0027c021f8037c00ff0035c009f0021c20df0027c00970027c40cf0027d40db003700010000000000000e2053c00d340370c29301f4c00930024c0013003dc0dfd0036400810024c00d10022400d34033c20de0030400f7403da87c0000000000000c
201b400c100034060d00c5400190033402) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ea0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (5007c04f7010f481bf0077c09bf007fc011f0074c01ff087fc00ff006ac61ff007cc01fb187fa0030000000000000e4017c08ff0d8f9003f0a2bc0c2f013ec023b003fc22fe00bee201f800ec00fb002ee00be100f4081f000ec40ff0e359805000000000000004003c06df2090c14510224c0a1
f0027c0017003cc0ef38135600532017c40dba024c00914004c20112006c40e3003a1003000000000000008043402cd01204841500224000d2232404010431400cd0030410090003400c10022400810001404058801600c101302010000000000000000007400dd09344405100644089d0027400150034400d1003
5401910867400d90024408d10434402910) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ec0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (dc40f3003f000ff003fd00ff003d80050000000000000e220bc0b1341074001900c7c40d70001c099f0037421dd0037c035d0036000de0037d00d70027c00df0034c00dd0037a80200000000000004800f410510027480d91057400d10007400dd00374009d00370111d0836420dd1034400d520
27400dc0034400dd0034a003000000000000040043000010803480090007400c510016008d00334008d00334004d0032400c90031400c50023600cd0030400cd0033a0100000000000000c61074a113004740111004740bf122774019700774049d80774011d0076c01dd207440bf12027401dd1074401dd007718
010000000000000e810fc0033100fe8030) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0ee0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1840fa1097b4092902d8405e1017b441ad017b405ad027a431ad017b421e90078409c1406f4a1ed007a401ed207a080600000000000008000c400018001400010800400c180436418d00334008d0033400090033402cd0031540c10067600cd0033400cd0032200300000000000002004c401d10
034c0ad30010400f10137400dd00374009780374019d0837407cd0034412f122f7400dd2036400cd0034a01300000000000004200cc0a930830c40131094d00d30037c089f0037e009f0037c24db0037c24df0034c04c38227c00df0037c00d700350803000000000000060817c00d70097c85d7080fc10df0037c
00f7003fc83ff003fc00bf003fc00ff003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0f00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01e5007b401ed0078409e1006f421ed207b4c1ed0079000400000000000004604c400c10038400e1401ac0acd0038400eb8838500e1003b460e1403b600ef0038404eb0039c00ed003b600ed003998330000000000000c0040c00530066c00d70014c24df0004c01c34070c00d34073c005b1073
c00df0036d14d30027c00df0037c00df8037a01000000000000006000bc28df0034c80d70013c08ff000fc88df0037c00d70237c00ff103fc00ff803fc09ff0027c00ff0036c00ff023da002000000000000084048d0dc34151d00c302c0485c14343c20cf0173405cd0073c01cb0173c01cf0230c01c11023ccdc
f0033c00cf007210120000000000000820) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0f20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000420400008f8024c008b0024c899f0027c009f2024c009f0027c019f3027c059f0025c01930027c009d0027c009f00250810000000000000060049c06170407c04172307c001f1407c00170007c001f0007c0c1b0007c021f0005c201b0007c001f0007c001f0005801200000000
00000e201e5007b009ec807300584004f011cd00710014c01530017c007700174005d0016c006100174005d0017c005f0017a8170000000000000c805a44bc94270409c90032400cd80b0409c90030408d10033401c50033400c50032400c14031400cd8033400cd00322036000000000000000012401e92072401
c10058405ed0078401e10078401e1007b4) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0f40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (bf0027c74af0027c20ff0027c009f1027c008f052bc009f3026c009f0027a8190000000000000a4079c045d0104c041b01044041f01074001f0004c001f0007c001f0007c00170005804130007c00170007c00170006b01c00000000000000a0536148d85204948105244148d052340089002140
08d00224008d0023400cd00206148500236008d00224008d002028140000000000000080716009d0424400d948644209d00274819d00244009d00274089d00274009408254189110e3400950027400950024a01c000000000000080006c029d00a45009100244019d00276019d00254009d00274059d00274029d0
0254039500a74009d00264009d00262001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0f60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (027c00910027a805000000000000040063400b5006c484b1002f400b100274009500274019d0027440dd08256009d00264009900276009d0027400910025201800000000000006884b483a50268501a98069402a140ab4008900234108d00234008500234008520204029101334008d002340081
002120120000000000000c6073400310084c0a130284c001100074801700074051d00074401d0005c001d20044021b01434001d0007400110007181c0000000000000e8063c04931124e849b0124c25930167c00bd082fc009f802f400af302fc00bf0024505b320bfe009f002fc00bb502da2180000000000000e
2066c00be002fc00bf482bd009f102fc00) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0f80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (2033080c100b0403cd8030400cd1030400cd0033604cd8832400c10093400cd1833400cd0032a014000000000000020050400541810c00510015c805100145137d00144007700154027708174237d181458165101b4205d00174005d0010a014000000000000042040c40332004c000b0007c000
30084c001f0004c001f2004e061f0007c081f0004c00130805c001f8007c001f0005081000000000000006004fc039b1025c009f0960d009f1463c14971027c009f0027c889f0025c009f0025c209f2427c009f0027c0097002580130000000000000e2017c02974024c029b0025e009306e7c009b0027c009d902
7c03970827400970024c009108274009d0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0fa0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (84014d21db405c1017b40ded03710815000000000000042403c013f006ec09bb087c441f3005bc09b3107ec09ff027fc01df8077c09df007c801dd014fc01dd407bc09df00752800000000000000060143c00df0015c00570005c401f4027c008f0037d0ef70037c40df0037c00df0835e005f00
17c40df0037c00df1035a010000000000000084044d01c34052d01c3406bc81a10070c01af087842dff0078441ef007bc01ef007ac0161044bc01ed107bc01ef007810110000000000000820044236000ba402610011400618028401bd8038405ed0039411f5003b480ed203850245081b400ed003b400ed003888
01000000000000080050401411072601c1) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0fc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (07c085f0475c11570017c005f4127c0a992037c00ff0037c121b2037c02df0035c000f0057c80d70037c00df003700010000000000000e00574025d0076c01d304f2c00d114f7c809f0034c00fd0037c058f80374409f00345005f0817c00d16037400df0035a0150000000000000420134048d0
0824000d01424000100834218d00326a0cd00334010118314000c00304000c0017400c00033600cd00312024000000000000040003401ad800a40481012e404a1001b404ad033c404fc003b4006d013b404ad00384002d000b484e1013b608ed3039000000000000000004285740d0d006248925015ec0d4102034
0dab017ec0dcd0173409a3017bc014d223) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0fe0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (4e5f1037c8e1f0037d1411013fc0edf0d37c20df23b6300000000000000000a04340c0580234040984944c64d00034100d0131404c501314040d8332410490031404050412410cd0132424cd003008100000000000000200074001d0027480918834400d500156011d0034400cd00344019d0037
6019d0035484512057400dd0037400dd0034a001000000000000080217400df00174a0534005c000d00274539d0035420df00354035d00374135d003551215b0d7400d91037440dd00362885000000000000040213c00f7801fc00f3002ec009f003fc00bf003cd20ff003ce00ff003fc003f003f40173801fc00f
7003fc00ff003f00840000000000000600) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1000) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000e8043400cd0482600016000400c50030400c98800000192410400090230410cd0021600050000400850003400011833a0100000000000000c2005c01dd0185401130924401d10075400d5104500111010440b5101bdc04d7026560131004446191000744110203f080100000000
00000e000fc01ff100ec0033020cc00f3083cc01f30048c013b004cd041b233cc01ff892cc0037080dc2197004bc81332037a0030000000000000e0017e029f8207c08174805d041f010fc201f0337c2ccf0237c0c3f033fc243f003fc102f1017c04fb0037e08ff033fa0050000000000000ac003c069f8287c00
930124c92970295c041d13b4c08fd03b44) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1020) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (d10802e009f20244811b003e400d180364009d00e700fd103e40101d003c201300000000000004200fc00d300bec00934080c20d30037c00d30005e021f1035c8487003ec40db0026c020f1403c00970084c021f0031080300000000000004061dc00ff024fc04f70057d00db4037c10f3004fc0
07d000fc01330035420f70177c003f002ec01bb002fc003f003d00870000000000000c2013c00df11568808300d4c00d30034c20cb4084c044b0854c029b0034c20dd00254131504c4c088720c7c03134035280000000000000006200f400dd0005400118224400d10035400dd0185408110464404551037400c90
025401110104500950467401110035a803) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1040) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (024c00034037a01500000000000006600bc00ff001ec28bf2037c08ff423fca0f70007c086f823dc00c7023ec00ff123e4007fa03fc08ff012dc002f20bdb80200000000000000405bc01c34245d29cb0050c01c30031c0dcb41414050d0153c03070233c00c34023408490013c05818122e000f
0070101200000000000002001b401e1037940d010168409e1807b401e9094a445b5006a401e8127b601e1046b4012d024b405a1434a5017d037880460000000000000a010f400c10021400498000400c08031602c900004408d0007409052837600c100636000902034208108064010d0032a00700000000000000
014f400d102a4c00d32104580e1083b602) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1060) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (101ec80514017c205b009ec4073015cc007b1017c005f0017c4073015fc014b00dcc05730015a8170000000000000c20cb400c108f3421cd01f3400c10033400d9a4b0480c10135406c10033400dd0273402c18470401c180f0443c90037281200000000000000000f401e1047b441e900fa449c
1c273401e9000e643310078021f9033b401e5006b48161405b401a9c0f8481210171000300000000000006204f400e1003144065203d604e1203b400e10028ca0e12039600f1013b400ed0039c20a12031c80a10038c006b00b988130000000000000e0057c00d3007cc00530034c20d39037c80d30002c00db083
4e00db04ffc00df8025c10130005c409b1) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1080) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0414814d2340081002340095052020100000000000000400634009d2024442d100364009000264029500244009980244489100244009d0024400910426622910226422d10024a0180000000000000800074009d00a40899b01e6c00920024c819d08245008b0024e81911027c009708244009102
e54029101e140285102620010000000000000c2043c809f00a4c00830224c00830022c099f0024c10932024d81831024c009d0124d00830020e08934464c0893802708100000000000000c004be001f0405892170001c801f0007c82174007c00178007c481f0003c001f0085e10170007d0a170085d101f200700
1200000000000006205fc0053c01fd077b) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (10a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (73400170052c68112144502110005c411f00045001d00474021d08c64010d00044081b0005c001b01474005a0cc7081c0000000000000e0063c009f126cc05a305ecd05b3002fc02b3003cc00bf0023c35bf0c67c009f002e40593256fc00b748abc00a30967a0190000000000000ee067c009e0
52f500af252fc009500274549d002fc00ef0d28c20bf0527c949f002fc00ff002dc00af4529c40bd0525b8190000000000000a4073c001f0104d04130106c04114106c00170004c001940044045101004401f0104c04110106400130006400110106101d0000000000000080434008d05306148905224148905204
008d882040081082141481052340085053) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (10c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (18130004ca01f0006c00170007c10130184c081b00050814000000000000040157c00970027d009f00a7d009b0021c009f2126c209f00270009f0826c009f0027c808f0021c409f0127c009740250015000000000000042117c009f00a4c0693c024c00974027c00930065c089f0067c009f0027
4609f00668029300a7c009501a3c2a931827080500000000000004a063400950026440918820400950025480dd20354409d02a74009d0026620990064401990127401d10027420990025a8180000000000000680436008d01a07008188204028580236008100256008d0d234008d05234148d00224008110634808
50123400801323a0100000000000000c20) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (10e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000004053c01e3407ac012b0078401eb007ad01fb007b4016f0178c01c300bcc0bed004ac01e7004be012300584012301701034000000000000020013400e100fa500290021540c98032403e9003f40061017d681e1013b481ed00ab600ed0009400214019401a54338800400000000
00000a0053420c128725100910b0420c82032607c90433420450030402c10030400cd0072400c500b3422c10070422c18036a03400000000000000001340051001ec0161009d4004100144827b315b20065201d4017100158005d801f4005d029dc10710c9d4087300142104000000000000042053c001308c4c08
130404c00134004c801b0807c021f0804c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1100) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (4101f14114504764010d0031440cd0042490c100820080910874210900372046000000000000040803484ed201a614e11018400e9003b424e1803f40061003b400a9003b420e9000b400e1100b48031000f4022101310008000000000000060055c05cd0062c08014a4440dcb017b400014133c2
547043440a6f0039c04ef002a420e0008ac002a0019c802b027988150000000000000e400bc41df2044c8d22005cc01c30277c053b813fc095b047dc01f3007fc01f3006fc01f3031cc0933005fc01330a77a802000000000000064043c00df001fc00176027c00d70035c20570033c005f0037c00df05bdc04ff0
007c00dd0007c00172017c001308359810) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1120) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (054400190034080100000000000008020f600d10846d051d0005c00d700374031b00336005b0037001552037420dd0044000de00454030104c5458154036218b0000000000000c2201c00f31229c0137000cc00eb0033c01b720bfc0073003fc40130035e00ff8005c40ff8004c0033401cc013b
003f00a10000000000000c0007c00df083fc001f043fc00df0837e02570037c405f1034ca0db203fc00f70006ca0cf0447c201f0305c0a1f00370009000000000000062053c00df0176c01030034d20db0037c005b01f763051087fe1b9b003fc00fb0107c22d30046c40130097c0303003da0340000000000000c
2019400cd0012401c10000400c90033400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1140) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (085cc08bb003cc0cb700adc003b000fc411f0047c601f007dc01d3184fc01df407fc01d10055a8830000000000000e2017c04ff030fc143f0085c0cf7023fc443f110bc0c7f813fc243f103f880fe000ec00f7200f4002d000bc0037013fb805000000000000080001c14d34105c82170004c24d
30037c0297000764453183700011003dc00fd0005c00dd0004c02130004c001b0534100100000000000000004340cc103224400d10f1402c1813340809808760c491232408450032400c90000400cd00014020108016001903302010000000000000020005400d10005428150074480d140374081d000748055003
6001910031400dd0447400dc0206401110) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1160) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (fa00fb000f800ff003fc00ff400d0081000000000000040e03400d30842c01530010c00cb1034c08134165c010f0287c435f0857c111d0035c00d70047c40df0037c00d10037208000000000000006000f420d102344301910164819800345209980644111504074019d80e7401150034400d50c
47400d18037400d100052003000000000000048143400c100124001100106488900304029150204400d00034004d00134020d1032500c50001440cd2833400c100012013000000000000040107c41d10014421130014c06ab403c40691a1244011100074011d00474231f1874400d10007401d12077401d1004700
030000000000000e810fc01f3006ec0033) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1180) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0b401e1005c60dad025b409e5167a40da5135a40d610f4b605ac010a4052900786ade1004b40ded007b405e501c8084b00000000000000800f400c544014028d0212500c500304008000134420500826000d0003403050031411d10007400c50073400c90010280300000000000000205f440d18
1544050d02d5400d1003c4008d20244821000374009d00244039d0035510d10917400dd02f3400d501c0a01f00000000000004001fc00d70015c861f1014c00df0030d00930025c06170183c00df0015c061f0036e00d30007c00d70037c00db10240027000000000000040205c00ff604fc0857081dd40ff0437c
01138023c801b0007c603f082fc001f003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (11a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01f100ff401ed1078401ed044a401ed007b401ed0069000000000000000004004f400e10018520e12018400a7133040633003ac00610002c80e3003f40069083ac80fd0008500ed003b400ed00090033000000000000044043400d30024c00d300148109300b4d00192034c00030004c01d30077
c00572034c00df0024d01cf0037c00df0035301000000000000004200be00ff021be28ff021dc08f3263dc00ff0015c047f280fc08df0035c087f083fe88ff021fc20ff003fc08ff0209200200000000000000004bc01c50051e4d8f0152c05c51230c09c30343841070343c074f0373c154f0a33d05d30047c85c
70473c0dcb014000120000000000000020) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (11c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000c0043c00930024e81930024d008308a4c80930026c81930063c009e0027c019f0025c04930026c009f0067c00970825001000000000000004004bc001f4105c001f0005c401f0007c001f0607c041f0606c0c1711074021b0006d001f0005c001f0087c001f0085001200000000
000006800fc2053405ec0863081cc10530014c457340dcc4273405c40073009fc067700144005f009ec005f0017c005d009da0030000000000000c004b400c100b248841001640085003444481407640ac10033403c100f3413c90030400dd21d2400cd8033400cd01012032000000000000040003401e100da401
81005c601a10178421a10070441e100784) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (11e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (b7952ec00bf052fc00af002fc00bf0027c149f053f8009f0827c809f002fa81900000000000008006fc20130004404133004c04150104c04138106c045301076001f0007c041b2005c00130007c001f0017c00170004001b00000000000004004340081002161485002141481452151481052045
48105234008d00234148d10204018500274008d00234408d002020100000000000000200634009144345009101a42009580244008160260089102274009d00274009900254009105274009d002740095006420180000000000000020074009100214099500e5c00910065400b110244418541e74009d002740e9d0
0244019500634809d02274009d04662803) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1200) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (027c00930063200500000000000006007360095063500491102644091102764a9d00244249500274029505274809d80274409162244009d0025400914125081c00000000000004005b4008505204028101244228506224008d10226428d80a34008d10234018d00224248100204008d002340081
402102160000000000000c0063440110005400110806d071301c7c0b1d05c44425701874001720074001d00074011185445001d0005c0011000708180000000000000e2067c0092002cc01b200acc43870128c07950427c04bf01aec009d0027c00ad0027882b7002cc00bf802fc0093002ba0190000000000000e
a067c009f252ac80bf252bc34af0527c54) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1220) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0070420d55076400cc0030582c901f3620cc2030407c51030403400277400cd0043400c900c0203000000000000000000340052201cc0171001840071001cc0059001440371445f4405d00154217d00144097b001f40041205f44051049d2100000000000000040043c40131006c02134104c801
b1004c001f9006c1a1300078201f3004c001f0004c40131887c801b0007c00190005001000000000000004014fc009b5027c008f4026c809700278008f0067c01970027c859f0067c259f0027c009b1027c209f0025c009f04250013000000000000040417c009540a0087930024c00971026c029f0227c018f06e
6c009f0027c429f8027c00914024c009d0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1240) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (8501b15bb4505e10003400e10459101500000000000004200bc21db0374401b4106c809d90064c09f1027bc41de0a47841ff827cc01df207cd011b037cd01c7004bc01fb4a41a002000000000000042043c00d74024c005f1037c48d10007c9afb223dc40930007c00db2837c001f2037d007f00
27c00db0023c00df0805a814000000000000000053c01e3407dc01a3807cc11e7807ac05ed0178081ab005fc01ef0078401ef0878c8173087fc01ef005bc01eb10481030000000000000002813420e900ab402010418000ed0418504c92138420c9004b400ed00394112d003861169003b600e5044b400e1200808
00000000000000002043400c10471500c1) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1260) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (07c00df0026c0cdb1017c00df0097c00ff0035c00df00c7c80df0037c22172035c80192035c00df0007c00df010500090000000000000c2003400d30134c83130030c00f10004c00f3813f401dd00d7401df0034500dd8036c005b02b6c00c70003c00db00c5201000000000000004210b480c50
472403010032540c94006440c920774018d8007012cc23f04100d80320005518e6440c10023400c100012042000000000000040523400e1123c400e1003c480c10028400e0013f440ac318b404ed02384002d023a40061a73a404e5000b400e90309094c00000000000004085744dc70172d06414372c21cb105ac
0cdb0173c1dcc21c341ded017840127003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1280) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (5adb29b7c04170035406530206400df0087c02df41060041000000000000008043404c90021408851211408c50110400c501b1404810a03400c500364180d083151c810023404c90083402c102000030000000000000008007460d900040015120a6400c18004440d19034481950047400d10037
414150035411910066600dd0047400dd0604200100000000000008828f400d10261c03952015c00dd1384480d50037c85c10045c00d500334011d00344231100c5480d10067400d100c22283000000000000042205a00f3401ec0043803cc00f30004c40e3003cc00f3400fc00fb003f001d7003cc0073001ce00f
f400fc80ff206d00890000000000000400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (12a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000e804f450cd24004000d0005400cd8030502010013400090806000992033490c1083260c010800040892821500cd0032a0100000000000000c200f404d10114408130507c01dd0074406850057421d10045401f10277400c500344005b0046c00110034400dd0077180100000000
00000e000fc01fb000cc24370044c01ff007cc0633005bc013b0048c00ab093fc01fb007dd0c39000ec00330068c00f7187fa003000000000000066007c02f72029c04ff0113c0cfc0a0f804ff60b7c1c3f088dc00df24b7c443f803ec003f010dc12f7002fc00ff030fa86100000000000008000fc08db0684c80
1105b6404f38104c08f301b46469700874) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (12c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (5b0930400db0034453d902b9428d90074405dd0034413d100b4403fd0034a21300000000000004200dc30d32004c02770004c00df1034c06371014c21d30085c109f0234c00db0134c004f00a2c049b1125c0cdf08350803000000000000060017c00fb0017c09af000fc10ff003fc007f025fc4
0f7004dc02f3103fc00ff003dc005f407fc42d7002ec00ff003d80050000000000000e2003800df0044c115f00c5c00cf0834c02130017c00db00825008a0037c00d30033c041102c44009b4021c00d70036a80000000000000006200f400d50074500110047000dd0034484950037000d12606420dd0037400d50
036400910414500898035480dd0035a003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (12e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (024e00df0037a81000000000000006600ac00cf0337c44df6122c0ccf023fc04df0036c40cf0217c02ff023fc00fa003dc00bf013ec64f3003ed10ff023d2202000000000000004049c0dc30340e30970363c1dcf0170c00470111401010331400cf1030c10cd0432c000d0031d008f0921cc0df
0a72101200000000000002001d401e1000a405ed002d404ed8178425e980d9407f9005c581e90079401ed007a621ec01684052d007d401ed007808060000000000000a009d400c10004400850423442cd0030502519011400090830502cd0030401cd00724008d00014000d10a0401dd0032200300000000000002
004c407d10136c009f0000c03dd0034450) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1300) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (005ac005f1816c0373045bc096f005fc005f8016c005f0016c057b019dd02774014c005f0017a0170000000000000c204b400d1027440bcd0032500cd0032410c5002140bc90373400c50032600cd0036401c901b1489d50830500cd00332036000000000000040007401e100584416d146e401e
5107a411a1c05f401ed806b401ed037a401ed887a40169007140185106c401cd0079000400000000000006204f400e1001c600c50028480ed1038400c10019c40ec000ac80c70138400f7003ac00e60038c00e10028424ed003988330000000000000e0057c00d00004e01730024c00df1034d00b30012c00d7002
6c02df0034c21d70834c81932014c20970) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1320) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (34d48105224148100214148d002028140000000000000200604009900274089980b76009d0024410c920a44009d10276009144276009900274109100264029d02204109d0024a01c000000000000080006c029101274019b10e54048d00244239140a6c059d80264088102a74009908664009100
244039100a54029d002628010000000000000c2040c24930027c019302248029f0824ca89b0164c059f8025c01970863c009b00e6c00930024c059f0024c008f002500100000000000000c004bc021f0087c04170005c021f0005c001840854821f0006c021f0805d00170007c021740008861a0087c001f000580
1200000000000006205fc0053105cd037f) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1340) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (73401110641c871510414001d0004c09110017420170005080110285c011d0146c0b1b000540f1d0044401171007001c0000000000000e0063c02b3006cc87b3002ec00af0025449b9402f800a9002fc11af006fc00bf022cc07b14164d83bf003fc11bf002728190000000000000e6067c14970
53fc14bf0529c008f0027c14bf082fc80af002dc40bf0827894970526c14a7002dc54bf052b8949f0027a0190000000000000ac070c001b4107c841b0007c201f20044241b1004c801d0005c44160907c001b0007404134106d041f0014c041f0006b01d000000000000008042400c905234348900276008d00205
148100264208d0022614c0052360089002) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1360) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (20070304c801f0004c021b0084c021f1406c101f0005001000000000000004005fc009f4063c509780e7c009f0025c008f0027c009f0125c809f0021c009f0427c01870063c019f10a7c00970025801300000000000004a017c009302a4c809e8026c208f0025c009a00e78409b80a7c009f0027
e009f0026c40920124c129f0067c0097002520050000000000000620634009100254009d00254009da0244209001264009180265009100254809d00264069901244048d082440095002528180000000000000e804b40481002048c8d04266008d20214808180274008920674008508234148d00224048180a04048
d052341085002128120000000000000c20) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1380) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000004053c01a30078e41f54038c012f0078c01e30078401670079401a71078c01ff0078c01c30070c01ff407ed017f00780011000000000000020013400a1043a400e500d84102d00384000d809c401fd1438400e180310016d0039600a94038400e540584026d0038800100000000
00000a0053400410072402c40072402cd8030406c954b0481c51070413c51030608cd00f0603c110305c3cd00b2403dd0032a0140000000000000000534117100def12710098c427d00144027d00586087900504077120dd44a7d049d41871001441875001c4007d0014a014000000000000042053c00130404c00
030104d101f0005c00130085d08130005d) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (13a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (4500c04030d0871441c5000364009080740a1100f22000108505405d08312016000000000000040000404ad000848425850e5002d883a40061020e61021833e418e1003b500a4102b4086504384047102384002d00390008000000000000062056c05830670c0d25014844f0d003040135255840
54f0378401e501086c62d001b680a1003ac05e10018c206d037118150000000000000e0008c4123006cc45730068c013f027cc09f3126ec89a3007ac05d3007ce01b7027fc01f3087c809cb00dac013f00752002000000000000066043c009f403dc009b503fc801f0037c00d60022c209b1037c00de20374405d2
035c00930037d009f0097c207e0035a810) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (13c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (4556581d003420010000000000000800045188704a74111340654011d00344819110674459c8037c011d04d6443910266c019d00344131100c14421d003420850000000000000c2280c00bf007fc0013002c8083f003cc19b614efc103f007fc209f0017c01f3003cc13f70034c01f3000dc013f
103f08050000000000000c0007c009b000dd185e001dc021f0835c000f0097c00d78136c009f08244c29f0027c009c0037c00570097c021f283500090000000000000620d0c009f4254c00570076c800f0036d07d30042c031321f6801830027c00d70037c00d7c2f4e05d34c54c001f1035a8140000000000000c
201a4008500104220500464000d0032402) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (13e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (024ec299b0074c00bf004cc411f1006c01ff004f401db013fc01d33048c011b000ec01f34077a0030000000000000e6017c04970107c001f6105c000f093f808130203c041f2227c88ff100ec803b000fc803f203cc003b500f0002f013f8005000000000000084000c149f0503c001b1005c1c1
f1034d001d0107c141d1125c44df0017c00434024c0017083651013000dc001f01b6900100000000000000004040c8503034104104934040d12304000d001740c4d0022440cd00026000500024008900324240500156200d04b028100000000000000a00044009d01074015901356401d0034400d900874081c092
4411dd08676085100344009508364a4810) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1400) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (dc80ff080fc01ff0051d40f7403d80050000000000000e0003c00dd0836c01930287c099f0034603df09c4c031b01c6c20df0847c00db0037c00d14055c0a1b0056c20db0037a82000000000000006000f420dc0036408d500044101500354019c2044600110047420dd1077600d188374a0dd04
47450510626400d90035a8030000000000000e8043400cd00324509121076005d00304008d0000440190002400cd0013400c90633480c148054000920100c0c90033a0130000000000000c0007481dd00744449501004041100756009d1044401110007400dd0856401d121b5c00df0047401510004001d1107708
030000000000000e200fc01df0074d41f3) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1420) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (18405e90078401e1007b40dad007a409a5004b401a1004a601e5015a641ed007b405e10ecf44561006b409ed0178800700000000000000200c402cd003040c8101434088d10734008d04c3422010002400c10682400cd00b7440c90043083010023400cd0032a00700000000000002084c408d30
0344018100330010d04b34011f0847403c10044100d50024400dd02bf420d150c3401510457400cd0030a00300000000000004000cc00df0035c00d340b7c025f0436c035f0007c04930044800d30006c00de0037c00d20817c0e134097c00df00350803000000000000060017c00ff003dd00ff003ec003b203fc
10ef000fd08b31003c00ff002ec00ff103) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1440) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01ed0079401ed107b441e10059401291078401e10079000100000000000006004f400ed003b400ad983ac00b180394a0ed003b400ad100b400ed0038400ed203b400eb080b400210038c00e1403988130000000000000e0043c00df0037c00df9004c00930075c20df0026c201f0847c00df0027
c00cf0037400d10037c00534034d01c34073a81500000000000004400bc08e7023fc08bf0a3fc083f093f840bf083fe00bd003dc08df0831c08cf003fc28db001fc007f001f680df003db002000000000000006048d05cf0071d0cd307b38854f0872c428d0673c1b834262809d30272c01cd0033e2dcb0003c0d0
30033ec0cf017010120000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1460) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000042043c009f8024c01932624c019e0064c048300e7c009b0124c409310a4c019f0064c009b0024c00920163c00970826001000000000000004284bc001f8007c001f8007cc01f0085c031f2807c221f0107c201f0085c001f1087c001f00c7c12170005c001f0007021200000000
00000400dfca05f0017c007f80dec01734015c417c029f4507f009f4405f21ddc204d8017c00530c1dc876b001cc00530815a0170000000000000c205b400cd2033421cd00f6401418033448cd00b3430cd82d7000cc04b0400cd0833400d90053403490370400c110332012000000000000040013401ed007b443
ad047a40361007c401cd047b4a1ed803b4) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1480) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (b7002fc80b9152fe409f002fc009f0527c009f002bd00bb252bc009f002790190000000000000ae073c001f0004c00130004c001700048441ba007c201f010442a110004c001d0114c2a1b0004c00172107c00170006b01d0000000000000080434008d002060095002260095003141489c02764
08505207008500254008d0d22400810030400d505234008d0020201000000000000002006340295202460a9108a44009512244009900274009510244009104344049d02244009902244019550274009d0024a8180000000000000000074029d00244038140a6c088700e54059701a348e9110244008500614019d0
0a6c009110204019140274409d00262201) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (14a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (127800930827a8050000000000000420634009d20244888120206109d00270829101274109500274009d2427400910027400950125500990127440910025881800000000000006804b4008d20204008100234008d20224028100234208140a34008d182340081002244481002040099022744081
0023a8120000000000000c00634001d1004500134005c051d00056c61b00174801109876011d00074001100874051500144005141c7400114006001c0000000000000e8073c00bf8026c00b3002ae02bf002c606b3002fc00b701afc429f002fc00b3056fc0297002cc00b2036fc00b3002fa0190000000000000e
4077c009f1027d14bb053fc94b7002bc14) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (14c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01704008d0173640cd80f3688c10073400cd0473481c50271400c10113401014033600cd0032a0140000000000000000434087d00145827b00dcc005f845c4807d885b42171201f4007d119f42051401f4005b409b41161115b4005d0010a014000000000000042053c001e0004c00130086c821
f0004821140107cc21300078201f0007c00130045400130085c03120007c001f0005081400000000000004205fc009f8027c01970225c009f2025c488f0067c049b4267c009f08a7c809f0023c009f0026c09970027c409f00258217000000000000040817e809c0024c019128a740b9f0826400914067c839704a
36609d00e7c60924026c009700244029b0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (14e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (8c05f5817840d210178405ed2179881500000000000004201bc011f0077c01d30277c25bf027f40d5e0074c09cf0077841ff007fc09bf005cc09f38354c01ad4074d21ef027fa002000000000000064043c00df0037c009f2037c169f0006d00990807c001d0027c00df0037820db1017c00df00
13c40df0027800df3035aa10000000000000046053e016f2078c01f30878d01fd007bc01ff005bc01a1407f401ed107bc81e7007dc03e3004bc0163106fc81ef087800150000000000000200134106d0038410e9843c641e51039410ed00bb020a000ab40ced003b410e5003b400e8203b400a1003b400ed103880
050000000000000a0043401cd0030410c1) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1500) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (17c009c0037c82d710b5c04de20a7c201c0825c061c0027820de0137c00df2885c00df21a7c039f0227c00df003700090000000000000600534001f0837424d942b78039d0027c91990966c051f0826c00fd0067400df0004000f304e0c021300f4900db1035a81400000000000004000b4200d0
0334410900030038d00234001d00026024d00a3000dd0083400cd8002580c500f0402410424480cd10332806000000000000040003408ad083b400e9063b404ed203b44469011a608ed062a404ed962b444e90008404e1222c440a13128404e902390018000000000000042057407ad007b40161014fc10ed002b4
452d014054ded116b425cd0353441ad081) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1520) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (04df8305c8ede1007c28d30837c0c530127c00df0336b00100000000000000a0434044d11305000d1001402c500a56000801004001910a0406cd08134008d0003404c10023400050122404cd013020100000000000000a2007401dd00344008d85344008100644111d10644911d00274c0dd0465
4009d0447400d100e7411d10027400dd0034a001000000000000080a05c031d00344121fa0455009501e14019d00444010d0064400dd00d7400dd00c7480d11047403d52827400dd08362201000000000000080203c00bf003cc0577004d400f3182cc20bd100cc203f04aec80f7000fc40ff300d440f3401fc10f
300afc00ff083f08010000000000000c00) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1540) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000068041400cd0033400cd0032414c500304000900234209d80134008d000340005201040009042341001000000001083500130000000000000c2004401dd0077401dd0074400d100354011100354019d0847401dd0077404db0d34480db1137404d18034504110277000300000000
00000e800cd01ff007fc01ff0074c01db027cc012b007ec01af004fc013f004fc0933004cc0133004fc0133004cc0833113fa9030000000000000c2015c7cfe1b3fc0837220fc00bf002fc083f040fc083f022fc48df0307c0cdf000fc06df022bc0c5f022b802df0337b005000000000000084003c025f0334c04
1f0904c02f300a44001f0504d081d0027c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1560) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1110f4404dd00a70811d00b74939d046641a1d00874129d0134418d1003ca01700000000000004200fc00df0037c00df0034c00d30874c001b0485c049f0297c04df1406e045f0096c00df0137c045f0084c00874035080f000000000000040296c00ff003fc00ff003dc00f3003fc003f411fc0
9bf082fc80bf003fc20bf003fc203f002fc00bb003fc025f00350881000000000000042201c00df0037c40df0036c00d70034c190b0497c008f0057c005f0347c52570004c00db0017c12510244d0313403521800000000000000e200d440dd0037400dd8036400c500314001100254009d04676005d0036480d90
420500d90013400d540b4500d100352803) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1580) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (034c00df0035201000000000000006600bc00df0037c00ff003dc00df0037c0037002fc009f003fc007f000fc207f000ec00fe201f4007f000ec00ff0035380200000000000000404bc08cf0033c00c70370c01d12034c00030535c048f0133c048f04334088f0033c000b0023c008f0031c0043
0030001200000000000002001b401ed807b401ed007a401e1007a441210078401ed004b401ed004b4016d125b401ed007b4896d0049501a10078000b0000000000000a001f600cd0033400c50030400c10430492014075403cd044300a0d00f34018d01234011900034038d01f5401010034201300000000000000
084f400cd0037400dd003441bd180b6c00) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (15a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0017c00530014c1367441cc014f00dfc014f0017c055b0014c235b0154e05530014c037f0017a00300000000000000204b400cd0033400cd0033400c58032406c500b0508cd02b34800d000140111000040e0d0044401010000500dd00312012000000000000040003401ed007b401ed007b401e
1007840125105c401ad007b601ed007b401e90078421ed0078401e10078401cd0279000000000000000004204f400ed003b400ed003b400e5003ac00211038480ed003b400ad0009c0023001c4002d0028400310008400ed01790013000000000000040053c00df0037c00df0037c00d30074c00130030c00cf003
7c005f0037c20d34064c00db0014d01d30) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (15c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (8400a9302b400a100284148d052020100000000000000000634009d00274009d00274009d0225400911024400950525480bd042d400bd002e400a9022d400b142a8400dd002420180000000000000800074009d00274009d00274089d80244109511204029110604129d00e54129d06e45049110
674429100e44109d102628030000000000000c2043c009f0027c009f0027c819f0025c00930164c00972065c649f00a48009f0024c059b0067c00930064c009f002500100000000000000c004bc001f0007c001f0007c001f0007c201b0187c001f040740a3f088fce03f000fd023f000fc003f400fc181f000500
1200000000000006201fc005f0017c005f) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (15e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (734001d0007c001d0007401170145c001120444201d1007440170005005110947495010945c051b414400701128710180000000000000e2063c00bf0027c409f0027c68bf002cc00b3402cc20bf282ec00bf002cc00b300afc00b300acc02b300acc11b30167a8190000000000000ee067c009e0
027c009f0027c949f0527c00af052f840bf002fc209f0027c149f0527c14970527c149f0527c14bf0027b8190000000000000a407bc001f0007c001f0007c001d0001c00130004d00170005c003f0005c001f2004c000b0007c00530000d041f0104001b0000000000000080434008d00234008d00234018d00604
00952024440c10024480ad8029400ad002) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1600) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (02170304c00130006c00131304c50130204c001f0005081000000000000006005fc009f00254009f0027c00970027c019f0026e009f0027c00970027d009f4127c209f4024d40970027c809f00210813000000000000048417c009f0027c209f0027c209f2826c189301a5d019f0ca6c629f0024
c80930027c80930124c00930024d1093082521050000000000000600634409d00274209d00274009500256809111254819d0127402958024420810023420910021480892020428815025a01c0000000000000e804b4008d80234008d00234008d04224008104214008d00226008d00206508100234008100204008
1002045081002100160000000000000c20) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1620) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000004043c01ef007bc01ed007b84163105dc816f107ec0167207bc41ef007ac01fb107ec01e3806ec81f3207cc016d00780014000000000000000013400ed003b400ed103b410e5004a4007d0038410a1007b400e9007a400ad0018481e1003a400610038400ad0038080400000000
0000002053680cd0033400cd0033404c181f140dc94034403c501b340ecd80b2500c904b0408c14032402c10170401cd103020100000000000000208134005d00174405d001740275009c40361001c50161001f00071101c4717f009c42a7100dc51173409c4107d00140000000000000000040053c001f0007c00
1f0007c40132205c02172006c04170207c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1640) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0d83445008d03c36110d01424820509004810d00824440102804065900332802000000000000040003400ed003b640ed00384002100084003d0039400ad102b4806d043b000ed10184c2ed00084006100180206130390008000000000000062157400ed083ac00ed037bc00710009400211238c0
0ad019b400ed003b41ca70718500fda61ac98a1002c110eb003900950000000000000e000bc01ff007f809ff0074c0133012cc0133007fc01af007fc09ff007fc09ff227cc01ff805cc01f3007cc01f3027f2802000000000000046043c80df0037c00df0037c20bf001dc00430007c008b0033c00970001c00171
827d001f0025c00570037d001d00352810) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1660) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (2354189d1034a00100000000000000821f400dd0037400dd0036c101908c6c031100050119d0056c031d04456025d02674001920174095104c44811c00342183000000000000042203c00ff003fc00ff803cc053d002cc1033083cc00bf000fe00b7802cc09ff083dc00ff027fc00b30028c01df
00350881000000000000040007c00df0036c00df0037c803f000fc00130037c039f00b7c001f0027c465f1007c02df0197c005f5417e821f00350021000000000000042043c00df0037400df0034c00930034c040f00b5e208f1067c869e20e7c835f00e4c04df00f4c03930074c41d3003528180000000000000c
200b400cd0030400cd0033400010001401) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1680) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (024cc20ff004ac00134060c341b0077c00fb010dc2433003cc81ff1104c1037040442433012fa0030000000000000ee017c00ff003fc00ff053fc043a000fc002f000bc40bf100ec003f000fc003f000fc403b000fc0037000ed203f003fb90100000000000000c003c00df0037c00dd00b4c021
d1000c00130034c009f00074005700154009f0015c801f00274000b0005c009f00360001000000000000008053480cd0033600cd04324420908024000140314008d10114004d00114000d00034000900034008900054000d28300010000000000000020007400dd0037400dd00344000d06044031100344019d006
7403dd10554020d20274981d2427400990) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (16a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (dd00f71000c403f246fc003f103d00850000000000000e2200d00db21c2c031221c0c00df00c68090ba035c000b2037c00df0045c031f0034840c70085c00170064c29130265280800000000000004000c4a0dd0057461140054400d500c4402110135500d40033420d100464010d0034400d152
06400510206440914005a803000000000000048040400c99916480018104422dd08014000920250000d2033410cd8f014400d0032480d50a01481450000408811203a013000000000000046004401d50005423150104443f70064401130034422100037424d10084408112074c21d100c44031100c6c031100e708
030000000000000e0a0cc01d300c4c541b) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (16c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1b415ed0f5840969015e541e1027f42529427c40d6d097b00de9005848929017b415e90179495812b5040d4d0358800f00000000000008000f401cd08d04000d0000402c162914080910210210d00f3400c100416000c00f3400c108b04818100905014d0002a00300000000000002004f400cd0
014c04454196c01e10006c0151003040edc02b7400fb00854009d24fb40bd1000500b51542040c9d0390201b00000000000004200fc00df0c34c02530414c44d10404c02530025c005f0237800db2b06d02170437c00d30484c00430024c008f00150803000000000000060017c40f6000d00057100fd40d7000f4
0017207ec04bb203fc00f70001c0013003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (16e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01ed105b411610978401f94079601c10070441c5007d020100000000000004604f400e5001940061001840ce500184a0e10038000cd2038502ef0038400e180b8420e38038480a1003ac006100198813000000000000040043c00d34054c20030014d0ac32010c00074030c01df0034d01df0004
d00570074d20d01035c20934034c20570007a01500000000000006080bc08df0015e8c77811b688df0a36e08b7083fc20df2237c00f7003dc005f033fc00d711bfc00df001fcc0ff003db00200000000000008404be05cf2050d014f9020e10c30201e050b0a616039f2373405c34351406470233c05c34570c85c
11150c05cf01f010160000000000000820) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1700) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000042043c019f0164c01930024c85936024c41832027c019300a7c009700a4c009f00a4d019310e0c08830222c00830067081000000000000006004bc001f0085c001f0205c00170187c881f0087c8a1f0007c001f0c07c001b6007c0217000fc023f008fc003f0283001200000000
00000e201fc0053001ef0063405ec00690018c407304184017f0814c005d001fe23710814c00430015d00510294c60550055a81700000000000000005b480c5013341bc10176400cd1810404c11070610cd0034440c500b4406d10030400c14030440c11032480c100332816000000000000040013401e1007a401
71007a401f9004850170207c541ed00784) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1720) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (bf052f814bf0527c1c8b052fc14af0221cc0af0023c409f9027c009f002bb01900000000000008c07fc801f0002c04134004c04110004c04110007664170007c00178104c041e0006c0013410dc84134116c84130116101c0000000000000020434008d002061491002041491002451481682741
4814023444850521454890122420854529414a10529414a1552000100000000000000200734409d0026408d100256009102a441891002740a9500a74809500b44409d002640891083d400b1002e408b1012420180000000000000800074099f0124c019106e45509100644009104a74039100a74009500e5540990
0244139500255519100254119110262001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1740) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0244029310a7a8050000000000000000634009c01256009506264009901374449102244089100234009100262049d002640099c024441910824420991125a81800000000000004004b4008d00206008110276c28d00234028104244048180234148918204008d10224809d023040285022040381
0223a0320000000000000c20734001d0005500150007c401d0007402134004444504507c091340045001102045001b00845001b00844001b0097081c0000000000000e2067c00af082cd00b7002ec25af002bc04b3002ac02b3002fc0593002cc0093486cc00b5116cc25b7016ce05b3016fa0180000000000000e
8867c0096052fd00bf252bc009f002fc00) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1760) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (40f0481c10033443c181304c2cd0172400cd0175400cc08b340cc90030525012060401010062a0140000000000000200504017b285c54073039ac1171049f093738098d857f01dc4007d105c4207d009e40371001c41175045c4107500dc2004000000000000040050c08174004c02130087c000
30007c001b0004cc41f0004d001f0006c021f0107840133046c00030844d01134481081400000000000006004fc809b0426c099f00274209f0c67c30970065c008f0825c20970225c41930021d009f0027d009f1023d808f002500170000000000000e0017c009f0464c938108e6c409f04a7c10914064d0091002
7c00990924c068f00264408f0020401950) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1780) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (a00d01110ac1501011ac588d01618811000000000000040008c09b3007cc41e32378d01e3026cc21ab0050c093f007cc0ddf0a74e0bff127ec81b50849481b3016cc0d3f006fa002000000000000060143c00db8005c00df10071805e0027c001100158801f0005c00df0024d0edf0027c401740
07c40df0027c005f0035b810000000000000084044c61a7307ec01e3007dc0163406bc01214058c01fd106a641ef0879e05ed087b401a94062c01630848c01a30040101c000000000000082004401ad047a400c1003a48061006b400a9143842065000a601cd3429404cd083a400290008400850000400c500a880
040000000000000c2050400c100b2409c0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (17a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (25c00df0037d009f0097c429f0027c409f00b5c18570086c80df1605c00df2034c001f0403c049f1413c12cf209700010000000000000e2052c009100b4143c301d4500c100a64919140764215f0014d00ff8066c00ff0034c00914424d031141764011f0415a81400000000000004005b400850
4800118500a04000501404400132174010d2805440d00043610cd00027000100c24414108824024d00232806000000000000040022408f1003c410b1013c40431002e40a21001e408bd000848ced220a404ed02384c021100840c80032a4c48d02290000000000000000046155401f5033c400e5223840565056fc
00aa40594053f0049401c70361405cd021) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (17c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (40dd2084c1cef18374081b0084c14db0234c029f0516100000000000000000a0436068d01815009d1022410890123600010101410054400404c90101424c9001341009400054c0540117004d0b100010000000000000020007408dd0084400dd2424403d10067410154184411110084440dd0064
400cd0037444190004403d900e4401dd005400010000000000000802174019d02c54209f0087c011b00634001540f5c43150004400dd04c5500d900274121b10444015540554135d01d62001000000000000042017c00ff103cc03f7049cc0073002fc8536007cc4023220cf00ff802d480fc003fc00bb016cc00e
30034c80bf002f08800000000000000600) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (17e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000068043420c100274004100034804104124241d0011401110037400450133482c100b1402450030406cd0133400c1083500130000000000000c20074019500474011100474149101204001d0044424110103401110047417d130b6c025d0034412f12935cc1d10077000300000000
00000e800fc01b3004fc0133004fc0133004cc092f004cc0923424fc0133c24fc00f3003cc047f007cc00fb123fc01f3007fa9030000000000000e0017c82df0007e50b7202fc001f00a74043f618dc041a0107c98ef070fc00df100fc000b450fc445e101fc147f1117b8050000000000000ac007c029f0584c00
970024c00130027c0a172284c2e110a844) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1800) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (8901544054100f34085100345009b2334400570434400f1003f400dd0034201700000000000004200fc00df0027c02534004c80534054c809f0014c10530237c405b0034c02d300b3c007f0035c00f70037c00df0835080f000000000000040217c00bf004fc003f400fc00bf002dc00bf000ed0
07f000fc803b000fc009f2036c027f003fd00fb003dc00ff003d0881000000000000042213c12930207c00130247c00130006c009f1085c20530007c02150003c42d310b5c005f0034c00db0037e00d3403520800000000000000e200f400d50027402510007400d140324011d1015400110037400550037411d10
5374105d0034400c50031400d100350803) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1820) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (037c00df0035281000000000000006600bc017f003fc08ff023bc00ff003fc087b033fc08b7003fe20f7003be847f022cc007f083fc02df003fc00df0035380200000000000000405bc004f0033c00c38070c00510010c004f0230c008b0033c00ca0030c40cb0023c004f0031c80d70037c00cd
0030001200000000000002011b4012d005b401a1007c511a100684817d0168601b9004b449a1904c44569007b4014502f8401e1007b401ed0078008b0000000000000a010f4000d00134008120304100101004804d01601028904c3402890000400c920f24005d0071600c50033400cd0036a01300000000000000
014f400dd0023400510000400d18034400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1840) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0014c80530014d00530014c005f0014c005f0014c057b001dc05730016c005b0017c005f0015280300000000000004204b400490030400cd0030500c50034400d10030500cd0030400cd1034401d14031412914032400c18033400dd0031201200000000000004000340169007c401fd00784017
10058481e1007c401ed0078441fd2078401e1005940161007a401e90173401ed0079000000000000000004204f4002b0018400ad0038400a5202c400e10828400fd1008400ad0008500c1083d400b1003ad06c308bb400ed00391013000000000000060053c00130054c018f0034c00030004c00d38064c00df000
4c019f0004c00db0015c00530036c02fb0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1860) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (34148110216148505224009d00202810000000000000028063400bd002f400bd203c408a1402e408bd103c420a1002f410f180244209102244409100214009100224009d002420180000000000000800074009d00274009d00244009100244069d0166c099101a34089500244009300e78409101
a54009500244009d102420010000000000000c2043c009f0027c009f2024e01930124c019f1124c81930027c01950024c00933464c00930225c00830024c009f002508100000000000000c004bc003f0007c001f0007c021f0007c031f4087c001f0087d001f0007c811f0002c001f0007c001f0007c001f000500
1200000000000006201fc005b0014d005f) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1880) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (734001d00074001140074050501474251140044251101444001501504031100c45031305444071101c74801d000500180000000000000e8063c009f0027c0093402bc20b3002fc00b3002cc00f300adc00b700a4d0993817cc2193002cd159b0de7c009f0027a8190000000000000e6067c009f0
023c009f0027d149f0525c149f2022c149f6527c008f0527c14b7052ec94bf4527c149d0525c009f0027881900000000000008c07bc003f0007c001f0004400530006c000f0004c00130007c00130004c44134104404130001c04130106d001d0004001b000000000000000043400ad002b400ad0028400a1006a5
00ad002a400a1002f480a5002851481053) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (18a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00130084c40131004c401f0404c001f0007c001f0005001000000000000004005fc019f2027c00970827c009f0027c109f2267c00930527c099700e7c00970022c008f0027c008f8023c009f00258013000000000000042017c009f01a7c009b0027c00930027c00930024c009f0465c009f0020
c00930065c009b0024c009b0027c009f002500050000000000000620634049d0027404990027401d50063400d108241008d40244809900244008941354009100204009100274009d0025201c0000000000000c004b4008d00234008908234508104234108108204308d01214008d01244068107214368940204508
900234408d002120160000000000000c20) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (18c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000004053c01ef005bc01e30078c41eda058d01370069c01b3405c401a303fad0dc3007e001ff0078c15f3a07fc01ef00790010000000000000000013400ed001b400e1003e0016d0028411e5043f420210408410b5813b404e1003b440ed003a404f5003b400ed0038000000000000
0000000453480cd0013400c10030403cd00b0480c58071406c10034404810032400c10132000cd02f0400c14033400cd003228100000000000000000134005d001f400510012c067d8e1c40071001ac027100dc40265001d40051411d0005d101ec005108174005d2014a100000000000000042053c001f0007c00
134004c901f0004c20130844c00130004c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (18e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (8d0033400050003400010036401d14083418c10006400d10037400cd00332002000000000000040000400fd001b400e1013a402e0008f480a5003b4002d003b40021003a420e10029400e1003a400e9003b400ed0039001c000000000000062255400ed0819c00e34172c0531200bc0ceb001b40
82f0009c02e1403ac04e1401ac00e3421ec00e1003b408ed003910150000000000000e0008c01ff005fc01f34870c091b026bc09f3107fc017f007fc01f3087cc11f3007dc11f3007ec01fb047fc01ff107d2902000000000000046043c20df0017c00df8037c003f000fc003b5022c003f000fd000f0035e26df0
035c20df0027c0cf304bfc00df00353814) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1900) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (037400dd1034200100000000000000020f400d10012c00cb00344000101804031d01a74071b8045402010035400d30005400d140c5400d50037420dd00342183000000000000042203c00f3001cc00ff003cc0533010cc013f003fc00f3104cc0032403cc00f300dcc00d300dcd00f30037c00ff
003d08a1000000000000040807c04df0015c00d70037c023700adc023b0087c023f200d802df0037c10df40a2c40c700b7c00ff003fc40df20350801000000000000002050c04df0017c00d34036c00930017c00170017c00dd0027c00d3003ec04f30235c00f30036c00fb003fc00df003520200000000000000c
2019483cd0011400c10032400010003400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1920) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (226cc0123000cc01230056c003b080dcc11f0106c0c332a0cc0123404dc34bb0008c013f005ba0030000000000000e4017c00ef101dc00f3003fc023f000fc003f003bc0037800fc003b003dc00f7000fc00ff400fc00ff003fc00ff003fb901000000000000084003c00d30014d00df20b4c001
30004d00170037400d14034c00170038c40e30000c00d10004c00e3003fc00dd00360001000000000000000043440c10012400d904b06041188044004d0013400090001400c51033600c14001400c10001600c50033400cd00300010000000000000000007400d14014400dd0034400110014404450077404d1113
0408d50034400d10034440d10424400d12) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1940) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (2d0037000fc80bb003fc007f007d80070000000000000e2008c01df0027c00db0020403112044c08110056c011300c1c030d80c7c011204c5c031300c5c009b08e4c411b02b7a80200000000000006200c4249d2037600dd0064630d5807740091404441119084440a1d00654011900654011944
471445500f45015d0025a8030000000000000c80404009d0033604c981245840110204408100060200100016009d820360c094901400091001500090020400190013a0100000000000000c20044019d0076404d50126c101580474011110148011310044011d0584406190124400192003c4281207c4015d084708
0100000000000006800cc01af007fc09f3) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1960) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1a401bd0279405e9027c4053d035840135405e4013d014b00520104b40569907a50535804b509a10078433e1004c80060000000000000a001e4018d0033603c910204121d02c04440114506810d00424230100c340219a1234021150c74009140f2401010012a00700000000000002004c408cd0
035c0bdb1635433d710d4400c50022c009d10454021104e70021100256031506c4400d104f44030100c4a01300000000000004200cd089f0027408d30016c021f0404c01930024e0a1b8084c069b4487c00170084c05174006c009301b2c005301a5080300000000000006001fd00ff043ec00f7003fcc9ff0019c
213b001dd0027500ec003f0026c1037000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1980) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01ada02b441e90039491b10058401a904704117900fd000300000000000006204d400e10039400f1403d400e5201b480eb201ac80690018c802d003b400e1001c400251008d00e50438400a1082988130000000000000e0054c00c30024c00d30026c00cb0003c00130016401134055c811f0067
c00530815cc0010806c009b5134c20434073a015000000000000064809c08bf083fc24ff0a39c00f7003fc08bf900a0007e101d00867203fc0073103dc00bf4024d08770837c00ec400db80200000000000000404ac018f0173c40cb0230d05cd0060c2e8344404015d05428158100e3c050b4023405874003c050
30032c2603041010120000000000000200) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (19a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000c2040c05930064c24912024c24930220e119940a7c00932023c02940025e08830061c00930026d00830824c009e026708100000000000000c004bc021f0085c02130104410140187c021f0046c20121407c001f0407408170487c401f1007c001f0087c00170007001200000000
000006205cc0173005ac0058015ac0177005ec0173001d42b77415fc4a7f045fc0179011dc0173405cc107b4258d006b021da8170000000000000c2049480c14273000c900f3409c52013448d980374c8cd0070402cd0077433c980b0400d50230453c540f04018900e3281200000000000004000c411e1006e401
f9285b401f5044a401a12469001ed001b4) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (19c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (bb253f440ab053bc20ab052fc14b7052fc14bf052dc54af002f000bf003fb81900000000000008c070d00130004d00170004c00110114400570003404114107c00110105404110115400534012c04130114c001d0006b01c00000000000000804240081002340089c024600c505224009d406141
4c50523400c185204148d15204808100205148105204009d202020100000000000000200604009102244008581a44209100246009500276849101376009100a5402d18025424d140265409102245039d88b4a018000000000000080006c11814467c069b00a45438f0026c0a9b0067c229100674039102e4402970
2e4401910260c009140644819d00260001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (19e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (060d019f00e7a8050000000000000620604009d00354a0910123400d52025480918024640918867440910024420d100a76209158244229100744009d0065a8180000000000000c80404009d00236008508214408500a16009124204038985224008100206408102234808100644249100a47009d
0023a0100000000000000c20706001d0005c00114007c001a0094c405b4104502114087400514014500111087405510d444811100144001d0007081c000000000000068060d00af002fe00b3002dc20b3112ee00b1002ec00b8042ac00a1082c420b3016fc08a3002cc0293106cd00bf002ba01800000000000006
c067c00bf002bc149b852fc14bf002f800) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1a00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00f2420cc842340ac504b7401412034601cd1037412d10072401c500f0400c140d2500c14042a01400000000000002005140361001dca171229c42b7a101f4036f009f40071401c40271009f4037146dc43071045d50061505c542610a9ca014000000000000042050c00130407c241100044201
f8087c841f2007c401b0004c1a178407c02130006c06170404c00130384c041300050814000000000000060057c859f0025c009f0027d049b2166d009f0067c049f2027c039f2027c009f4023c219f0227c029f0027c039f002580150000000000000a20140009c0027400974425c0785402140b910ae6c438b002
6c00930264c32910027c4b931060d00934) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1a20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (84270b2248508c10178501ed003988150000000000000e0800c81f3027cc01f2107cc01fa024fc29f7015cc0173407cc090f0277c0157017dc2193215c423f7026cc094f007fa000000000000000064043c00db0031c00570025c00db0017c409d4587c00971027d40170007c205f0015c009f00
83d00df0025c008f0035b010000000000000004055c4163107bc81eb407ec01fd004bc81a7105f401e30078c81ed107bc01e1007ed01a70258c01f34062c01e300581015000000000000020015400e5007f410e900ba110e5800b440ed201b49061002870139801340261001a401b1000d40ce1101a410f1044880
050000000000000a005145ac50033401c9) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1a40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (07c029f0067800df0095c005f0057ca29f0007c825b0427cc81f0087c081f0087caa9f0087c08df2331c005f08b70001000000000000062054400930065500d80374c22510017403994c20c00514876622df0407c48970045c00912004d01f70016c130f0165a8150000000000000c2011401c58
0314800500c74008500104100110004058502246120d20c34430d0080480091004400c10012402cd00032804000000000000042000414b1803d400e90018408e1800b488a9821c598a0013a400bd011b408241109408310088400e54002404fd00290000000000000000060055407d5087540dbf003bc108f0003c
1d2f235800d4b0362c072c035b4254d041) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1a60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0e9f0187c0c17000742015250ac02f30004c001f0006b0000000000000000080404028d00a34000988014008110134100120004444900a74040d1c034440d9003498010100440c151307101d001020100000000000000200044009d0867490510a25408d12115403910044481512077400dd0047
4011500c7481151006400c100244019d00148001000000000000080a0440a8d1075c821f01c4c00054117401116444c870b00274401d04c74211d00474219b04c4460d10ad45111d04e620810000000000000c2200d00bf001dc09b3203cd10b3101382033002ce0073002fc04fe1c0fce03f140f4c0b700cec00f
3007cc103f053f08800000000000000c00) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1a80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000e8043400cd00a04028d0033400cd00324044d28324840d00334028d00234000d4016410091001404010101404010513a0100000000000000c200740b1d20d44035d0077c01df0034400dd004440acd1077403b70067401d100604001104004941b0104480110017080100000000
00000e000fc007f000cc003f007ec01ff007cc09ff007cc083f007fc01bf006fc0133004cc0133104cc013338ccc8333005ba0030000000000000e2017c029f0035c081f000cd04af011fc201e14018580d0123c023f0d0fc0c3f200fc042f6007d34ef0097c203f000fb8050000000000000a8000e409f14b7e04
132001c8a932295c4013148c5065125274) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1aa0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (dd003440a5d0137411bd04a740ad10037401d500e70019d0067001910074a01300000000000004200fc08ff002cc02af0036c00d30037c065f04b4c023f0137c009f00a7c00130217c05d30167c019f0067c019b0075080300000000000006001fc003e001fc04ff003fc00ff003dc01bf000d88
0ff003fc00bf00efc00f3402dc00f7226ec09bf126e889bf083d80070000000000000e200bc015e0084c031f0036400dd0036d0a9f1036d101f0037c609f0067c001d8006d00db4065d01934065d01934037a80200000000000006200f4089d0474402dd0035400d500364105d02864000d0037400950027400dd0
032400190005400190005400110015a803) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ac0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (034c00df0037a01500000000000006600bc00ff003fc80ff0237c08ff003fc08ff0207c00bf003fc00bf005fc08f7003fc0037011fc087f021fc0877001db80200000000000000404bc00cf0020c008f0172c01c34037c10cf0430c040f0833c008f0093c080b0013c000b0013c004f0013c004b
0010101200000000000002001b4012d00584014d017b401e1007b401ed0078501ed007b449ad005b401e140ef4012d015b4016d005b40169405880060000000000000a001f4024d08004800d0033400c10033403dd00704000d00b36048d21534880900034021900974045d0017400590016a00700000000000002
004f4091d2014400dd0037400d10037403) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ae0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0017c00530014d4273225cd31732014c20570017c005f0017c07534094d82536094d825f0095a8170000000000000c2048506814030503cd0033400c10034447cd0230400c900336008d0013400cd0033401c10030400d50030400cd0033281200000000000004000c401c120604018d007b401e
1007840125007c401210079401a5005b4012d005b441e10078401e10078401ed0079000300000000000006204c4002100184006d003b400e1003c400ef0038400cb003ac028d001b400ed002b400e10038480e10038400ed003988130000000000000e0054c01530854c005f8037c00d34034c01930074c0133007
4c14970016c001f0007c00d30074c00d30) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1b00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (d401ad0069401a50069401ad00302010000000000000020063410dd04244109c00274409100274029c00274009d00240019d006f401b1006d400ad002c400b10028400ad0024a0180000000000000800074029d20a54029c00274009100274009c10e5c039d02641009d08274009140204029d00
a54439500a54039d02e620010000000000000c2043c009f0024c009f0027400930027c009e1127c029f0024c009f0027c409b00240009f0024c04930024c049f002708100000000000000c004bc001f0047c000f2007c201f0007c081b1087c001f00068800f000fc001f0007c101f0407c101a0407c101f040700
1200000000000006205cc0673001cc0c7f) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1b20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (704083d000442a1d00044001b00054451b00045091300044003d00074001d00004151a10474050105445011b0047081c0000000000000e0060c01970076c019f0024d00b30024c20b30028c09bf082ec918f0026c009f0026c00b300afc08b3002cc02b300aba0180000000000000e6067c00bf0
02fc00bf0027c009f4567c14bf0029c14ff0023800bf0027c009f0026c149f0527c149f0527c149f0527b8190000000000000ac073c041f0104c041f0007800130007c000f0017c041f0014c041f000fc001300055001f0800c00030000c000f0806b01c000000000000008043414890d214148d10234008100230
008d1021414cd00204948d002b400a1002) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1b40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (003f000fc0033000cc00130204c001f0005c041304050814000000000000060057d018f8265c009e0027c009f0027c009b0167402872024c008f0027c009f0425c009b0027c009b2427c009f002580150000000000000e2014c029780e6c0a9f0024c009340254048f00e4c209f0025d009f0027
e009f0024d009f0027c00972024c00930027a805000000000000062060408bd002e6009d00244009900254049d00a4400901027600bd002f400bd006c4008d0023400910020600890025a8180000000000000e8040441ad0a6a401ad0020400814021414dd08244008d0021400a9002b400ad00284008d01234008
54020604814023a0100000000000000c20) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1b60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000004054d01c34050d014f087be01e301fcc01630059c01ff08584016d085b4a161005bc0173005cc016f0059c016b005810150000000000000200144026108f8402ed0039480e9013b400f50038400690038400fd203b400e1407f400a58029481ad042b400a900a8800500000000
00000a0050401410070401cd0033400c10034400c03031611cc00704000d0003452010003404c00070404cc00f1482c92076a0140000000000000200504005100144005d0015c204b0015c007601d841079011c4005c029742051001550474001d4047c00df40271005ca014000000000000042050c00330004c00
0f0007c00134004c00110404d001f0106d) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1b80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (5900b24070140336008501c24200d8001400c10032400c90033400dd00132804000000000000040003401ad00084000d013b400e1003a40021003a40021002b40061003c402fd88b9400e10018400e9003b400ed001902000000000000000620574182d0328508ad0373400c5003c400eb022840
021023b400e52218c086d0119400e1003ec00fb003f400ad011988150000000000000e0003c013f026cc01bf007fc01f3487cc01b70078c0133027b04133006cc01af006cc01f3007cc01f3007fc01ff005fa000000000000000066043c00df0015c805f0037c00df0035c006f0037d00fb0035c409f0827c009f0
025c009f0027c00df0007c00574015b810) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ba0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0b4402dd0094a001000000000000080207400dd00144005d0037400db00344011c0294409dd10154121d0024400810027409dd0235400d90035500dd001620810000000000000c2203c00ff001cc007f003fc00f3003cc053f041cc00d7009cc00ef001cc0073001fc017f007cc407d013cc05ff
001e08800000000000000c0007c105f0077c05cf0037c00df0035c08bb0085c082f0017c825f0035c00df0037c00df0037c009f2037002df00070001000000000000062057c435f0a74c03df8037c00d3003ec43130126c41930027c00930184c051f0001c00d30034c00db0037c00df0015a8150000000000000c
20134208d00804000d0033440c51036412) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1bc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (100ec01b3903f4413708cec0133004ec001f2806c011f000cc0011000cc0033105cf61db007fa0030000000000000e6017c00bf000fc003f0237c04ff003fc003f003f0003f003fc003f000bc003f000f800ff003fc00fb203fc00ff001fb8050000000000000ac003c009f0004c001f0237c08d
30034c000f0034800170024c00dd0034c00d30037c00cf0034c00df0034c00df001430000000000000000080434000d00204008d0033400c940304018d00206000d00714004d0010400510017400cd0031400c90031400cd201020100000000000000200074001c00245009d0037400d100344001c08b46001d002
44009d0024400910027400dd00b4400cd8) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1be0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (7c001b001fd417f601fcb0ff003d80050000000000000e0213c005f0035c0303002690a1140b6c851741c6c03130043c011f00c6e001704c4c01170144c015318d0400cf0037a80800000000000004001f4805d08354119502344009122a7481100124423010c444111d04644069d00445111500
44024d10464600dd0035a8030000000000000480434044901314041100020008115224200121260000100034400d0202404010200408058000480810034620dd0033a0130000000000000c40074005d20354001522940009180374011110044801100444001d00844101d00c4403110000400510044401dd007708
0300000000000006020fc096f027cc0333) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1c00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (184097c087b4812d004a401a1027b4152c214840121014a40d21016b40561004a4152943c9509ed0168405ed0078800f00000000000000000c4004d0cb34810d00c64109500134430d08c04070500824021500834021100834110912074108d0012401cd0032a00700000000000002004c5245d2
0374a59d04b64409102bf4011d20705049124c6002d10127402d10485403800014424dd20a4401dd2034a01300000000000004200cc005f0037c001f0126c00971037c101f0426c00130486c119701a7826530105c02130087c008f0c76c00df0035080b000000000000062017c007f003fc10bf005fcc0bf0033c
203f200fc403f600ec007f0007c81ff200) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1c20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01cd0078501fd00fb401690050401ed0059401ed0079000100000000000004404c420610038480ad000ac00a140384002b002c4206100284006d0038000ed081b400610018400fd0028400ed00398813000000000000040050d81430074c009f0024c00830235c21014004c001b0004d009f3024
c818f0017c005b3004d00df0025c01df0037a01500000000000000000bc007f023fc08ff203fc00bf203fc003f0025c083f000bc001f1227c00ff003dc00f7210ec20ff020dc08ef003db8020000000000000060588054f0173c018f0012c02870823c850f0d60c01170142c05070143c01c24013c094b0343c009
f0172c15cf003010120000000000000028) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1c40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000042043c059f0164c109e0024c00934027c10930424c01930064c159f0027c08930067c00910964c058f0067c089f0027081000000000000004204be001f0087d001e0807c0a1f0102c021f0006462170005c021f0307c001f0c07c8a170907d221f34868021f0007001200000000
000004001cc00730014c047f001cc0371101dc9071005dd287b045ac117f009cc087f005fc217b2098c007f049dc005f0015a817000000000000040048400411030402dd84b2404d00030443c102b1623d82132403cd0070409cd10b3405c90030400cd0841400cd2033281200000000000000000060171207c401
ed0078001b180fd401212079403e9804e6) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1c60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (bf052fc14ee402bc14bf052fc54bf002fc00bb052fc34bf002fc00af0027b8190000000000000ae07bc001f2014c001f0104c00130107c00130004c00130004d041f0107c00110107c04170104c041f1005c801f2006b01d00000000000000a0534008d00215008d052140085052340089102542
08110246148d05234018125234348545204148d08234008d002020100000000000000200734009d08244109d00a44449102254019100a44269108244809d24254009148a7400950024510dd01a54109d0024a0180000000000000000074079d00a54289d00a54059500674059b02e15009103244058d02e7403910
2e34189100644019d20e74009d00262001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1c80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (067c009f0027a805000000000000040063400dd00274009100e6506991027420d126324248100274029100274049d0025404992424504dd16274809d0025a81800000000000004004b4008d00234208100a06049965334008180216008500234868111334008d00604408908a0406cd00234008d
0023a0120000000000000c40634801d084740051458400015a3c7400114002c841100074241101074005d20044001105c44035d10074001d0007081c0000000000000e0073c00bf022fc00b30068c02b7012fc00b0002dc28b3402fc06b300afcc0bf002cd00b3217cc07ff002fc00bf0027a0190000000000000e
2077c54bf052ac14af052fc14bf052bc00) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ca0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00f4420c90437403c111b2400c14170413c114b4403cd0073401c140734024d0233401cd0032a0140000000000000000404007d005c40273001d4047a001f4107700dc42b71211842271909c4007d081f41071205c4287d029f4817d0014a014000000000000002040c001d0044c00130c064001
74087c04130284c08130004c42132884c041f0607021130407d021f0087c081f0005081400000000000004204fc809f9027c099f0025c00970127c239f0027c419f10e7c449f1027c019f0226c00874063c408f0027c009f00258017000000000000040017c009f8027c029318a4c01890127833930065d0297202
7c02934367c239f00a44049b02e4c009f0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1cc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (b42da107204016102134006d00398815000000000000040418c21d3b247c0173006fc01910364d21b3207cc41d22344401ef007fc49db026ec21d31aecc29d3227b841ff007fa002000000000000062041c00de0017c001f2005c00db0837c009f00355145f2003c801f1007c005f0007c409f41
97d00fd2037c801f0035b810000000000000086042d01ff0078901334078c01fb0073cc1a3087ac01f10048d01314078d017d005bc21e3007fc01cf084bc016f00781015000000000000082802443ed00386036100a9400e9103b400a5003a5006100086836100104116d903b400a124084006d201b4006c003880
050000000000000c0042411cd0230413c1) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ce0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (17c009f0037c0a5f00a2c029f0237c021f0287c025f1407c80570007c461a0087c001f1007d42df1047c005f003700010000000000000a0050c00910037c0153046740291089448d100234c33d15044c27dd04474009f2007c22934064c05d330e6800df0035a81c000000000000040008400910
01740601008140ec101c04010140c04000100404120d018742b050083412012424400c100934800c00332806000000000000040000400b1011b44021000b400e11b28400b10108400e107085443d801a4082d020b404214028484e1403a4006d003900180000000000000440545098b006340401022ac41a1004ac
080b2374c015b0040405272a4b40561020) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1d00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (041501878001f0005c0c1708a8c04df00a7c081f1036b00100000000000000a0405028501234020100234048901134000d018070255630040c0505c34100d20034040520204508d00034000d003020100000000000000a00044019d20074011100a7401950a974211d0134400d5044544a153047
4511d0405401954064441dd02274009d0034a001000000000000080214403152007411110247407db40e74039d1044424c100c04611108474031d00c7411110854403dd24874811d00362001000000000000042210c0033826fc00330447c4077004bc00bb083cc12f5000dc0126800fc803f0507c00b0003cd00c
f043fc057f003f08010000000000000620) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1d20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000040043400c14032400490033400c102024088100b3400810030420910501440cd0033400c50130400c10022400cd0033a0100000000000000c6407401d30034400010077401d1006440111004440b150075434810020400dd023b401d10034414c10247401dd0077000100000000
00000e000fc01fb007ec007b0077c01f3001cc04f3013cc40f3007cc01b3002cc09ff137fc41f3027cc41fb100ec01ff007fa0030000000000000e2017c08ab040f4003f000fc02ff808fc04290207c0c7b120bc0c1b0007c103f200fc0c3b052fc00ff050fc043f003fb805000000000000006000c069b1403c02
130007c00570003c089b1184c22f72085c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1d40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (51227440151013050a91067545ad1003f400dc0034480d10027000dd0034a01300000000000004200fc00d30034c10df0037c00d70184c08930004c529f0134c089300b5c00d34437c00db0074c11d30033c00df00350803000000000000040217400f7043f5003f003fc00ff0121d002f0038c0
129003fc023f003ed00ff003fc00fb003fc80f70007c40ff003d8805000000000000042213c80d30032c009b0037c00d21096c53d30606c03d30034cc0030075c00df0037c00d60034c00d30016c00df0037a00400000000000006001f400d90034400510037400d100b640851800740a5540354009100f5400cd0
037400d50034400d10467400dd0035a807) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1d60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (037c00df0037a01400000000000006200bc00ff023fd087f0237c00db021fc00f7800dc00ff103bc00bf003f020fd423fc00ff003fc00f7001fc00ff003d380200000000000008404bc00c30234c084f2073c00c74420c000b3032c840f0030c88c32030c80d30033c00cf0030c00cb0003c00cf
0030181600000000000008201b401e102785092d047b401e50048401890042401810078401a10079509e1047b401ed0078401e9005b401ed0078000600000000000008000f400c100b04005d0073440c100f05054942b25094900b0401c100b4100c12033400cc2034402d90003000cd0030200300000000000000
004f400d141b45045d0033400d10074401) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1d80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0017800530017c82530614c045f0017c007b009cc00524017c005f0017c005f005fc005f001520170000000000000c0048400c140344015d0033400c1422358f0100405020d00334138104b4400c94033400cd0033400cd0073400cd00332832000000000000040000401e10078411cd007b401e
1105b481e10078501ed007b401e10070401e1027b401ed007b401ed047b401ed0079000000000000000004604c400e100384002d003b400e102004008100304008d003b400614038500eb0d3b420ed083b420ed003b400ed10398033000000000000040050d01c31034c009f0037c00d301b4c0053c004c005f003
7c005b0834c80d301b7c00df0037c00df0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1da0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (34008d00234018d05234008d002020100000000000000200734409106244009d002740091042c610b8012c4909906264008101a44068110274009d00674009d00274009d0024a0180000000000000800074009140a44009d00274009100a44029128644039140605069140e45039500274009d10
274009d00274009d00262001000000000000042043c00930024c089f0027c00935020d00934024d458b0024c05930024c00930027c009f0027c009f0027c009f0025081000000000000006004bc001f4007c101f0007c001f040c4002f000bc103f0007c4a1f4007c001f0003c001f0007c001f0047c001f000508
120000000000000e201cc00534014d027f) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1dc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (7340013404444301000740011008c420134004400190004c213b0bc04051b01474001d0045c011d00874001d000700180000000000000e0063c00b3002ce11b3482fc00930564d11934464d1197102cc02930374c08930267c009f00afc02bf0167c009f0027a01c0000000000000e2067c009f4
527c14bf0027c009f0027c00d70027c009f4025c14bf052fc149f0527c009f0527c149f002fc009f0027b81d00000000000000407bc40130000d041f0007c4013010cc041b0104d041b0006c00130104c00030103c801f0007c001f0107c001f0006b81c00000000000000a0534008140204148d00234008105284
14a90528414a10022400810d2040085452) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1de0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0233008ed4033000fc001f0007c101f0085c001f0005081400000000000006004fc00970425c049f0027c009f4266f20834023503830027c199b0123c009f0023c009f0025c009f0027c009f002508170000000000000e2417c00934026501930023c00930165808972024c80970022d03970064
c00930027c009f0027c009f01a7c009f0025200500000000000004006340091002240091002740091002d400b501ac402bd0024410ed40ac400a900274009d00254009d00274009d0025281800000000000004004b400810522414810023400811029400a50028400ad0023404a50028500a100ab4008d01234048
d00a34008d002100120000000000000c60) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1e00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000004043c0163404ec01af0069801e30061c01870050c01cf0058501e3087ac21f3005fc01ef007bc216f0079c01ed007818140000000000000020034006100184002d0039440e10439410e50038400ed0428402710838400e5002b400ed002b400ad003b400ed0038800400000000
0000000053400410092401dd0021400c140411810560005000d0170401810000400010193400cd0033401cd0033400cd0032a01000000000000002001340071001c5047d001dc005100544015100144005d001c4025140144005740974005d00174127d00174005d00142010000000000000042043c40132004c81
1f0007c00130008c0233000cc003f0004d) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1e20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0100a1402090000400190005400110004400cd00334004d0031400cd00312802000000000000040000400690008402b1012b400e10038484e10210400f10018420f10239408e9003b400ed003b4006d003b400ed0039000000000000000004205442061009ec4021017b405e10328418a1043941
8eb0018c04ab4439400e30009c00ed002b4086d0639c00ed00390015000000000000042408d0173005cc01e3406fc09f3025cc0d73004cc0133004cc0371004cc8133007fc01ff007fc01ff007fc01ff007da006000000000000042143c005f0587e001f0035c00df0016c005b2027c001f0027c020f0007c00174
027c00df0037c009f0037c00df0035b810) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1e40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (037400dd0036a00100000000000000021f4005100354061d0037600d100144005100844001104e05025b2004400110077400d90067401990037400dd00362081000000000000042213c0073002cc00bf007fc00f30020d00834038d00f3003dc01b3003cc00f30007c00ff002dc007f083fc00ff
003f0880000000000000042007c00570097c011f0037c00df0137c44df4117c04cf00b7c48df0c37c00df0037c00df0027c009f0835000df00370805000000000000040050c005b4034c00c34037c00d344c4d031300e4c03130024d00130085c201b0007c00df0037c00df0077c20df0035a01400000000000004
2018400490002400010033400c100c0402) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1e60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (004dd00b3012cc4937884c4013f0047c013b0049c00df050ec80db050c40113005fc01ff007f80030000000000000e2017c0067003fc40ff0333c00df000fc003f000fc003f000bc006f000fc8037001fc00fb002fc003b003fc00ff003fb8250000000000000a4003c0053002cc00df00b7400d
34034c20d30034c00c30015d00930030c00c30027c00df0025c001d0037c00df0036180000000000000000a043400494031400dd01b3410c10020400812810400c14010500c90030400c90013400c90023400090033400cd003000300000000000000a8007400510130401dd0237400d120144005000a440011004
4404110004400114227400dd01354049d0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1e80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (5c00fb0053c0477013fc00ff003d80050000000000000e2203c24550277c20030000c03170271c01050043c010e0145c310b0045400df0146c00df0104c01432177c00df0037a80000000000000004000f4009590265025986154015490855031420474119d9234401112045200dd1044400d101
04410910037600dd0035a0070000000000000400434000502236080100104025502116200508034001d0001420110005400c50000600cd0800020810033000cc1033a0100000000000000c60074019b80644019100444039110c44041100454011d0045401110047c01f900c4400e100c4401134077401dd007718
010000000000000e000fc1033802cc243a) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ea0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (194016c0069621ad00db501ed625f42125824e401ad197e405f1026f449e10058409e1004a401e1027b401ed007a080600000000000008008f4000d00234004d20034008c80130010540834000c2800481010641409c10080600d10083408c90033400cd0032200300000000000002004dc03dd0
0218045d00040004000174041000840089b00b540391205280bf504a4c00f08236441d14173400dd2034a01300000000000004200fc38571067c821f0084c025b10f7c001b0384c219723b4c44930006c00c70404c00d30206c02db0837a80df00350803000000000000060017c02fb003dc29b7004ec003b001ec
003b000cd003f084dc00bf000fc00db100) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ec0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (41ed004e449ed0458445c9105b441e1607d401e50079000000000000000004607c4006700384808d000ac00614018400bb1008400ed083b420e12828404cf001840ced801b400e1003b400ed00399013000000000000040040c011f1034c015f0004000130010c00930006c009d1037e00160001
805dd0016c00d90817000db0031400df0037a01400000000000006200bc00ff003fc08ff101cc00e2021bc00330029d80e31239c80ff023ec02ff003df30fe002e400ff003bc00ff003da8020000000000000840dbc008f0233c00cf0103c068f42134000701e34040f0340d11d32841c45c34200c2dc14003c0dc
b0033400cf023210120000000000000820) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1ee0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000042043c009f0027c009f2026c20930824d199b4124c009d2827c019b0065c00970022c009300e4c019b0067c009f0025081000000000000006004bc00170007c001f0107c04190107c001f0285c501d1007c06170007d821f0485c000e0407c0a170007c001f0005801200000000
00000e201cc107f0154d007f045e4226780d8c1171005ac467f01dfc007f0418c005d005ed4058315b400630019c005f0017a817000000000000040048501cd0070400cd00a05004500d0542c80070401cd04b3402c90070400c580b2400cd20f3401c10363200cd003320160000000000000402104018d0078421
ed084a401051458481a1006e401ad007b4) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1f00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (bf002ac00af002fc00bf082dc009f002fc1497902fd00bf002fc009f002798190000000000000ac077c041f0107c041f0006d04121104c001b0005d001e0007c001b2005c04170106c04134104c001b40074001f0006a01d00000000000000a0534148d95634148d002041490052440091002544
08d80224008190374348105226148905244009100234008d002020140000000000000200734109d80274009d20666309140244009900254089d10e74049909374489502266809120244029902274009d0024801c0000000000000800074029d00274809d00244029120244018101a44818d2067407910067e06911
127d009b006440b9100674409d00262001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1f20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (163c809f0027a805000000000000040063400b5002c403b9022d400b1802c4009100a74509d2237404b1022f600bd00a44008d80264009902274009d8025201800000000000004004b401a50229400a90029402b100a85108580234208d0021400a5882f400ad00214008d00634008900274008d
002100120000000000000c60734003108846001100046801100044051b80074801108076003900074001d00044001d80044005900074001d0007181c0000000000000e0067c11930964c11934021e05930164c20b3802ac00bb002dc009f0027c009f082f4409f802dc20a2002fc009e002780190000000000000e
2067c00bf002fc00bf002fd00bf002fc14) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1f40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00090212d0489400511073440cc0ab36020de080402050072600c40070708490273400c50032a0140000000000000200114805d0015c0051001000441001441053405b6637d10db40351215440751001ec005d04dc40261105f4005d0014a014000000000000042040c003d0007c00171006c021
34085c201b2107c001f0187c1a130006c00171046c80160904c021b0087c80170005081000000000000006004fc009b00e3c40870026c249f0963c029f1127c10930027c019f0427c109f0025c409f0025c10974067c009f002580130000000000000e2017c029640255019904e5424924124c219540678299f042
5c069e08234009e8027c809d20a7c00930) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1f60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (8401fd014b404a1036b405ed0039181500000000000004000fc01ff004fc013b2049c216f306dc017f025f8093f007fc01f60878a01f9007fc53ff0067c41f64067409ff007d2002000000000000062042c001f0035c005f0034d20800017c00570007c009f0007c00d30011c005b1033c06df28
07c00d74823c00df0035b810000000000000084044d010f006bc012f0059c01af2049c0173005b401af006be01ef2078c41e5007ac85e71078c01eb006bc01e700781011000000000000082025483a8001b40061002d4003d001050069043f410ad083a400ed903c721c500fa400cd001840079802b400ed003880
010000000000000800506018d080b4002d) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1f80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (27c059f0016c00df0027c011f0215c00df0895c409f0105c84530aa7d029d0007c00df1807c005f2027c00df203700090000000000000e205bc039f0007c019b00414010f1003c40dd003742a9f21e7c01dd0234400da8cf7c00fe14678405348e3c40df2035a81400000000000000001b4004d0
032418450470400cd08b26095d08034008d0001403c90030480cc0000400cc00034008003a3200cd003120060000000000000400234006d002b40021001d400fd002b4002d081b0882d002b4106d402c404b90289400ed01ab400e1212b400ed00390018000000000000046057428ed201a4006d26285086d02384
007d0713c38ad0209c2081207060ded803) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1fa0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0adf12b6c06cd0007c0eff0105c22934125c24dd0036b00100000000000000a043000c50013400c98024400510035620c900074a08d8002420c90930402c58001420cd8103422810423440cd00302810000000000000020007400d50007400950804400510824400d140074801d0064446dd0416
4145d0537480cd00c5400d14025400dd0034a001000000000000080217400110033406db00354009100154279304434019d0047481d90075401df0045400dd2047400910027440dd00362085000000000000042037c0032402fc00b1001cc00b3440ec05b3009f802bf002ee01bd023ec21ef083e000ff002fc09b
3012fc00ff003f08050000000000000600) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1fc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000048043400cd0033400cd0033400cd1113404cd0130404dd08304008d00334084d02034020d80b15809d8033408c10033a0130000000000000c2007401dd0077401dd0077401dd0577485dd0074411dd027c4009d1077441d70045c011700e44019d0077401910037080300000000
000006800fc01ff007fc01ff007fc01ff004fc033f024cd013f017ec01ff005fc003f010fc043f002cc01ef003fc0033007fa0030000000000000e0017c007a003fc00ff003ff00fe083f820b7050fc40bf090fc003f2207c061f000f44cdf0a0fc00bf002bc28df003fa0050000000000000ac007c00570027c00
970014c00d30024c00930087c001d0226c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (1fe0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1d08044001d003c401970077412dd0037400d30036c009d003f480dd0034a01300000000000004200fc00df0037c00df0037c00df0037c40df0036c00df1035c029f00b7c00df00a7c00530036c009f0037c029f0035080b000000000000040217c00ff003fc00ff003fc00ff001fc80ff003fc8
0cf003dc20bb027fc4577003dc0176000ec02bd003fc00ff003d800d000000000000042203c00df0037c00df0037c00df0027c001f0004c001f0034d028d0037c015f0027c005f04c5c008f2037c8693003788040000000000000e200f400dd0037400dd0037400dd00274001d20045001d00344909d0037400dd0
1874049d00754009d0037400d100358803) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2000) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (234c001f0037a01500000000000006400bc00ff003fc00ff003fc00ff002fc083f000fc203f803fc08b7003fc00ff003f880ff421bc00bf003fc80ff203db80200000000000000404bc00cf0033e00cf0033c00cd0013c00cf0232c08cf9031d109f80b3c000f0033c00830002c008d0033c00cf
0030101600000000000002001b401ed007b401ed007b401ed227b401ed2078441fd00784012d067b609ed005b60161405e501bd007b401ad007880070000000000000a001f400cd0033400cd0033400cd00034400d00024000d00304114d00724110d0012480810002000cc00336000d0036a00300000000000000
004f400dd0037400dd0037400dd0007480) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2020) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0017c005b0094c005f0017c00530014c007b00dac1073005ec1073029bc015f0016c027f0015a81700000000000004204b400cd0033400cd1033400c901004000d0003420010030540992062583c14170501c140936888d0032501cd00332812000000000000040003401ed007b401ed007b401e
90078401ed0079401e10378401b900fe401c10060401810043401ad817a4838d0079000100000000000004204f400ed003b400ed003b400eb0018400fd083b400e1413040021803844061001840061801b400ad0838420ed00398813000000000000040053c00df0037c00df0037c00d30064d011f0807c0013053
4c00030034c01530046c81930007c00df0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2040) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (3414890d274008d95206148d002020100000000000000000634009d00274009d00274009d082f400bd002f400b108244009150274109d0427410d904274009d10245109d082480180000000000000800074009d00274009d00274009d00274009d00274009100244019100674029d00a7c029b00
a74009d00244029d002620010000000000000c2043c009f0027c009f0027c009f0027c409f0027c00930020c05930227c009f0025c009b0027c009f0024c009f002708100000000000000c004bc001f0007c001f0007c001f000fcc03f000fc803f0007c08174405c041f0207c001f00074001f0005c100f000700
1200000000000006201fc005f0017c005f) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2060) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (734001d00074001d00074001105444015100544015d00074051d2005c823d00874021100845001b12874021d0107081c0000000000000e2063c009f0027c009f0027c00931024c00930224c009f0467c02bf002fc059f0067c01930064c00830127c119f0027a0180000000000000e6067c009f0
027c009f0027c009f0527c149f2527c149f0027c14bf202bc00bf002dc00bf002fc80bf0027c00bf0527981900000000000008407bc001f0007c001f0007c001f000bc001f0007c20130104c00130807c841f0105c041b0107c001f0104c041f0006b01c0000000000000000434008d00234008d00234008d002b4
00ad002b400a145205008180236148d052) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2080) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (001f0044c00330004c00130084c01130004c401f0005081400000000000006205fc809f0027c009f0027c009f4027d20974027d009f0027c009f0065c039f0027c009f0127c009f0023c009f002500170000000000000e0417c009f0027c009f0027c00930024c009b0024c009f0027c129f0067
c039f00a7c029140e4c89830027c0b9f002528050000000000000620634009d00274409d00274009100604018908604218d2027404dd2125400bd002f400b100ac400b9002f4009d0025a8180000000000000e804b4008d00234008d00234008100204108901204148d00234008d0063409ad00eb403a100bc400b
1803b401ad0523a0120000000000000c20) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (20a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000004053c01ef007bc01ef007bc01e3027fc0de3037cc09f70078c01ff0058d010b4060d018b4068c21230048d018f01781014000000000000000013400ed003b400ed003b400e1003b408e1223840ce500704816d0418403a900c860321500c4403100004032d0138800400000000
0000000053400cd0033400cd0033400c14033400c14030500c10030406cd00504018900484012900084002100084012d0032a0140000000000000200134005d00174005d00174005100174005100144005500144027d005c4405100144005100104005300144805d00140014000000000000042053c201f2007c00
1f0007c00130007c00130004c00170004d) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (20c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (dd00b5402d500334010d00734004d0033402c1003044881a013410cd00372806000000000000040003400ed003b400ed003b400ed0038400e10038400ed003a4007d04bb4086d003b400e10038600a1881b400ed00390000000000000000062257420ed003b400ed003b400ed06394b8e5063bc1
8e708394106d023b400ed001b40061001840ca1011b4006d003988150000000000000e000bc01ff007fc01ff007fc01ff047cc01fb007cc01ff007cc017f007fc01ff005fc21730058c09b3005fc017f047fa002000000000000046043c00df0037c00df0037c00df0137c22df08b7c04df0037c003f0017c00170
027e009f0023d001f6007c009f0035b810) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (20e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (037400510036a00100000000000000020f400dd0037600dd0037c00d50036c00db0836c00da00354015100764001900274009100244405110274009500362001000000000000042203c00ff003dc00ff003fc00f3003cc00f3003cc00f3003cc00f3003fc103f002fc10b3002cc007b002fc00b3
003f0880000000000000040007c00df0037c00df1037c00df0137c00d70137c04db0031c425f0037c019f0047c011f0047c005f0027c011f00370001000000000000042053c00df0037c80df0037c00df00fcc03f300fc403ff0036c00cf0063c419f2047c81130040c01430023c031f003da8140000000000000c
201b400cd0033400cd0033400cd00b5404) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2100) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (004c80033024fc0130412c4013f004e4013f007fc21f3000fc40250047c003b0077c01ff007fa0030000000000000e6017c00ff003fc00ff003fc00ff003fc00ff003fc00ff003fc006b003e4a07b003fc00ff003ec00ef003bc00ff003fb8050000000000000a4003c00df0035c00df0037400d
3003cc00e30038c00e30034400d300274005d0037400d14034c80d30037c00d300361000000000000000008043400cd0033400cd1031400c50032400c98832400c90031400510877400cd0013400410015400c1007340045003000100000000000000a8007400dd0037000dd0037400d10034400d00034400d1003
4401d10067400dd0017200510014401d10) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2120) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (bc00bb08afc001f003fc00ff003d80050000000000000e2003400d34066c911d10444031100c7c18130064c011f0446c071f0037c00d10147c03172043c031b0037c20df0037a80000000000000006200f400d104054011d00454611510414201100756c19d00474044d0037400d100474111504
17601910037420dd0035a8070000000000000ea043400c100024001d00004100100034000102200108d8000440050031400c12801480052005480090033400cd0833a0130000000000000c0007401d1402440a0d10054c4150805c211105854040d10454005d0037401d18007401110007400110033401dd107708
070000000000000e000fc01f3006ec003f) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2140) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1b401e10a684496d08584116d024b40129124a6092d004840971207b401e90178485a1007c409a10a7b405ed0078800f0000000000000a001f400c100244010d00004004d02c34010900267001d1281483090032400cd0001413010001601050137400cd0032a01700000000000002004f400d14
8244104d10444011d00074021b007440d9d2064487512037400d700244009102b4510910477400dd0034a01b00000000000004200fc20d30024c045f0206c021f0487cc0120624c209f0106c101b0036c00dd942584a9300b6c00970037c00df0035080300000000000006001fc00ff00eec007f000fc000f000fc
103f0017c003f100dc007f003fc00ff102) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2160) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (43a5007b441e10078403cd007a401c1007c401ed0079000100000000000006204f400e1403850061401a400a1000b400210019400ed003a80020083f400e1403c400ed0038400e10038500ed003988130000000000000e0057c40d30820c40120047c00960047c80130034c011e0004c00170037
e00d90044c015f0016c80d30034c01cf0037a01100000000000006200bc00ff002fc007f001dc007c000fc007f1a3d408bf001dc00ee003fc80f7813fc08ff0039e00ff2a3fc00ff083db00200000000000000004bc00c30424d004f1000d084f00a3c300b4a32c888f8a01d008b0076c01cd0031cc5c32061c804
70173c05cd023010120000000000000200) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2180) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000c2043c009300a48019f00254099b00a4c009340e6c92970064c00930025c209f0227c01930026c01930027c009f002708100000000000000c004bc001f0006c041f1086c10135007c121b0287c801f0887c001f4007c80170407c101f0007c041f0007c001f0007001200000000
000006205fc0053035c80273009fc427900dfc1175505c4437f10dc601650017c004b001c5017e105ec86730014c005f0015a8170000000000000c204b400c100b0482d124b3049c90b33403c5003500acd14f0501c12037400c100b0402cc16b4402d10034400cd0033281200000000000004000f401e1007c411
61004b401a9106f40165a078641fd00c86) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (21a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (bf052f614af002f414bd4527c809f052fe80bf052fc94bf052bc009f0027b8190000000000000ac077c00130015c041f0005c841b0004c00111102480170804c800308054001f0107c04130006c04130007c001f0006b01c0000000000000080434008900274148d00216148d103240091052340
08180244009120204008d05234148100204148100634008d002020100000000000000200634009110254009d0875500dd00244049100a6442d511245319100254009d04274069102a6408d100674009d0024a0180000000000000800074009b00a2c089d01e44008d00e6c048100e76019121a04039100244009d0
0674039140a44019140274009d00262001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (21c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0274209f002528050000000000000620634009100254069d00b54049102314489c00254008d0024420990827480910c64401dd0a344039100234209d0025a8180000000000000e8043400810122410c101206088100604008110260408d08214009d00214008100224208d08304008120334a08d
0023a0120000000000000c20734001100054001f0006c821100054205d08154801900040841140074001103c440a19215440f1101474001d1007081c0000000000000e0067c009300aec40bb00acd04b2002cc00bc002cc20bf102dc02b700a3c00b301eec05bf022d80db3022fc00bf0027a0180000000000000e
6067c009f052ed14af052ad14bd852bc00) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (21e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00b5602d1c07040ccd0030402cd03f1401c90037400c100b0500cd0430401cd00b3400cd0032a0140000000000000200534005d0c1ec007d005ec0171041c4826100d86037d005c40161001f40051011c4126d001c5017d009f4005d00142014000000000000042053c001f0006d001f2306c401
f0907c021a0107f041f1085c01131007c00170104c021f2084c021f0107c001f00050814000000000000060057c009f0127c019f0826c109f4027c01970127c489b0227ca9971027c009f0023c309b0067d009f0027c009f002500170000000000000e2017c009341e2c819b00a44019110244239340668119d046
5c049d0027c009240a6c129f00a4c02834) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2200) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (c609c1863c405e1001b400cd003988150000000000000e000bc01f3027ce09fd307cc017f007fc01330072c41ff027ec01df1277c09f3407ccc5fb027cc01f3007fc01ff007fa002000000000000064043c00df0827c008f0026c20d70035d00032030c00dd00374401d0037400db8037c20df80
37c40df0037400df0035b810000000000000004057c01ef0078c09ef8069c41f3407cc812f0078401ff0079401bb11fbc01e3407cc41ef0878c01ff007bc01ef00781014000000000000020017400ec003a400bd002b430e00038400350c3c610ed083841061013b400e10038400cd0838482ed003b400ed003880
040000000000000a0053400cd1430400dd) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2220) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (07c00df10a7c02db1007d025f0087c001f0115c0a9f0807c825f0037c80df2087c321f0087c809f0027c00df00370001000000000000062073c00d101344015f01c44115d10f74091100f0002df01b2d11cf003f840d102a4c02db4064c00d30037c00df0035a8140000000000000c205b400c50
0774109900000010d02834080120400521d0040400000033400c10240400018044440910807400cd00332806000000000000040003400e10038420ad001840069000b40020111c400ad128840c25003b404e10808480210888408a1002b400ed00390000000000000000062057400e520bbc9ca900284082d223b4
042107681286d1378405312077601c1013) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2240) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (041d02b7c06d31007c86130084c00930083c0adf00361000000000000000008043400c14001400cd00005000c00034000141045000101004101d3133400c100034820120804048100c3400cd00300810000000000000020007480d100544945d00144105d20374011101b4600d510344009d0037
420d100e7400d10064401d10037400dd0036a001000000000000080207400d10044503dd20c44010710874311130044071103045471d0037400d100c740b110044400910007400dd003620010000000000000c2007c00f3001c1215f050cc053f04bfc0033002dc0477203cc053f003fc40f3202bc01d3002cc10d
310dfc00ff003f08800000000000000c00) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2260) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000e804f400c10032402c50033400cd0033400814033400cd0031482c10026400cd02234008d02234088d00a3400890207a0100000000000000c200f401d10034403dd0077401dd1037401d10037401dd02fdc03f10870481dd00d7401570055c015d005740b5100f7100100000000
00000e000fc01f3003cc00f7007fc01ff007fc01f3006fc01ff007de01fb005cc01fb010fc103f000ec043f010fc0033012fa8030000000000000e4017c00ff000ac00bf080fc0027000f4003f000ec003f0087c803f023fc16df000fc881f000fc829f000fc80ff003fa8050000000000000ac007c00d30014e00
3f0814c001f8007c80131504c80070004c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2280) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (1101f7443d102ff40af14077400cd00b74005d00374009d0037400510010a01300000000000004200fc00d30037c00df0037c00df0237c00134437c20d30a37c00d30237c40df00a7c02df0027c001f0037c02db00050803000000000000060017800ff0035d00ed003fc00ff003fc00fe017fc5
0ff0037000ff001dc00fe025fc0077011d805bf003fc0037001d80050000000000000e2083c00d34036c00d70037c80df0037c01d304b7c00df0835c00db0016d00db00c7c021f0006c001f1007c021b0007a80000000000000006200f400d10036400dd0037400dd0037401d10037440dd1035000d14002400dc0
4374001d00b7400dd0007400594115a003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (22a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (044c01130057a81000000000000006600bc00ff003fc00ff003fc00ff223fc08ff003fc00ff84bfe00ff090fc08ff823fc00bf000fc00ff000fc00ff0019380200000000000000404bc00c38033c00cf0033c00cf0033c00c30037c18c30233c04c30023c00cf0013c008f0003c008f0023c008b
9010181200000000000002003f401e1007b401ed007b401ed007b401e1027b401e1407b401e141ff401ed146b409ed004b4016d005b409e1027c00060000000000000a001f400c14037420cd0033000cd1033480c108f7403c10833408c10013400cd04c34000d00034000d0003400090030200300000000000002
006f400d1003f400fd0037400dd02f7400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (22c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0017c00534017c0a73009fc005f0014d005346dec0053001cc0173029cc077300dcc0173009d28170000000000000c204b400cd0033400cd0033400c90037401410397400cd0030420c100f2400c14030501c14230504c14230501c140932816000000000000040007401ed017b401e5007b401e
1007b40361007f401e5007840de1007e401e10050403c10070401410070403c10051000400000000000006204f400ed00bb400ed003b400e1003b400e1003b480ed2038410c10018400e18028400e19038400e10038400a1001980130000000000000e0057c00df0037c00df0037c00d38037c00d30833c80df00b
6c02d31014d80c30844c81132074c01530) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (22e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (34148d05234148d05234148d052020100000000000000200634009d00244019d00274009104274409100674109140240009100246009d0427410dd04274109d0427410dd0424a0180000000000000800074009d0026c009d00274009b00e74009100674439b00245009000204808d00a70029d00
a74029d00a74029d00a420010000000000000c2043c009f0024c009f0027c00930267c80930027c04930024c00838264c809f0027c009f0027c009f0427c009f002508100000000000000c004bc001f0007c001f0007c00170087c401f6007c421f0003c001f0005c001f0007c001f0007c001f0007c001f010500
1200000000000006205fc005f0017c0047) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2300) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (734001d05c740a1d00074001d00474005108474003d008742a1140074401d000f4001d00074401d020740211008500180000000000000e0067c009f0467801bf0027c009f022fc0083002fc009f0467c019b0027c00bf0167c059f0167c059f0067c119b8067a01c0000000000000e6067c009f0
527c009f0027c009f0523c00bf052fc00978027c009f002bc809f202fc40bf002fc00bf002fc00bf002fb81d0000000000000ac077c001f0104c041f0007c00130807c80130007400130104c04114004d001f0107c441d0107c041f0107c441f0106b81c0000000000000080434408d05224148d00234008900234
008140334008905204548100244008d052) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2320) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0033008fc0013000cc00130004c00130004c00170005081400000000000006005fc009f0027c009f0027c009f00274089f0027c00990027800970027c009f0067c039f0027c009f0167c009f002108170000000000000e2017c409f0027c009f0027c009f0027c409300a78009f1027ca09b40e7
c009f02a7c039f00a7c029f00e7c029b002520050000000000000620634009d80274009d00274009d00274009142a7400bd002f480b1052f4009d002f400bd002f400bd002f408b1002528180000000000000e804b4008d00234008d00234008d0123440810423400a5002b400a5002f4008d00eb403ad00eb409a
d006b401a1426120120000000000000c20) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2340) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000004057c01ef01f8c01af007bc01ef005ac01e3007fc01ef184bc0123005bc01634040d01834060d01834060d018f00781814000000000000020017400ed013a401cd003b400ed041a401f1003b400ed003b400e1403f4006100e84032100c84032100c84032d0018800400000000
00000a0053400cd0030400cd0033400cd0072400c108774000d048345b0104834004100604012100484012100484012d0012a0100000000000000200534005d00144005d00174005d001c40051419f4005d00174015100134007100144005100144005100144005700142010000000000000042053c001f0004c00
1f0007c001f0004c00130407c003f000fc) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2360) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (c501974000500114000144024004d0413400cd0033410cd04b3400c100312002000000000000040023400ed003b400ad003b400e1001b400e1003b400e10028400e1003e4806d001b400ed003b400ed003b400e5003d0000000000000000062057400ed023b400ed003b400e5001f400e5103f60
0e502194082001184006d803b4006d001b4006d001b40061001910150000000000000e000bc01ff007fc01ff007fc01f3007fc01f3007fc0133006ec01f3006cd097f807fc017f005fc017f005fc017700592806000000000000066043c00df0035d009f0037c00df001dd00df8037c001f0037c00df00238005f0
007e009f0027c009f0027c009700359810) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2380) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (017400510016a001000000000000080007400dd00374009d0037400dd0057400d040674001b0066800d120234805d00074809900264009d002740091003620810000000000000c2007c00ff003fc03bf003fc00ff005fc00f3003fc00f300d4c0013401fc007f000fc00bf002fc00bf002fc00b3
403f08800000000000000c0007c00df0037c009f0037c00df0007c00df4237c00df3023c00cf1035c005f0867c111f0047c011f0047c111f00570005000000000000062013c00df003fc009f0037c00d30037c00d30077c00131014c80130006c005f00e7c011f0047c011f0047c01170051a8140000000000000c
205b400cd00334008d0033400c50013409) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (23a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0049821b7200cc4133004ec0133010d0c93f007cc04f3212c40033000cc0033007dc0033000fa0030000000000000e6017c00ff003fc00bf003fc00ff001fc00ff002fc003f000e8003f000fc006f001fc00fb003ec00ff003fc00ff003fb8050000000000000ac007c00df0037c009f0037c00d
f0017c40d30027c00d30834e00d34033c005e0817c00dd0037400df0037c00d300361800000000000000008043400cd00334008d0033400cd0013400c10033400c900024200100174004d00334004d00134004d00134004100140010000000000000020007400dd00374009d0037400dd0137400d1247748011003
4440d100274005d00374005d00174005d0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (23c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (7c00bf1027c00b7003fc019f007580070000000000000e220bc40da04848009a00c0c408700c3c41131102c030326c4c610f0034c00d30020413010140c050f0033d011300c7a8020000000000000e200f400dd2204400910c445209108264510040064031120344011d0034440d100244011100
44401990834418d10205a803000000000000048043400c90004400891000430910003534010506400110000404190830580c108204800100004000d0033400014003a010000000000000042007401d520444009120044849108744000508044211102444241d0074409f1226c40111204442111107440111004708
010000000000000e000fc01f3004cc00bb) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (23e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (18401ed0049401ad004e629a102786012982cb4412d007b4012d02f8489e1086b443a5006840321007840161007880060000000000000a001c411c500014008510c04908100304410100034020d00026400d0030402c10023400010000400010030400010002a00700000000000002004c402db0
800411db0606c059110744021b00074045d02334049d0034403f1182f40491002440091003440ed10034a01300000000000004200cc48d20a85c00d31084c00931004d04172047c421f08b7c109d0834d05c3c027c02930024c00130074d004340b10803000000000000060017c00f7200fd02af000fc05bf00b5c
403f0a0dc103f404fc003f003fc00df082) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2400) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01e5007a401cd036b403ed007b401ed0078401e10071000300000000000004004c400ed0009500f52008400a1083b40021080c4002d0038400210038408ed032b400ed003b400ed0038400e100398813000000000000040052c01df0004400932004400800037c001b4806041070034c00170070
d0cdf0927c005f0017c00df0034d00c30807a01500000000000006400bc00eb081ac80bb000fc20bf083fc003b020fc00ff083fc007f003fc00ff002fc00fb003fc00ef203bc00ff003db802000000000000004048d00c72201c00972000800934430c18013207c008d02024040f1030c00c10023c00c30030c00c
30030c0083003010120000000000000200) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2420) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000c20c3c009f0164c01970024c01930026c00931166c039300e4c049f0064c00930027c00970027c009f0025c008b002708100000000000000c004bc001f0107c02171007c00175007c00171107c401f0883c0a1f0885c020f0007c041f0007c701f0007c101f0003001200000000
000006209ec005f001cc0053005840573001bc5073219ec017f109ed007700168007f8017c017d005fc067f00144037306dda817000000000000042048400cd00b1489dd0970701c90273011c1803041acd0430407c00032400cd0023422cd06b3400cd0030409c140f32812000000000000042002441ed0048401
e100ec401f1007340121004a4012d00fa4) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2440) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (bf052fc40ff002fd14bf002dc009f002fc00bf002fc00bf0027c00bf002fb0190000000000000a807bc001f0004c04170004c00130116c001340064001341044200f0006d04530107c041f0107c041f0005c041b0106b01c0000000000000080434008d0022414c1902640081252040091002348
08105205408d08226148105674148d05634148d006041481052020100000000000000200634009d00244289581a44089100364069180a24209100244008d06264009140274009d00274019d0025400990434a0180000000000000800074009d0026c02910026c138140244218100276119109a44059d10e4400910
0234009d00274009d00245009100a62001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2460) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (026d039700e7a8050000000000000620604009101a64009140e54849108244229511214249901244209d2024400b1002c421b1082e400bd002e410bd0025a8180000000000000c204a4008100264048101204008148a44008100236009920200008d0020402a14228400a1002a402ad002a402a5
00eba0100000000000000c00704001100044041101054801130845001500044a01108044805d000442030088440a1102844021d00044021d0007081c0000000000000e8062c00b3002cc12b300ac400b3012cc20b1002ec00b3002ec80bf002cc05930164c05930964c059f0024c05970167a0180000000000000e
2067c008f002fc34bf052be54bd002f814) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2480) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (4074402c58230413dd00b1000c120b0510dd00b3400410030400c10030400cd0033400c10072a0140000000000000200534037d041f40071041c50371001ac437d04df41071011c4037d009f4004140144005100144005d0017400510014a014000000000000042053c001f0087c10131084c181
70004c281f0085c10130084d081f0307e00330004c02130004c021f0007c00030005081400000000000006005fc109f0065d049f0027c009f0167c009f1426c41974461c059f0827c009f0023d008f0261c098f0025c089f012580150000000000000e2016c00834062c019108a4480830064c08910127c008b012
4d009f1024d00930024d059341a6d129f0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (24a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (b4002d02384006d002b40021022980150000000000000e0003c09be004cc09f3007fc097f026fc81f6207fc09f3037fc81fb027cc0173007fc81f7007dc01ff007fc01f7006fa000000000000000062043c009f2827c009f1007c805f0007c00dc1007c201f0037c40df0037c00df0017c201f40
17d001f0007c001f0015b810000000000000080057c01ef006bc01a3007cc21751058c41ff0079c01e34070c01ff007b401e30050d01e30058c01af205bc01e340501015000000000000080017410ad182b642e10038400611022400ed003b440a10038400ed083b4006100384000100304004d002b4002100f880
05000000000000080053403cd04b34c1d1) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (24c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (07c001f0885c029f60c7c025f0107c0a5f00b7c069f00a7c4a170007c800f0027c001f0127c005f0027c011f017700010000000000000e2057c005f1486c009300174805f2187841d34233c129354e7c01db0024c00134023408d700a1c00df0037823d700f5a8150000000000000c20134000d0
9024008110070000d00834430082c3603010443001098000420c100134020d00104040d20034040100032804000000000000040003480ad020a408a1103b6406d100b60061003b608a1812b40829880c401e10013408e50019400ad001b400e5000908000000000000000621574002d1008418a1013f40c2d232b4
06a108bb40aa1021b400e1023842061003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (24e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (001f0004c00934007480d34007c009f0015c00df0006a0000000000000000080434000c00034008100134000100024001148054000d00034200d80004000528234800100234004d00234000d002020100000000000000200074021d8047423910017423510006588d101074211d20e7406dd00e4
400110127400d11127400dd1035400dd0024a0010000000000000802074001d01474219104874231186044c3010045c011d00c74001d08444009100474001100474001d00074001d00162081000000000000042203c007f000fca093009d800330848c11b3003fc00bf0007c01ff002cc0593004fc00f3004f8009
f001dc00ff001708800000000000000600) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2500) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000e8043400c10030724cd0033400cd1032400c14081508c542304024d1033400cd0030410cd0033400cd0033400cd0033a0100000000000000c2007481d14074484dd0877401dd0074401d120e45011100444001d02ff461dd2074404dd0077441d70077401dd0077080100000000
00000e000fc01f3003c409ff007fc01ff003cc01f3411cc00f3213cc64ff007fc01ff007cc01ff007fc01ff007fc01ff007fa0030000000000000ec017c003f100fc203f100fc003f000dc003f080dc203f200fc003f000bc00bb000fc403f000fc003f000fc003f000fa80500000000000000c003c001e0007c20
131017c00110006c00130003c001f1007c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2520) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (c14034411902034403dd003f400dd0034400dd0037400dd0037400dd0034a01300000000000004200fc00df0037c00df0037c00df0834c00d30000c02530000d481f0037c00df0034c00df0037c00df0037c00df0035080300000000000006001fc00ff003fc00ff003fc00ff003dc00ff002f00
2bf0037d407f003fc00ff003f800ff003fc00f7003fc00ff003d80070000000000000e200bc00d31030c00df0037c00df0836d00d30254c02472004c008f0037c00df0034c00df0837c00df0037c00df0037a80200000000000006200f400d10034400cd8037400dc0036400d100345001102044089d0037400dd0
034400cd0037400dd0037400dd0035a803) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2540) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (037c00df0037a01500000000000006600bc00ff003fc00ff003fc00ff003fc00ef0017e086f090fc24bf003f880ff003fc00ff003fc00ff003fc00ff003db80200000000000000404bc00cf0033c00cf0033c00cf0230c04c38020c008340b0c025f0033400cf0230c00df0033c00cf0033c00cf
0030101200000000000002001b401ed007b401ed007b401ed007a401e102404216105484052d027b401ed0078401ed107b401ed007b401ed007880060000000000000a001f400cd0133400cd0033420cc2830408c10030511810070413cd0033080cd2030400cc1033400cd0033400cd0032a00700000000000002
004f400dd003f400dd0037400dd003ec80) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2560) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0017c005f1017c005300d4d99434014d00530017c005f0014c005f0017c005f0017c005f0015a8170000000000000c204b400cd0033400cd0033400cd0033400c104e0402010000441010033400cd0030400cd0033400cd0033400cd0033281200000000000004000f401ed017b401ed007b401e
d017b401e1405c401e10078501e10a7b401ed0078401ed007b401ed007b401ed0079000300000000000006204f400ed00bb400ed003b400ed00bb400e1020c400c10030400410233020ed2838520ed203b400ed003b400ed003988130000000000000e0057c00df0037c00df0037c00df0037c00d321b490013000
4c009361f7cc0df0034c01df0037c00df0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2580) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (34008d00234008d00234008d002020100000000000000200634009101274009d00274009d002400891003c404f1002c4009d00274009d00274009d00274009d00274009d0024a0180000000000000800074009100634009d00274009d00240008100244019000640099d10274209d00274009d00
274009d00274009d002620010000000000000c2043c00930027c009f0027c009f0024c01930024d019340e4d108f0027c009f0027c009f0027c009f0027c009f002708100000000000000c004bc001f0007c401f0007c001f0006c001f020bc003f004bc083f2007c801f0007c801f0007c001f0007c001f000700
1200000000000006205fc005f0017c005f) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (25a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (734001140874051d00074001d008742011088442a1110944815d00874001d00044050d00074001d00074001d0007081c0000000000000e0063c0093046f8029f0027c009f0467c00b30464c01a3057cd07bf0467c009f0024d029f0027c009f0027c009f0027a0180000000000000e6067c009f0
027c149f0027c009f0027c009f2027c009e3027c549f1027c209f0827c149f0027c009f0027c009f0027b8190000000000000ac073c00130107c001f0007c001f0104d0053410cc84530104d041f0107c001f0007c000f0007c001f0007c001f0006b01c0000000000000080434008145234008d00234008d05204
00810528494a10d28414ad05234008d002) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (25c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (821f0007c001f0004c001f0007c001f0007c001f00050814000000000000060057c009f0023c009f0027c009f00264009e0263d048e0167c018e0027c009f0027c009f0027c009f0027c009f002580150000000000000e2017c00930027c00bf0027c009f0827c209320e4d079340a4c019f0027
c009f0024c009f0027c009f0027c009f0027a8050000000000000620634009100276009d00274009d00274009110a4500d108244089d00274409d00244009d00274009d00274009d0025a8180000000000000e80434008100234008d00234008d00234208140204808100204068d00234008d00204448d00234008
d00234008d0023a0100000000000000c20) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (25e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000004057c01ef006bc03ef007bc01ef007bc01e30070d01232050c21cf007bc01ef0078c01ef007bc01ef007bc01ef00781015000000000000020017400ed041b400ed003b400ed003b400210038500e100984006d203b400ed0038408ed003b400ed003b400ed0038800500000000
00000a0053400cd0033400cd0033400cd0033402417030410c14190500cd0033400cd0030400dd0033400cd0033400cd0032a0140000000000000200534005d005f4005d00174005d00174187110144007120584117d00174005d00144005d20174005d00174005d0014a014000000000000042053c001f0007c00
1f0007c001f0007c80131084d00132084c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2600) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0100f0404c132f144b451033400cd0032400cd0033400cd0033400cd00332804000000000000040003400ed0038400ed003b400e1003b400610039408a11039408c1023b400ed003a400ed003b400ed003b400ed00390000000000000000062057400ed001ac00ed003b400e5003b40061433849
0e1033848065003b400ed2038400fd003b400ed003b400ed003988150000000000000e0003c01ff007cc01ff007fc01f3007fc0133227dc01e3427cc01f3007fc01ff087cc03ff007fc01ff007fc01ff007fa000000000000000066043c00df0007c00df0037c00df0037c009f0837d80de0017c007f0037c00df0
037d02df0037c00df0037c00df0035b810) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2620) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (037400dd0034a001000000000000080207400d10004400dd0037400dd00374029100344015111f44015b0837020dd0037400dd0037400d90037400dd003620810000000000000c2203c00f3000cc00ff003fc00fe0037c00f30030c00330830c04630037c00ff003fc00ff003fc00ff003fc00ff
003f08800000000000000c0007c00df0017c00df0037c00df0037c02df2137c025f21365865f2033c00df0035c00df0037c00df0037c00df00370001000000000000062057c00df0010c00df0037c00d30037c009344f5c030308a5d02530037c00df0036d00ff0037c00df0037c00df0035a8150000000000000c
2013400cd0012400cd0033400c50033400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2640) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (004ec0073400ec00bf886ec8137004e401f3207ec0cf1003cc02b7003c003ff007fc01ff007fa0030000000000000e6017c00ff001fc00ff003fc00ff003fc003f003fd807f003fc007b183fc00ff003fc00ff003fc00fb003fc00ff003fb8050000000000000ac003c00d30014c00ef0037c00d
f0037c00534034c80130834c00530037c00df0037c00ff0037c00dd0037c00df0036b000000000000000008043400c14050400cd0033400cd00334004100304004160205804d0033400cd2033400cd0033400cd0033400cd00302010000000000000020007400d10014400cd0037400dd003742611203440111006
4410110037400dd0037400dd0037400dd0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2660) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (5440872037c00ff083fc00ff003d8005000000000000042202ea15320d6c06930204d00590046c05dd0066d02170046c00df0034c00cb0036400df0034c00df0037400df0037a8000000000000000e200d418958060448112005424990046400cd00264045d0046420dd0036400dd00364049900
34500cd1037400dd0035a80300000000000004a0424000108025c0090000420490806480cd20224200d2002600cd2830564cd00b2446cd2030404cd8033400cd0033a010000000000000040005481d510244004100454019100054009d00644005d0004000d1407440cf500bc502f1107c400dc0077401dd007708
010000000000000e000ec403b000ec0033) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2680) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (18601e9844a40f61804e401a180ca50d0d006b48161a069621ed0278409e90a7840da11078401ed007b401ed007880060000000000000a000c601851041401510002500c520435020d0022402598003400dd0030420c84034480cd2030480cd0033400cd0032a00700000000000000004c401cb0
0b6c01510422c00911482c04d78267643510005c20dd0030400f1203c420d1003c400dd0037440dd0034a01300000000000004200cd085f0495d0a1b0027c00470007c50db0026e0c1f0007e00df0036501d00836d009f0830c40df0037c00df00350803000000000000040217c815f182fc00ff804ec01970005c
09bf016d8817f040de00f3003dc20d7083) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (26a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01e10078401e98178441e52178081ed007b401ed0079000000000000000004204d400c10008420e1400840085000c400e10038400610038c00e1003848cf11038408e10130400ed003b400ed00398813000000000000040050c00d30014c00db0006c60d70804c005b0860c80170000e00d34070
c04db07b4904971174c00df0037c00df0037a01400000000000006200bc00df0207d045f0203c00df1017d24572027c005e0037c00df0834c30d70235c44df04b7500df0037c00df0035b802000000000000000058c00870085c044b0002c04470083d044d04224024b0497400cf0030400c90a30ca48f0830400d
f0a33c00cf003010120000000000000200) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (26c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000c2040c11830024801936024c009701239009f0024c00970064c009f0024d00930024c809f0024c009f0027c009f002708110000000000000c004be001f0287c04070005c920f00c7c00170007c121f0006c001f2006c000f0003c600f0007d001f0007c801f0007001200000000
000006201ce2173405cd0173001cd0277215cd0073011cc0077211cc00510014c005b4014c055500148005f00170005f0015a81700000000000004205940ac18044409c104b0400c50070419d14030400d10030500d10031500c10830421810030400dd0033400cd00332813000000000000040000401e10058401
c1006c601e5005810141806c50375005e4) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (26e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (bf002f414af052fc148f0026c149f0527c14bf1027d149f0027c009f0027b819000000000000084078d04130101c04130004c04574106c041d0004c005700044001f0005c04114100c040b2104c000f0007c001f0006b01c000000000000000040414890d2141481002441481252041485002050
08000204008d00214148105204148d05204008d00234008d002020100000000000000000604009100a5400918064404d508265809d00a44049519245009d00254019100245009920244009d00274009d0024a0180000000000000800044099b02a4408910020c029104644009f00244019100204009d0824400914
0244009d00244009d00274009d00262001) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2700) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (027c009d0027a80500000000000006206140899402744299102451091202450091b0245209140274009d08274008100264849d08274009500274009d0025a8180000000000000e80484088901a24028920254088908a44088148204209101274008d00205068012225088d00234048d00230208d
0023a0120000000000000c2071402110885406110004402110184416140004444510105c141d00044051140844171d00074010f00074001d0007081c0000000000000e0060404b000acd06b3103dc04bb09acc24bb0028c02b300ab8009f902ec07bb0164c059f002fc089f002fc009f0027a0180000000000000e
6067c80bf452ed94bd0029d80bf252ec14) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2720) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0071420c10070441c18870463c50030600cd3030408810032400c50030400cd0033400cd0032a0140000000000000200104027b021c4087d0010c0371001841073205c4016100186807d00144007b08144007100144005d00174005d0014a014000000000000042050c42172005c221f1005c021
30204c401a8804c00171006c201f0006c00131004820070004c001f0007c001f0005081400000000000006005f410830125c29874127c128f4267c15858827c109f0025c009f2024c20970021c409f0027c009f0027c009f002580170000000000000e2114c05920066c019b04654639b0424c41990020c0893022
74609d0024d00930026c009d0027c009d0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2740) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (8400e10038400f1003b400ed003988150000000000000e0008c0133007cc0171026c501ff017d001b34878c2533087c509fe087e801ff007cd01f3207cc13f3407bc01ff007fa002000000000000044043c00db6037c00de00254001e0017c00df0007d000f0025c01ff0035c169f2035c36d700
37d02df0037c00df0035b810000000000000004050d01870079c018f0069c8123204cc01e10078c01671068421ff0078d01f105f2d07f74070c85ef007bc01ed00781014000000000000000010410ed0420400ed042a410c14018540c1442c41031002c741ed0038440e9113a444e10078605ed003b400ed003880
04000000000000000050403c51035442cd) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2760) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (05c021f0127c20cf0827c04df0095c00df2027ca01f6097c00df2037c008f0036c00df0037c00df0037c00df00370001000000000000042052c03130034c01d30064803cf205640b900010d0b510034c00fd0034c60df003cc11f35030500f30037400df0035a8140000000000000c201b4b1410
031401c10020400cd029244a5110506830002e4600cd1031400cd0034501c01030400c11033400cd00332806000000000000040402490014438410214a2c400ed290a500a1003c44c212028640ed0038400ad0038400e10038400e1003b400ed00390000000000000000062055404614029404f10e28410ed00984
887104b841431012c40ced0039404ad003) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2780) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00df0034c00f7003cd00f35037400ff0037c00df0036b000000000000000008043000010020500c500244000d0000420410020400014011400cd0030580c18030480c10033440cd0033400cd003020100000000000000200074231102244005502244201c00446409100045001901b7400dd1834
400950034400c10037400dd0037400dd0034a00100000000000008820f403110114400d180205051c00d4420d10ac4447010015c20dd0034500d10034400d10037400dd0037400dd00362081000000000000042203c00336030c00b2102cc853f040cc04b3005cc0333047fc00ff003cc0897003cc00f30037c00f
f003fc00ff003f08800000000000000c00) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (27a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000040043400cd0033400cd0033400c10432458c10333406c94011460cd0531400c90031414cd0033400cd0033400cd0033a0100000000000000c6407441dd0077441dd0077401d101bc404f1113f406e10064441d72030406e109bc442fd0077401dd0077001dd0077080500000000
00000e000fc41ff007fc01ff007fc01f3053cc00f3033fc22b3202cc01ff107cc1cf31e3cd10ff007fc01ff007fc01ff007fa0030000000000000e6017c003f401fc40fa202bc202d000fc007f800fc803f001dc00ef803fc00bf003fc00ee003fc40fe003fc00ff003fb8050000000000000ac003800130014c00
154024c801f0004d00934004c001b0037c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (27c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (fd103c400d10034040c10034011f1003c400fd0037400dd0037400dd0034a01300000000000004200fc00df0037c00df0037c00d34033c08df0034c00930036c00d38034d00c34034d08df0037c00df0037c00df00350803000000000000060017c00ff303fc00ff003fc00ff0035d80ff003bc4
9b70432d00ff003fc00f70036800df003fc00ff003fc00ff003d80070000000000000e220bc00df0837c00df0037c00d34036c40d34037c01db04e5c00df0035d00db0834c00cf0037c00df0037c00df0037a80000000000000004000f400dd0037400dd0037400d10836420c10037420990075400d50034400d94
031400dd0037400dd0037400dd0035a807) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (27e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (037c00df0037a01100000000000006200bc00ff003fc00ff003fc08ff003fc20ff00bfc28ff0a3fc00e3003fc00ff043fc10ff003fc00ff003fc00ff003db80200000000000008405bc00cf0033c00cf0033c00c30933c80cf0130908834632c00cd0030c00c34030c80cf0033c00cf0033c00cf
0030101200000000000008201b401ed007b401ed007b401e9007b409ed10784a9a10278749ed4078409e10078401ed007b401ed007b401ed0078800600000000000008000f400cd0033400cd0033400c10033401cd0030400c12072400cd2030421c90030001cd0033400cd0033400cd0032a00700000000000002
004f400dd0037400dd0037420db083f401) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2800) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0017c00534014c80534016d005f40ddc00531014c00530014c005f0017c005f0017c005f0015a81700000000000004004b400cd0033400cd0033400c10030400c120324018926b0440c90030400d10034400cd2033400cd0033400cd00332812000000000000040013401ed007b401ed007b401e
10178401e1037a631ed0071401e94078509e14178725ed007b401ed007b401ed0079000300000000000004605f400ed003b400ed003b400e1423c416e10130410e10038400e94038434e1933048ced083b400ed003b400ed00398813000000000000040043c00df0037c00df0037c00d30374d44d300b4c0497407
5c00c30074c04d30134c04df1837c00df0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2820) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (04148d00234008d00234008d002020100000000000000200734009d00274009d00274009d00254449560204209d80244009d00244089100244049d00274009d00274009d0024a0180000000000000800074809d00274009d0027400970026c409100244009d11a44408d00244219100245009d00
274009d00274009d00262001000000000000042043c009f0027c009f0027c009f2024400914024c009f00e4d009f0024d01930026c009f0027c009f0027c009f0027081000000000000006004bc001f0007c001f0007c001f0007c800f2005c00071087c80170007c801f0007c800f0007c001f0007c001f000700
120000000000000e201fc005f0017c005f) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2840) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (734001d00074001d000740011014040f1122c44011100844001d20404031100c04030d08074001d00074001d0007081c0000000000000e0063c009f0027c009f0027c00934064d01b34264c2193156ac00b700a4d03b340e4c03bf0027c009f0027c009f0027a0180000000000000e0867c009f0
027c009f0027c00970526c149b0527d14bf003fc409f0523c149f4527c148f0027c009f0027c009f0027b8190000000000000ac07bc001f0007c001f0007c001f0105d04070104c040f0104c001d0004404030104c041f0007c001f0007c001f0006b01c00000000000000a0534008d00234008d00234008505234
148505204148d05204008da02043481052) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2860) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00134004c00130004c001f0007c001f0007c001f0005081400000000000006004fc009f0027c009f0027c009f0025c008f0027c028b0023d209f0027c008f0027c008f0027c009f0027c009f002500150000000000000e2017c009f0027c009f0027c00930026d00934024d019700e4c008f0024
d00930024d009f0027c009f0027c009f002528050000000000000400634009d00274009d00274009100264009100244009550644409d00244009100204209d00274009d00274009d0025a81800000000000004004b4008d00234008d00234008104a24108101204568500204008d01204068101a0406cd00234008
d00234008d0023a0100000000000000c60) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2880) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000084047c01ef007bc01ef007bc01e30078c81f30178d03f3007bc01e101f8401c10178d01ef007bc01ed007bc01ef00781014000000000000082007400ed003b400ed003b400e9003a410e90230400e1a03b400e91178450e14038620ed003b400ed003b400ed0038800400000000
0000080053400cd0033400cd0033400c10030400810030500c100d3409c108304418100304008d0033400cd0033400cd0032a0140000000000000200534005d00174005d00174005b0016c015b001440050015f40073801c5005100145007d08174005d00174005d00142014000000000000042043c001f0007c00
1f0007c00134000c80134000c00134487c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (28a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (c18030401c90033400810030400c10030400cd2033400cd0033400cd00332806000000000000040403400ed003b400ed003b400e10030400a10238540c504bb400a10038400a10038508ad003b400ed003b400ed00390000000000000000042057400ed003b400ed003b400e10038400b1403c48
4eb003b408a1023c400b1403c400bd003b400ed003b400ed00398815000000000000042003c01ff007fc01ff007fc01f300fcc03f3107cc81f7007fc01b300fcc03f330fcc03ff007fc01ff007fc01ff007fa002000000000000062043c00df0037c00df0037c00df0337c029f0d37c16df0037c00d700b7c029f0
2b7c029f0037c00df0037c00df0035b810) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (28c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (037400dd0036a001000000000000080217400dd0037400dd0037400d10034400d10034440d10077400dd0834401d10034500dd1037400dd0037400dd00362081000000000000042213c00ff003fc00ff003fc00f30038405b3103cd80e30273c00ff003cc05b3003cd00bf003fc00ff003fc00ff
003f0880000000000000060007c00df0037c80df2037c00df0037c008f6037c00df4037c40df2037c008f0033c008f0037c00df0037c00df003700010000000000000e2057c00df0037c00df0037c00d3003c500d3003cc05f70077c00d3403cd00d3683cd00df0037c00df0037c00df0035a81400000000000004
2013480cd0033400cd0033400c14030480) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (28e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (21410850021410852c414318500204108120a04008100004108924214328900214008500214000000000000000000e2017c00ff003fc00ff003fc00ff003eec0bf003fc00ff002fc20ff083fc80bf003fc00bf003fc00ff003fc00ff003fb8050000000000000ac003c00df0037c00df0037c00d
3003dc00f3083cc40f30037c00df003cd00f3003cc20ff0037c00df0037c00df0036100000000000000000a043400cd0033400cd0033400c14031500c10030400c12073480cd0030400c15030400cd0033400cd0033400cd00300010000000000000020007400dd0037400dd0037400d10035400916030420d1203
7401dd00344009100344019d0037400dd0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2900) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (320900c04000100004000100004000000000000000000000000040001000040001022040001000042c01033040cc10a10c24410000800820900c10c003304000100004000100000000000000000000000008000200008000200018004200528030a0030880020042803820010800400052820020
83280002000080002000000000000000000000000008440211008440211108444211128440e11038440a1133844ca211084440011280646110084402110084402110000000000000000000000008000200008000200228008200608000a0003800060020004c600008008021218008a20028000200008000200000
0000000000000000000008500214008500) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2920) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0008000200008000200108004200908030e00608000200928800200518908620b28000600008000200008000200000000000000000000000000850021400850021420852c214a08504214108500214a18d00214028000204d18500a1400850021000850023400000000000000000000000000000
00000000000230000000000004c00000820000630024000120800820230a20820330000000000000000000000000000000000000000040001000040001011040001000042481000040001092082c410120804810b20020c20000400010000400010000000000000000000000000010000400010000402010000400
0100c04002100024010104824200908024) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2940) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0c108509008340201320248108004008140004000100000000000000000000000000100004008100004328114204008100a04008110004120100c0420001800422010842c0001008040001000040000000000000000000000008400210338400210138420e10b38428e10b38420210938000a209
08104210938824a00c08400e10008400230000000000000000000020033800ce0033800ce00028028e00308000e0090802ce00008000220b1880c60023800422033800020033800ce20008000000000000000000000840021000840021002840c210708424a10108c00220208020210228c04a30318824a2000840
0214008400200000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2960) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000000000000000000000000003c83c29b000264018c24a482c2c03c1803ea409f015e400999bfd98000000000000000000000000000000000000f0f00000000000000000030a080800000300010f0a080800000300010f0b080800000100010c0000000000000000003c3c00000000
0000000000000000000000000001010000000000000009010000000000000009010000000001080008000000000000000000000000000000000004208000000000330000000130008c00900018c00b30000000830010c2090000402092181402000000080000000000010820000000000000000000004000100084
0001030840c210108424a10808c0001032) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2980) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (f7fffc0000000003fffffff80000000003ffdffffc0000000003fffffffc00000000000000000000000000000003fffffffc0000000003fffffffc0000000003effffffc0000000003dffffffc0000000003fffffffc00000000000000000000000000000003fffffffc0000000002ffffffdc00
00000003fffffffc0000000003ffbffffc0000000003fffffffc000000000000000000000000000000000000000000000000cc2014141000000000cc401848800000000111405f14880000000000000000000000000000000000000000000000000000000000000800000005400104000028080145400151492960
60035169e9780000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (29a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000180002000000000000000000000000008500214008500214008500214008500214118500a14428400a10008400614838400630008400214028500214000000000000000000000000000000003fffffffc0000000003f7f279fc0000000003f3ffff740000000003ffffeffc0000000003ffff
fffc00000000000000000000000000000003fffffffc0000000003f8edf6f00000000003f7effffc0000000003fffff3fc0000000003fffffffc00000000000000000000000000000003fffffffc0000000003ffeffcfc0000000003fffbfffc0000000003fffffffc0000000003fffffffc000000000000000000
00000000000003fffffffc0000000002ff) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (29c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0040001000042001080041100084041300008002100000001300080200001000040001000040000000000000000000000000400010000400010000400010100404010320500810210400414100500014910400004000400010000400010000000000000000000000000800020000800020000800
0200008000200018000a008080202002081002008080206000080002000080002000000000000000000000800008440211008440210008444211108444211118440a11428d60a11308544631138c706350085402110284402110000000000000000001000008000200008000200008008200208008200228100600
008010200308008a04a38100a200080002) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (29e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (23841ca30008400210008400234000000000000000000000000800020000800020000800020000800020010800c204028008e0412800820093810c6000080002000080002000000000000000000000800008500214008500214008500214008500214008404230818500e1421850421403842421
40085002140085002100000000000000000001000000000000000000000000000000000004000300104000010110004120104000d201040040000000000000000000000000000000000000000000400010000400010000400010100404010320404810a30c30414120504030330d24030000500010000400010000
0000000000000000000000100004000100) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2a00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000400010000400010000404010000400010120c00010308c04e30d00424810110430430c004000100004000300000000000000000000000000100004000100004000108004000100004230000000038138e00600100404a2001080040010000400010000400000000000000000000000084002
1000840021000840421000840021003892023400840ca10108414a10118500614008400210008400210000000000000000000020033800ce0033800ce0033800ce0000800ce0000802ce00c08024e00308034a00138004e0033800ce0033800ce00008000000000000000000000840021000840021000840021000
8400210208d0c210818c04e30318404a10) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2a20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (6802096c29202148021002001000000000000000000000000000000000000f8000000000000000000000000000000000000000098da7600002640d9820e83a9c03fd9bfd99980000000000000000000000000000000000103000000000000000000000000000000000000308080800000100010f
08080800000100010c0000000000000000003c3c00000000000000003000000000000000000000000000000000000102000000000108000901080000000200000800000000000000000000000000000000000c200000000000000000000000004000000000000010120004818008c0000000480050000000000000
0000000000000108200000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2a40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003ffffff7c0000000003fffffffc00000000000000000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc000000000000
00000000000000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc0000000003fffffffc00000000000000000000000000000000000000000000000000000000000000000111141984800000000111101544800000000000000000000000000000000000000000000000000000
0000000000000000000000014128212803) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2a60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (8c2023a808ea0232808ea023a808ea023a808ea023a808ea023a808ea022a200000000000000008c03b020e8083b000ec0839820ec0a3b000ec0039008e4083a020ec0e3b038ec083b028e80839028ec0e3b038ec082a3000000000000000000000000000003fffffffc0000000003fffffdfc00
00000003fffffffc0000000003fffff7fc0000000003fffffffc00000000000000000000000000000003fffffffc0000000003fff6fffc0000000003fffffffc0000000003fffffffc0000000003fffffffc00000000000000000000000000000003fffffffc0000000003fff4fffc0000000003fbfffffc000000
0003fffffbfc0000000003fffffffc0000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2a80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (011080442012a300000000000000008c01800060001008040201008060081800040201800060001800060001800040201800060001800060001800060002a3000000000000000a8803a804e20132886ca01b2006ea013a884ca21ba884ea0112804e2093880cc203b8804ea013a814e2013a80ce
a012a200000000000000000401a0006a003a10068401a10068003a100e8401a00068001a80068021a00068001a0006a001a00068001a0086800001000000000000000004012010480410010e8043a0104804100106804120104804100104804120004804120184804120184806120104804001000000000000000a
8803a808ea0230808c20231808ea023080) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2aa0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (4004100104004102104004102104004100104004100104004100104004100104004100104006a200000000000000088480800820030800020000800020020800020000800020000800c200208008200208008600108000200208008200200100000000000000000402a00ca8032a02ea803aa00e
a803aa00ca80baa00ea803aa01ca803aa00ea803aa00ea803aa00ea807aa00ca803801000000000000000a8800a81428042a814aa052a0142a0d08814aa050a814220508000220508814a207088142804088142a070a81c2a052a200000000000000008c010804420a188046201180044201108046281108044201
1080042031080c62011081442001080442) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2ac0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (32010ca0c32010c80432010c804001000000000000000000030000c00010000400010000c00010000400030000c00030000c00030000c00030000c00030000c00030008c000000000000000000000a88030810c20410810620418810c20410810428430810c20430830c20430810c20430810c20
430810c20430910c2042a200000000000000008c01b00068011b800ec003b8006c00138006c001b0006c00180046c001b0006c001b00068011b0006c001b0006c002a300000000000000008c01a8006e001a8026a009a8026a009a8006a009a8026a009b0006a009a8026a009a8026e009a8026a009a8006a00aa3
000000000000000a8c8010010400410010) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2ae0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (02a80180006a001aa0068801aa006a001a2006a801a20060001aa006a801a2006880180006a801aa006a801a2006a2000000000000000088018812c20498012620418810620498012620498812620430812620498812620498812c204188106204988126204aa200000000000000008c010010c0
0410010400410810400410010400410010400430010400410010400410010c0041001040041001040042a3000000000000000a8801a8106a0c1a0006a041a0106a041a0006a001a8006a04188306a041881062041a8106a0c1a8106a041a8006a042a3000000000000000004032010ca0c32810c80432010c80412
810480432010c80432810c80432010c804) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2b00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (018ec063b018ec063b018e8063b018ec063b018ec062a200000000000000008803a818ee063a808ea023a808ea063a808e20238018ea0639018ea063a418ea063a818ee0638818ea063a818ea062a3000000000000000a8c02b018ac0621018840601018ac062b01884062b018ac062b018ac062
b01884062b018ac062b018ac062b01aac062a300000000000000020c002012080480012000402010080482032000482012080402012080482012000482012080402010080482012080480000000000000000000000a01828062a018a8062801828060a018a0060a01828060a01828060a018a8060a01828060a018
28060a0182806000000000000000000a88) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2b20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000a8803a800ea003a100e8003a840ca003a000e2003a800ea0038800ea0038800ea0038800e2003a800ea003a800ea002a200000000000000000001a0186a061a8186a061a01868061a01868060801868061a81868061a01868061a0186a061a01868061a01868060000000000000
00000880012010e80412010480c1201048041201048041201048043a010480412010480412010e804120104804120104804000000000000000000a8803a818c2063a81aea063a018ea063b81aea069281aea8630818ea063a818ea063a818c2063a818ea063a818ea062a200000000000000008803b018e8063981
8ee8638018e40639818e4063b018ec063a) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2b40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (4000120004200108004200108004200108004200108004200108004200100000000000000000000002a030a80c02030a84c2a030a80c22030084c22030a80c2a030a80c2a030a84c2a030a80c2a030a80c2a030a80c000000000000000000a8800a81028040a000200008800aa0c0a0102a000a8
102a040a0102a040881022000a81020040a8102a040a8102a042a200000000000000008801081042041081040041081062041001042041081042041081042041081042041081042041081042041081042042a200000000000000008801801060041881060041801040041801060041801060041801060041801060
041801060041801060041801060042a200) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2b60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (06b0002c002000000000000000000000030800620030800c28030800c20030040c20030880c00018800c20030800c20030800620030800c20030800c20000000000000000000000001b000e8001b0006c001b0006c001a0006c001b00068003a0006c001b0006c001b000e8001b0006c001b0006
c002a100000000000000008801a8006e00128006a401b8006a001a8004a401a0006800198006a001a0006a001a8006e001a80062001a8006a002a2000000000000000a880010100404010920404802520405210520404a101004040101004040101004040101004040101004040101004042a20000000000000000
0000800420810000420010800420002000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2b80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (221308846220108844221188846261188846221188046221188846201188046201188846221000000000000000000000010002400090002c000b0002400198002400090002400a10002400090002400010002400090002400090002400000000000000000000000001a8316a0c508316a045a811
6a0c7a8114a045a8396a0c58831620c588396a0c58831620e5a8396a0e5a8316a0c400000000000000000000032028ca0a32028c80a32028c80a32028c80a32028c80a32828c80a32028c80a32028ca0a32038c80a32028c80a0000000000000000000000300024000b0102c000b0002c000b0002c040b009ac002
10002c002b000ac0003000a4002b000ac0) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2ba0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (3a804e6013a804ea013a804ea0100000000000000000000002b00cac032b00cac032b00c84032a00cac032b00ca8032b00cac032b00cac032b00cac032b00cac032b00cac03000000000000000000000002014080d02034080d02014000502214080d02014080502014080502014080d02014080
502014080502014080500000000000000000000000a10420410a104284108104a8410810420410810420410a10420510a10428410a00428410a00428010a004284100000000000000000000002a880a800228808a2022880aa20228800a2028880aa2028080aa2028848a22028880a8282a880aa002a800aa20000
0000000000000000000188846221108a4c) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2bc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0027e909fa426490992426492ffa4264909924be5f0997c27e92fffcbfff09fa4bfff0997cbe5f2fffcbfe909ffc000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000009fbf27
efc9fb727fdc9ff727edc9fbf27edc9fb72ffdc9fbf27edc9fb72fedc9fb727fdc9ff727edc9fbf2fedc000000000000000000000099b5242d490b424ad092b4266d090b5242d098b425ad090b5242d890b4252d091b624ad092b4242d090b5256d00000000000000000000003a804ee093a804e20138824e20139
804e2013a804e60139844ea213a804ea41) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2be0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01048003a010680412010480412010480412010480400000000000000000000003a818ea023a808ea0238808e20230808ea023a808ee023a808e80230808ca0210808ea023a808ea023a808ea02000000000000000000000039028e40838800e0083a020e88838038e40239828e68839038e00a3
9020ec0039800e00838020e00839000e40800000000000000000000000863721edc863121ec487b1218c48637218c4863727edc87b727ec49fb727ec49e3121edc9fb727edc9ff7278dc00000000000000000000009ff727fdc9fb727edc9fb72ffdc9fb727edcbfbf27efc9ff72fffcbfff27fdcbfff27efcbfbf
2fffcbff727ffc00000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2c00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (000000000000000001080662011000242009080242009080a42059003640011080e420998806620110006420090802420a90804420100000000000000000000001800040601800060001800040201800060001800060001800860001008840201800060001802060001802060000000000000000
00000000038804c20138084e20138804420138844e22138004e001388044a0130804c22138084e20138804e20138884e201000000000000000000000018008600018000620018980626018900600218000600018008600418100600038100620018800620018000600000000000000000000000001201048041201
0480432010c8843a018480412018480412) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2c20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0620018000620018800620018800620018000640019800660018800620020310000000000000000c001102040031000040001000040001000040001000040001000000001000040001000040001000040021020040020310000000000000000c00800220002080220018800620038800e2000880
0a20000800a22028800a2000080022001880062083a0000200000310000000000000000002800ca0072002ca0032800ca0072801ca00b2800ca0032800ca0033800ca00b2802ca0032800ca0032000ca003003100000000000000000008815a2074883120044801100004801122054881d20054881522016881da2
0548815200448031200448815220540000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2c40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0c1880062042a2020000000000000000030010c00430034c20430830c20430830c00420010c00430010c00430010c00410010c20c30810c20c30010c004000020000000000000000030000c00030004c00010000400010000c00030000c00030000c00010000c00010000c00030000c00030000c
000000020000000000000a88030810c20431810c20c18812620498812c20430810c20430810c20418812c20410812c20430830c20430818c2042a2020000000000000000419000640018000600138004e0013800464001900064001900064003900064001100060011800460011900064002800800000000000000
0c01880862001800066001980066001980) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2c60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00608018000608018200608018200608018200638018a006080182006080182006080182006000120000000000000a88428800a20020000800020000800020000a20028800a20028800a20028800e20028800800020000800028800a2002a2020000000000000000018810620410810c20430830
c20c30810620418810620418810620418810620418810c20c30810c2041881062042800a0000000000000000010010400418010c00430010c00430010400410010400410010400410010400410010c00430010c004100104004280020000000000000a88018810620438820620c188106204188326200188106204
1881062041881062001880062041883062) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2c80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (3a018c20630818c2063a818ea062a20a0000000000000208039018e40638818e00638018e0063a018e40639018e40638818e40639018e40639018e00638018e00639018e406080020000000000000000038808e20638818e60639808c20239808e20638818e20638818e20638808e20638808e60
639818e60638818e206280000000000000000a8802b01884062b018ac063b01884062b018ac06ab018ac062b018ac06210188406ab01aac062b018ac062b018ac062a20200000000000000000020104004028100804020100a04020100804020100804020100804000100004020100804020104804020100804000
120000000000000000008018a006080182) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2ca0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (018010401498032600410010400498012600498012600418012600498052600498012400c100104004980126004280020000000000000a88038801c20078801e20050801420078801e20078801e20078001e20078841e21078801c20070801c20078801e2006a200000000000000080001801860
061a81862061881862061881860061801860061801860061801860061801862061881862061801860060000200000000000000080120104804b0012e8043a010e804b2032480492012480412012480492012480492012e8043a010e804920124804020020000000000000a8843a818ea0630818c00630818c20638
818ea063a818ea063a018ea063a818ea06) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2cc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (01004040105004042181004050101404052101004042a20200000000000000800080042000308042201080002000080048001080042001080042001080040001200042000080002000200042001000020000000000000080028030a00c20010a00c28030a00c28030c00c28030a00c28030a00c2
8030000c30030a00c28030a00c20010a00c000020000000000000a88008810a24808030200400030000808010220408810220408810220408800220008810a00428030a00c0881022042a2020000000000000000010810620410810420410810420410810420410810420410010420410850420410810620418810
6204108104204280020000000000000080) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2ce0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000030020c00810038400e10020400810020c06a30038c00a30020c02a30020c00830028400810020400830020c0080000a0000000000000a88030a01c20051821600058801620050801c20070801c20070001c20070801c20070801620058801620070801c2006a20200000000
00000000019000640098002e000b8082e020b2000640099002640098000640099082645099142e000b8002e0009900064002800200000000000000000188006200188006200198806620198006200180006200198006200188806210188006600190006600188006200280020000000000000a8800101004053101
0000401054040701050840401010040400) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2d00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0a22228980a26228880a22220802a220a08a0a02028080a00028880a2202a2020000000000000000018884622018804620130880c220308846221188846221188846221308846221108046220188806220188846221280020000000000000000010000400110008400230004c001300004002100
004000100004002300004000180004001100044001100004000280020000000000000a88018830620c18830620c18810620418810620c18838620e18830620c18810620c38818620c18830620c18830620c2a2020000000000000000430028c00a9002ac20ab082ac24ab0828c00ab006ac00ab0028c00ab002ac0
0ab012ac20ab082ac20ab0008c00a00002) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2d20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (2d094b525ad400000000000000000000038804e20138804e20139804e60139804e20138904e20138844e21138824e20938804e60139804e60938804e201280020000000000000a8802b02c840b2b02ca80b2102c040b2b02cac0b2b06cac0b2a02cac0b2b02cac0b2b02c840b2102c040b2b02ca
c0b2a2020000000000000000002014000d028140a0500014080502014080502114080502814084502014080502014000500014080d020140805000000000000000000000008004204108104204128104004108144200108104204108184204108104204108104a04128104a041081042041000020000000000000a
88028880a200a8080a0202008080002000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2d40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (7efc9fb727fdcbff72fefcbfff27efcbff72fffc9ff727edc9fbf27edc9fb727fdc9fb727edc0000000000000000000000be4909fa4265f0997c264909fa4bfe92f97cbfff0997cbfe92fffc27e909924265f09924264909fa426490992400000000000000000000000000000000000000000000
0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000009fff2fedc9fb727fdc9ff727edc9fbf27edc9fb72ffdc9fbf27edc9fb72fedc9fb727fdc9ff727edcbfbf2fffc000000000000000000000092b5252d090b424ad092b4242d090b5242d090b425ad
090b5242d090b4252d090b424ad092b424) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2d60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
71c2000c000040408004000c0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000bfb727ec4863721edc87b121ec487b7278dc9fb727edc9fb727edc87b1278c4863721ec487b121ec49e3727edc00
00000000000000000000bfb727fdc9fbf2) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2d80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2da0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2dc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2de0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2e00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2e20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2e40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2e60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2e80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2ea0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2ec0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2ee0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2f00) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2f20) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000071c2000c000020408004000c0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2f40) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2f60) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2f80) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2fa0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2fc0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (2fe0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3000) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3020) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3040) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3060) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3080) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (30a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (30c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (30e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3100) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000071c200
0c000060408004000c0000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3120) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3140) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3160) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3180) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (31a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (31c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (31e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3200) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3220) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3240) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3260) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3280) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (32a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (32c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000001c2000c000010408004000c0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (32e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3300) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3320) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3340) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3360) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3380) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (33a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (33c0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (33e0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3400) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3420) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3440) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3460) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (3480) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fdata0' instruction. 
SIR 8 TDI (ed) ;
SDR 2048 TDI (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff0000000000000000000000000000000069da00008000000c020000008005000ca00000008001000c000000000000000000000000000000000000000000000000
00000000000000000000000000000000000000000000000000000000000000007002000cc00000008001000c78b600008000000c0000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000
0000000000000000000000000000000000) SMASK (ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff
ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (34a0) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) ;
SDR 16 TDI (0001) TDO (0000) MASK (0000) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'serase' instruction. 
SIR 8 TDI (0a) ;
RUNTEST 37000 TCK;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) SMASK (ffffffff) TDO (f5034093) MASK (0ffeffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) TDO (00) MASK (00) ;
SDR 16 TDI (4000) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'usercode' instruction. 
SIR 8 TDI (fd) TDO (00) ;
SDR 32 TDI (12340003) SMASK (ffffffff) TDO (00000000) MASK (00000000) ;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) TDO (00) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'usercode' instruction. 
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) TDO (f5034093) MASK (0ffeffff) ;
SIR 8 TDI (e6) TDO (00) ;
RUNTEST 50 TCK;
SDR 32 TDI (00000000) TDO (12340003) MASK (ffffffff) ;
//Loading device with 'conld' instruction.
SIR 8 TDI (f0) ;
RUNTEST 110000 TCK;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) TDO (f5034093) MASK (0ffeffff) ;
//Loading device with 'ispen' instruction.
SIR 8 TDI (e8) ;
SDR 6 TDI (34) SMASK (3f) ;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) SMASK (ffffffff) TDO (f5034093) MASK (0ffeffff) ;
// Loading device with a 'faddr' instruction. 
SIR 8 TDI (eb) TDO (00) ;
SDR 16 TDI (4000) SMASK (ffff) ;
RUNTEST 1 TCK;
RUNTEST 1 TCK;
// Loading device with a 'fdata3' instruction. 
SIR 8 TDI (f3) TDO (00) ;
SDR 6 TDI (3d) SMASK (3f) TDO (00) MASK (00) ;
// Loading device with a 'fpgm' instruction. 
SIR 8 TDI (ea) TDO (00) ;
RUNTEST 1 TCK;
RUNTEST 14000 TCK;
// Loading device with a 'fvfy3' instruction. 
SIR 8 TDI (e2) TDO (00) ;
RUNTEST 1 TCK;
RUNTEST 50 TCK;
SDR 6 TDI (3d) TDO (3d) ;
//Loading device with 'conld' instruction.
SIR 8 TDI (f0) ;
RUNTEST 110000 TCK;
//Loading device with 'idcode' instruction.
SIR 8 TDI (fe) ;
SDR 32 TDI (00000000) SMASK (ffffffff) TDO (f5034093) MASK (0ffeffff) ;
//Loading device with 'ispen' instruction.
SIR 8 TDI (e8) ;
SDR 6 TDI (34) SMASK (3f) ;
//Loading device with 'conld' instruction.
SIR 8 TDI (f0) ;
RUNTEST 110000 TCK;
//Loading device with 'bypass' instruction.
SIR 8 TDI (ff) ;
TIR 0 ;
HIR 0 ;
HDR 0 ;
TDR 0 ;
TIR 0 ;
HIR 0 ;
TDR 0 ;
HDR 0 ;
SIR 8 TDI (ff) ;
SDR 1 TDI (00) SMASK (01) ;
