Release 6.3i - Par G.35
Copyright (c) 1995-2004 Xilinx, Inc.  All rights reserved.

Mon Feb 11 18:41:30 2008


NOTE: This file is designed to be imported into a spreadsheet program
such as Microsoft Excel for viewing, printing and sorting. The |
character is used as the data field separator. This file is also designed
to support parsing.

INPUT FILE:       rosctrl_map.ncd
OUTPUT FILE:      rosctrl.pad
PART TYPE:        xc2s100e
SPEED GRADE:      -7
PACKAGE:          ft256

Pinout by Pin Number:

-----|-----|-----|-----|-----|-----|-----|-----|-----|-----|-----|-----|-----|
Pin Number|Signal Name|Pin Usage|Pin Name|Direction|IO Standard|IO Bank Number|Drive (mA)|Slew Rate|Termination|IOB Delay|Voltage|Constraint|
A1|||GND||||||||||
A2|||TCK||||||||||
A3|lives_p<0>|IOB|IO_L0N_YY|INPUT|LVTTL|0|||NONE**|NONE||LOCATED|
A4|txena_in|IOB|IO_L0P_YY|INPUT|LVTTL|0|||NONE**|NONE||LOCATED|
A5|db<13>|IOB|IO_L4P_Y|BIDIR|LVTTL|0|12|SLOW|NONE**|NONE||LOCATED|
A6|db<1>|IOB|IO|BIDIR|LVTTL|0|12|SLOW|NONE**|NONE||LOCATED|
A7|db<4>|IOB|IO|BIDIR|LVTTL|0|12|SLOW|NONE**|NONE||LOCATED|
A8||DLLIOB|IO_LVDS_DLL_L8P|UNUSED||1|||||||
A9|SC_L1A_p|IOB|IO_L9N|INPUT|LVTTL|1|||NONE**|NONE||LOCATED|
A10|db<5>|IOB|IO_L11N|BIDIR|LVTTL|1|12|SLOW|NONE**|NONE||LOCATED|
A11|led<0>|IOB|IO_L13N_Y|OUTPUT|LVTTL|1|12|SLOW|NONE**|||LOCATED|
A12|cs_control|IOB|IO_L16N_YY|INPUT|LVTTL|1|||NONE**|NONE||LOCATED|
A13||IOB|IO_WRITE_L18N_YY|UNUSED||1|||||||
A14||IOB|IO_CS_L18P_YY|UNUSED||1|||||||
A15|||CCLK||||||||||
A16|||GND||||||||||
B1|||TMS||||||||||
B2|||GND||||||||||
B3|lives_p<3>|IOB|IO|INPUT|LVTTL|0|||NONE**|NONE||LOCATED|
B4|ff|IOB|IO_L1P_YY|INPUT|LVTTL|0|||NONE**|NONE||LOCATED|
B5|db<14>|IOB|IO_VREF_0_L4N_Y|BIDIR|LVTTL|0|12|SLOW|NONE**|NONE||LOCATED|
B6|hasul|IOB|IO_L5P_Y|OUTPUT|LVTTL|0|12|SLOW|NONE**|||LOCATED|
B7|db<3>|IOB|IO_L6N|BIDIR|LVTTL|0|12|SLOW|NONE**|NONE||LOCATED|
B8||GCLKIOB|GCK2|UNUSED||1|||||||
B9|fout<11>|IOB|IO_L9P|INPUT|LVTTL|1|||NONE**|NONE||LOCATED|
B10|enw|IOB|IO_L11P|INPUT|LVTTL|1|||NONE**|NONE||LOCATED|
B11|evid_p<0>|IOB|IO_VREF_1_L13P_Y|OUTPUT|LVTTL|1|12|SLOW|NONE**|||LOCATED|
B12|ros_waiting|IOB|IO_L16P_YY|OUTPUT|LVTTL|1|12|SLOW|NONE**|||LOCATED|
B13|etr_x|IOB|IO_L17P_Y|INPUT|LVTTL|1|||NONE**|NONE||LOCATED|
B14|||TDO||||||||||
B15|||GND||||||||||
B16||IOB|IO_DIN_D0_L19N_YY|UNUSED||2|||||||
C1|event_reset_p|IOB|IO_L83N_Y|INPUT|LVTTL|7|||NONE**|NONE||LOCATED|
C2||IOB|IO_L83P_Y|UNUSED||7|||||||
C3|||VCCINT||||||||1.8||
C4|sff|IOB|IO_L1N_YY|OUTPUT|LVTTL|0|12|SLOW|NONE**|||LOCATED|
C5|add<0>|IOB|IO_VREF_0_L2N_YY|INPUT|LVTTL|0|||NONE**|NONE||LOCATED|
C6|lock|IOB|IO_L5N_Y|INPUT|LVTTL|0|||NONE**|NONE||LOCATED|
C7|db<11>|IOB|IO_L6P|BIDIR|LVTTL|0|12|SLOW|NONE**|NONE||LOCATED|
C8||GCLKIOB|GCK3|UNUSED||0|||||||
C9|fout<3>|IOB|IO_L10N|INPUT|LVTTL|1|||NONE**|NONE||LOCATED|
C10|ef|IOB|IO|INPUT|LVTTL|1|||NONE**|NONE||LOCATED|
C11|evid_p<3>|IOB|IO_L14N_Y|OUTPUT|LVTTL|1|12|SLOW|NONE**|||LOCATED|
C12|valen_p|IOB|IO_L17N_Y|OUTPUT|LVTTL|1|12|SLOW|NONE**|||LOCATED|
C13|||TDI||||||||||
C14|||VCCINT||||||||1.8||
C15||IOB|IO_DOUT_BUSY_L19P_YY|UNUSED||2|||||||
C16|evid_p<8>|IOB|IO_VREF_2_L22P|OUTPUT|LVTTL|2|12|SLOW|NONE**|||LOCATED|
D1|tp<1>|IOB|IO_L82N_YY|OUTPUT|LVTTL|7|12|SLOW|NONE**|||LOCATED|
D2|cspare_0|IOB|IO_L82P_YY|INPUT|LVTTL|7|||NONE**|NONE||LOCATED|
D3||IOB|IO|UNUSED||7|||||||
D4|||VCCINT||||||||1.8||
D5|add<1>|IOB|IO_L2P_YY|INPUT|LVTTL|0|||NONE**|NONE||LOCATED|
D6|db<12>|IOB|IO_L3P_Y|BIDIR|LVTTL|0|12|SLOW|NONE**|NONE||LOCATED|
D7|db<7>|IOB|IO_VREF_0_L7N|BIDIR|LVTTL|0|12|SLOW|NONE**|NONE||LOCATED|
D8||DLLIOB|IO_LVDS_DLL_L8N|UNUSED||0|||||||
D9|clk20_p|IOB|IO_VREF_1_L10P|OUTPUT|LVTTL|1|12|SLOW|NONE**|||LOCATED|
D10|db<9>|IOB|IO_L12N_Y|BIDIR|LVTTL|1|12|SLOW|NONE**|NONE||LOCATED|
D11|L1A_p|IOB|IO_L14P_Y|INPUT|LVTTL|1|||NONE**|NONE||LOCATED|
D12|evid_p<1>|IOB|IO_VREF_1_L15P_YY|OUTPUT|LVTTL|1|12|SLOW|NONE**|||LOCATED|
D13|||VCCINT||||||||1.8||
D14|tp<0>|IOB|IO_L20P_Y|OUTPUT|LVTTL|2|12|SLOW|NONE**|||LOCATED|
D15|evid_p<11>|IOB|IO_L22N|OUTPUT|LVTTL|2|12|SLOW|NONE**|||LOCATED|
D16|ceros_done_p<3>|IOB|IO_VREF_2_L24P|INPUT|LVTTL|2|||NONE**|NONE||LOCATED|
E1|cs_fifo|IOB|IO_L80N|INPUT|LVTTL|7|||NONE**|NONE||LOCATED|
E2|add<4>|IOB|IO_L80P|INPUT|LVTTL|7|||NONE**|NONE||LOCATED|
E3|add<3>|IOB|IO_VREF_7_L81P|INPUT|LVTTL|7|||NONE**|NONE||LOCATED|
E4|add<5>|IOB|IO_L81N|INPUT|LVTTL|7|||NONE**|NONE||LOCATED|
E5|||VCCINT||||||||1.8||
E6|db<15>|IOB|IO_L3N_Y|BIDIR|LVTTL|0|12|SLOW|NONE**|NONE||LOCATED|
E7|db<8>|IOB|IO_L7P|BIDIR|LVTTL|0|12|SLOW|NONE**|NONE||LOCATED|
E8|||VCCO_0|||0|||||3.30||
E9|||VCCO_1|||1|||||3.30||
E10|db<6>|IOB|IO_L12P_Y|BIDIR|LVTTL|1|12|SLOW|NONE**|NONE||LOCATED|
E11|evid_p<2>|IOB|IO_L15N_YY|OUTPUT|LVTTL|1|12|SLOW|NONE**|||LOCATED|
E12|||VCCINT||||||||1.8||
E13|evid_p<10>|IOB|IO_L20N_Y|OUTPUT|LVTTL|2|12|SLOW|NONE**|||LOCATED|
E14|evid_p<6>|IOB|IO_L23P|OUTPUT|LVTTL|2|12|SLOW|NONE**|||LOCATED|
E15||IOB|IO_D1_L24N|UNUSED||2|||||||
E16|trg_data_p<8>|IOB|IO_L26P_Y|INPUT|LVTTL|2|||NONE**|NONE||LOCATED|
F1|evcnt_high_strobe_p|IOB|IO_L78N_YY|INPUT|LVTTL|7|||NONE**|NONE||LOCATED|
F2|bcnt_p<7>|IOB|IO_L78P_YY|INPUT|LVTTL|7|||NONE**|NONE||LOCATED|
F3|dll_locked_p|IOB|IO_L79N|OUTPUT|LVTTL|7|12|SLOW|NONE**|||LOCATED|
F4|ceros_done_p<1>|IOB|IO_VREF_7_L79P|INPUT|LVTTL|7|||NONE**|NONE||LOCATED|
F5|evcnt_low_strobe_p|IOB|IO_L77P_Y|INPUT|LVTTL|7|||NONE**|NONE||LOCATED|
F6|||GND||||||||||
F7|||VCCO_0|||0|||||3.30||
F8|||VCCO_0|||0|||||3.30||
F9|||VCCO_1|||1|||||3.30||
F10|||VCCO_1|||1|||||3.30||
F11|||GND||||||||||
F12|evid_p<7>|IOB|IO_L21P_Y|OUTPUT|LVTTL|2|12|SLOW|NONE**|||LOCATED|
F13|evid_p<9>|IOB|IO_L23N|OUTPUT|LVTTL|2|12|SLOW|NONE**|||LOCATED|
F14||IOB|IO_D2_L25P_YY|UNUSED||2|||||||
F15|dout<4>|IOB|IO_L26N_Y|TRISTATE|LVTTL|2|12|SLOW|NONE**|||LOCATED|
F16|dout<2>|IOB|IO_VREF_2_L28P|TRISTATE|LVTTL|2|12|SLOW|NONE**|||LOCATED|
G1|dout<15>|IOB|IO_L75N|TRISTATE|LVTTL|7|12|SLOW|NONE**|||LOCATED|
G2|bcnt_p<8>|IOB|IO_VREF_7_L75P|INPUT|LVTTL|7|||NONE**|NONE||LOCATED|
G3|bcnt_p<5>|IOB|IO_L76P_YY|INPUT|LVTTL|7|||NONE**|NONE||LOCATED|
G4|token_p<0>|IOB|IO_L76N_YY|OUTPUT|LVTTL|7|12|SLOW|NONE**|||LOCATED|
G5|bcnt_p<9>|IOB|IO_L77N_Y|INPUT|LVTTL|7|||NONE**|NONE||LOCATED|
G6|||VCCO_7|||7|||||3.30||
G7|||GND||||||||||
G8|||GND||||||||||
G9|||GND||||||||||
G10|||GND||||||||||
G11|||VCCO_2|||2|||||3.30||
G12|evid_p<5>|IOB|IO_L21N_Y|OUTPUT|LVTTL|2|12|SLOW|NONE**|||LOCATED|
G13|token_p<3>|IOB|IO_L25N_YY|OUTPUT|LVTTL|2|12|SLOW|NONE**|||LOCATED|
G14|evid_p<4>|IOB|IO_L27P_YY|OUTPUT|LVTTL|2|12|SLOW|NONE**|||LOCATED|
G15||IOB|IO_D3_L28N|UNUSED||2|||||||
G16|dout<7>|IOB|IO_L30P_YY|TRISTATE|LVTTL|2|12|SLOW|NONE**|||LOCATED|
H1|dout<12>|IOB|IO_IRDY_L73N_YY|TRISTATE|LVTTL|7|12|SLOW|NONE**|||LOCATED|
H2|dout<14>|IOB|IO_L73P_YY|TRISTATE|LVTTL|7|12|SLOW|NONE**|||LOCATED|
H3|dout<5>|IOB|IO_L74N_Y|TRISTATE|LVTTL|7|12|SLOW|NONE**|||LOCATED|
H4|dout<11>|IOB|IO_L74P_Y|TRISTATE|LVTTL|7|12|SLOW|NONE**|||LOCATED|
H5|||VCCO_7|||7|||||3.30||
H6|||VCCO_7|||7|||||3.30||
H7|||GND||||||||||
H8|||GND||||||||||
H9|||GND||||||||||
H10|||GND||||||||||
H11|||VCCO_2|||2|||||3.30||
H12|||VCCO_2|||2|||||3.30||
H13|ren|IOB|IO_L27N_YY|OUTPUT|LVTTL|2|12|SLOW|NONE**|||LOCATED|
H14|dout<3>|IOB|IO_L29N_Y|TRISTATE|LVTTL|2|12|SLOW|NONE**|||LOCATED|
H15|dout<0>|IOB|IO_L29P_Y|TRISTATE|LVTTL|2|12|SLOW|NONE**|||LOCATED|
H16|ceros_done_p<2>|IOB|IO_IRDY_L30N_YY|INPUT|LVTTL|2|||NONE**|NONE||LOCATED|
J1|dout<8>|IOB|IO_L71P|TRISTATE|LVTTL|6|12|SLOW|NONE**|||LOCATED|
J2|dout<9>|IOB|IO_L72P_Y|TRISTATE|LVTTL|6|12|SLOW|NONE**|||LOCATED|
J3|dout<13>|IOB|IO_L72N_Y|TRISTATE|LVTTL|6|12|SLOW|NONE**|||LOCATED|
J4|dout<1>|IOB|IO_TRDY|TRISTATE|LVTTL|6|12|SLOW|NONE**|||LOCATED|
J5|||VCCO_6|||6|||||3.30||
J6|||VCCO_6|||6|||||3.30||
J7|||GND||||||||||
J8|||GND||||||||||
J9|||GND||||||||||
J10|||GND||||||||||
J11|||VCCO_3|||3|||||3.30||
J12|||VCCO_3|||3|||||3.30||
J13|dout<10>|IOB|IO_TRDY|TRISTATE|LVTTL|3|12|SLOW|NONE**|||LOCATED|
J14||IOB|IO_D4_L32P|UNUSED||3|||||||
J15|trg_data_p<7>|IOB|IO_L31N_Y|INPUT|LVTTL|3|||NONE**|NONE||LOCATED|
J16|txena|IOB|IO_L31P_Y|TRISTATE|LVTTL|3|12|SLOW|NONE**|||LOCATED|
K1|dout<6>|IOB|IO_VREF_6_L71N|TRISTATE|LVTTL|6|12|SLOW|NONE**|||LOCATED|
K2|bcnt_p<6>|IOB|IO_L70P_YY|INPUT|LVTTL|6|||NONE**|NONE||LOCATED|
K3|token_p<1>|IOB|IO_L70N_YY|OUTPUT|LVTTL|6|12|SLOW|NONE**|||LOCATED|
K4|bcnt_strobe_p|IOB|IO_L68P_YY|INPUT|LVTTL|6|||NONE**|NONE||LOCATED|
K5|fsi|IOB|IO_L68N_YY|OUTPUT|LVTTL|6|12|SLOW|NONE**|||LOCATED|
K6|||VCCO_6|||6|||||3.30||
K7|||GND||||||||||
K8|||GND||||||||||
K9|||GND||||||||||
K10|||GND||||||||||
K11|||VCCO_3|||3|||||3.30||
K12|trg_data_p<14>|IOB|IO_L33P_YY|INPUT|LVTTL|3|||NONE**|NONE||LOCATED|
K13|trg_data_p<15>|IOB|IO_VREF_3_L32N|INPUT|LVTTL|3|||NONE**|NONE||LOCATED|
K14|ceros_done_p<0>|IOB|IO_L35P_YY|INPUT|LVTTL|3|||NONE**|NONE||LOCATED|
K15|trg_data_p<3>|IOB|IO_L34N_Y|INPUT|LVTTL|3|||NONE**|NONE||LOCATED|
K16|trg_data_p<10>|IOB|IO_L34P_Y|INPUT|LVTTL|3|||NONE**|NONE||LOCATED|
L1|token_p<2>|IOB|IO_L69P_Y|OUTPUT|LVTTL|6|12|SLOW|NONE**|||LOCATED|
L2|db<0>|IOB|IO_L69N_Y|BIDIR|LVTTL|6|12|SLOW|NONE**|NONE||LOCATED|
L3|fout<8>|IOB|IO_L67P|INPUT|LVTTL|6|||NONE**|NONE||LOCATED|
L4|lives_p<1>|IOB|IO_L65P|INPUT|LVTTL|6|||NONE**|NONE||LOCATED|
L5|wclkena_p|IOB|IO_VREF_6_L65N|OUTPUT|LVTTL|6|12|SLOW|NONE**|||LOCATED|
L6|||GND||||||||||
L7|||VCCO_5|||5|||||3.30||
L8|||VCCO_5|||5|||||3.30||
L9|||VCCO_4|||4|||||3.30||
L10|||VCCO_4|||4|||||3.30||
L11|||GND||||||||||
L12|trg_data_p<13>|IOB|IO_L33N_YY|INPUT|LVTTL|3|||NONE**|NONE||LOCATED|
L13||IOB|IO_D5_L35N_YY|UNUSED||3|||||||
L14|trg_data_p<4>|IOB|IO|INPUT|LVTTL|3|||NONE**|NONE||LOCATED|
L15|trg_data_p<5>|IOB|IO_VREF_3_L36N|INPUT|LVTTL|3|||NONE**|NONE||LOCATED|
L16||IOB|IO_D6_L36P|UNUSED||3|||||||
M1|fout<9>|IOB|IO_L66P|INPUT|LVTTL|6|||NONE**|NONE||LOCATED|
M2|load_paepaf|IOB|IO_VREF_6_L67N|INPUT|LVTTL|6|||NONE**|NONE||LOCATED|
M3|reset|IOB|IO_L64P_YY|INPUT|LVTTL|6|||NONE**|NONE||LOCATED|
M4|mrs|IOB|IO_L64N_YY|INPUT|LVTTL|6|||NONE**|NONE||LOCATED|
M5|||VCCINT||||||||1.8||
M6|doneout|IOB|IO_L55N_Y|OUTPUT|LVTTL|5|12|SLOW|NONE**|||LOCATED|
M7|fout<13>|IOB|IO_VREF_5_L53N|INPUT|LVTTL|5|||NONE**|NONE||LOCATED|
M8|||VCCO_5|||5|||||3.30||
M9|||VCCO_4|||4|||||3.30||
M10|db<10>|IOB|IO_L48P_Y|BIDIR|LVTTL|4|12|SLOW|NONE**|NONE||LOCATED|
M11|lives_p<2>|IOB|IO_VREF_4_L45P_YY|INPUT|LVTTL|4|||NONE**|NONE||LOCATED|
M12|||VCCINT||||||||1.8||
M13|trg_data_p<6>|IOB|IO|INPUT|LVTTL|3|||NONE**|NONE||LOCATED|
M14|trg_data_p<11>|IOB|IO_L39P_YY|INPUT|LVTTL|3|||NONE**|NONE||LOCATED|
M15|trg_data_p<1>|IOB|IO_VREF_3_L38N|INPUT|LVTTL|3|||NONE**|NONE||LOCATED|
M16|trg_data_p<2>|IOB|IO_L38P|INPUT|LVTTL|3|||NONE**|NONE||LOCATED|
N1|recoff_p|IOB|IO_L66N|OUTPUT|LVTTL|6|12|SLOW|NONE**|||LOCATED|
N2|cmd_p<3>|IOB|IO_L63P_Y|INPUT|LVTTL|6|||NONE**|NONE||LOCATED|
N3|fmrs|IOB|IO_L63N_Y|OUTPUT|LVTTL|6|12|SLOW|NONE**|||LOCATED|
N4|||VCCINT||||||||1.8||
N5|bcnt_p<10>|IOB|IO_L59N_YY|INPUT|LVTTL|5|||NONE**|NONE||LOCATED|
N6|bcnt_p<0>|IOB|IO_L57N_Y|INPUT|LVTTL|5|||NONE**|NONE||LOCATED|
N7|cspare_1|IOB|IO_L55P_Y|INPUT|LVTTL|5|||NONE**|NONE||LOCATED|
N8|fout<6>|IOB|IO_L53P|INPUT|LVTTL|5|||NONE**|NONE||LOCATED|
N9|par<1>|IOB|IO_L51P|INPUT|LVTTL|4|||NONE**|NONE||LOCATED|
N10|fout<2>|IOB|IO_L48N_Y|INPUT|LVTTL|4|||NONE**|NONE||LOCATED|
N11|cmd_p<1>|IOB|IO_L45N_YY|INPUT|LVTTL|4|||NONE**|NONE||LOCATED|
N12|tp<3>|IOB|IO_L44P_YY|OUTPUT|LVTTL|4|12|SLOW|NONE**|||LOCATED|
N13|||VCCINT||||||||1.8||
N14|trg_data_p<0>|IOB|IO_L39N_YY|INPUT|LVTTL|3|||NONE**|NONE||LOCATED|
N15|add<2>|IOB|IO_L40N_Y|INPUT|LVTTL|3|||NONE**|NONE||LOCATED|
N16|ros_ready|IOB|IO_L40P_Y|OUTPUT|LVTTL|3|12|SLOW|NONE**|||LOCATED|
P1||IOB|IO_L62P_YY|UNUSED||6|||||||
P2|tp<2>|IOB|IO_L62N_YY|OUTPUT|LVTTL|6|12|SLOW|NONE**|||LOCATED|
P3|||VCCINT||||||||1.8||
P4|cmd_p<2>|IOB|IO_L61N_YY|INPUT|LVTTL|5|||NONE**|NONE||LOCATED|
P5|bcnt_p<3>|IOB|IO_L59P_YY|INPUT|LVTTL|5|||NONE**|NONE||LOCATED|
P6|fout<15>|IOB|IO_L57P_Y|INPUT|LVTTL|5|||NONE**|NONE||LOCATED|
P7|fout<10>|IOB|IO|INPUT|LVTTL|5|||NONE**|NONE||LOCATED|
P8|bcnt_p<2>|IOB|IO|INPUT|LVTTL|5|||NONE**|NONE||LOCATED|
P9|par<0>|IOB|IO_L51N|INPUT|LVTTL|4|||NONE**|NONE||LOCATED|
P10|fout<7>|IOB|IO_L49N|INPUT|LVTTL|4|||NONE**|NONE||LOCATED|
P11|paf|IOB|IO_L47N_Y|INPUT|LVTTL|4|||NONE**|NONE||LOCATED|
P12|bcnt_res_p|IOB|IO_L44N_YY|INPUT|LVTTL|4|||NONE**|NONE||LOCATED|
P13|trg_strobe_p|IOB|IO_L43P|INPUT|LVTTL|4|||NONE**|NONE||LOCATED|
P14|||VCCINT||||||||1.8||
P15||IOB|IO_INIT_L41N_YY|UNUSED||3|||||||
P16||IOB|IO_D7_L41P_YY|UNUSED||3|||||||
R1|||M1||||||||||
R2|||GND||||||||||
R3|||M2||||||||||
R4||IOB|IO_L61P_YY|UNUSED||5|||||||
R5|fout<5>|IOB|IO_VREF_5_L58N_YY|INPUT|LVTTL|5|||NONE**|NONE||LOCATED|
R6|bcnt_p<4>|IOB|IO_VREF_5_L56N_Y|INPUT|LVTTL|5|||NONE**|NONE||LOCATED|
R7|fout<14>|IOB|IO_L54N|INPUT|LVTTL|5|||NONE**|NONE||LOCATED|
R8||DLLIOB|IO_LVDS_DLL_L52N|UNUSED||5|||||||
R9||DLLIOB|IO_LVDS_DLL_L52P|UNUSED||4|||||||
R10|fout<0>|IOB|IO_VREF_4_L50P|INPUT|LVTTL|4|||NONE**|NONE||LOCATED|
R11|db<2>|IOB|IO_L49P|BIDIR|LVTTL|4|12|SLOW|NONE**|NONE||LOCATED|
R12|spaf_p|IOB|IO_VREF_4_L47P_Y|OUTPUT|LVTTL|4|12|SLOW|NONE**|||LOCATED|
R13|led<1>|IOB|IO_L43N|OUTPUT|LVTTL|4|12|SLOW|NONE**|||LOCATED|
R14|trg_data_p<9>|IOB|IO_L42P_YY|INPUT|LVTTL|4|||NONE**|NONE||LOCATED|
R15|||GND||||||||||
R16|||PROGRAM||||||||||
T1|||GND||||||||||
T2|||M0||||||||||
T3|fld|IOB|IO_L60N_Y|OUTPUT|LVTTL|5|12|SLOW|NONE**|||LOCATED|
T4|fsen|IOB|IO_L60P_Y|OUTPUT|LVTTL|5|12|SLOW|NONE**|||LOCATED|
T5|bcnt_p<1>|IOB|IO_L58P_YY|INPUT|LVTTL|5|||NONE**|NONE||LOCATED|
T6|bcnt_p<11>|IOB|IO_L56P_Y|INPUT|LVTTL|5|||NONE**|NONE||LOCATED|
T7|fout<12>|IOB|IO_L54P|INPUT|LVTTL|5|||NONE**|NONE||LOCATED|
T8|clkin_p|GCLKIOB|GCK1|INPUT|LVTTL|5||||||LOCATED|
T9|clk_slow|GCLKIOB|GCK0|INPUT|LVTTL|4||||||LOCATED|
T10|fout<4>|IOB|IO_L50N|INPUT|LVTTL|4|||NONE**|NONE||LOCATED|
T11|fout<1>|IOB|IO|INPUT|LVTTL|4|||NONE**|NONE||LOCATED|
T12|cmd_p<0>|IOB|IO_L46N_Y|INPUT|LVTTL|4|||NONE**|NONE||LOCATED|
T13|is_trigger|IOB|IO_L46P_Y|OUTPUT|LVTTL|4|12|SLOW|NONE**|||LOCATED|
T14|trg_data_p<12>|IOB|IO_L42N_YY|INPUT|LVTTL|4|||NONE**|NONE||LOCATED|
T15|||DONE||||||||||
T16|||GND||||||||||

-----|-----|-----|-----|-----|-----|-----|-----|-----|-----|-----|-----|-----|

* Default value.
** This default Pullup/Pulldown value can be overridden in Bitgen.

