Release 6.3i - Par G.35
Copyright (c) 1995-2004 Xilinx, Inc.  All rights reserved.

Fri Dec 05 10:30:52 2014


INPUT FILE:       rosctrl_map.ncd
OUTPUT FILE:      rosctrl_pad.txt
PART TYPE:        xc2s100e
SPEED GRADE:      -7
PACKAGE:          ft256

Pinout by Pin Number:

-----     |-----              |-----    |-----               |-----    |-----      |-----         |-----     |-----    |-----      |-----    |-----  |-----     |
Pin Number|Signal Name        |Pin Usage|Pin Name            |Direction|IO Standard|IO Bank Number|Drive (mA)|Slew Rate|Termination|IOB Delay|Voltage|Constraint|
A1        |                   |         |GND                 |         |           |              |          |         |           |         |       |          |
A2        |                   |         |TCK                 |         |           |              |          |         |           |         |       |          |
A3        |lives_p<0>         |IOB      |IO_L0N_YY           |INPUT    |LVTTL      |0             |          |         |NONE**     |NONE     |       |LOCATED   |
A4        |txena_in           |IOB      |IO_L0P_YY           |INPUT    |LVTTL      |0             |          |         |NONE**     |NONE     |       |LOCATED   |
A5        |db<13>             |IOB      |IO_L4P_Y            |BIDIR    |LVTTL      |0             |12        |SLOW     |NONE**     |NONE     |       |LOCATED   |
A6        |db<1>              |IOB      |IO                  |BIDIR    |LVTTL      |0             |12        |SLOW     |NONE**     |NONE     |       |LOCATED   |
A7        |db<4>              |IOB      |IO                  |BIDIR    |LVTTL      |0             |12        |SLOW     |NONE**     |NONE     |       |LOCATED   |
A8        |                   |DLLIOB   |IO_LVDS_DLL_L8P     |UNUSED   |           |1             |          |         |           |         |       |          |
A9        |SC_L1A_p           |IOB      |IO_L9N              |INPUT    |LVTTL      |1             |          |         |NONE**     |NONE     |       |LOCATED   |
A10       |db<5>              |IOB      |IO_L11N             |BIDIR    |LVTTL      |1             |12        |SLOW     |NONE**     |NONE     |       |LOCATED   |
A11       |led<0>             |IOB      |IO_L13N_Y           |OUTPUT   |LVTTL      |1             |12        |SLOW     |NONE**     |         |       |LOCATED   |
A12       |cs_control         |IOB      |IO_L16N_YY          |INPUT    |LVTTL      |1             |          |         |NONE**     |NONE     |       |LOCATED   |
A13       |                   |IOB      |IO_WRITE_L18N_YY    |UNUSED   |           |1             |          |         |           |         |       |          |
A14       |                   |IOB      |IO_CS_L18P_YY       |UNUSED   |           |1             |          |         |           |         |       |          |
A15       |                   |         |CCLK                |         |           |              |          |         |           |         |       |          |
A16       |                   |         |GND                 |         |           |              |          |         |           |         |       |          |
B1        |                   |         |TMS                 |         |           |              |          |         |           |         |       |          |
B2        |                   |         |GND                 |         |           |              |          |         |           |         |       |          |
B3        |lives_p<3>         |IOB      |IO                  |INPUT    |LVTTL      |0             |          |         |NONE**     |NONE     |       |LOCATED   |
B4        |ff                 |IOB      |IO_L1P_YY           |INPUT    |LVTTL      |0             |          |         |NONE**     |NONE     |       |LOCATED   |
B5        |db<14>             |IOB      |IO_VREF_0_L4N_Y     |BIDIR    |LVTTL      |0             |12        |SLOW     |NONE**     |NONE     |       |LOCATED   |
B6        |hasul              |IOB      |IO_L5P_Y            |OUTPUT   |LVTTL      |0             |12        |SLOW     |NONE**     |         |       |LOCATED   |
B7        |db<3>              |IOB      |IO_L6N              |BIDIR    |LVTTL      |0             |12        |SLOW     |NONE**     |NONE     |       |LOCATED   |
B8        |                   |GCLKIOB  |GCK2                |UNUSED   |           |1             |          |         |           |         |       |          |
B9        |fout<11>           |IOB      |IO_L9P              |INPUT    |LVTTL      |1             |          |         |NONE**     |NONE     |       |LOCATED   |
B10       |enw                |IOB      |IO_L11P             |INPUT    |LVTTL      |1             |          |         |NONE**     |NONE     |       |LOCATED   |
B11       |evid_p<0>          |IOB      |IO_VREF_1_L13P_Y    |OUTPUT   |LVTTL      |1             |12        |SLOW     |NONE**     |         |       |LOCATED   |
B12       |ros_waiting        |IOB      |IO_L16P_YY          |OUTPUT   |LVTTL      |1             |12        |SLOW     |NONE**     |         |       |LOCATED   |
B13       |etr_x              |IOB      |IO_L17P_Y           |INPUT    |LVTTL      |1             |          |         |NONE**     |NONE     |       |LOCATED   |
B14       |                   |         |TDO                 |         |           |              |          |         |           |         |       |          |
B15       |                   |         |GND                 |         |           |              |          |         |           |         |       |          |
B16       |                   |IOB      |IO_DIN_D0_L19N_YY   |UNUSED   |           |2             |          |         |           |         |       |          |
C1        |event_reset_p      |IOB      |IO_L83N_Y           |INPUT    |LVTTL      |7             |          |         |NONE**     |NONE     |       |LOCATED   |
C2        |                   |IOB      |IO_L83P_Y           |UNUSED   |           |7             |          |         |           |         |       |          |
C3        |                   |         |VCCINT              |         |           |              |          |         |           |         |1.8    |          |
C4        |TTChardreset_p     |IOB      |IO_L1N_YY           |OUTPUT   |LVTTL      |0             |12        |SLOW     |NONE**     |         |       |LOCATED   |
C5        |add<0>             |IOB      |IO_VREF_0_L2N_YY    |INPUT    |LVTTL      |0             |          |         |NONE**     |NONE     |       |LOCATED   |
C6        |lock               |IOB      |IO_L5N_Y            |INPUT    |LVTTL      |0             |          |         |NONE**     |NONE     |       |LOCATED   |
C7        |db<11>             |IOB      |IO_L6P              |BIDIR    |LVTTL      |0             |12        |SLOW     |NONE**     |NONE     |       |LOCATED   |
C8        |                   |GCLKIOB  |GCK3                |UNUSED   |           |0             |          |         |           |         |       |          |
C9        |fout<3>            |IOB      |IO_L10N             |INPUT    |LVTTL      |1             |          |         |NONE**     |NONE     |       |LOCATED   |
C10       |ef                 |IOB      |IO                  |INPUT    |LVTTL      |1             |          |         |NONE**     |NONE     |       |LOCATED   |
C11       |evid_p<3>          |IOB      |IO_L14N_Y           |OUTPUT   |LVTTL      |1             |12        |SLOW     |NONE**     |         |       |LOCATED   |
C12       |valen_p            |IOB      |IO_L17N_Y           |OUTPUT   |LVTTL      |1             |12        |SLOW     |NONE**     |         |       |LOCATED   |
C13       |                   |         |TDI                 |         |           |              |          |         |           |         |       |          |
C14       |                   |         |VCCINT              |         |           |              |          |         |           |         |1.8    |          |
C15       |                   |IOB      |IO_DOUT_BUSY_L19P_YY|UNUSED   |           |2             |          |         |           |         |       |          |
C16       |evid_p<8>          |IOB      |IO_VREF_2_L22P      |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |
D1        |tp<1>              |IOB      |IO_L82N_YY          |OUTPUT   |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |
D2        |softreset_RM       |IOB      |IO_L82P_YY          |INPUT    |LVTTL      |7             |          |         |NONE**     |NONE     |       |LOCATED   |
D3        |                   |IOB      |IO                  |UNUSED   |           |7             |          |         |           |         |       |          |
D4        |                   |         |VCCINT              |         |           |              |          |         |           |         |1.8    |          |
D5        |add<1>             |IOB      |IO_L2P_YY           |INPUT    |LVTTL      |0             |          |         |NONE**     |NONE     |       |LOCATED   |
D6        |db<12>             |IOB      |IO_L3P_Y            |BIDIR    |LVTTL      |0             |12        |SLOW     |NONE**     |NONE     |       |LOCATED   |
D7        |db<7>              |IOB      |IO_VREF_0_L7N       |BIDIR    |LVTTL      |0             |12        |SLOW     |NONE**     |NONE     |       |LOCATED   |
D8        |                   |DLLIOB   |IO_LVDS_DLL_L8N     |UNUSED   |           |0             |          |         |           |         |       |          |
D9        |clk20_p            |IOB      |IO_VREF_1_L10P      |OUTPUT   |LVTTL      |1             |12        |SLOW     |NONE**     |         |       |LOCATED   |
D10       |db<9>              |IOB      |IO_L12N_Y           |BIDIR    |LVTTL      |1             |12        |SLOW     |NONE**     |NONE     |       |LOCATED   |
D11       |L1A_p              |IOB      |IO_L14P_Y           |INPUT    |LVTTL      |1             |          |         |NONE**     |NONE     |       |LOCATED   |
D12       |evid_p<1>          |IOB      |IO_VREF_1_L15P_YY   |OUTPUT   |LVTTL      |1             |12        |SLOW     |NONE**     |         |       |LOCATED   |
D13       |                   |         |VCCINT              |         |           |              |          |         |           |         |1.8    |          |
D14       |tp<0>              |IOB      |IO_L20P_Y           |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |
D15       |evid_p<11>         |IOB      |IO_L22N             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |
D16       |ceros_done_p<3>    |IOB      |IO_VREF_2_L24P      |INPUT    |LVTTL      |2             |          |         |NONE**     |NONE     |       |LOCATED   |
E1        |cs_fifo            |IOB      |IO_L80N             |INPUT    |LVTTL      |7             |          |         |NONE**     |NONE     |       |LOCATED   |
E2        |add<4>             |IOB      |IO_L80P             |INPUT    |LVTTL      |7             |          |         |NONE**     |NONE     |       |LOCATED   |
E3        |add<3>             |IOB      |IO_VREF_7_L81P      |INPUT    |LVTTL      |7             |          |         |NONE**     |NONE     |       |LOCATED   |
E4        |add<5>             |IOB      |IO_L81N             |INPUT    |LVTTL      |7             |          |         |NONE**     |NONE     |       |LOCATED   |
E5        |                   |         |VCCINT              |         |           |              |          |         |           |         |1.8    |          |
E6        |db<15>             |IOB      |IO_L3N_Y            |BIDIR    |LVTTL      |0             |12        |SLOW     |NONE**     |NONE     |       |LOCATED   |
E7        |db<8>              |IOB      |IO_L7P              |BIDIR    |LVTTL      |0             |12        |SLOW     |NONE**     |NONE     |       |LOCATED   |
E8        |                   |         |VCCO_0              |         |           |0             |          |         |           |         |3.30   |          |
E9        |                   |         |VCCO_1              |         |           |1             |          |         |           |         |3.30   |          |
E10       |db<6>              |IOB      |IO_L12P_Y           |BIDIR    |LVTTL      |1             |12        |SLOW     |NONE**     |NONE     |       |LOCATED   |
E11       |evid_p<2>          |IOB      |IO_L15N_YY          |OUTPUT   |LVTTL      |1             |12        |SLOW     |NONE**     |         |       |LOCATED   |
E12       |                   |         |VCCINT              |         |           |              |          |         |           |         |1.8    |          |
E13       |evid_p<10>         |IOB      |IO_L20N_Y           |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |
E14       |evid_p<6>          |IOB      |IO_L23P             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |
E15       |                   |IOB      |IO_D1_L24N          |UNUSED   |           |2             |          |         |           |         |       |          |
E16       |trg_data_p<8>      |IOB      |IO_L26P_Y           |INPUT    |LVTTL      |2             |          |         |NONE**     |NONE     |       |LOCATED   |
F1        |evcnt_high_strobe_p|IOB      |IO_L78N_YY          |INPUT    |LVTTL      |7             |          |         |NONE**     |NONE     |       |LOCATED   |
F2        |bcnt_p<7>          |IOB      |IO_L78P_YY          |INPUT    |LVTTL      |7             |          |         |NONE**     |NONE     |       |LOCATED   |
F3        |dll_locked_p       |IOB      |IO_L79N             |OUTPUT   |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |
F4        |ceros_done_p<1>    |IOB      |IO_VREF_7_L79P      |INPUT    |LVTTL      |7             |          |         |NONE**     |NONE     |       |LOCATED   |
F5        |evcnt_low_strobe_p |IOB      |IO_L77P_Y           |INPUT    |LVTTL      |7             |          |         |NONE**     |NONE     |       |LOCATED   |
F6        |                   |         |GND                 |         |           |              |          |         |           |         |       |          |
F7        |                   |         |VCCO_0              |         |           |0             |          |         |           |         |3.30   |          |
F8        |                   |         |VCCO_0              |         |           |0             |          |         |           |         |3.30   |          |
F9        |                   |         |VCCO_1              |         |           |1             |          |         |           |         |3.30   |          |
F10       |                   |         |VCCO_1              |         |           |1             |          |         |           |         |3.30   |          |
F11       |                   |         |GND                 |         |           |              |          |         |           |         |       |          |
F12       |evid_p<7>          |IOB      |IO_L21P_Y           |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |
F13       |evid_p<9>          |IOB      |IO_L23N             |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |
F14       |                   |IOB      |IO_D2_L25P_YY       |UNUSED   |           |2             |          |         |           |         |       |          |
F15       |dout<4>            |IOB      |IO_L26N_Y           |TRISTATE |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |
F16       |dout<2>            |IOB      |IO_VREF_2_L28P      |TRISTATE |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |
G1        |dout<15>           |IOB      |IO_L75N             |TRISTATE |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |
G2        |bcnt_p<8>          |IOB      |IO_VREF_7_L75P      |INPUT    |LVTTL      |7             |          |         |NONE**     |NONE     |       |LOCATED   |
G3        |bcnt_p<5>          |IOB      |IO_L76P_YY          |INPUT    |LVTTL      |7             |          |         |NONE**     |NONE     |       |LOCATED   |
G4        |token_p<0>         |IOB      |IO_L76N_YY          |OUTPUT   |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |
G5        |bcnt_p<9>          |IOB      |IO_L77N_Y           |INPUT    |LVTTL      |7             |          |         |NONE**     |NONE     |       |LOCATED   |
G6        |                   |         |VCCO_7              |         |           |7             |          |         |           |         |3.30   |          |
G7        |                   |         |GND                 |         |           |              |          |         |           |         |       |          |
G8        |                   |         |GND                 |         |           |              |          |         |           |         |       |          |
G9        |                   |         |GND                 |         |           |              |          |         |           |         |       |          |
G10       |                   |         |GND                 |         |           |              |          |         |           |         |       |          |
G11       |                   |         |VCCO_2              |         |           |2             |          |         |           |         |3.30   |          |
G12       |evid_p<5>          |IOB      |IO_L21N_Y           |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |
G13       |token_p<3>         |IOB      |IO_L25N_YY          |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |
G14       |evid_p<4>          |IOB      |IO_L27P_YY          |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |
G15       |                   |IOB      |IO_D3_L28N          |UNUSED   |           |2             |          |         |           |         |       |          |
G16       |dout<7>            |IOB      |IO_L30P_YY          |TRISTATE |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |
H1        |dout<12>           |IOB      |IO_IRDY_L73N_YY     |TRISTATE |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |
H2        |dout<14>           |IOB      |IO_L73P_YY          |TRISTATE |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |
H3        |dout<5>            |IOB      |IO_L74N_Y           |TRISTATE |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |
H4        |dout<11>           |IOB      |IO_L74P_Y           |TRISTATE |LVTTL      |7             |12        |SLOW     |NONE**     |         |       |LOCATED   |
H5        |                   |         |VCCO_7              |         |           |7             |          |         |           |         |3.30   |          |
H6        |                   |         |VCCO_7              |         |           |7             |          |         |           |         |3.30   |          |
H7        |                   |         |GND                 |         |           |              |          |         |           |         |       |          |
H8        |                   |         |GND                 |         |           |              |          |         |           |         |       |          |
H9        |                   |         |GND                 |         |           |              |          |         |           |         |       |          |
H10       |                   |         |GND                 |         |           |              |          |         |           |         |       |          |
H11       |                   |         |VCCO_2              |         |           |2             |          |         |           |         |3.30   |          |
H12       |                   |         |VCCO_2              |         |           |2             |          |         |           |         |3.30   |          |
H13       |ren                |IOB      |IO_L27N_YY          |OUTPUT   |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |
H14       |dout<3>            |IOB      |IO_L29N_Y           |TRISTATE |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |
H15       |dout<0>            |IOB      |IO_L29P_Y           |TRISTATE |LVTTL      |2             |12        |SLOW     |NONE**     |         |       |LOCATED   |
H16       |ceros_done_p<2>    |IOB      |IO_IRDY_L30N_YY     |INPUT    |LVTTL      |2             |          |         |NONE**     |NONE     |       |LOCATED   |
J1        |dout<8>            |IOB      |IO_L71P             |TRISTATE |LVTTL      |6             |12        |SLOW     |NONE**     |         |       |LOCATED   |
J2        |dout<9>            |IOB      |IO_L72P_Y           |TRISTATE |LVTTL      |6             |12        |SLOW     |NONE**     |         |       |LOCATED   |
J3        |dout<13>           |IOB      |IO_L72N_Y           |TRISTATE |LVTTL      |6             |12        |SLOW     |NONE**     |         |       |LOCATED   |
J4        |dout<1>            |IOB      |IO_TRDY             |TRISTATE |LVTTL      |6             |12        |SLOW     |NONE**     |         |       |LOCATED   |
J5        |                   |         |VCCO_6              |         |           |6             |          |         |           |         |3.30   |          |
J6        |                   |         |VCCO_6              |         |           |6             |          |         |           |         |3.30   |          |
J7        |                   |         |GND                 |         |           |              |          |         |           |         |       |          |
J8        |                   |         |GND                 |         |           |              |          |         |           |         |       |          |
J9        |                   |         |GND                 |         |           |              |          |         |           |         |       |          |
J10       |                   |         |GND                 |         |           |              |          |         |           |         |       |          |
J11       |                   |         |VCCO_3              |         |           |3             |          |         |           |         |3.30   |          |
J12       |                   |         |VCCO_3              |         |           |3             |          |         |           |         |3.30   |          |
J13       |dout<10>           |IOB      |IO_TRDY             |TRISTATE |LVTTL      |3             |12        |SLOW     |NONE**     |         |       |LOCATED   |
J14       |                   |IOB      |IO_D4_L32P          |UNUSED   |           |3             |          |         |           |         |       |          |
J15       |trg_data_p<7>      |IOB      |IO_L31N_Y           |INPUT    |LVTTL      |3             |          |         |NONE**     |NONE     |       |LOCATED   |
J16       |txena              |IOB      |IO_L31P_Y           |TRISTATE |LVTTL      |3             |12        |SLOW     |NONE**     |         |       |LOCATED   |
K1        |dout<6>            |IOB      |IO_VREF_6_L71N      |TRISTATE |LVTTL      |6             |12        |SLOW     |NONE**     |         |       |LOCATED   |
K2        |bcnt_p<6>          |IOB      |IO_L70P_YY          |INPUT    |LVTTL      |6             |          |         |NONE**     |NONE     |       |LOCATED   |
K3        |token_p<1>         |IOB      |IO_L70N_YY          |OUTPUT   |LVTTL      |6             |12        |SLOW     |NONE**     |         |       |LOCATED   |
K4        |bcnt_strobe_p      |IOB      |IO_L68P_YY          |INPUT    |LVTTL      |6             |          |         |NONE**     |NONE     |       |LOCATED   |
K5        |fsi                |IOB      |IO_L68N_YY          |OUTPUT   |LVTTL      |6             |12        |SLOW     |NONE**     |         |       |LOCATED   |
K6        |                   |         |VCCO_6              |         |           |6             |          |         |           |         |3.30   |          |
K7        |                   |         |GND                 |         |           |              |          |         |           |         |       |          |
K8        |                   |         |GND                 |         |           |              |          |         |           |         |       |          |
K9        |                   |         |GND                 |         |           |              |          |         |           |         |       |          |
K10       |                   |         |GND                 |         |           |              |          |         |           |         |       |          |
K11       |                   |         |VCCO_3              |         |           |3             |          |         |           |         |3.30   |          |
K12       |trg_data_p<14>     |IOB      |IO_L33P_YY          |INPUT    |LVTTL      |3             |          |         |NONE**     |NONE     |       |LOCATED   |
K13       |trg_data_p<15>     |IOB      |IO_VREF_3_L32N      |INPUT    |LVTTL      |3             |          |         |NONE**     |NONE     |       |LOCATED   |
K14       |ceros_done_p<0>    |IOB      |IO_L35P_YY          |INPUT    |LVTTL      |3             |          |         |NONE**     |NONE     |       |LOCATED   |
K15       |trg_data_p<3>      |IOB      |IO_L34N_Y           |INPUT    |LVTTL      |3             |          |         |NONE**     |NONE     |       |LOCATED   |
K16       |trg_data_p<10>     |IOB      |IO_L34P_Y           |INPUT    |LVTTL      |3             |          |         |NONE**     |NONE     |       |LOCATED   |
L1        |token_p<2>         |IOB      |IO_L69P_Y           |OUTPUT   |LVTTL      |6             |12        |SLOW     |NONE**     |         |       |LOCATED   |
L2        |db<0>              |IOB      |IO_L69N_Y           |BIDIR    |LVTTL      |6             |12        |SLOW     |NONE**     |NONE     |       |LOCATED   |
L3        |fout<8>            |IOB      |IO_L67P             |INPUT    |LVTTL      |6             |          |         |NONE**     |NONE     |       |LOCATED   |
L4        |lives_p<1>         |IOB      |IO_L65P             |INPUT    |LVTTL      |6             |          |         |NONE**     |NONE     |       |LOCATED   |
L5        |wclkena_p          |IOB      |IO_VREF_6_L65N      |OUTPUT   |LVTTL      |6             |12        |SLOW     |NONE**     |         |       |LOCATED   |
L6        |                   |         |GND                 |         |           |              |          |         |           |         |       |          |
L7        |                   |         |VCCO_5              |         |           |5             |          |         |           |         |3.30   |          |
L8        |                   |         |VCCO_5              |         |           |5             |          |         |           |         |3.30   |          |
L9        |                   |         |VCCO_4              |         |           |4             |          |         |           |         |3.30   |          |
L10       |                   |         |VCCO_4              |         |           |4             |          |         |           |         |3.30   |          |
L11       |                   |         |GND                 |         |           |              |          |         |           |         |       |          |
L12       |trg_data_p<13>     |IOB      |IO_L33N_YY          |INPUT    |LVTTL      |3             |          |         |NONE**     |NONE     |       |LOCATED   |
L13       |                   |IOB      |IO_D5_L35N_YY       |UNUSED   |           |3             |          |         |           |         |       |          |
L14       |trg_data_p<4>      |IOB      |IO                  |INPUT    |LVTTL      |3             |          |         |NONE**     |NONE     |       |LOCATED   |
L15       |trg_data_p<5>      |IOB      |IO_VREF_3_L36N      |INPUT    |LVTTL      |3             |          |         |NONE**     |NONE     |       |LOCATED   |
L16       |                   |IOB      |IO_D6_L36P          |UNUSED   |           |3             |          |         |           |         |       |          |
M1        |fout<9>            |IOB      |IO_L66P             |INPUT    |LVTTL      |6             |          |         |NONE**     |NONE     |       |LOCATED   |
M2        |load_paepaf        |IOB      |IO_VREF_6_L67N      |INPUT    |LVTTL      |6             |          |         |NONE**     |NONE     |       |LOCATED   |
M3        |reset              |IOB      |IO_L64P_YY          |INPUT    |LVTTL      |6             |          |         |NONE**     |NONE     |       |LOCATED   |
M4        |mrs                |IOB      |IO_L64N_YY          |INPUT    |LVTTL      |6             |          |         |NONE**     |NONE     |       |LOCATED   |
M5        |                   |         |VCCINT              |         |           |              |          |         |           |         |1.8    |          |
M6        |doneout            |IOB      |IO_L55N_Y           |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |
M7        |fout<13>           |IOB      |IO_VREF_5_L53N      |INPUT    |LVTTL      |5             |          |         |NONE**     |NONE     |       |LOCATED   |
M8        |                   |         |VCCO_5              |         |           |5             |          |         |           |         |3.30   |          |
M9        |                   |         |VCCO_4              |         |           |4             |          |         |           |         |3.30   |          |
M10       |db<10>             |IOB      |IO_L48P_Y           |BIDIR    |LVTTL      |4             |12        |SLOW     |NONE**     |NONE     |       |LOCATED   |
M11       |lives_p<2>         |IOB      |IO_VREF_4_L45P_YY   |INPUT    |LVTTL      |4             |          |         |NONE**     |NONE     |       |LOCATED   |
M12       |                   |         |VCCINT              |         |           |              |          |         |           |         |1.8    |          |
M13       |trg_data_p<6>      |IOB      |IO                  |INPUT    |LVTTL      |3             |          |         |NONE**     |NONE     |       |LOCATED   |
M14       |trg_data_p<11>     |IOB      |IO_L39P_YY          |INPUT    |LVTTL      |3             |          |         |NONE**     |NONE     |       |LOCATED   |
M15       |trg_data_p<1>      |IOB      |IO_VREF_3_L38N      |INPUT    |LVTTL      |3             |          |         |NONE**     |NONE     |       |LOCATED   |
M16       |trg_data_p<2>      |IOB      |IO_L38P             |INPUT    |LVTTL      |3             |          |         |NONE**     |NONE     |       |LOCATED   |
N1        |recoff_p           |IOB      |IO_L66N             |OUTPUT   |LVTTL      |6             |12        |SLOW     |NONE**     |         |       |LOCATED   |
N2        |cmd_p<3>           |IOB      |IO_L63P_Y           |INPUT    |LVTTL      |6             |          |         |NONE**     |NONE     |       |LOCATED   |
N3        |fmrs               |IOB      |IO_L63N_Y           |OUTPUT   |LVTTL      |6             |12        |SLOW     |NONE**     |         |       |LOCATED   |
N4        |                   |         |VCCINT              |         |           |              |          |         |           |         |1.8    |          |
N5        |bcnt_p<10>         |IOB      |IO_L59N_YY          |INPUT    |LVTTL      |5             |          |         |NONE**     |NONE     |       |LOCATED   |
N6        |bcnt_p<0>          |IOB      |IO_L57N_Y           |INPUT    |LVTTL      |5             |          |         |NONE**     |NONE     |       |LOCATED   |
N7        |goltest_p          |IOB      |IO_L55P_Y           |INPUT    |LVTTL      |5             |          |         |NONE**     |NONE     |       |LOCATED   |
N8        |fout<6>            |IOB      |IO_L53P             |INPUT    |LVTTL      |5             |          |         |NONE**     |NONE     |       |LOCATED   |
N9        |par<1>             |IOB      |IO_L51P             |INPUT    |LVTTL      |4             |          |         |NONE**     |NONE     |       |LOCATED   |
N10       |fout<2>            |IOB      |IO_L48N_Y           |INPUT    |LVTTL      |4             |          |         |NONE**     |NONE     |       |LOCATED   |
N11       |cmd_p<1>           |IOB      |IO_L45N_YY          |INPUT    |LVTTL      |4             |          |         |NONE**     |NONE     |       |LOCATED   |
N12       |tp<3>              |IOB      |IO_L44P_YY          |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |
N13       |                   |         |VCCINT              |         |           |              |          |         |           |         |1.8    |          |
N14       |trg_data_p<0>      |IOB      |IO_L39N_YY          |INPUT    |LVTTL      |3             |          |         |NONE**     |NONE     |       |LOCATED   |
N15       |add<2>             |IOB      |IO_L40N_Y           |INPUT    |LVTTL      |3             |          |         |NONE**     |NONE     |       |LOCATED   |
N16       |ros_ready          |IOB      |IO_L40P_Y           |OUTPUT   |LVTTL      |3             |12        |SLOW     |NONE**     |         |       |LOCATED   |
P1        |                   |IOB      |IO_L62P_YY          |UNUSED   |           |6             |          |         |           |         |       |          |
P2        |tp<2>              |IOB      |IO_L62N_YY          |OUTPUT   |LVTTL      |6             |12        |SLOW     |NONE**     |         |       |LOCATED   |
P3        |                   |         |VCCINT              |         |           |              |          |         |           |         |1.8    |          |
P4        |cmd_p<2>           |IOB      |IO_L61N_YY          |INPUT    |LVTTL      |5             |          |         |NONE**     |NONE     |       |LOCATED   |
P5        |bcnt_p<3>          |IOB      |IO_L59P_YY          |INPUT    |LVTTL      |5             |          |         |NONE**     |NONE     |       |LOCATED   |
P6        |fout<15>           |IOB      |IO_L57P_Y           |INPUT    |LVTTL      |5             |          |         |NONE**     |NONE     |       |LOCATED   |
P7        |fout<10>           |IOB      |IO                  |INPUT    |LVTTL      |5             |          |         |NONE**     |NONE     |       |LOCATED   |
P8        |bcnt_p<2>          |IOB      |IO                  |INPUT    |LVTTL      |5             |          |         |NONE**     |NONE     |       |LOCATED   |
P9        |par<0>             |IOB      |IO_L51N             |INPUT    |LVTTL      |4             |          |         |NONE**     |NONE     |       |LOCATED   |
P10       |fout<7>            |IOB      |IO_L49N             |INPUT    |LVTTL      |4             |          |         |NONE**     |NONE     |       |LOCATED   |
P11       |paf                |IOB      |IO_L47N_Y           |INPUT    |LVTTL      |4             |          |         |NONE**     |NONE     |       |LOCATED   |
P12       |bcnt_res_p         |IOB      |IO_L44N_YY          |INPUT    |LVTTL      |4             |          |         |NONE**     |NONE     |       |LOCATED   |
P13       |trg_strobe_p       |IOB      |IO_L43P             |INPUT    |LVTTL      |4             |          |         |NONE**     |NONE     |       |LOCATED   |
P14       |                   |         |VCCINT              |         |           |              |          |         |           |         |1.8    |          |
P15       |                   |IOB      |IO_INIT_L41N_YY     |UNUSED   |           |3             |          |         |           |         |       |          |
P16       |                   |IOB      |IO_D7_L41P_YY       |UNUSED   |           |3             |          |         |           |         |       |          |
R1        |                   |         |M1                  |         |           |              |          |         |           |         |       |          |
R2        |                   |         |GND                 |         |           |              |          |         |           |         |       |          |
R3        |                   |         |M2                  |         |           |              |          |         |           |         |       |          |
R4        |                   |IOB      |IO_L61P_YY          |UNUSED   |           |5             |          |         |           |         |       |          |
R5        |fout<5>            |IOB      |IO_VREF_5_L58N_YY   |INPUT    |LVTTL      |5             |          |         |NONE**     |NONE     |       |LOCATED   |
R6        |bcnt_p<4>          |IOB      |IO_VREF_5_L56N_Y    |INPUT    |LVTTL      |5             |          |         |NONE**     |NONE     |       |LOCATED   |
R7        |fout<14>           |IOB      |IO_L54N             |INPUT    |LVTTL      |5             |          |         |NONE**     |NONE     |       |LOCATED   |
R8        |                   |DLLIOB   |IO_LVDS_DLL_L52N    |UNUSED   |           |5             |          |         |           |         |       |          |
R9        |                   |DLLIOB   |IO_LVDS_DLL_L52P    |UNUSED   |           |4             |          |         |           |         |       |          |
R10       |fout<0>            |IOB      |IO_VREF_4_L50P      |INPUT    |LVTTL      |4             |          |         |NONE**     |NONE     |       |LOCATED   |
R11       |db<2>              |IOB      |IO_L49P             |BIDIR    |LVTTL      |4             |12        |SLOW     |NONE**     |NONE     |       |LOCATED   |
R12       |softreset_RV       |IOB      |IO_VREF_4_L47P_Y    |INPUT    |LVTTL      |4             |          |         |NONE**     |NONE     |       |LOCATED   |
R13       |led<1>             |IOB      |IO_L43N             |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |
R14       |trg_data_p<9>      |IOB      |IO_L42P_YY          |INPUT    |LVTTL      |4             |          |         |NONE**     |NONE     |       |LOCATED   |
R15       |                   |         |GND                 |         |           |              |          |         |           |         |       |          |
R16       |                   |         |PROGRAM             |         |           |              |          |         |           |         |       |          |
T1        |                   |         |GND                 |         |           |              |          |         |           |         |       |          |
T2        |                   |         |M0                  |         |           |              |          |         |           |         |       |          |
T3        |fld                |IOB      |IO_L60N_Y           |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |
T4        |fsen               |IOB      |IO_L60P_Y           |OUTPUT   |LVTTL      |5             |12        |SLOW     |NONE**     |         |       |LOCATED   |
T5        |bcnt_p<1>          |IOB      |IO_L58P_YY          |INPUT    |LVTTL      |5             |          |         |NONE**     |NONE     |       |LOCATED   |
T6        |bcnt_p<11>         |IOB      |IO_L56P_Y           |INPUT    |LVTTL      |5             |          |         |NONE**     |NONE     |       |LOCATED   |
T7        |fout<12>           |IOB      |IO_L54P             |INPUT    |LVTTL      |5             |          |         |NONE**     |NONE     |       |LOCATED   |
T8        |clkin_p            |GCLKIOB  |GCK1                |INPUT    |LVTTL      |5             |          |         |           |         |       |LOCATED   |
T9        |clk_slow           |GCLKIOB  |GCK0                |INPUT    |LVTTL      |4             |          |         |           |         |       |LOCATED   |
T10       |fout<4>            |IOB      |IO_L50N             |INPUT    |LVTTL      |4             |          |         |NONE**     |NONE     |       |LOCATED   |
T11       |fout<1>            |IOB      |IO                  |INPUT    |LVTTL      |4             |          |         |NONE**     |NONE     |       |LOCATED   |
T12       |cmd_p<0>           |IOB      |IO_L46N_Y           |INPUT    |LVTTL      |4             |          |         |NONE**     |NONE     |       |LOCATED   |
T13       |is_trigger         |IOB      |IO_L46P_Y           |OUTPUT   |LVTTL      |4             |12        |SLOW     |NONE**     |         |       |LOCATED   |
T14       |trg_data_p<12>     |IOB      |IO_L42N_YY          |INPUT    |LVTTL      |4             |          |         |NONE**     |NONE     |       |LOCATED   |
T15       |                   |         |DONE                |         |           |              |          |         |           |         |       |          |
T16       |                   |         |GND                 |         |           |              |          |         |           |         |       |          |

-----     |-----              |-----    |-----               |-----    |-----      |-----         |-----     |-----    |-----      |-----    |-----  |-----     |

* Default value.
** This default Pullup/Pulldown value can be overridden in Bitgen.

