### Compiler Options

Option | Value
--- | ---
Device(s) Specified | xc2c512-7-PQ208
Optimization Method | DENSITY
Multi-Level Logic Optimization | ON
Ignore Timing Specifications | OFF
Default Register Power Up Value | LOW
Slew Rate | FAST
Keep User Location Constraints | ON
What-You-See-Is-What-You-Get | OFF
Exhaustive Fitting | OFF
Keep Unused Inputs | OFF
Set Unused I/O Pin Termination | FLOAT
Global Clock Optimization | ON
Global Set/Reset Optimization | ON
Global Ouput Enable Optimization | ON
Enable Input Registers | ON
Function Block Fan-in Limit | 38
Set Tristate Outputs to Termination Mode | KEEPER
Use DATA_GATE Attribute | ON
Default Voltage Standard for All Outputs | LVCMOS18
Input Limit (4-40) | 38
Pterm Limit (3-56) | 50