    cpldfit:  version G.35                              Xilinx Inc.
                                      Fitter Report
    Design Name: ffrp                                Date:  2-27-2006,  1:05PM
    Device Used: XC2C512-7-PQ208
    Fitting Status: Successful

    ****************************  Resource Summary  ****************************

    Macrocells     Product Terms    Registers      Pins           Function Block
    Used           Used             Used           Used           Inputs Used
    1  /512 (  1%) 3   /1792 (  1%) 1  /512 (  1%) 6  /173 (  3%) 3  /1280 (  1%)

    PIN RESOURCES:

    Signal Type    Required     Mapped  |  Pin Type            Used   Remaining
    ------------------------------------|---------------------------------------
    Input         :    3           3    |  I/O              :     2      161
    Output        :    1           1    |  GCK/IO           :     1        2
    Bidirectional :    0           0    |  GTS/IO           :     2        2
    GCK           :    1           1    |  GSR/IO           :     1        0
    GTS           :    0           0    |  CDR/IO           :     0        1
    GSR           :    1           1    |  DGE/IO           :     0        1
                     ----        ----
            Total      6           6

    MACROCELL RESOURCES:

    Total Macrocells Available                   512
    Registered Macrocells                          1
    Non-registered Macrocell driving I/O           0

    GLOBAL RESOURCES:

    Signal 'clk' mapped onto global clock net GCK1.
    Global output enable net(s) unused.
    Signal 'pr' mapped onto global set/reset net GSR.

    End of Resource Summary
    *************** Summary of Required Resources ******************

    ** LOGIC **
    Signal              Total Signals Loc     Slew Pin  Pin       Pin     Reg     I/O      I/O       Reg Init
    Name                Pt    Used            Rate #    Type      Use     Use     STD      Style     State
    q                   3       3     FB1_1   FAST 7    GTS/I/O   O       DEFF    LVCMOS18           RESET

    ** INPUTS **
    Signal                            Loc          Pin  Pin       Pin     Reg     I/O      I/O
    Name                                           #    Type      Use     Use     STD      Style
    ce                                FB1_2        6    I/O       I               LVCMOS18 KPR
    clk                               FB9_16       46   GCK/I/O   GCK             LVCMOS18 KPR
    cr                                FB1_3        5    GTS/I/O   I               LVCMOS18 KPR
    d                                 FB1_4        4    I/O       I               LVCMOS18 KPR
    pr                                FB1_16       206  GSR/I/O   GSR             LVCMOS18 KPR

    End of Resources

    Legend:
    I/O Style - OD    - OpenDrain
              - PU    - Pullup
              - KPR   - Keeper
              - S     - SchmittTrigger
              - DG    - DataGate
    Reg Use   - LATCH - Transparent latch
              - DFF   - D-flip-flop
              - DEFF  - D-flip-flop with clock enable
              - TFF   - T-flip-flop
              - TDFF  - Dual-edge-triggered T-flip-flop
              - DDFF  - Dual-edge-triggered flip-flop
              - DDEFF - Dual-edge-triggered flip-flop with clock enable
              /S (after any above flop/latch type) indicates initial state is Set

    *********************Function Block Resource Summary***********************
    Function    # of        FB Inputs   Signals     Total       O/IO      IO
    Block       Macrocells  Used        Used        Pt Used     Req       Avail
    FB1           1           3           3            3         1/0        8
    FB2           0           0           0            0         0/0        4
    FB3           0           0           0            0         0/0        6
    FB4           0           0           0            0         0/0        5
    FB5           0           0           0            0         0/0        7
    FB6           0           0           0            0         0/0        3
    FB7           0           0           0            0         0/0        8
    FB8           0           0           0            0         0/0        3
    FB9           0           0           0            0         0/0        5
    FB10          0           0           0            0         0/0        6
    FB11          0           0           0            0         0/0        7
    FB12          0           0           0            0         0/0        8
    FB13          0           0           0            0         0/0        5
    FB14          0           0           0            0         0/0        5
    FB15          0           0           0            0         0/0        5
    FB16          0           0           0            0         0/0        5
    FB17          0           0           0            0         0/0        9
    FB18          0           0           0            0         0/0        3
    FB19          0           0           0            0         0/0        3
    FB20          0           0           0            0         0/0        6
    FB21          0           0           0            0         0/0        3
    FB22          0           0           0            0         0/0        8
    FB23          0           0           0            0         0/0        3
    FB24          0           0           0            0         0/0        7
    FB25          0           0           0            0         0/0        8
    FB26          0           0           0            0         0/0        8
    FB27          0           0           0            0         0/0        4
    FB28          0           0           0            0         0/0        3
    FB29          0           0           0            0         0/0        3
    FB30          0           0           0            0         0/0        6
    FB31          0           0           0            0         0/0        4
    FB32          0           0           0            0         0/0        5
                ----                                -----       -----     -----
                  1                                    3         1/0      173
    *********************************** FB1 ***********************************
    This function block is part of I/O Bank number:               2
    Number of signals used by logic mapping into function block:  3
    Number of function block inputs used/remaining:               3/37
    Number of function block control terms used/remaining:        1/3
    Number of PLA product terms used/remaining:                   3/53
    Signal                            Total   Loc     Pin   Pin      Pin
    Name                              Pt               #    Type     Use
    q                                 3       FB1_1   7     GTS/I/O  O
    (unused)                          0       FB1_2   6     I/O      I
    (unused)                          0       FB1_3   5     GTS/I/O  I
    (unused)                          0       FB1_4   4     I/O      I
    (unused)                          0       FB1_5         (b)
    (unused)                          0       FB1_6         (b)
    (unused)                          0       FB1_7         (b)
    (unused)                          0       FB1_8         (b)
    (unused)                          0       FB1_9         (b)
    (unused)                          0       FB1_10        (b)
    (unused)                          0       FB1_11        (b)
    (unused)                          0       FB1_12        (b)
    (unused)                          0       FB1_13  3     GTS/I/O
    (unused)                          0       FB1_14  2     I/O
    (unused)                          0       FB1_15  208   I/O
    (unused)                          0       FB1_16  206   GSR/I/O  GSR

    Signals Used by Logic in Function Block
      1: ce                 2: cr                 3: d

    Signal                     1         2         3         4 Signals FB
    Name             0----+----0----+----0----+----0----+----0 Used    Inputs
    q                 XXX..................................... 3       3
                     0----+----1----+----2----+----3----+----4
                               0         0         0         0
    Legend:
    Total Pt     - Total product terms used by the macrocell signal
    Loc          - Location where logic was mapped in device
    Pin Type/Use - I  - Input             GCK - Global clock
                   O  - Output            GTS - Global Output Enable
                  (b) - Buried macrocell  GSR - Global Set/Reset
    *********************************** FB2 ***********************************
    This function block is part of I/O Bank number:               2
    Number of signals used by logic mapping into function block:  0
    Number of function block inputs used/remaining:               0/40
    Number of function block control terms used/remaining:        0/4
    Number of PLA product terms used/remaining:                   0/56
    Signal                            Total   Loc     Pin   Pin      Pin
    Name                              Pt               #    Type     Use
    (unused)                          0       FB2_1         (b)
    (unused)                          0       FB2_2   8     I/O
    (unused)                          0       FB2_3         (b)
    (unused)                          0       FB2_4         (b)
    (unused)                          0       FB2_5         (b)
    (unused)                          0       FB2_6         (b)
    (unused)                          0       FB2_7         (b)
    (unused)                          0       FB2_8         (b)
    (unused)                          0       FB2_9         (b)
    (unused)                          0       FB2_10        (b)
    (unused)                          0       FB2_11        (b)
    (unused)                          0       FB2_12        (b)
    (unused)                          0       FB2_13        (b)
    (unused)                          0       FB2_14  9     GTS/I/O
    (unused)                          0       FB2_15  10    I/O
    (unused)                          0       FB2_16  12    I/O
    Legend:
    Total Pt     - Total product terms used by the macrocell signal
    Loc          - Location where logic was mapped in device
    Pin Type/Use - I  - Input             GCK - Global clock
                   O  - Output            GTS - Global Output Enable
                  (b) - Buried macrocell  GSR - Global Set/Reset
    *********************************** FB3 ***********************************
    This function block is part of I/O Bank number:               2
    Number of signals used by logic mapping into function block:  0
    Number of function block inputs used/remaining:               0/40
    Number of function block control terms used/remaining:        0/4
    Number of PLA product terms used/remaining:                   0/56
    Signal                            Total   Loc     Pin   Pin      Pin
    Name                              Pt               #    Type     Use
    (unused)                          0       FB3_1   205   I/O
    (unused)                          0       FB3_2         (b)
    (unused)                          0       FB3_3   203   I/O
    (unused)                          0       FB3_4         (b)
    (unused)                          0       FB3_5   202   I/O
    (unused)                          0       FB3_6         (b)
    (unused)                          0       FB3_7         (b)
    (unused)                          0       FB3_8         (b)
    (unused)                          0       FB3_9         (b)
    (unused)                          0       FB3_10        (b)
    (unused)                          0       FB3_11        (b)
    (unused)                          0       FB3_12        (b)
    (unused)                          0       FB3_13  201   I/O
    (unused)                          0       FB3_14        (b)
    (unused)                          0       FB3_15  200   I/O
    (unused)                          0       FB3_16  199   I/O
    Legend:
    Total Pt     - Total product terms used by the macrocell signal
    Loc          - Location where logic was mapped in device
    Pin Type/Use - I  - Input             GCK - Global clock
                   O  - Output            GTS - Global Output Enable
                  (b) - Buried macrocell  GSR - Global Set/Reset
    *********************************** FB4 ***********************************
    This function block is part of I/O Bank number:               2
    Number of signals used by logic mapping into function block:  0
    Number of function block inputs used/remaining:               0/40
    Number of function block control terms used/remaining:        0/4
    Number of PLA product terms used/remaining:                   0/56
    Signal                            Total   Loc     Pin   Pin      Pin
    Name                              Pt               #    Type     Use
    (unused)                          0       FB4_1         (b)
    (unused)                          0       FB4_2   14    I/O
    (unused)                          0       FB4_3         (b)
    (unused)                          0       FB4_4   15    I/O
    (unused)                          0       FB4_5         (b)
    (unused)                          0       FB4_6         (b)
    (unused)                          0       FB4_7         (b)
    (unused)                          0       FB4_8         (b)
    (unused)                          0       FB4_9         (b)
    (unused)                          0       FB4_10        (b)
    (unused)                          0       FB4_11        (b)
    (unused)                          0       FB4_12        (b)
    (unused)                          0       FB4_13        (b)
    (unused)                          0       FB4_14  16    I/O
    (unused)                          0       FB4_15  17    I/O
    (unused)                          0       FB4_16  18    I/O
    Legend:
    Total Pt     - Total product terms used by the macrocell signal
    Loc          - Location where logic was mapped in device
    Pin Type/Use - I  - Input             GCK - Global clock
                   O  - Output            GTS - Global Output Enable
                  (b) - Buried macrocell  GSR - Global Set/Reset
    *********************************** FB5 ***********************************
    This function block is part of I/O Bank number:               2
    Number of signals used by logic mapping into function block:  0
    Number of function block inputs used/remaining:               0/40
    Number of function block control terms used/remaining:        0/4
    Number of PLA product terms used/remaining:                   0/56
    Signal                            Total   Loc     Pin   Pin      Pin
    Name                              Pt               #    Type     Use
    (unused)                          0       FB5_1   198   I/O
    (unused)                          0       FB5_2   197   I/O
    (unused)                          0       FB5_3   196   I/O
    (unused)                          0       FB5_4   195   I/O
    (unused)                          0       FB5_5   194   I/O
    (unused)                          0       FB5_6         (b)
    (unused)                          0       FB5_7         (b)
    (unused)                          0       FB5_8         (b)
    (unused)                          0       FB5_9         (b)
    (unused)                          0       FB5_10        (b)
    (unused)                          0       FB5_11        (b)
    (unused)                          0       FB5_12        (b)
    (unused)                          0       FB5_13  193   I/O
    (unused)                          0       FB5_14        (b)
    (unused)                          0       FB5_15  192   I/O
    (unused)                          0       FB5_16        (b)
    Legend:
    Total Pt     - Total product terms used by the macrocell signal
    Loc          - Location where logic was mapped in device
    Pin Type/Use - I  - Input             GCK - Global clock
                   O  - Output            GTS - Global Output Enable
                  (b) - Buried macrocell  GSR - Global Set/Reset
    *********************************** FB6 ***********************************
    This function block is part of I/O Bank number:               2
    Number of signals used by logic mapping into function block:  0
    Number of function block inputs used/remaining:               0/40
    Number of function block control terms used/remaining:        0/4
    Number of PLA product terms used/remaining:                   0/56
    Signal                            Total   Loc     Pin   Pin      Pin
    Name                              Pt               #    Type     Use
    (unused)                          0       FB6_1   19    I/O
    (unused)                          0       FB6_2   20    I/O
    (unused)                          0       FB6_3   21    I/O
    (unused)                          0       FB6_4         (b)
    (unused)                          0       FB6_5         (b)
    (unused)                          0       FB6_6         (b)
    (unused)                          0       FB6_7         (b)
    (unused)                          0       FB6_8         (b)
    (unused)                          0       FB6_9         (b)
    (unused)                          0       FB6_10        (b)
    (unused)                          0       FB6_11        (b)
    (unused)                          0       FB6_12        (b)
    (unused)                          0       FB6_13        (b)
    (unused)                          0       FB6_14        (b)
    (unused)                          0       FB6_15        (b)
    (unused)                          0       FB6_16        (b)
    Legend:
    Total Pt     - Total product terms used by the macrocell signal
    Loc          - Location where logic was mapped in device
    Pin Type/Use - I  - Input             GCK - Global clock
                   O  - Output            GTS - Global Output Enable
                  (b) - Buried macrocell  GSR - Global Set/Reset
    *********************************** FB7 ***********************************
    This function block is part of I/O Bank number:               2
    Number of signals used by logic mapping into function block:  0
    Number of function block inputs used/remaining:               0/40
    Number of function block control terms used/remaining:        0/4
    Number of PLA product terms used/remaining:                   0/56
    Signal                            Total   Loc     Pin   Pin      Pin
    Name                              Pt               #    Type     Use
    (unused)                          0       FB7_1   191   I/O
    (unused)                          0       FB7_2         (b)
    (unused)                          0       FB7_3   189   I/O
    (unused)                          0       FB7_4   188   I/O
    (unused)                          0       FB7_5   187   I/O
    (unused)                          0       FB7_6         (b)
    (unused)                          0       FB7_7         (b)
    (unused)                          0       FB7_8         (b)
    (unused)                          0       FB7_9         (b)
    (unused)                          0       FB7_10        (b)
    (unused)                          0       FB7_11        (b)
    (unused)                          0       FB7_12        (b)
    (unused)                          0       FB7_13  186   I/O
    (unused)                          0       FB7_14  185   I/O
    (unused)                          0       FB7_15  184   I/O
    (unused)                          0       FB7_16  183   I/O
    Legend:
    Total Pt     - Total product terms used by the macrocell signal
    Loc          - Location where logic was mapped in device
    Pin Type/Use - I  - Input             GCK - Global clock
                   O  - Output            GTS - Global Output Enable
                  (b) - Buried macrocell  GSR - Global Set/Reset
    *********************************** FB8 ***********************************
    This function block is part of I/O Bank number:               2
    Number of signals used by logic mapping into function block:  0
    Number of function block inputs used/remaining:               0/40
    Number of function block control terms used/remaining:        0/4
    Number of PLA product terms used/remaining:                   0/56
    Signal                            Total   Loc     Pin   Pin      Pin
    Name                              Pt               #    Type     Use
    (unused)                          0       FB8_1         (b)
    (unused)                          0       FB8_2   22    I/O
    (unused)                          0       FB8_3   23    I/O
    (unused)                          0       FB8_4         (b)
    (unused)                          0       FB8_5         (b)
    (unused)                          0       FB8_6         (b)
    (unused)                          0       FB8_7         (b)
    (unused)                          0       FB8_8         (b)
    (unused)                          0       FB8_9         (b)
    (unused)                          0       FB8_10        (b)
    (unused)                          0       FB8_11        (b)
    (unused)                          0       FB8_12        (b)
    (unused)                          0       FB8_13        (b)
    (unused)                          0       FB8_14  25    I/O
    (unused)                          0       FB8_15        (b)
    (unused)                          0       FB8_16        (b)
    Legend:
    Total Pt     - Total product terms used by the macrocell signal
    Loc          - Location where logic was mapped in device
    Pin Type/Use - I  - Input             GCK - Global clock
                   O  - Output            GTS - Global Output Enable
                  (b) - Buried macrocell  GSR - Global Set/Reset
    *********************************** FB9 ***********************************
    This function block is part of I/O Bank number:               1
    Number of signals used by logic mapping into function block:  0
    Number of function block inputs used/remaining:               0/40
    Number of function block control terms used/remaining:        0/4
    Number of PLA product terms used/remaining:                   0/56
    Signal                            Total   Loc     Pin   Pin      Pin
    Name                              Pt               #    Type     Use
    (unused)                          0       FB9_1         (b)
    (unused)                          0       FB9_2   50    I/O
    (unused)                          0       FB9_3   49    I/O
    (unused)                          0       FB9_4   48    I/O
    (unused)                          0       FB9_5         (b)
    (unused)                          0       FB9_6         (b)
    (unused)                          0       FB9_7         (b)
    (unused)                          0       FB9_8         (b)
    (unused)                          0       FB9_9         (b)
    (unused)                          0       FB9_10        (b)
    (unused)                          0       FB9_11        (b)
    (unused)                          0       FB9_12        (b)
    (unused)                          0       FB9_13        (b)
    (unused)                          0       FB9_14  47    I/O
    (unused)                          0       FB9_15        (b)
    (unused)                          0       FB9_16  46    GCK/I/O  GCK
    Legend:
    Total Pt     - Total product terms used by the macrocell signal
    Loc          - Location where logic was mapped in device
    Pin Type/Use - I  - Input             GCK - Global clock
                   O  - Output            GTS - Global Output Enable
                  (b) - Buried macrocell  GSR - Global Set/Reset
    *********************************** FB10 ***********************************
    This function block is part of I/O Bank number:               1
    Number of signals used by logic mapping into function block:  0
    Number of function block inputs used/remaining:               0/40
    Number of function block control terms used/remaining:        0/4
    Number of PLA product terms used/remaining:                   0/56
    Signal                            Total   Loc     Pin   Pin      Pin
    Name                              Pt               #    Type     Use
    (unused)                          0       FB10_1  51    CDR/I/O
    (unused)                          0       FB10_2  54    I/O
    (unused)                          0       FB10_3  55    GCK/I/O
    (unused)                          0       FB10_4  56    I/O
    (unused)                          0       FB10_5        (b)
    (unused)                          0       FB10_6        (b)
    (unused)                          0       FB10_7        (b)
    (unused)                          0       FB10_8        (b)
    (unused)                          0       FB10_9        (b)
    (unused)                          0       FB10_10       (b)
    (unused)                          0       FB10_11       (b)
    (unused)                          0       FB10_12       (b)
    (unused)                          0       FB10_13 57    I/O
    (unused)                          0       FB10_14 58    DGE/I/O
    (unused)                          0       FB10_15       (b)
    (unused)                          0       FB10_16       (b)
    Legend:
    Total Pt     - Total product terms used by the macrocell signal
    Loc          - Location where logic was mapped in device
    Pin Type/Use - I  - Input             GCK - Global clock
                   O  - Output            GTS - Global Output Enable
                  (b) - Buried macrocell  GSR - Global Set/Reset
    *********************************** FB11 ***********************************
    This function block is part of I/O Bank number:               1
    Number of signals used by logic mapping into function block:  0
    Number of function block inputs used/remaining:               0/40
    Number of function block control terms used/remaining:        0/4
    Number of PLA product terms used/remaining:                   0/56
    Signal                            Total   Loc     Pin   Pin      Pin
    Name                              Pt               #    Type     Use
    (unused)                          0       FB11_1  45    I/O
    (unused)                          0       FB11_2        (b)
    (unused)                          0       FB11_3  44    GCK/I/O
    (unused)                          0       FB11_4  43    I/O
    (unused)                          0       FB11_5        (b)
    (unused)                          0       FB11_6        (b)
    (unused)                          0       FB11_7        (b)
    (unused)                          0       FB11_8        (b)
    (unused)                          0       FB11_9        (b)
    (unused)                          0       FB11_10       (b)
    (unused)                          0       FB11_11       (b)
    (unused)                          0       FB11_12       (b)
    (unused)                          0       FB11_13 41    I/O
    (unused)                          0       FB11_14 40    I/O
    (unused)                          0       FB11_15 39    I/O
    (unused)                          0       FB11_16 38    I/O
    Legend:
    Total Pt     - Total product terms used by the macrocell signal
    Loc          - Location where logic was mapped in device
    Pin Type/Use - I  - Input             GCK - Global clock
                   O  - Output            GTS - Global Output Enable
                  (b) - Buried macrocell  GSR - Global Set/Reset
    *********************************** FB12 ***********************************
    This function block is part of I/O Bank number:               1
    Number of signals used by logic mapping into function block:  0
    Number of function block inputs used/remaining:               0/40
    Number of function block control terms used/remaining:        0/4
    Number of PLA product terms used/remaining:                   0/56
    Signal                            Total   Loc     Pin   Pin      Pin
    Name                              Pt               #    Type     Use
    (unused)                          0       FB12_1  60    I/O
    (unused)                          0       FB12_2  61    I/O
    (unused)                          0       FB12_3  62    I/O
    (unused)                          0       FB12_4  63    I/O
    (unused)                          0       FB12_5  64    I/O
    (unused)                          0       FB12_6        (b)
    (unused)                          0       FB12_7        (b)
    (unused)                          0       FB12_8        (b)
    (unused)                          0       FB12_9        (b)
    (unused)                          0       FB12_10       (b)
    (unused)                          0       FB12_11       (b)
    (unused)                          0       FB12_12       (b)
    (unused)                          0       FB12_13 65    I/O
    (unused)                          0       FB12_14 66    I/O
    (unused)                          0       FB12_15 67    I/O
    (unused)                          0       FB12_16       (b)
    Legend:
    Total Pt     - Total product terms used by the macrocell signal
    Loc          - Location where logic was mapped in device
    Pin Type/Use - I  - Input             GCK - Global clock
                   O  - Output            GTS - Global Output Enable
                  (b) - Buried macrocell  GSR - Global Set/Reset
    *********************************** FB13 ***********************************
    This function block is part of I/O Bank number:               1
    Number of signals used by logic mapping into function block:  0
    Number of function block inputs used/remaining:               0/40
    Number of function block control terms used/remaining:        0/4
    Number of PLA product terms used/remaining:                   0/56
    Signal                            Total   Loc     Pin   Pin      Pin
    Name                              Pt               #    Type     Use
    (unused)                          0       FB13_1  37    I/O
    (unused)                          0       FB13_2        (b)
    (unused)                          0       FB13_3  36    I/O
    (unused)                          0       FB13_4  35    I/O
    (unused)                          0       FB13_5        (b)
    (unused)                          0       FB13_6        (b)
    (unused)                          0       FB13_7        (b)
    (unused)                          0       FB13_8        (b)
    (unused)                          0       FB13_9        (b)
    (unused)                          0       FB13_10       (b)
    (unused)                          0       FB13_11       (b)
    (unused)                          0       FB13_12       (b)
    (unused)                          0       FB13_13       (b)
    (unused)                          0       FB13_14 34    I/O
    (unused)                          0       FB13_15 32    I/O
    (unused)                          0       FB13_16       (b)
    Legend:
    Total Pt     - Total product terms used by the macrocell signal
    Loc          - Location where logic was mapped in device
    Pin Type/Use - I  - Input             GCK - Global clock
                   O  - Output            GTS - Global Output Enable
                  (b) - Buried macrocell  GSR - Global Set/Reset
    *********************************** FB14 ***********************************
    This function block is part of I/O Bank number:               1
    Number of signals used by logic mapping into function block:  0
    Number of function block inputs used/remaining:               0/40
    Number of function block control terms used/remaining:        0/4
    Number of PLA product terms used/remaining:                   0/56
    Signal                            Total   Loc     Pin   Pin      Pin
    Name                              Pt               #    Type     Use
    (unused)                          0       FB14_1        (b)
    (unused)                          0       FB14_2        (b)
    (unused)                          0       FB14_3  69    I/O
    (unused)                          0       FB14_4  70    I/O
    (unused)                          0       FB14_5  71    I/O
    (unused)                          0       FB14_6        (b)
    (unused)                          0       FB14_7        (b)
    (unused)                          0       FB14_8        (b)
    (unused)                          0       FB14_9        (b)
    (unused)                          0       FB14_10       (b)
    (unused)                          0       FB14_11       (b)
    (unused)                          0       FB14_12       (b)
    (unused)                          0       FB14_13 72    I/O
    (unused)                          0       FB14_14       (b)
    (unused)                          0       FB14_15 73    I/O
    (unused)                          0       FB14_16       (b)
    Legend:
    Total Pt     - Total product terms used by the macrocell signal
    Loc          - Location where logic was mapped in device
    Pin Type/Use - I  - Input             GCK - Global clock
                   O  - Output            GTS - Global Output Enable
                  (b) - Buried macrocell  GSR - Global Set/Reset
    *********************************** FB15 ***********************************
    This function block is part of I/O Bank number:               1
    Number of signals used by logic mapping into function block:  0
    Number of function block inputs used/remaining:               0/40
    Number of function block control terms used/remaining:        0/4
    Number of PLA product terms used/remaining:                   0/56
    Signal                            Total   Loc     Pin   Pin      Pin
    Name                              Pt               #    Type     Use
    (unused)                          0       FB15_1  31    I/O
    (unused)                          0       FB15_2        (b)
    (unused)                          0       FB15_3  30    I/O
    (unused)                          0       FB15_4  29    I/O
    (unused)                          0       FB15_5        (b)
    (unused)                          0       FB15_6        (b)
    (unused)                          0       FB15_7        (b)
    (unused)                          0       FB15_8        (b)
    (unused)                          0       FB15_9        (b)
    (unused)                          0       FB15_10       (b)
    (unused)                          0       FB15_11       (b)
    (unused)                          0       FB15_12       (b)
    (unused)                          0       FB15_13 28    I/O
    (unused)                          0       FB15_14 27    I/O
    (unused)                          0       FB15_15       (b)
    (unused)                          0       FB15_16       (b)
    Legend:
    Total Pt     - Total product terms used by the macrocell signal
    Loc          - Location where logic was mapped in device
    Pin Type/Use - I  - Input             GCK - Global clock
                   O  - Output            GTS - Global Output Enable
                  (b) - Buried macrocell  GSR - Global Set/Reset
    *********************************** FB16 ***********************************
    This function block is part of I/O Bank number:               1
    Number of signals used by logic mapping into function block:  0
    Number of function block inputs used/remaining:               0/40
    Number of function block control terms used/remaining:        0/4
    Number of PLA product terms used/remaining:                   0/56
    Signal                            Total   Loc     Pin   Pin      Pin
    Name                              Pt               #    Type     Use
    (unused)                          0       FB16_1  74    I/O
    (unused)                          0       FB16_2        (b)
    (unused)                          0       FB16_3  75    I/O
    (unused)                          0       FB16_4  76    I/O
    (unused)                          0       FB16_5  77    I/O
    (unused)                          0       FB16_6        (b)
    (unused)                          0       FB16_7        (b)
    (unused)                          0       FB16_8        (b)
    (unused)                          0       FB16_9        (b)
    (unused)                          0       FB16_10       (b)
    (unused)                          0       FB16_11       (b)
    (unused)                          0       FB16_12       (b)
    (unused)                          0       FB16_13       (b)
    (unused)                          0       FB16_14 78    I/O
    (unused)                          0       FB16_15       (b)
    (unused)                          0       FB16_16       (b)
    Legend:
    Total Pt     - Total product terms used by the macrocell signal
    Loc          - Location where logic was mapped in device
    Pin Type/Use - I  - Input             GCK - Global clock
                   O  - Output            GTS - Global Output Enable
                  (b) - Buried macrocell  GSR - Global Set/Reset
    *********************************** FB17 ***********************************
    This function block is part of I/O Bank number:               4
    Number of signals used by logic mapping into function block:  0
    Number of function block inputs used/remaining:               0/40
    Number of function block control terms used/remaining:        0/4
    Number of PLA product terms used/remaining:                   0/56
    Signal                            Total   Loc     Pin   Pin      Pin
    Name                              Pt               #    Type     Use
    (unused)                          0       FB17_1  161   I/O
    (unused)                          0       FB17_2  162   I/O
    (unused)                          0       FB17_3  163   I/O
    (unused)                          0       FB17_4  164   I/O
    (unused)                          0       FB17_5  165   I/O
    (unused)                          0       FB17_6        (b)
    (unused)                          0       FB17_7        (b)
    (unused)                          0       FB17_8        (b)
    (unused)                          0       FB17_9        (b)
    (unused)                          0       FB17_10       (b)
    (unused)                          0       FB17_11       (b)
    (unused)                          0       FB17_12       (b)
    (unused)                          0       FB17_13 166   I/O
    (unused)                          0       FB17_14 167   I/O
    (unused)                          0       FB17_15 168   I/O
    (unused)                          0       FB17_16 169   I/O
    Legend:
    Total Pt     - Total product terms used by the macrocell signal
    Loc          - Location where logic was mapped in device
    Pin Type/Use - I  - Input             GCK - Global clock
                   O  - Output            GTS - Global Output Enable
                  (b) - Buried macrocell  GSR - Global Set/Reset
    *********************************** FB18 ***********************************
    This function block is part of I/O Bank number:               4
    Number of signals used by logic mapping into function block:  0
    Number of function block inputs used/remaining:               0/40
    Number of function block control terms used/remaining:        0/4
    Number of PLA product terms used/remaining:                   0/56
    Signal                            Total   Loc     Pin   Pin      Pin
    Name                              Pt               #    Type     Use
    (unused)                          0       FB18_1  160   I/O
    (unused)                          0       FB18_2        (b)
    (unused)                          0       FB18_3        (b)
    (unused)                          0       FB18_4  159   I/O
    (unused)                          0       FB18_5        (b)
    (unused)                          0       FB18_6        (b)
    (unused)                          0       FB18_7        (b)
    (unused)                          0       FB18_8        (b)
    (unused)                          0       FB18_9        (b)
    (unused)                          0       FB18_10       (b)
    (unused)                          0       FB18_11       (b)
    (unused)                          0       FB18_12       (b)
    (unused)                          0       FB18_13       (b)
    (unused)                          0       FB18_14       (b)
    (unused)                          0       FB18_15 158   I/O
    (unused)                          0       FB18_16       (b)
    Legend:
    Total Pt     - Total product terms used by the macrocell signal
    Loc          - Location where logic was mapped in device
    Pin Type/Use - I  - Input             GCK - Global clock
                   O  - Output            GTS - Global Output Enable
                  (b) - Buried macrocell  GSR - Global Set/Reset
    *********************************** FB19 ***********************************
    This function block is part of I/O Bank number:               4
    Number of signals used by logic mapping into function block:  0
    Number of function block inputs used/remaining:               0/40
    Number of function block control terms used/remaining:        0/4
    Number of PLA product terms used/remaining:                   0/56
    Signal                            Total   Loc     Pin   Pin      Pin
    Name                              Pt               #    Type     Use
    (unused)                          0       FB19_1  170   I/O
    (unused)                          0       FB19_2  171   I/O
    (unused)                          0       FB19_3  173   I/O
    (unused)                          0       FB19_4        (b)
    (unused)                          0       FB19_5        (b)
    (unused)                          0       FB19_6        (b)
    (unused)                          0       FB19_7        (b)
    (unused)                          0       FB19_8        (b)
    (unused)                          0       FB19_9        (b)
    (unused)                          0       FB19_10       (b)
    (unused)                          0       FB19_11       (b)
    (unused)                          0       FB19_12       (b)
    (unused)                          0       FB19_13       (b)
    (unused)                          0       FB19_14       (b)
    (unused)                          0       FB19_15       (b)
    (unused)                          0       FB19_16       (b)
    Legend:
    Total Pt     - Total product terms used by the macrocell signal
    Loc          - Location where logic was mapped in device
    Pin Type/Use - I  - Input             GCK - Global clock
                   O  - Output            GTS - Global Output Enable
                  (b) - Buried macrocell  GSR - Global Set/Reset
    *********************************** FB20 ***********************************
    This function block is part of I/O Bank number:               4
    Number of signals used by logic mapping into function block:  0
    Number of function block inputs used/remaining:               0/40
    Number of function block control terms used/remaining:        0/4
    Number of PLA product terms used/remaining:                   0/56
    Signal                            Total   Loc     Pin   Pin      Pin
    Name                              Pt               #    Type     Use
    (unused)                          0       FB20_1        (b)
    (unused)                          0       FB20_2        (b)
    (unused)                          0       FB20_3  155   I/O
    (unused)                          0       FB20_4  154   I/O
    (unused)                          0       FB20_5        (b)
    (unused)                          0       FB20_6        (b)
    (unused)                          0       FB20_7        (b)
    (unused)                          0       FB20_8        (b)
    (unused)                          0       FB20_9        (b)
    (unused)                          0       FB20_10       (b)
    (unused)                          0       FB20_11       (b)
    (unused)                          0       FB20_12       (b)
    (unused)                          0       FB20_13 153   I/O
    (unused)                          0       FB20_14 152   I/O
    (unused)                          0       FB20_15 151   I/O
    (unused)                          0       FB20_16 150   I/O
    Legend:
    Total Pt     - Total product terms used by the macrocell signal
    Loc          - Location where logic was mapped in device
    Pin Type/Use - I  - Input             GCK - Global clock
                   O  - Output            GTS - Global Output Enable
                  (b) - Buried macrocell  GSR - Global Set/Reset
    *********************************** FB21 ***********************************
    This function block is part of I/O Bank number:               4
    Number of signals used by logic mapping into function block:  0
    Number of function block inputs used/remaining:               0/40
    Number of function block control terms used/remaining:        0/4
    Number of PLA product terms used/remaining:                   0/56
    Signal                            Total   Loc     Pin   Pin      Pin
    Name                              Pt               #    Type     Use
    (unused)                          0       FB21_1        (b)
    (unused)                          0       FB21_2  174   I/O
    (unused)                          0       FB21_3  175   I/O
    (unused)                          0       FB21_4        (b)
    (unused)                          0       FB21_5  178   I/O
    (unused)                          0       FB21_6        (b)
    (unused)                          0       FB21_7        (b)
    (unused)                          0       FB21_8        (b)
    (unused)                          0       FB21_9        (b)
    (unused)                          0       FB21_10       (b)
    (unused)                          0       FB21_11       (b)
    (unused)                          0       FB21_12       (b)
    (unused)                          0       FB21_13       (b)
    (unused)                          0       FB21_14       (b)
    (unused)                          0       FB21_15       (b)
    (unused)                          0       FB21_16       (b)
    Legend:
    Total Pt     - Total product terms used by the macrocell signal
    Loc          - Location where logic was mapped in device
    Pin Type/Use - I  - Input             GCK - Global clock
                   O  - Output            GTS - Global Output Enable
                  (b) - Buried macrocell  GSR - Global Set/Reset
    *********************************** FB22 ***********************************
    This function block is part of I/O Bank number:               4
    Number of signals used by logic mapping into function block:  0
    Number of function block inputs used/remaining:               0/40
    Number of function block control terms used/remaining:        0/4
    Number of PLA product terms used/remaining:                   0/56
    Signal                            Total   Loc     Pin   Pin      Pin
    Name                              Pt               #    Type     Use
    (unused)                          0       FB22_1  149   I/O
    (unused)                          0       FB22_2  148   I/O
    (unused)                          0       FB22_3  147   I/O
    (unused)                          0       FB22_4  146   I/O
    (unused)                          0       FB22_5        (b)
    (unused)                          0       FB22_6        (b)
    (unused)                          0       FB22_7        (b)
    (unused)                          0       FB22_8        (b)
    (unused)                          0       FB22_9        (b)
    (unused)                          0       FB22_10       (b)
    (unused)                          0       FB22_11       (b)
    (unused)                          0       FB22_12       (b)
    (unused)                          0       FB22_13 145   I/O
    (unused)                          0       FB22_14 144   I/O
    (unused)                          0       FB22_15 143   I/O
    (unused)                          0       FB22_16 142   I/O
    Legend:
    Total Pt     - Total product terms used by the macrocell signal
    Loc          - Location where logic was mapped in device
    Pin Type/Use - I  - Input             GCK - Global clock
                   O  - Output            GTS - Global Output Enable
                  (b) - Buried macrocell  GSR - Global Set/Reset
    *********************************** FB23 ***********************************
    This function block is part of I/O Bank number:               4
    Number of signals used by logic mapping into function block:  0
    Number of function block inputs used/remaining:               0/40
    Number of function block control terms used/remaining:        0/4
    Number of PLA product terms used/remaining:                   0/56
    Signal                            Total   Loc     Pin   Pin      Pin
    Name                              Pt               #    Type     Use
    (unused)                          0       FB23_1  179   I/O
    (unused)                          0       FB23_2  180   I/O
    (unused)                          0       FB23_3        (b)
    (unused)                          0       FB23_4  182   I/O
    (unused)                          0       FB23_5        (b)
    (unused)                          0       FB23_6        (b)
    (unused)                          0       FB23_7        (b)
    (unused)                          0       FB23_8        (b)
    (unused)                          0       FB23_9        (b)
    (unused)                          0       FB23_10       (b)
    (unused)                          0       FB23_11       (b)
    (unused)                          0       FB23_12       (b)
    (unused)                          0       FB23_13       (b)
    (unused)                          0       FB23_14       (b)
    (unused)                          0       FB23_15       (b)
    (unused)                          0       FB23_16       (b)
    Legend:
    Total Pt     - Total product terms used by the macrocell signal
    Loc          - Location where logic was mapped in device
    Pin Type/Use - I  - Input             GCK - Global clock
                   O  - Output            GTS - Global Output Enable
                  (b) - Buried macrocell  GSR - Global Set/Reset
    *********************************** FB24 ***********************************
    This function block is part of I/O Bank number:               4
    Number of signals used by logic mapping into function block:  0
    Number of function block inputs used/remaining:               0/40
    Number of function block control terms used/remaining:        0/4
    Number of PLA product terms used/remaining:                   0/56
    Signal                            Total   Loc     Pin   Pin      Pin
    Name                              Pt               #    Type     Use
    (unused)                          0       FB24_1  140   I/O
    (unused)                          0       FB24_2  139   I/O
    (unused)                          0       FB24_3  138   I/O
    (unused)                          0       FB24_4  137   I/O
    (unused)                          0       FB24_5        (b)
    (unused)                          0       FB24_6        (b)
    (unused)                          0       FB24_7        (b)
    (unused)                          0       FB24_8        (b)
    (unused)                          0       FB24_9        (b)
    (unused)                          0       FB24_10       (b)
    (unused)                          0       FB24_11       (b)
    (unused)                          0       FB24_12       (b)
    (unused)                          0       FB24_13 136   I/O
    (unused)                          0       FB24_14 135   I/O
    (unused)                          0       FB24_15 134   I/O
    (unused)                          0       FB24_16       (b)
    Legend:
    Total Pt     - Total product terms used by the macrocell signal
    Loc          - Location where logic was mapped in device
    Pin Type/Use - I  - Input             GCK - Global clock
                   O  - Output            GTS - Global Output Enable
                  (b) - Buried macrocell  GSR - Global Set/Reset
    *********************************** FB25 ***********************************
    This function block is part of I/O Bank number:               3
    Number of signals used by logic mapping into function block:  0
    Number of function block inputs used/remaining:               0/40
    Number of function block control terms used/remaining:        0/4
    Number of PLA product terms used/remaining:                   0/56
    Signal                            Total   Loc     Pin   Pin      Pin
    Name                              Pt               #    Type     Use
    (unused)                          0       FB25_1  110   I/O
    (unused)                          0       FB25_2  111   I/O
    (unused)                          0       FB25_3  112   I/O
    (unused)                          0       FB25_4  113   I/O
    (unused)                          0       FB25_5        (b)
    (unused)                          0       FB25_6        (b)
    (unused)                          0       FB25_7        (b)
    (unused)                          0       FB25_8        (b)
    (unused)                          0       FB25_9        (b)
    (unused)                          0       FB25_10       (b)
    (unused)                          0       FB25_11       (b)
    (unused)                          0       FB25_12       (b)
    (unused)                          0       FB25_13 114   I/O
    (unused)                          0       FB25_14 115   I/O
    (unused)                          0       FB25_15 116   I/O
    (unused)                          0       FB25_16 117   I/O
    Legend:
    Total Pt     - Total product terms used by the macrocell signal
    Loc          - Location where logic was mapped in device
    Pin Type/Use - I  - Input             GCK - Global clock
                   O  - Output            GTS - Global Output Enable
                  (b) - Buried macrocell  GSR - Global Set/Reset
    *********************************** FB26 ***********************************
    This function block is part of I/O Bank number:               3
    Number of signals used by logic mapping into function block:  0
    Number of function block inputs used/remaining:               0/40
    Number of function block control terms used/remaining:        0/4
    Number of PLA product terms used/remaining:                   0/56
    Signal                            Total   Loc     Pin   Pin      Pin
    Name                              Pt               #    Type     Use
    (unused)                          0       FB26_1  109   I/O
    (unused)                          0       FB26_2  108   I/O
    (unused)                          0       FB26_3  107   I/O
    (unused)                          0       FB26_4  106   I/O
    (unused)                          0       FB26_5        (b)
    (unused)                          0       FB26_6        (b)
    (unused)                          0       FB26_7        (b)
    (unused)                          0       FB26_8        (b)
    (unused)                          0       FB26_9        (b)
    (unused)                          0       FB26_10       (b)
    (unused)                          0       FB26_11       (b)
    (unused)                          0       FB26_12       (b)
    (unused)                          0       FB26_13 103   I/O
    (unused)                          0       FB26_14 102   I/O
    (unused)                          0       FB26_15 101   I/O
    (unused)                          0       FB26_16 100   I/O
    Legend:
    Total Pt     - Total product terms used by the macrocell signal
    Loc          - Location where logic was mapped in device
    Pin Type/Use - I  - Input             GCK - Global clock
                   O  - Output            GTS - Global Output Enable
                  (b) - Buried macrocell  GSR - Global Set/Reset
    *********************************** FB27 ***********************************
    This function block is part of I/O Bank number:               3
    Number of signals used by logic mapping into function block:  0
    Number of function block inputs used/remaining:               0/40
    Number of function block control terms used/remaining:        0/4
    Number of PLA product terms used/remaining:                   0/56
    Signal                            Total   Loc     Pin   Pin      Pin
    Name                              Pt               #    Type     Use
    (unused)                          0       FB27_1  118   I/O
    (unused)                          0       FB27_2        (b)
    (unused)                          0       FB27_3  119   I/O
    (unused)                          0       FB27_4  120   I/O
    (unused)                          0       FB27_5        (b)
    (unused)                          0       FB27_6        (b)
    (unused)                          0       FB27_7        (b)
    (unused)                          0       FB27_8        (b)
    (unused)                          0       FB27_9        (b)
    (unused)                          0       FB27_10       (b)
    (unused)                          0       FB27_11       (b)
    (unused)                          0       FB27_12       (b)
    (unused)                          0       FB27_13       (b)
    (unused)                          0       FB27_14       (b)
    (unused)                          0       FB27_15 121   I/O
    (unused)                          0       FB27_16       (b)
    Legend:
    Total Pt     - Total product terms used by the macrocell signal
    Loc          - Location where logic was mapped in device
    Pin Type/Use - I  - Input             GCK - Global clock
                   O  - Output            GTS - Global Output Enable
                  (b) - Buried macrocell  GSR - Global Set/Reset
    *********************************** FB28 ***********************************
    This function block is part of I/O Bank number:               3
    Number of signals used by logic mapping into function block:  0
    Number of function block inputs used/remaining:               0/40
    Number of function block control terms used/remaining:        0/4
    Number of PLA product terms used/remaining:                   0/56
    Signal                            Total   Loc     Pin   Pin      Pin
    Name                              Pt               #    Type     Use
    (unused)                          0       FB28_1  99    I/O
    (unused)                          0       FB28_2  97    I/O
    (unused)                          0       FB28_3  95    I/O
    (unused)                          0       FB28_4        (b)
    (unused)                          0       FB28_5        (b)
    (unused)                          0       FB28_6        (b)
    (unused)                          0       FB28_7        (b)
    (unused)                          0       FB28_8        (b)
    (unused)                          0       FB28_9        (b)
    (unused)                          0       FB28_10       (b)
    (unused)                          0       FB28_11       (b)
    (unused)                          0       FB28_12       (b)
    (unused)                          0       FB28_13       (b)
    (unused)                          0       FB28_14       (b)
    (unused)                          0       FB28_15       (b)
    (unused)                          0       FB28_16       (b)
    Legend:
    Total Pt     - Total product terms used by the macrocell signal
    Loc          - Location where logic was mapped in device
    Pin Type/Use - I  - Input             GCK - Global clock
                   O  - Output            GTS - Global Output Enable
                  (b) - Buried macrocell  GSR - Global Set/Reset
    *********************************** FB29 ***********************************
    This function block is part of I/O Bank number:               3
    Number of signals used by logic mapping into function block:  0
    Number of function block inputs used/remaining:               0/40
    Number of function block control terms used/remaining:        0/4
    Number of PLA product terms used/remaining:                   0/56
    Signal                            Total   Loc     Pin   Pin      Pin
    Name                              Pt               #    Type     Use
    (unused)                          0       FB29_1        (b)
    (unused)                          0       FB29_2        (b)
    (unused)                          0       FB29_3  122   I/O
    (unused)                          0       FB29_4  123   I/O
    (unused)                          0       FB29_5        (b)
    (unused)                          0       FB29_6        (b)
    (unused)                          0       FB29_7        (b)
    (unused)                          0       FB29_8        (b)
    (unused)                          0       FB29_9        (b)
    (unused)                          0       FB29_10       (b)
    (unused)                          0       FB29_11       (b)
    (unused)                          0       FB29_12       (b)
    (unused)                          0       FB29_13       (b)
    (unused)                          0       FB29_14 125   I/O
    (unused)                          0       FB29_15       (b)
    (unused)                          0       FB29_16       (b)
    Legend:
    Total Pt     - Total product terms used by the macrocell signal
    Loc          - Location where logic was mapped in device
    Pin Type/Use - I  - Input             GCK - Global clock
                   O  - Output            GTS - Global Output Enable
                  (b) - Buried macrocell  GSR - Global Set/Reset
    *********************************** FB30 ***********************************
    This function block is part of I/O Bank number:               3
    Number of signals used by logic mapping into function block:  0
    Number of function block inputs used/remaining:               0/40
    Number of function block control terms used/remaining:        0/4
    Number of PLA product terms used/remaining:                   0/56
    Signal                            Total   Loc     Pin   Pin      Pin
    Name                              Pt               #    Type     Use
    (unused)                          0       FB30_1        (b)
    (unused)                          0       FB30_2  91    I/O
    (unused)                          0       FB30_3  90    I/O
    (unused)                          0       FB30_4  89    I/O
    (unused)                          0       FB30_5        (b)
    (unused)                          0       FB30_6        (b)
    (unused)                          0       FB30_7        (b)
    (unused)                          0       FB30_8        (b)
    (unused)                          0       FB30_9        (b)
    (unused)                          0       FB30_10       (b)
    (unused)                          0       FB30_11       (b)
    (unused)                          0       FB30_12       (b)
    (unused)                          0       FB30_13 88    I/O
    (unused)                          0       FB30_14 87    I/O
    (unused)                          0       FB30_15       (b)
    (unused)                          0       FB30_16 86    I/O
    Legend:
    Total Pt     - Total product terms used by the macrocell signal
    Loc          - Location where logic was mapped in device
    Pin Type/Use - I  - Input             GCK - Global clock
                   O  - Output            GTS - Global Output Enable
                  (b) - Buried macrocell  GSR - Global Set/Reset
    *********************************** FB31 ***********************************
    This function block is part of I/O Bank number:               3
    Number of signals used by logic mapping into function block:  0
    Number of function block inputs used/remaining:               0/40
    Number of function block control terms used/remaining:        0/4
    Number of PLA product terms used/remaining:                   0/56
    Signal                            Total   Loc     Pin   Pin      Pin
    Name                              Pt               #    Type     Use
    (unused)                          0       FB31_1  126   I/O
    (unused)                          0       FB31_2        (b)
    (unused)                          0       FB31_3  127   I/O
    (unused)                          0       FB31_4  128   I/O
    (unused)                          0       FB31_5        (b)
    (unused)                          0       FB31_6        (b)
    (unused)                          0       FB31_7        (b)
    (unused)                          0       FB31_8        (b)
    (unused)                          0       FB31_9        (b)
    (unused)                          0       FB31_10       (b)
    (unused)                          0       FB31_11       (b)
    (unused)                          0       FB31_12       (b)
    (unused)                          0       FB31_13       (b)
    (unused)                          0       FB31_14       (b)
    (unused)                          0       FB31_15       (b)
    (unused)                          0       FB31_16 131   I/O
    Legend:
    Total Pt     - Total product terms used by the macrocell signal
    Loc          - Location where logic was mapped in device
    Pin Type/Use - I  - Input             GCK - Global clock
                   O  - Output            GTS - Global Output Enable
                  (b) - Buried macrocell  GSR - Global Set/Reset
    *********************************** FB32 ***********************************
    This function block is part of I/O Bank number:               3
    Number of signals used by logic mapping into function block:  0
    Number of function block inputs used/remaining:               0/40
    Number of function block control terms used/remaining:        0/4
    Number of PLA product terms used/remaining:                   0/56
    Signal                            Total   Loc     Pin   Pin      Pin
    Name                              Pt               #    Type     Use
    (unused)                          0       FB32_1  85    I/O
    (unused)                          0       FB32_2  84    I/O
    (unused)                          0       FB32_3        (b)
    (unused)                          0       FB32_4  83    I/O
    (unused)                          0       FB32_5        (b)
    (unused)                          0       FB32_6        (b)
    (unused)                          0       FB32_7        (b)
    (unused)                          0       FB32_8        (b)
    (unused)                          0       FB32_9        (b)
    (unused)                          0       FB32_10       (b)
    (unused)                          0       FB32_11       (b)
    (unused)                          0       FB32_12       (b)
    (unused)                          0       FB32_13 82    I/O
    (unused)                          0       FB32_14 80    I/O
    (unused)                          0       FB32_15       (b)
    (unused)                          0       FB32_16       (b)
    Legend:
    Total Pt     - Total product terms used by the macrocell signal
    Loc          - Location where logic was mapped in device
    Pin Type/Use - I  - Input             GCK - Global clock
                   O  - Output            GTS - Global Output Enable
                  (b) - Buried macrocell  GSR - Global Set/Reset
    ;;-----------------------------------------------------------------;;
    ; Implemented Equations.

    FDCPE_q: FDCPE port map (q,d,clk,cr,pr,ce);

    Register Legend:
     FDCPE (Q,D,C,CLR,PRE,CE);
     FDDCPE (Q,D,C,CLR,PRE,CE);
     FTCPE (Q,D,C,CLR,PRE,CE);
     FTDCPE (Q,D,C,CLR,PRE,CE);
     LDCP  (Q,D,G,CLR,PRE);

    ****************************  Device Pin Out ****************************

    Device : XC2C512-7-PQ208

    Pin Signal                         Pin Signal
    No. Name                           No. Name
      1 VCC                             105 VCCIO-UNUSED
      2 TIE                             106 TIE
      3 TIE                             107 TIE
      4 d                               108 TIE
      5 cr                              109 TIE
      6 ce                              110 TIE
      7 q                               111 TIE
      8 TIE                             112 TIE
      9 TIE                             113 TIE
     10 TIE                             114 TIE
     11 VCCAUX                          115 TIE
     12 TIE                             116 TIE
     13 GND                             117 TIE
     14 TIE                             118 TIE
     15 TIE                             119 TIE
     16 TIE                             120 TIE
     17 TIE                             121 TIE
     18 TIE                             122 TIE
     19 TIE                             123 TIE
     20 TIE                             124 VCC
     21 TIE                             125 TIE
     22 TIE                             126 TIE
     23 TIE                             127 TIE
     24 GND                             128 TIE
     25 TIE                             129 GND
     26 VCCIO-1.8                       130 GND
     27 TIE                             131 TIE
     28 TIE                             132 VCCIO-UNUSED
     29 TIE                             133 VCCIO-UNUSED
     30 TIE                             134 TIE
     31 TIE                             135 TIE
     32 TIE                             136 TIE
     33 VCCIO-1.8                       137 TIE
     34 TIE                             138 TIE
     35 TIE                             139 TIE
     36 TIE                             140 TIE
     37 TIE                             141 GND
     38 TIE                             142 TIE
     39 TIE                             143 TIE
     40 TIE                             144 TIE
     41 TIE                             145 TIE
     42 GND                             146 TIE
     43 TIE                             147 TIE
     44 TIE                             148 TIE
     45 TIE                             149 TIE
     46 clk                             150 TIE
     47 TIE                             151 TIE
     48 TIE                             152 TIE
     49 TIE                             153 TIE
     50 TIE                             154 TIE
     51 TIE                             155 TIE
     52 GND                             156 GND
     53 VCC                             157 VCCIO-UNUSED
     54 TIE                             158 TIE
     55 TIE                             159 TIE
     56 TIE                             160 TIE
     57 TIE                             161 TIE
     58 TIE                             162 TIE
     59 VCCIO-1.8                       163 TIE
     60 TIE                             164 TIE
     61 TIE                             165 TIE
     62 TIE                             166 TIE
     63 TIE                             167 TIE
     64 TIE                             168 TIE
     65 TIE                             169 TIE
     66 TIE                             170 TIE
     67 TIE                             171 TIE
     68 GND                             172 VCCIO-UNUSED
     69 TIE                             173 TIE
     70 TIE                             174 TIE
     71 TIE                             175 TIE
     72 TIE                             176 TDO
     73 TIE                             177 GND
     74 TIE                             178 TIE
     75 TIE                             179 TIE
     76 TIE                             180 TIE
     77 TIE                             181 VCCIO-UNUSED
     78 TIE                             182 TIE
     79 VCCIO-1.8                       183 TIE
     80 TIE                             184 TIE
     81 GND                             185 TIE
     82 TIE                             186 TIE
     83 TIE                             187 TIE
     84 TIE                             188 TIE
     85 TIE                             189 TIE
     86 TIE                             190 GND
     87 TIE                             191 TIE
     88 TIE                             192 TIE
     89 TIE                             193 TIE
     90 TIE                             194 TIE
     91 TIE                             195 TIE
     92 VCCIO-UNUSED                    196 TIE
     93 GND                             197 TIE
     94 TDI                             198 TIE
     95 TIE                             199 TIE
     96 TMS                             200 TIE
     97 TIE                             201 TIE
     98 TCK                             202 TIE
     99 TIE                             203 TIE
    100 TIE                             204 VCCIO-1.8
    101 TIE                             205 TIE
    102 TIE                             206 pr
    103 TIE                             207 GND
    104 GND                             208 TIE

    Legend :  NC  = Not Connected, unbonded pin
            PGND  = Unused I/O configured as additional Ground pin
             KPR  = Unused I/O with weak keeper (leave unconnected)
             WPU  = Unused I/O with weak pull up (leave unconnected)
             TIE  = Unused I/O floating -- must tie to VCC, GND or other signal
             VCC  = Dedicated Power Pin
          VCCAUX  = Power supply for JTAG pins
       VCCIO-3.3  = I/O supply voltage for LVTTL, LVCMOS33, SSTL3_I
       VCCIO-2.5  = I/O supply voltage for LVCMOS25, SSTL2_I
       VCCIO-1.8  = I/O supply voltage for LVCMOS18
       VCCIO-1.5  = I/O supply voltage for LVCMOS15, HSTL_I
            VREF  = Reference voltage for indicated input standard
           *VREF  = Reference voltage pin selected by software
             GND  = Dedicated Ground Pin
             TDI  = Test Data In, JTAG pin
             TDO  = Test Data Out, JTAG pin
             TCK  = Test Clock, JTAG pin
             TMS  = Test Mode Select, JTAG pin
      PROHIBITED  = User reserved pin
    ****************************  Compiler Options  ****************************

    Following is a list of all global compiler options used by the fitter run.

    Device(s) Specified                         : xc2c512-7-PQ208
    Optimization Method                         : DENSITY
    Multi-Level Logic Optimization              : ON
    Ignore Timing Specifications                : OFF
    Default Register Power Up Value             : LOW
    Keep User Location Constraints              : ON
    What-You-See-Is-What-You-Get                : OFF
    Exhaustive Fitting                          : OFF
    Keep Unused Inputs                          : OFF
    Slew Rate                                   : FAST
    Set Unused I/O Pin Termination              : FLOAT
    Global Clock Optimization                   : ON
    Global Set/Reset Optimization               : ON
    Global Ouput Enable Optimization            : ON
    Enable Input Registers                      : ON
    Function Block Fan-in Limit                 : 38
    Use DATA_GATE Attribute                     : ON
    Set Tristate Outputs to Termination Mode    : KEEPER
    Default Voltage Standard for All Outputs    : LVCMOS18
    Input Limit                                 : 38
    Pterm Limit                                 : 50