### Summary

Design Name | rosmem
Fitting Status | Successful
SW Version | G.35
Device Used | XC2C512-7-PQ208
Date | 1-22-2009, 4:58PM

##### RESOURCES SUMMARY

Macrocells Used | Pterms Used | Registers Used | Pins Used | Function Block Inputs Used
--- | --- | --- | --- | ---
397/512 (78%) | 920/1792 (52%) | 284/512 (56%) | 138/173 (80%) | 1004/1280 (79%)

##### PIN RESOURCES

Signal Type | Required | Mapped
--- | --- | ---
Input | 38 | 38
Output | 48 | 48
Bidirectional | 49 | 49
GCK | 2 | 2
GTS | 0 | 0
GSR | 1 | 1

Pin Type | Used | Remaining
--- | --- | ---
I/O | 129 | 34
GCK/IO | 3 | 0
GTS/IO | 4 | 0
GSR/IO | 1 | 0

##### MACROCELL RESOURCES

Total Macrocells Available | 512
Registered Macrocells | 284
Non-registered Macrocells driving I/O | 61

##### GLOBAL RESOURCES

Signal mapped onto global clock net (GCK0) | dsdly<0>
Signal mapped onto global clock net (GCK1) | clk
Signal mapped onto global output enable net (GTS0) | _n0086_MC.GLB
Signal mapped onto global output enable net (GTS3) | _n0088_MC.GLB
Signal mapped onto global output enable net (GSR) | reset