### Summary

Design Name | rosvme
Fitting Status | Successful
SW Version | G.35
Device Used | XC2C384-7-PQ208
Date | 12- 4-2009, 5:41PM

##### RESOURCES SUMMARY

Macrocells Used | Pterms Used | Registers Used | Pins Used | Function Block Inputs Used
--- | --- | --- | --- | ---
223/384 (59%) | 540/1344 (41%) | 142/384 (37%) | 163/173 (95%) | 648/960 (68%)

##### PIN RESOURCES

Signal Type | Required | Mapped
--- | --- | ---
Input | 61 | 61
Output | 83 | 83
Bidirectional | 16 | 16
GCK | 2 | 2
GTS | 0 | 0
GSR | 1 | 1

Pin Type | Used | Remaining
--- | --- | ---
I/O | 154 | 9
GCK/IO | 3 | 0
GTS/IO | 4 | 0
GSR/IO | 1 | 0

##### MACROCELL RESOURCES

Total Macrocells Available | 384
Registered Macrocells | 142
Non-registered Macrocells driving I/O | 67

##### GLOBAL RESOURCES

Signal mapped onto global clock net (GCK0) | clk_slow
Signal mapped onto global clock net (GCK1) | clk
Signal mapped onto global output enable net (GTS0) | _n0009_MC.GLB
Signal mapped onto global output enable net (GSR) | sysreset