24/03/03
14:48
ROB serial number  F0018

Tarjeta encendida con RON: 0
CRC  0	0	0	0	0	0	0

ROM Code26	14	B1	24	0	0	0	1A

ERROR CRC en encendido  FALSE
Voltage V3.3:  3,270000     Temp:  33,062500      Voltage V2.5:  2,490000   Current:  0,971775
TDC nš: 0
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
vernier error
coarse error
channel select error
TDC have read-out token
read-out fifo full
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 3   ROF= 255   TRF= 0   

TDC nš: 2
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

TDC nš: 0
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
vernier error
coarse error
channel select error
TDC have read-out token
read-out fifo full
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 3   ROF= 255   TRF= 0   

TDC nš: 2
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

TDC nš: 0
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
vernier error
coarse error
channel select error
TDC have read-out token
read-out fifo full
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 3   ROF= 255   TRF= 0   

TDC nš: 2
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

TDC nš: 0
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
vernier error
coarse error
channel select error
TDC have read-out token
read-out fifo full
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 3   ROF= 255   TRF= 0   

TDC nš: 2
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

TDC nš: 0
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
vernier error
coarse error
channel select error
TDC have read-out token
read-out fifo full
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 3   ROF= 255   TRF= 0   

TDC nš: 2
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

TDC nš: 0
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
vernier error
coarse error
channel select error
TDC have read-out token
read-out fifo full
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 3   ROF= 255   TRF= 0   

TDC nš: 2
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

TDC nš: 0
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
vernier error
coarse error
channel select error
TDC have read-out token
read-out fifo full
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 3   ROF= 255   TRF= 0   

TDC nš: 2
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

TDC nš: 0
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
vernier error
coarse error
channel select error
TDC have read-out token
read-out fifo full
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 3   ROF= 255   TRF= 0   

TDC nš: 2
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

Tras mandar muchos hits  
TDC nš: 0
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
vernier error
coarse error
channel select error
TDC have read-out token
read-out fifo full
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 3   ROF= 255   TRF= 0   

TDC nš: 2
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

Setup de nuevo para dejarlo listo tras hits  
TDC nš: 0
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
vernier error
coarse error
channel select error
TDC have read-out token
read-out fifo full
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 3   ROF= 255   TRF= 0   

TDC nš: 2
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

TDC nš: 0
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
vernier error
coarse error
channel select error
TDC have read-out token
read-out fifo full
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 3   ROF= 255   TRF= 0   

TDC nš: 2
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

TDC nš: 0
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
vernier error
coarse error
channel select error
TDC have read-out token
read-out fifo full
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 3   ROF= 255   TRF= 0   

TDC nš: 2
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

TDC nš: 0
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
vernier error
coarse error
channel select error
TDC have read-out token
read-out fifo full
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 3   ROF= 255   TRF= 0   

TDC nš: 2
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

TDC nš: 0
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
vernier error
coarse error
channel select error
TDC have read-out token
read-out fifo full
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 3   ROF= 255   TRF= 0   

TDC nš: 2
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

TDC nš: 0
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
vernier error
coarse error
channel select error
TDC have read-out token
read-out fifo full
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 3   ROF= 255   TRF= 0   

TDC nš: 2
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

TDC nš: 0
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
vernier error
coarse error
channel select error
TDC have read-out token
read-out fifo full
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 3   ROF= 255   TRF= 0   

TDC nš: 2
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

TDC nš: 0
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
vernier error
coarse error
channel select error
TDC have read-out token
read-out fifo full
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 3   ROF= 255   TRF= 0   

TDC nš: 2
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

Test of readout fifo ended
Test of readout fifo failed
Test of group 3 L1 buffer failed
Test of group 2 L1 buffer ended
Test of group 2 L1 buffer failed
Test of group 1 L1 buffer ended
Test of group 1 L1 buffer failed
Test of group 0 L1 buffer ended
Test of readout fifo ended
Test of readout fifo failed
Test of group 3 L1 buffer failed
Test of group 2 L1 buffer ended
Test of group 2 L1 buffer failed
Test of group 1 L1 buffer ended
Test of group 1 L1 buffer failed
Test of group 0 L1 buffer ended
Test of group 0 L1 buffer failed
Test of readout fifo failed
Test of group 3 L1 buffer ended
Test of group 3 L1 buffer failed
Test of group 2 L1 buffer ended
Test of group 2 L1 buffer failed
Test of group 1 L1 buffer ended
Test of group 1 L1 buffer failed
Test of group 0 L1 buffer ended
Test of group 0 L1 buffer failed
Test of readout fifo failed
Test of group 3 L1 buffer ended
Test of group 3 L1 buffer failed
Test of group 2 L1 buffer failed
Test of group 1 L1 buffer ended
Test of group 1 L1 buffer failed
Test of group 0 L1 buffer ended
TDC nš: 0
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
vernier error
coarse error
channel select error
TDC have read-out token
read-out fifo full
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 3   ROF= 255   TRF= 0   

TDC nš: 2
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

TDC nš: 0
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
vernier error
coarse error
channel select error
TDC have read-out token
read-out fifo full
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 3   ROF= 255   TRF= 0   

TDC nš: 2
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

TDC nš: 0
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
vernier error
coarse error
channel select error
TDC have read-out token
read-out fifo full
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 3   ROF= 255   TRF= 0   

TDC nš: 2
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

TDC nš: 0
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
vernier error
coarse error
channel select error
TDC have read-out token
read-out fifo full
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 3   ROF= 255   TRF= 0   

TDC nš: 2
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

TDC nš: 0
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
vernier error
coarse error
channel select error
TDC have read-out token
read-out fifo full
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 3   ROF= 255   TRF= 0   

TDC nš: 2
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

TDC nš: 0
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
vernier error
coarse error
channel select error
TDC have read-out token
read-out fifo full
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 3   ROF= 255   TRF= 0   

TDC nš: 2
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

TDC nš: 0
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
vernier error
coarse error
channel select error
TDC have read-out token
read-out fifo full
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 3   ROF= 255   TRF= 0   

TDC nš: 2
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

TDC nš: 0
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
vernier error
coarse error
channel select error
TDC have read-out token
read-out fifo full
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 3   ROF= 255   TRF= 0   

TDC nš: 2
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

TDC nš: 0
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
vernier error
coarse error
channel select error
TDC have read-out token
read-out fifo full
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 3   ROF= 255   TRF= 0   

TDC nš: 2
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

TDC nš: 0
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
vernier error
coarse error
channel select error
TDC have read-out token
read-out fifo full
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 3   ROF= 255   TRF= 0   

TDC nš: 2
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

