09/04/03
9:14
ROB serial number  F0171

Tarjeta encendida con RON: 0
CRC  0	0	0	0	0	0	0

ROM Code26	1B	B5	24	0	0	0	21

ERROR CRC en encendido  FALSE
Voltage V3.3:  3,270000     Temp:  22,781250      Voltage V2.5:  2,480000   Current:  0,971775
TDC nš: 0
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 2
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 0
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 2
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

Tras mandar muchos hits  
TDC nš: 0
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

TDC nš: 1
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

TDC nš: 2
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

Setup de nuevo para dejarlo listo tras hits  
TDC nš: 0
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 2
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 0
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 2
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

Test of readout fifo ended
Test of group 3 L1 buffer ended
Test of group 2 L1 buffer ended
Test of group 1 L1 buffer ended
Test of group 0 L1 buffer ended
Test of readout fifo ended
Test of group 3 L1 buffer ended
Test of group 2 L1 buffer ended
Test of group 1 L1 buffer ended
Test of group 0 L1 buffer ended
Test of readout fifo ended
Test of group 3 L1 buffer ended
Test of group 2 L1 buffer ended
Test of group 1 L1 buffer ended
Test of group 0 L1 buffer ended
Test of readout fifo ended
Test of group 3 L1 buffer ended
Test of group 2 L1 buffer ended
Test of group 1 L1 buffer ended
Test of group 0 L1 buffer ended
TDC nš: 0
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 2
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 0
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 2
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 0
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 2
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 0
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 2
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

ADQUISICION
Bloque nš: 0
Repetido TDC 3 Canal 20 hay 2 en vez de 1
Repetido TDC 3 Canal 30 hay 2 en vez de 1
Faltan canales?:  TRUE
Canal intruso: FALSE
Nš de códigos desconocidos recibidos: 0

Leading fuera rango. TDC  3   Ch  20
Width fuera rango. TDC  3   Ch  20
Leading fuera rango. TDC  3   Ch  30
Width fuera rango. TDC  3   Ch  30



Bloque nš: 1
Repetido TDC 3 Canal 20 hay 2 en vez de 1
Repetido TDC 3 Canal 30 hay 2 en vez de 1
Faltan canales?:  TRUE
Canal intruso: FALSE
Nš de códigos desconocidos recibidos: 0

Leading fuera rango. TDC  3   Ch  20
Width fuera rango. TDC  3   Ch  20
Leading fuera rango. TDC  3   Ch  30
Width fuera rango. TDC  3   Ch  30



Bloque nš: 2
Repetido TDC 3 Canal 20 hay 2 en vez de 1
Repetido TDC 3 Canal 30 hay 2 en vez de 1
Faltan canales?:  TRUE
Canal intruso: FALSE
Nš de códigos desconocidos recibidos: 0

Leading fuera rango. TDC  3   Ch  20
Width fuera rango. TDC  3   Ch  20
Leading fuera rango. TDC  3   Ch  30
Width fuera rango. TDC  3   Ch  30



Bloque nš: 3
Repetido TDC 3 Canal 20 hay 2 en vez de 1
Repetido TDC 3 Canal 30 hay 2 en vez de 1
Faltan canales?:  TRUE
Canal intruso: FALSE
Nš de códigos desconocidos recibidos: 0

Leading fuera rango. TDC  3   Ch  20
Width fuera rango. TDC  3   Ch  20
Leading fuera rango. TDC  3   Ch  30
Width fuera rango. TDC  3   Ch  30



Bloque nš: 4
Repetido TDC 3 Canal 20 hay 2 en vez de 1
Repetido TDC 3 Canal 30 hay 2 en vez de 1
Faltan canales?:  TRUE
Canal intruso: FALSE
Nš de códigos desconocidos recibidos: 0

Leading fuera rango. TDC  3   Ch  20
Width fuera rango. TDC  3   Ch  20
Leading fuera rango. TDC  3   Ch  30
Width fuera rango. TDC  3   Ch  30



Bloque nš: 5
Repetido TDC 3 Canal 20 hay 2 en vez de 1
Repetido TDC 3 Canal 30 hay 2 en vez de 1
Faltan canales?:  TRUE
Canal intruso: FALSE
Nš de códigos desconocidos recibidos: 0

Leading fuera rango. TDC  3   Ch  20
Width fuera rango. TDC  3   Ch  20
Leading fuera rango. TDC  3   Ch  30
Width fuera rango. TDC  3   Ch  30



Bloque nš: 6
Repetido TDC 3 Canal 20 hay 2 en vez de 1
Repetido TDC 3 Canal 30 hay 2 en vez de 1
Faltan canales?:  TRUE
Canal intruso: FALSE
Nš de códigos desconocidos recibidos: 0

Leading fuera rango. TDC  3   Ch  20
Width fuera rango. TDC  3   Ch  20
Leading fuera rango. TDC  3   Ch  30
Width fuera rango. TDC  3   Ch  30



Bloque nš: 7
Repetido TDC 3 Canal 20 hay 2 en vez de 1
Repetido TDC 3 Canal 30 hay 2 en vez de 1
Faltan canales?:  TRUE
Canal intruso: FALSE
Nš de códigos desconocidos recibidos: 0

Leading fuera rango. TDC  3   Ch  20
Width fuera rango. TDC  3   Ch  20
Leading fuera rango. TDC  3   Ch  30
Width fuera rango. TDC  3   Ch  30



Bloque nš: 8
Repetido TDC 3 Canal 20 hay 2 en vez de 1
Repetido TDC 3 Canal 30 hay 2 en vez de 1
Faltan canales?:  TRUE
Canal intruso: FALSE
Nš de códigos desconocidos recibidos: 0

Leading fuera rango. TDC  3   Ch  20
Width fuera rango. TDC  3   Ch  20
Leading fuera rango. TDC  3   Ch  30
Width fuera rango. TDC  3   Ch  30



Bloque nš: 9
Repetido TDC 3 Canal 20 hay 2 en vez de 1
Repetido TDC 3 Canal 30 hay 2 en vez de 1
Faltan canales?:  TRUE
Canal intruso: FALSE
Nš de códigos desconocidos recibidos: 0

Leading fuera rango. TDC  3   Ch  20
Width fuera rango. TDC  3   Ch  20
Leading fuera rango. TDC  3   Ch  30
Width fuera rango. TDC  3   Ch  30



TDC nš: 0
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 2
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 0
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 2
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TRACK TESTFaltan canales track: FALSE
Canal repetido: FALSE
Canales ajenos:  FALSE
Todos datos de un trigger:  FALSE
Dato repetido: TDC 3Canal  30
Dato repetido: TDC 3Canal  30
Dato repetido: TDC 3Canal  30
Dato repetido: TDC 3Canal  30
Dato repetido: TDC 3Canal  30
Dato repetido: TDC 3Canal  30
Dato repetido: TDC 3Canal  30
Dato repetido: TDC 3Canal  30
Dato repetido: TDC 3Canal  30
Dato repetido: TDC 3Canal  20
Dato repetido: TDC 3Canal  20
Dato repetido: TDC 3Canal  20
Dato repetido: TDC 3Canal  20
Dato repetido: TDC 3Canal  20
Dato repetido: TDC 3Canal  20
Dato repetido: TDC 3Canal  20
Dato repetido: TDC 3Canal  20
Dato repetido: TDC 3Canal  20
Nš de códigos desconocidos recibidos: 0

