26/03/03
13:51
ROB serial number  F0083

Tarjeta encendida con RON: 0
CRC  0	0	0	0	0	0	0

ROM Code26	39	B5	24	0	0	0	F9

ERROR CRC en encendido  FALSE
Voltage V3.3:  3,310000     Temp:  28,406250      Voltage V2.5:  2,480000   Current:  0,995711
TDC nš: 0
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 2
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 0
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 2
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

Tras mandar muchos hits  
TDC nš: 0
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

TDC nš: 1
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

TDC nš: 2
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

Setup de nuevo para dejarlo listo tras hits  
TDC nš: 0
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 2
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 0
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 2
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

Test of readout fifo ended
Test of group 3 L1 buffer ended
Test of group 2 L1 buffer ended
Test of group 1 L1 buffer ended
Test of group 0 L1 buffer ended
Test of readout fifo ended
Test of group 3 L1 buffer ended
Test of group 2 L1 buffer ended
Test of group 1 L1 buffer ended
Test of group 0 L1 buffer ended
Test of readout fifo ended
Test of group 3 L1 buffer ended
Test of group 2 L1 buffer ended
Test of group 1 L1 buffer ended
Test of group 0 L1 buffer ended
Test of readout fifo ended
Test of group 3 L1 buffer ended
Test of group 2 L1 buffer ended
Test of group 1 L1 buffer ended
Test of group 0 L1 buffer ended
TDC nš: 0
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 2
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 0
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 2
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 0
idcode error: E0000000
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
idcode error: 00280000
coarse error
channel select error
L1 buffer parity error
trigger fifo parity error
trigger matching state error
readout fifo parity error
LG0= 0   LG1= 0   LG2= 0   LG3= 165   ROF= 165   TRF= 0   

TDC nš: 2
idcode error: 00002800
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
idcode error: 00000028
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 0
idcode error: E0FFFFFF
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
idcode error: FF28FFFF
coarse error
channel select error
L1 buffer parity error
trigger fifo parity error
trigger matching state error
readout fifo parity error
LG0= 0   LG1= 0   LG2= 0   LG3= 165   ROF= 165   TRF= 0   

TDC nš: 2
idcode error: FFFF28FF
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
idcode error: FFFFFF28
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 0
idcode error: FFFFFFFF
vernier error
coarse error
channel select error
L1 buffer parity error
trigger fifo parity error
trigger matching state error
readout fifo parity error
readout state error
setup parity error
control parity error
jtag instruction error
TDC have read-out token
read-out fifo full
read-out fifo empty
trigger fifo full
trigger fifo empty
DLL in lock
LG0= 255   LG1= 255   LG2= 255   LG3= 255   ROF= 255   TRF= 15   

TDC nš: 1
idcode error: FFFFFFFF
vernier error
coarse error
channel select error
L1 buffer parity error
trigger fifo parity error
trigger matching state error
readout fifo parity error
readout state error
setup parity error
control parity error
jtag instruction error
TDC have read-out token
read-out fifo full
read-out fifo empty
trigger fifo full
trigger fifo empty
DLL in lock
LG0= 255   LG1= 255   LG2= 255   LG3= 255   ROF= 255   TRF= 15   

TDC nš: 2
idcode error: FFFFFFFF
vernier error
coarse error
channel select error
L1 buffer parity error
trigger fifo parity error
trigger matching state error
readout fifo parity error
readout state error
setup parity error
control parity error
jtag instruction error
TDC have read-out token
read-out fifo full
read-out fifo empty
trigger fifo full
trigger fifo empty
DLL in lock
LG0= 255   LG1= 255   LG2= 255   LG3= 255   ROF= 255   TRF= 15   

TDC nš: 3
idcode error: FFFFFFFF
vernier error
coarse error
channel select error
L1 buffer parity error
trigger fifo parity error
trigger matching state error
readout fifo parity error
readout state error
setup parity error
control parity error
jtag instruction error
TDC have read-out token
read-out fifo full
read-out fifo empty
trigger fifo full
trigger fifo empty
DLL in lock
LG0= 255   LG1= 255   LG2= 255   LG3= 255   ROF= 255   TRF= 15   

TDC nš: 0
idcode error: FFFFFFFF
vernier error
coarse error
channel select error
L1 buffer parity error
trigger fifo parity error
trigger matching state error
readout fifo parity error
readout state error
setup parity error
control parity error
jtag instruction error
TDC have read-out token
read-out fifo full
read-out fifo empty
trigger fifo full
trigger fifo empty
DLL in lock
LG0= 255   LG1= 255   LG2= 255   LG3= 255   ROF= 255   TRF= 15   

TDC nš: 1
idcode error: FFFFFFFF
vernier error
coarse error
channel select error
L1 buffer parity error
trigger fifo parity error
trigger matching state error
readout fifo parity error
readout state error
setup parity error
control parity error
jtag instruction error
TDC have read-out token
read-out fifo full
read-out fifo empty
trigger fifo full
trigger fifo empty
DLL in lock
LG0= 255   LG1= 255   LG2= 255   LG3= 255   ROF= 255   TRF= 15   

TDC nš: 2
idcode error: FFFFFFFF
vernier error
coarse error
channel select error
L1 buffer parity error
trigger fifo parity error
trigger matching state error
readout fifo parity error
readout state error
setup parity error
control parity error
jtag instruction error
TDC have read-out token
read-out fifo full
read-out fifo empty
trigger fifo full
trigger fifo empty
DLL in lock
LG0= 255   LG1= 255   LG2= 255   LG3= 255   ROF= 255   TRF= 15   

TDC nš: 3
idcode error: FFFFFFFF
vernier error
coarse error
channel select error
L1 buffer parity error
trigger fifo parity error
trigger matching state error
readout fifo parity error
readout state error
setup parity error
control parity error
jtag instruction error
TDC have read-out token
read-out fifo full
read-out fifo empty
trigger fifo full
trigger fifo empty
DLL in lock
LG0= 255   LG1= 255   LG2= 255   LG3= 255   ROF= 255   TRF= 15   

TDC nš: 0
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 2
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 0
idcode error: 00000000
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
idcode error: 00000000
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 2
idcode error: 00000000
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
idcode error: 00004631
coarse error
L1 buffer parity error
readout fifo parity error
setup parity error
TDC have read-out token
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 2   TRF= 0   

TDC nš: 0
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 2
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 0
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 2
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

