24/03/03
12:14
ROB serial number  F0012

Tarjeta encendida con RON: 0
CRC  0	0	0	0	0	0	0

ROM Code26	9E	B3	24	0	0	0	BC

ERROR CRC en encendido  FALSE
Voltage V3.3:  3,270000     Temp:  28,625000      Voltage V2.5:  2,490000   Current:  0,938266
TDC nš: 0
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 2
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 0
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 2
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

Tras mandar muchos hits  
TDC nš: 0
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

TDC nš: 1
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

TDC nš: 2
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 1   LG1= 1   LG2= 1   LG3= 1   ROF= 0   TRF= 0   

Setup de nuevo para dejarlo listo tras hits  
TDC nš: 0
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 2
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 0
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 2
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

Test of readout fifo ended
Test of group 3 L1 buffer ended
Test of group 2 L1 buffer ended
Test of group 1 L1 buffer ended
Test of group 0 L1 buffer ended
Test of readout fifo ended
Test of group 3 L1 buffer ended
Test of group 2 L1 buffer ended
Test of group 1 L1 buffer ended
Test of group 0 L1 buffer ended
Test of readout fifo ended
Test of group 3 L1 buffer ended
Test of group 2 L1 buffer ended
Test of group 1 L1 buffer ended
Test of group 0 L1 buffer ended
Test of readout fifo ended
Test of group 3 L1 buffer ended
Test of group 2 L1 buffer ended
Test of group 1 L1 buffer ended
Test of group 0 L1 buffer ended
TDC nš: 0
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 2
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 0
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 2
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 0
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 2
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 0
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 2
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

ADQUISICION
Bloque nš: 0
Faltan canales?:  FALSE
Canal intruso: FALSE
Nš de códigos desconocidos recibidos: 0




Bloque nš: 1
Faltan canales?:  FALSE
Canal intruso: FALSE
Nš de códigos desconocidos recibidos: 0




Bloque nš: 2
Faltan canales?:  FALSE
Canal intruso: FALSE
Nš de códigos desconocidos recibidos: 0




Bloque nš: 3
Faltan canales?:  FALSE
Canal intruso: FALSE
Nš de códigos desconocidos recibidos: 0




Bloque nš: 4
Faltan canales?:  FALSE
Canal intruso: FALSE
Nš de códigos desconocidos recibidos: 0




Bloque nš: 5
Faltan canales?:  FALSE
Canal intruso: FALSE
Nš de códigos desconocidos recibidos: 0




Bloque nš: 6
Faltan canales?:  FALSE
Canal intruso: FALSE
Nš de códigos desconocidos recibidos: 0




Bloque nš: 7
Faltan canales?:  FALSE
Canal intruso: FALSE
Nš de códigos desconocidos recibidos: 0




Bloque nš: 8
Faltan canales?:  FALSE
Canal intruso: FALSE
Nš de códigos desconocidos recibidos: 0




Bloque nš: 9
Faltan canales?:  FALSE
Canal intruso: FALSE
Nš de códigos desconocidos recibidos: 0




TDC nš: 0
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 2
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 0
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 1
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 2
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TDC nš: 3
TDC have read-out token
read-out fifo empty
trigger fifo empty
DLL in lock
LG0= 0   LG1= 0   LG2= 0   LG3= 0   ROF= 0   TRF= 0   

TRACK TESTFaltan canales track: FALSE
Canal repetido: FALSE
Canales ajenos:  FALSE
Todos datos de un trigger:  FALSE
Nš de códigos desconocidos recibidos: 0

