
#PINLOCK_BEGIN

#Sat Jul 03 19:21:20 2004
INST "evcntl_str" IOBDELAY=IBUF;

NET "add_p<0>"         LOC =  "S:PIN137";
NET "add_p<1>"         LOC =  "S:PIN120";
NET "add_p<2>"         LOC =  "S:PIN87";
NET "add_p<3>"         LOC =  "S:PIN140";
NET "add_p<4>"         LOC =  "S:PIN83";
NET "bcnt<0>"        LOC =  "S:PIN111";
NET "bcnt<10>"       LOC =  "S:PIN14";
NET "bcnt<11>"       LOC =  "S:PIN2";
NET "bcnt<1>"        LOC =  "S:PIN58";
NET "bcnt<2>"        LOC =  "S:PIN97";
NET "bcnt<3>"        LOC =  "S:PIN113";
NET "bcnt<4>"        LOC =  "S:PIN46";
NET "bcnt<5>"        LOC =  "S:PIN77";
NET "bcnt<6>"        LOC =  "S:PIN78";
NET "bcnt<7>"        LOC =  "S:PIN116";
NET "bcnt<8>"        LOC =  "S:PIN128";
NET "bcnt<9>"        LOC =  "S:PIN71";
NET "bcnt_str"       LOC =  "S:PIN107";
NET "brcst<2>"       LOC =  "S:PIN118";
NET "brcst<3>"       LOC =  "S:PIN102";
NET "brcst<4>"       LOC =  "S:PIN76";
NET "brcst<5>"       LOC =  "S:PIN136";
NET "brcst<6>"       LOC =  "S:PIN82";
NET "brcst<7>"       LOC =  "S:PIN96";
NET "brcst_str_1"    LOC =  "S:PIN5";
NET "brcst_str_2"    LOC =  "S:PIN66";
NET "clk"            LOC =  "S:PIN30";
NET "dberr_str"      LOC =  "S:PIN81";
NET "dout<0>"        LOC =  "S:PIN110";
NET "dout<1>"        LOC =  "S:PIN61";
NET "dout<2>"        LOC =  "S:PIN92";
NET "dout<3>"        LOC =  "S:PIN93";
NET "dout<4>"        LOC =  "S:PIN59";
NET "dout<5>"        LOC =  "S:PIN28";
NET "dout<6>"        LOC =  "S:PIN70";
NET "dout<7>"        LOC =  "S:PIN124";
NET "dout_str"       LOC =  "S:PIN135";
NET "dq<0>"          LOC =  "S:PIN134";
NET "dq<1>"          LOC =  "S:PIN91";
NET "dq<2>"          LOC =  "S:PIN3";
NET "dq<3>"          LOC =  "S:PIN104";
NET "evcnth_str"     LOC =  "S:PIN25";
NET "evcntl_str"     LOC =  "S:PIN10";
NET "i2c_int"        LOC =  "S:PIN75";
NET "qpll_error"     LOC =  "S:PIN32";
NET "qpll_locked"    LOC =  "S:PIN98";
NET "reset_p"          LOC =  "S:PIN143";
NET "sinerr_str"     LOC =  "S:PIN125";
NET "subaddr<0>"     LOC =  "S:PIN38";
NET "subaddr<1>"     LOC =  "S:PIN139";
NET "subaddr<2>"     LOC =  "S:PIN23";
NET "subaddr<3>"     LOC =  "S:PIN7";
NET "subaddr<4>"     LOC =  "S:PIN79";
NET "subaddr<5>"     LOC =  "S:PIN130";
NET "subaddr<6>"     LOC =  "S:PIN53";
NET "subaddr<7>"     LOC =  "S:PIN88";
NET "etr"            LOC =  "S:PIN86";
NET "enw"            LOC =  "S:PIN13";
NET "ttc_ready"      LOC =  "S:PIN48";
NET "ttc_sel_p"        LOC =  "S:PIN131";
NET "cmd<0>"         LOC =  "S:PIN52";
NET "cmd<1>"         LOC =  "S:PIN54";
NET "cmd<2>"         LOC =  "S:PIN57";
NET "cmd<3>"         LOC =  "S:PIN60";
NET "cmy"         LOC =  "S:PIN64";
NET "db<0>"          LOC =  "S:PIN11";
NET "db<10>"         LOC =  "S:PIN15";
NET "db<11>"         LOC =  "S:PIN39";
NET "db<12>"         LOC =  "S:PIN129";
NET "db<13>"         LOC =  "S:PIN21";
NET "db<14>"         LOC =  "S:PIN24";
NET "db<15>"         LOC =  "S:PIN44";
NET "db<1>"          LOC =  "S:PIN19";
NET "db<2>"          LOC =  "S:PIN95";
NET "db<3>"          LOC =  "S:PIN35";
NET "db<4>"          LOC =  "S:PIN94";
NET "db<5>"          LOC =  "S:PIN126";
NET "db<6>"          LOC =  "S:PIN4";
NET "db<7>"          LOC =  "S:PIN9";
NET "db<8>"          LOC =  "S:PIN103";
NET "db<9>"          LOC =  "S:PIN105";
NET "i2c_rst"        LOC =  "S:PIN34";
NET "i2c_wr"         LOC =  "S:PIN49";
NET "int_led"        LOC =  "S:PIN106";
NET "interrupt"      LOC =  "S:PIN112";
NET "qpll_reset"     LOC =  "S:PIN40";
NET "reset_b"        LOC =  "S:PIN43";
NET "spare"          LOC =  "S:PIN16";
NET "on_245"         LOC =  "S:PIN115";
NET "tp1"            LOC =  "S:PIN132";
NET "i2c_rd"         LOC =  "S:PIN27";
NET "tp2"            LOC =  "S:PIN51";
NET "tp3"            LOC =  "S:PIN138";
NET "ttc_on"         LOC =  "S:PIN121";
#PINLOCK_END
