<?xml version='1.0' encoding='utf-8' ?>
<!DOCTYPE ibis [
<!ELEMENT ibis (part, pin+)>
<!ELEMENT part EMPTY>
<!ELEMENT pin EMPTY>
<!ATTLIST part
  arch   CDATA #REQUIRED
  device CDATA #REQUIRED
  spg    CDATA #REQUIRED
  pkg    CDATA #REQUIRED>
<!ATTLIST pin
  nm     CDATA #REQUIRED
  no     CDATA #REQUIRED
  iostd  (TTL|LVTTL|LVCMOS2|NA) "NA"
  sr     (SLOW|FAST|slow|fast) "SLOW"
  dir    (BIDIR|bidir|INPUT|input|OUTPUT|output) "BIDIR">
]>
<ibis><part pkg="TQ144" spg="-6" arch="xc9500xl" device="XC95288XL"/><pin nm="clk" no="30" dir="input"/><pin nm="iack" no="130" dir="input"/><pin nm="ds0" no="143" dir="input"/><pin nm="add_in&lt;0&gt;" no="60" dir="input"/><pin nm="add_in&lt;1&gt;" no="82" dir="input"/><pin nm="add_in&lt;2&gt;" no="77" dir="input"/><pin nm="local_clk" no="28" dir="input"/><pin nm="ttc_on" no="116" dir="input"/><pin nm="lword" no="113" dir="input"/><pin nm="am3" no="135" dir="input"/><pin nm="write" no="79" dir="input"/><pin nm="as" no="119" dir="input"/><pin nm="ds1" no="103" dir="input"/><pin nm="int_ttc" no="86" dir="input"/><pin nm="i2c_int" no="131" dir="input"/><pin nm="am0" no="20" dir="input"/><pin nm="am1" no="2" dir="input"/><pin nm="am4" no="139" dir="input"/><pin nm="am5" no="12" dir="input"/><pin nm="iackin" no="105" dir="input"/><pin nm="sysreset" no="3" dir="input"/><pin nm="add_in&lt;3&gt;" no="33" dir="input"/><pin nm="add_in&lt;4&gt;" no="124" dir="input"/><pin nm="brd_sel" no="6" dir="input"/><pin nm="add_in&lt;5&gt;" no="118" dir="input"/><pin nm="add_in&lt;6&gt;" no="10" dir="input"/><pin nm="iackout" no="126" sr="fast" dir="output"/><pin nm="irq&lt;7&gt;" no="61" sr="fast" dir="output"/><pin nm="ttc_sel" no="11" sr="fast" dir="output"/><pin nm="g245" no="80" sr="fast" dir="output"/><pin nm="pca_add&lt;0&gt;" no="102" sr="fast" dir="output"/><pin nm="reset_p" no="25" sr="fast" dir="output"/><pin nm="pca_add&lt;1&gt;" no="97" sr="fast" dir="output"/><pin nm="tp1" no="125" sr="fast" dir="output"/><pin nm="i2c_rst" no="23" sr="fast" dir="output"/><pin nm="irq&lt;1&gt;" no="52" sr="fast" dir="output"/><pin nm="irq&lt;2&gt;" no="53" sr="fast" dir="output"/><pin nm="irq&lt;3&gt;" no="69" sr="fast" dir="output"/><pin nm="irq&lt;4&gt;" no="138" sr="fast" dir="output"/><pin nm="irq&lt;5&gt;" no="56" sr="fast" dir="output"/><pin nm="irq&lt;6&gt;" no="58" sr="fast" dir="output"/><pin nm="dtack" no="112" sr="fast" dir="output"/><pin nm="etr_p" no="129" sr="fast" dir="output"/><pin nm="i2c_ce0" no="9" sr="fast" dir="output"/><pin nm="i2c_ce1" no="24" sr="fast" dir="output"/><pin nm="i2c_rd" no="132" sr="fast" dir="output"/><pin nm="i2c_wr" no="121" sr="fast" dir="output"/><pin nm="intled" no="106" sr="fast" dir="output"/><pin nm="enw_p" no="115" sr="fast" dir="output"/><pin nm="tp3" no="87" sr="fast" dir="output"/><pin nm="w245" no="14" sr="fast" dir="output"/><pin nm="spare" no="59" sr="fast" dir="output"/><pin nm="on245" no="35" sr="fast" dir="output"/><pin nm="db&lt;0&gt;" no="91" sr="fast" dir="bidir"/><pin nm="db&lt;1&gt;" no="41" sr="fast" dir="bidir"/><pin nm="db&lt;2&gt;" no="34" sr="fast" dir="bidir"/><pin nm="db&lt;3&gt;" no="40" sr="fast" dir="bidir"/><pin nm="db&lt;4&gt;" no="45" sr="fast" dir="bidir"/><pin nm="db&lt;5&gt;" no="51" sr="fast" dir="bidir"/><pin nm="db&lt;6&gt;" no="71" sr="fast" dir="bidir"/><pin nm="db&lt;7&gt;" no="92" sr="fast" dir="bidir"/><pin nm="db&lt;10&gt;" no="96" sr="fast" dir="bidir"/><pin nm="db&lt;11&gt;" no="142" sr="fast" dir="bidir"/><pin nm="db&lt;12&gt;" no="4" sr="fast" dir="bidir"/><pin nm="db&lt;13&gt;" no="15" sr="fast" dir="bidir"/><pin nm="db&lt;14&gt;" no="21" sr="fast" dir="bidir"/><pin nm="db&lt;15&gt;" no="76" sr="fast" dir="bidir"/><pin nm="db&lt;8&gt;" no="100" sr="fast" dir="bidir"/><pin nm="db&lt;9&gt;" no="104" sr="fast" dir="bidir"/><pin nm="pca_db&lt;0&gt;" no="22" sr="fast" dir="bidir"/><pin nm="pca_db&lt;1&gt;" no="39" sr="fast" dir="bidir"/><pin nm="pca_db&lt;2&gt;" no="70" sr="fast" dir="bidir"/><pin nm="pca_db&lt;3&gt;" no="94" sr="fast" dir="bidir"/><pin nm="pca_db&lt;4&gt;" no="136" sr="fast" dir="bidir"/><pin nm="pca_db&lt;5&gt;" no="46" sr="fast" dir="bidir"/><pin nm="pca_db&lt;6&gt;" no="68" sr="fast" dir="bidir"/><pin nm="pca_db&lt;7&gt;" no="81" sr="fast" dir="bidir"/></ibis>
