NET "clkin_p" TNM_NET = "clkin_p";
TIMESPEC "TS_clkin_p" = PERIOD "clkin_p" 20 ns HIGH 50 %;
NET "clk_slow" TNM_NET = "clk_slow";
TIMESPEC "TS_clk_slow" = PERIOD "clk_slow" 10000 ns HIGH 50 %;
NET "dout<0>" OFFSET = OUT 10 ns AFTER "clkin_p"  ;
NET "dout<1>" OFFSET = OUT 10 ns AFTER "clkin_p"  ;
NET "dout<2>" OFFSET = OUT 10 ns AFTER "clkin_p"  ;
NET "dout<3>" OFFSET = OUT 10 ns AFTER "clkin_p"  ;
NET "dout<4>" OFFSET = OUT 10 ns AFTER "clkin_p"  ;
NET "dout<5>" OFFSET = OUT 10 ns AFTER "clkin_p"  ;
NET "dout<6>" OFFSET = OUT 10 ns AFTER "clkin_p"  ;
NET "dout<7>" OFFSET = OUT 10 ns AFTER "clkin_p"  ;
NET "dout<8>" OFFSET = OUT 10 ns AFTER "clkin_p"  ;
NET "dout<9>" OFFSET = OUT 10 ns AFTER "clkin_p"  ;
NET "dout<10>" OFFSET = OUT 10 ns AFTER "clkin_p"  ;
NET "dout<11>" OFFSET = OUT 10 ns AFTER "clkin_p"  ;
NET "dout<12>" OFFSET = OUT 10 ns AFTER "clkin_p"  ;
NET "dout<13>" OFFSET = OUT 10 ns AFTER "clkin_p"  ;
NET "dout<14>" OFFSET = OUT 10 ns AFTER "clkin_p"  ;
NET "dout<15>" OFFSET = OUT 10 ns AFTER "clkin_p"  ;
NET "txena_p" OFFSET = OUT 10 ns AFTER "clkin_p"  ;
#PINLOCK_BEGIN
#Sun Feb 13 11:03:06 2005
#PINLOCK_END
NET "fsen" OFFSET = OUT 10 ns AFTER "clkin_p"  ;
NET "fsi" OFFSET = OUT 10 ns AFTER "clkin_p"  ;
NET "fld" OFFSET = OUT 10 ns AFTER "clkin_p"  ;
#PACE: Start of Constraints generated by PACE

#PACE: Start of PACE I/O Pin Assignments
NET "add<0>"  LOC = "M11"  ;
NET "add<1>"  LOC = "N8"  ;
NET "add<2>"  LOC = "L12"  ;
NET "add<3>"  LOC = "C12"  ;
NET "add<4>"  LOC = "A7"  ;
NET "add<5>"  LOC = "A6"  ;
NET "ceros_done_p"  LOC = "P5"  ;
NET "ceros_id<0>"  LOC = "C5"  ;
NET "ceros_id<1>"  LOC = "C6"  ;
NET "clk20_p"  LOC = "P8"  ;
NET "clk_slow"  LOC = "T9"  ;
NET "clkin_p"  LOC = "T8"  ;
NET "cs"  LOC = "R7"  ;
NET "db<0>"  LOC = "B10"  ;
NET "db<10>"  LOC = "K12"  ;
NET "db<11>"  LOC = "E10"  ;
NET "db<12>"  LOC = "F15"  ;
NET "db<13>"  LOC = "H16"  ;
NET "db<14>"  LOC = "H14"  ;
NET "db<15>"  LOC = "D14"  ;
NET "db<1>"  LOC = "A10"  ;
NET "db<2>"  LOC = "M14"  ;
NET "db<3>"  LOC = "R12"  ;
NET "db<4>"  LOC = "L1"  ;
NET "db<5>"  LOC = "T13"  ;
NET "db<6>"  LOC = "T12"  ;
NET "db<7>"  LOC = "K14"  ;
NET "db<8>"  LOC = "K15"  ;
NET "db<9>"  LOC = "K16"  ;
NET "donein"  LOC = "T4"  ;
NET "doneout"  LOC = "R4"  ;
NET "dout<0>"  LOC = "H4"  ;
NET "dout<10>"  LOC = "P6"  ;
NET "dout<11>"  LOC = "F2"  ;
NET "dout<12>"  LOC = "D6"  ;
NET "dout<13>"  LOC = "T5"  ;
NET "dout<14>"  LOC = "F1"  ;
NET "dout<15>"  LOC = "E1"  ;
NET "dout<1>"  LOC = "A5"  ;
NET "dout<2>"  LOC = "M1"  ;
NET "dout<3>"  LOC = "L3"  ;
NET "dout<4>"  LOC = "M2"  ;
NET "dout<5>"  LOC = "J3"  ;
NET "dout<6>"  LOC = "N6"  ;
NET "dout<7>"  LOC = "K5"  ;
NET "dout<8>"  LOC = "K1"  ;
NET "dout<9>"  LOC = "K2"  ;
NET "ef<0>"  LOC = "E7"  ;
NET "ef<1>"  LOC = "B6"  ;
NET "ef<2>"  LOC = "B5"  ;
NET "ef<3>"  LOC = "H2"  ;
NET "ef<4>"  LOC = "J4"  ;
NET "ef<5>"  LOC = "D7"  ;
NET "enw"  LOC = "N11"  ;
NET "etr_x"  LOC = "T6"  ;
NET "evid<0>"  LOC = "G5"  ;
NET "evid<10>"  LOC = "G3"  ;
NET "evid<11>"  LOC = "H3"  ;
NET "evid<1>"  LOC = "E6"  ;
NET "evid<2>"  LOC = "G2"  ;
NET "evid<3>"  LOC = "F5"  ;
NET "evid<4>"  LOC = "H1"  ;
NET "evid<5>"  LOC = "L2"  ;
NET "evid<6>"  LOC = "J2"  ;
NET "evid<7>"  LOC = "J1"  ;
NET "evid<8>"  LOC = "T3"  ;
NET "evid<9>"  LOC = "G1"  ;
NET "ff<0>"  LOC = "M15"  ;
NET "ff<1>"  LOC = "N15"  ;
NET "ff<2>"  LOC = "L14"  ;
NET "ff<3>"  LOC = "M13"  ;
NET "ff<4>"  LOC = "M16"  ;
NET "ff<5>"  LOC = "L15"  ;
NET "fld"  LOC = "T7"  ;
NET "fmrs"  LOC = "T14"  ;
NET "negfout<0>"  LOC = "P7"  ;
NET "negfout<10>"  LOC = "G16"  ;
NET "negfout<11>"  LOC = "J13"  ;
NET "negfout<12>"  LOC = "A11"  ;
NET "negfout<13>"  LOC = "D11"  ;
NET "negfout<14>"  LOC = "C9"  ;
NET "negfout<15>"  LOC = "D10"  ;
NET "negfout<1>"  LOC = "T11"  ;
NET "negfout<2>"  LOC = "R10"  ;
NET "negfout<3>"  LOC = "P10"  ;
NET "negfout<4>"  LOC = "C10"  ;
NET "negfout<5>"  LOC = "K3"  ;
NET "negfout<6>"  LOC = "B9"  ;
NET "negfout<7>"  LOC = "A9"  ;
NET "negfout<8>"  LOC = "J15"  ;
NET "negfout<9>"  LOC = "J16"  ;
NET "fsen"  LOC = "M6"  ;
NET "fsi"  LOC = "N14"  ;
NET "hasul<0>"  LOC = "E13"  ;
NET "hasul<1>"  LOC = "E14"  ;
NET "hasul<2>"  LOC = "G12"  ;
NET "hasul<3>"  LOC = "B13"  ;
NET "hasul<4>"  LOC = "F16"  ;
NET "hasul<5>"  LOC = "D15"  ;
NET "led<0>"  LOC = "R5"  ;
NET "led<1>"  LOC = "N9"  ;
NET "load_paepaf"  LOC = "N7"  ;
NET "lock<0>"  LOC = "A12"  ;
NET "lock<1>"  LOC = "F12"  ;
NET "lock<2>"  LOC = "H13"  ;
NET "lock<3>"  LOC = "F13"  ;
NET "lock<4>"  LOC = "H15"  ;
NET "lock<5>"  LOC = "C11"  ;
NET "locked_p"  LOC = "D9"  ;
NET "mrs"  LOC = "P12"  ;
NET "oe<0>"  LOC = "D12"  ;
NET "oe<1>"  LOC = "R13"  ;
NET "oe<2>"  LOC = "C16"  ;
NET "oe<3>"  LOC = "G13"  ;
NET "oe<4>"  LOC = "G14"  ;
NET "oe<5>"  LOC = "E16"  ;
NET "paf<0>"  LOC = "R11"  ;
NET "paf<1>"  LOC = "M10"  ;
NET "paf<2>"  LOC = "P11"  ;
NET "paf<3>"  LOC = "T10"  ;
NET "paf<4>"  LOC = "N10"  ;
NET "paf<5>"  LOC = "M7"  ;
NET "par<0>"  LOC = "B12"  ;
NET "par<1>"  LOC = "E11"  ;
NET "recoff_p"  LOC = "C7"  ;
NET "ren<0>"  LOC = "B11" | SLEW = FAST ;
NET "ren<1>"  LOC = "P13" | SLEW = FAST ;
NET "ren<2>"  LOC = "N12" | SLEW = FAST ;
NET "ren<3>"  LOC = "D16" | SLEW = FAST ;
NET "ren<4>"  LOC = "R6" | SLEW = FAST ;
NET "ren<5>"  LOC = "K13" | SLEW = FAST ;
NET "reset"  LOC = "R14"  ;
NET "sff"  LOC = "N16"  ;
NET "spaf_p"  LOC = "P9"  ;
NET "token"  LOC = "G4"  ;
NET "tp<0>"  LOC = "C2"  ;
NET "tp<1>"  LOC = "P4"  ;
NET "tp<2>"  LOC = "P1"  ;
NET "tp<3>"  LOC = "A4"  ;
NET "txena_p"  LOC = "D5" | SLEW = FAST  | DRIVE = 24 ;
NET "valen"  LOC = "B4"  ;
NET "wclkena_p"  LOC = "B7"  ;

#NET "fspare<0>"  LOC = "N5"  ;
#NET "fspare<1>"  LOC = "B3"  ;
#NET "fspare<2>"  LOC = "D2"  ;
NET "lives_p"  LOC = "N5"  ;
NET "cspare_0"  LOC = "B3"  ;
NET "cspare_1"  LOC = "D2"  ;

NET "vspare_0"  LOC = "A3"  ;
NET "vspare_1"  LOC = "N1"  ;

#PACE: Start of PACE Area Constraints

#PACE: Start of PACE Prohibit Constraints
CONFIG PROHIBIT = C15;
CONFIG PROHIBIT = B16;
CONFIG PROHIBIT = E15;
CONFIG PROHIBIT = F14;
CONFIG PROHIBIT = G15;
CONFIG PROHIBIT = J14;
CONFIG PROHIBIT = L13;
CONFIG PROHIBIT = L16;
CONFIG PROHIBIT = P16;
CONFIG PROHIBIT = P15;
CONFIG PROHIBIT = D8;
CONFIG PROHIBIT = A8;
CONFIG PROHIBIT = A13;
CONFIG PROHIBIT = A14;
CONFIG PROHIBIT = R8;
CONFIG PROHIBIT = R9;

#PACE: End of Constraints generated by PACE
