<?xml version="1.0" encoding="UTF-8"?>
<!DOCTYPE twReport [
<!ELEMENT twReport (twHead, (twWarn | twDebug | twInfo)*, twBody, twSum?, twFoot, twClientInfo?)>
<!ELEMENT twHead (twExecVer?, twCopyright, twCmdLine?, twDesign?, twPCF?, twDevInfo, twRptInfo, twEnvVar*)>
<!ELEMENT twExecVer (#PCDATA)>
<!ELEMENT twCopyright (#PCDATA)>
<!ELEMENT twCmdLine (#PCDATA)>
<!ELEMENT twDesign (#PCDATA)>
<!ELEMENT twPCF (#PCDATA)>
<!ELEMENT twDevInfo (twDevName, twSpeedGrade, twSpeedVer?)>
<!ELEMENT twDevName (#PCDATA)>
<!ATTLIST twDevInfo arch CDATA #IMPLIED>
<!ELEMENT twSpeedGrade (#PCDATA)>
<!ELEMENT twSpeedVer (#PCDATA)>
<!ELEMENT twRptInfo (twItemLimit?, (twUnconst, twUnconstLimit?)?)>
<!ATTLIST twRptInfo twRptLvl (twErr | twVerbose | twTerseErr | twSum | twTimeGrp) #REQUIRED>
<!ATTLIST twRptInfo twAdvRpt  (TRUE | FALSE) "FALSE">
<!ATTLIST twRptInfo twTimeUnits (twPsec | twNsec | twUsec | twMsec | twSec) "twNsec">
<!ATTLIST twRptInfo twFreqUnits (twGHz | twMHz | twHz) "twMHz">
<!ELEMENT twItemLimit (#PCDATA)>
<!ELEMENT twUnconst EMPTY>
<!ELEMENT twUnconstLimit (#PCDATA)>
<!ELEMENT twEnvVar EMPTY>
<!ATTLIST twEnvVar name CDATA #REQUIRED>
<!ATTLIST twEnvVar description CDATA #REQUIRED>
<!ELEMENT twWarn (#PCDATA)>
<!ELEMENT twInfo (#PCDATA)>
<!ELEMENT twDebug (#PCDATA)>
<!ELEMENT twBody (twDerating?, (twSumRpt | twVerboseRpt | twErrRpt | twTerseErrRpt | twTimeGrpRpt), twNonDedClks?)>
<!ATTLIST twBody twFastPaths CDATA #IMPLIED>
<!ELEMENT twDerating (twProc?, twTemp?, twVolt?)>
<!ELEMENT twProc (#PCDATA)>
<!ELEMENT twTemp (#PCDATA)>
<!ELEMENT twVolt (#PCDATA)>
<!ELEMENT twSumRpt (twConstList?, twUnmetConstCnt?, twDebug*, twDataSheet?, twClkTbl?)>
<!ELEMENT twErrRpt (twCycles?, (twConst | twTIG)*, twUnmetConstCnt?, twDataSheet?, twClkTbl?, twTimeGrp*)>
<!ELEMENT twTerseErrRpt (twConstList, twUnmetConstCnt?, twDataSheet?, twClkTbl?)>
<!ELEMENT twVerboseRpt (twCycles?, (twConst | twTIG)*, twUnmetConstCnt?, twDataSheet?, twClkTbl?, twTimeGrp*)>
<!ELEMENT twCycles (twSigConn+)>
<!ATTLIST twCycles twNum CDATA #REQUIRED>
<!ELEMENT twSigConn (twSig, twDriver, twLoad)>
<!ELEMENT twSig (#PCDATA)>
<!ELEMENT twDriver (#PCDATA)>
<!ELEMENT twLoad (#PCDATA)> 
<!ELEMENT twConst (twConstHead, ((twPathRpt*, twPathRptBanner, twPathRpt*) |  (twPathRpt*, twRacePathRpt?) |  (twNetRpt*)))>
<!ATTLIST twConst twConstType (twPathConst | twNetConst) "twPathConst">
<!ELEMENT twConstHead (twConstName, twItemCnt, twErrCntSetup, twErrCntHold, twMinPer?, twMaxDel?, twMaxFreq?, twMaxNetDel?, twMaxNetSkew?, twMinOff?, twMaxOff?)>
<!ELEMENT twConstName (#PCDATA)>
<!ELEMENT twItemCnt (#PCDATA)>
<!ELEMENT twErrCnt (#PCDATA)>
<!ELEMENT twErrCntSetup (#PCDATA)>
<!ELEMENT twErrCntHold (#PCDATA)>
<!ATTLIST twErrCntHold twRaceChecked (TRUE | FALSE) "FALSE">
<!ELEMENT twMinPer (#PCDATA)>
<!ELEMENT twMaxDel (#PCDATA)>
<!ELEMENT twMaxFreq (#PCDATA)>
<!ELEMENT twMinOff (#PCDATA)>
<!ELEMENT twMaxOff (#PCDATA)>
<!ELEMENT twTIG (twTIGHead, (twPathRpt*,twRacePathRpt?))>
<!ELEMENT twTIGHead (twTIGName, twInstantiated, twBlocked)>
<!ELEMENT twTIGName (#PCDATA)>
<!ELEMENT twInstantiated (#PCDATA)>
<!ELEMENT twBlocked (#PCDATA)>
<!ELEMENT twRacePathRpt (twRacePath+)>
<!ELEMENT twPathRpt (twUnconstPath | twConstPath | twUnconstOffIn | twConstOffIn | twUnconstOffOut | twConstOffOut | twModOffOut)>
<!ELEMENT twUnconstPath (twTotDel, twSrc, twDest,  (twDel, twSUTime)?, twTotPathDel?, twClkSkew?, tw2Phase?, twClkUncert?, twDetPath?)>
<!ELEMENT twTotDel (#PCDATA)>
<!ELEMENT twSrc (#PCDATA)>
<!ATTLIST twSrc BELType CDATA #IMPLIED>
<!ELEMENT twDest (#PCDATA)>
<!ATTLIST twDest BELType CDATA #IMPLIED>
<!ELEMENT twDel (#PCDATA)>
<!ELEMENT twSUTime (#PCDATA)>
<!ELEMENT twTotPathDel (#PCDATA)>
<!ELEMENT twClkSkew (#PCDATA)>
<!ELEMENT twClkSkew (#PCDATA)>
<!ELEMENT twConstPath (twSlack, twSrc, twDest, twTotPathDel?, twClkSkew?, twDelConst, tw2Phase?, twClkUncert?, twDetPath?)>
<!ATTLIST twConstPath twDataPathType CDATA "twDataPathMaxDelay">
<!ATTLIST twConstPath constType (period | fromto | unknown) "unknown">
<!ELEMENT twSlack (#PCDATA)>
<!ELEMENT twDelConst (#PCDATA)>
<!ELEMENT tw2Phase EMPTY>
<!ELEMENT twRacePath (twSlack, twSrc, twDest, twClkSkew, twDelConst?, twClkUncert?, twDetPath)>
<!ELEMENT twPathRptBanner (#PCDATA)>
<!ELEMENT twUnconstOffIn (twOff, twSrc, twDest, twGuaranteed?, twClkUncert?, (twDataPath, twClkPath)?)>
<!ELEMENT twOff (#PCDATA)>
<!ELEMENT twGuaranteed EMPTY>
<!ELEMENT twConstOffIn (twSlack, twSrc, twDest, ((twClkDel, twClkSrc, twClkDest) | twGuarInSetup), twOff, twOffSrc, twOffDest, twClkUncert?, (twDataPath, twClkPath)?)>
<!ATTLIST twConstOffIn twDataPathType CDATA "twDataPathMaxDelay">
<!ATTLIST twConstOffIn twDurationNotSpecified CDATA #IMPLIED>
<!ELEMENT twClkDel (#PCDATA)>
<!ELEMENT twClkSrc (#PCDATA)>
<!ELEMENT twClkDest (#PCDATA)>
<!ELEMENT twGuarInSetup (#PCDATA)>
<!ELEMENT twOffSrc (#PCDATA)>
<!ELEMENT twOffDest (#PCDATA)>
<!ELEMENT twUnconstOffOut (twOff, twSrc, twDest, twClkUncert?, (twClkPath, twDataPath)?)>
<!ELEMENT twConstOffOut (twSlack, twSrc, twDest, twClkDel, twClkSrc, twClkDest, twDataDel, twDataSrc, twDataDest, twOff, twOffSrc, twOffDest, twClkUncert?, (twClkPath, twDataPath)?)>
<!ATTLIST twConstOffOut twDataPathType CDATA "twDataPathMaxDelay">
<!ELEMENT twDataDel (#PCDATA)>
<!ELEMENT twDataSrc (#PCDATA)>
<!ELEMENT twDataDest (#PCDATA)>
<!ELEMENT twModOffOut (twSlack, twDest, twDataDel, twDataSrc, twDataDest, twClkUncert?, twDataPath?)>
<!ELEMENT twDetPath (twSrc, twDest, twLogLvls, twSrcSite, twSrcClk?, twPathDel*, (twLogDel, twRouteDel, twTotDel)?, twDestClk?, (twPctLog, twPctRoute)?)>
<!ATTLIST twDetPath maxSiteLen CDATA #IMPLIED>
<!ELEMENT twDataPath (twSrc, twDest, twLogLvls, twSrcSite, twSrcClk?, twPathDel*, (twLogDel, twRouteDel, twTotDel)?, twDestClk?, (twPctLog, twPctRoute)?)>
<!ATTLIST twDataPath maxSiteLen CDATA #IMPLIED>
<!ELEMENT twClkPath (twSrc, twDest, twLogLvls, twSrcSite, twSrcClk?, twPathDel*, (twLogDel, twRouteDel, twTotDel)?, twDestClk?, (twPctLog, twPctRoute)?)>
<!ATTLIST twClkPath maxSiteLen CDATA #IMPLIED>
<!ELEMENT twLogLvls (#PCDATA)>
<!ELEMENT twSrcSite (#PCDATA)>
<!ELEMENT twSrcClk (#PCDATA)>
<!ATTLIST twSrcClk twEdge (twRising | twFalling) "twRising">
<!ATTLIST twSrcClk twArriveTime CDATA #IMPLIED>
<!ATTLIST twSrcClk twClkRes CDATA #IMPLIED>
<!ELEMENT twPathDel (twSite, twDelType, twFanCnt?, twDelInfo?, twComp, twNet?, twBEL*)>
<!ATTLIST twPathDel twHoldTime (TRUE | FALSE) "FALSE">
<!ELEMENT twDelInfo (#PCDATA)>
<!ATTLIST twDelInfo twEdge (twRising | twFalling | twIndet) #REQUIRED>
<!ATTLIST twDelInfo twAcc (twRouted | twEst | twApprox) "twRouted">
<!ELEMENT twSite (#PCDATA)>
<!ELEMENT twDelType (#PCDATA)>
<!ELEMENT twFanCnt (#PCDATA)>
<!ELEMENT twComp (#PCDATA)>
<!ELEMENT twNet (#PCDATA)>
<!ELEMENT twBEL (#PCDATA)>
<!ELEMENT twLogDel (#PCDATA)>
<!ELEMENT twRouteDel (#PCDATA)>
<!ELEMENT twDestClk (#PCDATA)>
<!ATTLIST twDestClk twEdge (twRising | twFalling) "twRising">
<!ATTLIST twDestClk twArriveTime CDATA #IMPLIED>
<!ATTLIST twDestClk twClkRes CDATA #IMPLIED>
<!ELEMENT twPctLog (#PCDATA)>
<!ELEMENT twPctRoute (#PCDATA)>
<!ELEMENT twNetRpt (twDelNet | twSlackNet | twSkewNet)>
<!ELEMENT twDelNet (twDel, twNet, twDetNet?)>
<!ELEMENT twSlackNet (twSlack, twNet, twDel, twNotMet?, twTimeConst, twAbsSlack, twDetNet?)>
<!ELEMENT twTimeConst (#PCDATA)>
<!ELEMENT twAbsSlack (#PCDATA)>
<!ELEMENT twSkewNet (twSlack, twNet, twSkew, twNotMet?, twTimeConst, twAbsSlack, twDetSkewNet?)>
<!ELEMENT twSkew (#PCDATA)>
<!ELEMENT twDetNet (twNetDel*)>
<!ELEMENT twNetDel (twSrc, twDest, twNetDelInfo)>
<!ELEMENT twNetDelInfo (#PCDATA)>
<!ATTLIST twNetDelInfo twAcc (twRouted | twEst | twApprox) "twRouted">
<!ELEMENT twDetSkewNet (twNetSkew*)>
<!ELEMENT twNetSkew (twSrc, twDest, twNetDelInfo, twSkew)>
<!ELEMENT twConstList (twConstListItem)*>
<!ELEMENT twConstListItem (twConstName, twNotMet?, twReqVal?, twActVal?, twLogLvls?)> 
<!ATTLIST twConstListItem twUnits (twTime | twFreq) "twTime">
<!ELEMENT twNotMet EMPTY>
<!ELEMENT twReqVal (#PCDATA)>
<!ELEMENT twActVal (#PCDATA)>
<!ELEMENT twTimeGrp (twTimeGrpName, twCompList?, twSigList?, twBELList?, twMacList?, twPinList?)>
<!ELEMENT twTimeGrpName (#PCDATA)>
<!ELEMENT twCompList (twCompName+)>
<!ELEMENT twCompName (#PCDATA)>
<!ELEMENT twSigList (twSigName+)>
<!ELEMENT twSigName (#PCDATA)>
<!ELEMENT twBELList (twBELName+)>
<!ELEMENT twBELName (#PCDATA)>
<!ELEMENT twMacList (twMacName+)>
<!ELEMENT twMacName (#PCDATA)>
<!ELEMENT twPinList (twPinName+)>
<!ELEMENT twPinName (#PCDATA)>
<!ELEMENT twUnmetConstCnt (#PCDATA)>
<!ELEMENT twDataSheet (twSUH2ClkList*, (twClk2PadList|twClk2OutList)*, twClk2SUList*, twPad2PadList?)>
<!ATTLIST twDataSheet twNameLen CDATA #REQUIRED>
<!ELEMENT twSUH2ClkList (twDest, twSUH2Clk+)>
<!ATTLIST twSUH2ClkList twDestWidth CDATA #IMPLIED>
<!ATTLIST twSUH2ClkList twPhaseWidth CDATA #IMPLIED>
<!ELEMENT twSUH2Clk (twSrc, twSUHTime, twSUHTime?)>
<!ELEMENT twSUHTime (twSU2ClkTime?,twH2ClkTime?)>
<!ATTLIST twSUHTime twInternalClk CDATA #IMPLIED>
<!ATTLIST twSUHTime twClkPhase CDATA #IMPLIED>
<!ELEMENT twSU2ClkTime (#PCDATA)>
<!ATTLIST twSU2ClkTime twEdge (twRising | twFalling | twIndet) #REQUIRED>
<!ELEMENT twH2ClkTime (#PCDATA)>
<!ATTLIST twH2ClkTime twEdge (twRising | twFalling | twIndet) #REQUIRED>
<!ELEMENT twClk2PadList (twSrc, twClk2Pad+)>
<!ELEMENT twClk2Pad (twDest, twTime)>
<!ELEMENT twTime (#PCDATA)>
<!ATTLIST twTime twEdge (twRising | twFalling | twIndet) #REQUIRED>
<!ELEMENT twClk2OutList (twSrc, twClk2Out+)>
<!ATTLIST twClk2OutList twDestWidth CDATA #REQUIRED>
<!ATTLIST twClk2OutList twPhaseWidth CDATA #REQUIRED>
<!ELEMENT twClk2Out EMPTY>
<!ATTLIST twClk2Out twOutPad CDATA #REQUIRED>
<!ATTLIST twClk2Out twMinTime CDATA #REQUIRED>
<!ATTLIST twClk2Out twMinEdge CDATA #REQUIRED>
<!ATTLIST twClk2Out twMaxTime CDATA #REQUIRED>
<!ATTLIST twClk2Out twMaxEdge CDATA #REQUIRED>
<!ATTLIST twClk2Out twInternalClk CDATA #REQUIRED>
<!ATTLIST twClk2Out twClkPhase CDATA #REQUIRED>
<!ELEMENT twClk2SUList (twDest, twClk2SU+)>
<!ATTLIST twClk2SUList twDestWidth CDATA #IMPLIED>
<!ELEMENT twClk2SU (twSrc, twRiseRise?, twFallRise?, twRiseFall?, twFallFall?)>
<!ELEMENT twRiseRise (#PCDATA)>
<!ELEMENT twFallRise (#PCDATA)>
<!ELEMENT twRiseFall (#PCDATA)>
<!ELEMENT twFallFall (#PCDATA)>
<!ELEMENT twPad2PadList (twPad2Pad+)>
<!ATTLIST twPad2PadList twSrcWidth CDATA #IMPLIED>
<!ATTLIST twPad2PadList twDestWidth CDATA #IMPLIED>
<!ELEMENT twPad2Pad (twSrc, twDest, twDel)>
<!ELEMENT twNonDedClks ((twWarn | twInfo), twNonDedClk+)>
<!ELEMENT twNonDedClk (#PCDATA)>
<!ELEMENT twSum ( twErrCnt, twScore, twConstCov, twStats)>
<!ELEMENT twScore (#PCDATA)>
<!ELEMENT twConstCov (twPathCnt, twNetCnt, twConnCnt, twPct?)>
<!ELEMENT twPathCnt (#PCDATA)>
<!ELEMENT twNetCnt (#PCDATA)>
<!ELEMENT twConnCnt (#PCDATA)>
<!ELEMENT twPct (#PCDATA)>
<!ELEMENT twStats ( twMinPer?, twMaxFreq?, twMaxCombDel?, twMaxFromToDel?, twMaxNetDel?, twMaxNetSkew?, twMaxInAfterClk?, twMinInBeforeClk?, twMaxOutBeforeClk?, twMinOutAfterClk?, (twInfo | twWarn)*)>
<!ELEMENT twMaxCombDel (#PCDATA)>
<!ELEMENT twMaxFromToDel (#PCDATA)>
<!ELEMENT twMaxNetDel (#PCDATA)>
<!ELEMENT twMaxNetSkew (#PCDATA)>
<!ELEMENT twMaxInAfterClk (#PCDATA)>
<!ELEMENT twMinInBeforeClk (#PCDATA)>
<!ELEMENT twMaxOutBeforeClk (#PCDATA)>
<!ELEMENT twMinOutAfterClk (#PCDATA)>
<!ELEMENT twFoot (twTimestamp)>
<!ELEMENT twTimestamp (#PCDATA)>
<!ELEMENT twClientInfo (twClientName, twAttrList?)>
<!ELEMENT twClientName (#PCDATA)>
<!ELEMENT twAttrList (twAttrListItem)*>
<!ELEMENT twAttrListItem (twName, twValue*)>
<!ELEMENT twName (#PCDATA)>
<!ELEMENT twValue (#PCDATA)>
]>
<twReport><twHead><twExecVer>Release 6.3i Trace G.35</twExecVer><twCopyright>Copyright (c) 1995-2004 Xilinx, Inc.  All rights reserved.</twCopyright><twCmdLine>C:/Xilinx6/bin/nt/trce.exe -intstyle ise -e 3 -l 3 -xml rosctrl rosctrl.ncd -o
rosctrl.twr rosctrl.pcf

</twCmdLine><twDesign>rosctrl.ncd</twDesign><twPCF>rosctrl.pcf</twPCF><twDevInfo arch="spartan2e"><twDevName>xc2s100e</twDevName><twSpeedGrade>-7</twSpeedGrade><twSpeedVer>PRODUCTION 1.17 2004-06-25</twSpeedVer></twDevInfo><twRptInfo twRptLvl="twErr"></twRptInfo><twEnvVar name="NONE" description="No environment variables were set" /></twHead><twInfo>INFO:Timing:2752 - To get complete path coverage, use the unconstrained paths option. All paths that are not constrained will be reported in the unconstrained paths section(s) of the report.</twInfo><twBody><twErrRpt><twConst twConstType="twPathConst"><twConstHead><twConstName>TS_clkin_p = PERIOD TIMEGRP &quot;clkin_p&quot;  20 nS   HIGH 50.000000 % ;</twConstName><twItemCnt>0</twItemCnt><twErrCntSetup>0</twErrCntSetup><twErrCntHold twRaceChecked="FALSE">0</twErrCntHold></twConstHead></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>TS_clk_slow = PERIOD TIMEGRP &quot;clk_slow&quot;  10 uS   HIGH 50.000000 % ;</twConstName><twItemCnt>2</twItemCnt><twErrCntSetup>0</twErrCntSetup><twErrCntHold twRaceChecked="TRUE">0</twErrCntHold><twMinPer>1.995</twMinPer></twConstHead></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>TS_CLK0 = PERIOD TIMEGRP &quot;CLK0&quot; TS_clkin_p * 1.000000  HIGH 50.000 % ;</twConstName><twItemCnt>14055</twItemCnt><twErrCntSetup>0</twErrCntSetup><twErrCntHold twRaceChecked="TRUE">0</twErrCntHold><twMinPer>15.201</twMinPer></twConstHead></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>COMP &quot;txena&quot; OFFSET = OUT 11 nS  AFTER COMP &quot;clkin_p&quot; ;</twConstName><twItemCnt>23</twItemCnt><twErrCntSetup>0</twErrCntSetup><twErrCntHold twRaceChecked="FALSE">0</twErrCntHold><twMinOff>10.961</twMinOff></twConstHead></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>COMP &quot;dout&lt;15&gt;&quot; OFFSET = OUT 11 nS  AFTER COMP &quot;clkin_p&quot; ;</twConstName><twItemCnt>23</twItemCnt><twErrCntSetup>0</twErrCntSetup><twErrCntHold twRaceChecked="FALSE">0</twErrCntHold><twMinOff>10.845</twMinOff></twConstHead></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>COMP &quot;dout&lt;14&gt;&quot; OFFSET = OUT 11 nS  AFTER COMP &quot;clkin_p&quot; ;</twConstName><twItemCnt>23</twItemCnt><twErrCntSetup>0</twErrCntSetup><twErrCntHold twRaceChecked="FALSE">0</twErrCntHold><twMinOff>10.940</twMinOff></twConstHead></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>COMP &quot;dout&lt;13&gt;&quot; OFFSET = OUT 11 nS  AFTER COMP &quot;clkin_p&quot; ;</twConstName><twItemCnt>23</twItemCnt><twErrCntSetup>1</twErrCntSetup><twErrCntHold twRaceChecked="FALSE">0</twErrCntHold><twMinOff>11.230</twMinOff></twConstHead><twPathRpt><twConstOffOut twDataPathType = "twDataPathMaxDelay"><twSlack>-0.230</twSlack><twSrc BELType="FF">U4_token</twSrc><twDest BELType="PAD">dout&lt;13&gt;</twDest><twClkDel>-0.108</twClkDel><twClkSrc>clkin_p</twClkSrc><twClkDest>U4_token</twClkDest><twDataDel>11.338</twDataDel><twDataSrc>U4_token</twDataSrc><twDataDest>dout&lt;13&gt;</twDataDest><twOff>11.000</twOff><twOffSrc>clkin_p</twOffSrc><twOffDest>dout&lt;13&gt;</twOffDest><twClkUncert>0.000</twClkUncert><twClkPath maxSiteLen="16"><twSrc BELType="PAD">clkin_p</twSrc><twDest BELType="FF">U4_token</twDest><twLogLvls>3</twLogLvls><twSrcSite>T8.PAD</twSrcSite><twPathDel><twSite>T8.GCLKOUT</twSite><twDelType>Tgpio</twDelType><twDelInfo twEdge="twRising">0.700</twDelInfo><twComp>clkin_p</twComp><twBEL>clkin_p</twBEL><twBEL>UBUF1</twBEL></twPathDel><twPathDel><twSite>DLL1.CLKIN</twSite><twDelType>net</twDelType><twFanCnt>1</twFanCnt><twDelInfo twEdge="twRising">0.000</twDelInfo><twComp>CLKIN</twComp></twPathDel><twPathDel><twSite>DLL1.CLK0</twSite><twDelType>Tdllino</twDelType><twDelInfo twEdge="twRising">-1.579</twDelInfo><twComp>UDLL1</twComp><twBEL>UDLL1</twBEL></twPathDel><twPathDel><twSite>GCLKBUF1.IN</twSite><twDelType>net</twDelType><twFanCnt>1</twFanCnt><twDelInfo twEdge="twRising">0.000</twDelInfo><twComp>CLK0</twComp></twPathDel><twPathDel><twSite>GCLKBUF1.OUT</twSite><twDelType>Tgio</twDelType><twDelInfo twEdge="twRising">0.446</twDelInfo><twComp>UBUF2</twComp><twBEL>UBUF2</twBEL></twPathDel><twPathDel><twSite>CLB_R9C16.S0.CLK</twSite><twDelType>net</twDelType><twFanCnt>561</twFanCnt><twDelInfo twEdge="twRising">0.325</twDelInfo><twComp>tp_1_OBUF</twComp></twPathDel><twLogDel>-0.433</twLogDel><twRouteDel>0.325</twRouteDel><twTotDel>-0.108</twTotDel></twClkPath><twDataPath maxSiteLen="16"><twSrc BELType="FF">U4_token</twSrc><twDest BELType="PAD">dout&lt;13&gt;</twDest><twLogLvls>3</twLogLvls><twSrcSite>CLB_R9C16.S0.CLK</twSrcSite><twSrcClk twEdge ="twRising" twArriveTime ="0.000">tp_1_OBUF</twSrcClk><twPathDel><twSite>CLB_R9C16.S0.YQ</twSite><twDelType>Tcko</twDelType><twDelInfo twEdge="twRising">0.886</twDelInfo><twComp>U4_token</twComp><twBEL>U4_token</twBEL></twPathDel><twPathDel><twSite>CLB_R10C15.S1.G2</twSite><twDelType>net</twDelType><twFanCnt>10</twFanCnt><twDelInfo twEdge="twRising">0.763</twDelInfo><twComp>U4_token</twComp></twPathDel><twPathDel><twSite>CLB_R10C15.S1.Y</twSite><twDelType>Tilo</twDelType><twDelInfo twEdge="twRising">0.418</twDelInfo><twComp>U3_hastoken</twComp><twBEL>U4__n00031</twBEL></twPathDel><twPathDel><twSite>CLB_R9C17.S0.G3</twSite><twDelType>net</twDelType><twFanCnt>18</twFanCnt><twDelInfo twEdge="twRising">1.196</twDelInfo><twComp>token&lt;4&gt;</twComp></twPathDel><twPathDel><twSite>CLB_R9C17.S0.Y</twSite><twDelType>Tilo</twDelType><twDelInfo twEdge="twRising">0.418</twDelInfo><twComp>N52353</twComp><twBEL>_n0030</twBEL></twPathDel><twPathDel><twSite>J3.T</twSite><twDelType>net</twDelType><twFanCnt>17</twFanCnt><twDelInfo twEdge="twRising">3.026</twDelInfo><twComp>_n0030</twComp></twPathDel><twPathDel><twSite>J3.PAD</twSite><twDelType>Tioton</twDelType><twDelInfo twEdge="twRising">4.631</twDelInfo><twComp>dout&lt;13&gt;</twComp><twBEL>dout_13_OBUFT</twBEL><twBEL>dout&lt;13&gt;</twBEL></twPathDel><twLogDel>6.353</twLogDel><twRouteDel>4.985</twRouteDel><twTotDel>11.338</twTotDel><twPctLog>56.0</twPctLog><twPctRoute>44.0</twPctRoute></twDataPath></twConstOffOut></twPathRpt><twPathRpt><twConstOffOut twDataPathType = "twDataPathMaxDelay"><twSlack>-0.219</twSlack><twSrc BELType="FF">U4_token</twSrc><twDest BELType="PAD">dout&lt;13&gt;</twDest><twClkDel>-0.108</twClkDel><twClkSrc>clkin_p</twClkSrc><twClkDest>U4_token</twClkDest><twDataDel>11.327</twDataDel><twDataSrc>U4_token</twDataSrc><twDataDest>dout&lt;13&gt;</twDataDest><twOff>11.000</twOff><twOffSrc>clkin_p</twOffSrc><twOffDest>dout&lt;13&gt;</twOffDest><twClkUncert>0.000</twClkUncert><twClkPath maxSiteLen="16"><twSrc BELType="PAD">clkin_p</twSrc><twDest BELType="FF">U4_token</twDest><twLogLvls>3</twLogLvls><twSrcSite>T8.PAD</twSrcSite><twPathDel><twSite>T8.GCLKOUT</twSite><twDelType>Tgpio</twDelType><twDelInfo twEdge="twRising">0.700</twDelInfo><twComp>clkin_p</twComp><twBEL>clkin_p</twBEL><twBEL>UBUF1</twBEL></twPathDel><twPathDel><twSite>DLL1.CLKIN</twSite><twDelType>net</twDelType><twFanCnt>1</twFanCnt><twDelInfo twEdge="twRising">0.000</twDelInfo><twComp>CLKIN</twComp></twPathDel><twPathDel><twSite>DLL1.CLK0</twSite><twDelType>Tdllino</twDelType><twDelInfo twEdge="twRising">-1.579</twDelInfo><twComp>UDLL1</twComp><twBEL>UDLL1</twBEL></twPathDel><twPathDel><twSite>GCLKBUF1.IN</twSite><twDelType>net</twDelType><twFanCnt>1</twFanCnt><twDelInfo twEdge="twRising">0.000</twDelInfo><twComp>CLK0</twComp></twPathDel><twPathDel><twSite>GCLKBUF1.OUT</twSite><twDelType>Tgio</twDelType><twDelInfo twEdge="twRising">0.446</twDelInfo><twComp>UBUF2</twComp><twBEL>UBUF2</twBEL></twPathDel><twPathDel><twSite>CLB_R9C16.S0.CLK</twSite><twDelType>net</twDelType><twFanCnt>561</twFanCnt><twDelInfo twEdge="twRising">0.325</twDelInfo><twComp>tp_1_OBUF</twComp></twPathDel><twLogDel>-0.433</twLogDel><twRouteDel>0.325</twRouteDel><twTotDel>-0.108</twTotDel></twClkPath><twDataPath maxSiteLen="15"><twSrc BELType="FF">U4_token</twSrc><twDest BELType="PAD">dout&lt;13&gt;</twDest><twLogLvls>4</twLogLvls><twSrcSite>CLB_R9C16.S0.CLK</twSrcSite><twSrcClk twEdge ="twRising" twArriveTime ="0.000">tp_1_OBUF</twSrcClk><twPathDel><twSite>CLB_R9C16.S0.YQ</twSite><twDelType>Tcko</twDelType><twDelInfo twEdge="twRising">0.886</twDelInfo><twComp>U4_token</twComp><twBEL>U4_token</twBEL></twPathDel><twPathDel><twSite>CLB_R8C17.S0.F3</twSite><twDelType>net</twDelType><twFanCnt>10</twFanCnt><twDelInfo twEdge="twRising">0.590</twDelInfo><twComp>U4_token</twComp></twPathDel><twPathDel><twSite>CLB_R8C17.S0.X</twSite><twDelType>Tilo</twDelType><twDelInfo twEdge="twRising">0.418</twDelInfo><twComp>token_p_0_OBUF</twComp><twBEL>U4__n00071</twBEL></twPathDel><twPathDel><twSite>CLB_R9C17.S0.F4</twSite><twDelType>net</twDelType><twFanCnt>2</twFanCnt><twDelInfo twEdge="twRising">0.674</twDelInfo><twComp>token_p_0_OBUF</twComp></twPathDel><twPathDel><twSite>CLB_R9C17.S0.X</twSite><twDelType>Tilo</twDelType><twDelInfo twEdge="twRising">0.418</twDelInfo><twComp>N52353</twComp><twBEL>_n0030_SW0</twBEL></twPathDel><twPathDel><twSite>CLB_R9C17.S0.G4</twSite><twDelType>net</twDelType><twFanCnt>1</twFanCnt><twDelInfo twEdge="twRising">0.266</twDelInfo><twComp>N52353</twComp></twPathDel><twPathDel><twSite>CLB_R9C17.S0.Y</twSite><twDelType>Tilo</twDelType><twDelInfo twEdge="twRising">0.418</twDelInfo><twComp>N52353</twComp><twBEL>_n0030</twBEL></twPathDel><twPathDel><twSite>J3.T</twSite><twDelType>net</twDelType><twFanCnt>17</twFanCnt><twDelInfo twEdge="twRising">3.026</twDelInfo><twComp>_n0030</twComp></twPathDel><twPathDel><twSite>J3.PAD</twSite><twDelType>Tioton</twDelType><twDelInfo twEdge="twRising">4.631</twDelInfo><twComp>dout&lt;13&gt;</twComp><twBEL>dout_13_OBUFT</twBEL><twBEL>dout&lt;13&gt;</twBEL></twPathDel><twLogDel>6.771</twLogDel><twRouteDel>4.556</twRouteDel><twTotDel>11.327</twTotDel><twPctLog>59.8</twPctLog><twPctRoute>40.2</twPctRoute></twDataPath></twConstOffOut></twPathRpt><twPathRpt><twConstOffOut twDataPathType = "twDataPathMaxDelay"><twSlack>-0.188</twSlack><twSrc BELType="FF">U4_ceros_id_0</twSrc><twDest BELType="PAD">dout&lt;13&gt;</twDest><twClkDel>-0.108</twClkDel><twClkSrc>clkin_p</twClkSrc><twClkDest>U4_ceros_id&lt;1&gt;</twClkDest><twDataDel>11.296</twDataDel><twDataSrc>U4_ceros_id&lt;1&gt;</twDataSrc><twDataDest>dout&lt;13&gt;</twDataDest><twOff>11.000</twOff><twOffSrc>clkin_p</twOffSrc><twOffDest>dout&lt;13&gt;</twOffDest><twClkUncert>0.000</twClkUncert><twClkPath maxSiteLen="16"><twSrc BELType="PAD">clkin_p</twSrc><twDest BELType="FF">U4_ceros_id_0</twDest><twLogLvls>3</twLogLvls><twSrcSite>T8.PAD</twSrcSite><twPathDel><twSite>T8.GCLKOUT</twSite><twDelType>Tgpio</twDelType><twDelInfo twEdge="twRising">0.700</twDelInfo><twComp>clkin_p</twComp><twBEL>clkin_p</twBEL><twBEL>UBUF1</twBEL></twPathDel><twPathDel><twSite>DLL1.CLKIN</twSite><twDelType>net</twDelType><twFanCnt>1</twFanCnt><twDelInfo twEdge="twRising">0.000</twDelInfo><twComp>CLKIN</twComp></twPathDel><twPathDel><twSite>DLL1.CLK0</twSite><twDelType>Tdllino</twDelType><twDelInfo twEdge="twRising">-1.579</twDelInfo><twComp>UDLL1</twComp><twBEL>UDLL1</twBEL></twPathDel><twPathDel><twSite>GCLKBUF1.IN</twSite><twDelType>net</twDelType><twFanCnt>1</twFanCnt><twDelInfo twEdge="twRising">0.000</twDelInfo><twComp>CLK0</twComp></twPathDel><twPathDel><twSite>GCLKBUF1.OUT</twSite><twDelType>Tgio</twDelType><twDelInfo twEdge="twRising">0.446</twDelInfo><twComp>UBUF2</twComp><twBEL>UBUF2</twBEL></twPathDel><twPathDel><twSite>CLB_R9C16.S1.CLK</twSite><twDelType>net</twDelType><twFanCnt>561</twFanCnt><twDelInfo twEdge="twRising">0.325</twDelInfo><twComp>tp_1_OBUF</twComp></twPathDel><twLogDel>-0.433</twLogDel><twRouteDel>0.325</twRouteDel><twTotDel>-0.108</twTotDel></twClkPath><twDataPath maxSiteLen="15"><twSrc BELType="FF">U4_ceros_id_0</twSrc><twDest BELType="PAD">dout&lt;13&gt;</twDest><twLogLvls>4</twLogLvls><twSrcSite>CLB_R9C16.S1.CLK</twSrcSite><twSrcClk twEdge ="twRising" twArriveTime ="0.000">tp_1_OBUF</twSrcClk><twPathDel><twSite>CLB_R9C16.S1.YQ</twSite><twDelType>Tcko</twDelType><twDelInfo twEdge="twRising">0.886</twDelInfo><twComp>U4_ceros_id&lt;1&gt;</twComp><twBEL>U4_ceros_id_0</twBEL></twPathDel><twPathDel><twSite>CLB_R8C17.S0.F4</twSite><twDelType>net</twDelType><twFanCnt>14</twFanCnt><twDelInfo twEdge="twRising">0.559</twDelInfo><twComp>U4_ceros_id&lt;0&gt;</twComp></twPathDel><twPathDel><twSite>CLB_R8C17.S0.X</twSite><twDelType>Tilo</twDelType><twDelInfo twEdge="twRising">0.418</twDelInfo><twComp>token_p_0_OBUF</twComp><twBEL>U4__n00071</twBEL></twPathDel><twPathDel><twSite>CLB_R9C17.S0.F4</twSite><twDelType>net</twDelType><twFanCnt>2</twFanCnt><twDelInfo twEdge="twRising">0.674</twDelInfo><twComp>token_p_0_OBUF</twComp></twPathDel><twPathDel><twSite>CLB_R9C17.S0.X</twSite><twDelType>Tilo</twDelType><twDelInfo twEdge="twRising">0.418</twDelInfo><twComp>N52353</twComp><twBEL>_n0030_SW0</twBEL></twPathDel><twPathDel><twSite>CLB_R9C17.S0.G4</twSite><twDelType>net</twDelType><twFanCnt>1</twFanCnt><twDelInfo twEdge="twRising">0.266</twDelInfo><twComp>N52353</twComp></twPathDel><twPathDel><twSite>CLB_R9C17.S0.Y</twSite><twDelType>Tilo</twDelType><twDelInfo twEdge="twRising">0.418</twDelInfo><twComp>N52353</twComp><twBEL>_n0030</twBEL></twPathDel><twPathDel><twSite>J3.T</twSite><twDelType>net</twDelType><twFanCnt>17</twFanCnt><twDelInfo twEdge="twRising">3.026</twDelInfo><twComp>_n0030</twComp></twPathDel><twPathDel><twSite>J3.PAD</twSite><twDelType>Tioton</twDelType><twDelInfo twEdge="twRising">4.631</twDelInfo><twComp>dout&lt;13&gt;</twComp><twBEL>dout_13_OBUFT</twBEL><twBEL>dout&lt;13&gt;</twBEL></twPathDel><twLogDel>6.771</twLogDel><twRouteDel>4.525</twRouteDel><twTotDel>11.296</twTotDel><twPctLog>59.9</twPctLog><twPctRoute>40.1</twPctRoute></twDataPath></twConstOffOut></twPathRpt></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>COMP &quot;dout&lt;12&gt;&quot; OFFSET = OUT 11 nS  AFTER COMP &quot;clkin_p&quot; ;</twConstName><twItemCnt>23</twItemCnt><twErrCntSetup>1</twErrCntSetup><twErrCntHold twRaceChecked="FALSE">0</twErrCntHold><twMinOff>11.027</twMinOff></twConstHead><twPathRpt><twConstOffOut twDataPathType = "twDataPathMaxDelay"><twSlack>-0.027</twSlack><twSrc BELType="FF">U4_token</twSrc><twDest BELType="PAD">dout&lt;12&gt;</twDest><twClkDel>-0.108</twClkDel><twClkSrc>clkin_p</twClkSrc><twClkDest>U4_token</twClkDest><twDataDel>11.135</twDataDel><twDataSrc>U4_token</twDataSrc><twDataDest>dout&lt;12&gt;</twDataDest><twOff>11.000</twOff><twOffSrc>clkin_p</twOffSrc><twOffDest>dout&lt;12&gt;</twOffDest><twClkUncert>0.000</twClkUncert><twClkPath maxSiteLen="16"><twSrc BELType="PAD">clkin_p</twSrc><twDest BELType="FF">U4_token</twDest><twLogLvls>3</twLogLvls><twSrcSite>T8.PAD</twSrcSite><twPathDel><twSite>T8.GCLKOUT</twSite><twDelType>Tgpio</twDelType><twDelInfo twEdge="twRising">0.700</twDelInfo><twComp>clkin_p</twComp><twBEL>clkin_p</twBEL><twBEL>UBUF1</twBEL></twPathDel><twPathDel><twSite>DLL1.CLKIN</twSite><twDelType>net</twDelType><twFanCnt>1</twFanCnt><twDelInfo twEdge="twRising">0.000</twDelInfo><twComp>CLKIN</twComp></twPathDel><twPathDel><twSite>DLL1.CLK0</twSite><twDelType>Tdllino</twDelType><twDelInfo twEdge="twRising">-1.579</twDelInfo><twComp>UDLL1</twComp><twBEL>UDLL1</twBEL></twPathDel><twPathDel><twSite>GCLKBUF1.IN</twSite><twDelType>net</twDelType><twFanCnt>1</twFanCnt><twDelInfo twEdge="twRising">0.000</twDelInfo><twComp>CLK0</twComp></twPathDel><twPathDel><twSite>GCLKBUF1.OUT</twSite><twDelType>Tgio</twDelType><twDelInfo twEdge="twRising">0.446</twDelInfo><twComp>UBUF2</twComp><twBEL>UBUF2</twBEL></twPathDel><twPathDel><twSite>CLB_R9C16.S0.CLK</twSite><twDelType>net</twDelType><twFanCnt>561</twFanCnt><twDelInfo twEdge="twRising">0.325</twDelInfo><twComp>tp_1_OBUF</twComp></twPathDel><twLogDel>-0.433</twLogDel><twRouteDel>0.325</twRouteDel><twTotDel>-0.108</twTotDel></twClkPath><twDataPath maxSiteLen="16"><twSrc BELType="FF">U4_token</twSrc><twDest BELType="PAD">dout&lt;12&gt;</twDest><twLogLvls>3</twLogLvls><twSrcSite>CLB_R9C16.S0.CLK</twSrcSite><twSrcClk twEdge ="twRising" twArriveTime ="0.000">tp_1_OBUF</twSrcClk><twPathDel><twSite>CLB_R9C16.S0.YQ</twSite><twDelType>Tcko</twDelType><twDelInfo twEdge="twRising">0.886</twDelInfo><twComp>U4_token</twComp><twBEL>U4_token</twBEL></twPathDel><twPathDel><twSite>CLB_R10C15.S1.G2</twSite><twDelType>net</twDelType><twFanCnt>10</twFanCnt><twDelInfo twEdge="twRising">0.763</twDelInfo><twComp>U4_token</twComp></twPathDel><twPathDel><twSite>CLB_R10C15.S1.Y</twSite><twDelType>Tilo</twDelType><twDelInfo twEdge="twRising">0.418</twDelInfo><twComp>U3_hastoken</twComp><twBEL>U4__n00031</twBEL></twPathDel><twPathDel><twSite>CLB_R9C17.S0.G3</twSite><twDelType>net</twDelType><twFanCnt>18</twFanCnt><twDelInfo twEdge="twRising">1.196</twDelInfo><twComp>token&lt;4&gt;</twComp></twPathDel><twPathDel><twSite>CLB_R9C17.S0.Y</twSite><twDelType>Tilo</twDelType><twDelInfo twEdge="twRising">0.418</twDelInfo><twComp>N52353</twComp><twBEL>_n0030</twBEL></twPathDel><twPathDel><twSite>H1.T</twSite><twDelType>net</twDelType><twFanCnt>17</twFanCnt><twDelInfo twEdge="twRising">2.823</twDelInfo><twComp>_n0030</twComp></twPathDel><twPathDel><twSite>H1.PAD</twSite><twDelType>Tioton</twDelType><twDelInfo twEdge="twRising">4.631</twDelInfo><twComp>dout&lt;12&gt;</twComp><twBEL>dout_12_OBUFT</twBEL><twBEL>dout&lt;12&gt;</twBEL></twPathDel><twLogDel>6.353</twLogDel><twRouteDel>4.782</twRouteDel><twTotDel>11.135</twTotDel><twPctLog>57.1</twPctLog><twPctRoute>42.9</twPctRoute></twDataPath></twConstOffOut></twPathRpt><twPathRpt><twConstOffOut twDataPathType = "twDataPathMaxDelay"><twSlack>-0.016</twSlack><twSrc BELType="FF">U4_token</twSrc><twDest BELType="PAD">dout&lt;12&gt;</twDest><twClkDel>-0.108</twClkDel><twClkSrc>clkin_p</twClkSrc><twClkDest>U4_token</twClkDest><twDataDel>11.124</twDataDel><twDataSrc>U4_token</twDataSrc><twDataDest>dout&lt;12&gt;</twDataDest><twOff>11.000</twOff><twOffSrc>clkin_p</twOffSrc><twOffDest>dout&lt;12&gt;</twOffDest><twClkUncert>0.000</twClkUncert><twClkPath maxSiteLen="16"><twSrc BELType="PAD">clkin_p</twSrc><twDest BELType="FF">U4_token</twDest><twLogLvls>3</twLogLvls><twSrcSite>T8.PAD</twSrcSite><twPathDel><twSite>T8.GCLKOUT</twSite><twDelType>Tgpio</twDelType><twDelInfo twEdge="twRising">0.700</twDelInfo><twComp>clkin_p</twComp><twBEL>clkin_p</twBEL><twBEL>UBUF1</twBEL></twPathDel><twPathDel><twSite>DLL1.CLKIN</twSite><twDelType>net</twDelType><twFanCnt>1</twFanCnt><twDelInfo twEdge="twRising">0.000</twDelInfo><twComp>CLKIN</twComp></twPathDel><twPathDel><twSite>DLL1.CLK0</twSite><twDelType>Tdllino</twDelType><twDelInfo twEdge="twRising">-1.579</twDelInfo><twComp>UDLL1</twComp><twBEL>UDLL1</twBEL></twPathDel><twPathDel><twSite>GCLKBUF1.IN</twSite><twDelType>net</twDelType><twFanCnt>1</twFanCnt><twDelInfo twEdge="twRising">0.000</twDelInfo><twComp>CLK0</twComp></twPathDel><twPathDel><twSite>GCLKBUF1.OUT</twSite><twDelType>Tgio</twDelType><twDelInfo twEdge="twRising">0.446</twDelInfo><twComp>UBUF2</twComp><twBEL>UBUF2</twBEL></twPathDel><twPathDel><twSite>CLB_R9C16.S0.CLK</twSite><twDelType>net</twDelType><twFanCnt>561</twFanCnt><twDelInfo twEdge="twRising">0.325</twDelInfo><twComp>tp_1_OBUF</twComp></twPathDel><twLogDel>-0.433</twLogDel><twRouteDel>0.325</twRouteDel><twTotDel>-0.108</twTotDel></twClkPath><twDataPath maxSiteLen="15"><twSrc BELType="FF">U4_token</twSrc><twDest BELType="PAD">dout&lt;12&gt;</twDest><twLogLvls>4</twLogLvls><twSrcSite>CLB_R9C16.S0.CLK</twSrcSite><twSrcClk twEdge ="twRising" twArriveTime ="0.000">tp_1_OBUF</twSrcClk><twPathDel><twSite>CLB_R9C16.S0.YQ</twSite><twDelType>Tcko</twDelType><twDelInfo twEdge="twRising">0.886</twDelInfo><twComp>U4_token</twComp><twBEL>U4_token</twBEL></twPathDel><twPathDel><twSite>CLB_R8C17.S0.F3</twSite><twDelType>net</twDelType><twFanCnt>10</twFanCnt><twDelInfo twEdge="twRising">0.590</twDelInfo><twComp>U4_token</twComp></twPathDel><twPathDel><twSite>CLB_R8C17.S0.X</twSite><twDelType>Tilo</twDelType><twDelInfo twEdge="twRising">0.418</twDelInfo><twComp>token_p_0_OBUF</twComp><twBEL>U4__n00071</twBEL></twPathDel><twPathDel><twSite>CLB_R9C17.S0.F4</twSite><twDelType>net</twDelType><twFanCnt>2</twFanCnt><twDelInfo twEdge="twRising">0.674</twDelInfo><twComp>token_p_0_OBUF</twComp></twPathDel><twPathDel><twSite>CLB_R9C17.S0.X</twSite><twDelType>Tilo</twDelType><twDelInfo twEdge="twRising">0.418</twDelInfo><twComp>N52353</twComp><twBEL>_n0030_SW0</twBEL></twPathDel><twPathDel><twSite>CLB_R9C17.S0.G4</twSite><twDelType>net</twDelType><twFanCnt>1</twFanCnt><twDelInfo twEdge="twRising">0.266</twDelInfo><twComp>N52353</twComp></twPathDel><twPathDel><twSite>CLB_R9C17.S0.Y</twSite><twDelType>Tilo</twDelType><twDelInfo twEdge="twRising">0.418</twDelInfo><twComp>N52353</twComp><twBEL>_n0030</twBEL></twPathDel><twPathDel><twSite>H1.T</twSite><twDelType>net</twDelType><twFanCnt>17</twFanCnt><twDelInfo twEdge="twRising">2.823</twDelInfo><twComp>_n0030</twComp></twPathDel><twPathDel><twSite>H1.PAD</twSite><twDelType>Tioton</twDelType><twDelInfo twEdge="twRising">4.631</twDelInfo><twComp>dout&lt;12&gt;</twComp><twBEL>dout_12_OBUFT</twBEL><twBEL>dout&lt;12&gt;</twBEL></twPathDel><twLogDel>6.771</twLogDel><twRouteDel>4.353</twRouteDel><twTotDel>11.124</twTotDel><twPctLog>60.9</twPctLog><twPctRoute>39.1</twPctRoute></twDataPath></twConstOffOut></twPathRpt></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>COMP &quot;dout&lt;11&gt;&quot; OFFSET = OUT 11 nS  AFTER COMP &quot;clkin_p&quot; ;</twConstName><twItemCnt>23</twItemCnt><twErrCntSetup>0</twErrCntSetup><twErrCntHold twRaceChecked="FALSE">0</twErrCntHold><twMinOff>10.706</twMinOff></twConstHead></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>COMP &quot;dout&lt;10&gt;&quot; OFFSET = OUT 11 nS  AFTER COMP &quot;clkin_p&quot; ;</twConstName><twItemCnt>23</twItemCnt><twErrCntSetup>0</twErrCntSetup><twErrCntHold twRaceChecked="FALSE">0</twErrCntHold><twMinOff>10.886</twMinOff></twConstHead></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>COMP &quot;dout&lt;9&gt;&quot; OFFSET = OUT 11 nS  AFTER COMP &quot;clkin_p&quot; ;</twConstName><twItemCnt>23</twItemCnt><twErrCntSetup>1</twErrCntSetup><twErrCntHold twRaceChecked="FALSE">0</twErrCntHold><twMinOff>11.143</twMinOff></twConstHead><twPathRpt><twConstOffOut twDataPathType = "twDataPathMaxDelay"><twSlack>-0.143</twSlack><twSrc BELType="FF">U4_token</twSrc><twDest BELType="PAD">dout&lt;9&gt;</twDest><twClkDel>-0.108</twClkDel><twClkSrc>clkin_p</twClkSrc><twClkDest>U4_token</twClkDest><twDataDel>11.251</twDataDel><twDataSrc>U4_token</twDataSrc><twDataDest>dout&lt;9&gt;</twDataDest><twOff>11.000</twOff><twOffSrc>clkin_p</twOffSrc><twOffDest>dout&lt;9&gt;</twOffDest><twClkUncert>0.000</twClkUncert><twClkPath maxSiteLen="16"><twSrc BELType="PAD">clkin_p</twSrc><twDest BELType="FF">U4_token</twDest><twLogLvls>3</twLogLvls><twSrcSite>T8.PAD</twSrcSite><twPathDel><twSite>T8.GCLKOUT</twSite><twDelType>Tgpio</twDelType><twDelInfo twEdge="twRising">0.700</twDelInfo><twComp>clkin_p</twComp><twBEL>clkin_p</twBEL><twBEL>UBUF1</twBEL></twPathDel><twPathDel><twSite>DLL1.CLKIN</twSite><twDelType>net</twDelType><twFanCnt>1</twFanCnt><twDelInfo twEdge="twRising">0.000</twDelInfo><twComp>CLKIN</twComp></twPathDel><twPathDel><twSite>DLL1.CLK0</twSite><twDelType>Tdllino</twDelType><twDelInfo twEdge="twRising">-1.579</twDelInfo><twComp>UDLL1</twComp><twBEL>UDLL1</twBEL></twPathDel><twPathDel><twSite>GCLKBUF1.IN</twSite><twDelType>net</twDelType><twFanCnt>1</twFanCnt><twDelInfo twEdge="twRising">0.000</twDelInfo><twComp>CLK0</twComp></twPathDel><twPathDel><twSite>GCLKBUF1.OUT</twSite><twDelType>Tgio</twDelType><twDelInfo twEdge="twRising">0.446</twDelInfo><twComp>UBUF2</twComp><twBEL>UBUF2</twBEL></twPathDel><twPathDel><twSite>CLB_R9C16.S0.CLK</twSite><twDelType>net</twDelType><twFanCnt>561</twFanCnt><twDelInfo twEdge="twRising">0.325</twDelInfo><twComp>tp_1_OBUF</twComp></twPathDel><twLogDel>-0.433</twLogDel><twRouteDel>0.325</twRouteDel><twTotDel>-0.108</twTotDel></twClkPath><twDataPath maxSiteLen="16"><twSrc BELType="FF">U4_token</twSrc><twDest BELType="PAD">dout&lt;9&gt;</twDest><twLogLvls>3</twLogLvls><twSrcSite>CLB_R9C16.S0.CLK</twSrcSite><twSrcClk twEdge ="twRising" twArriveTime ="0.000">tp_1_OBUF</twSrcClk><twPathDel><twSite>CLB_R9C16.S0.YQ</twSite><twDelType>Tcko</twDelType><twDelInfo twEdge="twRising">0.886</twDelInfo><twComp>U4_token</twComp><twBEL>U4_token</twBEL></twPathDel><twPathDel><twSite>CLB_R10C15.S1.G2</twSite><twDelType>net</twDelType><twFanCnt>10</twFanCnt><twDelInfo twEdge="twRising">0.763</twDelInfo><twComp>U4_token</twComp></twPathDel><twPathDel><twSite>CLB_R10C15.S1.Y</twSite><twDelType>Tilo</twDelType><twDelInfo twEdge="twRising">0.418</twDelInfo><twComp>U3_hastoken</twComp><twBEL>U4__n00031</twBEL></twPathDel><twPathDel><twSite>CLB_R9C17.S0.G3</twSite><twDelType>net</twDelType><twFanCnt>18</twFanCnt><twDelInfo twEdge="twRising">1.196</twDelInfo><twComp>token&lt;4&gt;</twComp></twPathDel><twPathDel><twSite>CLB_R9C17.S0.Y</twSite><twDelType>Tilo</twDelType><twDelInfo twEdge="twRising">0.418</twDelInfo><twComp>N52353</twComp><twBEL>_n0030</twBEL></twPathDel><twPathDel><twSite>J2.T</twSite><twDelType>net</twDelType><twFanCnt>17</twFanCnt><twDelInfo twEdge="twRising">2.939</twDelInfo><twComp>_n0030</twComp></twPathDel><twPathDel><twSite>J2.PAD</twSite><twDelType>Tioton</twDelType><twDelInfo twEdge="twRising">4.631</twDelInfo><twComp>dout&lt;9&gt;</twComp><twBEL>dout_9_OBUFT</twBEL><twBEL>dout&lt;9&gt;</twBEL></twPathDel><twLogDel>6.353</twLogDel><twRouteDel>4.898</twRouteDel><twTotDel>11.251</twTotDel><twPctLog>56.5</twPctLog><twPctRoute>43.5</twPctRoute></twDataPath></twConstOffOut></twPathRpt><twPathRpt><twConstOffOut twDataPathType = "twDataPathMaxDelay"><twSlack>-0.132</twSlack><twSrc BELType="FF">U4_token</twSrc><twDest BELType="PAD">dout&lt;9&gt;</twDest><twClkDel>-0.108</twClkDel><twClkSrc>clkin_p</twClkSrc><twClkDest>U4_token</twClkDest><twDataDel>11.240</twDataDel><twDataSrc>U4_token</twDataSrc><twDataDest>dout&lt;9&gt;</twDataDest><twOff>11.000</twOff><twOffSrc>clkin_p</twOffSrc><twOffDest>dout&lt;9&gt;</twOffDest><twClkUncert>0.000</twClkUncert><twClkPath maxSiteLen="16"><twSrc BELType="PAD">clkin_p</twSrc><twDest BELType="FF">U4_token</twDest><twLogLvls>3</twLogLvls><twSrcSite>T8.PAD</twSrcSite><twPathDel><twSite>T8.GCLKOUT</twSite><twDelType>Tgpio</twDelType><twDelInfo twEdge="twRising">0.700</twDelInfo><twComp>clkin_p</twComp><twBEL>clkin_p</twBEL><twBEL>UBUF1</twBEL></twPathDel><twPathDel><twSite>DLL1.CLKIN</twSite><twDelType>net</twDelType><twFanCnt>1</twFanCnt><twDelInfo twEdge="twRising">0.000</twDelInfo><twComp>CLKIN</twComp></twPathDel><twPathDel><twSite>DLL1.CLK0</twSite><twDelType>Tdllino</twDelType><twDelInfo twEdge="twRising">-1.579</twDelInfo><twComp>UDLL1</twComp><twBEL>UDLL1</twBEL></twPathDel><twPathDel><twSite>GCLKBUF1.IN</twSite><twDelType>net</twDelType><twFanCnt>1</twFanCnt><twDelInfo twEdge="twRising">0.000</twDelInfo><twComp>CLK0</twComp></twPathDel><twPathDel><twSite>GCLKBUF1.OUT</twSite><twDelType>Tgio</twDelType><twDelInfo twEdge="twRising">0.446</twDelInfo><twComp>UBUF2</twComp><twBEL>UBUF2</twBEL></twPathDel><twPathDel><twSite>CLB_R9C16.S0.CLK</twSite><twDelType>net</twDelType><twFanCnt>561</twFanCnt><twDelInfo twEdge="twRising">0.325</twDelInfo><twComp>tp_1_OBUF</twComp></twPathDel><twLogDel>-0.433</twLogDel><twRouteDel>0.325</twRouteDel><twTotDel>-0.108</twTotDel></twClkPath><twDataPath maxSiteLen="15"><twSrc BELType="FF">U4_token</twSrc><twDest BELType="PAD">dout&lt;9&gt;</twDest><twLogLvls>4</twLogLvls><twSrcSite>CLB_R9C16.S0.CLK</twSrcSite><twSrcClk twEdge ="twRising" twArriveTime ="0.000">tp_1_OBUF</twSrcClk><twPathDel><twSite>CLB_R9C16.S0.YQ</twSite><twDelType>Tcko</twDelType><twDelInfo twEdge="twRising">0.886</twDelInfo><twComp>U4_token</twComp><twBEL>U4_token</twBEL></twPathDel><twPathDel><twSite>CLB_R8C17.S0.F3</twSite><twDelType>net</twDelType><twFanCnt>10</twFanCnt><twDelInfo twEdge="twRising">0.590</twDelInfo><twComp>U4_token</twComp></twPathDel><twPathDel><twSite>CLB_R8C17.S0.X</twSite><twDelType>Tilo</twDelType><twDelInfo twEdge="twRising">0.418</twDelInfo><twComp>token_p_0_OBUF</twComp><twBEL>U4__n00071</twBEL></twPathDel><twPathDel><twSite>CLB_R9C17.S0.F4</twSite><twDelType>net</twDelType><twFanCnt>2</twFanCnt><twDelInfo twEdge="twRising">0.674</twDelInfo><twComp>token_p_0_OBUF</twComp></twPathDel><twPathDel><twSite>CLB_R9C17.S0.X</twSite><twDelType>Tilo</twDelType><twDelInfo twEdge="twRising">0.418</twDelInfo><twComp>N52353</twComp><twBEL>_n0030_SW0</twBEL></twPathDel><twPathDel><twSite>CLB_R9C17.S0.G4</twSite><twDelType>net</twDelType><twFanCnt>1</twFanCnt><twDelInfo twEdge="twRising">0.266</twDelInfo><twComp>N52353</twComp></twPathDel><twPathDel><twSite>CLB_R9C17.S0.Y</twSite><twDelType>Tilo</twDelType><twDelInfo twEdge="twRising">0.418</twDelInfo><twComp>N52353</twComp><twBEL>_n0030</twBEL></twPathDel><twPathDel><twSite>J2.T</twSite><twDelType>net</twDelType><twFanCnt>17</twFanCnt><twDelInfo twEdge="twRising">2.939</twDelInfo><twComp>_n0030</twComp></twPathDel><twPathDel><twSite>J2.PAD</twSite><twDelType>Tioton</twDelType><twDelInfo twEdge="twRising">4.631</twDelInfo><twComp>dout&lt;9&gt;</twComp><twBEL>dout_9_OBUFT</twBEL><twBEL>dout&lt;9&gt;</twBEL></twPathDel><twLogDel>6.771</twLogDel><twRouteDel>4.469</twRouteDel><twTotDel>11.240</twTotDel><twPctLog>60.2</twPctLog><twPctRoute>39.8</twPctRoute></twDataPath></twConstOffOut></twPathRpt><twPathRpt><twConstOffOut twDataPathType = "twDataPathMaxDelay"><twSlack>-0.101</twSlack><twSrc BELType="FF">U4_ceros_id_0</twSrc><twDest BELType="PAD">dout&lt;9&gt;</twDest><twClkDel>-0.108</twClkDel><twClkSrc>clkin_p</twClkSrc><twClkDest>U4_ceros_id&lt;1&gt;</twClkDest><twDataDel>11.209</twDataDel><twDataSrc>U4_ceros_id&lt;1&gt;</twDataSrc><twDataDest>dout&lt;9&gt;</twDataDest><twOff>11.000</twOff><twOffSrc>clkin_p</twOffSrc><twOffDest>dout&lt;9&gt;</twOffDest><twClkUncert>0.000</twClkUncert><twClkPath maxSiteLen="16"><twSrc BELType="PAD">clkin_p</twSrc><twDest BELType="FF">U4_ceros_id_0</twDest><twLogLvls>3</twLogLvls><twSrcSite>T8.PAD</twSrcSite><twPathDel><twSite>T8.GCLKOUT</twSite><twDelType>Tgpio</twDelType><twDelInfo twEdge="twRising">0.700</twDelInfo><twComp>clkin_p</twComp><twBEL>clkin_p</twBEL><twBEL>UBUF1</twBEL></twPathDel><twPathDel><twSite>DLL1.CLKIN</twSite><twDelType>net</twDelType><twFanCnt>1</twFanCnt><twDelInfo twEdge="twRising">0.000</twDelInfo><twComp>CLKIN</twComp></twPathDel><twPathDel><twSite>DLL1.CLK0</twSite><twDelType>Tdllino</twDelType><twDelInfo twEdge="twRising">-1.579</twDelInfo><twComp>UDLL1</twComp><twBEL>UDLL1</twBEL></twPathDel><twPathDel><twSite>GCLKBUF1.IN</twSite><twDelType>net</twDelType><twFanCnt>1</twFanCnt><twDelInfo twEdge="twRising">0.000</twDelInfo><twComp>CLK0</twComp></twPathDel><twPathDel><twSite>GCLKBUF1.OUT</twSite><twDelType>Tgio</twDelType><twDelInfo twEdge="twRising">0.446</twDelInfo><twComp>UBUF2</twComp><twBEL>UBUF2</twBEL></twPathDel><twPathDel><twSite>CLB_R9C16.S1.CLK</twSite><twDelType>net</twDelType><twFanCnt>561</twFanCnt><twDelInfo twEdge="twRising">0.325</twDelInfo><twComp>tp_1_OBUF</twComp></twPathDel><twLogDel>-0.433</twLogDel><twRouteDel>0.325</twRouteDel><twTotDel>-0.108</twTotDel></twClkPath><twDataPath maxSiteLen="15"><twSrc BELType="FF">U4_ceros_id_0</twSrc><twDest BELType="PAD">dout&lt;9&gt;</twDest><twLogLvls>4</twLogLvls><twSrcSite>CLB_R9C16.S1.CLK</twSrcSite><twSrcClk twEdge ="twRising" twArriveTime ="0.000">tp_1_OBUF</twSrcClk><twPathDel><twSite>CLB_R9C16.S1.YQ</twSite><twDelType>Tcko</twDelType><twDelInfo twEdge="twRising">0.886</twDelInfo><twComp>U4_ceros_id&lt;1&gt;</twComp><twBEL>U4_ceros_id_0</twBEL></twPathDel><twPathDel><twSite>CLB_R8C17.S0.F4</twSite><twDelType>net</twDelType><twFanCnt>14</twFanCnt><twDelInfo twEdge="twRising">0.559</twDelInfo><twComp>U4_ceros_id&lt;0&gt;</twComp></twPathDel><twPathDel><twSite>CLB_R8C17.S0.X</twSite><twDelType>Tilo</twDelType><twDelInfo twEdge="twRising">0.418</twDelInfo><twComp>token_p_0_OBUF</twComp><twBEL>U4__n00071</twBEL></twPathDel><twPathDel><twSite>CLB_R9C17.S0.F4</twSite><twDelType>net</twDelType><twFanCnt>2</twFanCnt><twDelInfo twEdge="twRising">0.674</twDelInfo><twComp>token_p_0_OBUF</twComp></twPathDel><twPathDel><twSite>CLB_R9C17.S0.X</twSite><twDelType>Tilo</twDelType><twDelInfo twEdge="twRising">0.418</twDelInfo><twComp>N52353</twComp><twBEL>_n0030_SW0</twBEL></twPathDel><twPathDel><twSite>CLB_R9C17.S0.G4</twSite><twDelType>net</twDelType><twFanCnt>1</twFanCnt><twDelInfo twEdge="twRising">0.266</twDelInfo><twComp>N52353</twComp></twPathDel><twPathDel><twSite>CLB_R9C17.S0.Y</twSite><twDelType>Tilo</twDelType><twDelInfo twEdge="twRising">0.418</twDelInfo><twComp>N52353</twComp><twBEL>_n0030</twBEL></twPathDel><twPathDel><twSite>J2.T</twSite><twDelType>net</twDelType><twFanCnt>17</twFanCnt><twDelInfo twEdge="twRising">2.939</twDelInfo><twComp>_n0030</twComp></twPathDel><twPathDel><twSite>J2.PAD</twSite><twDelType>Tioton</twDelType><twDelInfo twEdge="twRising">4.631</twDelInfo><twComp>dout&lt;9&gt;</twComp><twBEL>dout_9_OBUFT</twBEL><twBEL>dout&lt;9&gt;</twBEL></twPathDel><twLogDel>6.771</twLogDel><twRouteDel>4.438</twRouteDel><twTotDel>11.209</twTotDel><twPctLog>60.4</twPctLog><twPctRoute>39.6</twPctRoute></twDataPath></twConstOffOut></twPathRpt></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>COMP &quot;dout&lt;8&gt;&quot; OFFSET = OUT 11 nS  AFTER COMP &quot;clkin_p&quot; ;</twConstName><twItemCnt>23</twItemCnt><twErrCntSetup>0</twErrCntSetup><twErrCntHold twRaceChecked="FALSE">0</twErrCntHold><twMinOff>10.915</twMinOff></twConstHead></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>COMP &quot;dout&lt;7&gt;&quot; OFFSET = OUT 11 nS  AFTER COMP &quot;clkin_p&quot; ;</twConstName><twItemCnt>23</twItemCnt><twErrCntSetup>0</twErrCntSetup><twErrCntHold twRaceChecked="FALSE">0</twErrCntHold><twMinOff>10.693</twMinOff></twConstHead></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>COMP &quot;dout&lt;6&gt;&quot; OFFSET = OUT 11 nS  AFTER COMP &quot;clkin_p&quot; ;</twConstName><twItemCnt>23</twItemCnt><twErrCntSetup>1</twErrCntSetup><twErrCntHold twRaceChecked="FALSE">0</twErrCntHold><twMinOff>11.173</twMinOff></twConstHead><twPathRpt><twConstOffOut twDataPathType = "twDataPathMaxDelay"><twSlack>-0.173</twSlack><twSrc BELType="FF">U4_token</twSrc><twDest BELType="PAD">dout&lt;6&gt;</twDest><twClkDel>-0.108</twClkDel><twClkSrc>clkin_p</twClkSrc><twClkDest>U4_token</twClkDest><twDataDel>11.281</twDataDel><twDataSrc>U4_token</twDataSrc><twDataDest>dout&lt;6&gt;</twDataDest><twOff>11.000</twOff><twOffSrc>clkin_p</twOffSrc><twOffDest>dout&lt;6&gt;</twOffDest><twClkUncert>0.000</twClkUncert><twClkPath maxSiteLen="16"><twSrc BELType="PAD">clkin_p</twSrc><twDest BELType="FF">U4_token</twDest><twLogLvls>3</twLogLvls><twSrcSite>T8.PAD</twSrcSite><twPathDel><twSite>T8.GCLKOUT</twSite><twDelType>Tgpio</twDelType><twDelInfo twEdge="twRising">0.700</twDelInfo><twComp>clkin_p</twComp><twBEL>clkin_p</twBEL><twBEL>UBUF1</twBEL></twPathDel><twPathDel><twSite>DLL1.CLKIN</twSite><twDelType>net</twDelType><twFanCnt>1</twFanCnt><twDelInfo twEdge="twRising">0.000</twDelInfo><twComp>CLKIN</twComp></twPathDel><twPathDel><twSite>DLL1.CLK0</twSite><twDelType>Tdllino</twDelType><twDelInfo twEdge="twRising">-1.579</twDelInfo><twComp>UDLL1</twComp><twBEL>UDLL1</twBEL></twPathDel><twPathDel><twSite>GCLKBUF1.IN</twSite><twDelType>net</twDelType><twFanCnt>1</twFanCnt><twDelInfo twEdge="twRising">0.000</twDelInfo><twComp>CLK0</twComp></twPathDel><twPathDel><twSite>GCLKBUF1.OUT</twSite><twDelType>Tgio</twDelType><twDelInfo twEdge="twRising">0.446</twDelInfo><twComp>UBUF2</twComp><twBEL>UBUF2</twBEL></twPathDel><twPathDel><twSite>CLB_R9C16.S0.CLK</twSite><twDelType>net</twDelType><twFanCnt>561</twFanCnt><twDelInfo twEdge="twRising">0.325</twDelInfo><twComp>tp_1_OBUF</twComp></twPathDel><twLogDel>-0.433</twLogDel><twRouteDel>0.325</twRouteDel><twTotDel>-0.108</twTotDel></twClkPath><twDataPath maxSiteLen="16"><twSrc BELType="FF">U4_token</twSrc><twDest BELType="PAD">dout&lt;6&gt;</twDest><twLogLvls>3</twLogLvls><twSrcSite>CLB_R9C16.S0.CLK</twSrcSite><twSrcClk twEdge ="twRising" twArriveTime ="0.000">tp_1_OBUF</twSrcClk><twPathDel><twSite>CLB_R9C16.S0.YQ</twSite><twDelType>Tcko</twDelType><twDelInfo twEdge="twRising">0.886</twDelInfo><twComp>U4_token</twComp><twBEL>U4_token</twBEL></twPathDel><twPathDel><twSite>CLB_R10C15.S1.G2</twSite><twDelType>net</twDelType><twFanCnt>10</twFanCnt><twDelInfo twEdge="twRising">0.763</twDelInfo><twComp>U4_token</twComp></twPathDel><twPathDel><twSite>CLB_R10C15.S1.Y</twSite><twDelType>Tilo</twDelType><twDelInfo twEdge="twRising">0.418</twDelInfo><twComp>U3_hastoken</twComp><twBEL>U4__n00031</twBEL></twPathDel><twPathDel><twSite>CLB_R9C17.S0.G3</twSite><twDelType>net</twDelType><twFanCnt>18</twFanCnt><twDelInfo twEdge="twRising">1.196</twDelInfo><twComp>token&lt;4&gt;</twComp></twPathDel><twPathDel><twSite>CLB_R9C17.S0.Y</twSite><twDelType>Tilo</twDelType><twDelInfo twEdge="twRising">0.418</twDelInfo><twComp>N52353</twComp><twBEL>_n0030</twBEL></twPathDel><twPathDel><twSite>K1.T</twSite><twDelType>net</twDelType><twFanCnt>17</twFanCnt><twDelInfo twEdge="twRising">2.969</twDelInfo><twComp>_n0030</twComp></twPathDel><twPathDel><twSite>K1.PAD</twSite><twDelType>Tioton</twDelType><twDelInfo twEdge="twRising">4.631</twDelInfo><twComp>dout&lt;6&gt;</twComp><twBEL>dout_6_OBUFT</twBEL><twBEL>dout&lt;6&gt;</twBEL></twPathDel><twLogDel>6.353</twLogDel><twRouteDel>4.928</twRouteDel><twTotDel>11.281</twTotDel><twPctLog>56.3</twPctLog><twPctRoute>43.7</twPctRoute></twDataPath></twConstOffOut></twPathRpt><twPathRpt><twConstOffOut twDataPathType = "twDataPathMaxDelay"><twSlack>-0.162</twSlack><twSrc BELType="FF">U4_token</twSrc><twDest BELType="PAD">dout&lt;6&gt;</twDest><twClkDel>-0.108</twClkDel><twClkSrc>clkin_p</twClkSrc><twClkDest>U4_token</twClkDest><twDataDel>11.270</twDataDel><twDataSrc>U4_token</twDataSrc><twDataDest>dout&lt;6&gt;</twDataDest><twOff>11.000</twOff><twOffSrc>clkin_p</twOffSrc><twOffDest>dout&lt;6&gt;</twOffDest><twClkUncert>0.000</twClkUncert><twClkPath maxSiteLen="16"><twSrc BELType="PAD">clkin_p</twSrc><twDest BELType="FF">U4_token</twDest><twLogLvls>3</twLogLvls><twSrcSite>T8.PAD</twSrcSite><twPathDel><twSite>T8.GCLKOUT</twSite><twDelType>Tgpio</twDelType><twDelInfo twEdge="twRising">0.700</twDelInfo><twComp>clkin_p</twComp><twBEL>clkin_p</twBEL><twBEL>UBUF1</twBEL></twPathDel><twPathDel><twSite>DLL1.CLKIN</twSite><twDelType>net</twDelType><twFanCnt>1</twFanCnt><twDelInfo twEdge="twRising">0.000</twDelInfo><twComp>CLKIN</twComp></twPathDel><twPathDel><twSite>DLL1.CLK0</twSite><twDelType>Tdllino</twDelType><twDelInfo twEdge="twRising">-1.579</twDelInfo><twComp>UDLL1</twComp><twBEL>UDLL1</twBEL></twPathDel><twPathDel><twSite>GCLKBUF1.IN</twSite><twDelType>net</twDelType><twFanCnt>1</twFanCnt><twDelInfo twEdge="twRising">0.000</twDelInfo><twComp>CLK0</twComp></twPathDel><twPathDel><twSite>GCLKBUF1.OUT</twSite><twDelType>Tgio</twDelType><twDelInfo twEdge="twRising">0.446</twDelInfo><twComp>UBUF2</twComp><twBEL>UBUF2</twBEL></twPathDel><twPathDel><twSite>CLB_R9C16.S0.CLK</twSite><twDelType>net</twDelType><twFanCnt>561</twFanCnt><twDelInfo twEdge="twRising">0.325</twDelInfo><twComp>tp_1_OBUF</twComp></twPathDel><twLogDel>-0.433</twLogDel><twRouteDel>0.325</twRouteDel><twTotDel>-0.108</twTotDel></twClkPath><twDataPath maxSiteLen="15"><twSrc BELType="FF">U4_token</twSrc><twDest BELType="PAD">dout&lt;6&gt;</twDest><twLogLvls>4</twLogLvls><twSrcSite>CLB_R9C16.S0.CLK</twSrcSite><twSrcClk twEdge ="twRising" twArriveTime ="0.000">tp_1_OBUF</twSrcClk><twPathDel><twSite>CLB_R9C16.S0.YQ</twSite><twDelType>Tcko</twDelType><twDelInfo twEdge="twRising">0.886</twDelInfo><twComp>U4_token</twComp><twBEL>U4_token</twBEL></twPathDel><twPathDel><twSite>CLB_R8C17.S0.F3</twSite><twDelType>net</twDelType><twFanCnt>10</twFanCnt><twDelInfo twEdge="twRising">0.590</twDelInfo><twComp>U4_token</twComp></twPathDel><twPathDel><twSite>CLB_R8C17.S0.X</twSite><twDelType>Tilo</twDelType><twDelInfo twEdge="twRising">0.418</twDelInfo><twComp>token_p_0_OBUF</twComp><twBEL>U4__n00071</twBEL></twPathDel><twPathDel><twSite>CLB_R9C17.S0.F4</twSite><twDelType>net</twDelType><twFanCnt>2</twFanCnt><twDelInfo twEdge="twRising">0.674</twDelInfo><twComp>token_p_0_OBUF</twComp></twPathDel><twPathDel><twSite>CLB_R9C17.S0.X</twSite><twDelType>Tilo</twDelType><twDelInfo twEdge="twRising">0.418</twDelInfo><twComp>N52353</twComp><twBEL>_n0030_SW0</twBEL></twPathDel><twPathDel><twSite>CLB_R9C17.S0.G4</twSite><twDelType>net</twDelType><twFanCnt>1</twFanCnt><twDelInfo twEdge="twRising">0.266</twDelInfo><twComp>N52353</twComp></twPathDel><twPathDel><twSite>CLB_R9C17.S0.Y</twSite><twDelType>Tilo</twDelType><twDelInfo twEdge="twRising">0.418</twDelInfo><twComp>N52353</twComp><twBEL>_n0030</twBEL></twPathDel><twPathDel><twSite>K1.T</twSite><twDelType>net</twDelType><twFanCnt>17</twFanCnt><twDelInfo twEdge="twRising">2.969</twDelInfo><twComp>_n0030</twComp></twPathDel><twPathDel><twSite>K1.PAD</twSite><twDelType>Tioton</twDelType><twDelInfo twEdge="twRising">4.631</twDelInfo><twComp>dout&lt;6&gt;</twComp><twBEL>dout_6_OBUFT</twBEL><twBEL>dout&lt;6&gt;</twBEL></twPathDel><twLogDel>6.771</twLogDel><twRouteDel>4.499</twRouteDel><twTotDel>11.270</twTotDel><twPctLog>60.1</twPctLog><twPctRoute>39.9</twPctRoute></twDataPath></twConstOffOut></twPathRpt><twPathRpt><twConstOffOut twDataPathType = "twDataPathMaxDelay"><twSlack>-0.131</twSlack><twSrc BELType="FF">U4_ceros_id_0</twSrc><twDest BELType="PAD">dout&lt;6&gt;</twDest><twClkDel>-0.108</twClkDel><twClkSrc>clkin_p</twClkSrc><twClkDest>U4_ceros_id&lt;1&gt;</twClkDest><twDataDel>11.239</twDataDel><twDataSrc>U4_ceros_id&lt;1&gt;</twDataSrc><twDataDest>dout&lt;6&gt;</twDataDest><twOff>11.000</twOff><twOffSrc>clkin_p</twOffSrc><twOffDest>dout&lt;6&gt;</twOffDest><twClkUncert>0.000</twClkUncert><twClkPath maxSiteLen="16"><twSrc BELType="PAD">clkin_p</twSrc><twDest BELType="FF">U4_ceros_id_0</twDest><twLogLvls>3</twLogLvls><twSrcSite>T8.PAD</twSrcSite><twPathDel><twSite>T8.GCLKOUT</twSite><twDelType>Tgpio</twDelType><twDelInfo twEdge="twRising">0.700</twDelInfo><twComp>clkin_p</twComp><twBEL>clkin_p</twBEL><twBEL>UBUF1</twBEL></twPathDel><twPathDel><twSite>DLL1.CLKIN</twSite><twDelType>net</twDelType><twFanCnt>1</twFanCnt><twDelInfo twEdge="twRising">0.000</twDelInfo><twComp>CLKIN</twComp></twPathDel><twPathDel><twSite>DLL1.CLK0</twSite><twDelType>Tdllino</twDelType><twDelInfo twEdge="twRising">-1.579</twDelInfo><twComp>UDLL1</twComp><twBEL>UDLL1</twBEL></twPathDel><twPathDel><twSite>GCLKBUF1.IN</twSite><twDelType>net</twDelType><twFanCnt>1</twFanCnt><twDelInfo twEdge="twRising">0.000</twDelInfo><twComp>CLK0</twComp></twPathDel><twPathDel><twSite>GCLKBUF1.OUT</twSite><twDelType>Tgio</twDelType><twDelInfo twEdge="twRising">0.446</twDelInfo><twComp>UBUF2</twComp><twBEL>UBUF2</twBEL></twPathDel><twPathDel><twSite>CLB_R9C16.S1.CLK</twSite><twDelType>net</twDelType><twFanCnt>561</twFanCnt><twDelInfo twEdge="twRising">0.325</twDelInfo><twComp>tp_1_OBUF</twComp></twPathDel><twLogDel>-0.433</twLogDel><twRouteDel>0.325</twRouteDel><twTotDel>-0.108</twTotDel></twClkPath><twDataPath maxSiteLen="15"><twSrc BELType="FF">U4_ceros_id_0</twSrc><twDest BELType="PAD">dout&lt;6&gt;</twDest><twLogLvls>4</twLogLvls><twSrcSite>CLB_R9C16.S1.CLK</twSrcSite><twSrcClk twEdge ="twRising" twArriveTime ="0.000">tp_1_OBUF</twSrcClk><twPathDel><twSite>CLB_R9C16.S1.YQ</twSite><twDelType>Tcko</twDelType><twDelInfo twEdge="twRising">0.886</twDelInfo><twComp>U4_ceros_id&lt;1&gt;</twComp><twBEL>U4_ceros_id_0</twBEL></twPathDel><twPathDel><twSite>CLB_R8C17.S0.F4</twSite><twDelType>net</twDelType><twFanCnt>14</twFanCnt><twDelInfo twEdge="twRising">0.559</twDelInfo><twComp>U4_ceros_id&lt;0&gt;</twComp></twPathDel><twPathDel><twSite>CLB_R8C17.S0.X</twSite><twDelType>Tilo</twDelType><twDelInfo twEdge="twRising">0.418</twDelInfo><twComp>token_p_0_OBUF</twComp><twBEL>U4__n00071</twBEL></twPathDel><twPathDel><twSite>CLB_R9C17.S0.F4</twSite><twDelType>net</twDelType><twFanCnt>2</twFanCnt><twDelInfo twEdge="twRising">0.674</twDelInfo><twComp>token_p_0_OBUF</twComp></twPathDel><twPathDel><twSite>CLB_R9C17.S0.X</twSite><twDelType>Tilo</twDelType><twDelInfo twEdge="twRising">0.418</twDelInfo><twComp>N52353</twComp><twBEL>_n0030_SW0</twBEL></twPathDel><twPathDel><twSite>CLB_R9C17.S0.G4</twSite><twDelType>net</twDelType><twFanCnt>1</twFanCnt><twDelInfo twEdge="twRising">0.266</twDelInfo><twComp>N52353</twComp></twPathDel><twPathDel><twSite>CLB_R9C17.S0.Y</twSite><twDelType>Tilo</twDelType><twDelInfo twEdge="twRising">0.418</twDelInfo><twComp>N52353</twComp><twBEL>_n0030</twBEL></twPathDel><twPathDel><twSite>K1.T</twSite><twDelType>net</twDelType><twFanCnt>17</twFanCnt><twDelInfo twEdge="twRising">2.969</twDelInfo><twComp>_n0030</twComp></twPathDel><twPathDel><twSite>K1.PAD</twSite><twDelType>Tioton</twDelType><twDelInfo twEdge="twRising">4.631</twDelInfo><twComp>dout&lt;6&gt;</twComp><twBEL>dout_6_OBUFT</twBEL><twBEL>dout&lt;6&gt;</twBEL></twPathDel><twLogDel>6.771</twLogDel><twRouteDel>4.468</twRouteDel><twTotDel>11.239</twTotDel><twPctLog>60.2</twPctLog><twPctRoute>39.8</twPctRoute></twDataPath></twConstOffOut></twPathRpt></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>COMP &quot;dout&lt;5&gt;&quot; OFFSET = OUT 11 nS  AFTER COMP &quot;clkin_p&quot; ;</twConstName><twItemCnt>23</twItemCnt><twErrCntSetup>0</twErrCntSetup><twErrCntHold twRaceChecked="FALSE">0</twErrCntHold><twMinOff>10.861</twMinOff></twConstHead></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>COMP &quot;dout&lt;4&gt;&quot; OFFSET = OUT 11 nS  AFTER COMP &quot;clkin_p&quot; ;</twConstName><twItemCnt>23</twItemCnt><twErrCntSetup>0</twErrCntSetup><twErrCntHold twRaceChecked="FALSE">0</twErrCntHold><twMinOff>10.815</twMinOff></twConstHead></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>COMP &quot;dout&lt;3&gt;&quot; OFFSET = OUT 11 nS  AFTER COMP &quot;clkin_p&quot; ;</twConstName><twItemCnt>23</twItemCnt><twErrCntSetup>0</twErrCntSetup><twErrCntHold twRaceChecked="FALSE">0</twErrCntHold><twMinOff>10.590</twMinOff></twConstHead></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>COMP &quot;dout&lt;2&gt;&quot; OFFSET = OUT 11 nS  AFTER COMP &quot;clkin_p&quot; ;</twConstName><twItemCnt>23</twItemCnt><twErrCntSetup>0</twErrCntSetup><twErrCntHold twRaceChecked="FALSE">0</twErrCntHold><twMinOff>10.744</twMinOff></twConstHead></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>COMP &quot;dout&lt;1&gt;&quot; OFFSET = OUT 11 nS  AFTER COMP &quot;clkin_p&quot; ;</twConstName><twItemCnt>23</twItemCnt><twErrCntSetup>1</twErrCntSetup><twErrCntHold twRaceChecked="FALSE">0</twErrCntHold><twMinOff>11.192</twMinOff></twConstHead><twPathRpt><twConstOffOut twDataPathType = "twDataPathMaxDelay"><twSlack>-0.192</twSlack><twSrc BELType="FF">U4_token</twSrc><twDest BELType="PAD">dout&lt;1&gt;</twDest><twClkDel>-0.108</twClkDel><twClkSrc>clkin_p</twClkSrc><twClkDest>U4_token</twClkDest><twDataDel>11.300</twDataDel><twDataSrc>U4_token</twDataSrc><twDataDest>dout&lt;1&gt;</twDataDest><twOff>11.000</twOff><twOffSrc>clkin_p</twOffSrc><twOffDest>dout&lt;1&gt;</twOffDest><twClkUncert>0.000</twClkUncert><twClkPath maxSiteLen="16"><twSrc BELType="PAD">clkin_p</twSrc><twDest BELType="FF">U4_token</twDest><twLogLvls>3</twLogLvls><twSrcSite>T8.PAD</twSrcSite><twPathDel><twSite>T8.GCLKOUT</twSite><twDelType>Tgpio</twDelType><twDelInfo twEdge="twRising">0.700</twDelInfo><twComp>clkin_p</twComp><twBEL>clkin_p</twBEL><twBEL>UBUF1</twBEL></twPathDel><twPathDel><twSite>DLL1.CLKIN</twSite><twDelType>net</twDelType><twFanCnt>1</twFanCnt><twDelInfo twEdge="twRising">0.000</twDelInfo><twComp>CLKIN</twComp></twPathDel><twPathDel><twSite>DLL1.CLK0</twSite><twDelType>Tdllino</twDelType><twDelInfo twEdge="twRising">-1.579</twDelInfo><twComp>UDLL1</twComp><twBEL>UDLL1</twBEL></twPathDel><twPathDel><twSite>GCLKBUF1.IN</twSite><twDelType>net</twDelType><twFanCnt>1</twFanCnt><twDelInfo twEdge="twRising">0.000</twDelInfo><twComp>CLK0</twComp></twPathDel><twPathDel><twSite>GCLKBUF1.OUT</twSite><twDelType>Tgio</twDelType><twDelInfo twEdge="twRising">0.446</twDelInfo><twComp>UBUF2</twComp><twBEL>UBUF2</twBEL></twPathDel><twPathDel><twSite>CLB_R9C16.S0.CLK</twSite><twDelType>net</twDelType><twFanCnt>561</twFanCnt><twDelInfo twEdge="twRising">0.325</twDelInfo><twComp>tp_1_OBUF</twComp></twPathDel><twLogDel>-0.433</twLogDel><twRouteDel>0.325</twRouteDel><twTotDel>-0.108</twTotDel></twClkPath><twDataPath maxSiteLen="16"><twSrc BELType="FF">U4_token</twSrc><twDest BELType="PAD">dout&lt;1&gt;</twDest><twLogLvls>3</twLogLvls><twSrcSite>CLB_R9C16.S0.CLK</twSrcSite><twSrcClk twEdge ="twRising" twArriveTime ="0.000">tp_1_OBUF</twSrcClk><twPathDel><twSite>CLB_R9C16.S0.YQ</twSite><twDelType>Tcko</twDelType><twDelInfo twEdge="twRising">0.886</twDelInfo><twComp>U4_token</twComp><twBEL>U4_token</twBEL></twPathDel><twPathDel><twSite>CLB_R10C15.S1.G2</twSite><twDelType>net</twDelType><twFanCnt>10</twFanCnt><twDelInfo twEdge="twRising">0.763</twDelInfo><twComp>U4_token</twComp></twPathDel><twPathDel><twSite>CLB_R10C15.S1.Y</twSite><twDelType>Tilo</twDelType><twDelInfo twEdge="twRising">0.418</twDelInfo><twComp>U3_hastoken</twComp><twBEL>U4__n00031</twBEL></twPathDel><twPathDel><twSite>CLB_R9C17.S0.G3</twSite><twDelType>net</twDelType><twFanCnt>18</twFanCnt><twDelInfo twEdge="twRising">1.196</twDelInfo><twComp>token&lt;4&gt;</twComp></twPathDel><twPathDel><twSite>CLB_R9C17.S0.Y</twSite><twDelType>Tilo</twDelType><twDelInfo twEdge="twRising">0.418</twDelInfo><twComp>N52353</twComp><twBEL>_n0030</twBEL></twPathDel><twPathDel><twSite>J4.T</twSite><twDelType>net</twDelType><twFanCnt>17</twFanCnt><twDelInfo twEdge="twRising">2.988</twDelInfo><twComp>_n0030</twComp></twPathDel><twPathDel><twSite>J4.PAD</twSite><twDelType>Tioton</twDelType><twDelInfo twEdge="twRising">4.631</twDelInfo><twComp>dout&lt;1&gt;</twComp><twBEL>dout_1_OBUFT</twBEL><twBEL>dout&lt;1&gt;</twBEL></twPathDel><twLogDel>6.353</twLogDel><twRouteDel>4.947</twRouteDel><twTotDel>11.300</twTotDel><twPctLog>56.2</twPctLog><twPctRoute>43.8</twPctRoute></twDataPath></twConstOffOut></twPathRpt><twPathRpt><twConstOffOut twDataPathType = "twDataPathMaxDelay"><twSlack>-0.181</twSlack><twSrc BELType="FF">U4_token</twSrc><twDest BELType="PAD">dout&lt;1&gt;</twDest><twClkDel>-0.108</twClkDel><twClkSrc>clkin_p</twClkSrc><twClkDest>U4_token</twClkDest><twDataDel>11.289</twDataDel><twDataSrc>U4_token</twDataSrc><twDataDest>dout&lt;1&gt;</twDataDest><twOff>11.000</twOff><twOffSrc>clkin_p</twOffSrc><twOffDest>dout&lt;1&gt;</twOffDest><twClkUncert>0.000</twClkUncert><twClkPath maxSiteLen="16"><twSrc BELType="PAD">clkin_p</twSrc><twDest BELType="FF">U4_token</twDest><twLogLvls>3</twLogLvls><twSrcSite>T8.PAD</twSrcSite><twPathDel><twSite>T8.GCLKOUT</twSite><twDelType>Tgpio</twDelType><twDelInfo twEdge="twRising">0.700</twDelInfo><twComp>clkin_p</twComp><twBEL>clkin_p</twBEL><twBEL>UBUF1</twBEL></twPathDel><twPathDel><twSite>DLL1.CLKIN</twSite><twDelType>net</twDelType><twFanCnt>1</twFanCnt><twDelInfo twEdge="twRising">0.000</twDelInfo><twComp>CLKIN</twComp></twPathDel><twPathDel><twSite>DLL1.CLK0</twSite><twDelType>Tdllino</twDelType><twDelInfo twEdge="twRising">-1.579</twDelInfo><twComp>UDLL1</twComp><twBEL>UDLL1</twBEL></twPathDel><twPathDel><twSite>GCLKBUF1.IN</twSite><twDelType>net</twDelType><twFanCnt>1</twFanCnt><twDelInfo twEdge="twRising">0.000</twDelInfo><twComp>CLK0</twComp></twPathDel><twPathDel><twSite>GCLKBUF1.OUT</twSite><twDelType>Tgio</twDelType><twDelInfo twEdge="twRising">0.446</twDelInfo><twComp>UBUF2</twComp><twBEL>UBUF2</twBEL></twPathDel><twPathDel><twSite>CLB_R9C16.S0.CLK</twSite><twDelType>net</twDelType><twFanCnt>561</twFanCnt><twDelInfo twEdge="twRising">0.325</twDelInfo><twComp>tp_1_OBUF</twComp></twPathDel><twLogDel>-0.433</twLogDel><twRouteDel>0.325</twRouteDel><twTotDel>-0.108</twTotDel></twClkPath><twDataPath maxSiteLen="15"><twSrc BELType="FF">U4_token</twSrc><twDest BELType="PAD">dout&lt;1&gt;</twDest><twLogLvls>4</twLogLvls><twSrcSite>CLB_R9C16.S0.CLK</twSrcSite><twSrcClk twEdge ="twRising" twArriveTime ="0.000">tp_1_OBUF</twSrcClk><twPathDel><twSite>CLB_R9C16.S0.YQ</twSite><twDelType>Tcko</twDelType><twDelInfo twEdge="twRising">0.886</twDelInfo><twComp>U4_token</twComp><twBEL>U4_token</twBEL></twPathDel><twPathDel><twSite>CLB_R8C17.S0.F3</twSite><twDelType>net</twDelType><twFanCnt>10</twFanCnt><twDelInfo twEdge="twRising">0.590</twDelInfo><twComp>U4_token</twComp></twPathDel><twPathDel><twSite>CLB_R8C17.S0.X</twSite><twDelType>Tilo</twDelType><twDelInfo twEdge="twRising">0.418</twDelInfo><twComp>token_p_0_OBUF</twComp><twBEL>U4__n00071</twBEL></twPathDel><twPathDel><twSite>CLB_R9C17.S0.F4</twSite><twDelType>net</twDelType><twFanCnt>2</twFanCnt><twDelInfo twEdge="twRising">0.674</twDelInfo><twComp>token_p_0_OBUF</twComp></twPathDel><twPathDel><twSite>CLB_R9C17.S0.X</twSite><twDelType>Tilo</twDelType><twDelInfo twEdge="twRising">0.418</twDelInfo><twComp>N52353</twComp><twBEL>_n0030_SW0</twBEL></twPathDel><twPathDel><twSite>CLB_R9C17.S0.G4</twSite><twDelType>net</twDelType><twFanCnt>1</twFanCnt><twDelInfo twEdge="twRising">0.266</twDelInfo><twComp>N52353</twComp></twPathDel><twPathDel><twSite>CLB_R9C17.S0.Y</twSite><twDelType>Tilo</twDelType><twDelInfo twEdge="twRising">0.418</twDelInfo><twComp>N52353</twComp><twBEL>_n0030</twBEL></twPathDel><twPathDel><twSite>J4.T</twSite><twDelType>net</twDelType><twFanCnt>17</twFanCnt><twDelInfo twEdge="twRising">2.988</twDelInfo><twComp>_n0030</twComp></twPathDel><twPathDel><twSite>J4.PAD</twSite><twDelType>Tioton</twDelType><twDelInfo twEdge="twRising">4.631</twDelInfo><twComp>dout&lt;1&gt;</twComp><twBEL>dout_1_OBUFT</twBEL><twBEL>dout&lt;1&gt;</twBEL></twPathDel><twLogDel>6.771</twLogDel><twRouteDel>4.518</twRouteDel><twTotDel>11.289</twTotDel><twPctLog>60.0</twPctLog><twPctRoute>40.0</twPctRoute></twDataPath></twConstOffOut></twPathRpt><twPathRpt><twConstOffOut twDataPathType = "twDataPathMaxDelay"><twSlack>-0.150</twSlack><twSrc BELType="FF">U4_ceros_id_0</twSrc><twDest BELType="PAD">dout&lt;1&gt;</twDest><twClkDel>-0.108</twClkDel><twClkSrc>clkin_p</twClkSrc><twClkDest>U4_ceros_id&lt;1&gt;</twClkDest><twDataDel>11.258</twDataDel><twDataSrc>U4_ceros_id&lt;1&gt;</twDataSrc><twDataDest>dout&lt;1&gt;</twDataDest><twOff>11.000</twOff><twOffSrc>clkin_p</twOffSrc><twOffDest>dout&lt;1&gt;</twOffDest><twClkUncert>0.000</twClkUncert><twClkPath maxSiteLen="16"><twSrc BELType="PAD">clkin_p</twSrc><twDest BELType="FF">U4_ceros_id_0</twDest><twLogLvls>3</twLogLvls><twSrcSite>T8.PAD</twSrcSite><twPathDel><twSite>T8.GCLKOUT</twSite><twDelType>Tgpio</twDelType><twDelInfo twEdge="twRising">0.700</twDelInfo><twComp>clkin_p</twComp><twBEL>clkin_p</twBEL><twBEL>UBUF1</twBEL></twPathDel><twPathDel><twSite>DLL1.CLKIN</twSite><twDelType>net</twDelType><twFanCnt>1</twFanCnt><twDelInfo twEdge="twRising">0.000</twDelInfo><twComp>CLKIN</twComp></twPathDel><twPathDel><twSite>DLL1.CLK0</twSite><twDelType>Tdllino</twDelType><twDelInfo twEdge="twRising">-1.579</twDelInfo><twComp>UDLL1</twComp><twBEL>UDLL1</twBEL></twPathDel><twPathDel><twSite>GCLKBUF1.IN</twSite><twDelType>net</twDelType><twFanCnt>1</twFanCnt><twDelInfo twEdge="twRising">0.000</twDelInfo><twComp>CLK0</twComp></twPathDel><twPathDel><twSite>GCLKBUF1.OUT</twSite><twDelType>Tgio</twDelType><twDelInfo twEdge="twRising">0.446</twDelInfo><twComp>UBUF2</twComp><twBEL>UBUF2</twBEL></twPathDel><twPathDel><twSite>CLB_R9C16.S1.CLK</twSite><twDelType>net</twDelType><twFanCnt>561</twFanCnt><twDelInfo twEdge="twRising">0.325</twDelInfo><twComp>tp_1_OBUF</twComp></twPathDel><twLogDel>-0.433</twLogDel><twRouteDel>0.325</twRouteDel><twTotDel>-0.108</twTotDel></twClkPath><twDataPath maxSiteLen="15"><twSrc BELType="FF">U4_ceros_id_0</twSrc><twDest BELType="PAD">dout&lt;1&gt;</twDest><twLogLvls>4</twLogLvls><twSrcSite>CLB_R9C16.S1.CLK</twSrcSite><twSrcClk twEdge ="twRising" twArriveTime ="0.000">tp_1_OBUF</twSrcClk><twPathDel><twSite>CLB_R9C16.S1.YQ</twSite><twDelType>Tcko</twDelType><twDelInfo twEdge="twRising">0.886</twDelInfo><twComp>U4_ceros_id&lt;1&gt;</twComp><twBEL>U4_ceros_id_0</twBEL></twPathDel><twPathDel><twSite>CLB_R8C17.S0.F4</twSite><twDelType>net</twDelType><twFanCnt>14</twFanCnt><twDelInfo twEdge="twRising">0.559</twDelInfo><twComp>U4_ceros_id&lt;0&gt;</twComp></twPathDel><twPathDel><twSite>CLB_R8C17.S0.X</twSite><twDelType>Tilo</twDelType><twDelInfo twEdge="twRising">0.418</twDelInfo><twComp>token_p_0_OBUF</twComp><twBEL>U4__n00071</twBEL></twPathDel><twPathDel><twSite>CLB_R9C17.S0.F4</twSite><twDelType>net</twDelType><twFanCnt>2</twFanCnt><twDelInfo twEdge="twRising">0.674</twDelInfo><twComp>token_p_0_OBUF</twComp></twPathDel><twPathDel><twSite>CLB_R9C17.S0.X</twSite><twDelType>Tilo</twDelType><twDelInfo twEdge="twRising">0.418</twDelInfo><twComp>N52353</twComp><twBEL>_n0030_SW0</twBEL></twPathDel><twPathDel><twSite>CLB_R9C17.S0.G4</twSite><twDelType>net</twDelType><twFanCnt>1</twFanCnt><twDelInfo twEdge="twRising">0.266</twDelInfo><twComp>N52353</twComp></twPathDel><twPathDel><twSite>CLB_R9C17.S0.Y</twSite><twDelType>Tilo</twDelType><twDelInfo twEdge="twRising">0.418</twDelInfo><twComp>N52353</twComp><twBEL>_n0030</twBEL></twPathDel><twPathDel><twSite>J4.T</twSite><twDelType>net</twDelType><twFanCnt>17</twFanCnt><twDelInfo twEdge="twRising">2.988</twDelInfo><twComp>_n0030</twComp></twPathDel><twPathDel><twSite>J4.PAD</twSite><twDelType>Tioton</twDelType><twDelInfo twEdge="twRising">4.631</twDelInfo><twComp>dout&lt;1&gt;</twComp><twBEL>dout_1_OBUFT</twBEL><twBEL>dout&lt;1&gt;</twBEL></twPathDel><twLogDel>6.771</twLogDel><twRouteDel>4.487</twRouteDel><twTotDel>11.258</twTotDel><twPctLog>60.1</twPctLog><twPctRoute>39.9</twPctRoute></twDataPath></twConstOffOut></twPathRpt></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>COMP &quot;dout&lt;0&gt;&quot; OFFSET = OUT 11 nS  AFTER COMP &quot;clkin_p&quot; ;</twConstName><twItemCnt>23</twItemCnt><twErrCntSetup>0</twErrCntSetup><twErrCntHold twRaceChecked="FALSE">0</twErrCntHold><twMinOff>10.535</twMinOff></twConstHead></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>COMP &quot;bcnt_res_p&quot; OFFSET = IN 1000 pS  BEFORE COMP &quot;clkin_p&quot; ;</twConstName><twItemCnt>2</twItemCnt><twErrCntSetup>0</twErrCntSetup><twErrCntHold twRaceChecked="TRUE">0</twErrCntHold><twMinOff>-5.668</twMinOff></twConstHead></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>COMP &quot;evcnt_high_strobe_p&quot; OFFSET = IN 3 nS  AFTER COMP &quot;clkin_p&quot; ;</twConstName><twItemCnt>1</twItemCnt><twErrCntSetup>0</twErrCntSetup><twErrCntHold twRaceChecked="TRUE">0</twErrCntHold><twMaxOff>18.400</twMaxOff></twConstHead></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>COMP &quot;evcnt_low_strobe_p&quot; OFFSET = IN 3 nS  AFTER COMP &quot;clkin_p&quot; ;</twConstName><twItemCnt>1</twItemCnt><twErrCntSetup>0</twErrCntSetup><twErrCntHold twRaceChecked="TRUE">0</twErrCntHold><twMaxOff>18.400</twMaxOff></twConstHead></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>COMP &quot;txena_in&quot; OFFSET = IN 11 nS  BEFORE COMP &quot;clkin_p&quot; ;</twConstName><twItemCnt>18</twItemCnt><twErrCntSetup>0</twErrCntSetup><twErrCntHold twRaceChecked="TRUE">0</twErrCntHold><twMinOff>4.726</twMinOff></twConstHead></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>COMP &quot;bcnt_p&lt;11&gt;&quot; OFFSET = IN 10 nS  AFTER COMP &quot;clkin_p&quot; ;</twConstName><twItemCnt>1</twItemCnt><twErrCntSetup>0</twErrCntSetup><twErrCntHold twRaceChecked="TRUE">0</twErrCntHold><twMaxOff>18.400</twMaxOff></twConstHead></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>COMP &quot;bcnt_p&lt;10&gt;&quot; OFFSET = IN 10 nS  AFTER COMP &quot;clkin_p&quot; ;</twConstName><twItemCnt>1</twItemCnt><twErrCntSetup>0</twErrCntSetup><twErrCntHold twRaceChecked="TRUE">0</twErrCntHold><twMaxOff>18.400</twMaxOff></twConstHead></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>COMP &quot;bcnt_p&lt;9&gt;&quot; OFFSET = IN 10 nS  AFTER COMP &quot;clkin_p&quot; ;</twConstName><twItemCnt>1</twItemCnt><twErrCntSetup>0</twErrCntSetup><twErrCntHold twRaceChecked="TRUE">0</twErrCntHold><twMaxOff>18.400</twMaxOff></twConstHead></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>COMP &quot;bcnt_p&lt;8&gt;&quot; OFFSET = IN 10 nS  AFTER COMP &quot;clkin_p&quot; ;</twConstName><twItemCnt>1</twItemCnt><twErrCntSetup>0</twErrCntSetup><twErrCntHold twRaceChecked="TRUE">0</twErrCntHold><twMaxOff>18.400</twMaxOff></twConstHead></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>COMP &quot;bcnt_p&lt;7&gt;&quot; OFFSET = IN 10 nS  AFTER COMP &quot;clkin_p&quot; ;</twConstName><twItemCnt>1</twItemCnt><twErrCntSetup>0</twErrCntSetup><twErrCntHold twRaceChecked="TRUE">0</twErrCntHold><twMaxOff>18.400</twMaxOff></twConstHead></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>COMP &quot;bcnt_p&lt;6&gt;&quot; OFFSET = IN 10 nS  AFTER COMP &quot;clkin_p&quot; ;</twConstName><twItemCnt>1</twItemCnt><twErrCntSetup>0</twErrCntSetup><twErrCntHold twRaceChecked="TRUE">0</twErrCntHold><twMaxOff>18.400</twMaxOff></twConstHead></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>COMP &quot;bcnt_p&lt;5&gt;&quot; OFFSET = IN 10 nS  AFTER COMP &quot;clkin_p&quot; ;</twConstName><twItemCnt>1</twItemCnt><twErrCntSetup>0</twErrCntSetup><twErrCntHold twRaceChecked="TRUE">0</twErrCntHold><twMaxOff>18.400</twMaxOff></twConstHead></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>COMP &quot;bcnt_p&lt;4&gt;&quot; OFFSET = IN 10 nS  AFTER COMP &quot;clkin_p&quot; ;</twConstName><twItemCnt>1</twItemCnt><twErrCntSetup>0</twErrCntSetup><twErrCntHold twRaceChecked="TRUE">0</twErrCntHold><twMaxOff>18.400</twMaxOff></twConstHead></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>COMP &quot;bcnt_p&lt;3&gt;&quot; OFFSET = IN 10 nS  AFTER COMP &quot;clkin_p&quot; ;</twConstName><twItemCnt>1</twItemCnt><twErrCntSetup>0</twErrCntSetup><twErrCntHold twRaceChecked="TRUE">0</twErrCntHold><twMaxOff>18.400</twMaxOff></twConstHead></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>COMP &quot;bcnt_p&lt;2&gt;&quot; OFFSET = IN 10 nS  AFTER COMP &quot;clkin_p&quot; ;</twConstName><twItemCnt>1</twItemCnt><twErrCntSetup>0</twErrCntSetup><twErrCntHold twRaceChecked="TRUE">0</twErrCntHold><twMaxOff>18.400</twMaxOff></twConstHead></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>COMP &quot;bcnt_p&lt;1&gt;&quot; OFFSET = IN 10 nS  AFTER COMP &quot;clkin_p&quot; ;</twConstName><twItemCnt>1</twItemCnt><twErrCntSetup>0</twErrCntSetup><twErrCntHold twRaceChecked="TRUE">0</twErrCntHold><twMaxOff>18.400</twMaxOff></twConstHead></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>COMP &quot;bcnt_p&lt;0&gt;&quot; OFFSET = IN 10 nS  AFTER COMP &quot;clkin_p&quot; ;</twConstName><twItemCnt>1</twItemCnt><twErrCntSetup>0</twErrCntSetup><twErrCntHold twRaceChecked="TRUE">0</twErrCntHold><twMaxOff>18.400</twMaxOff></twConstHead></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>COMP &quot;fsen&quot; OFFSET = OUT 11 nS  AFTER COMP &quot;clkin_p&quot; ;</twConstName><twItemCnt>1</twItemCnt><twErrCntSetup>0</twErrCntSetup><twErrCntHold twRaceChecked="FALSE">0</twErrCntHold><twMinOff>6.566</twMinOff></twConstHead></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>COMP &quot;ros_ready&quot; OFFSET = OUT 11 nS  AFTER COMP &quot;clkin_p&quot; ;</twConstName><twItemCnt>1</twItemCnt><twErrCntSetup>0</twErrCntSetup><twErrCntHold twRaceChecked="FALSE">0</twErrCntHold><twMinOff>7.859</twMinOff></twConstHead></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>COMP &quot;fsi&quot; OFFSET = OUT 11 nS  AFTER COMP &quot;clkin_p&quot; ;</twConstName><twItemCnt>2</twItemCnt><twErrCntSetup>0</twErrCntSetup><twErrCntHold twRaceChecked="FALSE">0</twErrCntHold><twMinOff>8.260</twMinOff></twConstHead></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>COMP &quot;ren&quot; OFFSET = OUT 11 nS  AFTER COMP &quot;clkin_p&quot; ;</twConstName><twItemCnt>4</twItemCnt><twErrCntSetup>0</twErrCntSetup><twErrCntHold twRaceChecked="FALSE">0</twErrCntHold><twMinOff>10.980</twMinOff></twConstHead></twConst><twConst twConstType="twPathConst"><twConstHead><twConstName>TIMEGRP &quot;grp_bcnt&quot; OFFSET = IN 6 nS   VALID 3 nS  BEFORE COMP &quot;clkin_p&quot; HIGH;</twConstName><twItemCnt>0</twItemCnt><twErrCntSetup>0</twErrCntSetup><twErrCntHold twRaceChecked="FALSE">0</twErrCntHold></twConstHead></twConst><twUnmetConstCnt>5</twUnmetConstCnt><twDataSheet twNameLen="19"><twSUH2ClkList twDestWidth = "19" twPhaseWidth = "9"><twDest>clkin_p</twDest><twSUH2Clk ><twSrc>bcnt_p&lt;0&gt;</twSrc><twSUHTime twInternalClk ="tp_1_OBUF" twClkPhase ="0.000" ><twSU2ClkTime twEdge="twRising">1.600</twSU2ClkTime><twH2ClkTime twEdge="twRising">-0.400</twH2ClkTime></twSUHTime></twSUH2Clk><twSUH2Clk ><twSrc>bcnt_p&lt;10&gt;</twSrc><twSUHTime twInternalClk ="tp_1_OBUF" twClkPhase ="0.000" ><twSU2ClkTime twEdge="twRising">1.600</twSU2ClkTime><twH2ClkTime twEdge="twRising">-0.400</twH2ClkTime></twSUHTime></twSUH2Clk><twSUH2Clk ><twSrc>bcnt_p&lt;11&gt;</twSrc><twSUHTime twInternalClk ="tp_1_OBUF" twClkPhase ="0.000" ><twSU2ClkTime twEdge="twRising">1.600</twSU2ClkTime><twH2ClkTime twEdge="twRising">-0.400</twH2ClkTime></twSUHTime></twSUH2Clk><twSUH2Clk ><twSrc>bcnt_p&lt;1&gt;</twSrc><twSUHTime twInternalClk ="tp_1_OBUF" twClkPhase ="0.000" ><twSU2ClkTime twEdge="twRising">1.600</twSU2ClkTime><twH2ClkTime twEdge="twRising">-0.400</twH2ClkTime></twSUHTime></twSUH2Clk><twSUH2Clk ><twSrc>bcnt_p&lt;2&gt;</twSrc><twSUHTime twInternalClk ="tp_1_OBUF" twClkPhase ="0.000" ><twSU2ClkTime twEdge="twRising">1.600</twSU2ClkTime><twH2ClkTime twEdge="twRising">-0.400</twH2ClkTime></twSUHTime></twSUH2Clk><twSUH2Clk ><twSrc>bcnt_p&lt;3&gt;</twSrc><twSUHTime twInternalClk ="tp_1_OBUF" twClkPhase ="0.000" ><twSU2ClkTime twEdge="twRising">1.600</twSU2ClkTime><twH2ClkTime twEdge="twRising">-0.400</twH2ClkTime></twSUHTime></twSUH2Clk><twSUH2Clk ><twSrc>bcnt_p&lt;4&gt;</twSrc><twSUHTime twInternalClk ="tp_1_OBUF" twClkPhase ="0.000" ><twSU2ClkTime twEdge="twRising">1.600</twSU2ClkTime><twH2ClkTime twEdge="twRising">-0.400</twH2ClkTime></twSUHTime></twSUH2Clk><twSUH2Clk ><twSrc>bcnt_p&lt;5&gt;</twSrc><twSUHTime twInternalClk ="tp_1_OBUF" twClkPhase ="0.000" ><twSU2ClkTime twEdge="twRising">1.600</twSU2ClkTime><twH2ClkTime twEdge="twRising">-0.400</twH2ClkTime></twSUHTime></twSUH2Clk><twSUH2Clk ><twSrc>bcnt_p&lt;6&gt;</twSrc><twSUHTime twInternalClk ="tp_1_OBUF" twClkPhase ="0.000" ><twSU2ClkTime twEdge="twRising">1.600</twSU2ClkTime><twH2ClkTime twEdge="twRising">-0.400</twH2ClkTime></twSUHTime></twSUH2Clk><twSUH2Clk ><twSrc>bcnt_p&lt;7&gt;</twSrc><twSUHTime twInternalClk ="tp_1_OBUF" twClkPhase ="0.000" ><twSU2ClkTime twEdge="twRising">1.600</twSU2ClkTime><twH2ClkTime twEdge="twRising">-0.400</twH2ClkTime></twSUHTime></twSUH2Clk><twSUH2Clk ><twSrc>bcnt_p&lt;8&gt;</twSrc><twSUHTime twInternalClk ="tp_1_OBUF" twClkPhase ="0.000" ><twSU2ClkTime twEdge="twRising">1.600</twSU2ClkTime><twH2ClkTime twEdge="twRising">-0.400</twH2ClkTime></twSUHTime></twSUH2Clk><twSUH2Clk ><twSrc>bcnt_p&lt;9&gt;</twSrc><twSUHTime twInternalClk ="tp_1_OBUF" twClkPhase ="0.000" ><twSU2ClkTime twEdge="twRising">1.600</twSU2ClkTime><twH2ClkTime twEdge="twRising">-0.400</twH2ClkTime></twSUHTime></twSUH2Clk><twSUH2Clk ><twSrc>bcnt_res_p</twSrc><twSUHTime twClkPhase="10.000" twInternalClk ="tp_1_OBUF"><twSU2ClkTime twEdge="twFalling">-5.668</twSU2ClkTime><twH2ClkTime twEdge="twFalling">9.335</twH2ClkTime></twSUHTime></twSUH2Clk><twSUH2Clk ><twSrc>evcnt_high_strobe_p</twSrc><twSUHTime twInternalClk ="tp_1_OBUF" twClkPhase ="0.000" ><twSU2ClkTime twEdge="twRising">1.600</twSU2ClkTime><twH2ClkTime twEdge="twRising">-0.400</twH2ClkTime></twSUHTime></twSUH2Clk><twSUH2Clk ><twSrc>evcnt_low_strobe_p</twSrc><twSUHTime twInternalClk ="tp_1_OBUF" twClkPhase ="0.000" ><twSU2ClkTime twEdge="twRising">1.600</twSU2ClkTime><twH2ClkTime twEdge="twRising">-0.400</twH2ClkTime></twSUHTime></twSUH2Clk><twSUH2Clk ><twSrc>txena_in</twSrc><twSUHTime twInternalClk ="tp_1_OBUF" twClkPhase ="0.000" ><twSU2ClkTime twEdge="twRising">4.726</twSU2ClkTime><twH2ClkTime twEdge="twRising">-1.660</twH2ClkTime></twSUHTime></twSUH2Clk></twSUH2ClkList><twClk2OutList twDestWidth = "9" twPhaseWidth = "9"><twSrc>clkin_p</twSrc><twClk2Out  twOutPad = "dout&lt;0&gt;" twMinTime = "8.380" twMinEdge ="twRising" twMaxTime = "10.535" twMaxEdge ="twRising" twInternalClk="tp_1_OBUF" twClkPhase="0.000" ></twClk2Out><twClk2Out  twOutPad = "dout&lt;10&gt;" twMinTime = "8.869" twMinEdge ="twRising" twMaxTime = "10.886" twMaxEdge ="twRising" twInternalClk="tp_1_OBUF" twClkPhase="0.000" ></twClk2Out><twClk2Out  twOutPad = "dout&lt;11&gt;" twMinTime = "9.336" twMinEdge ="twRising" twMaxTime = "10.706" twMaxEdge ="twRising" twInternalClk="tp_1_OBUF" twClkPhase="0.000" ></twClk2Out><twClk2Out  twOutPad = "dout&lt;12&gt;" twMinTime = "8.368" twMinEdge ="twRising" twMaxTime = "11.027" twMaxEdge ="twRising" twInternalClk="tp_1_OBUF" twClkPhase="0.000" ></twClk2Out><twClk2Out  twOutPad = "dout&lt;13&gt;" twMinTime = "9.538" twMinEdge ="twRising" twMaxTime = "11.230" twMaxEdge ="twRising" twInternalClk="tp_1_OBUF" twClkPhase="0.000" ></twClk2Out><twClk2Out  twOutPad = "dout&lt;14&gt;" twMinTime = "9.198" twMinEdge ="twRising" twMaxTime = "10.940" twMaxEdge ="twRising" twInternalClk="tp_1_OBUF" twClkPhase="0.000" ></twClk2Out><twClk2Out  twOutPad = "dout&lt;15&gt;" twMinTime = "7.835" twMinEdge ="twRising" twMaxTime = "10.845" twMaxEdge ="twRising" twInternalClk="tp_1_OBUF" twClkPhase="0.000" ></twClk2Out><twClk2Out  twOutPad = "dout&lt;1&gt;" twMinTime = "8.700" twMinEdge ="twRising" twMaxTime = "11.192" twMaxEdge ="twRising" twInternalClk="tp_1_OBUF" twClkPhase="0.000" ></twClk2Out><twClk2Out  twOutPad = "dout&lt;2&gt;" twMinTime = "8.112" twMinEdge ="twRising" twMaxTime = "10.744" twMaxEdge ="twRising" twInternalClk="tp_1_OBUF" twClkPhase="0.000" ></twClk2Out><twClk2Out  twOutPad = "dout&lt;3&gt;" twMinTime = "8.690" twMinEdge ="twRising" twMaxTime = "10.590" twMaxEdge ="twRising" twInternalClk="tp_1_OBUF" twClkPhase="0.000" ></twClk2Out><twClk2Out  twOutPad = "dout&lt;4&gt;" twMinTime = "8.462" twMinEdge ="twRising" twMaxTime = "10.815" twMaxEdge ="twRising" twInternalClk="tp_1_OBUF" twClkPhase="0.000" ></twClk2Out><twClk2Out  twOutPad = "dout&lt;5&gt;" twMinTime = "8.931" twMinEdge ="twRising" twMaxTime = "10.861" twMaxEdge ="twRising" twInternalClk="tp_1_OBUF" twClkPhase="0.000" ></twClk2Out><twClk2Out  twOutPad = "dout&lt;6&gt;" twMinTime = "8.752" twMinEdge ="twRising" twMaxTime = "11.173" twMaxEdge ="twRising" twInternalClk="tp_1_OBUF" twClkPhase="0.000" ></twClk2Out><twClk2Out  twOutPad = "dout&lt;7&gt;" twMinTime = "8.464" twMinEdge ="twRising" twMaxTime = "10.693" twMaxEdge ="twRising" twInternalClk="tp_1_OBUF" twClkPhase="0.000" ></twClk2Out><twClk2Out  twOutPad = "dout&lt;8&gt;" twMinTime = "8.885" twMinEdge ="twRising" twMaxTime = "10.915" twMaxEdge ="twRising" twInternalClk="tp_1_OBUF" twClkPhase="0.000" ></twClk2Out><twClk2Out  twOutPad = "dout&lt;9&gt;" twMinTime = "9.533" twMinEdge ="twRising" twMaxTime = "11.143" twMaxEdge ="twRising" twInternalClk="tp_1_OBUF" twClkPhase="0.000" ></twClk2Out><twClk2Out  twOutPad = "fsen" twMinTime = "6.566" twMinEdge ="twRising" twMaxTime = "6.566" twMaxEdge ="twRising" twInternalClk="tp_1_OBUF" twClkPhase="0.000" ></twClk2Out><twClk2Out  twOutPad = "fsi" twMinTime = "7.987" twMinEdge ="twRising" twMaxTime = "8.260" twMaxEdge ="twRising" twInternalClk="tp_1_OBUF" twClkPhase="0.000" ></twClk2Out><twClk2Out  twOutPad = "ren" twMinTime = "9.332" twMinEdge ="twRising" twMaxTime = "10.980" twMaxEdge ="twRising" twInternalClk="tp_1_OBUF" twClkPhase="0.000" ></twClk2Out><twClk2Out  twOutPad = "ros_ready" twMinTime = "7.859" twMinEdge ="twRising" twMaxTime = "7.859" twMaxEdge ="twRising" twInternalClk="tp_1_OBUF" twClkPhase="0.000" ></twClk2Out><twClk2Out  twOutPad = "txena" twMinTime = "9.258" twMinEdge ="twRising" twMaxTime = "10.961" twMaxEdge ="twRising" twInternalClk="tp_1_OBUF" twClkPhase="0.000" ></twClk2Out></twClk2OutList><twClk2SUList twDestWidth = "8"><twDest>clk_slow</twDest><twClk2SU><twSrc>clk_slow</twSrc><twRiseRise>1.995</twRiseRise></twClk2SU></twClk2SUList><twClk2SUList twDestWidth = "7"><twDest>clkin_p</twDest><twClk2SU><twSrc>clkin_p</twSrc><twRiseRise>15.201</twRiseRise><twFallRise>7.192</twFallRise></twClk2SU></twClk2SUList></twDataSheet></twErrRpt></twBody><twSum><twErrCnt>5</twErrCnt><twScore>765</twScore><twConstCov><twPathCnt>14490</twPathCnt><twNetCnt>0</twNetCnt><twConnCnt>5824</twConnCnt></twConstCov><twStats><twMinPer>15.201</twMinPer><twMaxFreq>65.785</twMaxFreq><twMaxInAfterClk>18.400</twMaxInAfterClk><twMinInBeforeClk>4.726</twMinInBeforeClk><twMinOutAfterClk>11.230</twMinOutAfterClk></twStats></twSum><twFoot><twTimestamp>Sat May 26 18:45:19 2012</twTimestamp></twFoot><twClientInfo><twClientName>Trace</twClientName><twAttrList><twAttrListItem><twName>Trace Settings</twName><twValue>Peak Memory Usage: 60 MB
</twValue></twAttrListItem></twAttrList></twClientInfo></twReport>
