### Summary

Design Name | rm_registros
Fitting Status | Successful
SW Version | G.35
Device Used | XC2C512-7-PQ208
Date | 2-22-2006, 4:31PM

##### RESOURCES SUMMARY

Macrocells Used | Pterms Used | Registers Used | Pins Used | Function Block Inputs Used
--- | --- | --- | --- | ---
288/512 (57%) | 629/1792 (36%) | 225/512 (44%) | 67/173 (39%) | 588/1280 (46%)

##### PIN RESOURCES

Signal Type | Required | Mapped
--- | --- | ---
Input | 26 | 26
Output | 39 | 39
Bidirectional | 0 | 0
GCK | 1 | 1
GTS | 0 | 0
GSR | 1 | 1

Pin Type | Used | Remaining
--- | --- | ---
I/O | 57 | 106
GCK/IO | 3 | 0
GTS/IO | 4 | 0
GSR/IO | 1 | 0

##### MACROCELL RESOURCES

Total Macrocells Available | 512
Registered Macrocells | 225
Non-registered Macrocells driving I/O | 18

##### GLOBAL RESOURCES

Signal mapped onto global clock net (GCK1) | clk
Signal mapped onto global output enable net (GSR) | reset