### Summary

Design Name | ffrp
Fitting Status | Successful
SW Version | G.35
Device Used | XC2C512-7-PQ208
Date | 2-27-2006, 1:05PM

##### RESOURCES SUMMARY

Macrocells Used | Pterms Used | Registers Used | Pins Used | Function Block Inputs Used
--- | --- | --- | --- | ---
1/512 (1%) | 3/1792 (1%) | 1/512 (1%) | 6/173 (4%) | 3/1280 (1%)

##### PIN RESOURCES

Signal Type | Required | Mapped
--- | --- | ---
Input | 3 | 3
Output | 1 | 1
Bidirectional | 0 | 0
GCK | 1 | 1
GTS | 0 | 0
GSR | 1 | 1

Pin Type | Used | Remaining
--- | --- | ---
I/O | 2 | 161
GCK/IO | 1 | 2
GTS/IO | 2 | 2
GSR/IO | 1 | 0

##### MACROCELL RESOURCES

Total Macrocells Available | 512
Registered Macrocells | 1
Non-registered Macrocells driving I/O | 0

##### GLOBAL RESOURCES

Signal mapped onto global clock net (GCK1) | clk
Signal mapped onto global output enable net (GSR) | pr