### Summary

Design Name | rm_memadd
Fitting Status | Successful
SW Version | G.35
Device Used | XC2C512-7-PQ208
Date | 1-11-2006, 6:18PM

##### RESOURCES SUMMARY

Macrocells Used | Pterms Used | Registers Used | Pins Used | Function Block Inputs Used
--- | --- | --- | --- | ---
64/512 (13%) | 135/1792 (8%) | 31/512 (7%) | 58/173 (34%) | 141/1280 (12%)

##### PIN RESOURCES

Signal Type | Required | Mapped
--- | --- | ---
Input | 38 | 38
Output | 18 | 18
Bidirectional | 0 | 0
GCK | 2 | 2
GTS | 0 | 0
GSR | 0 | 0

Pin Type | Used | Remaining
--- | --- | ---
I/O | 48 | 115
GCK/IO | 3 | 0
GTS/IO | 4 | 0
GSR/IO | 1 | 0

##### MACROCELL RESOURCES

Total Macrocells Available | 512
Registered Macrocells | 31
Non-registered Macrocells driving I/O | 18

##### GLOBAL RESOURCES

Signal mapped onto global clock net (GCK1) | as
Signal mapped onto global clock net (GCK2) | inc_add