### Summary

Design Name | timttc
Fitting Status | Successful
SW Version | G.35
Device Used | XC95288XL-6-TQ144
Date | 9-16-2008, 9:39AM

##### RESOURCES SUMMARY

Macrocells Used | Pterms Used | Registers Used | Pins Used | Function Block Inputs Used
--- | --- | --- | --- | ---
192/288 (67%) | 1022/1440 (71%) | 158/288 (55%) | 94/117 (81%) | 455/864 (53%)

##### PIN RESOURCES

Signal Type | Required | Mapped
--- | --- | ---
Input | 58 | 58
Output | 18 | 18
Bidirectional | 16 | 16
GCK | 2 | 2
GTS | 0 | 0
GSR | 0 | 0

Pin Type | Used | Remaining
--- | --- | ---
I/O | 87 | 22
GCK/IO | 3 | 0
GTS/IO | 3 | 1
GSR/IO | 1 | 0

##### MACROCELL RESOURCES

Total Macrocells Available | 288
Registered Macrocells | 158
Non-registered Macrocells driving I/O | 33

##### GLOBAL RESOURCES

Signal mapped onto global clock net (GCK1) | clk
Signal mapped onto global clock net (GCK2) | qpll_error

##### POWER DATA

Macrocells in high performance mode (MCHP) | 192
Macrocells in low power mode (MCLP) | 0
Total macrocells used (MC) | 192