### Summary

Design Name | timvme1
Fitting Status | Successful
SW Version | G.35
Device Used | XC95288XL-6-TQ144
Date | 8- 9-2007, 8:01PM

##### RESOURCES SUMMARY

Macrocells Used | Pterms Used | Registers Used | Pins Used | Function Block Inputs Used
--- | --- | --- | --- | ---
89/288 (31%) | 326/1440 (23%) | 41/288 (15%) | 77/117 (66%) | 315/864 (37%)

##### PIN RESOURCES

Signal Type | Required | Mapped
--- | --- | ---
Input | 25 | 25
Output | 27 | 27
Bidirectional | 24 | 24
GCK | 1 | 1
GTS | 0 | 0
GSR | 0 | 0

Pin Type | Used | Remaining
--- | --- | ---
I/O | 72 | 37
GCK/IO | 1 | 2
GTS/IO | 3 | 1
GSR/IO | 1 | 0

##### MACROCELL RESOURCES

Total Macrocells Available | 288
Registered Macrocells | 41
Non-registered Macrocells driving I/O | 46

##### GLOBAL RESOURCES

Signal mapped onto global clock net (GCK1) | clk

##### POWER DATA

Macrocells in high performance mode (MCHP) | 89
Macrocells in low power mode (MCLP) | 0
Total macrocells used (MC) | 89